{"text_format":"2","workbook":"xlsx","n_sheets":2,"sheets":["Instructions","Actions"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Instructions","index":0,"n_rows":9724,"n_cols":19,"rows_kept":4500,"cut":true,"hidden":false,"merged":[],"bounds":{"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0}}
["Code métier","Autre identifiant","Nom établissement","Nom instruction","Statut instruction","Date début","Date fin","Description","Code INSEE","Nom commune","Nom département","Nom région","Géolocalisation","Coordonnée X","Coordonnée y","Code ICPE","NAF","NAF Rev1","NAF Rev2"]
["SSP000000101","94.0016","MOIA",null,"En cours",null,null,"En cours","94016","CACHAN","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.3337371,48.79317]
["SSP000000201","93.0023","Ancienne usine à gaz",null,"Clôturée",null,null,"Clôturée","93077","VILLEMOMBLE","SEINE-SAINT-DENIS","ILE-DE-FRANCE","Polygone",2.5057652,48.893593,"J1 - Cokéfaction, usines à gaz"]
["SSP000000301",null,"Actis France",null,"Clôturée",null,null,"Clôturée","93006","BAGNOLET","SEINE-SAINT-DENIS","ILE-DE-FRANCE","Polygone",2.4224894,48.875893]
["SSP000000401",null,"Les Ateliers Bettencourt",null,"Clôturée",null,null,"Clôturée","93006","BAGNOLET","SEINE-SAINT-DENIS","ILE-DE-FRANCE","Polygone",2.4223976,48.85905]
["SSP000000501",null,"Oil France",null,"Clôturée",null,null,"Clôturée","93077","VILLEMOMBLE","SEINE-SAINT-DENIS","ILE-DE-FRANCE","Polygone",2.5018208,48.884968]
["SSP000000601",null,"SIPC",null,"Clôturée",null,null,"Clôturée","93006","BAGNOLET","SEINE-SAINT-DENIS","ILE-DE-FRANCE","Polygone",2.4182765,48.858917]
["SSP000000701","93.0030","FIRSTINOX (ex SFRM)",null,"En cours",null,null,"En cours","93007","LE BLANC MESNIL","SEINE-SAINT-DENIS","ILE-DE-FRANCE","Polygone",2.4405918,48.9371,"J52 - Fonderie des métaux non ferreux"]
["SSP000000901",null,"Auto Joffre",null,"Clôturée",null,null,"Clôturée","93031","EPINAY SUR SEINE","SEINE-SAINT-DENIS","ILE-DE-FRANCE","Polygone",2.2988193,48.960335]
["SSP000001001",null,"Lefortier",null,"Clôturée",null,null,"Clôturée","93077","VILLEMOMBLE","SEINE-SAINT-DENIS","ILE-DE-FRANCE","Polygone",2.5186875,48.88871]
["SSP000001201",null,"Total ELF ANTAR",null,"Clôturée",null,null,"Clôturée","91468","ORMOY","ESSONNE","ILE-DE-FRANCE","Polygone",2.4607036,48.570232]
["SSP000001401",null,"BP Descartes",null,"Clôturée",null,null,"Clôturée","93007","LE BLANC MESNIL","SEINE-SAINT-DENIS","ILE-DE-FRANCE","Polygone",2.461094,48.94924]
["SSP000001501",null,"Guy Dauphin Environnement (GDE)",null,"Clôturée",null,null,"Clôturée","93064","ROSNY SOUS BOIS","SEINE-SAINT-DENIS","ILE-DE-FRANCE","Polygone",2.4861755,48.86573]
["SSP000001601",null,"OA France",null,"Clôturée",null,null,"Clôturée","93031","EPINAY SUR SEINE","SEINE-SAINT-DENIS","ILE-DE-FRANCE","Polygone",2.327381,48.948242]
["SSP000001701","93.0061","Station-service Total",null,"En cours",null,null,"En cours","93031","EPINAY SUR SEINE","SEINE-SAINT-DENIS","ILE-DE-FRANCE","Polygone",2.3089654,48.955944,"L23 - Détail de carburants"]
["SSP000001901","93.0003","B.A.S.F.",null,"En cours",null,null,"En cours","93013","LE BOURGET","SEINE-SAINT-DENIS","ILE-DE-FRANCE","Polygone",2.4211824,48.932735,"D4 - Encres, vernis, peintures, colles (fabrication de)"]
["SSP000002101",null,"STECCO (époux FIOT)",null,"Clôturée",null,null,"Clôturée","91390","MEREVILLE","ESSONNE","ILE-DE-FRANCE","Polygone",2.0990438,48.316143]
["SSP000002301","78.0018","SOCIETE COPRIM RESIDENCES (SHELL DIRECT)",null,"En cours",null,null,"En cours","78158","LE CHESNAY","YVELINES","ILE-DE-FRANCE","Polygone",2.1279,48.819004,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000002401",null,"Décharge du MESNIL",null,"Clôturée",null,null,"Clôturée","91593","SERMAISE","ESSONNE","ILE-DE-FRANCE","Polygone",2.0993679,48.53563]
["SSP000002501","78.0068","Station ELF (BP)",null,"En cours",null,null,"En cours","78158","LE CHESNAY","YVELINES","ILE-DE-FRANCE","Polygone",2.1288168,48.82826,"L23 - Détail de carburants"]
["SSP000002601","78.0056","FENWICK - LINDE",null,"En cours",null,null,"En cours","78158","LE CHESNAY","YVELINES","ILE-DE-FRANCE","Polygone",2.121599,48.820362]
["SSP000002801","78.0019","RESIDENCE DU PETIT BONTEMPS",null,"En cours",null,null,"En cours","78490","PLAISIR","YVELINES","ILE-DE-FRANCE","Polygone",1.9506054,48.82587,"I21 - Chaufferies urbaines"]
["SSP000002901","78.0106","SGI",null,"En cours",null,null,"En cours","78490","PLAISIR","YVELINES","ILE-DE-FRANCE","Polygone",1.9802709,48.80361,"H - Mécanique, traitements des surfaces"]
["SSP000003001","77.0021","Centre EDF / GDF Service Ile de France","Centre EDF / GDF Service Ile de France","En cours",null,null,"En cours","77108","CHELLES","SEINE-ET-MARNE","ILE-DE-FRANCE","Polygone",2.5882773,48.872215,"J1 - Cokéfaction, usines à gaz"]
["SSP000003101",null,"Société NICOLITCH",null,"Clôturée",null,null,"Clôturée","91338","LIMOURS","ESSONNE","ILE-DE-FRANCE","Polygone",2.0909708,48.643612]
["SSP000003201",null,"Société MELCO",null,"Clôturée",null,null,"Clôturée","91338","LIMOURS","ESSONNE","ILE-DE-FRANCE","Polygone",2.0915117,48.64381]
["SSP000003301","78.0114","WOREX SNC",null,"En cours",null,null,"En cours","78490","PLAISIR","YVELINES","ILE-DE-FRANCE","Polygone",1.972185,48.802666,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000003401","78.0048","Ancienne usine à gaz de Montfort l'Amaury",null,"En cours",null,null,"En cours","78420","MONTFORT L'AMAURY","YVELINES","ILE-DE-FRANCE","Polygone",1.8145587,48.781677,"J1 - Cokéfaction, usines à gaz"]
["SSP000003501","78.0009","Ancienne usine à gaz de Mantes-la-Jolie",null,"En cours",null,null,"En cours","78361","MANTES LA JOLIE","YVELINES","ILE-DE-FRANCE","Polygone",1.7226619,48.98726,"J1 - Cokéfaction, usines à gaz"]
["SSP000003601","78.0062","CCM Sulzer",null,"En cours",null,null,"En cours","78362","MANTES LA VILLE","YVELINES","ILE-DE-FRANCE","Polygone",1.6985024,48.986504]
["SSP000003602","78.0063","CCM Sulzer",null,"En cours",null,null,"En cours","78362","MANTES LA VILLE","YVELINES","ILE-DE-FRANCE","Polygone",1.6985024,48.986504]
["SSP000003701","78.0066","SNCF",null,"En cours",null,null,"En cours","78361","MANTES LA JOLIE","YVELINES","ILE-DE-FRANCE","Polygone",1.6966051,48.99045]
["SSP000003801","78.0067","ECOVALOR",null,"En cours",null,null,"En cours","78361","MANTES LA JOLIE","YVELINES","ILE-DE-FRANCE","Polygone",1.6922321,48.99102]
["SSP000003901","78.0094","Grand Garage de Chantereine (station-service)",null,"En cours",null,null,"En cours","78361","MANTES LA JOLIE","YVELINES","ILE-DE-FRANCE","Polygone",1.6782293,48.996872,"L23 - Détail de carburants"]
["SSP000004001","91.0039","Ancienne Compagnie Papetière de l'Essone (CPE)",null,"Clôturée",null,null,"Clôturée","91174","CORBEIL ESSONNES","ESSONNE","ILE-DE-FRANCE","Polygone",2.469352,48.59138,"C22 - Fabrication de papiers et carton"]
["SSP000004101","91.0074","Ancienne Usine à Gaz",null,"En cours",null,null,"En cours","91174","CORBEIL ESSONNES","ESSONNE","ILE-DE-FRANCE","Polygone",2.4747875,48.617283,"J1 - Cokéfaction, usines à gaz"]
["SSP000004201","91.0119","Imprimerie HELIO CORBEIL",null,"En cours",null,null,"En cours","91174","CORBEIL ESSONNES","ESSONNE","ILE-DE-FRANCE","Polygone",2.4782047,48.61312,"H21 - Imprimerie, presse, édition"]
["SSP000004301","91.0037","Société MIGNON et FILS (SMF)",null,"Clôturée",null,null,"Clôturée","91174","CORBEIL ESSONNES","ESSONNE","ILE-DE-FRANCE","Polygone",2.4821954,48.602055,"K35 - Regroupement, reconditionnement de déchets"]
["SSP000004401","91.0105","MARREL DECAUVILLE SA",null,"En cours",null,null,"En cours","91174","CORBEIL ESSONNES","ESSONNE","ILE-DE-FRANCE","Polygone",2.468949,48.621918,"H1 - Mécanique, électrique, traitement de surface"]
["SSP000004501","78.0087","FCI MICROCONNECTIONS",null,"En cours",null,null,"En cours","78361","MANTES LA JOLIE","YVELINES","ILE-DE-FRANCE","Polygone",1.6840442,48.99248,"H13 - Traitement de surface"]
["SSP000004601","78.0013","PHOTEC INDUSTRIES",null,"En cours",null,null,"En cours","78361","MANTES LA JOLIE","YVELINES","ILE-DE-FRANCE","Polygone",1.7146585,48.98202,"H18 - Composants électroniques (fabrication de)"]
["SSP000004701","78.0104","SOPRAL (ex-Dunlopillo)",null,"En cours",null,null,"En cours","78361","MANTES LA JOLIE","YVELINES","ILE-DE-FRANCE","Polygone",1.7038152,49.003258,"D7 - Caoutchouc et matières plastiques"]
["SSP000004801","92.0081","SOCIETE DES PETROLES SHELL",null,"En cours",null,null,"En cours","92060","LE PLESSIS ROBINSON","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.281025,48.783398,"L23 - Détail de carburants"]
["SSP000005001","95.0057","HUTCHINSON MAPA",null,"En cours",null,null,"En cours","95680","VILLIERS LE BEL","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.409296,49.000214]
["SSP000005101",null,"Société Commerciale Automobile (SCA) _ ex DESRUES",null,"Clôturée",null,null,"Clôturée","91174","CORBEIL ESSONNES","ESSONNE","ILE-DE-FRANCE","Polygone",2.4781826,48.591015]
["SSP000005201",null,"Etablissements GONCALVES",null,"Clôturée",null,null,"Clôturée","91174","CORBEIL ESSONNES","ESSONNE","ILE-DE-FRANCE","Polygone",2.4636724,48.607647]
["SSP000005401","95.0013","OSNY PHARMA SAS (ex CATALENT PHARMA SOLUTIONS)",null,"En cours",null,null,"En cours","95476","OSNY","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.0681999,49.060413,"M3 - Santé"]
["SSP000005501","78.0026","ETABLISSEMENT PETROLIER DE GARGENVILLE - TOTAL Raffinage France",null,"En cours",null,null,"En cours","78267","GARGENVILLE","YVELINES","ILE-DE-FRANCE","Polygone",1.7915324,48.975,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000005601",null,"Station Service BP Montconseil",null,"Clôturée",null,null,"Clôturée","91174","CORBEIL ESSONNES","ESSONNE","ILE-DE-FRANCE","Polygone",2.480215,48.600826]
["SSP000005701",null,"Ecole élémentaire Jacques Prévert",null,"Clôturée",null,null,"Clôturée","91174","CORBEIL ESSONNES","ESSONNE","ILE-DE-FRANCE","Polygone",2.4635193,48.618164]
["SSP000005801","78.0072","PORCHER",null,"En cours",null,null,"En cours","78267","GARGENVILLE","YVELINES","ILE-DE-FRANCE","Polygone",1.8077713,48.980373]
["SSP000005901",null,"Ancienne décharge de Méréville",null,"Clôturée",null,null,"Clôturée","91390","MEREVILLE","ESSONNE","ILE-DE-FRANCE","Polygone",2.0819714,48.31257]
["SSP000006001",null,"Aluza",null,"Clôturée",null,null,"Clôturée","95203","EAUBONNE","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.2773895,49.00331]
["SSP000006101",null,"Casse RN16",null,"Clôturée",null,null,"Clôturée","95680","VILLIERS LE BEL","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.3844714,49.00467]
["SSP000006201","78.0033","S.A.R.P. INDUSTRIES",null,"En cours",null,null,"En cours","78335","LIMAY","YVELINES","ILE-DE-FRANCE","Polygone",1.7506636,48.974113,"K3 - Traitement de déchets industriels"]
["SSP000006301","92.0091","STATION-SERVICE ELF RELAIS DE BAGNEUX",null,"En cours",null,null,"En cours","92007","BAGNEUX","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.3188057,48.80283,"L23 - Détail de carburants"]
["SSP000006601","92.0036","ALCATEL CABLES (ex CABLES DE LYON)",null,"En cours",null,null,"En cours","92024","CLICHY","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.2973294,48.90173,"H17 - Fils et câbles électriques (fabrication de)"]
["SSP000006801","78.0046","Site de l'ancienne usine à gaz de Houdan",null,"En cours",null,null,"En cours","78310","HOUDAN","YVELINES","ILE-DE-FRANCE","Polygone",1.6045253,48.79478,"J1 - Cokéfaction, usines à gaz"]
["SSP000006901","93.0005","Station service SHELL",null,"En cours",null,null,"En cours","93048","MONTREUIL","SEINE-SAINT-DENIS","ILE-DE-FRANCE","Polygone",2.4321296,48.8688,"L23 - Détail de carburants"]
["SSP000007001","78.0024","C.P.T. EDF PORCHEVILLE",null,"En cours",null,null,"En cours","78501","PORCHEVILLE","YVELINES","ILE-DE-FRANCE","Polygone",1.7586497,48.97102,"I11 - Centrales électriques thermiques"]
["SSP000007201","91.0087","Didier SIPC",null,"En cours",null,null,"En cours","91105","BREUILLET","ESSONNE","ILE-DE-FRANCE","Polygone",2.1661437,48.564487,"G14 - Fabrication d'autres matériaux de construction"]
["SSP000007401","91.0022","Usine Sofra PCB",null,"En cours",null,null,"En cours","91386","MENNECY","ESSONNE","ILE-DE-FRANCE","Polygone",2.4310484,48.560345,"H18 - Composants électroniques (fabrication de)"]
["SSP000007601","91.0038","Ancien site papetier de SIRP (Societe Industrielle de Recyclage de Papier)","SIRP","Clôturée",null,null,"Clôturée","91174","CORBEIL ESSONNES","ESSONNE","ILE-DE-FRANCE","Polygone",2.4673398,48.592567,"C22 - Fabrication de papiers et carton"]
["SSP000007701","91.0006","Lotissement la Basiniere \"Les Terres Noires\"",null,"En cours",null,null,"En cours","91540","SAINT CHERON","ESSONNE","ILE-DE-FRANCE","Polygone",2.12926,48.551197,"H16 - Piles électriques et accumulateurs (fabrication de)"]
["SSP000007801","91.0035","Ancien site DEBONO",null,"En cours",null,null,"En cours","91540","SAINT CHERON","ESSONNE","ILE-DE-FRANCE","Polygone",2.1064477,48.54188,"D32 - Chimie minérale inorganique autre"]
["SSP000007901","91.0009","Société VERALINE",null,"En cours",null,null,"En cours","91468","ORMOY","ESSONNE","ILE-DE-FRANCE","Polygone",2.4542618,48.569466,"C13 - Traitement du bois"]
["SSP000008001",null,"Société MIGNON et FILS (SMF)",null,"Clôturée",null,null,"Clôturée","91135","CHAMPCUEIL","ESSONNE","ILE-DE-FRANCE","Polygone",2.4330099,48.511833]
["SSP000008101","91.0005","Total - Relais des Cordiers",null,"En cours",null,null,"En cours","91471","ORSAY","ESSONNE","ILE-DE-FRANCE","Polygone",2.1859827,48.69733,"L23 - Détail de carburants"]
["SSP000008201",null,"Station-service SHELL",null,"Clôturée",null,null,"Clôturée","91471","ORSAY","ESSONNE","ILE-DE-FRANCE","Polygone",2.1820726,48.69338]
["SSP000008301",null,"Société BONNERON-GUNET",null,"Clôturée",null,null,"Clôturée","91390","MEREVILLE","ESSONNE","ILE-DE-FRANCE","Polygone",2.090056,48.316025]
["SSP000008501","91.0020","ALTIS Semiconductor",null,"En cours",null,null,"En cours","91174","CORBEIL ESSONNES","ESSONNE","ILE-DE-FRANCE","Polygone",2.474813,48.57097,"H18 - Composants électroniques (fabrication de)"]
["SSP000008601","91.0115","OIL FRANCE",null,"Clôturée",null,null,"Clôturée","91687","VIRY CHATILLON","ESSONNE","ILE-DE-FRANCE","Polygone",2.3785582,48.671467]
["SSP000008801",null,"DUNO INTERMARCHE",null,"Clôturée",null,null,"Clôturée","91468","ORMOY","ESSONNE","ILE-DE-FRANCE","Polygone",2.4574602,48.569855]
["SSP000008901",null,"Société SAMSON",null,"Clôturée",null,null,"Clôturée","91533","SACLAS","ESSONNE","ILE-DE-FRANCE","Polygone",2.1065807,48.337]
["SSP000009101","93.0060","PROTEC DECORS","Réhabilitation","En cours",null,null,"En cours","93010","BONDY","SEINE-SAINT-DENIS","ILE-DE-FRANCE","Polygone",2.4921632,48.890453,"H13 - Traitement de surface"]
["SSP000009301","92.0012","Gaz de France Centre National de l'Equipement",null,"En cours",null,null,"En cours","92024","CLICHY","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.2951407,48.90346,"J1 - Cokéfaction, usines à gaz"]
["SSP000009501",null,"LRVS",null,"Clôturée",null,null,"Clôturée","78501","PORCHEVILLE","YVELINES","ILE-DE-FRANCE","Polygone",1.7642384,48.9891]
["SSP000009601",null,"PROCEDES RENFORS SA",null,"Clôturée",null,null,"Clôturée","92024","CLICHY","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.3077197,48.90219]
["SSP000009701",null,"SEMERCLI BIC",null,"Clôturée",null,null,"Clôturée","92024","CLICHY","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.304346,48.897392]
["SSP000010101","94.0102","ESSCOUNT",null,"En cours",null,null,"En cours","94011","BONNEUIL SUR MARNE","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.4782202,48.767544,"L23 - Détail de carburants"]
["SSP000010201","94.0015","PHYTO LABO (ex)",null,"En cours",null,null,"En cours","94011","BONNEUIL SUR MARNE","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.5031896,48.782135]
["SSP000010301","94.0006","TOTAL DEPOT PETROLIER IVRY","Cessation d'activité","En cours",null,null,"En cours","94041","IVRY SUR SEINE","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.4073734,48.812717,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000010401","94.0054","KODAK",null,"En cours",null,null,"En cours","94080","VINCENNES","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.4297626,48.842987,"D5 - Fabrication de produits photographiques"]
["SSP000010501","94.0025","SOFICOR MADER (EX BOLLORE JIVAL)",null,"En cours",null,null,"En cours","94081","VITRY SUR SEINE","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.4149337,48.793533,"D4 - Encres, vernis, peintures, colles (fabrication de)"]
["SSP000010701","94.0056","AIR LIQUIDE","Dépollution du site","En cours",null,null,"En cours","94017","CHAMPIGNY SUR MARNE","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.5039165,48.81219]
["SSP000010801","94.0052","TOTAL RELAIS LUSSAC",null,"En cours",null,null,"En cours","94019","CHENNEVIERES SUR MARNE","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.5421777,48.79857]
["SSP000010901","94.0043","Aerospatiale Matra Missiles",null,"En cours",null,null,"En cours","94041","IVRY SUR SEINE","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.390903,48.819523]
["SSP000011001","94.0057","SNDI",null,"En cours",null,null,"En cours","94041","IVRY SUR SEINE","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.386027,48.818077,"E3 - Laveries, blanchisseries, pressing"]
["SSP000011101","94.0008","STATION-SERVICE ELF CONTACT",null,"En cours",null,null,"En cours","94037","GENTILLY","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.349997,48.813797,"L23 - Détail de carburants"]
["SSP000011201","94.0050","BP FRANCE",null,"En cours",null,null,"En cours","94052","NOGENT SUR MARNE","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.478066,48.838516,"L23 - Détail de carburants"]
["SSP000011501","94.0058","FACOM",null,"En cours",null,null,"En cours","94077","VILLENEUVE LE ROI","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.4317703,48.739063,"H1 - Mécanique, électrique, traitement de surface"]
["SSP000011701","94.0090","SITA ILE DE FRANCE",null,"En cours",null,null,"En cours","94003","ARCUEIL","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.3427072,48.805492,"K22 - Regroupement d'OM, DIB"]
["SSP000011801","94.0051","ZSCHIMMER & SCHWARZ FRANCE",null,"En cours",null,null,"En cours","94003","ARCUEIL","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.3400662,48.807293,"D62 - Fabrication de détergents"]
["SSP000011901","94.0086","BP ACACIAS",null,"En cours",null,null,"En cours","94004","BOISSY SAINT LEGER","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.5000274,48.76009,"L23 - Détail de carburants"]
["SSP000012001","94.0065","BERGERAT MONNOYEUR",null,"En cours",null,null,"En cours","94011","BONNEUIL SUR MARNE","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.5000546,48.78158,"L21 - Vente et réparation automobile"]
["SSP000012101",null,"ARMABESSAIRE",null,"Clôturée",null,null,"Clôturée","94019","CHENNEVIERES SUR MARNE","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.52649,48.799374]
["SSP000012201","94.0097","LA PIECE AUTOMOBILE",null,"En cours",null,null,"En cours","94021","CHEVILLY LARUE","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.3667881,48.775635]
["SSP000012301","94.0074","BHV",null,"En cours",null,null,"En cours","94041","IVRY SUR SEINE","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.4018893,48.81652,"L1 - Entreposage, manutention, commerces"]
["SSP000012401","94.0064","VIT'APPRETS",null,"En cours",null,null,"En cours","94041","IVRY SUR SEINE","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.3833244,48.81678,"E3 - Laveries, blanchisseries, pressing"]
["SSP000012501","94.0070","BIG AUTO",null,"En cours",null,null,"En cours","94081","VITRY SUR SEINE","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.3704064,48.77317]
["SSP000012601","94.0069","D. ANTONELLI",null,"En cours",null,null,"En cours","94081","VITRY SUR SEINE","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.3688262,48.772617,"K5 - Récupération, dépôts de ferrailles"]
["SSP000012701","94.0027","TRANSRACK",null,"En cours",null,null,"En cours","94068","SAINT MAUR DES FOSSES","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.4860988,48.785507,"H13 - Traitement de surface"]
["SSP000012801","94.0048","LE METAL OUVRE",null,"En cours",null,null,"En cours","94068","SAINT MAUR DES FOSSES","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.4765403,48.792927,"J52 - Fonderie des métaux non ferreux"]
["SSP000012901","94.0046","CERLIVE",null,"En cours",null,null,"En cours","94068","SAINT MAUR DES FOSSES","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.4837503,48.78561,"H13 - Traitement de surface"]
["SSP000013001",null,"ESSO",null,"Clôturée",null,null,"Clôturée","94080","VINCENNES","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.430485,48.84572]
["SSP000013101","94.0077","TOTAL RELAIS ELF LE-PERREUX",null,"En cours",null,null,"En cours","94058","LE PERREUX SUR MARNE","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.5089564,48.849873,"L23 - Détail de carburants"]
["SSP000013201","94.0076","SHELL",null,"En cours",null,null,"En cours","94058","LE PERREUX SUR MARNE","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.49501,48.851578]
["SSP000013301","94.0094","SHELL",null,"En cours",null,null,"En cours","94041","IVRY SUR SEINE","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.3930893,48.82183]
["SSP000013401","94.0080","TOTAL RELAIS MIREBEAU",null,"En cours",null,null,"En cours","94016","CACHAN","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.32819,48.784855,"L23 - Détail de carburants"]
["SSP000013601","94.0071","ACUMENT",null,"En cours",null,null,"En cours","94011","BONNEUIL SUR MARNE","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.4804769,48.77899,"H13 - Traitement de surface"]
["SSP000013801",null,"KAPS",null,"Clôturée",null,null,"Clôturée","94068","SAINT MAUR DES FOSSES","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.4894514,48.785316]
["SSP000014401",null,"ENDUITOIT",null,"Clôturée",null,null,"Clôturée","94016","CACHAN","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.333438,48.792686]
["SSP000014501",null,"TOTAL RELAIS DU KREMLIN-BICETRE",null,"Clôturée",null,null,"Clôturée","94043","LE KREMLIN BICETRE","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.3490841,48.806133]
["SSP000014601","94.0081","ERCUIS",null,"En cours",null,null,"En cours","94060","LA QUEUE EN BRIE","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.5856006,48.787037,"H1 - Mécanique, électrique, traitement de surface"]
["SSP000014701",null,"SDF NOEL",null,"Clôturée",null,null,"Clôturée","94017","CHAMPIGNY SUR MARNE","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.4938421,48.821636]
["SSP000014801","94.0079","TOTAL RELAIS STE COLOMBE",null,"En cours",null,null,"En cours","94038","L'HAY LES ROSES","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.36627,48.779415,"L23 - Détail de carburants"]
["SSP000015101",null,"TOTAL RELAIS NOTRE-DAME",null,"Clôturée",null,null,"Clôturée","94060","LA QUEUE EN BRIE","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.577518,48.78032]
["SSP000015201","94.0087","MANUFACTURE CARTIER LUNETTES (MCL)",null,"En cours",null,null,"En cours","94042","JOINVILLE LE PONT","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.4685717,48.815662,"H13 - Traitement de surface"]
["SSP000015301","94.0084","TOTAL RELAIS ELF-ARCUEIL",null,"En cours",null,null,"En cours","94003","ARCUEIL","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.331908,48.812645]
["SSP000015401","94.0078","CASINO CARBURANTS",null,"En cours",null,null,"En cours","94004","BOISSY SAINT LEGER","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.5112536,48.745853,"L23 - Détail de carburants"]
["SSP000015501","94.0021","SAD",null,"En cours",null,null,"En cours","94046","MAISONS ALFORT","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.4194858,48.815495,"D - Chimie, parachimie, pétrole"]
["SSP000015601",null,"GARAGE DE LA MAIRIE",null,"Clôturée",null,null,"Clôturée","94067","SAINT MANDE","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.4181976,48.84525]
["SSP000015901",null,"LE HAMEAU DES BORDS DE MARNE (EX THOMSON)",null,"Clôturée",null,null,"Clôturée","94042","JOINVILLE LE PONT","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.4742568,48.82936]
["SSP000016001","94.0047","CALDEO",null,"En cours",null,null,"En cours","94015","BRY SUR MARNE","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.5182643,48.8392,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000016201",null,"Patin SCP (Société Charbonnière Pétrolière)",null,"Clôturée",null,null,"Clôturée","94011","BONNEUIL SUR MARNE","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.4752247,48.78577]
["SSP000016301",null,"FER",null,"Clôturée",null,null,"Clôturée","94016","CACHAN","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.333591,48.792908]
["SSP000016401",null,"TOTAL RELAIS DE LA BIEVRE",null,"Clôturée",null,null,"Clôturée","94003","ARCUEIL","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.3413415,48.807766]
["SSP000016801","94.0083","BP - VILLEJUIF",null,"En cours",null,null,"En cours","94076","VILLEJUIF","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.3558717,48.78115]
["SSP000016901","94.0093","TOTAL - RELAIS DE LA SURETTE",null,"En cours",null,null,"En cours","94077","VILLENEUVE LE ROI","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.439542,48.727123,"L23 - Détail de carburants"]
["SSP000017001","94.0107","AUTO SERVICE 94",null,"En cours",null,null,"En cours","94038","L'HAY LES ROSES","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.3440444,48.775867,"L23 - Détail de carburants"]
["SSP000017201","94.0089","DIDERON-CIG",null,"En cours",null,null,"En cours","94011","BONNEUIL SUR MARNE","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.5012336,48.783176,"K3 - Traitement de déchets industriels"]
["SSP000017501","94.0101","SOCIETE D'EXPLOITATION DES ETABLISSEMENTS MARANNE",null,"En cours",null,null,"En cours","94017","CHAMPIGNY SUR MARNE","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.5074813,48.81914,"K5 - Récupération, dépôts de ferrailles"]
["SSP000017601",null,"ZAC ALBERT 1ER",null,"Clôturée",null,null,"Clôturée","94052","NOGENT SUR MARNE","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.493572,48.832924]
["SSP000017801","78.0037","ALPA",null,"En cours",null,null,"En cours","78501","PORCHEVILLE","YVELINES","ILE-DE-FRANCE","Polygone",1.762652,48.983208,"J51 - Fonderie des métaux ferreux"]
["SSP000018001",null,"CMBP",null,"Clôturée",null,null,"Clôturée","78501","PORCHEVILLE","YVELINES","ILE-DE-FRANCE","Polygone",1.7672033,48.988506]
["SSP000018101","93.0031","Benitah",null,"En cours",null,null,"En cours","93059","PIERREFITTE SUR SEINE","SEINE-SAINT-DENIS","ILE-DE-FRANCE","Polygone",2.355865,48.96105]
["SSP000018201",null,"AB INDUSTRIE",null,"Clôturée",null,null,"Clôturée","78501","PORCHEVILLE","YVELINES","ILE-DE-FRANCE","Polygone",1.7661296,48.988373]
["SSP000018301","78.0044","Ancienne usine à gaz de TRIEL SUR SEINE",null,"En cours",null,null,"En cours","78624","TRIEL SUR SEINE","YVELINES","ILE-DE-FRANCE","Polygone",2.0089417,48.970432,"J1 - Cokéfaction, usines à gaz"]
["SSP000018501","78.0086","LABO - SERVICES",null,"En cours",null,null,"En cours","78624","TRIEL SUR SEINE","YVELINES","ILE-DE-FRANCE","Polygone",1.9997976,48.97236,"K35 - Regroupement, reconditionnement de déchets"]
["SSP000018601","95.0034","OPAC de l'Oise",null,"En cours",null,null,"En cours","95277","GONESSE","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.421557,48.994614,"D7 - Caoutchouc et matières plastiques"]
["SSP000018701","92.0041","TRIMETAL - AKZONOBEL",null,"En cours",null,null,"En cours","92036","GENNEVILLIERS","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.3118994,48.93333,"D42 - Fabrication de peintures"]
["SSP000018801","92.0037","CIM - GENNEVILLIERS",null,"En cours",null,null,"En cours","92036","GENNEVILLIERS","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.316197,48.92228,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000018901","92.0043","DOCKS PETROLIERS DE PARIS (Labo services)",null,"En cours",null,null,"En cours","92036","GENNEVILLIERS","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.2961285,48.94879,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000019101","53.0024","FONDERIE MAYENNAISE SAS",null,"En cours",null,null,"En cours","53147","MAYENNE","MAYENNE","PAYS DE LA LOIRE","Polygone",-0.60552704,48.319073,"J5 - Fonderie et travail des métaux"]
["SSP000019201","41.0001","Usine à Gaz",null,"En cours",null,null,"En cours","41018","BLOIS","LOIR-ET-CHER","CENTRE-VAL DE LOIRE","Polygone",1.3259753,47.586517,"J1 - Cokéfaction, usines à gaz"]
["SSP000019301","41.0056","Blois DECAP",null,"En cours",null,null,"En cours","41018","BLOIS","LOIR-ET-CHER","CENTRE-VAL DE LOIRE","Polygone",1.349209,47.587482,"H13 - Traitement de surface"]
["SSP000019401","41.0046","SAGANA",null,"En cours",null,null,"En cours","41018","BLOIS","LOIR-ET-CHER","CENTRE-VAL DE LOIRE","Polygone",1.3177761,47.583397,"H1 - Mécanique, électrique, traitement de surface"]
["SSP000019601","41.0059","EUROCOATINGS",null,"En cours",null,null,"En cours","41018","BLOIS","LOIR-ET-CHER","CENTRE-VAL DE LOIRE","Polygone",1.3226221,47.6011]
["SSP000019701","41.0030","DUMAS",null,"En cours",null,null,"En cours","41018","BLOIS","LOIR-ET-CHER","CENTRE-VAL DE LOIRE","Polygone",1.3419797,47.584717,"K51 - Récupération non ferreux"]
["SSP000019801","93.0008","BASF (Les Couleurs de Paris)",null,"Clôturée",null,null,"Clôturée","93061","LE PRE SAINT GERVAIS","SEINE-SAINT-DENIS","ILE-DE-FRANCE","Polygone",2.405379,48.88786,"D4 - Encres, vernis, peintures, colles (fabrication de)"]
["SSP000019901",null,"Occamat",null,"Clôturée",null,null,"Clôturée","95277","GONESSE","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.4743319,48.990974]
["SSP000020101","77.0010","SOPALUNA  - TSO",null,"En cours",null,null,"En cours","77108","CHELLES","SEINE-ET-MARNE","ILE-DE-FRANCE","Polygone",2.6092167,48.868793]
["SSP000020201","45.0018","Centre EDF-GDF Services Loiret",null,"En cours",null,null,"En cours","45234","ORLEANS","LOIRET","CENTRE-VAL DE LOIRE","Polygone",1.9075357,47.90748,"J1 - Cokéfaction, usines à gaz"]
["SSP000020301","45.0047","Ex Garage PETITNET",null,"En cours",null,null,"En cours","45232","OLIVET","LOIRET","CENTRE-VAL DE LOIRE","Polygone",1.9036113,47.87578,"L23 - Détail de carburants"]
["SSP000020401","45.0066","Station service \"Relais du Bois Joli\"",null,"En cours",null,null,"En cours","45302","SARAN","LOIRET","CENTRE-VAL DE LOIRE","Polygone",1.8931034,47.942924,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000020501","45.0052","Station service ELF \"Relais de Piquerolière\"",null,"En cours",null,null,"En cours","45075","LA CHAPELLE SAINT MESMIN","LOIRET","CENTRE-VAL DE LOIRE","Polygone",1.8519998,47.893887,"L23 - Détail de carburants"]
["SSP000020601",null,"DRC (Durand Raucher et Camuzat)",null,"Clôturée",null,null,"Clôturée","95277","GONESSE","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.4512901,48.984837]
["SSP000020701","77.0010","SOPALUNA - Auto Eco",null,"En cours",null,null,"En cours","77108","CHELLES","SEINE-ET-MARNE","ILE-DE-FRANCE","Polygone",2.6104026,48.868782]
["SSP000020901","77.0032","BERTHOLLET AMM INDUSTRIE (EX Meurant TS Ex Chelles Electrolyse)","BERTHOLLET AMM INDUSTRIE (EX Meurant TS Ex Chelles Electrolyse)","En cours",null,null,"En cours","77108","CHELLES","SEINE-ET-MARNE","ILE-DE-FRANCE","Polygone",2.5973825,48.87036]
["SSP000021001","77.0034","PAREXLANKO (ex Lafarge Produits Formules)","PAREXLANKO (ex Lafarge Produits Formules)","En cours",null,null,"En cours","77243","LAGNY SUR MARNE","SEINE-ET-MARNE","ILE-DE-FRANCE","Polygone",2.681611,48.8755]
["SSP000021101","77.0098","NODET GOUGIS (Site des Noues)","NODET GOUGIS (Site des Noues)","En cours",null,null,"En cours","77305","MONTEREAU FAULT YONNE","SEINE-ET-MARNE","ILE-DE-FRANCE","Polygone",2.9533145,48.380737,"J53 - Travail des métaux, chaudronnerie, poudres"]
["SSP000021201","77.0121","MAVIDIS Centre E leclerc",null,"En cours",null,null,"En cours","77514","VILLEPARISIS","SEINE-ET-MARNE","ILE-DE-FRANCE","Polygone",2.6083407,48.953]
["SSP000021301","77.0090","ARLEQUIN (ex-LDF)","ARLEQUIN (ex-LDF)","En cours",null,null,"En cours","77294","MITRY MORY","SEINE-ET-MARNE","ILE-DE-FRANCE","Polygone",2.631083,48.983704]
["SSP000021401","77.0120","Devoisselle","Devoisselle","En cours",null,null,"En cours","77152","DAMMARIE LES LYS","SEINE-ET-MARNE","ILE-DE-FRANCE","Polygone",2.6240804,48.51786]
["SSP000021501","77.0105","Ets Gilles VANNIER - SUD",null,"En cours",null,null,"En cours","77118","CLAYE SOUILLY","SEINE-ET-MARNE","ILE-DE-FRANCE","Polygone",2.681461,48.94556]
["SSP000021601","77.0086","SDPA (Societe Dammarienne de Pieces Automobiles)","SDPA (Societe Dammarienne de Pieces Automobiles)","En cours",null,null,"En cours","77152","DAMMARIE LES LYS","SEINE-ET-MARNE","ILE-DE-FRANCE","Polygone",2.6460238,48.52885]
["SSP000021701","77.0127","MOULINS DE MELUN","MOULINS DE MELUN","En cours",null,null,"En cours","77288","MELUN","SEINE-ET-MARNE","ILE-DE-FRANCE","Polygone",2.656614,48.536503,"B1 - Industrie agro-alimentaire"]
["SSP000022101","77.0110","FEDIAC","FEDIAC","En cours",null,null,"En cours","77243","LAGNY SUR MARNE","SEINE-ET-MARNE","ILE-DE-FRANCE","Polygone",2.6871822,48.877964,"D3 - Chimie, phytosanitaire, pharmacie"]
["SSP000022301","77.0105","Ets Gilles VANNIER - CTM",null,"En cours",null,null,"En cours","77118","CLAYE SOUILLY","SEINE-ET-MARNE","ILE-DE-FRANCE","Polygone",2.6817734,48.946236,"H1 - Mécanique, électrique, traitement de surface"]
["SSP000022401","77.0137","COOPER Dammarie-les-Lys",null,"Clôturée",null,null,"Clôturée","77152","DAMMARIE LES LYS","SEINE-ET-MARNE","ILE-DE-FRANCE","Polygone",2.6383555,48.529125,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000022501","77.0150","Yara FRANCE","Yara FRANCE","En cours",null,null,"En cours","77305","MONTEREAU FAULT YONNE","SEINE-ET-MARNE","ILE-DE-FRANCE","Polygone",2.977563,48.38586,"D36 - Fabrication des engrais"]
["SSP000022601","92.0054","RECUPERATION SERVICE GENNEVILLIERS - RSG CFF Recycling",null,"En cours",null,null,"En cours","92036","GENNEVILLIERS","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.3130047,48.92825,"K5 - Récupération, dépôts de ferrailles"]
["SSP000022701",null,"IDFA",null,"Clôturée",null,null,"Clôturée","92036","GENNEVILLIERS","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.29272,48.946102]
["SSP000022801",null,"Société JR Traitements de Surface des Métaux",null,"Clôturée",null,null,"Clôturée","92036","GENNEVILLIERS","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.3028915,48.917866]
["SSP000022901","92.0062","LUCAS AEROSPACE FMS",null,"En cours",null,null,"En cours","92004","ASNIERES SUR SEINE","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.2939937,48.918777,"H18 - Composants électroniques (fabrication de)"]
["SSP000023001",null,"Shell",null,"Clôturée",null,null,"Clôturée","93007","LE BLANC MESNIL","SEINE-SAINT-DENIS","ILE-DE-FRANCE","Polygone",2.4323883,48.940975]
["SSP000023201","92.0083","UNILEVER BESTFOOD FRANCE",null,"En cours",null,null,"En cours","92004","ASNIERES SUR SEINE","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.316842,48.91786,"B13 - Huiles et graisses animales ou végétales (industrie de)"]
["SSP000023701","77.0010","SOPALUNA - friche",null,"En cours",null,null,"En cours","77108","CHELLES","SEINE-ET-MARNE","ILE-DE-FRANCE","Polygone",2.611065,48.868717]
["SSP000023801","95.0030","ATOTECH",null,"En cours",null,null,"En cours","95572","SAINT OUEN L'AUMONE","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.139859,49.054054,"D3 - Chimie, phytosanitaire, pharmacie"]
["SSP000023901","92.0040","DELACHAUX",null,"En cours",null,null,"En cours","92036","GENNEVILLIERS","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.3156228,48.923996,"J3 - Métallurgie des métaux non ferreux, affinage"]
["SSP000024001","78.0102","Société SAS POLYFILMS",null,"En cours",null,null,"En cours","78362","MANTES LA VILLE","YVELINES","ILE-DE-FRANCE","Polygone",1.7244111,48.978756,"D72 - Transformation des matières plastiques"]
["SSP000024201","95.0064","Compagnie Générale des Insecticides",null,"En cours",null,null,"En cours","95572","SAINT OUEN L'AUMONE","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.1182203,49.05632,"K35 - Regroupement, reconditionnement de déchets"]
["SSP000024401","78.0029","AXALTA COATING SYSTEMS FRANCE (Ex DUPONT PERFORMANCE COATINGS FRANCE)",null,"En cours",null,null,"En cours","78362","MANTES LA VILLE","YVELINES","ILE-DE-FRANCE","Polygone",1.7219471,48.979786,"D42 - Fabrication de peintures"]
["SSP000024601",null,"Demyttenaere",null,"Clôturée",null,null,"Clôturée","93007","LE BLANC MESNIL","SEINE-SAINT-DENIS","ILE-DE-FRANCE","Polygone",2.4656472,48.93315]
["SSP000024701",null,"Shell",null,"Clôturée",null,null,"Clôturée","93064","ROSNY SOUS BOIS","SEINE-SAINT-DENIS","ILE-DE-FRANCE","Polygone",2.474284,48.884594]
["SSP000025001","78.0001","SOCIETE NOUVELLE FRADIN (S.N.F.)",null,"En cours",null,null,"En cours","78440","LES MUREAUX","YVELINES","ILE-DE-FRANCE","Polygone",1.8987463,48.988533,"K42 - Régénération de solvants"]
["SSP000025101",null,"Le Profil",null,"Clôturée",null,null,"Clôturée","78440","LES MUREAUX","YVELINES","ILE-DE-FRANCE","Polygone",1.8998061,48.98628]
["SSP000025301","95.0066","LABORATOIRE LUMINA",null,"En cours",null,null,"En cours","95051","BEAUCHAMP","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.1782537,49.014843,"H14 - Application de peinture"]
["SSP000025401","78.0036","EADS ASTRIUM SPACE TRANSPORTATION",null,"En cours",null,null,"En cours","78440","LES MUREAUX","YVELINES","ILE-DE-FRANCE","Polygone",1.9259876,48.999325,"H1 - Mécanique, électrique, traitement de surface"]
["SSP000025501","92.0048","Anciennement BP",null,"En cours",null,null,"En cours","92036","GENNEVILLIERS","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.3091862,48.923527]
["SSP000025601","92.0042","DISTRICHIMIE",null,"En cours",null,null,"En cours","92036","GENNEVILLIERS","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.296553,48.947372,"D - Chimie, parachimie, pétrole"]
["SSP000025701","93.0063","Johnson Diversey",null,"Clôturée",null,null,"Clôturée","93008","BOBIGNY","SEINE-SAINT-DENIS","ILE-DE-FRANCE","Polygone",2.44857,48.900356,"D62 - Fabrication de détergents"]
["SSP000025801","78.0060","SEAM Matexon",null,"En cours",null,null,"En cours","78440","LES MUREAUX","YVELINES","ILE-DE-FRANCE","Polygone",1.9215816,48.993088]
["SSP000025901","92.0058","ESPACE BONGARDE",null,"En cours",null,null,"En cours","92036","GENNEVILLIERS","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.3207152,48.925846,"H16 - Piles électriques et accumulateurs (fabrication de)"]
["SSP000026101","78.0061","MORELLEC",null,"En cours",null,null,"En cours","78440","LES MUREAUX","YVELINES","ILE-DE-FRANCE","Polygone",1.8958365,48.990532,"H13 - Traitement de surface"]
["SSP000026201","78.0052","CHARBONNIERE LES MUREAUX / Société Pétrolière d'Importation",null,"En cours",null,null,"En cours","78440","LES MUREAUX","YVELINES","ILE-DE-FRANCE","Polygone",1.9118865,48.990894]
["SSP000026301","93.0046","ELM Leblanc BOSCH",null,"En cours",null,null,"En cours","93008","BOBIGNY","SEINE-SAINT-DENIS","ILE-DE-FRANCE","Polygone",2.4298167,48.914215,"H - Mécanique, traitements des surfaces"]
["SSP000026401",null,"Total",null,"Clôturée",null,null,"Clôturée","78440","LES MUREAUX","YVELINES","ILE-DE-FRANCE","Polygone",1.912221,48.98052]
["SSP000026501",null,"BP",null,"Clôturée",null,null,"Clôturée","78440","LES MUREAUX","YVELINES","ILE-DE-FRANCE","Polygone",1.9194038,48.999397]
["SSP000026801",null,"SHELL station servive",null,"Clôturée",null,null,"Clôturée","77108","CHELLES","SEINE-ET-MARNE","ILE-DE-FRANCE","Polygone",2.5809505,48.869812]
["SSP000026901",null,"JAMES AUTO",null,"Clôturée",null,null,"Clôturée","77108","CHELLES","SEINE-ET-MARNE","ILE-DE-FRANCE","Polygone",2.6112404,48.90175]
["SSP000027001",null,"ICI VALENTINE",null,"Clôturée",null,null,"Clôturée","92036","GENNEVILLIERS","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.3102827,48.919807]
["SSP000027101",null,"CEREP (PARC DE SEINE)",null,"Clôturée",null,null,"Clôturée","92036","GENNEVILLIERS","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.3094459,48.925484]
["SSP000027201","95.0019","SILAR",null,"En cours",null,null,"En cours","95051","BEAUCHAMP","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.209866,49.004566]
["SSP000027301","93.0020","PARAMELT ex TISCO",null,"En cours",null,null,"En cours","93008","BOBIGNY","SEINE-SAINT-DENIS","ILE-DE-FRANCE","Polygone",2.45423,48.90137]
["SSP000027501","93.0021","AKZO NOBEL (ex TRIMETAL)",null,"En cours",null,null,"En cours","93001","AUBERVILLIERS","SEINE-SAINT-DENIS","ILE-DE-FRANCE","Polygone",2.3863947,48.910206,"D42 - Fabrication de peintures"]
["SSP000027701","94.0075","CALDEO",null,"En cours",null,null,"En cours","94075","VILLECRESNES","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.5373092,48.72782]
["SSP000027801","94.0073","AS24",null,"En cours",null,null,"En cours","94074","VALENTON","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.4429386,48.76227,"L23 - Détail de carburants"]
["SSP000027901","92.0055","THOMSON CSF",null,"En cours",null,null,"En cours","92036","GENNEVILLIERS","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.3080046,48.928947,"H18 - Composants électroniques (fabrication de)"]
["SSP000028001",null,"GDE (Guy Dauphin Environnement)",null,"Clôturée",null,null,"Clôturée","95051","BEAUCHAMP","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.1785743,49.017056]
["SSP000028101","92.0085","STATION TOTAL LANTERNIER",null,"En cours",null,null,"En cours","92036","GENNEVILLIERS","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.2858803,48.930637,"L23 - Détail de carburants"]
["SSP000028201","92.0051","TRAPIL T1 EST",null,"En cours",null,null,"En cours","92036","GENNEVILLIERS","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.2961361,48.945805,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000028601","93.0077","BP LA COURNEUVE",null,"En cours",null,null,"En cours","93027","LA COURNEUVE","SEINE-SAINT-DENIS","ILE-DE-FRANCE","Polygone",2.4174333,48.92661,"L23 - Détail de carburants"]
["SSP000028701","93.0029","MORGAN (ex TEINTURERIE INDUSTRIELLE)","Réhabilitation","En cours",null,null,"En cours","93027","LA COURNEUVE","SEINE-SAINT-DENIS","ILE-DE-FRANCE","Polygone",2.4101043,48.91935,"E13 - Blanchiment, teinture, impression"]
["SSP000028801","93.0036","EVER",null,"En cours",null,null,"En cours","93051","NOISY LE GRAND","SEINE-SAINT-DENIS","ILE-DE-FRANCE","Polygone",2.5714314,48.850517,"D4 - Encres, vernis, peintures, colles (fabrication de)"]
["SSP000028901","93.0035","VETURA ex SCHWEPPES",null,"En cours",null,null,"En cours","93055","PANTIN","SEINE-SAINT-DENIS","ILE-DE-FRANCE","Polygone",2.4039183,48.902,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000029001",null,"Société PARIS PETROLE DISTRIBUTION",null,"Clôturée",null,null,"Clôturée","91330","LARDY","ESSONNE","ILE-DE-FRANCE","Polygone",2.2632985,48.52205]
["SSP000029201","78.0049","Ancienne usine à gaz d'Andrésy",null,"En cours",null,null,"En cours","78015","ANDRESY","YVELINES","ILE-DE-FRANCE","Polygone",2.0710073,48.991245,"J1 - Cokéfaction, usines à gaz"]
["SSP000029401",null,"DELEK France",null,"Clôturée",null,null,"Clôturée","78015","ANDRESY","YVELINES","ILE-DE-FRANCE","Polygone",2.0657265,48.988907]
["SSP000029501","93.0009","CACI",null,"En cours",null,null,"En cours","93066","SAINT DENIS","SEINE-SAINT-DENIS","ILE-DE-FRANCE","Polygone",2.3495483,48.926155,"D - Chimie, parachimie, pétrole"]
["SSP000029701","78.0020","DRAKA COMTEQ",null,"En cours",null,null,"En cours","78172","CONFLANS SAINTE HONORINE","YVELINES","ILE-DE-FRANCE","Polygone",2.1038098,49.004066,"H18 - Composants électroniques (fabrication de)"]
["SSP000029801","78.0083","NYCO",null,"En cours",null,null,"En cours","78172","CONFLANS SAINTE HONORINE","YVELINES","ILE-DE-FRANCE","Polygone",2.1010063,48.998325]
["SSP000029901","78.0040","LTT",null,"En cours",null,null,"En cours","78172","CONFLANS SAINTE HONORINE","YVELINES","ILE-DE-FRANCE","Polygone",2.10339,48.999477]
["SSP000030001","78.0012","ANCIENNE STATION FLUVIALE SHELL",null,"En cours",null,null,"En cours","78172","CONFLANS SAINTE HONORINE","YVELINES","ILE-DE-FRANCE","Polygone",2.077392,48.986206,"L23 - Détail de carburants"]
["SSP000030101","78.0115","CSF",null,"En cours",null,null,"En cours","78172","CONFLANS SAINTE HONORINE","YVELINES","ILE-DE-FRANCE","Polygone",2.1182334,49.006344,"L23 - Détail de carburants"]
["SSP000030201","78.0085","SAINT GERMAIN PRESSING",null,"En cours",null,null,"En cours","78551","SAINT GERMAIN EN LAYE","YVELINES","ILE-DE-FRANCE","Polygone",2.0934827,48.895206,"E3 - Laveries, blanchisseries, pressing"]
["SSP000030301",null,"SCIC CLOREN ( ancien site PIOT et TIROUFLET)",null,"Clôturée",null,null,"Clôturée","91386","MENNECY","ESSONNE","ILE-DE-FRANCE","Polygone",2.4417264,48.56936]
["SSP000030401",null,"CALDEO",null,"Clôturée",null,null,"Clôturée","78551","SAINT GERMAIN EN LAYE","YVELINES","ILE-DE-FRANCE","Polygone",2.0718563,48.905148]
["SSP000030601",null,"Claas Tractor",null,"Clôturée",null,null,"Clôturée","95625","US","VAL-D'OISE","ILE-DE-FRANCE","Polygone",1.9702787,49.10288]
["SSP000030701",null,"Bionaz",null,"Clôturée",null,null,"Clôturée","93010","BONDY","SEINE-SAINT-DENIS","ILE-DE-FRANCE","Polygone",2.4789941,48.90633]
["SSP000030801","93.0033","ARDEA (ex ALCOOL PETROLE CHIMIE ex DOCK DES ALCOOLS)",null,"En cours",null,null,"En cours","93001","AUBERVILLIERS","SEINE-SAINT-DENIS","ILE-DE-FRANCE","Polygone",2.368168,48.918438,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000031001","93.0037","ex GRISET",null,"En cours",null,null,"En cours","93001","AUBERVILLIERS","SEINE-SAINT-DENIS","ILE-DE-FRANCE","Polygone",2.396909,48.912884,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000031101",null,"VALREN",null,"Clôturée",null,null,"Clôturée","92036","GENNEVILLIERS","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.2990725,48.947147]
["SSP000031301",null,"Ancienne décharge KAPPA",null,"Clôturée",null,null,"Clôturée","91386","MENNECY","ESSONNE","ILE-DE-FRANCE","Polygone",2.4218507,48.568295]
["SSP000031401","37.0011","Agence d'exploitation EDF/GDF",null,"En cours",null,null,"En cours","37261","TOURS","INDRE-ET-LOIRE","CENTRE-VAL DE LOIRE","Polygone",0.6731884,47.37838,"J1 - Cokéfaction, usines à gaz"]
["SSP000031501","37.0028","MARCADET Mobilier",null,"En cours",null,null,"En cours","37139","LUYNES","INDRE-ET-LOIRE","CENTRE-VAL DE LOIRE","Polygone",0.5445101,47.404396,"K - Déchets et traitements"]
["SSP000031601","37.0022","Liants Routiers de la Vallée de la Loire",null,"En cours",null,null,"En cours","37195","LA RICHE","INDRE-ET-LOIRE","CENTRE-VAL DE LOIRE","Polygone",0.66503793,47.38097,"G22 - Centrales d'enrobés"]
["SSP000031701","37.0004","S.A. DUSOLIER",null,"En cours",null,null,"En cours","37233","SAINT PIERRE DES CORPS","INDRE-ET-LOIRE","CENTRE-VAL DE LOIRE","Polygone",0.7431188,47.385403,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000031801","37.0009","T.S.A.",null,"En cours",null,null,"En cours","37195","LA RICHE","INDRE-ET-LOIRE","CENTRE-VAL DE LOIRE","Polygone",0.61513096,47.376972,"H1 - Mécanique, électrique, traitement de surface"]
["SSP000031901","37.0032","Imprimerie MAME",null,"En cours",null,null,"En cours","37261","TOURS","INDRE-ET-LOIRE","CENTRE-VAL DE LOIRE","Polygone",0.6688748,47.39307,"H2 - Imprimerie, presse-édition, photographie"]
["SSP000032001","37.0025","TOTAL",null,"En cours",null,null,"En cours","37261","TOURS","INDRE-ET-LOIRE","CENTRE-VAL DE LOIRE","Polygone",0.6952394,47.4205,"L23 - Détail de carburants"]
["SSP000032101","95.0010","GDF DFT RIF + GDF CDM Cergy + Institut Français de l'Energie",null,"En cours",null,null,"En cours","95607","TAVERNY","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.2162993,49.027485,"J1 - Cokéfaction, usines à gaz"]
["SSP000032201","41.0017","MAGNIEZ-Ronsard",null,"En cours",null,null,"En cours","41269","VENDOME","LOIR-ET-CHER","CENTRE-VAL DE LOIRE","Polygone",1.051087,47.79675,"H13 - Traitement de surface"]
["SSP000032301","41.0033","POLYROC",null,"En cours",null,null,"En cours","41269","VENDOME","LOIR-ET-CHER","CENTRE-VAL DE LOIRE","Polygone",1.0512397,47.801678,"D72 - Transformation des matières plastiques"]
["SSP000032401","41.0011","Agence d'exploitation et clientèle EDF/GDF",null,"En cours",null,null,"En cours","41269","VENDOME","LOIR-ET-CHER","CENTRE-VAL DE LOIRE","Polygone",1.0678685,47.79959,"J1 - Cokéfaction, usines à gaz"]
["SSP000032501","41.0020","Les Tanneries Solognotes",null,"En cours",null,null,"En cours","41269","VENDOME","LOIR-ET-CHER","CENTRE-VAL DE LOIRE","Polygone",1.0539478,47.79638,"E21 - Tannerie, mégisserie"]
["SSP000032601","41.0055","LORCET",null,"En cours",null,null,"En cours","41269","VENDOME","LOIR-ET-CHER","CENTRE-VAL DE LOIRE","Polygone",1.0541515,47.795162,"G15 - Industrie du verre"]
["SSP000032701","41.0049","HUSQVARNA Rte Nationale",null,"Clôturée",null,"2012-05-25","Clôturée","41047","LA CHAUSSEE SAINT VICTOR","LOIR-ET-CHER","CENTRE-VAL DE LOIRE","Polygone",1.3509583,47.605526,"H1 - Mécanique, électrique, traitement de surface"]
["SSP000032801","95.0037","Garage de la Piscine",null,"En cours",null,null,"En cours","95428","MONTMORENCY","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.31048,48.973602,"L21 - Vente et réparation automobile"]
["SSP000032901",null,"BP Fioul Services",null,"Clôturée",null,null,"Clôturée","91471","ORSAY","ESSONNE","ILE-DE-FRANCE","Polygone",2.186376,48.69809]
["SSP000033101",null,"Domaine de Corbeville",null,"Clôturée",null,null,"Clôturée","91471","ORSAY","ESSONNE","ILE-DE-FRANCE","Polygone",2.1866152,48.712643]
["SSP000033201",null,"Esso SAF",null,"Clôturée",null,null,"Clôturée","95424","MONTIGNY LES CORMEILLES","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.1958146,48.99417]
["SSP000033401","93.0040","Ancienne usine à gaz (EDF/GDF)",null,"En cours",null,null,"En cours","93049","NEUILLY PLAISANCE","SEINE-SAINT-DENIS","ILE-DE-FRANCE","Polygone",2.5175552,48.86078,"J1 - Cokéfaction, usines à gaz"]
["SSP000033501",null,"Société Minière Industrielle Franco-Brésilienne",null,"Clôturée",null,null,"Clôturée","92024","CLICHY","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.3141737,48.912807]
["SSP000033701","92.0056","LE NIGEN PHARMA",null,"En cours",null,null,"En cours","92036","GENNEVILLIERS","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.326086,48.923462,"D3 - Chimie, phytosanitaire, pharmacie"]
["SSP000033901","92.0092","TOTAL RAFFINAGE MARKETING (ex TOTAL SUPPLY MARKETING)",null,"En cours",null,null,"En cours","92024","CLICHY","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.3069372,48.898716,"L23 - Détail de carburants"]
["SSP000034101","93.0042","Euridep ex La Seigneurie",null,"En cours",null,null,"En cours","93008","BOBIGNY","SEINE-SAINT-DENIS","ILE-DE-FRANCE","Polygone",2.4375658,48.903862,"D42 - Fabrication de peintures"]
["SSP000034201","93.0047","Polidécor",null,"En cours",null,null,"En cours","93055","PANTIN","SEINE-SAINT-DENIS","ILE-DE-FRANCE","Polygone",2.4269145,48.89512]
["SSP000034401","93.0051","Jean-Louis",null,"En cours",null,null,"En cours","93055","PANTIN","SEINE-SAINT-DENIS","ILE-DE-FRANCE","Polygone",2.418008,48.89193,"H13 - Traitement de surface"]
["SSP000034501",null,"Tournier - Fischer",null,"Clôturée",null,null,"Clôturée","77108","CHELLES","SEINE-ET-MARNE","ILE-DE-FRANCE","Polygone",2.603037,48.877235]
["SSP000034901",null,"BP Jaurès",null,"Clôturée",null,null,"Clôturée","93055","PANTIN","SEINE-SAINT-DENIS","ILE-DE-FRANCE","Polygone",2.3971357,48.907925]
["SSP000035001","18.0005","Ancienne usine à gaz",null,"En cours",null,null,"En cours","18279","VIERZON","CHER","CENTRE-VAL DE LOIRE","Polygone",2.0646796,47.22205,"J1 - Cokéfaction, usines à gaz"]
["SSP000035101","18.0010","Usine FFDM-PNEUMAT",null,"En cours",null,null,"En cours","18033","BOURGES","CHER","CENTRE-VAL DE LOIRE","Polygone",2.3830397,47.083935,"H11 - Usinage"]
["SSP000035201","18.0011","Site GAUMET",null,"En cours",null,null,"En cours","18033","BOURGES","CHER","CENTRE-VAL DE LOIRE","Polygone",2.383364,47.083492,"B15 - Stockage de céréales"]
["SSP000035301","18.0013","Usine CEAC-FULMEN",null,"En cours",null,null,"En cours","18279","VIERZON","CHER","CENTRE-VAL DE LOIRE","Polygone",2.0958576,47.217056,"H16 - Piles électriques et accumulateurs (fabrication de)"]
["SSP000035401","18.0022","Gaz de France - Région Centre Ouest",null,"En cours",null,null,"En cours","18279","VIERZON","CHER","CENTRE-VAL DE LOIRE","Polygone",2.0785801,47.218098,"J1 - Cokéfaction, usines à gaz"]
["SSP000035501","18.0023","Site CASE",null,"En cours",null,null,"En cours","18279","VIERZON","CHER","CENTRE-VAL DE LOIRE","Polygone",2.0594788,47.22386,"H11 - Usinage"]
["SSP000035601","18.0030","Station service SHELL",null,"En cours",null,null,"En cours","18205","SAINT DOULCHARD","CHER","CENTRE-VAL DE LOIRE","Point",0.0,0.0]
["SSP000035701","18.0055","S.A. GIAT Industrie - Site Lahitolle",null,"En cours",null,null,"En cours","18033","BOURGES","CHER","CENTRE-VAL DE LOIRE","Polygone",2.4173887,47.079956,"H11 - Usinage"]
["SSP000035801","18.0058","BRABANT CHIMIE",null,"En cours",null,null,"En cours","18033","BOURGES","CHER","CENTRE-VAL DE LOIRE","Polygone",2.4407322,47.119354]
["SSP000035901","18.0060","Station service SASTUARS",null,"En cours",null,null,"En cours","18279","VIERZON","CHER","CENTRE-VAL DE LOIRE","Polygone",2.078105,47.23578,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000036001","37.0040","Schenker Joyau",null,"En cours",null,null,"En cours","37233","SAINT PIERRE DES CORPS","INDRE-ET-LOIRE","CENTRE-VAL DE LOIRE","Polygone",0.71653545,47.385624,"L22 - Transports"]
["SSP000036101","18.0002","Dépôt de boues de la ville de Vierzon",null,"En cours",null,null,"En cours","18279","VIERZON","CHER","CENTRE-VAL DE LOIRE","Polygone",2.0274413,47.23153,"K36 - Mise en décharge"]
["SSP000036201","18.0003","Déposante Jean Gesset",null,"En cours",null,null,"En cours","18279","VIERZON","CHER","CENTRE-VAL DE LOIRE","Polygone",2.0267737,47.23071,"K36 - Mise en décharge"]
["SSP000036301","18.0007","Déposante Patrick Gesset",null,"En cours",null,null,"En cours","18279","VIERZON","CHER","CENTRE-VAL DE LOIRE","Polygone",2.0292509,47.230198,"K36 - Mise en décharge"]
["SSP000036501","80.0085","Ets Germain Benoît - Benoît et Co",null,"En cours",null,null,"En cours","80021","AMIENS","SOMME","HAUTS-DE-FRANCE","Polygone",2.301184,49.900196,"E1 - Textile et habillement, teinture, impression"]
["SSP000036502","80.0094","Ets Germain Benoît - Benoît et Co",null,"En cours",null,null,"En cours","80021","AMIENS","SOMME","HAUTS-DE-FRANCE","Polygone",2.301184,49.900196,"E1 - Textile et habillement, teinture, impression"]
["SSP000036701","77.0022","SODAP","SODAP","En cours",null,null,"En cours","77309","MONTHYON","SEINE-ET-MARNE","ILE-DE-FRANCE","Polygone",2.8216884,49.013584]
["SSP000036801","80.0008","Ancien établissement LEGUICHARD",null,"En cours",null,null,"En cours","80021","AMIENS","SOMME","HAUTS-DE-FRANCE","Polygone",2.2856462,49.888706,"H13 - Traitement de surface"]
["SSP000036901",null,"AGRATI",null,"Clôturée",null,null,"Clôturée","80021","AMIENS","SOMME","HAUTS-DE-FRANCE","Polygone",2.3022866,49.870125]
["SSP000037001","80.0104","PRM Peintures",null,"En cours",null,null,"En cours","80021","AMIENS","SOMME","HAUTS-DE-FRANCE","Polygone",2.2594366,49.888016,"D4 - Encres, vernis, peintures, colles (fabrication de)"]
["SSP000037101","80.0101","SAREME",null,"En cours",null,null,"En cours","80021","AMIENS","SOMME","HAUTS-DE-FRANCE","Polygone",2.2810297,49.93053]
["SSP000037201","80.0041","Abélia Décors SA",null,"En cours",null,null,"En cours","80001","ABBEVILLE","SOMME","HAUTS-DE-FRANCE","Polygone",1.862731,50.114784,"D72 - Transformation des matières plastiques"]
["SSP000037301","80.0065","COMAP (Ancien site)",null,"En cours",null,null,"En cours","80001","ABBEVILLE","SOMME","HAUTS-DE-FRANCE","Polygone",1.8186328,50.109116,"H1 - Mécanique, électrique, traitement de surface"]
["SSP000037401","80.0038","Margot",null,"En cours",null,null,"En cours","80001","ABBEVILLE","SOMME","HAUTS-DE-FRANCE","Polygone",1.8270857,50.101307,"H13 - Traitement de surface"]
["SSP000037501","80.0040","Norminter Picardie (ex  : Friche Maillard)",null,"En cours",null,null,"En cours","80001","ABBEVILLE","SOMME","HAUTS-DE-FRANCE","Polygone",1.8040094,50.106647,"H - Mécanique, traitements des surfaces"]
["SSP000037601","80.0036","PIC INDUSTRIES PRODUCTION",null,"En cours",null,null,"En cours","80013","AIRAINES","SOMME","HAUTS-DE-FRANCE","Polygone",1.9458015,49.966873,"D4 - Encres, vernis, peintures, colles (fabrication de)"]
["SSP000037701","80.0016","ASM",null,"En cours",null,null,"En cours","80190","CHEPY","SOMME","HAUTS-DE-FRANCE","Polygone",1.6395208,50.06674]
["SSP000037801","80.0091","MEWA (ex EURONET)",null,"En cours",null,null,"En cours","80274","EPPEVILLE","SOMME","HAUTS-DE-FRANCE","Polygone",3.0415006,49.739098,"E3 - Laveries, blanchisseries, pressing"]
["SSP000037901","80.0110","TOTAL",null,"En cours",null,null,"En cours","80149","BUIGNY SAINT MACLOU","SOMME","HAUTS-DE-FRANCE","Polygone",1.8189489,50.152718]
["SSP000038001","80.0100","PETIT et Fils SARL",null,"En cours",null,null,"En cours","80296","L'ETOILE","SOMME","HAUTS-DE-FRANCE","Polygone",2.0253384,50.021618,"K - Déchets et traitements"]
["SSP000038101","80.0099","FFM (ex Filature Française de Mohair)",null,"En cours",null,null,"En cours","80620","PERONNE","SOMME","HAUTS-DE-FRANCE","Polygone",2.935929,49.91253,"E12 - Filtène, filature, tissage, tricotage"]
["SSP000038201","80.0081","GDLS",null,"En cours",null,null,"En cours","80827","WOINCOURT","SOMME","HAUTS-DE-FRANCE","Polygone",1.5355608,50.055347,"H13 - Traitement de surface"]
["SSP000038301","35.0025","ST Microelectronics",null,"En cours",null,null,"En cours","35238","RENNES","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.6654434,48.0876,"H18 - Composants électroniques (fabrication de)"]
["SSP000038401",null,"ANCIENNE FONDERIE DE SERVON-sur-VILAINE",null,"Clôturée",null,null,"Clôturée","35327","SERVON SUR VILAINE","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.4607787,48.11072]
["SSP000038501","35.0029","FAURECIA INDUSTRIES SA",null,"En cours",null,null,"En cours","35090","CREVIN","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.6635103,47.94142,"M1 - Industries diverses"]
["SSP000038601","35.0010","Agence EDF-GDF Services de Fougères (Ancienne UAG)",null,"En cours",null,null,"En cours","35115","FOUGERES","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.1900623,48.346474,"J1 - Cokéfaction, usines à gaz"]
["SSP000038701",null,"TEN CAT ENBI (ex CREATEC ROLLERS)",null,"Clôturée",null,null,"Clôturée","35324","LA SELLE EN LUITRE","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.1703207,48.330856]
["SSP000038801","35.0001","Ancienne mine de Pont-Péan",null,"En cours",null,null,"En cours","35363","PONT PEAN","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.7158256,48.01587,"F2 - Minerais métalliques (extraction de)"]
["SSP000038901","35.0012","Ancienne usine à gaz",null,"En cours",null,null,"En cours","35238","RENNES","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.7021092,48.105946,"J1 - Cokéfaction, usines à gaz"]
["SSP000039001","34.0043","Ancien pressing S.A.R.L ARCEAUX 17",null,"En cours",null,null,"En cours","34172","MONTPELLIER","HERAULT","OCCITANIE","Polygone",3.8649669,43.611404,"E3 - Laveries, blanchisseries, pressing"]
["SSP000039101","34.0021","Sud Fertilisants / CEDEST Engrais","","En cours",null,null,"En cours","34023","BALARUC LES BAINS","HERAULT","OCCITANIE","Polygone",3.701445,43.442207,"D36 - Fabrication des engrais"]
["SSP000039201","30.0015","Anciens services techniques d'EDF GDF",null,"En cours",null,null,"En cours","30202","PONT SAINT ESPRIT","GARD","OCCITANIE","Polygone",4.6463714,44.24774,null,null,null,"20.11Z - Fabrication de gaz industriels"]
["SSP000039301","94.0016","ETABLISSEMENTS  MOIA (COGEDIM)",null,"En cours",null,null,"En cours","94016","CACHAN","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.3337665,48.79318,"H13 - Traitement de surface"]
["SSP000039401",null,"VAL D'OISE AGRICOLE",null,"Clôturée",null,null,"Clôturée","95211","ENNERY","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.1018467,49.075836]
["SSP000039501",null,"Chemin de l'Arange",null,"Clôturée",null,null,"Clôturée","77139","COURTRY","SEINE-ET-MARNE","ILE-DE-FRANCE","Polygone",2.6091769,48.922054]
["SSP000039601","42.0005","DECHARGE EMCO",null,"En cours",null,null,"En cours","42094","FEURS","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.198584,45.753597]
["SSP000039701","42.0007","ZAC Îlot de Molières",null,"En cours",null,null,"En cours","42044","LE CHAMBON FEUGEROLLES","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.3194246,45.395016]
["SSP000039801","42.0009","TERRAIN PORCHER, BOIS DE LA PORTE",null,"En cours",null,null,"En cours","42166","PARIGNY","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.090657,45.986095,"K36 - Mise en décharge"]
["SSP000039901","42.0015","SACCA  FRANCE",null,"En cours",null,null,"En cours","42304","SURY LE COMTAL","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.2036676,45.532673,"H13 - Traitement de surface"]
["SSP000040001","42.0018","EURODEC (ex SMDO) - THERMOZ WAELES LOIRE",null,"En cours",null,null,"En cours","42044","LE CHAMBON FEUGEROLLES","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.304991,45.395523,"H11 - Usinage"]
["SSP000040101","42.0019","ISOCHROME",null,"En cours",null,null,"En cours","42302","SORBIERS","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.446627,45.47995,"H13 - Traitement de surface"]
["SSP000040201","42.0022","PUITS COUCHOUD - (La Mure)",null,"En cours",null,null,"En cours","42110","L'HORME","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.553963,45.495724]
["SSP000040301","42.0028","Etablissements MARTIN",null,"En cours",null,null,"En cours","42218","SAINT ETIENNE","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.3981285,45.41,"C12 - Produits en bois, ameublement (fabrication de)"]
["SSP000040401","42.0030","PAPETERIES NAVARRE DE ROANNE (P.N.R.)",null,"En cours",null,null,"En cours","42187","ROANNE","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.084533,46.043667,"C23 - Transformation de papiers et carton"]
["SSP000040501","42.0034","VITALE RECYCLAGE (ex SERDEX , ex ECODEC, ex ECOLEC, ex Bourgier)",null,"En cours",null,null,"En cours","42211","SAINT CYPRIEN","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.222367,45.542427]
["SSP000040601","42.0036","PRAT",null,"En cours",null,null,"En cours","42059","CHAZELLES SUR LYON","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.392063,45.640305]
["SSP000040701","42.0037","ATELIERS DU MAUPAS",null,"En cours",null,null,"En cours","42323","VEAUCHE","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.2902837,45.564995,"H13 - Traitement de surface"]
["SSP000040801","42.0038","BAYLE",null,"En cours",null,null,"En cours","42271","SAINT PAUL EN JAREZ","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.563633,45.49506,"K - Déchets et traitements"]
["SSP000040901","42.0041","parking RN 86",null,"En cours",null,null,"En cours","42056","CHAVANAY","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.7446795,45.434685]
["SSP000041001","42.0045","PORCHER",null,"En cours",null,null,"En cours","42071","LE COTEAU","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.0897045,46.022087]
["SSP000041101","42.0046","Ancienne Usine à Gaz",null,"En cours",null,null,"En cours","42094","FEURS","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.218303,45.74204,"J1 - Cokéfaction, usines à gaz"]
["SSP000041201","42.0047","Ancienne Usine à Gaz",null,"En cours",null,null,"En cours","42147","MONTBRISON","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.0723634,45.60569,"J1 - Cokéfaction, usines à gaz"]
["SSP000041301","42.0048","Ancienne Usine à Gaz",null,"En cours",null,null,"En cours","42187","ROANNE","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.074911,46.03195,"J1 - Cokéfaction, usines à gaz"]
["SSP000041401","42.0049","GDF Ancienne usine à gaz",null,"En cours",null,null,"En cours","42059","CHAZELLES SUR LYON","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.389718,45.641983,"J1 - Cokéfaction, usines à gaz"]
["SSP000041501","42.0050","Ancienne Usine à Gaz",null,"En cours",null,null,"En cours","42052","CHARLIEU","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.1640587,46.155827,"J1 - Cokéfaction, usines à gaz"]
["SSP000041601","42.0051","Ancienne Usine A Gaz",null,"En cours",null,null,"En cours","42186","RIVE DE GIER","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.6279087,45.53375,"J1 - Cokéfaction, usines à gaz"]
["SSP000041701","42.0052","Ancienne Usine à Gaz",null,"En cours",null,null,"En cours","42218","SAINT ETIENNE","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.3910937,45.46404,"J1 - Cokéfaction, usines à gaz"]
["SSP000041801","42.0055","Verrerie VDG",null,"En cours",null,null,"En cours","42186","RIVE DE GIER","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.605486,45.531048]
["SSP000041901","42.0061","SNAAM (ex MURE CENTRE)",null,"En cours",null,null,"En cours","42044","LE CHAMBON FEUGEROLLES","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.320392,45.396843,"H11 - Usinage"]
["SSP000042001","42.0063","SICAME",null,"En cours",null,null,"En cours","42044","LE CHAMBON FEUGEROLLES","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.321617,45.39746,"H1 - Mécanique, électrique, traitement de surface"]
["SSP000042101","42.0068","REMY BARRERE ENGRENAGES",null,"En cours",null,null,"En cours","42218","SAINT ETIENNE","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.3991804,45.450516]
["SSP000042201","42.0069","NITECH",null,"Clôturée",null,"2015-07-17","Clôturée","42207","SAINT CHAMOND","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.5135155,45.482365]
["SSP000042301","42.0070","ancienne chapellerie MORETTON",null,"En cours",null,null,"En cours","42059","CHAZELLES SUR LYON","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.3925014,45.641064,"E14 - Confection de vêtements, bonneterie"]
["SSP000042401","42.0073","UIOM et décharge d'ESTIVAREILLES",null,"En cours",null,null,"En cours","42091","ESTIVAREILLES","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.0419593,45.43184,"K2 - Traitement de déchets urbains"]
["SSP000042501","42.0081","SUPERVOX AUTOMOTIV (ex F2A)",null,"En cours",null,null,"En cours","42316","UNIEUX","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.255899,45.403168,"H14 - Application de peinture"]
["SSP000042601","42.0083","TEINTURERIES ET DEVELOPPEMENT D'IZIEUX",null,"En cours",null,null,"En cours","42207","SAINT CHAMOND","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.5034547,45.456875,"E1 - Textile et habillement, teinture, impression"]
["SSP000042701","42.0084","site industriel PEYRAVERNEY",null,"En cours",null,null,"En cours","42272","SAINT PIERRE DE BOEUF","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.7458377,45.38988]
["SSP000042801","42.0085","JEAN RIVIERE et SEER",null,"En cours",null,null,"En cours","42316","UNIEUX","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.2588696,45.398777,"H1 - Mécanique, électrique, traitement de surface"]
["SSP000042802","42.0089","JEAN RIVIERE et SEER",null,"En cours",null,null,"En cours","42316","UNIEUX","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.2588696,45.398777,"H1 - Mécanique, électrique, traitement de surface"]
["SSP000042901","42.0086","ECOMARCHE",null,"En cours",null,null,"En cours","42285","SAINT ROMAIN LE PUY","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.1218047,45.55474,"L23 - Détail de carburants"]
["SSP000043001","42.0087","SNF SAS",null,"En cours",null,null,"En cours","42218","SAINT ETIENNE","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.4187713,45.449432,"D32 - Chimie minérale inorganique autre"]
["SSP000043101","42.0095","Atelier Traitement de Surfaces",null,"Clôturée",null,"2015-09-25","Clôturée","42218","SAINT ETIENNE","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.380999,45.416946,"H13 - Traitement de surface"]
["SSP000043201","42.0096","Forges de la Becque",null,"En cours",null,null,"En cours","42211","SAINT CYPRIEN","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.223161,45.53945]
["SSP000043301","42.0097","FORGES DE LAVIEU",null,"En cours",null,null,"En cours","42207","SAINT CHAMOND","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.503773,45.475876,"J5 - Fonderie et travail des métaux"]
["SSP000043401","42.0098","Chapellerie FERRIER",null,"En cours",null,null,"En cours","42013","BELLEGARDE EN FOREZ","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.296861,45.644474,"E2 - Industrie des cuirs et peaux, tannerie"]
["SSP000043501","42.0101","MIDAC Décharge",null,"En cours",null,null,"En cours","42304","SURY LE COMTAL","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.189998,45.528442]
["SSP000043601","42.0103","TISSAFIL",null,"En cours",null,null,"En cours","42103","LA GRAND CROIX","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.5709295,45.50786,"E1 - Textile et habillement, teinture, impression"]
["SSP000043701","42.0105","PROPLAN ADHESIFS",null,"En cours",null,null,"En cours","42123","LORETTE","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.5732083,45.513573,"D72 - Transformation des matières plastiques"]
["SSP000043801","42.0106","CASINO SERVICE - 63 rue Montat",null,"En cours",null,null,"En cours","42218","SAINT ETIENNE","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.404497,45.441647,"M - Divers et services"]
["SSP000043901","42.0107","THYSSENKRUPP MAVILOR",null,"En cours",null,null,"En cours","42110","L'HORME","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.5546618,45.488922,"H - Mécanique, traitements des surfaces"]
["SSP000044001","42.0109","SOCIETE VASTI-DUMAS (ex DUMAS TITOULET)",null,"En cours",null,null,"En cours","42218","SAINT ETIENNE","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.4001684,45.441288,"H2 - Imprimerie, presse-édition, photographie"]
["SSP000044101","42.0112","AGIP FRANCAISE",null,"En cours",null,null,"En cours","42218","SAINT ETIENNE","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.382837,45.456345,"L23 - Détail de carburants"]
["SSP000044201","42.0119","Société PREVOST",null,"En cours",null,null,"En cours","42218","SAINT ETIENNE","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.381908,45.418423,"H13 - Traitement de surface"]
["SSP000044301","42.0121","Ets JEAN RIVIERE & CIE",null,"En cours",null,null,"En cours","42218","SAINT ETIENNE","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.3949776,45.41868,"H13 - Traitement de surface"]
["SSP000044401","42.0125","Société DUBOEUF",null,"Clôturée",null,"2011-09-23","Clôturée","42218","SAINT ETIENNE","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.390908,45.41712,"H - Mécanique, traitements des surfaces"]
["SSP000044501","42.0127","SOCIETE ECUYER-THOMAS",null,"En cours",null,null,"En cours","42059","CHAZELLES SUR LYON","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.390854,45.641747,"E - Textile, cuir et peaux"]
["SSP000044601","42.0128","ARTEXTILE SA",null,"En cours",null,null,"En cours","42187","ROANNE","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.062513,46.03489,"E13 - Blanchiment, teinture, impression"]
["SSP000044701","42.0131","RIMEF-Technico",null,"En cours",null,null,"En cours","42044","LE CHAMBON FEUGEROLLES","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.3234706,45.39351,"K52 - Dépôts de ferraille"]
["SSP000044801","42.0140","CMF (Charpentes et Menuiseries Foreziennes)",null,"En cours",null,null,"En cours","42248","SAINT JUST EN CHEVALET","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",3.8438733,45.907005,"C13 - Traitement du bois"]
["SSP000044901","42.0141","TEINTURERIE DU BERNAY",null,"En cours",null,null,"En cours","42218","SAINT ETIENNE","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.407576,45.412556,"E13 - Blanchiment, teinture, impression"]
["SSP000045001","42.0142","ACF (Atelier Crozet Fourneyron ex ATAMEC)",null,"En cours",null,null,"En cours","42218","SAINT ETIENNE","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.4033546,45.460224,"J5 - Fonderie et travail des métaux"]
["SSP000045101","42.0145","UNICUM",null,"En cours",null,null,"En cours","42218","SAINT ETIENNE","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.4004016,45.448883,"J5 - Fonderie et travail des métaux"]
["SSP000045201","42.0149","Sécurité 2000 (ex : VITALE)",null,"En cours",null,null,"En cours","42218","SAINT ETIENNE","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.39869,45.4542]
["SSP000045301","42.0158","SICTOM de Bussières",null,"En cours",null,null,"En cours","42029","BUSSIERES","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.275297,45.848286,"K31 - Incinération"]
["SSP000045401","42.0160","UIOM DE ST SAUVEUR EN RUE",null,"En cours",null,null,"En cours","42287","SAINT SAUVEUR EN RUE","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.5209103,45.275127,"K31 - Incinération"]
["SSP000045501","42.0163","STATION SERVICE TARDY",null,"En cours",null,null,"En cours","42329","LA VERSANNE","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.500935,45.320957]
["SSP000045601","42.0165","Etablissement COLOMB",null,"En cours",null,null,"En cours","42207","SAINT CHAMOND","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.510728,45.48384,"J22 - Production d'acier brut, aciéries"]
["SSP000045701","42.0170","PLM AUTO",null,"En cours",null,null,"En cours","42172","PLANFOY","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.4415445,45.377163,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000045801","42.0172","SACCA OUTILLAGE",null,"En cours",null,null,"En cours","42304","SURY LE COMTAL","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.1820574,45.532856,"J - Sidérurgie, métallurgie, coke"]
["SSP000045901","42.0174","TITOULET",null,"En cours",null,null,"En cours","42183","LA RICAMARIE","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.3720865,45.4101,"C23 - Transformation de papiers et carton"]
["SSP000046001","42.0175","SEG SAMRO (ex TROUILLET Semi Remorques)",null,"En cours",null,null,"En cours","42011","BALBIGNY","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.186423,45.821445,"H - Mécanique, traitements des surfaces"]
["SSP000046101","42.0178","RUHL",null,"En cours",null,null,"En cours","42186","RIVE DE GIER","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.6240606,45.525684,"J - Sidérurgie, métallurgie, coke"]
["SSP000046201","42.0182","Station service AVIA",null,"En cours",null,null,"En cours","42218","SAINT ETIENNE","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.3776846,45.466194,"L23 - Détail de carburants"]
["SSP000046301","42.0183","RONDARD ARCHIMBAUD",null,"Clôturée",null,null,"Clôturée","42276","SAINT PRIEST LA PRUGNE","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",3.7544243,45.95554,"L23 - Détail de carburants"]
["SSP000046401","42.0186","GARAGE DES TROIS BOULEVARDS",null,"En cours",null,null,"En cours","42187","ROANNE","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.0802474,46.044823,"L23 - Détail de carburants"]
["SSP000046501","42.0193","Manufacture de Ressorts de Terrenoire (MRT)",null,"En cours",null,null,"En cours","42218","SAINT ETIENNE","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.433772,45.432003,"J - Sidérurgie, métallurgie, coke"]
["SSP000046601","42.0194","MOTOROP BRM INDUSTRIES",null,"En cours",null,null,"En cours","42187","ROANNE","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.087134,46.053623,"H1 - Mécanique, électrique, traitement de surface"]
["SSP000046701","01.0003","Ancienne décharge d'Avrillat",null,"En cours",null,null,"En cours","01303","PONCIN","AIN","AUVERGNE-RHONE-ALPES","Polygone",5.429044,46.100018,"K36 - Mise en décharge"]
["SSP000046801","01.0005","SA CONVERT",null,"En cours",null,null,"En cours","01283","OYONNAX","AIN","AUVERGNE-RHONE-ALPES","Polygone",5.6568866,46.249317,"D34 - Fabrication de matières plastiques de base"]
["SSP000046901","01.0006","ANCIEN DEPOTOIR A VIDANGE DES ETABLISSEMENTS LEMOINE",null,"En cours",null,null,"En cours","01320","REPLONGES","AIN","AUVERGNE-RHONE-ALPES","Polygone",4.8719215,46.291584]
["SSP000047001","01.0026","Ancienne usine à gaz",null,"En cours",null,null,"En cours","01262","MONTLUEL","AIN","AUVERGNE-RHONE-ALPES","Polygone",5.0564294,45.84863,"J1 - Cokéfaction, usines à gaz"]
["SSP000047101","01.0027","Ancienne usine à gaz - Site de la vinaigrerie",null,"En cours",null,null,"En cours","01053","BOURG EN BRESSE","AIN","AUVERGNE-RHONE-ALPES","Polygone",5.224809,46.199566,"J1 - Cokéfaction, usines à gaz"]
["SSP000047102","01.0066","Ancienne usine à gaz - Site de la vinaigrerie",null,"En cours",null,null,"En cours","01053","BOURG EN BRESSE","AIN","AUVERGNE-RHONE-ALPES","Polygone",5.224809,46.199566,"J1 - Cokéfaction, usines à gaz"]
["SSP000047201","01.0050","GOYOT",null,"En cours",null,null,"En cours","01033","BELLEGARDE SUR VALSERINE","AIN","AUVERGNE-RHONE-ALPES","Polygone",5.8234363,46.1045,"H13 - Traitement de surface"]
["SSP000047301","01.0052","UIOM de GROISSIAT",null,"En cours",null,null,"En cours","01181","GROISSIAT","AIN","AUVERGNE-RHONE-ALPES","Polygone",5.6207294,46.233067,"K2 - Traitement de déchets urbains"]
["SSP000047401","01.0067","SATEM",null,"En cours",null,null,"En cours","01049","LA BOISSE","AIN","AUVERGNE-RHONE-ALPES","Polygone",5.0371284,45.84507,"L23 - Détail de carburants"]
["SSP000047501","01.0072","TOTAL",null,"En cours",null,null,"En cours","01118","CORBONOD","AIN","AUVERGNE-RHONE-ALPES","Polygone",5.831724,45.966045,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000047601","01.0075","Bernard Trucks Avenue des sports",null,"En cours",null,null,"En cours","01053","BOURG EN BRESSE","AIN","AUVERGNE-RHONE-ALPES","Polygone",5.235825,46.20889,"L21 - Vente et réparation automobile"]
["SSP000047701","01.0090","VERNICOLOR (ex CRIMACOLOR)",null,"En cours",null,null,"En cours","01283","OYONNAX","AIN","AUVERGNE-RHONE-ALPES","Polygone",5.657405,46.270077,"H14 - Application de peinture"]
["SSP000047801","01.0093","DDE de l'Ain",null,"En cours",null,null,"En cours","01053","BOURG EN BRESSE","AIN","AUVERGNE-RHONE-ALPES","Polygone",5.219624,46.19286,"G22 - Centrales d'enrobés"]
["SSP000047901","01.0102","SKW Bellegarde SAS",null,"En cours",null,null,"En cours","01033","BELLEGARDE SUR VALSERINE","AIN","AUVERGNE-RHONE-ALPES","Polygone",5.819406,46.10099,"J53 - Travail des métaux, chaudronnerie, poudres"]
["SSP000048001","01.0106","Gérard MASSE",null,"En cours",null,null,"En cours","01022","ARTEMARE","AIN","AUVERGNE-RHONE-ALPES","Polygone",5.6894865,45.87244]
["SSP000048101","01.0120","GUY NOEL PRODUCTION",null,"En cours",null,null,"En cours","01004","AMBERIEU EN BUGEY","AIN","AUVERGNE-RHONE-ALPES","Polygone",5.34523,45.964603,"J5 - Fonderie et travail des métaux"]
["SSP000048201","01.0121","CARROSSERIE INDUSTRIELLE DE L'AIN",null,"En cours",null,null,"En cours","01053","BOURG EN BRESSE","AIN","AUVERGNE-RHONE-ALPES","Polygone",5.2461505,46.185154,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000048301","07.0001","S.A. GAILLARD-RONDINO",null,"En cours",null,null,"En cours","07281","SAINT PERAY","ARDECHE","AUVERGNE-RHONE-ALPES","Polygone",4.850207,44.950745,"C13 - Traitement du bois"]
["SSP000048401",null,"Ancienne usine à gaz",null,"Clôturée",null,null,"Clôturée","07349","LA VOULTE SUR RHONE","ARDECHE","AUVERGNE-RHONE-ALPES","Polygone",4.778991,44.805214]
["SSP000048501","07.0011","Ancienne usine à gaz",null,"En cours",null,null,"En cours","07186","PRIVAS","ARDECHE","AUVERGNE-RHONE-ALPES","Polygone",4.601556,44.73327,"J1 - Cokéfaction, usines à gaz"]
["SSP000048601","07.0020","Fonderies TRIVINO",null,"En cours",null,null,"En cours","07349","LA VOULTE SUR RHONE","ARDECHE","AUVERGNE-RHONE-ALPES","Polygone",4.791417,44.806335]
["SSP000048701","07.0024","NEW MAILLE STOP",null,"En cours",null,null,"En cours","07265","SAINT MARCEL LES ANNONAY","ARDECHE","AUVERGNE-RHONE-ALPES","Polygone",4.6301684,45.28573]
["SSP000048801","26.0002","SOCIETE SARMA",null,"En cours",null,null,"En cours","26341","SERVES SUR RHONE","DROME","AUVERGNE-RHONE-ALPES","Polygone",4.8188567,45.13102,"H1 - Mécanique, électrique, traitement de surface"]
["SSP000048901","26.0005","PIERI CHIMIE",null,"En cours",null,null,"En cours","26252","PORTES LES VALENCE","DROME","AUVERGNE-RHONE-ALPES","Polygone",4.885808,44.88157,"D61 - Fabrication de produits savonniers"]
["SSP000049001","26.0020","Agence EDF GDF Services",null,"En cours",null,null,"En cours","26333","SAINT VALLIER","DROME","AUVERGNE-RHONE-ALPES","Polygone",4.8186264,45.17425,"J1 - Cokéfaction, usines à gaz"]
["SSP000049101","26.0032","LA CARTOUCHERIE",null,"En cours",null,null,"En cours","26058","BOURG LES VALENCE","DROME","AUVERGNE-RHONE-ALPES","Polygone",4.900371,44.942978,"D81 - Poudres et explosifs (fabrication de)"]
["SSP000049201","26.0040","LA CELLONITE",null,"En cours",null,null,"En cours","26281","ROMANS SUR ISERE","DROME","AUVERGNE-RHONE-ALPES","Polygone",5.040506,45.04558,"D4 - Encres, vernis, peintures, colles (fabrication de)"]
["SSP000049301","26.0042","SODIMAS (ex RENAU)",null,"En cours",null,null,"En cours","26250","PONT DE L'ISERE","DROME","AUVERGNE-RHONE-ALPES","Polygone",4.8718233,45.01263,"H13 - Traitement de surface"]
["SSP000049401","26.0044","CET de ROCHEGUDE - Centre d'Enfouissement Technique",null,"En cours",null,null,"En cours","26275","ROCHEGUDE","DROME","AUVERGNE-RHONE-ALPES","Polygone",4.833827,44.267006,"K22 - Regroupement d'OM, DIB"]
["SSP000049501","26.0050","THEVENIN DUCROT DISTRIBUTION VALENCE",null,"Clôturée",null,"2018-04-12","Clôturée","26362","VALENCE","DROME","AUVERGNE-RHONE-ALPES","Polygone",4.8847485,44.91168,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000049601","26.0058","Ancienne carrière GIRARD",null,"En cours",null,null,"En cours","26058","BOURG LES VALENCE","DROME","AUVERGNE-RHONE-ALPES","Polygone",4.8932796,44.960472,"F32 - Carrières"]
["SSP000049701","26.0061","CHAMPAGNE METAUX RHONE",null,"En cours",null,null,"En cours","26058","BOURG LES VALENCE","DROME","AUVERGNE-RHONE-ALPES","Polygone",4.9114857,44.949806,"K52 - Dépôts de ferraille"]
["SSP000049801","26.0062","CMRJ (ex René JOURDAN)",null,"En cours",null,null,"En cours","26362","VALENCE","DROME","AUVERGNE-RHONE-ALPES","Polygone",4.905068,44.926292,"H1 - Mécanique, électrique, traitement de surface"]
["SSP000049901","26.0069","CHATAIN René",null,"En cours",null,null,"En cours","26333","SAINT VALLIER","DROME","AUVERGNE-RHONE-ALPES","Polygone",4.813094,45.189426,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000050001","26.0072","Garage RUBIS",null,"En cours",null,null,"En cours","26113","DIE","DROME","AUVERGNE-RHONE-ALPES","Polygone",5.361472,44.759323,"L23 - Détail de carburants"]
["SSP000050101","26.0074","MONDI LEMBACEL SAS à Aouste-sur-Sye",null,"En cours",null,null,"En cours","26011","AOUSTE SUR SYE","DROME","AUVERGNE-RHONE-ALPES","Polygone",5.0600843,44.7164,"C22 - Fabrication de papiers et carton"]
["SSP000050201","26.0077","Garage USCLARD",null,"En cours",null,null,"En cours","26307","SAINT JEAN EN ROYANS","DROME","AUVERGNE-RHONE-ALPES","Polygone",5.2919393,45.0198,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000050301","26.0078","PNEU MAT X",null,"En cours",null,null,"En cours","26166","LORIOL SUR DROME","DROME","AUVERGNE-RHONE-ALPES","Polygone",4.8090725,44.729412]
["SSP000050401","26.0084","PAPETERIE EMIN LEYDIER",null,"En cours",null,null,"En cours","26160","LAVEYRON","DROME","AUVERGNE-RHONE-ALPES","Polygone",4.8316813,45.17765,"C22 - Fabrication de papiers et carton"]
["SSP000050501","38.0020","Mr MARRA Antoine",null,"En cours",null,null,"En cours","38075","CHAPAREILLAN","ISERE","AUVERGNE-RHONE-ALPES","Polygone",5.9829373,45.482887]
["SSP000050601","38.0047","MIVA",null,"En cours",null,null,"En cours","38372","SAINT BUEIL","ISERE","AUVERGNE-RHONE-ALPES","Polygone",5.6925435,45.477596,"E13 - Blanchiment, teinture, impression"]
["SSP000050701","38.0068","Ancienne usine à gaz de la Tour du Pin",null,"En cours",null,null,"En cours","38509","LA TOUR DU PIN","ISERE","AUVERGNE-RHONE-ALPES","Polygone",5.439842,45.567158,"J1 - Cokéfaction, usines à gaz"]
["SSP000050801","38.0070","Agence d'exploitation EDF GDF Services",null,"En cours",null,null,"En cours","38563","VOIRON","ISERE","AUVERGNE-RHONE-ALPES","Polygone",5.5952253,45.362686,"J1 - Cokéfaction, usines à gaz"]
["SSP000050901","38.0081","JACQUIER INDUSTRIES",null,"En cours",null,null,"En cours","38053","BOURGOIN JALLIEU","ISERE","AUVERGNE-RHONE-ALPES","Polygone",5.2577567,45.606182,"K52 - Dépôts de ferraille"]
["SSP000051001","38.0089","THOMSON",null,"En cours",null,null,"En cours","38382","SAINT EGREVE","ISERE","AUVERGNE-RHONE-ALPES","Polygone",5.6818995,45.24285]
["SSP000051101","38.0090","CHABROUD GALVA",null,"En cours",null,null,"En cours","38389","SAINT GEORGES D'ESPERANCHE","ISERE","AUVERGNE-RHONE-ALPES","Polygone",5.0858617,45.558228,"J53 - Travail des métaux, chaudronnerie, poudres"]
["SSP000051201","38.0098","KNAUF PACK SUD EST",null,"En cours",null,null,"En cours","38174","LA FRETTE","ISERE","AUVERGNE-RHONE-ALPES","Polygone",5.353728,45.391018,"D72 - Transformation des matières plastiques"]
["SSP000051301","38.0100","Rhone Alpes Fonte Industrie",null,"En cours",null,null,"En cours","38053","BOURGOIN JALLIEU","ISERE","AUVERGNE-RHONE-ALPES","Polygone",5.2728662,45.59167,"J51 - Fonderie des métaux ferreux"]
["SSP000051401","38.0104","Nouvelle Société BONMARTIN",null,"En cours",null,null,"En cours","38150","DOMENE","ISERE","AUVERGNE-RHONE-ALPES","Polygone",5.828815,45.199833,"J5 - Fonderie et travail des métaux"]
["SSP000051501","38.0106","M.I.P (Menuiserie Industrielle de Pontcharra)",null,"En cours",null,null,"En cours","38314","PONTCHARRA","ISERE","AUVERGNE-RHONE-ALPES","Polygone",6.0061355,45.428425]
["SSP000051601","38.0112","EUROMAG",null,"En cours",null,null,"En cours","38140","CROLLES","ISERE","AUVERGNE-RHONE-ALPES","Polygone",5.8850517,45.274143,"J53 - Travail des métaux, chaudronnerie, poudres"]
["SSP000051701","38.0124","Sté SOTEMO",null,"En cours",null,null,"En cours","38261","MORESTEL","ISERE","AUVERGNE-RHONE-ALPES","Polygone",5.4920926,45.67015,"E13 - Blanchiment, teinture, impression"]
["SSP000051801","38.0126","CHIMIDEROUIL",null,"En cours",null,null,"En cours","38087","CHASSE SUR RHONE","ISERE","AUVERGNE-RHONE-ALPES","Polygone",4.7948575,45.577473,"H13 - Traitement de surface"]
["SSP000051901","38.0133","FERRAZ SCHAWMUT",null,"En cours",null,null,"En cours","38537","LA VERPILLIERE","ISERE","AUVERGNE-RHONE-ALPES","Polygone",5.1517825,45.62627,"H - Mécanique, traitements des surfaces"]
["SSP000052001","38.0140","AUBERGE LE COURRAY JOSEPH DUBOIS SA",null,"En cours",null,null,"En cours","38139","CREYS MEPIEU","ISERE","AUVERGNE-RHONE-ALPES","Polygone",5.4820447,45.751358,"I - Energie"]
["SSP000052101","38.0144","RIPS",null,"En cours",null,null,"En cours","38048","BONNEFAMILLE","ISERE","AUVERGNE-RHONE-ALPES","Polygone",5.130854,45.601025,"K5 - Récupération, dépôts de ferrailles"]
["SSP000052201","38.0145","Sarl MARIS (Ex.  AGIP)",null,"En cours",null,null,"En cours","38185","GRENOBLE","ISERE","AUVERGNE-RHONE-ALPES","Polygone",5.7407947,45.18137,"L23 - Détail de carburants"]
["SSP000052301","38.0152","BILLION MAYOR",null,"En cours",null,null,"En cours","38182","LE GRAND LEMPS","ISERE","AUVERGNE-RHONE-ALPES","Polygone",5.4171147,45.399925,"E - Textile, cuir et peaux"]
["SSP000052401","38.0153","GALLIACOLOR",null,"En cours",null,null,"En cours","38197","JANNEYRIAS","ISERE","AUVERGNE-RHONE-ALPES","Polygone",5.103806,45.75725,"D42 - Fabrication de peintures"]
["SSP000052501","38.0158","Sté Papeterie des Deux Guiers",null,"En cours",null,null,"En cours","38155","ENTRE DEUX GUIERS","ISERE","AUVERGNE-RHONE-ALPES","Polygone",5.7403827,45.43451,"C22 - Fabrication de papiers et carton"]
["SSP000052601","38.0166","Papeteries de Pont de Claix",null,"En cours",null,null,"En cours","38317","LE PONT DE CLAIX","ISERE","AUVERGNE-RHONE-ALPES","Polygone",5.70272,45.11543,"C2 - Industrie du papier et du carton"]
["SSP000052701","38.0176","Papeteries de Voiron et Lancey - Site le Pruney",null,"En cours",null,null,"En cours","38538","LE VERSOUD","ISERE","AUVERGNE-RHONE-ALPES","Polygone",5.874071,45.22859,"C2 - Industrie du papier et du carton"]
["SSP000052801","38.0199","TWO CAST EUROPE",null,"En cours",null,null,"En cours","38553","VILLEFONTAINE","ISERE","AUVERGNE-RHONE-ALPES","Polygone",5.155936,45.62421,"J52 - Fonderie des métaux non ferreux"]
["SSP000052901","38.0201","Papeterie de Lancey",null,"En cours",null,null,"En cours","38547","VILLARD BONNOT","ISERE","AUVERGNE-RHONE-ALPES","Polygone",5.8851786,45.234528,"C2 - Industrie du papier et du carton"]
["SSP000053001","38.0207","Société CERIM - Bosonnet",null,"En cours",null,null,"En cours","38185","GRENOBLE","ISERE","AUVERGNE-RHONE-ALPES","Polygone",5.750326,45.179577,"H11 - Usinage"]
["SSP000053101","38.0214","ONDEO NALCO FRANCE",null,"En cours",null,null,"En cours","38140","CROLLES","ISERE","AUVERGNE-RHONE-ALPES","Polygone",5.886417,45.273933,"D3 - Chimie, phytosanitaire, pharmacie"]
["SSP000053201","38.0215","ISOBOX",null,"En cours",null,null,"En cours","38314","PONTCHARRA","ISERE","AUVERGNE-RHONE-ALPES","Polygone",6.0059633,45.42495,"D72 - Transformation des matières plastiques"]
["SSP000053301","38.0216","Papeterie du Moulin Vieux",null,"En cours",null,null,"En cours","38314","PONTCHARRA","ISERE","AUVERGNE-RHONE-ALPES","Polygone",6.0167985,45.427486,"C21 - Fabrication de pâte à papier"]
["SSP000053401","38.0218","Laminoirs d'Aluminium de Froges (LAF) (Ex-Pechiney Rhenalu)",null,"En cours",null,null,"En cours","38175","FROGES","ISERE","AUVERGNE-RHONE-ALPES","Polygone",5.91848,45.27005,"H13 - Traitement de surface"]
["SSP000053501","38.0221","HOLLIDAY Encre",null,"En cours",null,null,"En cours","38317","LE PONT DE CLAIX","ISERE","AUVERGNE-RHONE-ALPES","Polygone",5.696224,45.134125,"D41 - Fabrication d'encres"]
["SSP000053601","38.0224","FONCIERE DU DAUPHINE - GEODIS (Ex Castorama)",null,"En cours",null,null,"En cours","38185","GRENOBLE","ISERE","AUVERGNE-RHONE-ALPES","Polygone",5.7165565,45.159927]
["SSP000053701","38.0226","Avia",null,"En cours",null,null,"En cours","38185","GRENOBLE","ISERE","AUVERGNE-RHONE-ALPES","Polygone",5.7053075,45.185837,"L23 - Détail de carburants"]
["SSP000053801","38.0228","T2A -Teinturerie & Apprêts des Alpes",null,"En cours",null,null,"En cours","38185","GRENOBLE","ISERE","AUVERGNE-RHONE-ALPES","Polygone",5.7133837,45.183018,"E1 - Textile et habillement, teinture, impression"]
["SSP000053901","38.0231","EZT SARL  (Ex. OUTOKUMPU HEATCRAFT)",null,"En cours",null,null,"En cours","38138","CREMIEU","ISERE","AUVERGNE-RHONE-ALPES","Polygone",5.2412567,45.722515,"H - Mécanique, traitements des surfaces"]
["SSP000054001","38.0234","PHOENIX",null,"En cours",null,null,"En cours","38085","CHARVIEU CHAVAGNEUX","ISERE","AUVERGNE-RHONE-ALPES","Polygone",5.166172,45.75127,"D7 - Caoutchouc et matières plastiques"]
["SSP000054101","38.0235","SOCIETE NOUVELLE IMPRESSION SAINT JEAN",null,"En cours",null,null,"En cours","38223","MAUBEC","ISERE","AUVERGNE-RHONE-ALPES","Polygone",5.2743917,45.578823,"E1 - Textile et habillement, teinture, impression"]
["SSP000054201","38.0236","SOCIETE NIVON FRERES",null,"En cours",null,null,"En cours","38400","SAINT JEAN DE MOIRANS","ISERE","AUVERGNE-RHONE-ALPES","Polygone",5.5855174,45.348972,"L23 - Détail de carburants"]
["SSP000054301","38.0237","AGIP",null,"En cours",null,null,"En cours","38416","SAINT MARCELLIN","ISERE","AUVERGNE-RHONE-ALPES","Polygone",5.3188753,45.151928]
["SSP000054401","38.0238","TECSAS",null,"En cours",null,null,"En cours","38474","SASSENAGE","ISERE","AUVERGNE-RHONE-ALPES","Polygone",5.681558,45.20563,"H1 - Mécanique, électrique, traitement de surface"]
["SSP000054501","38.0243","MORA (Ex. SAPRA)",null,"En cours",null,null,"En cours","38490","SILLANS","ISERE","AUVERGNE-RHONE-ALPES","Polygone",5.3763566,45.338165,"D72 - Transformation des matières plastiques"]
["SSP000054601","38.0245","NS COMPO (Ex. ZAPOLY)",null,"Clôturée",null,"2012-03-12","Clôturée","38039","BERNIN","ISERE","AUVERGNE-RHONE-ALPES","Polygone",5.8746915,45.26918,"D72 - Transformation des matières plastiques"]
["SSP000054701","38.0246","GDE (Ex. GUILLET RECUP'MAT)",null,"En cours",null,null,"En cours","38540","VEUREY VOROIZE","ISERE","AUVERGNE-RHONE-ALPES","Polygone",5.621166,45.2559,"K5 - Récupération, dépôts de ferrailles"]
["SSP000054801","38.0251","LIDL (Ex. SUPER U / SOCIETE STEGEDIS)",null,"En cours",null,null,"En cours","38384","SAINT ETIENNE DE SAINT GEOIRS","ISERE","AUVERGNE-RHONE-ALPES","Polygone",5.3494124,45.341022,"L23 - Détail de carburants"]
["SSP000054901","38.0253","Station service  Relais des 7 Laux (Ex. TOTAL)",null,"En cours",null,null,"En cours","38547","VILLARD BONNOT","ISERE","AUVERGNE-RHONE-ALPES","Polygone",5.90416,45.260624,"L23 - Détail de carburants"]
["SSP000055001","38.0262","ALLIANCE TEXTILES - Friche",null,"En cours",null,null,"En cours","38562","VIZILLE","ISERE","AUVERGNE-RHONE-ALPES","Polygone",5.768096,45.08106,"E12 - Filtène, filature, tissage, tricotage"]
["SSP000055101","38.0263","TANNERIES DE VARCES",null,"En cours",null,null,"En cours","38524","VARCES ALLIERES ET RISSET","ISERE","AUVERGNE-RHONE-ALPES","Polygone",5.6830535,45.095745,"E21 - Tannerie, mégisserie"]
["SSP000055201","38.0129","ZAC Vigny Musset - Ilot U",null,"Clôturée",null,null,"Clôturée","38185","GRENOBLE","ISERE","AUVERGNE-RHONE-ALPES","Polygone",5.7278028,45.16524]
["SSP000055301","69.0001","LES ATELIERS DE BADAN (ex Gaz Liquide Industrie )",null,"Clôturée",null,null,"Clôturée","69096","GRIGNY","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.7890153,45.603664,"H15 - Assemblage, montage"]
["SSP000055401","69.0008","SITE REI",null,"En cours",null,null,"En cours","69123","LYON","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.8722906,45.758217,"H13 - Traitement de surface"]
["SSP000055501","69.0009","SITE GAZECHIM RHONE ALPES",null,"En cours",null,null,"En cours","69259","VENISSIEUX","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.8764715,45.71241]
["SSP000055601","69.0018","Décharge de Lissieu",null,"Clôturée",null,null,"Clôturée","69117","LISSIEU","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.736603,45.85948,"K36 - Mise en décharge"]
["SSP000055701","69.0044","CHIMICOLOR",null,"Clôturée",null,"2018-12-14","Clôturée","69123","LYON","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.8233156,45.72912,"H13 - Traitement de surface"]
["SSP000055801","69.0048","RENCAST DEVELOPPEMENT et VMT  (ex Fonderies DURANTON SICFOND )",null,"En cours",null,null,"En cours","69259","VENISSIEUX","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.879436,45.72116,"J52 - Fonderie des métaux non ferreux"]
["SSP000055901","69.0079","PCUK",null,"En cours",null,null,"En cours","69100","IRIGNY","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.8304176,45.692074,"D32 - Chimie minérale inorganique autre"]
["SSP000056001","69.0081","CELLIOSE",null,"Clôturée",null,null,"Clôturée","69152","PIERRE BENITE","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.8313265,45.704716,"D4 - Encres, vernis, peintures, colles (fabrication de)"]
["SSP000056101","69.0099","Fort de Genas",null,"En cours",null,null,"En cours","69277","GENAS","RHONE","AUVERGNE-RHONE-ALPES","Polygone",5.01375,45.730274,"J32 - Métallurgie de l'aluminium"]
["SSP000056201","69.0106","ARCHEMIS (ex RP-CRIT)",null,"En cours",null,null,"En cours","69275","DECINES CHARPIEU","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.9395375,45.76673,"D32 - Chimie minérale inorganique autre"]
["SSP000056301","69.0114","Ancienne usine à gaz de Lyon Perrache",null,"En cours",null,null,"En cours","69123","LYON","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.817039,45.74345]
["SSP000056401","69.0115","Agence d'exploitation de Lyon Vaise",null,"En cours",null,null,"En cours","69123","LYON","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.8003764,45.770626,"J1 - Cokéfaction, usines à gaz"]
["SSP000056501","69.0116","Agence d'exploitation EDF GDF Services",null,"En cours",null,null,"En cours","69266","VILLEURBANNE","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.896562,45.757412,"J1 - Cokéfaction, usines à gaz"]
["SSP000056601","69.0118","Agence d'exploitation et Plate-forme comptable EDF GDF Services",null,"Clôturée",null,"2016-05-19","Clôturée","69264","VILLEFRANCHE SUR SAONE","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.72346,45.990772,"J1 - Cokéfaction, usines à gaz"]
["SSP000056701","69.0119","Agences clientèle et d'exploitation EDF GDF Services",null,"Clôturée",null,null,"Clôturée","69091","GIVORS","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.7694087,45.584175,"J1 - Cokéfaction, usines à gaz"]
["SSP000056801","69.0120","Ancienne usine à gaz de Thizy",null,"Clôturée",null,"2018-04-06","Clôturée","69248","THIZY LES BOURGS","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.314776,46.03401,"J1 - Cokéfaction, usines à gaz"]
["SSP000056901","69.0123","RHODIACETA",null,"En cours",null,null,"En cours","69123","LYON","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.807048,45.769417,"E - Textile, cuir et peaux"]
["SSP000057001","69.0126","Kherachi Transports",null,"En cours",null,null,"En cours","69285","PUSIGNAN","RHONE","AUVERGNE-RHONE-ALPES","Polygone",5.0789995,45.76308,"L1 - Entreposage, manutention, commerces"]
["SSP000057101","69.0128","PINDALP   (ex-VIPAM)",null,"En cours",null,null,"En cours","69259","VENISSIEUX","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.8586397,45.715,"H14 - Application de peinture"]
["SSP000057201","69.0129","Société des Pétroles SHELL",null,"En cours",null,null,"En cours","69123","LYON","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.831981,45.717663,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000057301","69.0133","POINSONNET",null,"Clôturée",null,"2018-12-14","Clôturée","69266","VILLEURBANNE","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.8878727,45.78429,"K32 - Traitements physico-chimiques"]
["SSP000057401","69.0143","POL EQUIPEMENT",null,"En cours",null,null,"En cours","69091","GIVORS","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.7697144,45.583637,"H15 - Assemblage, montage"]
["SSP000057501","69.0145","TANNERIE RONZON",null,"En cours",null,null,"En cours","69238","SAINT SYMPHORIEN SUR COISE","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.455146,45.635017,"E21 - Tannerie, mégisserie"]
["SSP000057601","69.0148","PEGUERA",null,"En cours",null,null,"En cours","69275","DECINES CHARPIEU","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.9403024,45.756577,"K5 - Récupération, dépôts de ferrailles"]
["SSP000057701","69.0155","SOCIETE NOUVELLE DE LA BUIRE AUTOMOBILE",null,"Clôturée",null,"2019-01-07","Clôturée","69123","LYON","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.8561206,45.752865,"H1 - Mécanique, électrique, traitement de surface"]
["SSP000057801","69.0168","BRIDAY PNEUS",null,"En cours",null,null,"En cours","69123","LYON","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.8576355,45.764145,"L23 - Détail de carburants"]
["SSP000057901","69.0169","ZAC DE LA BUIRE",null,"Clôturée",null,"2019-01-07","Clôturée","69123","LYON","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.858257,45.752216,"H1 - Mécanique, électrique, traitement de surface"]
["SSP000058001","69.0172","SIRM",null,"En cours",null,null,"En cours","69123","LYON","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.840979,45.720688,"K5 - Récupération, dépôts de ferrailles"]
["SSP000058101","69.0173","ERTOL  (ex MERLE ex OXAL)",null,"En cours",null,null,"En cours","69204","SAINT GENIS LAVAL","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.7727804,45.711597,"H13 - Traitement de surface"]
["SSP000058201","69.0174","VULLIOD ANCEL",null,"Clôturée",null,"2017-08-21","Clôturée","69123","LYON","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.8703146,45.751026,"E13 - Blanchiment, teinture, impression"]
["SSP000058301","69.0186","BOYER",null,"Clôturée",null,"2018-02-16","Clôturée","69123","LYON","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.8335075,45.73879,"H11 - Usinage"]
["SSP000058401","69.0192","NERGUISIAN",null,"En cours",null,null,"En cours","69040","CHAMPAGNE AU MONT D'OR","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.780133,45.80412,"E1 - Textile et habillement, teinture, impression"]
["SSP000058501","69.0201","Société KODAK",null,"Clôturée",null,"2018-12-14","Clôturée","69096","GRIGNY","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.7727685,45.606358,"M1 - Industries diverses"]
["SSP000058601","69.0203","station service de l'aire de l'A47 - sens StEtienne-Lyon",null,"En cours",null,null,"En cours","69236","SAINT ROMAIN EN GIER","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.712426,45.57068,"L23 - Détail de carburants"]
["SSP000058701","69.0214","STATION SERVICE TOTAL FRANCE GERLAND",null,"Clôturée",null,null,"Clôturée","69123","LYON","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.823393,45.729565,"L23 - Détail de carburants"]
["SSP000058801","69.0217","Pôle de Loisirs et Culturelle de Lyon Confluence - SNC RANDOLI",null,"En cours",null,null,"En cours","69123","LYON","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.8172064,45.741158]
["SSP000058901","69.0218","TOTAL FRANCE - station-service cours Lafayette - Lyon 3",null,"En cours",null,null,"En cours","69383","LYON 3E ARRONDISSEMENT","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.861502,45.76327,"L23 - Détail de carburants"]
["SSP000059001","69.0222","ESPACE CHROME",null,"Clôturée",null,"2018-06-06","Clôturée","69266","VILLEURBANNE","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.8823566,45.774357,"H13 - Traitement de surface"]
["SSP000059101","69.0223","SCI Métral (ex SPEL qui a généré la pollution)",null,"En cours",null,null,"En cours","69266","VILLEURBANNE","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.870651,45.772648,"H13 - Traitement de surface"]
["SSP000059201","69.0224","Site BEAUCOURT",null,"En cours",null,null,"En cours","69271","CHASSIEU","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.9334955,45.74321,"K3 - Traitement de déchets industriels"]
["SSP000059301","69.0225","Société POURPRIX",null,"Clôturée",null,"2019-01-07","Clôturée","69123","LYON","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.841992,45.741665,"H13 - Traitement de surface"]
["SSP000059401","69.0231","E.T.V.S (Saint Priest)",null,"En cours",null,null,"En cours","69290","SAINT PRIEST","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.9139686,45.68884]
["SSP000059501","69.0234","GARAGE MARCEL",null,"Clôturée",null,"2018-12-14","Clôturée","69290","SAINT PRIEST","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.9329476,45.692665,"L23 - Détail de carburants"]
["SSP000059601","69.0236","METALEX",null,"En cours",null,null,"En cours","69290","SAINT PRIEST","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.9135747,45.68837]
["SSP000059701","69.0237","FRANCE TELECOM",null,"En cours",null,null,"En cours","69199","SAINT FONS","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.863507,45.712585,"M1 - Industries diverses"]
["SSP000059801","69.0241","BP France (station 40-42 rue Léon Blum)",null,"Clôturée",null,"2018-12-14","Clôturée","69266","VILLEURBANNE","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.894064,45.759357,"L23 - Détail de carburants"]
["SSP000059901","69.0245","EBENOID",null,"Clôturée",null,"2018-12-14","Clôturée","69266","VILLEURBANNE","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.895082,45.755157,"D72 - Transformation des matières plastiques"]
["SSP000060001","69.0247","OTC (office de Triage et de Conditionnement)",null,"Clôturée",null,"2017-10-27","Clôturée","69266","VILLEURBANNE","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.8942294,45.756798,"C23 - Transformation de papiers et carton"]
["SSP000060101","69.0249","CARREDA",null,"Clôturée",null,"2018-12-14","Clôturée","69266","VILLEURBANNE","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.8753676,45.762783,"H14 - Application de peinture"]
["SSP000060201","69.0253","ETAINS DE LYON (ex Dinanderie Lyonnaise Gros et Fils)",null,"Clôturée",null,"2018-02-16","Clôturée","69266","VILLEURBANNE","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.86961,45.770645,"J53 - Travail des métaux, chaudronnerie, poudres"]
["SSP000060301","69.0254","CIMOP",null,"Clôturée",null,"2018-02-16","Clôturée","69266","VILLEURBANNE","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.8935246,45.759224,"H11 - Usinage"]
["SSP000060401","69.0256","VOS LOGISTICS",null,"En cours",null,null,"En cours","69259","VENISSIEUX","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.8783317,45.70795,"L - Entreposage, transport, commerce"]
["SSP000060501","69.0257","CLARIANT SERVICES (FRANCE)",null,"Clôturée",null,"2017-04-21","Clôturée","69027","BRIGNAIS","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.768756,45.676403,"D - Chimie, parachimie, pétrole"]
["SSP000060601","69.0258","Les Fermetures Pontilles",null,"Clôturée",null,"2017-05-09","Clôturée","69123","LYON","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.8498683,45.74147,"H15 - Assemblage, montage"]
["SSP000060701","69.0259","SOCIETE DES MAGASINS GENERAUX",null,"En cours",null,null,"En cours","69123","LYON","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.8365335,45.737606,"J5 - Fonderie et travail des métaux"]
["SSP000060801","69.0260","Société MB",null,"Clôturée",null,"2018-02-16","Clôturée","69264","VILLEFRANCHE SUR SAONE","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.7298822,45.985912,"J53 - Travail des métaux, chaudronnerie, poudres"]
["SSP000060901","69.0262","SOCIETE DIETAL BELLEVILLE (Ex. THORN EUROPHANE)",null,"Clôturée",null,"2018-07-17","Clôturée","69019","BELLEVILLE","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.7303042,46.10681,"H15 - Assemblage, montage"]
["SSP000061001","69.0264","HOUGHTON",null,"En cours",null,null,"En cours","69264","VILLEFRANCHE SUR SAONE","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.737558,45.996273,"D33 - Pétrochimie carbochimie organique"]
["SSP000061101","69.0269","TOTAL FRANCE (A7) PIERRE-BENITE",null,"Clôturée",null,"2002-08-08","Clôturée","69152","PIERRE BENITE","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.8308287,45.708332,"D1 - Industrie pétrolière, gaz naturel"]
["SSP000061201","69.0272","THIVOLET",null,"En cours",null,null,"En cours","69123","LYON","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.8486714,45.741726,"J53 - Travail des métaux, chaudronnerie, poudres"]
["SSP000061301","69.0278","PARADES",null,"En cours",null,null,"En cours","69266","VILLEURBANNE","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.90749,45.760204,"C2 - Industrie du papier et du carton"]
["SSP000061401","69.0281","Ancienne usine textile",null,"Clôturée",null,null,"Clôturée","69143","NEUVILLE SUR SAONE","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.8303733,45.885387,"E - Textile, cuir et peaux"]
["SSP000061501","69.0290","Aeroport de Lyon-Bron (ex Kuwait Petroleum France)",null,"En cours",null,null,"En cours","69029","BRON","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.934949,45.73208]
["SSP000061601","69.0292","Centre Pénitenciaire de Corbas (ex Perrier TP)",null,"En cours",null,null,"En cours","69273","CORBAS","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.9312053,45.67919,"F32 - Carrières"]
["SSP000061701","69.0302","HOSPICES CIVILS DE LYON (ex BEAUFRERE)",null,"Clôturée",null,"2017-10-27","Clôturée","69123","LYON","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.7970676,45.77163,"H1 - Mécanique, électrique, traitement de surface"]
["SSP000061801","69.0303","TCM (ex Furukawa Loaders S.A.S)",null,"En cours",null,null,"En cours","69277","GENAS","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.9767456,45.71996,"D4 - Encres, vernis, peintures, colles (fabrication de)"]
["SSP000061901","69.0305","ESSO SAF Les Halles",null,"En cours",null,null,"En cours","69123","LYON","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.8512063,45.762333,"L23 - Détail de carburants"]
["SSP000062001","69.0313","Renolift (ex Schindler)",null,"Clôturée",null,null,"Clôturée","69282","MEYZIEU","RHONE","AUVERGNE-RHONE-ALPES","Polygone",5.0246744,45.769775,"J - Sidérurgie, métallurgie, coke"]
["SSP000062101","69.0320","Polyclinique des Minguettes",null,"En cours",null,null,"En cours","69259","VENISSIEUX","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.8695164,45.703526,"M3 - Santé"]
["SSP000062201","69.0330","AVISO-INTERMARCHE",null,"Clôturée",null,"2018-02-16","Clôturée","69123","LYON","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.801169,45.77676,"L23 - Détail de carburants"]
["SSP000062301","69.0331","DELTA MAINTENANCE SERVICES (DMS)",null,"En cours",null,null,"En cours","69275","DECINES CHARPIEU","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.9810495,45.769577,"H - Mécanique, traitements des surfaces"]
["SSP000062401","69.0333","LYON CONFLUENCE-SNCF Marchandises sud",null,"En cours",null,null,"En cours","69123","LYON","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.816908,45.740864]
["SSP000062501","69.0334","LYON CONFLUENCE-SNCF Marchandises nord",null,"En cours",null,null,"En cours","69123","LYON","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.818294,45.74333]
["SSP000062601","69.0335","LYON CONFLUENCE-SNCF Montrochet",null,"En cours",null,null,"En cours","69123","LYON","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.8154473,45.739986]
["SSP000062701","69.0351","Royal Services (ex Blanchisserie ODIN)",null,"En cours",null,null,"En cours","69028","BRINDAS","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.704653,45.717934,"E3 - Laveries, blanchisseries, pressing"]
["SSP000062801","69.0356","SSCV Galline Salengro",null,"En cours",null,null,"En cours","69266","VILLEURBANNE","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.8695083,45.775764,"H13 - Traitement de surface"]
["SSP000062901","69.0357","RENAULT Marius Berliet",null,"Clôturée",null,"2018-12-14","Clôturée","69123","LYON","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.860464,45.74076]
["SSP000063001","69.0360","VIDEOCOLOR",null,"Clôturée",null,"2018-02-16","Clôturée","69123","LYON","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.8693085,45.734215,"M1 - Industries diverses"]
["SSP000063101","69.0363","Papeterie du Val d'Ardières",null,"Clôturée",null,"2016-01-15","Clôturée","69012","LES ARDILLATS","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.5583997,46.16846]
["SSP000063201","69.0373","MARDUEL",null,"Clôturée",null,"2016-05-19","Clôturée","69264","VILLEFRANCHE SUR SAONE","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.7243423,45.989754,"E12 - Filtène, filature, tissage, tricotage"]
["SSP000063301","69.0038","DEPOT LES FILS CHARVET",null,"Clôturée",null,"2002-02-25","Clôturée","69025","BOURG-DE-THIZY","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.296902,46.03358,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000063401","73.0010","Décharge des Teppes",null,"En cours",null,null,"En cours","73119","FRENEY","SAVOIE","AUVERGNE-RHONE-ALPES","Polygone",6.6054764,45.199318,"K36 - Mise en décharge"]
["SSP000063501","73.0021","LAGUNES ZOLPAN SAVOIE",null,"En cours",null,null,"En cours","73058","LA BRIDOIRE","SAVOIE","AUVERGNE-RHONE-ALPES","Polygone",5.7309217,45.530895,"D42 - Fabrication de peintures"]
["SSP000063601","73.0035","RUBANOX",null,"En cours",null,null,"En cours","73065","CHAMBERY","SAVOIE","AUVERGNE-RHONE-ALPES","Polygone",5.908764,45.574635]
["SSP000063701","73.0038","Ancienne décharge La Contamine",null,"En cours",null,null,"En cours","73253","SAINT MARCEL","SAVOIE","AUVERGNE-RHONE-ALPES","Polygone",6.5567484,45.49379]
["SSP000063801","73.0042","PEM AR",null,"En cours",null,null,"En cours","73002","AIGUEBELLE","SAVOIE","AUVERGNE-RHONE-ALPES","Polygone",6.3103595,45.518448]
["SSP000063901","73.0046","Ancienne usine à gaz",null,"En cours",null,null,"En cours","73065","CHAMBERY","SAVOIE","AUVERGNE-RHONE-ALPES","Polygone",5.916236,45.574177,"J1 - Cokéfaction, usines à gaz"]
["SSP000064001","73.0051","PAPETERIES MATUSSIERE ET FOREST",null,"En cours",null,null,"En cours","73117","FOURNEAUX","SAVOIE","AUVERGNE-RHONE-ALPES","Polygone",6.6458507,45.191307,"C22 - Fabrication de papiers et carton"]
["SSP000064101","73.0053","Ancienne Usine à Gaz - La Calamine",null,"En cours",null,null,"En cours","73065","CHAMBERY","SAVOIE","AUVERGNE-RHONE-ALPES","Polygone",5.923291,45.56202,"J1 - Cokéfaction, usines à gaz"]
["SSP000064201","73.0066","EKA-CHIMIE Les Mollettes",null,"En cours",null,null,"En cours","73159","LES MOLLETTES","SAVOIE","AUVERGNE-RHONE-ALPES","Polygone",6.0483947,45.46275,"D44 - Fabrication de colles et mastics"]
["SSP000064301","73.0073","SICVEN France",null,"En cours",null,null,"En cours","73002","AIGUEBELLE","SAVOIE","AUVERGNE-RHONE-ALPES","Polygone",6.309562,45.521015]
["SSP000064401","73.0078","LA MURE BIANCO",null,"En cours",null,null,"En cours","73290","TERMIGNON","SAVOIE","AUVERGNE-RHONE-ALPES","Polygone",6.7719812,45.225853]
["SSP000064501","73.0090","Ancienne UIOM de Saint-Jean-de-Couz",null,"En cours",null,null,"En cours","73246","SAINT JEAN DE COUZ","SAVOIE","AUVERGNE-RHONE-ALPES","Polygone",5.808169,45.466084,"K31 - Incinération"]
["SSP000064601","73.0097","PINGUELY HAULOTTE",null,"En cours",null,null,"En cours","73031","BASSENS","SAVOIE","AUVERGNE-RHONE-ALPES","Polygone",5.9423776,45.57017]
["SSP000064701","73.0103","Dépôt de combustible ACTS",null,"En cours",null,null,"En cours","73032","LA BATHIE","SAVOIE","AUVERGNE-RHONE-ALPES","Polygone",6.4381967,45.643097,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000064801","73.0107","Ancienne station service AS24",null,"En cours",null,null,"En cours","73065","CHAMBERY","SAVOIE","AUVERGNE-RHONE-ALPES","Polygone",5.894509,45.598145]
["SSP000064901","73.0112","DECAPAGE METALBOI",null,"En cours",null,null,"En cours","73213","LA RAVOIRE","SAVOIE","AUVERGNE-RHONE-ALPES","Polygone",5.9685326,45.562263,"H13 - Traitement de surface"]
["SSP000065001","73.0114","ALBEA (ex CEBAL SAVOIE)",null,"En cours",null,null,"En cours","73011","ALBERTVILLE","SAVOIE","AUVERGNE-RHONE-ALPES","Polygone",6.3753557,45.662098,"D72 - Transformation des matières plastiques"]
["SSP000065101","73.0121","SPMI",null,"En cours",null,null,"En cours","73187","LA LECHERE","SAVOIE","AUVERGNE-RHONE-ALPES","Polygone",6.466419,45.543205]
["SSP000065201","73.0129","RETIA - Usine de PREMONT (ex. ARKEMA)",null,"En cours",null,null,"En cours","73194","ORELLE","SAVOIE","AUVERGNE-RHONE-ALPES","Polygone",6.529578,45.2082,"D3 - Chimie, phytosanitaire, pharmacie"]
["SSP000065301","73.0137","SITOM de Moûtiers - Décharge de Chalenson",null,"En cours",null,null,"En cours","73257","SAINT MARTIN DE BELLEVILLE","SAVOIE","AUVERGNE-RHONE-ALPES","Polygone",6.5121303,45.45073,"K21 - Décharges d'ordures ménagères"]
["SSP000065401","73.0143","Ancienne décharge LELY",null,"En cours",null,null,"En cours","73240","SAINTE HELENE DU LAC","SAVOIE","AUVERGNE-RHONE-ALPES","Polygone",6.0348606,45.471867,"K36 - Mise en décharge"]
["SSP000065501","74.0001","DECHARGE DE L'USINE PECHINEY ELECTROMETALLURGIE",null,"En cours",null,null,"En cours","74241","SAINT JEOIRE","HAUTE-SAVOIE","AUVERGNE-RHONE-ALPES","Polygone",6.4873347,46.12766,"J4 - Electrométallurgie"]
["SSP000065601","74.0008","EATON HYDRAULICS SAS (ex TUTHILL)",null,"En cours",null,null,"En cours","74305","VILLE LA GRAND","HAUTE-SAVOIE","AUVERGNE-RHONE-ALPES","Polygone",6.266288,46.199463,"J5 - Fonderie et travail des métaux"]
["SSP000065701","74.0020","Décharge communale de Faverges",null,"En cours",null,null,"En cours","74123","FAVERGES","HAUTE-SAVOIE","AUVERGNE-RHONE-ALPES","Polygone",6.280111,45.75622,"K21 - Décharges d'ordures ménagères"]
["SSP000065801","74.0025","DEPOT TOTAL (ex SARAM)",null,"En cours",null,null,"En cours","74243","SAINT JULIEN EN GENEVOIS","HAUTE-SAVOIE","AUVERGNE-RHONE-ALPES","Polygone",6.091484,46.14016,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000065901","74.0026","GDF - Ancienne usine à gaz d'Annemasse",null,"En cours",null,null,"En cours","74008","AMBILLY","HAUTE-SAVOIE","AUVERGNE-RHONE-ALPES","Polygone",6.2340126,46.19919,"J1 - Cokéfaction, usines à gaz"]
["SSP000066101","74.0036","PORTIGLIATI",null,"En cours",null,null,"En cours","74010","ANNECY","HAUTE-SAVOIE","AUVERGNE-RHONE-ALPES","Polygone",6.1141696,45.89569,"K52 - Dépôts de ferraille"]
["SSP000066201","74.0040","BASF Performance Products France (ex-CIBA SPECIALITY CHEMICALS MASTERBACH)",null,"En cours",null,null,"En cours","74164","MARIGNIER","HAUTE-SAVOIE","AUVERGNE-RHONE-ALPES","Polygone",6.5007987,46.113678,"D - Chimie, parachimie, pétrole"]
["SSP000066301","74.0044","ALPES COMPLEXE EMBALLAGES / COFRADEC",null,"En cours",null,null,"En cours","74031","BEAUMONT","HAUTE-SAVOIE","AUVERGNE-RHONE-ALPES","Polygone",6.0983043,46.09506,"H21 - Imprimerie, presse, édition"]
["SSP000066401","74.0047","Papeteries de Cran",null,"En cours",null,null,"En cours","74010","ANNECY","HAUTE-SAVOIE","AUVERGNE-RHONE-ALPES","Polygone",6.103122,45.90673,"C22 - Fabrication de papiers et carton"]
["SSP000066501","74.0049","COTTERLAZ-CARRAT",null,"En cours",null,null,"En cours","74208","PASSY","HAUTE-SAVOIE","AUVERGNE-RHONE-ALPES","Polygone",6.7259555,45.91931,"K52 - Dépôts de ferraille"]
["SSP000066601","74.0051","Ancien site PINDALP",null,"En cours",null,null,"En cours","74010","ANNECY","HAUTE-SAVOIE","AUVERGNE-RHONE-ALPES","Polygone",6.1158667,45.886574,"H14 - Application de peinture"]
["SSP000066701","74.0057","Ancienne station sevice Casino",null,"En cours",null,null,"En cours","74010","ANNECY","HAUTE-SAVOIE","AUVERGNE-RHONE-ALPES","Polygone",6.110692,45.907413,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000066801","74.0064","STATION SERVICE '' ELF LES HOUCHES SUD ''",null,"En cours",null,null,"En cours","74143","LES HOUCHES","HAUTE-SAVOIE","AUVERGNE-RHONE-ALPES","Polygone",6.810785,45.897594,"L23 - Détail de carburants"]
["SSP000066901","74.0065","LEMAN INDUSTRIE",null,"En cours",null,null,"En cours","74298","VETRAZ MONTHOUX","HAUTE-SAVOIE","AUVERGNE-RHONE-ALPES","Polygone",6.276597,46.185795,"H11 - Usinage"]
["SSP000067001","74.0066","SALOMON",null,"Clôturée",null,"2018-01-10","Clôturée","74225","RUMILLY","HAUTE-SAVOIE","AUVERGNE-RHONE-ALPES","Polygone",5.9601536,45.8379,"M1 - Industries diverses"]
["SSP000067101","74.0067","CUENOD",null,"Clôturée",null,"2018-01-10","Clôturée","74305","VILLE LA GRAND","HAUTE-SAVOIE","AUVERGNE-RHONE-ALPES","Polygone",6.271714,46.200077,"M1 - Industries diverses"]
["SSP000067201","74.0068","DECHARGE de Bons-en-Chablais",null,"En cours",null,null,"En cours","74043","BONS EN CHABLAIS","HAUTE-SAVOIE","AUVERGNE-RHONE-ALPES","Polygone",6.3832145,46.291077,"K21 - Décharges d'ordures ménagères"]
["SSP000067301","74.0070","DECHARGE de Nangy",null,"En cours",null,null,"En cours","74197","NANGY","HAUTE-SAVOIE","AUVERGNE-RHONE-ALPES","Polygone",6.2980976,46.14833,"K21 - Décharges d'ordures ménagères"]
["SSP000067401","74.0071","DECHARGE de Veigy-Foncenex",null,"En cours",null,null,"En cours","74293","VEIGY FONCENEX","HAUTE-SAVOIE","AUVERGNE-RHONE-ALPES","Polygone",6.26974,46.27894,"K21 - Décharges d'ordures ménagères"]
["SSP000067501","74.0072","DECHARGE de Vailly",null,"Clôturée",null,"2018-01-10","Clôturée","74287","VAILLY","HAUTE-SAVOIE","AUVERGNE-RHONE-ALPES","Polygone",6.5529046,46.284378,"K21 - Décharges d'ordures ménagères"]
["SSP000067601","74.0075","VAW INTERNATIONAL CAPSULES SAS",null,"En cours",null,null,"En cours","74096","CRUSEILLES","HAUTE-SAVOIE","AUVERGNE-RHONE-ALPES","Polygone",6.1088476,46.030315]
["SSP000067701","74.0076","DECHARGE de Reignier",null,"En cours",null,null,"En cours","74220","REIGNIER ESERY","HAUTE-SAVOIE","AUVERGNE-RHONE-ALPES","Polygone",6.2867565,46.121803,"K21 - Décharges d'ordures ménagères"]
["SSP000067801","74.0077","DECHARGE de Pers-Jussy",null,"En cours",null,null,"En cours","74211","PERS JUSSY","HAUTE-SAVOIE","AUVERGNE-RHONE-ALPES","Polygone",6.284681,46.112644,"K21 - Décharges d'ordures ménagères"]
["SSP000067901","74.0078","DECHARGE de Monnetier-Mornex",null,"En cours",null,null,"En cours","74185","MONNETIER MORNEX","HAUTE-SAVOIE","AUVERGNE-RHONE-ALPES","Polygone",6.231672,46.16001,"K21 - Décharges d'ordures ménagères"]
["SSP000068001","74.0079","DECHARGE de La Muraz",null,"En cours",null,null,"En cours","74193","LA MURAZ","HAUTE-SAVOIE","AUVERGNE-RHONE-ALPES","Polygone",6.205752,46.11859,"K21 - Décharges d'ordures ménagères"]
["SSP000068101","74.0081","DECHARGE de Bellevaux",null,"Clôturée",null,"2018-01-15","Clôturée","74032","BELLEVAUX","HAUTE-SAVOIE","AUVERGNE-RHONE-ALPES","Polygone",6.5153017,46.24041,"K21 - Décharges d'ordures ménagères"]
["SSP000068201","74.0082","SAVOIE CHROME DUR SERVICES",null,"En cours",null,null,"En cours","74305","VILLE LA GRAND","HAUTE-SAVOIE","AUVERGNE-RHONE-ALPES","Polygone",6.284286,46.206715,"H13 - Traitement de surface"]
["SSP000068301","74.0083","BRIFFAZ ALBERT",null,"En cours",null,null,"En cours","74169","MARNAZ","HAUTE-SAVOIE","AUVERGNE-RHONE-ALPES","Polygone",6.518208,46.070797,"H11 - Usinage"]
["SSP000068401","74.0084","DECHARGE de Vongy (SERTE)",null,"En cours",null,null,"En cours","74281","THONON LES BAINS","HAUTE-SAVOIE","AUVERGNE-RHONE-ALPES","Polygone",6.5089235,46.391415,"K21 - Décharges d'ordures ménagères"]
["SSP000068501","74.0085","LA MURE BIANCO ( SAMOËNS )",null,"Clôturée",null,"2018-01-15","Clôturée","74258","SAMOENS","HAUTE-SAVOIE","AUVERGNE-RHONE-ALPES","Polygone",6.720379,46.078945,"L23 - Détail de carburants"]
["SSP000068601","74.0086","DANC",null,"En cours",null,null,"En cours","74012","ANNEMASSE","HAUTE-SAVOIE","AUVERGNE-RHONE-ALPES","Polygone",6.2396445,46.182144,"H13 - Traitement de surface"]
["SSP000068701","74.0089","T2R",null,"En cours",null,null,"En cours","74278","THYEZ","HAUTE-SAVOIE","AUVERGNE-RHONE-ALPES","Polygone",6.5351086,46.07805,"H13 - Traitement de surface"]
["SSP000068801","74.0092","Garage du Mont Veyrier Strina et Fils",null,"En cours",null,null,"En cours","74010","ANNECY","HAUTE-SAVOIE","AUVERGNE-RHONE-ALPES","Polygone",6.1421957,45.91243,"L23 - Détail de carburants"]
["SSP000068901","74.0097","Pole Position",null,"En cours",null,null,"En cours","74123","FAVERGES","HAUTE-SAVOIE","AUVERGNE-RHONE-ALPES","Polygone",6.277209,45.752888,"L23 - Détail de carburants"]
["SSP000069001","74.0098","HILITE EBEA",null,"En cours",null,null,"En cours","74169","MARNAZ","HAUTE-SAVOIE","AUVERGNE-RHONE-ALPES","Polygone",6.5260463,46.062866,"H11 - Usinage"]
["SSP000069101","74.0106","Ancienne décharge de Lullin",null,"En cours",null,null,"En cours","74155","LULLIN","HAUTE-SAVOIE","AUVERGNE-RHONE-ALPES","Polygone",6.529119,46.288174,"K21 - Décharges d'ordures ménagères"]
["SSP000069201","74.0107","Décharge de Groisy",null,"En cours",null,null,"En cours","74137","GROISY","HAUTE-SAVOIE","AUVERGNE-RHONE-ALPES","Polygone",6.155971,46.012722,"K21 - Décharges d'ordures ménagères"]
["SSP000069301","74.0108","Ancienne décharge du Lyaud",null,"En cours",null,null,"En cours","74157","LYAUD","HAUTE-SAVOIE","AUVERGNE-RHONE-ALPES","Polygone",6.5114946,46.338852,"K21 - Décharges d'ordures ménagères"]
["SSP000069401","74.0109","Ancienne décharge du Parc de Calvi",null,"En cours",null,null,"En cours","74213","POISY","HAUTE-SAVOIE","AUVERGNE-RHONE-ALPES","Polygone",6.07168,45.93595,"K21 - Décharges d'ordures ménagères"]
["SSP000069501","74.0117","Ancienne usine Rencast",null,"En cours",null,null,"En cours","74105","DOUVAINE","HAUTE-SAVOIE","AUVERGNE-RHONE-ALPES","Polygone",6.306733,46.298157,"J52 - Fonderie des métaux non ferreux"]
["SSP000069601","24.0055","SAINT MARTIN DISTRIBUTION",null,"En cours",null,null,"En cours","24037","BERGERAC","DORDOGNE","NOUVELLE-AQUITAINE","Polygone",0.4821031,44.85828,"L23 - Détail de carburants"]
["SSP000069701",null,"Ancienne décharge et ancien stockage de déchets de marées noires du Spernot",null,"Clôturée",null,null,"Clôturée","29019","BREST","FINISTERE","BRETAGNE","Polygone",-4.5134525,48.413116]
["SSP000069801","34.0008","RAFFINERIE DU MIDI","Raffinerie du Midi","En cours",null,null,"En cours","34023","BALARUC LES BAINS","HERAULT","OCCITANIE","Polygone",3.692453,43.44604,"D12 - Raffinage de pétrole, carburants et lubrifiants"]
["SSP000069901","53.0031","SERGA et SOGI DISTRIBUTION",null,"En cours",null,null,"En cours","53147","MAYENNE","MAYENNE","PAYS DE LA LOIRE","Polygone",-0.61326545,48.297966,"L23 - Détail de carburants"]
["SSP000069902","53.0032","SERGA et SOGI DISTRIBUTION",null,"En cours",null,null,"En cours","53147","MAYENNE","MAYENNE","PAYS DE LA LOIRE","Polygone",-0.61326545,48.297966,"L23 - Détail de carburants"]
["SSP000070001","53.0014","SFR (Société Française de Revues)",null,"En cours",null,null,"En cours","53147","MAYENNE","MAYENNE","PAYS DE LA LOIRE","Polygone",-0.612214,48.29499]
["SSP000070101","11.0020","DDTM Le Parc",null,"En cours",null,null,"En cours","11069","CARCASSONNE","AUDE","OCCITANIE","Polygone",2.3314314,43.217045,"G2 - Chantiers, construction, bitumes, enrobés"]
["SSP000070301",null,"Ancienne décharge de Keréozen",null,"Clôturée",null,null,"Clôturée","29210","PLOUVORN","FINISTERE","BRETAGNE","Polygone",-4.041913,48.539055]
["SSP000070501","80.0094","C&V COSSERAT",null,"En cours",null,null,"En cours","80021","AMIENS","SOMME","HAUTS-DE-FRANCE","Polygone",2.2743,49.90907,"E1 - Textile et habillement, teinture, impression"]
["SSP000070601","80.0007","Ancien dépot BP",null,"En cours",null,null,"En cours","80131","BOVES","SOMME","HAUTS-DE-FRANCE","Polygone",2.3638182,49.867493]
["SSP000070701","35.0022","SNC LES BAUDIERES - MONIER",null,"En cours",null,null,"En cours","35238","RENNES","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.7322503,48.104744,"M1 - Industries diverses"]
["SSP000072201","22.0009","Etablissements JULOU",null,"Clôturée",null,"2017-01-30","Clôturée","22055","ETABLES SUR MER","COTES-D'ARMOR","BRETAGNE","Polygone",-2.8271701,48.605423,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000072301","22.0005","Etablissement Fichou",null,"En cours",null,null,"En cours","22025","CALLAC","COTES-D'ARMOR","BRETAGNE","Polygone",-3.4291592,48.407124,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000072401","29.0022","SOFERTI (DIOR)",null,"Clôturée",null,"2014-12-04","Clôturée","29103","LANDERNEAU","FINISTERE","BRETAGNE","Point",0.0,0.0,"D36 - Fabrication des engrais"]
["SSP000072501","29.0065","EASYDIS",null,"Clôturée",null,"2016-12-30","Clôturée","29105","LANDIVISIAU","FINISTERE","BRETAGNE","Polygone",-4.0838776,48.515312,"L - Entreposage, transport, commerce"]
["SSP000072601","29.0050","LE FUR (ESSO)",null,"Clôturée",null,"2019-01-07","Clôturée","29189","PLOUGASTEL DAOULAS","FINISTERE","BRETAGNE","Polygone",-4.3590794,48.38165,"L23 - Détail de carburants"]
["SSP000072701","29.0056","Ex VEZO Quimper",null,"En cours",null,null,"En cours","29232","QUIMPER","FINISTERE","BRETAGNE","Polygone",-4.067835,47.974415,"C13 - Traitement du bois"]
["SSP000072801","29.0020","Société SODIQA",null,"En cours",null,null,"En cours","29233","QUIMPERLE","FINISTERE","BRETAGNE","Polygone",-3.5572221,47.87133,"L21 - Vente et réparation automobile"]
["SSP000072901","29.0045","Bonduelle Traiteur International",null,"Clôturée",null,"2015-06-25","Clôturée","29241","ROSPORDEN","FINISTERE","BRETAGNE","Polygone",-3.8272803,47.952885,"B17 - Autres industries agro-alimentaires"]
["SSP000073001","29.0008","Station de déballastage (CCI  -  BREST )",null,"En cours",null,null,"En cours","29019","BREST","FINISTERE","BRETAGNE","Polygone",-4.445485,48.38825,"K3 - Traitement de déchets industriels"]
["SSP000073101","29.0052","GROUPE LE FLOCH",null,"En cours",null,null,"En cours","29049","ELLIANT","FINISTERE","BRETAGNE","Polygone",-3.8769279,47.96961,"K5 - Récupération, dépôts de ferrailles"]
["SSP000073201","29.0047","Ancienne décharge du Cam",null,"En cours",null,null,"En cours","29075","GUIPAVAS","FINISTERE","BRETAGNE","Polygone",-4.3996983,48.42784,"K21 - Décharges d'ordures ménagères"]
["SSP000073301","29.0006","Ancien dépôt de ferrailles JONCOUR",null,"Clôturée",null,"2014-12-01","Clôturée","29174","PLONEOUR LANVERN","FINISTERE","BRETAGNE","Polygone",-4.264317,47.902542,"K5 - Récupération, dépôts de ferrailles"]
["SSP000073401","29.0007","Dépôt de mâchefers de Ty Korm",null,"En cours",null,null,"En cours","29192","PLOUGOULM","FINISTERE","BRETAGNE","Polygone",-4.0473504,48.64435,"K31 - Incinération"]
["SSP000073501","29.0057","DOUX ALIMENTS DE CORNOUAILLE",null,"Clôturée",null,"2016-02-05","Clôturée","29216","PLUGUFFAN","FINISTERE","BRETAGNE","Polygone",-4.1727705,47.960896,"B3 - Fabrication d'aliments pour animaux"]
["SSP000073601","29.0005","JONCOUR",null,"Clôturée",null,"2014-12-01","Clôturée","29220","PONT L'ABBE","FINISTERE","BRETAGNE","Polygone",-4.227274,47.861446,"K5 - Récupération, dépôts de ferrailles"]
["SSP000073701","29.0066","COMBUSTIBLES DE L'OUEST",null,"En cours",null,null,"En cours","29254","SAINT MARTIN DES CHAMPS","FINISTERE","BRETAGNE","Polygone",-3.855397,48.56621,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000073801","56.0021","Société Laboratoire et Services KODAK",null,"En cours",null,null,"En cours","56036","CAUDAN","MORBIHAN","BRETAGNE","Polygone",-3.331292,47.783123,"H22 - Laboratoires photographiques"]
["SSP000073901","56.0014","Ex site ALAG",null,"Clôturée",null,"2015-01-09","Clôturée","56121","LORIENT","MORBIHAN","BRETAGNE","Polygone",-3.3597574,47.738983,"D36 - Fabrication des engrais"]
["SSP000074001","56.0020","KOLORIAN",null,"En cours",null,null,"En cours","56121","LORIENT","MORBIHAN","BRETAGNE","Polygone",-3.361302,47.733326,"D42 - Fabrication de peintures"]
["SSP000074101","56.0002","LYDALL FILTRATION/SEPARATION",null,"En cours",null,null,"En cours","56128","MELRAND","MORBIHAN","BRETAGNE","Polygone",-3.0660336,47.94878,"C2 - Industrie du papier et du carton"]
["SSP000074201","56.0001","ACIERIE API",null,"En cours",null,null,"En cours","56165","PLOERMEL","MORBIHAN","BRETAGNE","Polygone",-2.4058955,47.93602,"J5 - Fonderie et travail des métaux"]
["SSP000074801","59.0517","INTEREP (ex SOCATEX)",null,"En cours",null,null,"En cours","59247","FOREST SUR MARQUE","NORD","HAUTS-DE-FRANCE","Polygone",3.1876159,50.633427,"D71 - Industrie du caoutchouc"]
["SSP000075201","22.0004","Ancienne mine de Trémuson",null,"En cours",null,null,"En cours","22372","TREMUSON","COTES-D'ARMOR","BRETAGNE","Polygone",-2.8253455,48.530373,"F2 - Minerais métalliques (extraction de)"]
["SSP000075501",null,"Ancienne décharge de Linqueniac",null,"Clôturée",null,null,"Clôturée","35156","LONGAULNAY","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.9453872,48.299423]
["SSP000075801",null,"Ancienne décharge de Celar",null,"Clôturée",null,null,"Clôturée","35047","BRUZ","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.747018,47.991306]
["SSP000075901",null,"Ancienne décharge des Garennes",null,"Clôturée",null,null,"Clôturée","35047","BRUZ","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.751062,48.003235]
["SSP000076001",null,"Ancienne décharge de Pince-Poche",null,"Clôturée",null,null,"Clôturée","35051","CESSON SEVIGNE","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.6060385,48.111256]
["SSP000076201","35.0017","ZAC des Trois Marches",null,"Clôturée",null,"2016-12-12","Clôturée","35353","VEZIN LE COQUET","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.7383287,48.102287,"L13 - Entrepôts de produits dangereux"]
["SSP000076301",null,"Ancienne décharge des Rochers",null,"Clôturée",null,null,"Clôturée","35055","CHANTEPIE","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.5798645,48.08673]
["SSP000076501",null,"Ancienne décharge de la Sillandais",null,"Clôturée",null,null,"Clôturée","35076","CHAVAGNE","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.7906607,48.047592]
["SSP000076601",null,"Ancienne déharge de La Drille",null,"Clôturée",null,null,"Clôturée","35059","LA CHAPELLE DES FOUGERETZ","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.7471737,48.165424]
["SSP000076701",null,"PEUGEOT CITROEN AUTOMOBILES SA",null,"Clôturée",null,null,"Clôturée","35139","LAILLE","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.6895282,47.98531]
["SSP000076801",null,"Ancienne décharge de la Haute Porte",null,"Clôturée",null,null,"Clôturée","35139","LAILLE","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.7286658,47.998764]
["SSP000076901",null,"Ancienne décharge de Coutance",null,"Clôturée",null,null,"Clôturée","35240","LE RHEU","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.7553017,48.08483]
["SSP000077101",null,"Ancienne décharge controlée NETRA",null,"Clôturée",null,null,"Clôturée","35240","LE RHEU","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.7596127,48.10717]
["SSP000077201",null,"Ancienne décharge de La Hardinais",null,"Clôturée",null,null,"Clôturée","35351","LE VERGER","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.9425589,48.05379]
["SSP000077401",null,"Ancienne décharge des Marcades",null,"Clôturée",null,null,"Clôturée","35180","MINIAC SOUS BECHEREL","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.933309,48.29555]
["SSP000077801",null,"Ancienne décharge de la Petite Saudrais",null,"Clôturée",null,null,"Clôturée","35206","NOYAL CHATILLON SUR SEICHE","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.6551138,48.045727]
["SSP000077901",null,"Ancienne décharge du Pâtis du Coudray",null,"Clôturée",null,null,"Clôturée","35206","NOYAL CHATILLON SUR SEICHE","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.6596756,48.031418]
["SSP000078001",null,"Ancienne décharge de la Guibertière",null,"Clôturée",null,null,"Clôturée","35208","ORGERES","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.6648829,47.976784]
["SSP000078101",null,"Ancienne décharge du Bois de la Boulais",null,"Clôturée",null,null,"Clôturée","35208","ORGERES","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.6839772,47.989437]
["SSP000078601",null,"Ancienne décharge du Pont Hazard",null,"Clôturée",null,null,"Clôturée","35275","SAINT GILLES","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.8364152,48.15772]
["SSP000078701",null,"Ancienne décharge de Mille Club",null,"Clôturée",null,null,"Clôturée","35278","SAINT GREGOIRE","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.7115448,48.171272]
["SSP000079001",null,"Ancienne décharge du Poncel",null,"Clôturée",null,null,"Clôturée","35352","VERN SUR SEICHE","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.6059256,48.037704]
["SSP000079101",null,"Ancienne décharge du Lozeret",null,"Clôturée",null,null,"Clôturée","35353","VEZIN LE COQUET","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.7543464,48.1117]
["SSP000082201",null,"Ancienne décharge de la Grée de la Roche du Theil",null,"Clôturée",null,null,"Clôturée","35013","BAINS SUR OUST","ILLE-ET-VILAINE","BRETAGNE","Polygone",-2.0926366,47.67964]
["SSP000082301",null,"Ancienne décharge de la Ninochais",null,"Clôturée",null,null,"Clôturée","35013","BAINS SUR OUST","ILLE-ET-VILAINE","BRETAGNE","Polygone",-2.0753388,47.704132]
["SSP000082401",null,"Ancienne décharge de Tournebride",null,"Clôturée",null,null,"Clôturée","35013","BAINS SUR OUST","ILLE-ET-VILAINE","BRETAGNE","Polygone",-2.0666964,47.67976]
["SSP000082601",null,"Ancienne décharge du Binon",null,"Clôturée",null,null,"Clôturée","35013","BAINS SUR OUST","ILLE-ET-VILAINE","BRETAGNE","Polygone",-2.1051116,47.72966]
["SSP000082701",null,"Ancienne décharge de Bellevue",null,"Clôturée",null,null,"Clôturée","35045","BRUC SUR AFF","ILLE-ET-VILAINE","BRETAGNE","Polygone",-2.0132568,47.797638]
["SSP000083001",null,"Ancienne décharge de la Morinais",null,"Clôturée",null,null,"Clôturée","35145","LANGON","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.8757453,47.714348]
["SSP000083101",null,"Garage de l'Yvette",null,"Clôturée",null,null,"Clôturée","91272","GIF SUR YVETTE","ESSONNE","ILE-DE-FRANCE","Polygone",2.112874,48.704754]
["SSP000083201",null,"Ancienne décharge de la Croix Bouexic",null,"Clôturée",null,null,"Clôturée","35151","LIEURON","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.9331192,47.851604]
["SSP000083401",null,"Ancienne décharge de La Cordais",null,"Clôturée",null,null,"Clôturée","35219","PIPRIAC","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.9219426,47.823193]
["SSP000083501",null,"Ancienne décharge de la Marionnette",null,"Clôturée",null,null,"Clôturée","35236","REDON","ILLE-ET-VILAINE","BRETAGNE","Polygone",-2.0949078,47.67801]
["SSP000083601",null,"Ancienne décharge de la Praie",null,"Clôturée",null,null,"Clôturée","35237","RENAC","ILLE-ET-VILAINE","BRETAGNE","Polygone",-2.0164816,47.733543]
["SSP000083801",null,"Ancienne décharge de la Vionnais",null,"Clôturée",null,null,"Clôturée","35268","SAINT GANTON","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.8912559,47.786446]
["SSP000083901",null,"Ancienne décharge de Bénihel",null,"Clôturée",null,null,"Clôturée","35285","SAINT JUST","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.9973611,47.78401]
["SSP000084001",null,"Ancienne décharge des Essarts",null,"Clôturée",null,null,"Clôturée","35294","SAINTE MARIE","ILLE-ET-VILAINE","BRETAGNE","Polygone",-2.0351121,47.67325]
["SSP000084101",null,"Ancienne décharge de la Roche",null,"Clôturée",null,null,"Clôturée","35294","SAINTE MARIE","ILLE-ET-VILAINE","BRETAGNE","Polygone",-2.0048277,47.68431]
["SSP000084201",null,"Ancienne décharge de la Grotte",null,"Clôturée",null,null,"Clôturée","35328","SIXT SUR AFF","ILLE-ET-VILAINE","BRETAGNE","Polygone",-2.0742812,47.77332]
["SSP000084301",null,"Ancienne décharge de Linel",null,"Clôturée",null,null,"Clôturée","35328","SIXT SUR AFF","ILLE-ET-VILAINE","BRETAGNE","Polygone",-2.0457616,47.809013]
["SSP000084601",null,"Ancienne décharge de la Pellerie",null,"Clôturée",null,null,"Clôturée","35086","COMBOURTILLE","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.2635612,48.263847]
["SSP000084801",null,"Ancienne décharge de la Charpenterie",null,"Clôturée",null,null,"Clôturée","35112","FLEURIGNE","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.1259416,48.366257]
["SSP000084901",null,"Ancienne décharge de la zone industrielle",null,"Clôturée",null,null,"Clôturée","35115","FOUGERES","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.1908584,48.348183]
["SSP000085001",null,"Ancienne décharge de l'Aumaillerie",null,"Clôturée",null,null,"Clôturée","35021","BEAUCE","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.1728693,48.34094]
["SSP000085101",null,"Ancienne décharge de l'Artoire",null,"Clôturée",null,null,"Clôturée","35142","LANDEAN","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.1712347,48.415333]
["SSP000085501",null,"Ancienne décharge de la Boyère",null,"Clôturée",null,null,"Clôturée","35310","SAINT SAUVEUR DES LANDES","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.332963,48.345795]
["SSP000085801",null,"Ancienne décharge des Landiers des Herillets",null,"Clôturée",null,null,"Clôturée","35169","MAXENT","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.9977674,47.964153]
["SSP000086001",null,"Ancienne décharge de la butte du Vau",null,"Clôturée",null,null,"Clôturée","35211","PAIMPONT","ILLE-ET-VILAINE","BRETAGNE","Polygone",-2.1717763,48.015038]
["SSP000086201",null,"Ancienne décharge de Cannehils",null,"Clôturée",null,null,"Clôturée","35223","PLELAN LE GRAND","ILLE-ET-VILAINE","BRETAGNE","Polygone",-2.0740285,48.004795]
["SSP000086301",null,"Ancienne décharge de la Chenaie",null,"Clôturée",null,null,"Clôturée","35223","PLELAN LE GRAND","ILLE-ET-VILAINE","BRETAGNE","Polygone",-2.0729797,48.00099]
["SSP000086401","95.0033","USINE VULLI",null,"En cours",null,null,"En cours","95026","ASNIERES SUR OISE","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.3622794,49.13488,"D7 - Caoutchouc et matières plastiques"]
["SSP000086601",null,"Ancienne décharge de La Jaroussay",null,"Clôturée",null,null,"Clôturée","35305","SAINT PERAN","ILLE-ET-VILAINE","BRETAGNE","Polygone",-2.0583935,48.063015]
["SSP000086701",null,"Ancienne décharge de la Lande du Presbytère",null,"Clôturée",null,null,"Clôturée","35340","TREFFENDEL","ILLE-ET-VILAINE","BRETAGNE","Polygone",-2.0045328,48.041676]
["SSP000086801",null,"Ancienne décharge de la Lande du Foutez Loup",null,"Clôturée",null,null,"Clôturée","35340","TREFFENDEL","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.998867,48.044147]
["SSP000087001",null,"Ancienne décharge du Pré Henry",null,"Clôturée",null,null,"Clôturée","35056","LA CHAPELLE AUX FILTZMEENS","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.8259883,48.388317]
["SSP000087201",null,"Ancienne décharge du Pin",null,"Clôturée",null,null,"Clôturée","35222","PLEINE FOUGERES","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.5951905,48.539932]
["SSP000087401",null,"Ancienne décharge du Chesnay",null,"Clôturée",null,null,"Clôturée","35222","PLEINE FOUGERES","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.5857254,48.529278]
["SSP000087501",null,"Ancienne décharge du Vaux Vert",null,"Clôturée",null,null,"Clôturée","35247","ROZ SUR COUESNON","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.6053991,48.589714]
["SSP000087601",null,"Ancienne décharge de Saint Broladre",null,"Clôturée",null,null,"Clôturée","35248","SAINS","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.6045821,48.55259]
["SSP000087701",null,"Ancienne décharge du Bois Rouge",null,"Clôturée",null,null,"Clôturée","35259","SAINT BROLADRE","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.6509056,48.562572]
["SSP000087801",null,"Ancienne décharge du Pré",null,"Clôturée",null,null,"Clôturée","35291","SAINT MARCAN","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.622285,48.57497]
["SSP000088401",null,"Ancienne décharge du bourg",null,"Clôturée",null,null,"Clôturée","35007","AUBIGNE","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.6325501,48.295643]
["SSP000088801",null,"Ancienne décharge du Château Baguer",null,"Clôturée",null,null,"Clôturée","35009","BAGUER MORVAN","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.7794026,48.50083]
["SSP000088901",null,"Ancienne décharge de la Janaie",null,"Clôturée",null,null,"Clôturée","35010","BAGUER PICAN","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.7196654,48.554707]
["SSP000089101",null,"Ancienne décharge du Riffray",null,"Clôturée",null,null,"Clôturée","35012","BAIN DE BRETAGNE","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.6438166,47.82937]
["SSP000089501",null,"Ancienne décharge de Bélouze",null,"Clôturée",null,null,"Clôturée","35016","BAULON","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.9125859,47.974583]
["SSP000089901",null,"Ancienne décharge de la Croix de la Grée",null,"Clôturée",null,null,"Clôturée","35028","BOISTRUDAN","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.3899093,47.98396]
["SSP000090001",null,"Ancienne décharge des Maisons Neuves",null,"Clôturée",null,null,"Clôturée","35028","BOISTRUDAN","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.3753054,47.987816]
["SSP000090101",null,"Ancienne décharge de Saint Thomas",null,"Clôturée",null,null,"Clôturée","35033","BOURG DES COMPTES","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.73224,47.92665]
["SSP000090201",null,"Ancienne décharge de Hade",null,"Clôturée",null,null,"Clôturée","35035","BOVEL","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.9513124,47.934006]
["SSP000091301",null,"Ancienne décharge des Caves",null,"Clôturée",null,null,"Clôturée","35082","COESMES","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.4347409,47.879906]
["SSP000091401",null,"Ancienne décharge du Coudray",null,"Clôturée",null,null,"Clôturée","35084","COMBLESSAC","ILLE-ET-VILAINE","BRETAGNE","Polygone",-2.0904405,47.89983]
["SSP000092501",null,"Ancienne décharge de la Motte",null,"Clôturée",null,null,"Clôturée","35104","EPINIAC","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.6985804,48.50766]
["SSP000092801",null,"Ancienne décharge de la Fleuriais",null,"Clôturée",null,null,"Clôturée","35106","ERCE EN LAMEE","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.594579,47.80002]
["SSP000092901",null,"Ancienne décharge de Essé",null,"Clôturée",null,null,"Clôturée","35108","ESSE","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.4237506,47.957783]
["SSP000093301",null,"Ancienne décharge du Bois Martin",null,"Clôturée",null,null,"Clôturée","35123","GOVEN","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.8209684,48.01842]
["SSP000093401",null,"Ancienne décharge de la Lande de la Bigotière",null,"Clôturée",null,null,"Clôturée","35124","GRAND FOUGERAY","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.7410328,47.74434]
["SSP000093601",null,"Ancienne décharge de l'Hôtel Morel",null,"Clôturée",null,null,"Clôturée","35124","GRAND FOUGERAY","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.6795171,47.721382]
["SSP000093701",null,"Ancienne décharge de la Drouais",null,"Clôturée",null,null,"Clôturée","35126","GUICHEN","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.7986002,47.980152]
["SSP000093901",null,"Ancienne décharge de la Poterie",null,"Clôturée",null,null,"Clôturée","35128","GUIPEL","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.7412311,48.2992]
["SSP000094001",null,"Ancienne décharge de Trapusset",null,"Clôturée",null,null,"Clôturée","35129","GUIPRY","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.8518295,47.812756]
["SSP000094101",null,"Ancienne décharge du Hill",null,"Clôturée",null,null,"Clôturée","35129","GUIPRY","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.8340079,47.84421]
["SSP000094401",null,"Ancienne décharge du Placis Rogue",null,"Clôturée",null,null,"Clôturée","35017","LA BAUSSAINE","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.8900898,48.31277]
["SSP000094501",null,"Ancienne décharge des Chasses",null,"Clôturée",null,null,"Clôturée","35018","LA BAZOUGE DU DESERT","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.1446608,48.448196]
["SSP000094701",null,"Ancienne décharge de La Roche Pointue",null,"Clôturée",null,null,"Clôturée","35031","LA BOUEXIERE","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.4356977,48.1645]
["SSP000094801",null,"Ancienne décharge de la Giraudais",null,"Clôturée",null,null,"Clôturée","35031","LA BOUEXIERE","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.4223825,48.180824]
["SSP000094901",null,"Ancienne décharge de la Cordais",null,"Clôturée",null,null,"Clôturée","35098","LA DOMINELAIS","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.6638778,47.747623]
["SSP000095401",null,"Ancienne décharge de Bénéhard",null,"Clôturée",null,null,"Clôturée","35177","LA MEZIERE","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.7520609,48.215656]
["SSP000095501",null,"Ancienne décharge de la Benerais",null,"Clôturée",null,null,"Clôturée","35202","LA NOE BLANCHE","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.7409183,47.787605]
["SSP000095601",null,"Ancienne décharge de Servignac",null,"Clôturée",null,null,"Clôturée","35202","LA NOE BLANCHE","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.7320095,47.809547]
["SSP000096101",null,"Ancienne décharge de la Chauvinaie",null,"Clôturée",null,null,"Clôturée","35071","LE CHATELLIER","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.2480643,48.42743]
["SSP000096901",null,"Ancienne décharge du Chemin des moulins",null,"Clôturée",null,null,"Clôturée","35361","LE VIVIER SUR MER","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.789107,48.600166]
["SSP000097001",null,"Ancienne décharge du Rocher Morin",null,"Clôturée",null,null,"Clôturée","35154","LIVRE SUR CHANGEON","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.361903,48.22025]
["SSP000097301",null,"Ancienne décharge du Landier",null,"Clôturée",null,null,"Clôturée","35160","LOUTEHEL","ILLE-ET-VILAINE","BRETAGNE","Polygone",-2.0754004,47.938343,"K21 - Décharges d'ordures ménagères"]
["SSP000097401",null,"Ancienne décharge de la Ribaudière",null,"Clôturée",null,null,"Clôturée","35162","LOUVIGNE DU DESERT","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.1371821,48.506462]
["SSP000097801",null,"Ancienne décharge de la rue des Epines",null,"Clôturée",null,null,"Clôturée","35168","MAURE DE BRETAGNE","ILLE-ET-VILAINE","BRETAGNE","Polygone",-2.0007763,47.89167]
["SSP000097901",null,"Ancienne décharge de La Guesnaye",null,"Clôturée",null,null,"Clôturée","35171","MEDREAC","ILLE-ET-VILAINE","BRETAGNE","Polygone",-2.0482054,48.277725]
["SSP000098101",null,"Ancienne décharge de Tréguily",null,"Clôturée",null,null,"Clôturée","35176","MESSAC","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.8416579,47.811306]
["SSP000098201",null,"Ancienne décharge de Lannelou",null,"Clôturée",null,null,"Clôturée","35184","MONTAUBAN DE BRETAGNE","ILLE-ET-VILAINE","BRETAGNE","Polygone",-2.1061122,48.223038]
["SSP000098501",null,"Ancienne décharge des Landes de Bouttier",null,"Clôturée",null,null,"Clôturée","35226","PLEUGUENEUC","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.876519,48.413223]
["SSP000098601",null,"Ancienne décharge de L'ivenais",null,"Clôturée",null,null,"Clôturée","35228","PLEURTUIT","ILLE-ET-VILAINE","BRETAGNE","Polygone",-2.0740983,48.60444]
["SSP000098701",null,"Ancienne décharge de Sainte Croix",null,"Clôturée",null,null,"Clôturée","35239","RETIERS","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.3930349,47.892582]
["SSP000098801",null,"Ancienne décharge de la Fichepalais",null,"Clôturée",null,null,"Clôturée","35244","ROMAZY","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.5008682,48.368256]
["SSP000099401",null,"Ancienne décharge de Foulvandier",null,"Clôturée",null,null,"Clôturée","35289","SAINT MALO DE PHILY","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.7812281,47.866688]
["SSP000099501",null,"Ancienne décharge du Pont du Chat",null,"Clôturée",null,null,"Clôturée","35303","SAINT OUEN LA ROUERIE","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.433172,48.466125]
["SSP000099701",null,"Ancienne décharge de la Galivelais",null,"Clôturée",null,null,"Clôturée","35316","SAINT SULPICE DES LANDES","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.6293333,47.790108]
["SSP000099801",null,"Ancienne décharge des Landes d'Auvert",null,"Clôturée",null,null,"Clôturée","35249","SAINTE ANNE SUR VILAINE","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.8052117,47.7281]
["SSP000099901",null,"Ancienne décharge du Bois Gerouin",null,"Clôturée",null,null,"Clôturée","35354","VIEUX VIEL","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.5369693,48.513744]
["SSP000100201",null,"Ancienne décharge de la Picardière",null,"Clôturée",null,null,"Clôturée","35335","THOURIE","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.4489383,47.836296]
["SSP000100301",null,"Ancienne décharge de Roussette",null,"Clôturée",null,null,"Clôturée","35341","TREMBLAY","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.4849199,48.42449]
["SSP000100501",null,"Ancienne décharge de la Rose des Vents",null,"Clôturée",null,null,"Clôturée","35191","MONTOURS","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.2982733,48.439247]
["SSP000100601",null,"Ancienne décharge du Tertre d'Uzel",null,"Clôturée",null,null,"Clôturée","35221","PLECHATEL","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.771727,47.885677]
["SSP000100901",null,"Ancienne décharge de l'Epinay",null,"Clôturée",null,null,"Clôturée","35273","SAINT GERMAIN EN COGLES","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.2837726,48.410355]
["SSP000101001",null,"Ancienne décharge du Grand Chevrigé",null,"Clôturée",null,null,"Clôturée","35280","SAINT HILAIRE DES LANDES","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.3440795,48.331455]
["SSP000101201",null,"Ancienne décharge de la Ville Morin",null,"Clôturée",null,null,"Clôturée","35307","SAINT PERN","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.9961953,48.293877]
["SSP000101401",null,"Ancienne décharge des Rochers",null,"Clôturée",null,null,"Clôturée","56006","AUGAN","MORBIHAN","BRETAGNE","Polygone",-2.2402701,47.916595]
["SSP000101501",null,"Ancienne décharge de Kerguénolé",null,"Clôturée",null,null,"Clôturée","56152","LE PALAIS","MORBIHAN","BRETAGNE","Polygone",-3.1588812,47.326115]
["SSP000101601",null,"Ancienne décharge du Crann",null,"Clôturée",null,null,"Clôturée","56010","BAUD","MORBIHAN","BRETAGNE","Polygone",-3.042855,47.88976]
["SSP000101701",null,"Ancienne décharge de Kervéno",null,"Clôturée",null,null,"Clôturée","56021","BRANDERION","MORBIHAN","BRETAGNE","Polygone",-3.184608,47.791443]
["SSP000101801",null,"Ancienne décharge de Saint Isidore",null,"Clôturée",null,null,"Clôturée","56024","BREHAN","MORBIHAN","BRETAGNE","Polygone",-2.6697237,48.096634]
["SSP000101901",null,"Ancienne décharge de la Ville Agno",null,"Clôturée",null,null,"Clôturée","56024","BREHAN","MORBIHAN","BRETAGNE","Polygone",-2.6718102,48.031918]
["SSP000102001",null,"Ancienne décharge de Saint Trémeur",null,"Clôturée",null,null,"Clôturée","56026","BUBRY","MORBIHAN","BRETAGNE","Polygone",-3.1525366,47.966187]
["SSP000102301",null,"Ancienne décharge de Montauban",null,"Clôturée",null,null,"Clôturée","56034","CARNAC","MORBIHAN","BRETAGNE","Polygone",-3.0559676,47.591896]
["SSP000102401",null,"Ancienne décharge du Grand Village",null,"Clôturée",null,null,"Clôturée","56035","CARO","MORBIHAN","BRETAGNE","Polygone",-2.3382022,47.858303]
["SSP000102501",null,"Ancienne décharge de la Villeneuve",null,"Clôturée",null,null,"Clôturée","56042","COLPO","MORBIHAN","BRETAGNE","Polygone",-2.810644,47.833828]
["SSP000102601",null,"Ancienne décharge du bois du doyen",null,"Clôturée",null,null,"Clôturée","56044","COURNON","MORBIHAN","BRETAGNE","Polygone",-2.075184,47.74358]
["SSP000102701",null,"Ancienne décharge du Runio",null,"Clôturée",null,null,"Clôturée","56047","CREDIN","MORBIHAN","BRETAGNE","Polygone",-2.7795248,48.0395]
["SSP000102801",null,"Ancienne décharge de Kerléger",null,"Clôturée",null,null,"Clôturée","56053","ELVEN","MORBIHAN","BRETAGNE","Polygone",-2.621823,47.75807]
["SSP000103201",null,"Ancienne décharge de Roch  Ar Vran",null,"Clôturée",null,null,"Clôturée","56066","GOURIN","MORBIHAN","BRETAGNE","Polygone",-3.589116,48.168133]
["SSP000103301",null,"Ancienne décharge de Kerbus",null,"Clôturée",null,null,"Clôturée","56069","GROIX","MORBIHAN","BRETAGNE","Polygone",-3.4736323,47.637207]
["SSP000103601",null,"Ancienne décharge de Pichery",null,"Clôturée",null,null,"Clôturée","56074","GUENIN","MORBIHAN","BRETAGNE","Polygone",-2.9710116,47.90928]
["SSP000103801",null,"Ancienne décharge de Saint-Yves",null,"Clôturée",null,null,"Clôturée","56076","GUERN","MORBIHAN","BRETAGNE","Polygone",-3.1022687,48.035805]
["SSP000103901",null,"Ancienne décharge de Penguily",null,"Clôturée",null,null,"Clôturée","56081","GUISCRIFF","MORBIHAN","BRETAGNE","Polygone",-3.565442,48.048607]
["SSP000104101",null,"Ancienne décharge de Hoëdic",null,"Clôturée",null,null,"Clôturée","56085","HOEDIC","MORBIHAN","BRETAGNE","Polygone",-2.8685157,47.34106]
["SSP000104201",null,"Ancienne décharge de Portz Plouz",null,"Clôturée",null,null,"Clôturée","56086","ILE D'HOUAT","MORBIHAN","BRETAGNE","Polygone",-2.975015,47.38976]
["SSP000104301",null,"Ancienne décharge de Hervéno",null,"Clôturée",null,null,"Clôturée","56089","INGUINIEL","MORBIHAN","BRETAGNE","Polygone",-3.2901168,47.993202]
["SSP000104401",null,"Ancienne décharge de Peroz",null,"Clôturée",null,null,"Clôturée","56090","INZINZAC LOCHRIST","MORBIHAN","BRETAGNE","Polygone",-3.2997327,47.84105]
["SSP000104501",null,"Ancienne décharge de Kervellec",null,"Clôturée",null,null,"Clôturée","56092","KERFOURN","MORBIHAN","BRETAGNE","Polygone",-2.86891,48.042538]
["SSP000105201",null,"Ancienne décharge de Kervic",null,"Clôturée",null,null,"Clôturée","56100","LANGONNET","MORBIHAN","BRETAGNE","Polygone",-3.5028481,48.166134]
["SSP000105301",null,"Ancienne décharge de Kerhern-Liven",null,"Clôturée",null,null,"Clôturée","56101","LANGUIDIC","MORBIHAN","BRETAGNE","Polygone",-3.164532,47.797512]
["SSP000105501",null,"Ancienne décharge de Kervènic",null,"Clôturée",null,null,"Clôturée","56104","LANVAUDAN","MORBIHAN","BRETAGNE","Polygone",-3.2776043,47.88025]
["SSP000105601",null,"Ancienne décharge du Bourg",null,"Clôturée",null,null,"Clôturée","56048","LE CROISTY","MORBIHAN","BRETAGNE","Polygone",-3.359724,48.06529]
["SSP000105701",null,"Ancien dépôt de mâchefers et ancienne décharge de Cosquéric",null,"Clôturée",null,null,"Clôturée","56057","LE FAOUET","MORBIHAN","BRETAGNE","Polygone",-3.5143924,48.049736]
["SSP000105901",null,"Ancienne décharge du Val Jouin",null,"Clôturée",null,null,"Clôturée","56112","LIZIO","MORBIHAN","BRETAGNE","Polygone",-2.5198774,47.87276]
["SSP000106001",null,"Ancienne décharge contrôlée",null,"Clôturée",null,null,"Clôturée","56115","LOCMARIA GRAND CHAMP","MORBIHAN","BRETAGNE","Polygone",-2.7907703,47.734863]
["SSP000106101",null,"Ancienne décharge de Poulvern",null,"Clôturée",null,null,"Clôturée","56119","LOCOAL MENDON","MORBIHAN","BRETAGNE","Polygone",-3.0785177,47.72889]
["SSP000106301",null,"Ancienne décharge de Kervezet",null,"Clôturée",null,null,"Clôturée","56125","MALGUENAC","MORBIHAN","BRETAGNE","Polygone",-3.071412,48.07566]
["SSP000106601",null,"Ancienne décharge de Mellet",null,"Clôturée",null,null,"Clôturée","56133","MISSIRIAC","MORBIHAN","BRETAGNE","Polygone",-2.3416667,47.837154]
["SSP000106701",null,"Ancienne décharge de la Carrière Bouin",null,"Clôturée",null,null,"Clôturée","56136","MONTENEUF","MORBIHAN","BRETAGNE","Polygone",-2.2098823,47.87971]
["SSP000107001",null,"Ancienne décharge de Coëtsiec",null,"Clôturée",null,null,"Clôturée","56144","NAIZIN","MORBIHAN","BRETAGNE","Polygone",-2.862502,47.966873]
["SSP000107201",null,"Ancienne décharge de Guernal 2",null,"Clôturée",null,null,"Clôturée","56146","NEULLIAC","MORBIHAN","BRETAGNE","Polygone",-2.988355,48.09633]
["SSP000107301",null,"Ancienne décharge du Stumo",null,"Clôturée",null,null,"Clôturée","56146","NEULLIAC","MORBIHAN","BRETAGNE","Polygone",-3.0034304,48.141308]
["SSP000107401",null,"Ancienne décharge d'Auquinian",null,"Clôturée",null,null,"Clôturée","56146","NEULLIAC","MORBIHAN","BRETAGNE","Polygone",-3.0066853,48.125027]
["SSP000107501",null,"Ancienne décharge de la Butte du Lin",null,"Clôturée",null,null,"Clôturée","56147","NIVILLAC","MORBIHAN","BRETAGNE","Polygone",-2.2123625,47.54923]
["SSP000107601",null,"Ancienne décharge de Trémondet",null,"Clôturée",null,null,"Clôturée","56149","NOYAL MUZILLAC","MORBIHAN","BRETAGNE","Polygone",-2.4536185,47.60571]
["SSP000107701",null,"Ancienne décharge de Théra",null,"Clôturée",null,null,"Clôturée","56153","PEAULE","MORBIHAN","BRETAGNE","Polygone",-2.3414943,47.56965]
["SSP000107801",null,"Ancienne décharge du Bas Coëllo",null,"Clôturée",null,null,"Clôturée","56160","PLEUGRIFFET","MORBIHAN","BRETAGNE","Polygone",-2.6874053,48.009045]
["SSP000108001",null,"Ancienne décharge de Kermoisan",null,"Clôturée",null,null,"Clôturée","56173","PLUMELIAU","MORBIHAN","BRETAGNE","Polygone",-2.9693742,47.943962]
["SSP000108101",null,"Ancienne décharge de la Croix Courte",null,"Clôturée",null,null,"Clôturée","56177","PLUVIGNER","MORBIHAN","BRETAGNE","Polygone",-2.9925244,47.773907]
["SSP000108201",null,"Ancienne décharge de Guernal",null,"Clôturée",null,null,"Clôturée","56178","PONTIVY","MORBIHAN","BRETAGNE","Polygone",-2.9930515,48.09443]
["SSP000108301",null,"Ancienne décharge de Villons",null,"Clôturée",null,null,"Clôturée","56180","PORCARO","MORBIHAN","BRETAGNE","Polygone",-2.1959355,47.920273]
["SSP000108401",null,"Ancienne décharge de Quilvien",null,"Clôturée",null,null,"Clôturée","56182","PRIZIAC","MORBIHAN","BRETAGNE","Polygone",-3.4334886,48.05848]
["SSP000108501",null,"Ancienne décharge du Quily",null,"Clôturée",null,null,"Clôturée","56184","QUESTEMBERT","MORBIHAN","BRETAGNE","Polygone",-2.4002705,47.658176]
["SSP000108601",null,"Ancienne décharge de Léren",null,"Clôturée",null,null,"Clôturée","56190","REGUINY","MORBIHAN","BRETAGNE","Polygone",-2.7786002,47.98395]
["SSP000108701",null,"Ancienne décharge de l'Eclys",null,"Clôturée",null,null,"Clôturée","56194","RIEUX","MORBIHAN","BRETAGNE","Polygone",-2.1514263,47.601875]
["SSP000108801",null,"Ancienne décharge du Tertre",null,"Clôturée",null,null,"Clôturée","56198","ROHAN","MORBIHAN","BRETAGNE","Polygone",-2.7475564,48.094807]
["SSP000108901",null,"Ancienne décharge de Roscoat",null,"Clôturée",null,null,"Clôturée","56199","ROUDOUALLEC","MORBIHAN","BRETAGNE","Polygone",-3.6768935,48.141994]
["SSP000109001",null,"Ancienne décharge des Landes de l'Espérance",null,"Clôturée",null,null,"Clôturée","56200","RUFFIAC","MORBIHAN","BRETAGNE","Polygone",-2.3010225,47.827713]
["SSP000109101",null,"Ancienne décharge de Penbos",null,"Clôturée",null,null,"Clôturée","56242","SEGLIEN","MORBIHAN","BRETAGNE","Polygone",-3.1729088,48.10333]
["SSP000109201",null,"Ancienne décharge de Grehalet",null,"Clôturée",null,null,"Clôturée","56202","SAINT ABRAHAM","MORBIHAN","BRETAGNE","Polygone",-2.3986738,47.860947]
["SSP000109301",null,"Ancienne décharge de La Montagne",null,"Clôturée",null,null,"Clôturée","29001","ARGOL","FINISTERE","BRETAGNE","Polygone",-4.2922006,48.236782]
["SSP000109601",null,"Ancienne décharge de Kervennou",null,"Clôturée",null,null,"Clôturée","29010","BODILIS","FINISTERE","BRETAGNE","Polygone",-4.108301,48.512375]
["SSP000109801",null,"Ancienne décharge de Coat Mocum",null,"Clôturée",null,null,"Clôturée","29018","BRENNILIS","FINISTERE","BRETAGNE","Polygone",-3.8058302,48.36168]
["SSP000109901",null,"Ancienne décharge de Kermorvan",null,"Clôturée",null,null,"Clôturée","29018","BRENNILIS","FINISTERE","BRETAGNE","Polygone",-3.8407423,48.36193]
["SSP000110501",null,"Ancienne décharge de Langantec",null,"Clôturée",null,null,"Clôturée","29029","CLEDEN POHER","FINISTERE","BRETAGNE","Polygone",-3.6268232,48.25025]
["SSP000110901",null,"Ancienne décharge de Penhellec",null,"Clôturée",null,null,"Clôturée","56210","SAINT CARADEC TREGOMEL","MORBIHAN","BRETAGNE","Polygone",-3.3360605,48.031467]
["SSP000111001",null,"Ancienne décharge de La Née",null,"Clôturée",null,null,"Clôturée","56211","SAINT CONGARD","MORBIHAN","BRETAGNE","Polygone",-2.3163373,47.77566]
["SSP000111101",null,"Ancienne décharge de Cran",null,"Clôturée",null,null,"Clôturée","56213","SAINT GERAND","MORBIHAN","BRETAGNE","Polygone",-2.910254,48.101467]
["SSP000111301",null,"Ancienne décharge des Buttes des 5 Moulins",null,"Clôturée",null,null,"Clôturée","56221","SAINT JACUT LES PINS","MORBIHAN","BRETAGNE","Polygone",-2.2253082,47.694523]
["SSP000111601",null,"Ancienne décharge de Trélan",null,"Clôturée",null,null,"Clôturée","56228","SAINT MARCEL","MORBIHAN","BRETAGNE","Polygone",-2.4255476,47.819866]
["SSP000111801",null,"Ancienne décharge de la rue du stade",null,"Clôturée",null,null,"Clôturée","56234","SAINT PIERRE QUIBERON","MORBIHAN","BRETAGNE","Polygone",-3.1418974,47.512253]
["SSP000112001",null,"Ancienne décharge du Paty",null,"Clôturée",null,null,"Clôturée","56239","SAINT VINCENT SUR OUST","MORBIHAN","BRETAGNE","Polygone",-2.1386797,47.686836]
["SSP000112301",null,"Ancienne décharge de Cost er Ronz",null,"Clôturée",null,null,"Clôturée","56170","PLOURAY","MORBIHAN","BRETAGNE","Polygone",-3.3374307,48.13481]
["SSP000112401",null,"Ancienne décharge de Kerbodo",null,"Clôturée",null,null,"Clôturée","56143","MUZILLAC","MORBIHAN","BRETAGNE","Polygone",-2.5164053,47.562008]
["SSP000112501",null,"Ancienne décharge du terrain des nomades",null,"Clôturée",null,null,"Clôturée","56144","NAIZIN","MORBIHAN","BRETAGNE","Polygone",-2.8395162,47.993507]
["SSP000112801",null,"Ancienne décharge de la Corderie et ancien stockage de déchets de marées noires",null,"Clôturée",null,null,"Clôturée","22016","ILE DE BREHAT","COTES-D'ARMOR","BRETAGNE","Polygone",-3.000212,48.84923]
["SSP000113001",null,"Ancienne décharge du Bois Gory",null,"Clôturée",null,null,"Clôturée","22026","CALORGUEN","COTES-D'ARMOR","BRETAGNE","Polygone",-2.02701,48.417866]
["SSP000113101",null,"Ancienne décharge des Broussettes",null,"Clôturée",null,null,"Clôturée","22027","LE CAMBOUT","COTES-D'ARMOR","BRETAGNE","Polygone",-2.5958145,48.070892]
["SSP000113201",null,"Ancienne décharge d'Ar Rest",null,"Clôturée",null,null,"Clôturée","22031","CARNOET","COTES-D'ARMOR","BRETAGNE","Polygone",-3.526595,48.36469]
["SSP000113301",null,"Ancienne décharge de Kerstéphan",null,"Clôturée",null,null,"Clôturée","22034","CAVAN","COTES-D'ARMOR","BRETAGNE","Polygone",-3.3721826,48.685116]
["SSP000113401",null,"Ancienne décharge du Bloc",null,"Clôturée",null,null,"Clôturée","22035","LES CHAMPS GERAUX","COTES-D'ARMOR","BRETAGNE","Polygone",-1.9629326,48.437393]
["SSP000113501",null,"Ancienne décharge de La Colombière",null,"Clôturée",null,null,"Clôturée","22039","LA CHEZE","COTES-D'ARMOR","BRETAGNE","Polygone",-2.6535497,48.134148]
["SSP000113601",null,"Ancienne décharge de La Bosse",null,"Clôturée",null,null,"Clôturée","22046","COLLINEE","COTES-D'ARMOR","BRETAGNE","Polygone",-2.5058987,48.29547]
["SSP000113701",null,"Ancienne décharge de Guerlouic",null,"Clôturée",null,null,"Clôturée","22047","CORLAY","COTES-D'ARMOR","BRETAGNE","Polygone",-3.0377955,48.312756]
["SSP000113801",null,"Ancienne décharge du Vaugourieux",null,"Clôturée",null,null,"Clôturée","22049","CREHEN","COTES-D'ARMOR","BRETAGNE","Polygone",-2.2053518,48.538258]
["SSP000114101",null,"Ancienne décharge du Port à la Duc",null,"Clôturée",null,null,"Clôturée","22179","FREHEL","COTES-D'ARMOR","BRETAGNE","Polygone",-2.3425143,48.61612]
["SSP000114201",null,"Ancienne décharge du Rézy",null,"Clôturée",null,null,"Clôturée","22060","GAUSSON","COTES-D'ARMOR","BRETAGNE","Polygone",-2.7643712,48.3089]
["SSP000114501",null,"Ancienne décharge de Penanros",null,"Clôturée",null,null,"Clôturée","29038","COMMANA","FINISTERE","BRETAGNE","Polygone",-3.969236,48.403946]
["SSP000114601",null,"Ancienne décharge de Kereil",null,"Clôturée",null,null,"Clôturée","29039","CONCARNEAU","FINISTERE","BRETAGNE","Polygone",-3.8971393,47.894108]
["SSP000114801",null,"Ancienne décharge de Kerdanvez",null,"Clôturée",null,null,"Clôturée","29042","CROZON","FINISTERE","BRETAGNE","Polygone",-4.444608,48.25382]
["SSP000115001",null,"Ancienne décharge de Lesperbé",null,"Clôturée",null,null,"Clôturée","29046","DOUARNENEZ","FINISTERE","BRETAGNE","Polygone",-4.312268,48.05567]
["SSP000115301",null,"Ancienne décharge du stum",null,"Clôturée",null,null,"Clôturée","29053","LE FAOU","FINISTERE","BRETAGNE","Polygone",-4.1204433,48.307823]
["SSP000115401",null,"Ancienne décharge de Dour Braz",null,"Clôturée",null,null,"Clôturée","29054","LA FEUILLEE","FINISTERE","BRETAGNE","Polygone",-3.8594403,48.39277]
["SSP000116401",null,"Ancienne décharge de Kermenguy",null,"Clôturée",null,null,"Clôturée","29087","LE JUCH","FINISTERE","BRETAGNE","Polygone",-4.295679,48.048824]
["SSP000116801",null,"Ancienne décharge de Kergreven",null,"Clôturée",null,null,"Clôturée","29097","LAMPAUL GUIMILIAU","FINISTERE","BRETAGNE","Polygone",-4.0415664,48.47969]
["SSP000117001",null,"Ancienne décharge de Pen Ar C'hoat",null,"Clôturée",null,null,"Clôturée","29105","LANDIVISIAU","FINISTERE","BRETAGNE","Polygone",-4.0254593,48.517155]
["SSP000117901",null,"Ancienne décharge de Kerjézéquel",null,"Clôturée",null,null,"Clôturée","29124","LESNEVEN","FINISTERE","BRETAGNE","Polygone",-4.3196464,48.58824]
["SSP000118001",null,"Ancienne décharge de Kerzéven",null,"Clôturée",null,null,"Clôturée","29131","LOCMELAR","FINISTERE","BRETAGNE","Polygone",-4.069508,48.44446]
["SSP000118101",null,"Ancienne décharge de Lambezegou",null,"Clôturée",null,null,"Clôturée","29139","LOPEREC","FINISTERE","BRETAGNE","Polygone",-4.058524,48.264275]
["SSP000118201",null,"Ancienne décharge de Kergueven",null,"Clôturée",null,null,"Clôturée","29141","LOQUEFFRET","FINISTERE","BRETAGNE","Polygone",-3.8421485,48.341957]
["SSP000118301",null,"Ancienne décharge de Pen Ar Prat",null,"Clôturée",null,null,"Clôturée","29146","MELGVEN","FINISTERE","BRETAGNE","Polygone",-3.8762825,47.931084]
["SSP000119001",null,"Ancienne décharge de Pen ar Ménez",null,"Clôturée",null,null,"Clôturée","29169","PLOGONNEC","FINISTERE","BRETAGNE","Polygone",-4.1377206,48.09008]
["SSP000119101",null,"Ancienne décharge de Prat Youen",null,"Clôturée",null,null,"Clôturée","29169","PLOGONNEC","FINISTERE","BRETAGNE","Polygone",-4.190593,48.090588]
["SSP000119201",null,"Ancienne décharge de Kerbernez",null,"Clôturée",null,null,"Clôturée","29170","PLOMELIN","FINISTERE","BRETAGNE","Polygone",-4.131583,47.949192]
["SSP000119501",null,"Ancienne décharge de Pen Goayen",null,"Clôturée",null,null,"Clôturée","29173","PLONEIS","FINISTERE","BRETAGNE","Polygone",-4.191988,48.007282]
["SSP000120001",null,"Ancienne décharge de Releac'h",null,"Clôturée",null,null,"Clôturée","29179","PLOUDANIEL","FINISTERE","BRETAGNE","Polygone",-4.2862577,48.530273]
["SSP000120201",null,"Ancienne décharge de Dourlez",null,"Clôturée",null,null,"Clôturée","29187","PLOUGAR","FINISTERE","BRETAGNE","Polygone",-4.173438,48.553432]
["SSP000121501",null,"Ancienne décharge de Kermoal",null,"Clôturée",null,null,"Clôturée","29217","PONT AVEN","FINISTERE","BRETAGNE","Polygone",-3.7618806,47.90054]
["SSP000121801",null,"Ancienne décharge de la Kerbaol",null,"Clôturée",null,null,"Clôturée","29227","POULLAOUEN","FINISTERE","BRETAGNE","Polygone",-3.6434436,48.35126]
["SSP000122001",null,"Ancienne décharge de la Forêt du Duc",null,"Clôturée",null,null,"Clôturée","29229","QUEMENEVEN","FINISTERE","BRETAGNE","Polygone",-4.181786,48.104527]
["SSP000122801",null,"Ancienne décharge de Kéréon",null,"Clôturée",null,null,"Clôturée","29262","SAINT SAUVEUR","FINISTERE","BRETAGNE","Polygone",-3.9844542,48.462486]
["SSP000122901",null,"Ancienne décharge de Penvern",null,"Clôturée",null,null,"Clôturée","29264","SAINT SERVAIS","FINISTERE","BRETAGNE","Polygone",-4.1760316,48.50835]
["SSP000123201","33.0222","Décharge de Bègles Hourcade",null,"En cours",null,null,"En cours","33039","BEGLES","GIRONDE","NOUVELLE-AQUITAINE","Polygone",-0.55481505,44.791058,"K21 - Décharges d'ordures ménagères"]
["SSP000123401",null,"Ancienne décharge de la Motte",null,"Clôturée",null,null,"Clôturée","29277","SIZUN","FINISTERE","BRETAGNE","Polygone",-4.050835,48.40272]
["SSP000123501",null,"Ancienne décharge de Kerrouanec Vihan",null,"Clôturée",null,null,"Clôturée","29293","TREGUNC","FINISTERE","BRETAGNE","Polygone",-3.826963,47.858685]
["SSP000123601",null,"Ancienne décharge de kervoazou",null,"Clôturée",null,null,"Clôturée","29024","CARHAIX PLOUGUER","FINISTERE","BRETAGNE","Polygone",-3.5280652,48.28518]
["SSP000123901","33.0331","BAIGTS",null,"En cours",null,null,"En cours","33039","BEGLES","GIRONDE","NOUVELLE-AQUITAINE","Polygone",-0.5664096,44.79759]
["SSP000124001","33.0047","GRE",null,"En cours",null,null,"En cours","33039","BEGLES","GIRONDE","NOUVELLE-AQUITAINE","Polygone",-0.5548022,44.793736,"K36 - Mise en décharge"]
["SSP000124201","33.0174","VERRIERS D'AQUITAINE",null,"En cours",null,null,"En cours","33039","BEGLES","GIRONDE","NOUVELLE-AQUITAINE","Polygone",-0.5482082,44.81554,"G1 - Céramique, verre, matériaux de construction"]
["SSP000124401",null,"Ancienne décharge de Kerambellec",null,"Clôturée",null,null,"Clôturée","29153","NEVEZ","FINISTERE","BRETAGNE","Polygone",-3.7779772,47.806026]
["SSP000124501",null,"Ancienne décharge de Pen Ar Roc'h",null,"Clôturée",null,null,"Clôturée","29155","OUESSANT","FINISTERE","BRETAGNE","Polygone",-5.0889993,48.443344]
["SSP000124701",null,"Ancienne décharge de Kerleit",null,"Clôturée",null,null,"Clôturée","29211","PLOUYE","FINISTERE","BRETAGNE","Polygone",-3.7702813,48.329967]
["SSP000125001","33.0004","ELF Ancienne raffinerie d'Ambès",null,"En cours",null,null,"En cours","33004","AMBES","GIRONDE","NOUVELLE-AQUITAINE","Polygone",-0.5925332,45.03195,"D12 - Raffinage de pétrole, carburants et lubrifiants"]
["SSP000125101","24.0043","Ancienne décharge POLYREY",null,"En cours",null,null,"En cours","24023","BANEUIL","DORDOGNE","NOUVELLE-AQUITAINE","Polygone",0.70135343,44.85104,"C12 - Produits en bois, ameublement (fabrication de)"]
["SSP000125301","33.0176","WINTERSTEIN A",null,"En cours",null,null,"En cours","33056","BLANQUEFORT","GIRONDE","NOUVELLE-AQUITAINE","Polygone",-0.61779803,44.93582]
["SSP000125401","33.0275","ARDEA",null,"En cours",null,null,"En cours","33063","BORDEAUX","GIRONDE","NOUVELLE-AQUITAINE","Polygone",-0.55311424,44.83639,"D21 - Stockage et conditionnement des gaz et liquéfiés"]
["SSP000125501","62.0081","NITROCHIMIE (Société EPC France)",null,"En cours",null,null,"En cours","62132","BILLY BERCLAU","PAS-DE-CALAIS","HAUTS-DE-FRANCE","Polygone",2.8775,50.510754,"D - Chimie, parachimie, pétrole"]
["SSP000125601",null,"Ancienne décharge du Gros Chêne",null,"Clôturée",null,null,"Clôturée","56001","ALLAIRE","MORBIHAN","BRETAGNE","Polygone",-2.1952157,47.64171]
["SSP000125701",null,"Ancienne décharge de la Ville au Vent",null,"Clôturée",null,null,"Clôturée","56004","ARZAL","MORBIHAN","BRETAGNE","Polygone",-2.3852112,47.5219]
["SSP000126001",null,"Ancienne décharge du Fouliguet",null,"Clôturée",null,null,"Clôturée","56018","BILLIERS","MORBIHAN","BRETAGNE","Polygone",-2.4750345,47.526512]
["SSP000126101",null,"Ancienne décharge de Coet Nohennec",null,"Clôturée",null,null,"Clôturée","56041","CLEGUEREC","MORBIHAN","BRETAGNE","Polygone",-3.120609,48.141315]
["SSP000126201",null,"Ancienne décharge de Saint Nicolas",null,"Clôturée",null,null,"Clôturée","56069","GROIX","MORBIHAN","BRETAGNE","Polygone",-3.4803574,47.633503]
["SSP000126801",null,"Anciennes décharge du Camp",null,"Clôturée",null,null,"Clôturée","22061","GLOMEL","COTES-D'ARMOR","BRETAGNE","Polygone",-3.3905702,48.233105]
["SSP000126901",null,"Ancienne décharge de La Guenaye Nord",null,"Clôturée",null,null,"Clôturée","22062","GOMENE","COTES-D'ARMOR","BRETAGNE","Polygone",-2.4794393,48.174026]
["SSP000127001",null,"Ancienne décharge de la route de Saint-Gilles",null,"Clôturée",null,null,"Clôturée","22064","GOUAREC","COTES-D'ARMOR","BRETAGNE","Polygone",-3.1909485,48.234623]
["SSP000127201",null,"Ancienne décharge des Bruyères",null,"Clôturée",null,null,"Clôturée","22068","GRACE UZEL","COTES-D'ARMOR","BRETAGNE","Polygone",-2.7834032,48.24231]
["SSP000127401",null,"Ancienne décharge de la Salle",null,"Clôturée",null,null,"Clôturée","22077","HENANSAL","COTES-D'ARMOR","BRETAGNE","Polygone",-2.452267,48.538883]
["SSP000127501",null,"Ancienne décharge de Fétabry",null,"Clôturée",null,null,"Clôturée","22079","HENON","COTES-D'ARMOR","BRETAGNE","Polygone",-2.6598048,48.374508]
["SSP000127601",null,"Ancienne décharge de la Ville Indeloup",null,"Clôturée",null,null,"Clôturée","22081","HILLION","COTES-D'ARMOR","BRETAGNE","Polygone",-2.6316602,48.513416]
["SSP000127701","18.0062","Décharge du bois blanc",null,"En cours",null,null,"En cours","18279","VIERZON","CHER","CENTRE-VAL DE LOIRE","Polygone",2.1162958,47.20203,"K - Déchets et traitements"]
["SSP000127801","18.0061","FUJIFILM",null,"En cours",null,null,"En cours","18205","SAINT DOULCHARD","CHER","CENTRE-VAL DE LOIRE","Polygone",2.39002,47.105732,"H22 - Laboratoires photographiques"]
["SSP000128001",null,"Ancienne décharge de Bilvero",null,"Clôturée",null,null,"Clôturée","22085","KERBORS","COTES-D'ARMOR","BRETAGNE","Polygone",-3.1960764,48.818195]
["SSP000128101",null,"Ancienne décharge de la Route de Locarn",null,"Clôturée",null,null,"Clôturée","22087","KERGRIST MOELOU","COTES-D'ARMOR","BRETAGNE","Polygone",-3.3228095,48.309483]
["SSP000128201","59.0017","DEPOTS RHONE POULENC (Friche PCUK)",null,"En cours",null,null,"En cours","59339","LEERS","NORD","HAUTS-DE-FRANCE","Polygone",3.2182176,50.688698,"K - Déchets et traitements"]
["SSP000128401","59.0237","CLEMENT RPC",null,"En cours",null,null,"En cours","59350","LILLE","NORD","HAUTS-DE-FRANCE","Polygone",3.0099506,50.626457,"M - Divers et services"]
["SSP000128501","59.0343","Société AMEDEE PRODUCTION",null,"En cours",null,null,"En cours","59512","ROUBAIX","NORD","HAUTS-DE-FRANCE","Polygone",3.1965802,50.701508,"E11 - Peignage, cardage des fibres textiles"]
["SSP000128601","59.0351","LAINIERE DE ROUBAIX",null,"En cours",null,null,"En cours","59512","ROUBAIX","NORD","HAUTS-DE-FRANCE","Polygone",3.1928596,50.70759,"E13 - Blanchiment, teinture, impression"]
["SSP000128801","59.0480","SCI WILSON (Alty)",null,"En cours",null,null,"En cours","59560","SECLIN","NORD","HAUTS-DE-FRANCE","Polygone",3.039754,50.562515,"L23 - Détail de carburants"]
["SSP000128901","59.0490","TOTAL MOUVAUX",null,"En cours",null,null,"En cours","59421","MOUVAUX","NORD","HAUTS-DE-FRANCE","Polygone",3.1365159,50.715405]
["SSP000129001","59.0475","MOSSLEY BADIN",null,"En cours",null,null,"En cours","59350","LILLE","NORD","HAUTS-DE-FRANCE","Polygone",3.1047704,50.62984,"E12 - Filtène, filature, tissage, tricotage"]
["SSP000129101","59.0002","PROMOFRANCE",null,"En cours",null,null,"En cours","59350","LILLE","NORD","HAUTS-DE-FRANCE","Polygone",3.046218,50.625183,"E14 - Confection de vêtements, bonneterie"]
["SSP000129201","59.0003","PROTECTAL",null,"En cours",null,null,"En cours","59350","LILLE","NORD","HAUTS-DE-FRANCE","Polygone",3.0445704,50.614788,"H13 - Traitement de surface"]
["SSP000129301","59.0005","STATION TOTAL (supermarché metro)",null,"En cours",null,null,"En cours","59350","LILLE","NORD","HAUTS-DE-FRANCE","Polygone",2.9720032,50.640865,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000129401","59.0006","PRODUITS CHIMIQUES DE LOOS",null,"En cours",null,null,"En cours","59360","LOOS","NORD","HAUTS-DE-FRANCE","Polygone",3.0089934,50.62274,"D - Chimie, parachimie, pétrole"]
["SSP000129501","59.0007","GRANDS MOULINS DE PARIS",null,"En cours",null,null,"En cours","59386","MARQUETTE LEZ LILLE","NORD","HAUTS-DE-FRANCE","Polygone",3.0596454,50.672115,"M - Divers et services"]
["SSP000129601","59.0008","IHF ANCIENNE DECHARGE DU CHEMIN DES SERRES",null,"En cours",null,null,"En cours","59646","WASQUEHAL","NORD","HAUTS-DE-FRANCE","Polygone",3.1335185,50.68173,"K22 - Regroupement d'OM, DIB"]
["SSP000129701","59.0009","DECHARGE DECOTTEGNIE",null,"En cours",null,null,"En cours","59252","FRELINGHIEN","NORD","HAUTS-DE-FRANCE","Polygone",2.942737,50.724888,"K36 - Mise en décharge"]
["SSP000129801","59.0010","ETABLISSEMENTS BEUQUE",null,"En cours",null,null,"En cours","59512","ROUBAIX","NORD","HAUTS-DE-FRANCE","Polygone",3.1827197,50.696747,"H15 - Assemblage, montage"]
["SSP000129901","59.0012","PLANQUE MAINTENANCE INDUSTRIELLE REUNIS (PMIR)",null,"En cours",null,null,"En cours","59512","ROUBAIX","NORD","HAUTS-DE-FRANCE","Polygone",3.1842778,50.704346,"H13 - Traitement de surface"]
["SSP000130001","59.0019","ANCIENNE USINE TEINTURES ET IMPRESSIONS DU NORD",null,"En cours",null,null,"En cours","59670","DON","NORD","HAUTS-DE-FRANCE","Polygone",2.90087,50.539677,"E13 - Blanchiment, teinture, impression"]
["SSP000130101","59.0020","SOCIETE DES HUILES LEMAHIEU",null,"En cours",null,null,"En cours","59266","GONDECOURT","NORD","HAUTS-DE-FRANCE","Polygone",2.959519,50.563236,"K41 - Régénération d'huiles"]
["SSP000130201","59.0021","SOCIETE DE FABRICATION ET DE DISTRIBUTION DE PRODUITS INDUSTRIELS (SFDPI)",null,"En cours",null,null,"En cours","59266","GONDECOURT","NORD","HAUTS-DE-FRANCE","Polygone",2.986173,50.54156,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000130301","59.0022","Quaron ex DISTRICHIMIE (anciennement SA DOCKS DES ALCOOLS)",null,"En cours",null,null,"En cours","59286","HAUBOURDIN","NORD","HAUTS-DE-FRANCE","Polygone",2.981014,50.602077,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000130401","59.0023","ANCIENNE USINE SANDER",null,"En cours",null,null,"En cours","59286","HAUBOURDIN","NORD","HAUTS-DE-FRANCE","Polygone",2.980016,50.590576,"E1 - Textile et habillement, teinture, impression"]
["SSP000130501","59.0024","RELAIS TOTAL DE PHALEMPIN",null,"En cours",null,null,"En cours","59560","SECLIN","NORD","HAUTS-DE-FRANCE","Polygone",3.0456748,50.53162,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000130601","59.0075","Ilôt Ste Helène",null,"En cours",null,null,"En cours","59527","SAINT ANDRE LEZ LILLE","NORD","HAUTS-DE-FRANCE","Polygone",3.0565953,50.65837,"D42 - Fabrication de peintures"]
["SSP000130701","59.0079","LOGICIL WATTRELOS",null,"En cours",null,null,"En cours","59650","WATTRELOS","NORD","HAUTS-DE-FRANCE","Polygone",3.1895187,50.71111,"K22 - Regroupement d'OM, DIB"]
["SSP000130801","59.0080","MACOFA",null,"En cours",null,null,"En cours","59350","LILLE","NORD","HAUTS-DE-FRANCE","Polygone",3.076298,50.612206,"E12 - Filtène, filature, tissage, tricotage"]
["SSP000130901","59.0082","DECHARGE DU GRAND COTTIGNIES (JOVENEAUX)",null,"En cours",null,null,"En cours","59646","WASQUEHAL","NORD","HAUTS-DE-FRANCE","Polygone",3.1319983,50.680252,"K22 - Regroupement d'OM, DIB"]
["SSP000131001","59.0083","SOTIRA 59 (THEOLAUR)",null,"En cours",null,null,"En cours","59646","WASQUEHAL","NORD","HAUTS-DE-FRANCE","Polygone",3.1351123,50.6707,"D7 - Caoutchouc et matières plastiques"]
["SSP000131101","59.0100","AIR TOTAL (TOTAL RAFFINAGE DISTRIBUTION S.A.)",null,"En cours",null,null,"En cours","59343","LESQUIN","NORD","HAUTS-DE-FRANCE","Polygone",3.095293,50.574318,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000131201","59.0105","SMIE",null,"En cours",null,null,"En cours","59360","LOOS","NORD","HAUTS-DE-FRANCE","Polygone",3.0197515,50.622128,"K35 - Regroupement, reconditionnement de déchets"]
["SSP000131301","59.0109","BRENNTAG (anciens établissements DEBAUCHE)",null,"En cours",null,null,"En cours","59650","WATTRELOS","NORD","HAUTS-DE-FRANCE","Polygone",3.1831164,50.715836,"K3 - Traitement de déchets industriels"]
["SSP000131401","59.0110","SCI VICTOR HUGO",null,"En cours",null,null,"En cours","59317","HOUPLINES","NORD","HAUTS-DE-FRANCE","Polygone",2.8997238,50.690113,"M - Divers et services"]
["SSP000131501","59.0129","DEPOT DE CENDRES EDF COMINES",null,"En cours",null,null,"En cours","59152","COMINES","NORD","HAUTS-DE-FRANCE","Polygone",3.0191128,50.76991,"I11 - Centrales électriques thermiques"]
["SSP000131601","59.0130","DEPOT DE CENDRES EDF ANSEREUILLES",null,"En cours",null,null,"En cours","59005","ALLENNES LES MARAIS","NORD","HAUTS-DE-FRANCE","Polygone",2.9444003,50.55146,"I11 - Centrales électriques thermiques"]
["SSP000131701","59.0134","SOCOCHIM",null,"En cours",null,null,"En cours","59512","ROUBAIX","NORD","HAUTS-DE-FRANCE","Polygone",3.2030504,50.692398,"L13 - Entrepôts de produits dangereux"]
["SSP000131801","59.0135","SOCIETE NOUVELLE DE TEINTURERIE DE FRELINGHIEN",null,"En cours",null,null,"En cours","59252","FRELINGHIEN","NORD","HAUTS-DE-FRANCE","Polygone",2.9313478,50.71117,"E1 - Textile et habillement, teinture, impression"]
["SSP000131901","59.0136","STATION SERVICE AUCHAN RONCQ",null,"En cours",null,null,"En cours","59508","RONCQ","NORD","HAUTS-DE-FRANCE","Polygone",3.1385677,50.740208,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000132001","59.0147","PEINTURES AVI",null,"En cours",null,null,"En cours","59421","MOUVAUX","NORD","HAUTS-DE-FRANCE","Polygone",3.1423116,50.71316,"D42 - Fabrication de peintures"]
["SSP000132101","59.0149","SRRHU",null,"En cours",null,null,"En cours","59421","MOUVAUX","NORD","HAUTS-DE-FRANCE","Polygone",3.132682,50.713245,"K35 - Regroupement, reconditionnement de déchets"]
["SSP000132201","59.0150","PJT INDUSTRIES",null,"En cours",null,null,"En cours","59599","TOURCOING","NORD","HAUTS-DE-FRANCE","Polygone",3.1493905,50.721546,"E1 - Textile et habillement, teinture, impression"]
["SSP000132301","59.0152","SDEZ",null,"En cours",null,null,"En cours","59350","LILLE","NORD","HAUTS-DE-FRANCE","Polygone",3.0088003,50.629562,"E13 - Blanchiment, teinture, impression"]
["SSP000132401","59.0153","PEUGEOT LILLE usine A",null,"En cours",null,null,"En cours","59350","LILLE","NORD","HAUTS-DE-FRANCE","Polygone",3.0939534,50.637928,"H15 - Assemblage, montage"]
["SSP000132501","59.0154","EPR (entrepôts pétroliers régionaux)",null,"En cours",null,null,"En cours","59378","MARCQ EN BAROEUL","NORD","HAUTS-DE-FRANCE","Polygone",3.0736582,50.67184,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000132601","59.0155","CHRU",null,"En cours",null,null,"En cours","59350","LILLE","NORD","HAUTS-DE-FRANCE","Polygone",3.0381038,50.612488,"I22 - Production de chaleur autres"]
["SSP000132701","59.0157","VANNES LEFEBVRE",null,"En cours",null,null,"En cours","59350","LILLE","NORD","HAUTS-DE-FRANCE","Polygone",3.071099,50.613754,"J5 - Fonderie et travail des métaux"]
["SSP000132801","59.0159","STATION SERVICE ESSO (ex FINA LAMBERSART)",null,"En cours",null,null,"En cours","59328","LAMBERSART","NORD","HAUTS-DE-FRANCE","Polygone",3.0281887,50.644653,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000132901","59.0160","THEODORE LEFEBVRE",null,"En cours",null,null,"En cours","59350","LILLE","NORD","HAUTS-DE-FRANCE","Polygone",3.0744562,50.619682,"D42 - Fabrication de peintures"]
["SSP000133001","59.0161","TOLERIE DN",null,"En cours",null,null,"En cours","59386","MARQUETTE LEZ LILLE","NORD","HAUTS-DE-FRANCE","Polygone",3.0580378,50.678364,"H13 - Traitement de surface"]
["SSP000133101","59.0164","TOLERIES DE LA DEULE",null,"En cours",null,null,"En cours","59482","QUESNOY SUR DEULE","NORD","HAUTS-DE-FRANCE","Polygone",2.9930387,50.71203,"H14 - Application de peinture"]
["SSP000133201","59.0166","ETS ALFRED DUPONT",null,"En cours",null,null,"En cours","59599","TOURCOING","NORD","HAUTS-DE-FRANCE","Polygone",3.1523273,50.716476,"E12 - Filtène, filature, tissage, tricotage"]
["SSP000133301","59.0167","GRILTEX (ex SARNEIGE - GVG SPORTS)",null,"En cours",null,null,"En cours","59650","WATTRELOS","NORD","HAUTS-DE-FRANCE","Polygone",3.2392037,50.705162,"D72 - Transformation des matières plastiques"]
["SSP000133401","59.0182","DE TAYRAC",null,"En cours",null,null,"En cours","59011","ANNOEULLIN","NORD","HAUTS-DE-FRANCE","Polygone",2.9377575,50.523838,"E2 - Industrie des cuirs et peaux, tannerie"]
["SSP000133501","59.0190","HOLLIDAY PIGMENT",null,"En cours",null,null,"En cours","59152","COMINES","NORD","HAUTS-DE-FRANCE","Polygone",3.033933,50.768906,"D - Chimie, parachimie, pétrole"]
["SSP000133601","59.0196","RECHIM",null,"En cours",null,null,"En cours","59163","CROIX","NORD","HAUTS-DE-FRANCE","Polygone",3.142994,50.679935,"H13 - Traitement de surface"]
["SSP000133701","59.0212","Flint Group  (anciennement xsys print solutions et  ex BASF-SYSTEME D'IMPRESSION",null,"En cours",null,null,"En cours","59256","FRETIN","NORD","HAUTS-DE-FRANCE","Polygone",3.1314452,50.553665,"D4 - Encres, vernis, peintures, colles (fabrication de)"]
["SSP000133801","59.0213","PREFERNOR",null,"En cours",null,null,"En cours","59256","FRETIN","NORD","HAUTS-DE-FRANCE","Polygone",3.1394188,50.564846,"K3 - Traitement de déchets industriels"]
["SSP000133901","59.0215","BOURIGEAUD Industry EURL",null,"En cours",null,null,"En cours","59266","GONDECOURT","NORD","HAUTS-DE-FRANCE","Polygone",2.9631808,50.563606,"D - Chimie, parachimie, pétrole"]
["SSP000134001","59.0216","ARPADIS GONDECOURT (Ex CATRY)",null,"En cours",null,null,"En cours","59266","GONDECOURT","NORD","HAUTS-DE-FRANCE","Polygone",2.981051,50.559433,"D4 - Encres, vernis, peintures, colles (fabrication de)"]
["SSP000134301","59.0223","TOPAZE (appartenant à Unilever France)",null,"En cours",null,null,"En cours","59286","HAUBOURDIN","NORD","HAUTS-DE-FRANCE","Polygone",2.9764266,50.60539,"D62 - Fabrication de détergents"]
["SSP000134401","59.0225","CHIMIE DERIVES",null,"En cours",null,null,"En cours","59350","LILLE","NORD","HAUTS-DE-FRANCE","Polygone",3.1035688,50.633507,"K2 - Traitement de déchets urbains"]
["SSP000134501","59.0233","OUVRIE  - PMC",null,"En cours",null,null,"En cours","59343","LESQUIN","NORD","HAUTS-DE-FRANCE","Polygone",3.1149929,50.58895,"D3 - Chimie, phytosanitaire, pharmacie"]
["SSP000134601","59.0234","Elcobrandt (ex SELNOR)",null,"En cours",null,null,"En cours","59343","LESQUIN","NORD","HAUTS-DE-FRANCE","Polygone",3.123848,50.587296,"H15 - Assemblage, montage"]
["SSP000134701","59.0236","VERBRUGGE",null,"En cours",null,null,"En cours","59350","LILLE","NORD","HAUTS-DE-FRANCE","Polygone",3.052904,50.613106,"H13 - Traitement de surface"]
["SSP000134801","59.0242","CIBIE",null,"En cours",null,null,"En cours","59386","MARQUETTE LEZ LILLE","NORD","HAUTS-DE-FRANCE","Polygone",3.0575812,50.67559,"K5 - Récupération, dépôts de ferrailles"]
["SSP000134901","59.0245","CERPLEX",null,"En cours",null,null,"En cours","59426","NEUVILLE EN FERRAIN","NORD","HAUTS-DE-FRANCE","Polygone",3.1629965,50.760975,"H1 - Mécanique, électrique, traitement de surface"]
["SSP000135001","59.0249","OLEA",null,"En cours",null,null,"En cours","59437","NOYELLES LES SECLIN","NORD","HAUTS-DE-FRANCE","Polygone",3.0187244,50.57547,"D62 - Fabrication de détergents"]
["SSP000135101","59.0252","AGFA GEVAERT",null,"En cours",null,null,"En cours","59466","PONT A MARCQ","NORD","HAUTS-DE-FRANCE","Polygone",3.1253388,50.517143,"D51 - Fabrication de surfaces sensibles"]
["SSP000135201","59.0254","FLIPO RICHIR",null,"En cours",null,null,"En cours","59512","ROUBAIX","NORD","HAUTS-DE-FRANCE","Polygone",3.1586723,50.690445,"H18 - Composants électroniques (fabrication de)"]
["SSP000135301","59.0255","BARCROM (ex Ets Lecomte)",null,"En cours",null,null,"En cours","59512","ROUBAIX","NORD","HAUTS-DE-FRANCE","Polygone",3.198586,50.685963,"H13 - Traitement de surface"]
["SSP000135401","59.0256","REGESOLVE",null,"En cours",null,null,"En cours","59512","ROUBAIX","NORD","HAUTS-DE-FRANCE","Polygone",3.1650379,50.70507,"K42 - Régénération de solvants"]
["SSP000135501","59.0257","FONDERIE DE CROIX",null,"En cours",null,null,"En cours","59512","ROUBAIX","NORD","HAUTS-DE-FRANCE","Polygone",3.2047126,50.686546,"J51 - Fonderie des métaux ferreux"]
["SSP000135601","59.0262","REFINAL",null,"En cours",null,null,"En cours","59350","LILLE","NORD","HAUTS-DE-FRANCE","Polygone",3.0074983,50.626213]
["SSP000135701","59.0265","UNIVAR EUROPE (ex  LAMBERT RIVIERE)",null,"En cours",null,null,"En cours","59527","SAINT ANDRE LEZ LILLE","NORD","HAUTS-DE-FRANCE","Polygone",3.0578332,50.668747,"D32 - Chimie minérale inorganique autre"]
["SSP000135801","59.0268","BRABANT",null,"En cours",null,null,"En cours","59602","TRESSIN","NORD","HAUTS-DE-FRANCE","Polygone",3.1867757,50.613472,"K42 - Régénération de solvants"]
["SSP000135901","59.0277","TSB",null,"En cours",null,null,"En cours","59646","WASQUEHAL","NORD","HAUTS-DE-FRANCE","Polygone",3.126856,50.669632,"H13 - Traitement de surface"]
["SSP000136001","59.0283","TAPISIFT",null,"En cours",null,null,"En cours","59599","TOURCOING","NORD","HAUTS-DE-FRANCE","Polygone",3.1413672,50.71054,"E13 - Blanchiment, teinture, impression"]
["SSP000136101","59.0295","INSTALLATION TECHNIQUE DE GAZ DE FRANCE GDF",null,"En cours",null,null,"En cours","59650","WATTRELOS","NORD","HAUTS-DE-FRANCE","Polygone",3.2153716,50.70441,"J1 - Cokéfaction, usines à gaz"]
["SSP000136201","59.0297","ANCIENNE USINE A GAZ",null,"En cours",null,null,"En cours","59017","ARMENTIERES","NORD","HAUTS-DE-FRANCE","Polygone",2.8888924,50.68444,"J1 - Cokéfaction, usines à gaz"]
["SSP000136301","59.0304","ANCIEN MAGASIN PRISUNIC",null,"En cours",null,null,"En cours","59350","LILLE","NORD","HAUTS-DE-FRANCE","Polygone",3.056212,50.629425,"I - Energie"]
["SSP000136401","59.0305","PAINDAVOINE DEMANGHON",null,"En cours",null,null,"En cours","59386","MARQUETTE LEZ LILLE","NORD","HAUTS-DE-FRANCE","Polygone",3.0577548,50.67325,"K - Déchets et traitements"]
["SSP000136501","59.0313","HOPITAL LA CHARITE",null,"En cours",null,null,"En cours","59350","LILLE","NORD","HAUTS-DE-FRANCE","Polygone",3.0482137,50.61926,"M3 - Santé"]
["SSP000136601","59.0315","VERHAEGHE BIOTECHNOLOGIE",null,"En cours",null,null,"En cours","59512","ROUBAIX","NORD","HAUTS-DE-FRANCE","Polygone",3.1837645,50.695614,"E13 - Blanchiment, teinture, impression"]
["SSP000136701","59.0317","MALTEUROP (Recybois FMD SAS)",null,"En cours",null,null,"En cours","59044","BAISIEUX","NORD","HAUTS-DE-FRANCE","Polygone",3.241741,50.61795,"B17 - Autres industries agro-alimentaires"]
["SSP000136801","59.0322","DELATTRE",null,"En cours",null,null,"En cours","59512","ROUBAIX","NORD","HAUTS-DE-FRANCE","Polygone",3.2088163,50.690308,"K32 - Traitements physico-chimiques"]
["SSP000136901","59.0323","POULLET DEMEESTERE",null,"En cours",null,null,"En cours","59512","ROUBAIX","NORD","HAUTS-DE-FRANCE","Polygone",3.160807,50.693974,"E21 - Tannerie, mégisserie"]
["SSP000137001","59.0324","TEINTURERIE DU PILE",null,"En cours",null,null,"En cours","59512","ROUBAIX","NORD","HAUTS-DE-FRANCE","Polygone",3.1918793,50.68805,"E13 - Blanchiment, teinture, impression"]
["SSP000137101","59.0326","WOREX",null,"En cours",null,null,"En cours","59143","LA CHAPELLE D'ARMENTIERES","NORD","HAUTS-DE-FRANCE","Polygone",2.8859448,50.677574,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000137201","59.0327","POUDRES INDUSTRIELLES DU NORD - PINFLOC",null,"En cours",null,null,"En cours","59299","HEM","NORD","HAUTS-DE-FRANCE","Polygone",3.1967146,50.659348,"E13 - Blanchiment, teinture, impression"]
["SSP000137301","59.0330","SOCOWA - SIDEC",null,"En cours",null,null,"En cours","59650","WATTRELOS","NORD","HAUTS-DE-FRANCE","Polygone",3.2124715,50.705967,"K3 - Traitement de déchets industriels"]
["SSP000137401","59.0331","TEINTURERIE MEILLASSOUX - MULATON (TMM)",null,"En cours",null,null,"En cours","59299","HEM","NORD","HAUTS-DE-FRANCE","Polygone",3.179564,50.652607,"E13 - Blanchiment, teinture, impression"]
["SSP000137501","59.0332","AVELANA ex DECLERCQ (SNDF)",null,"En cours",null,null,"En cours","59299","HEM","NORD","HAUTS-DE-FRANCE","Polygone",3.1743724,50.65426,"E13 - Blanchiment, teinture, impression"]
["SSP000137601","59.0333","SI ENERGIE ( ALSTOM (STEIN INDUSTRIES))",null,"En cours",null,null,"En cours","59367","LYS LEZ LANNOY","NORD","HAUTS-DE-FRANCE","Polygone",3.2049396,50.66719,"H - Mécanique, traitements des surfaces"]
["SSP000137701","59.0335","FARATEX",null,"En cours",null,null,"En cours","59339","LEERS","NORD","HAUTS-DE-FRANCE","Polygone",3.2446828,50.67187,"E13 - Blanchiment, teinture, impression"]
["SSP000137801","59.0337","FCB, site Fivcar (Ateliers de Fives SA)",null,"En cours",null,null,"En cours","59350","LILLE","NORD","HAUTS-DE-FRANCE","Polygone",3.0944338,50.625896,"H11 - Usinage"]
["SSP000137901","59.0339","GROUPE DISTILLERIE CLAEYSSENS",null,"En cours",null,null,"En cours","59360","LOOS","NORD","HAUTS-DE-FRANCE","Polygone",3.010544,50.616707,"B21 - Distillation d'alcool et d'eau de vie"]
["SSP000138001","59.0340","EDF (CENTRE DE REGROUPEMENT DE TRANSFORMATEURS USAGES)",null,"En cours",null,null,"En cours","59368","LA MADELEINE","NORD","HAUTS-DE-FRANCE","Polygone",3.078389,50.647945,"K35 - Regroupement, reconditionnement de déchets"]
["SSP000138101","59.0341","SARL TRANSPORTS JOVENEAUX",null,"En cours",null,null,"En cours","59386","MARQUETTE LEZ LILLE","NORD","HAUTS-DE-FRANCE","Polygone",3.070355,50.6823,"K22 - Regroupement d'OM, DIB"]
["SSP000138201","59.0344","LAJTOS",null,"En cours",null,null,"En cours","59512","ROUBAIX","NORD","HAUTS-DE-FRANCE","Polygone",3.1706069,50.689644,"H13 - Traitement de surface"]
["SSP000138301","59.0345","SOTEMA",null,"En cours",null,null,"En cours","59512","ROUBAIX","NORD","HAUTS-DE-FRANCE","Polygone",3.1615722,50.68534,"E13 - Blanchiment, teinture, impression"]
["SSP000138401","59.0347","AVD (ATELIERS VANDERSCHELDEN DANIEL)",null,"En cours",null,null,"En cours","59512","ROUBAIX","NORD","HAUTS-DE-FRANCE","Polygone",3.206252,50.683594,"H13 - Traitement de surface"]
["SSP000138501","59.0348","NOUVELLES FILATURES LAINIERES DE ROUBAIX",null,"En cours",null,null,"En cours","59512","ROUBAIX","NORD","HAUTS-DE-FRANCE","Polygone",3.1932538,50.707413,"E12 - Filtène, filature, tissage, tricotage"]
["SSP000138601","59.0355","SOCIETE CHIMIQUE DE LA COURNEUVE (Caldic spécialité)",null,"En cours",null,null,"En cours","59527","SAINT ANDRE LEZ LILLE","NORD","HAUTS-DE-FRANCE","Polygone",3.057334,50.66932,"D - Chimie, parachimie, pétrole"]
["SSP000138701","59.0356","ANCIEN DEPÔT ESSO",null,"En cours",null,null,"En cours","59386","MARQUETTE LEZ LILLE","NORD","HAUTS-DE-FRANCE","Polygone",3.0585856,50.670406,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000138801","59.0357","GUERMONPREZ",null,"En cours",null,null,"En cours","59527","SAINT ANDRE LEZ LILLE","NORD","HAUTS-DE-FRANCE","Polygone",3.0481381,50.652832,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000138901","59.0362","FCB, site de la Compagnie de Fives-Lille",null,"En cours",null,null,"En cours","59350","LILLE","NORD","HAUTS-DE-FRANCE","Polygone",3.0935953,50.62703,"H - Mécanique, traitements des surfaces"]
["SSP000139001","59.0363","D'HAUSSY IMPRIMEURS",null,"En cours",null,null,"En cours","59599","TOURCOING","NORD","HAUTS-DE-FRANCE","Polygone",3.0875895,50.74956,"E1 - Textile et habillement, teinture, impression"]
["SSP000139101","59.0369","COVENTRY (ex BILORE)",null,"En cours",null,null,"En cours","59286","HAUBOURDIN","NORD","HAUTS-DE-FRANCE","Polygone",2.9804378,50.605007,"D62 - Fabrication de détergents"]
["SSP000139201","59.0370","T.R.A (Traitement et Revalorisation de produits Alimentaires ou agricoles)",null,"En cours",null,null,"En cours","59585","TEMPLEMARS","NORD","HAUTS-DE-FRANCE","Polygone",3.0526218,50.570694,"K - Déchets et traitements"]
["SSP000139301","59.0371","DANONE",null,"En cours",null,null,"En cours","59560","SECLIN","NORD","HAUTS-DE-FRANCE","Polygone",3.0239272,50.541397,"B12 - Industrie laitière"]
["SSP000139401","59.0372","AGACHE - LINCRUSTA",null,"En cours",null,null,"En cours","59560","SECLIN","NORD","HAUTS-DE-FRANCE","Polygone",3.037026,50.549786,"E12 - Filtène, filature, tissage, tricotage"]
["SSP000139501","59.0374","DESCAMPS ASSAINISSEMENT",null,"En cours",null,null,"En cours","59017","ARMENTIERES","NORD","HAUTS-DE-FRANCE","Polygone",2.8706682,50.691666,"K34 - Solidification de déchets liquides"]
["SSP000139701","59.0388","MAN ORGA INDUSTRIE",null,"En cours",null,null,"En cours","59512","ROUBAIX","NORD","HAUTS-DE-FRANCE","Polygone",3.2256215,50.670784,"J53 - Travail des métaux, chaudronnerie, poudres"]
["SSP000139801","59.0389","VANOUTRYVE",null,"En cours",null,null,"En cours","59512","ROUBAIX","NORD","HAUTS-DE-FRANCE","Polygone",3.1583474,50.700035,"E13 - Blanchiment, teinture, impression"]
["SSP000139901","59.0390","MIELLET",null,"En cours",null,null,"En cours","59512","ROUBAIX","NORD","HAUTS-DE-FRANCE","Polygone",3.1993454,50.694504,"L - Entreposage, transport, commerce"]
["SSP000140001","59.0391","UNION BISCUITS",null,"En cours",null,null,"En cours","59512","ROUBAIX","NORD","HAUTS-DE-FRANCE","Polygone",3.178793,50.69309,"B1 - Industrie agro-alimentaire"]
["SSP000140101","59.0397","Fonderie HW (ex fonderie Honore)",null,"En cours",null,null,"En cours","59512","ROUBAIX","NORD","HAUTS-DE-FRANCE","Polygone",3.1906903,50.68608,"J51 - Fonderie des métaux ferreux"]
["SSP000140201","59.0398","IMERYS - Tuilerie Huguenot Fénal de Wahagnies",null,"En cours",null,null,"En cours","59630","WAHAGNIES","NORD","HAUTS-DE-FRANCE","Polygone",3.023797,50.4917,"G12 - Fabrication de produits céramiques"]
["SSP000140301","59.0404","WIPAK GRYSPEERT (ancien site)",null,"En cours",null,null,"En cours","59098","BOUSBECQUE","NORD","HAUTS-DE-FRANCE","Polygone",3.062578,50.774273]
["SSP000140401","59.0415","DEPRAT",null,"En cours",null,null,"En cours","59339","LEERS","NORD","HAUTS-DE-FRANCE","Polygone",3.2378223,50.67329,"H13 - Traitement de surface"]
["SSP000140501","59.0420","DIFRAMA",null,"En cours",null,null,"En cours","59339","LEERS","NORD","HAUTS-DE-FRANCE","Polygone",3.2213733,50.68847]
["SSP000140601","59.0432","CHRU de Lille (ex-friche Herbaut)",null,"En cours",null,null,"En cours","59286","HAUBOURDIN","NORD","HAUTS-DE-FRANCE","Polygone",2.9923525,50.608414,"B17 - Autres industries agro-alimentaires"]
["SSP000140701","59.0439","VISTEON SYSTEMES INTERIEURS",null,"En cours",null,null,"En cours","59266","GONDECOURT","NORD","HAUTS-DE-FRANCE","Polygone",2.9890406,50.539177,"D34 - Fabrication de matières plastiques de base"]
["SSP000140801","59.0463","QUALISTOCK",null,"En cours",null,null,"En cours","59585","TEMPLEMARS","NORD","HAUTS-DE-FRANCE","Polygone",3.0707412,50.567837,"L13 - Entrepôts de produits dangereux"]
["SSP000140901","59.0464","PANOFRANCE NORD",null,"En cours",null,null,"En cours","59343","LESQUIN","NORD","HAUTS-DE-FRANCE","Polygone",3.1153648,50.578365,"C13 - Traitement du bois"]
["SSP000141001","59.0467","VRAU",null,"En cours",null,null,"En cours","59350","LILLE","NORD","HAUTS-DE-FRANCE","Polygone",3.0921848,50.643394,"E12 - Filtène, filature, tissage, tricotage"]
["SSP000141101","59.0468","FLANDRE ALUMINIUM",null,"En cours",null,null,"En cours","59350","LILLE","NORD","HAUTS-DE-FRANCE","Polygone",3.0535612,50.621384,"J32 - Métallurgie de l'aluminium"]
["SSP000141201","59.0478","BOSTIK",null,"En cours",null,null,"En cours","59034","AVELIN","NORD","HAUTS-DE-FRANCE","Polygone",3.0932968,50.543816,"D44 - Fabrication de colles et mastics"]
["SSP000141301","59.0481","GUERMONPREZ",null,"En cours",null,null,"En cours","59220","FACHES THUMESNIL","NORD","HAUTS-DE-FRANCE","Polygone",3.0659094,50.603313,"H21 - Imprimerie, presse, édition"]
["SSP000141401","59.0483","GARAGE DU TRIANGLE",null,"En cours",null,null,"En cours","59599","TOURCOING","NORD","HAUTS-DE-FRANCE","Polygone",3.1690164,50.72548,"L21 - Vente et réparation automobile"]
["SSP000141501","59.0484","STEVERLYNCK",null,"En cours",null,null,"En cours","59350","LILLE","NORD","HAUTS-DE-FRANCE","Polygone",3.0440562,50.62548,"D61 - Fabrication de produits savonniers"]
["SSP000141601","59.0487","LE JOINT FRANCAIS",null,"En cours",null,null,"En cours","59512","ROUBAIX","NORD","HAUTS-DE-FRANCE","Polygone",3.1845515,50.686146,"D71 - Industrie du caoutchouc"]
["SSP000141701","59.0156","ARBEL FAUVET RAIL",null,"En cours",null,null,"En cours","59350","LILLE","NORD","HAUTS-DE-FRANCE","Polygone",3.0398452,50.613,"H1 - Mécanique, électrique, traitement de surface"]
["SSP000141801","59.0165","DISTRICHIMIE",null,"En cours",null,null,"En cours","59512","ROUBAIX","NORD","HAUTS-DE-FRANCE","Polygone",3.1664007,50.70603,"L13 - Entrepôts de produits dangereux"]
["SSP000141901","59.0214","RMN",null,"En cours",null,null,"En cours","59256","FRETIN","NORD","HAUTS-DE-FRANCE","Polygone",3.1409438,50.564625,"G23 - Centrales à béton"]
["SSP000142001","59.0238","TRAITEMENTS LAMBIN",null,"En cours",null,null,"En cours","59350","LILLE","NORD","HAUTS-DE-FRANCE","Polygone",3.0078704,50.647915,"H13 - Traitement de surface"]
["SSP000142101","59.0275","HAEGEBAERT-FREMAUX",null,"En cours",null,null,"En cours","59009","VILLENEUVE D'ASCQ","NORD","HAUTS-DE-FRANCE","Polygone",3.124452,50.622585,"D42 - Fabrication de peintures"]
["SSP000142201","59.0306","DUMORTIER FRERES",null,"En cours",null,null,"En cours","59599","TOURCOING","NORD","HAUTS-DE-FRANCE","Polygone",3.1351182,50.719616,"B13 - Huiles et graisses animales ou végétales (industrie de)"]
["SSP000142301","59.0433","CNH Usine de CROIX (ex CASE France)",null,"En cours",null,null,"En cours","59163","CROIX","NORD","HAUTS-DE-FRANCE","Polygone",3.139098,50.67611,"H - Mécanique, traitements des surfaces"]
["SSP000142401","59.0076","ZAC DE RAVENNES LES FRANCS",null,"En cours",null,null,"En cours","59090","BONDUES","NORD","HAUTS-DE-FRANCE","Polygone",3.133499,50.721992,"K36 - Mise en décharge"]
["SSP000142501","59.0474","WILVIA MEUBLEX",null,"En cours",null,null,"En cours","59350","LILLE","NORD","HAUTS-DE-FRANCE","Polygone",2.9968212,50.647114,"C1 - Bois et de l'ameublement (industrie du)"]
["SSP000142601","59.0107","LADOE",null,"En cours",null,null,"En cours","59426","NEUVILLE EN FERRAIN","NORD","HAUTS-DE-FRANCE","Polygone",3.1655087,50.746017,"E11 - Peignage, cardage des fibres textiles"]
["SSP000142801","59.0151","NORD HELIO GRAVURE",null,"En cours",null,null,"En cours","59599","TOURCOING","NORD","HAUTS-DE-FRANCE","Polygone",3.1495075,50.73947,"H13 - Traitement de surface"]
["SSP000142901","59.0276","CORNU",null,"En cours",null,null,"En cours","59646","WASQUEHAL","NORD","HAUTS-DE-FRANCE","Polygone",3.1348655,50.674263,"K5 - Récupération, dépôts de ferrailles"]
["SSP000143101","59.0314","STATION BP DIDEROT",null,"En cours",null,null,"En cours","59350","LILLE","NORD","HAUTS-DE-FRANCE","Polygone",3.0701985,50.622784,"L2 - Transports, automobile, carburants"]
["SSP000143201","59.0342","PEIGNAGE AMEDEE (Miellet)",null,"En cours",null,null,"En cours","59512","ROUBAIX","NORD","HAUTS-DE-FRANCE","Polygone",3.1929107,50.707623,"E11 - Peignage, cardage des fibres textiles"]
["SSP000143301","59.0366","GALLAY SA",null,"En cours",null,null,"En cours","59527","SAINT ANDRE LEZ LILLE","NORD","HAUTS-DE-FRANCE","Polygone",3.0460422,50.655746,"H14 - Application de peinture"]
["SSP000143401","59.0396","SHELL station",null,"En cours",null,null,"En cours","59512","ROUBAIX","NORD","HAUTS-DE-FRANCE","Polygone",3.1823325,50.67172,"L23 - Détail de carburants"]
["SSP000143501","59.0004","usine RHODIA INTERMEDIAIRES (Site sur LA MADELEINE, SAINT-ANDRE et MARQUETTE)",null,"En cours",null,null,"En cours","59368","LA MADELEINE","NORD","HAUTS-DE-FRANCE","Polygone",3.0601573,50.666153,"D3 - Chimie, phytosanitaire, pharmacie"]
["SSP000143601","59.0416","ANCIEN SITE MASSEY-FERGUSON/ SITE BOUVERNE",null,"En cours",null,null,"En cours","59386","MARQUETTE LEZ LILLE","NORD","HAUTS-DE-FRANCE","Polygone",3.0535014,50.67828,"J53 - Travail des métaux, chaudronnerie, poudres"]
["SSP000143701","59.0472","FCB, site du lycée technique",null,"En cours",null,null,"En cours","59350","LILLE","NORD","HAUTS-DE-FRANCE","Polygone",3.1014032,50.62608,"H - Mécanique, traitements des surfaces"]
["SSP000143801","59.0001","EXIDE",null,"En cours",null,null,"En cours","59350","LILLE","NORD","HAUTS-DE-FRANCE","Polygone",3.057288,50.60934,"H16 - Piles électriques et accumulateurs (fabrication de)"]
["SSP000143901","59.0321","WENDERBECQ (Synchrony Logistique)",null,"En cours",null,null,"En cours","59512","ROUBAIX","NORD","HAUTS-DE-FRANCE","Polygone",3.1943684,50.6994,"L22 - Transports"]
["SSP000144001","59.0162","PAINDAVOINE - ZAC DES MARGUERITOIS",null,"En cours",null,null,"En cours","59350","LILLE","NORD","HAUTS-DE-FRANCE","Polygone",3.0672522,50.611073,"H15 - Assemblage, montage"]
["SSP000144101","59.0018","FRICHE RHONE POULENC",null,"En cours",null,null,"En cours","59009","VILLENEUVE D'ASCQ","NORD","HAUTS-DE-FRANCE","Polygone",3.1393855,50.671383,"D - Chimie, parachimie, pétrole"]
["SSP000144201","59.0013","ANCIENNE USINE KUHLMANN",null,"En cours",null,null,"En cours","59650","WATTRELOS","NORD","HAUTS-DE-FRANCE","Polygone",3.2217093,50.691902,"D32 - Chimie minérale inorganique autre"]
["SSP000144301","59.0282","MORY COMBUSTIBLES / VANDERPERRE",null,"En cours",null,null,"En cours","59599","TOURCOING","NORD","HAUTS-DE-FRANCE","Polygone",3.1630697,50.70692,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000144401","59.0137","DEPOT ELF ANTAR PORT DE LILLE",null,"En cours",null,null,"En cours","59360","LOOS","NORD","HAUTS-DE-FRANCE","Polygone",3.019354,50.62336,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000144501","59.0489","MAERTEN",null,"En cours",null,null,"En cours","59586","TEMPLEUVE","NORD","HAUTS-DE-FRANCE","Polygone",3.1635249,50.522526]
["SSP000144701","59.0515","Jules de Surmont et Fils",null,"En cours",null,null,"En cours","59599","TOURCOING","NORD","HAUTS-DE-FRANCE","Polygone",3.1458988,50.715054]
["SSP000144801","59.0516","BEKAERT CARDING SOLUTIONS S.A.S",null,"En cours",null,null,"En cours","59512","ROUBAIX","NORD","HAUTS-DE-FRANCE","Polygone",3.1831992,50.67731,"H1 - Mécanique, électrique, traitement de surface"]
["SSP000144901","59.0508","ONDUCLAIR (ex-STRATINOR)",null,"En cours",null,null,"En cours","59646","WASQUEHAL","NORD","HAUTS-DE-FRANCE","Polygone",3.134457,50.669144]
["SSP000145001","59.0528","COATS FRANCE",null,"En cours",null,null,"En cours","59360","LOOS","NORD","HAUTS-DE-FRANCE","Polygone",3.0210571,50.618942,"E12 - Filtène, filature, tissage, tricotage"]
["SSP000145101","59.0530","COATS FRANCE (Ex DMC)",null,"En cours",null,null,"En cours","59360","LOOS","NORD","HAUTS-DE-FRANCE","Polygone",3.003403,50.61673,"E1 - Textile et habillement, teinture, impression"]
["SSP000145201","59.0531","Décharge Boone Comenor",null,"En cours",null,null,"En cours","59173","DEULEMONT","NORD","HAUTS-DE-FRANCE","Polygone",2.9600205,50.719894,"K21 - Décharges d'ordures ménagères"]
["SSP000145301","59.0534","PROVOST (ancien site rue Emile Zola)",null,"En cours",null,null,"En cours","59279","HALLUIN","NORD","HAUTS-DE-FRANCE","Polygone",3.1249604,50.78417,"J53 - Travail des métaux, chaudronnerie, poudres"]
["SSP000145401","59.0535","SCOWARTON",null,"En cours",null,null,"En cours","59643","WARNETON","NORD","HAUTS-DE-FRANCE","Polygone",2.9503622,50.750534,"E1 - Textile et habillement, teinture, impression"]
["SSP000145501","59.0536","NALCO France",null,"En cours",null,null,"En cours","59646","WASQUEHAL","NORD","HAUTS-DE-FRANCE","Polygone",3.1445525,50.69192,"D3 - Chimie, phytosanitaire, pharmacie"]
["SSP000145601","59.0537","PACOFA",null,"En cours",null,null,"En cours","59279","HALLUIN","NORD","HAUTS-DE-FRANCE","Polygone",3.1146388,50.78602,"C2 - Industrie du papier et du carton"]
["SSP000145701",null,"Ancienne décharge du bas du Bourg",null,"Clôturée",null,null,"Clôturée","22088","KERIEN","COTES-D'ARMOR","BRETAGNE","Polygone",-3.2131913,48.39443]
["SSP000145801",null,"Ancienne décharge de Saint Norgant",null,"Clôturée",null,null,"Clôturée","22088","KERIEN","COTES-D'ARMOR","BRETAGNE","Polygone",-3.2611995,48.413296]
["SSP000146001",null,"Ancienne décharge de la Poterie",null,"Clôturée",null,null,"Clôturée","22093","LAMBALLE","COTES-D'ARMOR","BRETAGNE","Polygone",-2.470107,48.479446]
["SSP000146101",null,"Ancienne décharge des Bruyères",null,"Clôturée",null,null,"Clôturée","22098","LANDEHEN","COTES-D'ARMOR","BRETAGNE","Polygone",-2.5473464,48.4256]
["SSP000146201",null,"Ancienne décharge des Roselais",null,"Clôturée",null,null,"Clôturée","22099","LANFAINS","COTES-D'ARMOR","BRETAGNE","Polygone",-2.9081693,48.351818]
["SSP000146401",null,"Ancienne décharge de Kergreiz",null,"Clôturée",null,null,"Clôturée","22107","LANISCAT","COTES-D'ARMOR","BRETAGNE","Polygone",-3.107118,48.238125]
["SSP000146601",null,"Ancienne décharge du Bois Thomas",null,"Clôturée",null,null,"Clôturée","22113","LANNION","COTES-D'ARMOR","BRETAGNE","Polygone",-3.4107013,48.725456]
["SSP000146701",null,"Ancienne décharge de La Raslais",null,"Clôturée",null,null,"Clôturée","22114","LANRELAS","COTES-D'ARMOR","BRETAGNE","Polygone",-2.275411,48.2228]
["SSP000146901",null,"Ancienne décharge des Rochettes",null,"Clôturée",null,null,"Clôturée","22118","LANVALLAY","COTES-D'ARMOR","BRETAGNE","Polygone",-2.0372114,48.44456]
["SSP000147001",null,"Ancienne décharge du Moulin du Corré",null,"Clôturée",null,null,"Clôturée","22121","LANVOLLON","COTES-D'ARMOR","BRETAGNE","Polygone",-2.997039,48.627712]
["SSP000147101",null,"Ancienne décharge du Pont de Quévran",null,"Clôturée",null,null,"Clôturée","22122","LAURENAN","COTES-D'ARMOR","BRETAGNE","Polygone",-2.5389085,48.202675]
["SSP000147201",null,"Ancienne décharge de Keryvon",null,"Clôturée",null,null,"Clôturée","22124","LESCOUET GOUAREC","COTES-D'ARMOR","BRETAGNE","Polygone",-3.223531,48.160717]
["SSP000147301",null,"Ancienne décharge de Pommelin",null,"Clôturée",null,null,"Clôturée","22127","LEZARDRIEUX","COTES-D'ARMOR","BRETAGNE","Polygone",-3.1008863,48.827904]
["SSP000147501",null,"Ancienne décharge de Porz-Meur",null,"Clôturée",null,null,"Clôturée","22131","LOGUIVY PLOUGRAS","COTES-D'ARMOR","BRETAGNE","Polygone",-3.496576,48.53341]
["SSP000147601",null,"Ancienne décharge de Kersamson - Convenant Pont",null,"Clôturée",null,null,"Clôturée","22134","LOUANNEC","COTES-D'ARMOR","BRETAGNE","Polygone",-3.4009936,48.7751]
["SSP000147801",null,"Ancienne décharge de Pont Cam",null,"Clôturée",null,null,"Clôturée","22137","MAEL CARHAIX","COTES-D'ARMOR","BRETAGNE","Polygone",-3.4288125,48.263184]
["SSP000147901",null,"Ancienne décharge de Keriou",null,"Clôturée",null,null,"Clôturée","22139","MAGOAR","COTES-D'ARMOR","BRETAGNE","Polygone",-3.1651235,48.417118]
["SSP000148001",null,"Ancienne décharge de la Forge",null,"Clôturée",null,null,"Clôturée","22145","MEGRIT","COTES-D'ARMOR","BRETAGNE","Polygone",-2.2791338,48.396828]
["SSP000148201",null,"Ancienne décharge de Kervanno",null,"Clôturée",null,null,"Clôturée","22150","LE MERZER","COTES-D'ARMOR","BRETAGNE","Polygone",-3.099657,48.57779]
["SSP000148401",null,"Ancienne décharge de Pont Rolland",null,"Clôturée",null,null,"Clôturée","22154","MORIEUX","COTES-D'ARMOR","BRETAGNE","Polygone",-2.6200147,48.520897]
["SSP000148501",null,"Ancienne décharge de La Croix Jartel",null,"Clôturée",null,null,"Clôturée","22155","LA MOTTE","COTES-D'ARMOR","BRETAGNE","Polygone",-2.727358,48.232613]
["SSP000148601",null,"Ancienne décharge du Bongoat",null,"Clôturée",null,null,"Clôturée","22156","MOUSTERU","COTES-D'ARMOR","BRETAGNE","Polygone",-2.8096542,48.52435]
["SSP000148701",null,"Ancienne décharge de Kerprigent",null,"Clôturée",null,null,"Clôturée","22166","PENVENAN","COTES-D'ARMOR","BRETAGNE","Polygone",-3.2821639,48.80546]
["SSP000148901",null,"Ancienne décharge de L'Ejuhel",null,"Clôturée",null,null,"Clôturée","22173","PLANGUENOUAL","COTES-D'ARMOR","BRETAGNE","Polygone",-2.5723207,48.55107]
["SSP000149101",null,"Ancienne décharge de Kervénou",null,"Clôturée",null,null,"Clôturée","22177","PLEGUIEN","COTES-D'ARMOR","BRETAGNE","Polygone",-2.9557176,48.64181]
["SSP000149201",null,"Ancienne décharge de Barach",null,"Clôturée",null,null,"Clôturée","22181","PLELAUFF","COTES-D'ARMOR","BRETAGNE","Polygone",-3.2161088,48.20044]
["SSP000149301",null,"Ancienne décharge de La Ville Even",null,"Clôturée",null,null,"Clôturée","22182","PLELO","COTES-D'ARMOR","BRETAGNE","Polygone",-2.9269347,48.553196]
["SSP000149401",null,"Ancienne décharge du Long Réage",null,"Clôturée",null,null,"Clôturée","22182","PLELO","COTES-D'ARMOR","BRETAGNE","Polygone",-2.918285,48.540855]
["SSP000149501",null,"Ancienne décharge du Hambo",null,"Clôturée",null,null,"Clôturée","22183","PLEMET","COTES-D'ARMOR","BRETAGNE","Polygone",-2.5429814,48.1809]
["SSP000149601",null,"Ancienne décharge de Mille Motte",null,"Clôturée",null,null,"Clôturée","22186","PLENEUF VAL ANDRE","COTES-D'ARMOR","BRETAGNE","Polygone",-2.519888,48.572735]
["SSP000149701",null,"Ancienne décharge de la Ville Gervaux",null,"Clôturée",null,null,"Clôturée","22187","PLERIN","COTES-D'ARMOR","BRETAGNE","Polygone",-2.7645085,48.548126]
["SSP000149801",null,"Ancienne décharge de Quercy",null,"Clôturée",null,null,"Clôturée","22193","PLESTAN","COTES-D'ARMOR","BRETAGNE","Polygone",-2.3978257,48.419285]
["SSP000149901",null,"Ancienne décharge de Goasorguen",null,"Clôturée",null,null,"Clôturée","22194","PLESTIN LES GREVES","COTES-D'ARMOR","BRETAGNE","Polygone",-3.5866094,48.634315]
["SSP000150001",null,"Ancien stockage de déchets de marées noires et ancienne décharge de Keraliès",null,"Clôturée",null,null,"Clôturée","22198","PLEUMEUR BODOU","COTES-D'ARMOR","BRETAGNE","Polygone",-3.5317838,48.802326]
["SSP000150101",null,"Ancienne décharge de Kerlogoden",null,"Clôturée",null,null,"Clôturée","22199","PLEUMEUR GAUTIER","COTES-D'ARMOR","BRETAGNE","Polygone",-3.1440372,48.797676]
["SSP000150201",null,"Ancienne décharge de Minez Zant Yann",null,"Clôturée",null,null,"Clôturée","22202","PLEVIN","COTES-D'ARMOR","BRETAGNE","Polygone",-3.4904623,48.211227]
["SSP000150301",null,"Ancienne décharge du Tertre Loyer",null,"Clôturée",null,null,"Clôturée","22171","PLAINTEL","COTES-D'ARMOR","BRETAGNE","Polygone",-2.801992,48.439064]
["SSP000150401",null,"Ancienne décharge de la Berthaudière",null,"Clôturée",null,null,"Clôturée","22171","PLAINTEL","COTES-D'ARMOR","BRETAGNE","Polygone",-2.819005,48.39385]
["SSP000150501",null,"Ancienne décharge de la Bécane",null,"Clôturée",null,null,"Clôturée","22203","PLOEUC SUR LIE","COTES-D'ARMOR","BRETAGNE","Polygone",-2.8047316,48.323547]
["SSP000150701",null,"Ancienne décharge de Saint-Mathieu",null,"Clôturée",null,null,"Clôturée","22207","PLOUARET","COTES-D'ARMOR","BRETAGNE","Polygone",-3.483975,48.58208]
["SSP000150801",null,"Ancienne décharge du Traou",null,"Clôturée",null,null,"Clôturée","22210","PLOUBAZLANEC","COTES-D'ARMOR","BRETAGNE","Polygone",-3.0627646,48.78863]
["SSP000150901",null,"Ancienne décharge de Lan Meur",null,"Clôturée",null,null,"Clôturée","22216","PLOUGONVER","COTES-D'ARMOR","BRETAGNE","Polygone",-3.3519046,48.48498]
["SSP000151001",null,"Ancienne décharge de Questel",null,"Clôturée",null,null,"Clôturée","22220","PLOUGUERNEVEL","COTES-D'ARMOR","BRETAGNE","Polygone",-3.246417,48.20296]
["SSP000151101",null,"Ancienne décharge de Créven",null,"Clôturée",null,null,"Clôturée","22221","PLOUGUIEL","COTES-D'ARMOR","BRETAGNE","Polygone",-3.2553215,48.789444]
["SSP000151201",null,"Ancienne décharge de Poull Fanc",null,"Clôturée",null,null,"Clôturée","22222","PLOUHA","COTES-D'ARMOR","BRETAGNE","Polygone",-2.956424,48.686226]
["SSP000151301",null,"Ancienne décharge de la Croix Prigent",null,"Clôturée",null,null,"Clôturée","22225","PLOUMAGOAR","COTES-D'ARMOR","BRETAGNE","Polygone",-3.1027832,48.5276]
["SSP000151401",null,"Station-service AVIA-RASPAIL",null,"Clôturée",null,null,"Clôturée","75107","PARIS 7E ARRONDISSEMENT","PARIS","ILE-DE-FRANCE","Polygone",2.3254526,48.85488]
["SSP000151501",null,"Ancienne décharge de Guerguilléguen",null,"Clôturée",null,null,"Clôturée","22226","PLOUMILLIAU","COTES-D'ARMOR","BRETAGNE","Polygone",-3.5445695,48.688435]
["SSP000151601",null,"Ancienne décharge de Poul Breiz",null,"Clôturée",null,null,"Clôturée","22229","PLOUNEVEZ QUINTIN","COTES-D'ARMOR","BRETAGNE","Polygone",-3.2318852,48.275948]
["SSP000151701",null,"Ancienne décharge du bourg",null,"Clôturée",null,null,"Clôturée","22233","PLOURIVO","COTES-D'ARMOR","BRETAGNE","Polygone",-3.0705624,48.746296]
["SSP000151801",null,"Ancienne décharge de la Ville Davy",null,"Clôturée",null,null,"Clôturée","22237","PLUDUNO","COTES-D'ARMOR","BRETAGNE","Polygone",-2.3185096,48.51191]
["SSP000151901",null,"Ancienne décharge des Champs Deniaux",null,"Clôturée",null,null,"Clôturée","22239","PLUMAUDAN","COTES-D'ARMOR","BRETAGNE","Polygone",-2.1353178,48.383774]
["SSP000152001",null,"Ancienne décharge du Bruhalier",null,"Clôturée",null,null,"Clôturée","22242","PLURIEN","COTES-D'ARMOR","BRETAGNE","Polygone",-2.415905,48.619064]
["SSP000152201",null,"Ancienne décharge de Kerguen",null,"Clôturée",null,null,"Clôturée","22247","POMMERIT JAUDY","COTES-D'ARMOR","BRETAGNE","Polygone",-3.2219303,48.716873]
["SSP000152301",null,"Ancienne décharge de Dour Goas Hallec",null,"Clôturée",null,null,"Clôturée","22249","PONT MELVEZ","COTES-D'ARMOR","BRETAGNE","Polygone",-3.2742174,48.45982]
["SSP000152401",null,"Ancienne décharge de Pen Suler",null,"Clôturée",null,null,"Clôturée","22249","PONT MELVEZ","COTES-D'ARMOR","BRETAGNE","Polygone",-3.27545,48.481766]
["SSP000152501",null,"Ancienne décharge de la Ville Calard",null,"Clôturée",null,null,"Clôturée","22251","PORDIC","COTES-D'ARMOR","BRETAGNE","Polygone",-2.8654425,48.56839]
["SSP000152701",null,"Ancienne décharge de Kerbrézellic",null,"Clôturée",null,null,"Clôturée","22256","QUEMPER GUEZENNEC","COTES-D'ARMOR","BRETAGNE","Polygone",-3.1138217,48.71651]
["SSP000152801",null,"Ancienne décharge de Kergozou",null,"Clôturée",null,null,"Clôturée","22256","QUEMPER GUEZENNEC","COTES-D'ARMOR","BRETAGNE","Polygone",-3.1390743,48.693226]
["SSP000153001",null,"Ancienne décharge du Rocher Merlin",null,"Clôturée",null,null,"Clôturée","22260","LE QUILLIO","COTES-D'ARMOR","BRETAGNE","Polygone",-2.9168718,48.23725]
["SSP000153101",null,"Ancienne décharge de Goasper",null,"Clôturée",null,null,"Clôturée","22265","ROSPEZ","COTES-D'ARMOR","BRETAGNE","Polygone",-3.3885865,48.731842]
["SSP000153201",null,"Ancienne décharge de Kéringant",null,"Clôturée",null,null,"Clôturée","22266","ROSTRENEN","COTES-D'ARMOR","BRETAGNE","Polygone",-3.2958012,48.227066]
["SSP000153301",null,"Ancienne décharge de Kermélin",null,"Clôturée",null,null,"Clôturée","22267","ROUILLAC","COTES-D'ARMOR","BRETAGNE","Polygone",-2.3726373,48.292377]
["SSP000153401",null,"Ancienne décharge de Frameur",null,"Clôturée",null,null,"Clôturée","22275","SAINT BARNABE","COTES-D'ARMOR","BRETAGNE","Polygone",-2.6717792,48.14483]
["SSP000153501",null,"Ancienne décharge de la Jaloussée",null,"Clôturée",null,null,"Clôturée","22277","SAINT BRANDAN","COTES-D'ARMOR","BRETAGNE","Polygone",-2.8654618,48.394287]
["SSP000153601",null,"Ancienne décharge de la Ville Jegu",null,"Clôturée",null,null,"Clôturée","22279","SAINT CARADEC","COTES-D'ARMOR","BRETAGNE","Polygone",-2.8346632,48.184536]
["SSP000153701",null,"Ancienne décharge de La Cotte à Bouffi",null,"Clôturée",null,null,"Clôturée","22281","SAINT CARREUC","COTES-D'ARMOR","BRETAGNE","Polygone",-2.7557852,48.40443]
["SSP000153801",null,"Ancienne décharge de La Cour",null,"Clôturée",null,null,"Clôturée","22282","SAINT CAST LE GUILDO","COTES-D'ARMOR","BRETAGNE","Polygone",-2.261568,48.605145]
["SSP000153901",null,"Ancienne décharge de la lande du Goheu",null,"Clôturée",null,null,"Clôturée","22285","SAINT CONNEC","COTES-D'ARMOR","BRETAGNE","Polygone",-2.907235,48.174034]
["SSP000154001",null,"Ancienne décharge des Granges",null,"Clôturée",null,null,"Clôturée","22290","SAINT GELVEN","COTES-D'ARMOR","BRETAGNE","Polygone",-3.1017196,48.21927]
["SSP000154101",null,"Ancienne décharge de Keravel",null,"Clôturée",null,null,"Clôturée","22294","SAINT GILLES PLIGEAUX","COTES-D'ARMOR","BRETAGNE","Polygone",-3.0881782,48.3656]
["SSP000154201",null,"Ancienne décharge de la Lande",null,"Clôturée",null,null,"Clôturée","22298","SAINT GUEN","COTES-D'ARMOR","BRETAGNE","Polygone",-2.947056,48.218628]
["SSP000154501",null,"Ancienne décharge de Cabrac",null,"Clôturée",null,null,"Clôturée","22306","SAINT JUDOCE","COTES-D'ARMOR","BRETAGNE","Polygone",-1.9522836,48.36084]
["SSP000154801",null,"Ancienne décharge de Cussuliou",null,"Clôturée",null,null,"Clôturée","22321","SAINT NICOLAS DU PELEM","COTES-D'ARMOR","BRETAGNE","Polygone",-3.1858146,48.30937]
["SSP000155001",null,"Ancienne décharge de La Livraudais",null,"Clôturée",null,null,"Clôturée","22326","SAINT RIEUL","COTES-D'ARMOR","BRETAGNE","Polygone",-2.432573,48.443283]
["SSP000155101",null,"Ancienne décharge de Kerparquic",null,"Clôturée",null,null,"Clôturée","22328","SAINT SERVAIS","COTES-D'ARMOR","BRETAGNE","Polygone",-3.383515,48.356213]
["SSP000155201",null,"Ancienne décharge du Pré Guelnée",null,"Clôturée",null,null,"Clôturée","22330","SAINT THELO","COTES-D'ARMOR","BRETAGNE","Polygone",-2.857026,48.23476]
["SSP000155401",null,"Ancienne décharge de Toul Ar Woas",null,"Clôturée",null,null,"Clôturée","22343","TREBEURDEN","COTES-D'ARMOR","BRETAGNE","Polygone",-3.54952,48.768898]
["SSP000155501",null,"Ancienne décharge de Bellevue",null,"Clôturée",null,null,"Clôturée","22344","TREBRIVAN","COTES-D'ARMOR","BRETAGNE","Polygone",-3.4874494,48.30414]
["SSP000155701",null,"Ancienne décharge de Pellem",null,"Clôturée",null,null,"Clôturée","22359","TREGROM","COTES-D'ARMOR","BRETAGNE","Polygone",-3.4006076,48.618313]
["SSP000155801",null,"Ancienne décharge de Kéribot",null,"Clôturée",null,null,"Clôturée","22363","TRELEVERN","COTES-D'ARMOR","BRETAGNE","Polygone",-3.359492,48.794395]
["SSP000155901","37.0044","LA NOUVELLE REPUBLIQUE DU CENTRE OUEST",null,"En cours",null,null,"En cours","37261","TOURS","INDRE-ET-LOIRE","CENTRE-VAL DE LOIRE","Polygone",0.69713163,47.375244]
["SSP000156001",null,"Station-Service ESSO SAINT-MARTIN",null,"Clôturée",null,null,"Clôturée","75110","PARIS 10E ARRONDISSEMENT","PARIS","ILE-DE-FRANCE","Polygone",2.3618493,48.8769]
["SSP000156101",null,"Ancienne décharge de la Grande Rivonnais",null,"Clôturée",null,null,"Clôturée","22364","TRELIVAN","COTES-D'ARMOR","BRETAGNE","Polygone",-2.1268632,48.421623]
["SSP000156201",null,"Ancienne décharge du Vau Ruzé",null,"Clôturée",null,null,"Clôturée","22369","TREMEUR","COTES-D'ARMOR","BRETAGNE","Polygone",-2.282258,48.371517]
["SSP000156301",null,"Ancienne décharge de la Côte Thomine",null,"Clôturée",null,null,"Clôturée","22372","TREMUSON","COTES-D'ARMOR","BRETAGNE","Polygone",-2.8408773,48.516247]
["SSP000156401","37.0042","TOTAL - Relais St Avertin",null,"En cours",null,null,"En cours","37208","SAINT AVERTIN","INDRE-ET-LOIRE","CENTRE-VAL DE LOIRE","Polygone",0.72843635,47.36878,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000156501",null,"Ancienne décharge de Kerbéha",null,"Clôturée",null,null,"Clôturée","22376","TREVE","COTES-D'ARMOR","BRETAGNE","Polygone",-2.7814896,48.2156]
["SSP000156601",null,"Ancienne décharge de la Ville Herry",null,"Clôturée",null,null,"Clôturée","22385","LA VICOMTE SUR RANCE","COTES-D'ARMOR","BRETAGNE","Polygone",-1.9794673,48.496727]
["SSP000156701",null,"Ancienne décharge des Hauts Champs",null,"Clôturée",null,null,"Clôturée","22388","VILDE GUINGALAN","COTES-D'ARMOR","BRETAGNE","Polygone",-2.14547,48.43477]
["SSP000156801",null,"Ancienne décharge de la Haute Lande",null,"Clôturée",null,null,"Clôturée","22389","YFFINIAC","COTES-D'ARMOR","BRETAGNE","Polygone",-2.688065,48.463367]
["SSP000156901",null,"Ancienne décharge du Haut Plouha",null,"Clôturée",null,null,"Clôturée","22391","YVIGNAC LA TOUR","COTES-D'ARMOR","BRETAGNE","Polygone",-2.18629,48.343838]
["SSP000157001",null,"Ancienne décharge de Chaudrée",null,"Clôturée",null,null,"Clôturée","35167","MARTIGNE FERCHAUD","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.3376784,47.850536]
["SSP000157101",null,"Ancienne décharge de Launay Brunard",null,"Clôturée",null,null,"Clôturée","35168","MAURE DE BRETAGNE","ILLE-ET-VILAINE","BRETAGNE","Polygone",-2.001909,47.906372]
["SSP000157301",null,"Ancienne décharge de Lauviais",null,"Clôturée",null,null,"Clôturée","35172","MEILLAC","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.8693976,48.426]
["SSP000157401",null,"Ancienne décharge de la Lande Cormeré",null,"Clôturée",null,null,"Clôturée","35176","MESSAC","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.8228347,47.810787]
["SSP000157501",null,"Ancienne décharge du Bodel",null,"Clôturée",null,null,"Clôturée","35176","MESSAC","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.7909799,47.81428]
["SSP000157601",null,"Ancienne décharge du Faux",null,"Clôturée",null,null,"Clôturée","35176","MESSAC","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.7838253,47.823505]
["SSP000157701",null,"Ancienne décharge de la Gomeriais",null,"Clôturée",null,null,"Clôturée","35178","MEZIERES SUR COUESNON","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.4381776,48.300175]
["SSP000158001",null,"Station-service AAS CARBURANTS",null,"Clôturée",null,null,"Clôturée","75104","PARIS 4E ARRONDISSEMENT","PARIS","ILE-DE-FRANCE","Polygone",2.36569,48.848137]
["SSP000158201",null,"Ancienne décharge de l'Epinay",null,"Clôturée",null,null,"Clôturée","35195","MONTREUIL SUR ILLE","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.6631296,48.326252]
["SSP000158301",null,"Ancienne décharge de la Haie de Saules",null,"Clôturée",null,null,"Clôturée","35197","MOUAZE","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.6223193,48.22829]
["SSP000158601","75.0011","GSTS QUALITE OR",null,"En cours",null,null,"En cours","75056","PARIS","PARIS","ILE-DE-FRANCE","Polygone",2.3616076,48.86252,"H13 - Traitement de surface"]
["SSP000158701","59.0016","BERRY DECOR",null,"En cours",null,null,"En cours","59098","BOUSBECQUE","NORD","HAUTS-DE-FRANCE","Polygone",3.072548,50.77477,"C23 - Transformation de papiers et carton"]
["SSP000158801",null,"Ancienne décharge des Buttes de la Roche Heulin",null,"Clôturée",null,null,"Clôturée","35207","NOYAL SUR VILAINE","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.4513341,48.088867]
["SSP000159001","75.0012","CPCU VILLETTE",null,"En cours",null,null,"En cours","75056","PARIS","PARIS","ILE-DE-FRANCE","Polygone",2.3842416,48.890038,"I21 - Chaufferies urbaines"]
["SSP000159201","75.0007","ex SOCIETE DECORELEC",null,"En cours",null,null,"En cours","75056","PARIS","PARIS","ILE-DE-FRANCE","Polygone",2.3891902,48.88742,"H - Mécanique, traitements des surfaces"]
["SSP000159901",null,"Ancienne décharge de Maigressec",null,"Clôturée",null,null,"Clôturée","35282","SAINT JEAN SUR COUESNON","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.330001,48.276493]
["SSP000160001",null,"Ancienne décharge du Poussier",null,"Clôturée",null,null,"Clôturée","35287","SAINT LUNAIRE","ILLE-ET-VILAINE","BRETAGNE","Polygone",-2.1078422,48.62675]
["SSP000160301",null,"Ancienne décharge de la Brohardais",null,"Clôturée",null,null,"Clôturée","35289","SAINT MALO DE PHILY","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.7838761,47.848534]
["SSP000160401",null,"Ancienne décharge de la Marette",null,"Clôturée",null,null,"Clôturée","35290","SAINT MALON SUR MEL","ILLE-ET-VILAINE","BRETAGNE","Polygone",-2.1078413,48.080063]
["SSP000160501",null,"Ancienne décharge de La Vallée Olive",null,"Clôturée",null,null,"Clôturée","35292","SAINT MARC LE BLANC","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.3963656,48.362244]
["SSP000160801",null,"Ancienne décharge du Champ Doyen",null,"Clôturée",null,null,"Clôturée","35296","SAINT MEDARD SUR ILLE","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.6595529,48.27504]
["SSP000161001",null,"Ancienne décharge de la Rofinière",null,"Clôturée",null,null,"Clôturée","35304","SAINT OUEN DES ALLEUX","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.4746733,48.324364]
["SSP000161101",null,"Ancienne décharge de Moulin Bouri",null,"Clôturée",null,null,"Clôturée","35311","SAINT SEGLIN","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.9999459,47.854675]
["SSP000161201",null,"Ancienne décharge de la Chapelle du Percheot",null,"Clôturée",null,null,"Clôturée","35312","SAINT SENOUX","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.7864771,47.917118]
["SSP000161301",null,"Ancienne décharge des Vallées",null,"Clôturée",null,null,"Clôturée","35318","SAINT THUAL","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.9192356,48.332314]
["SSP000161401",null,"Ancienne décharge de la Croix Goyet",null,"Clôturée",null,null,"Clôturée","35319","SAINT THURIAL","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.9344562,48.0364,"K21 - Décharges d'ordures ménagères"]
["SSP000161501",null,"Ancienne décharge des Oriais",null,"Clôturée",null,null,"Clôturée","35321","SAULNIERES","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.5818485,47.90841]
["SSP000161601",null,"Ancienne décharge de la Thebaudais",null,"Clôturée",null,null,"Clôturée","35332","TEILLAY","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.516562,47.805996]
["SSP000161801",null,"Les Garages Modernes de Paris",null,"Clôturée",null,null,"Clôturée","75117","PARIS 17E ARRONDISSEMENT","PARIS","ILE-DE-FRANCE","Polygone",2.30517,48.88966]
["SSP000162001",null,"Ancienne décharge des Landelles",null,"Clôturée",null,null,"Clôturée","35344","TRESSE","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.8799819,48.481606]
["SSP000162201","69.0007","TECHNICOR",null,"En cours",null,null,"En cours","69275","DECINES CHARPIEU","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.9400373,45.75443]
["SSP000162301",null,"DELEK FRANCE",null,"Clôturée",null,null,"Clôturée","75117","PARIS 17E ARRONDISSEMENT","PARIS","ILE-DE-FRANCE","Polygone",2.312128,48.896343]
["SSP000162401",null,"Ancienne décharge de La Lande de Pavée",null,"Clôturée",null,null,"Clôturée","35355","VIEUX VY SUR COUESNON","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.4780544,48.33307]
["SSP000162801",null,"Ancienne décharge de la Lande Coëtquen",null,"Clôturée",null,null,"Clôturée","35225","PLESDER","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.9216918,48.43224]
["SSP000162901",null,"Ancienne décharge du Tertre de la Chesnelais",null,"Clôturée",null,null,"Clôturée","35227","PLEUMELEUC","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.8924553,48.157536]
["SSP000163001",null,"Ancienne décharge de la Berlaudais",null,"Clôturée",null,null,"Clôturée","35231","POLIGNE","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.6924306,47.8993]
["SSP000163201",null,"Ancienne décharge de Saint-Seliac",null,"Clôturée",null,null,"Clôturée","35233","QUEBRIAC","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.8102323,48.35507]
["SSP000163701",null,"Ancienne décharge du Bois au Coq",null,"Clôturée",null,null,"Clôturée","35246","ROZ LANDRIEUX","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.7896364,48.531147]
["SSP000163801",null,"Ancienne décharge des Burons",null,"Clôturée",null,null,"Clôturée","35246","ROZ LANDRIEUX","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.8259836,48.538677]
["SSP000164101",null,"Ancienne décharge du Tertre",null,"Clôturée",null,null,"Clôturée","35274","SAINT GERMAIN SUR ILLE","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.6635463,48.249146]
["SSP000164201",null,"Ancienne décharge du Cruel",null,"Clôturée",null,null,"Clôturée","35274","SAINT GERMAIN SUR ILLE","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.6452937,48.25783]
["SSP000164301",null,"Ancienne décharge du Pont Roinel",null,"Clôturée",null,null,"Clôturée","22371","TREMOREL","COTES-D'ARMOR","BRETAGNE","Polygone",-2.30433,48.209442]
["SSP000164401",null,"Ancienne décharge de la Fontaine Saint Conogan",null,"Clôturée",null,null,"Clôturée","22373","TREOGAN","COTES-D'ARMOR","BRETAGNE","Polygone",-3.5257561,48.18997]
["SSP000164501",null,"Station de distribution gare de triage de Vaires sur Marne  (SNCF)",null,"Clôturée",null,null,"Clôturée","77108","CHELLES","SEINE-ET-MARNE","ILE-DE-FRANCE","Polygone",2.6114686,48.87345]
["SSP000164601",null,"Ancienne décharge du Bourg",null,"Clôturée",null,null,"Clôturée","22375","TRESSIGNAUX","COTES-D'ARMOR","BRETAGNE","Polygone",-2.9800906,48.613934]
["SSP000164701",null,"Ancienne décharge des Ecobués",null,"Clôturée",null,null,"Clôturée","22376","TREVE","COTES-D'ARMOR","BRETAGNE","Polygone",-2.7877584,48.228695]
["SSP000164901",null,"Ancienne décharge de Kerlan",null,"Clôturée",null,null,"Clôturée","22377","TREVENEUC","COTES-D'ARMOR","BRETAGNE","Polygone",-2.8785632,48.661224]
["SSP000165101",null,"Ancienne décharge de Mézéhier",null,"Clôturée",null,null,"Clôturée","22378","TREVEREC","COTES-D'ARMOR","BRETAGNE","Polygone",-3.041334,48.65673]
["SSP000165201",null,"Hanier Plaisance",null,"Clôturée",null,null,"Clôturée","94076","VILLEJUIF","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.356237,48.799618]
["SSP000165301",null,"Ancienne décharge de Cose Trevenou",null,"Clôturée",null,null,"Clôturée","22379","TREVOU TREGUIGNEC","COTES-D'ARMOR","BRETAGNE","Polygone",-3.3529167,48.802677]
["SSP000165501",null,"Ancienne décharge de Ker An Har",null,"Clôturée",null,null,"Clôturée","22381","TREZENY","COTES-D'ARMOR","BRETAGNE","Polygone",-3.355327,48.755116]
["SSP000165601",null,"Ancienne décharge de La Roche aux Coucous",null,"Clôturée",null,null,"Clôturée","22384","UZEL","COTES-D'ARMOR","BRETAGNE","Polygone",-2.8524146,48.27577]
["SSP000165701",null,"Galvano Force Industrie",null,"Clôturée",null,null,"Clôturée","75111","PARIS 11E ARRONDISSEMENT","PARIS","ILE-DE-FRANCE","Polygone",2.3712752,48.865177]
["SSP000165801",null,"Ancienne décharge du Jard",null,"Clôturée",null,null,"Clôturée","22388","VILDE GUINGALAN","COTES-D'ARMOR","BRETAGNE","Polygone",-2.1511204,48.441933]
["SSP000165901",null,"Ancienne décharge de la Ville Guérinelle",null,"Clôturée",null,null,"Clôturée","22389","YFFINIAC","COTES-D'ARMOR","BRETAGNE","Polygone",-2.7227838,48.472675]
["SSP000166001",null,"Ancienne décharge de Pen an Croic'h",null,"Clôturée",null,null,"Clôturée","22390","YVIAS","COTES-D'ARMOR","BRETAGNE","Polygone",-3.0691233,48.714573]
["SSP000166101",null,"Ancienne décharge de Lannouée",null,"Clôturée",null,null,"Clôturée","22391","YVIGNAC LA TOUR","COTES-D'ARMOR","BRETAGNE","Polygone",-2.159787,48.38698]
["SSP000166201",null,"ERDF",null,"Clôturée",null,null,"Clôturée","75111","PARIS 11E ARRONDISSEMENT","PARIS","ILE-DE-FRANCE","Polygone",2.3959477,48.853176]
["SSP000166301",null,"Ancienne décharge du Mont Gicquel",null,"Clôturée",null,null,"Clôturée","22332","SAINT TRIMOEL","COTES-D'ARMOR","BRETAGNE","Polygone",-2.5330145,48.39537]
["SSP000166401",null,"Ancienne décharge du Pont de Kermartail",null,"Clôturée",null,null,"Clôturée","22331","SAINTE TREPHINE","COTES-D'ARMOR","BRETAGNE","Polygone",-3.1486886,48.269512]
["SSP000166501",null,"Ancienne décharge de Prajou Bras",null,"Clôturée",null,null,"Clôturée","22335","SENVEN LEHART","COTES-D'ARMOR","BRETAGNE","Polygone",-3.0855784,48.439922]
["SSP000166601",null,"Ancienne décharge de Leurmin",null,"Clôturée",null,null,"Clôturée","22335","SENVEN LEHART","COTES-D'ARMOR","BRETAGNE","Polygone",-3.0733378,48.442165]
["SSP000166701",null,"Ancienne décharge de Rochereuil",null,"Clôturée",null,null,"Clôturée","22337","SEVIGNAC","COTES-D'ARMOR","BRETAGNE","Polygone",-2.3608866,48.325417]
["SSP000166901",null,"Ancienne décharge de Trelino",null,"Clôturée",null,null,"Clôturée","22338","SQUIFFIEC","COTES-D'ARMOR","BRETAGNE","Polygone",-3.1551945,48.647198]
["SSP000167101",null,"Ancienne décharge de Ker Meur",null,"Clôturée",null,null,"Clôturée","22340","TONQUEDEC","COTES-D'ARMOR","BRETAGNE","Polygone",-3.4187431,48.697475]
["SSP000167201",null,"Ancienne décharge de Prat An Colay",null,"Clôturée",null,null,"Clôturée","22340","TONQUEDEC","COTES-D'ARMOR","BRETAGNE","Polygone",-3.396362,48.67206]
["SSP000167301",null,"Ancienne décharge du Tertre de Lessien",null,"Clôturée",null,null,"Clôturée","22341","TRAMAIN","COTES-D'ARMOR","BRETAGNE","Polygone",-2.3909938,48.39967]
["SSP000167401",null,"Ancienne décharge des Landes",null,"Clôturée",null,null,"Clôturée","22342","TREBEDAN","COTES-D'ARMOR","BRETAGNE","Polygone",-2.1707754,48.39433]
["SSP000167501",null,"Ancienne décharge de La Ville Blanche",null,"Clôturée",null,null,"Clôturée","22345","TREBRY","COTES-D'ARMOR","BRETAGNE","Polygone",-2.5634377,48.36657]
["SSP000167601",null,"Ancienne décharge de La Ville Moisan",null,"Clôturée",null,null,"Clôturée","22346","TREDANIEL","COTES-D'ARMOR","BRETAGNE","Polygone",-2.5961194,48.35484]
["SSP000167701",null,"Ancienne décharge de Sainte Marguerite",null,"Clôturée",null,null,"Clôturée","22347","TREDARZEC","COTES-D'ARMOR","BRETAGNE","Polygone",-3.191131,48.790257]
["SSP000168101",null,"Ancienne décharge de Golven",null,"Clôturée",null,null,"Clôturée","22353","TREGASTEL","COTES-D'ARMOR","BRETAGNE","Polygone",-3.5102973,48.815144]
["SSP000168201",null,"Ancienne décharge et ancien stockage de déchets de marées noires de Waz Wenn",null,"Clôturée",null,null,"Clôturée","22353","TREGASTEL","COTES-D'ARMOR","BRETAGNE","Polygone",-3.5038095,48.802254]
["SSP000168401",null,"Ancienne décharge de Mézou",null,"Clôturée",null,null,"Clôturée","22354","TREGLAMUS","COTES-D'ARMOR","BRETAGNE","Polygone",-3.267082,48.545174]
["SSP000168501",null,"Ancienne décharge de La Ville Quinio",null,"Clôturée",null,null,"Clôturée","22356","TREGOMEUR","COTES-D'ARMOR","BRETAGNE","Polygone",-2.9014828,48.57715]
["SSP000168601",null,"Ancienne décharge de Tonquin",null,"Clôturée",null,null,"Clôturée","22360","TREGUEUX","COTES-D'ARMOR","BRETAGNE","Polygone",-2.7937348,48.459743]
["SSP000168701",null,"Ancienne décharge de la Croix Gibat",null,"Clôturée",null,null,"Clôturée","22360","TREGUEUX","COTES-D'ARMOR","BRETAGNE","Polygone",-2.7214575,48.47367]
["SSP000168801",null,"Ancienne décharge de la Ville Biot",null,"Clôturée",null,null,"Clôturée","22360","TREGUEUX","COTES-D'ARMOR","BRETAGNE","Polygone",-2.7041135,48.4851]
["SSP000168901",null,"Ancienne décharge de Malassis",null,"Clôturée",null,null,"Clôturée","22361","TREGUIDEL","COTES-D'ARMOR","BRETAGNE","Polygone",-2.9480317,48.61062]
["SSP000169001",null,"Ancienne décharge de Sainte Catherine",null,"Clôturée",null,null,"Clôturée","22152","MINIHY TREGUIER","COTES-D'ARMOR","BRETAGNE","Polygone",-3.2241845,48.780605]
["SSP000169101",null,"Ancienne décharge du Hellez",null,"Clôturée",null,null,"Clôturée","22365","TREMARGAT","COTES-D'ARMOR","BRETAGNE","Polygone",-3.272913,48.33581]
["SSP000169201",null,"Ancienne décharge de Leur Ar Maguet",null,"Clôturée",null,null,"Clôturée","22366","TREMEL","COTES-D'ARMOR","BRETAGNE","Polygone",-3.6383471,48.61403]
["SSP000169301",null,"Ancienne décharge de Ker Viel",null,"Clôturée",null,null,"Clôturée","22366","TREMEL","COTES-D'ARMOR","BRETAGNE","Polygone",-3.598561,48.61195]
["SSP000169401",null,"Ancienne décharge du bois de Javelle Pré",null,"Clôturée",null,null,"Clôturée","22367","TREMELOIR","COTES-D'ARMOR","BRETAGNE","Polygone",-2.8634152,48.560726]
["SSP000169501",null,"Ancienne décharge du Vieux moulin",null,"Clôturée",null,null,"Clôturée","22368","TREMEREUC","COTES-D'ARMOR","BRETAGNE","Polygone",-2.072243,48.554028]
["SSP000169601",null,"Ancienne décharge des Landes",null,"Clôturée",null,null,"Clôturée","22368","TREMEREUC","COTES-D'ARMOR","BRETAGNE","Polygone",-2.0490572,48.564224]
["SSP000169701",null,"Ancienne décharge de Saint Jacques",null,"Clôturée",null,null,"Clôturée","22370","TREMEVEN","COTES-D'ARMOR","BRETAGNE","Polygone",-3.0421176,48.679897]
["SSP000169801",null,"Ancienne décharge de Lizelec'h",null,"Clôturée",null,null,"Clôturée","22370","TREMEVEN","COTES-D'ARMOR","BRETAGNE","Polygone",-3.0328887,48.68319]
["SSP000170001",null,"Ancienne décharge du Bois de la Landelle",null,"Clôturée",null,null,"Clôturée","22043","COETLOGON","COTES-D'ARMOR","BRETAGNE","Polygone",-2.552816,48.14145]
["SSP000170101",null,"Ancienne décharge de la Trinité",null,"Clôturée",null,null,"Clôturée","22043","COETLOGON","COTES-D'ARMOR","BRETAGNE","Polygone",-2.545585,48.107124]
["SSP000170201",null,"Ancienne décharge des Ponts Neufs",null,"Clôturée",null,null,"Clôturée","22044","COETMIEUX","COTES-D'ARMOR","BRETAGNE","Polygone",-2.6119397,48.50399]
["SSP000170301",null,"Ancienne décharge de La Vallée",null,"Clôturée",null,null,"Clôturée","22045","COHINIAC","COTES-D'ARMOR","BRETAGNE","Polygone",-2.9396174,48.458626]
["SSP000170401",null,"Ancienne décharge de la Moignerais",null,"Clôturée",null,null,"Clôturée","22048","CORSEUL","COTES-D'ARMOR","BRETAGNE","Polygone",-2.1832874,48.46881]
["SSP000170501",null,"Ancienne décharge de la Poissonnais",null,"Clôturée",null,null,"Clôturée","22048","CORSEUL","COTES-D'ARMOR","BRETAGNE","Polygone",-2.183657,48.493294]
["SSP000170601",null,"LG TRAITMAT",null,"Clôturée",null,null,"Clôturée","35047","BRUZ","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.7313865,48.032543]
["SSP000170701",null,"Ancienne décharge de l'Hôtel Fairier",null,"Clôturée",null,null,"Clôturée","22048","CORSEUL","COTES-D'ARMOR","BRETAGNE","Polygone",-2.1804688,48.47807]
["SSP000170801",null,"Ancienne décharge de la Bertache",null,"Clôturée",null,null,"Clôturée","22048","CORSEUL","COTES-D'ARMOR","BRETAGNE","Polygone",-2.1794782,48.506157]
["SSP000170901",null,"Ancienne décharge du Pont de Corseul",null,"Clôturée",null,null,"Clôturée","22048","CORSEUL","COTES-D'ARMOR","BRETAGNE","Polygone",-2.166216,48.478226]
["SSP000171501",null,"Ancienne décharge de la Lande des Tertres",null,"Clôturée",null,null,"Clôturée","22049","CREHEN","COTES-D'ARMOR","BRETAGNE","Polygone",-2.1851645,48.53805]
["SSP000171601",null,"Ancienne décharge de la Touche du Bourg",null,"Clôturée",null,null,"Clôturée","22049","CREHEN","COTES-D'ARMOR","BRETAGNE","Polygone",-2.2155678,48.550343]
["SSP000171701",null,"Ancienne décharge du Moulin Rault",null,"Clôturée",null,null,"Clôturée","22049","CREHEN","COTES-D'ARMOR","BRETAGNE","Polygone",-2.200802,48.52034]
["SSP000171801","59.0334","BRIQUETERIES DE L'ENTREPRISE",null,"En cours",null,null,"En cours","59299","HEM","NORD","HAUTS-DE-FRANCE","Polygone",3.1996372,50.648487,"G14 - Fabrication d'autres matériaux de construction"]
["SSP000171802","59.0532","BRIQUETERIES DE L'ENTREPRISE",null,"En cours",null,null,"En cours","59350","LILLE","NORD","HAUTS-DE-FRANCE","Polygone",3.1996372,50.648487,"G14 - Fabrication d'autres matériaux de construction"]
["SSP000171901","59.0580","STRAP",null,"En cours",null,null,"En cours","59512","ROUBAIX","NORD","HAUTS-DE-FRANCE","Polygone",3.163665,50.688854,"K35 - Regroupement, reconditionnement de déchets"]
["SSP000172201",null,"Ancienne décharge de la route de la gare",null,"Clôturée",null,null,"Clôturée","22051","DOLO","COTES-D'ARMOR","BRETAGNE","Polygone",-2.349824,48.379463]
["SSP000172301",null,"Ancienne décharge du Bouquet Jalu",null,"Clôturée",null,null,"Clôturée","22051","DOLO","COTES-D'ARMOR","BRETAGNE","Polygone",-2.323628,48.397327]
["SSP000172401",null,"Ancienne décharge de Ker Lan",null,"Clôturée",null,null,"Clôturée","22052","DUAULT","COTES-D'ARMOR","BRETAGNE","Polygone",-3.4216294,48.369946]
["SSP000172501",null,"Ancienne décharge de la Ville Bedel",null,"Clôturée",null,null,"Clôturée","22053","EREAC","COTES-D'ARMOR","BRETAGNE","Polygone",-2.3623967,48.280975]
["SSP000172601",null,"Ancienne décharge de Bougueneuf",null,"Clôturée",null,null,"Clôturée","22053","EREAC","COTES-D'ARMOR","BRETAGNE","Polygone",-2.3416252,48.286064]
["SSP000172701",null,"Ancienne décharge de la Fosse Eyrand",null,"Clôturée",null,null,"Clôturée","22054","ERQUY","COTES-D'ARMOR","BRETAGNE","Polygone",-2.4364612,48.651615]
["SSP000172801",null,"Ancienne décharge de la Ville Es Renais",null,"Clôturée",null,null,"Clôturée","22054","ERQUY","COTES-D'ARMOR","BRETAGNE","Polygone",-2.4259567,48.63322]
["SSP000172901",null,"Ancienne décharge de la Côte des Noës",null,"Clôturée",null,null,"Clôturée","22055","ETABLES SUR MER","COTES-D'ARMOR","BRETAGNE","Polygone",-2.8439803,48.631947]
["SSP000173201","69.0117","Ancienne usine à gaz  de Lyon Guillotière",null,"En cours",null,null,"En cours","69123","LYON","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.849848,45.75551,"J1 - Cokéfaction, usines à gaz"]
["SSP000173401",null,"Ancienne décharge du bourg",null,"Clôturée",null,null,"Clôturée","29016","BRASPARTS","FINISTERE","BRETAGNE","Polygone",-3.958672,48.30097]
["SSP000173501",null,"Ancienne décharge du Quinquis",null,"Clôturée",null,null,"Clôturée","29016","BRASPARTS","FINISTERE","BRETAGNE","Polygone",-3.939913,48.303074]
["SSP000173601",null,"Ancienne décharge de Toulahouat",null,"Clôturée",null,null,"Clôturée","29016","BRASPARTS","FINISTERE","BRETAGNE","Polygone",-3.9617906,48.30776]
["SSP000173701",null,"Ancienne décharge du Menez Gwen",null,"Clôturée",null,null,"Clôturée","29018","BRENNILIS","FINISTERE","BRETAGNE","Polygone",-3.848425,48.3679]
["SSP000173901","29.0003","Ancien décharge de Prat Ar Garguic",null,"En cours",null,null,"En cours","29019","BREST","FINISTERE","BRETAGNE","Polygone",-4.489114,48.443813,"K36 - Mise en décharge"]
["SSP000174001",null,"Ancienne décharge de Pennisquin",null,"Clôturée",null,null,"Clôturée","29020","BRIEC","FINISTERE","BRETAGNE","Polygone",-4.008695,48.087997]
["SSP000175201",null,"Ancienne décharge de l'étang de Kerloch",null,"Clôturée",null,null,"Clôturée","29042","CROZON","FINISTERE","BRETAGNE","Polygone",-4.5495024,48.261086]
["SSP000175601",null,"Ancienne décharge de Pouldavid",null,"Clôturée",null,null,"Clôturée","29046","DOUARNENEZ","FINISTERE","BRETAGNE","Polygone",-4.329802,48.080154]
["SSP000175701",null,"Ancienne décharge de Coat Dregat",null,"Clôturée",null,null,"Clôturée","29048","EDERN","FINISTERE","BRETAGNE","Polygone",-3.9891849,48.07986]
["SSP000175801",null,"Ancienne décharge de Kernevez Lagadec",null,"Clôturée",null,null,"Clôturée","29049","ELLIANT","FINISTERE","BRETAGNE","Polygone",-3.8628504,47.99193]
["SSP000175901",null,"Ancienne décharge de Kerganou",null,"Clôturée",null,null,"Clôturée","29051","ERGUE GABERIC","FINISTERE","BRETAGNE","Polygone",-3.9775164,48.011566]
["SSP000176401",null,"Ancienne décharge de Saint-Fiacre",null,"Clôturée",null,null,"Clôturée","29069","GUILERS","FINISTERE","BRETAGNE","Polygone",-4.5890207,48.429096]
["SSP000177501",null,"Ancienne décharge du Rohou",null,"Clôturée",null,null,"Clôturée","29090","KERLAZ","FINISTERE","BRETAGNE","Polygone",-4.25266,48.077286]
["SSP000177601",null,"Ancienne décharge de Kerleo",null,"Clôturée",null,null,"Clôturée","29094","KERNOUES","FINISTERE","BRETAGNE","Polygone",-4.352654,48.58627]
["SSP000177701",null,"Ancienne décharge du Moulin de Poulaliou",null,"Clôturée",null,null,"Clôturée","29094","KERNOUES","FINISTERE","BRETAGNE","Polygone",-4.3527884,48.591404]
["SSP000178301",null,"Ancienne décharge de Trézel",null,"Clôturée",null,null,"Clôturée","29094","KERNOUES","FINISTERE","BRETAGNE","Polygone",-4.3615427,48.590034]
["SSP000178501",null,"Ancienne décharge de Kerroc'h",null,"Clôturée",null,null,"Clôturée","29097","LAMPAUL GUIMILIAU","FINISTERE","BRETAGNE","Polygone",-4.020348,48.45849]
["SSP000178801",null,"Ancienne décharge de Ty Sablé",null,"Clôturée",null,null,"Clôturée","29106","LANDREVARZEC","FINISTERE","BRETAGNE","Polygone",-4.0738015,48.072308]
["SSP000179501",null,"Ancienne usine d'incinération",null,"Clôturée",null,null,"Clôturée","35337","TINTENIAC","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.8056444,48.330994]
["SSP000179701","29.0024","Société ROMI",null,"En cours",null,null,"En cours","29232","QUIMPER","FINISTERE","BRETAGNE","Polygone",-4.104177,47.969627,"K5 - Récupération, dépôts de ferrailles"]
["SSP000180101",null,"Ancienne décharge de Quiella",null,"Clôturée",null,null,"Clôturée","29053","LE FAOU","FINISTERE","BRETAGNE","Polygone",-4.1656895,48.301537]
["SSP000180201",null,"Ancienne décharge de Kermenez",null,"Clôturée",null,null,"Clôturée","29087","LE JUCH","FINISTERE","BRETAGNE","Polygone",-4.268953,48.056873]
["SSP000181001",null,"Ancienne décharge de Guérouel",null,"Clôturée",null,null,"Clôturée","29139","LOPEREC","FINISTERE","BRETAGNE","Polygone",-4.0404835,48.279697]
["SSP000181301",null,"Ancienne décharge du Quinquis",null,"Clôturée",null,null,"Clôturée","29146","MELGVEN","FINISTERE","BRETAGNE","Polygone",-3.8418305,47.920334]
["SSP000181401",null,"Ancienne décharge de Rozangall",null,"Clôturée",null,null,"Clôturée","29146","MELGVEN","FINISTERE","BRETAGNE","Polygone",-3.8676496,47.945343]
["SSP000181501","69.0017","DECHARGE DE BOUQUIS",null,"En cours",null,null,"En cours","69072","DARDILLY","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.7508974,45.824745,"K36 - Mise en décharge"]
["SSP000181801","69.0024","ZONE INDUSTRIELLE NORD- Rue Solomon",null,"En cours",null,null,"En cours","69199","SAINT FONS","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.8542194,45.713634,"K21 - Décharges d'ordures ménagères"]
["SSP000183301",null,"Ancienne décharge de Rudaou",null,"Clôturée",null,null,"Clôturée","29170","PLOMELIN","FINISTERE","BRETAGNE","Polygone",-4.1782837,47.927135]
["SSP000183601","29.0019","Société Hydroservices de l'Ouest",null,"En cours",null,null,"En cours","29006","BENODET","FINISTERE","BRETAGNE","Polygone",-4.0412707,47.881226,"K2 - Traitement de déchets urbains"]
["SSP000183701","29.0054","VALCOR (ex UIOM)",null,"En cours",null,null,"En cours","29145","CONFORT MEILARS","FINISTERE","BRETAGNE","Polygone",-4.4402456,48.06148,"K31 - Incinération"]
["SSP000183801","29.0001","Zone Industrielle Portuaire de Brest",null,"En cours",null,null,"En cours","29019","BREST","FINISTERE","BRETAGNE","Polygone",-4.448566,48.38627]
["SSP000183901","29.0023","COMPAGNIE PETROLIERE DE L'OUEST",null,"En cours",null,null,"En cours","29069","GUILERS","FINISTERE","BRETAGNE","Polygone",-4.539619,48.40331,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000184001","29.0044","BOLLORE",null,"Clôturée",null,"2020-07-08","Clôturée","29274","SCAER","FINISTERE","BRETAGNE","Polygone",-3.6775472,47.99887,"D72 - Transformation des matières plastiques"]
["SSP000184201",null,"Ancien dépôt de mâchefer",null,"Clôturée",null,null,"Clôturée","29046","DOUARNENEZ","FINISTERE","BRETAGNE","Polygone",-4.3191857,48.07946]
["SSP000184301",null,"Ancienne décharge de Bohalen",null,"Clôturée",null,null,"Clôturée","29016","BRASPARTS","FINISTERE","BRETAGNE","Polygone",-3.9589136,48.31527]
["SSP000184401",null,"Ancienne décharge du Port",null,"Clôturée",null,null,"Clôturée","29019","BREST","FINISTERE","BRETAGNE","Polygone",-4.4686913,48.382484]
["SSP000184501",null,"Serres du Portzic",null,"Clôturée",null,null,"Clôturée","29019","BREST","FINISTERE","BRETAGNE","Polygone",-4.5506196,48.371098]
["SSP000184601",null,"Ancienne usine à gaz",null,"Clôturée",null,null,"Clôturée","29019","BREST","FINISTERE","BRETAGNE","Polygone",-4.5031424,48.38901]
["SSP000184701",null,"Ancienne usine à gaz de Bougainville",null,"Clôturée",null,null,"Clôturée","29039","CONCARNEAU","FINISTERE","BRETAGNE","Polygone",-3.9267063,47.8723]
["SSP000184901",null,"Ancienne usine à gaz",null,"Clôturée",null,null,"Clôturée","29046","DOUARNENEZ","FINISTERE","BRETAGNE","Polygone",-4.3310246,48.08748]
["SSP000185401",null,"Ancienne décharge communale",null,"Clôturée",null,null,"Clôturée","29104","LANDEVENNEC","FINISTERE","BRETAGNE","Polygone",-4.2650633,48.290016]
["SSP000185701",null,"Ancienne décharge de Kernou",null,"Clôturée",null,null,"Clôturée","29169","PLOGONNEC","FINISTERE","BRETAGNE","Polygone",-4.139761,48.05824]
["SSP000187201","56.0005","Fonderie de Bretagne - FDB (ex SBFM)",null,"En cours",null,null,"En cours","56036","CAUDAN","MORBIHAN","BRETAGNE","Polygone",-3.3274772,47.78039,"J5 - Fonderie et travail des métaux"]
["SSP000187301",null,"Ancienne décharge de Penalein",null,"Clôturée",null,null,"Clôturée","29189","PLOUGASTEL DAOULAS","FINISTERE","BRETAGNE","Polygone",-4.352766,48.352203]
["SSP000187401","56.0022","SA FREQUELIN ELECTROLYSE",null,"En cours",null,null,"En cours","56036","CAUDAN","MORBIHAN","BRETAGNE","Polygone",-3.3444624,47.785664,"H13 - Traitement de surface"]
["SSP000187501","29.0010","GROUPEMENT PETROLIER DE BREST (GPB)",null,"En cours",null,null,"En cours","29019","BREST","FINISTERE","BRETAGNE","Polygone",-4.467381,48.38751,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000187801",null,"Ancienne décharge de Kernabat",null,"Clôturée",null,null,"Clôturée","29068","GUICLAN","FINISTERE","BRETAGNE","Polygone",-3.9602127,48.54193]
["SSP000189501","11.0002","ANCIENS ETABLISSEMENTS BOILLETOT",null,"En cours",null,null,"En cours","11304","QUILLAN","AUDE","OCCITANIE","Polygone",2.183736,42.870163]
["SSP000189701","11.0004","MELPOMEN  - Atelier avenue d'Occitanie",null,"En cours",null,null,"En cours","11266","PORT LA NOUVELLE","AUDE","OCCITANIE","Polygone",3.032831,43.02202,"D37 - Phytosanitaires, pesticides (fabrication de)"]
["SSP000189801",null,"Ancienne décharge de Vellinic",null,"Clôturée",null,null,"Clôturée","29203","PLOUNEOUR TREZ","FINISTERE","BRETAGNE","Polygone",-4.3183155,48.64576]
["SSP000189901","11.0011","Centre EDF / GDF Services Vallée d'Aude",null,"En cours",null,null,"En cours","11069","CARCASSONNE","AUDE","OCCITANIE","Polygone",2.359093,43.21325]
["SSP000190201","11.0013","Agence clientèle de Limoux","GDF Limoux","En cours",null,null,"En cours","11206","LIMOUX","AUDE","OCCITANIE","Polygone",2.2194629,43.056755,"J1 - Cokéfaction, usines à gaz"]
["SSP000190301","11.0012","Agence d'exploitation EDF-GDF",null,"En cours",null,null,"En cours","11262","NARBONNE","AUDE","OCCITANIE","Polygone",2.9947462,43.186176]
["SSP000190401","11.0017","HUNTSMAN SAS",null,"En cours",null,null,"En cours","11304","QUILLAN","AUDE","OCCITANIE","Polygone",2.1916375,42.90454,"D72 - Transformation des matières plastiques"]
["SSP000190501","11.0019","SOFT",null,"En cours",null,null,"En cours","11266","PORT LA NOUVELLE","AUDE","OCCITANIE","Polygone",3.036662,43.01931,"D37 - Phytosanitaires, pesticides (fabrication de)"]
["SSP000190601","11.0021","Société Languedocienne de Micron-Couleur (S.L.M.C.)",null,"En cours",null,null,"En cours","11262","NARBONNE","AUDE","OCCITANIE","Polygone",2.9745038,43.213585,"D32 - Chimie minérale inorganique autre"]
["SSP000190701","11.0022","MELPOMEN - Site principal Ave Catalogne",null,"En cours",null,null,"En cours","11266","PORT LA NOUVELLE","AUDE","OCCITANIE","Polygone",3.0361526,43.01883]
["SSP000190801",null,"Ancien stockage de déchets de marées noires de Port Poullic ar Lor",null,"Clôturée",null,null,"Clôturée","29019","BREST","FINISTERE","BRETAGNE","Polygone",-4.4648886,48.386543]
["SSP000190901","30.0002","UGINE",null,"En cours",null,null,"En cours","30141","LAUDUN L'ARDOISE","GARD","OCCITANIE","Polygone",4.7133417,44.089024,"J22 - Production d'acier brut, aciéries"]
["SSP000191001","30.0004","INVER France","INVER France","En cours",null,null,"En cours","30209","PUJAUT","GARD","OCCITANIE","Polygone",4.797923,44.018757,"D4 - Encres, vernis, peintures, colles (fabrication de)"]
["SSP000191201","30.0005","AVENTIS - AGRICULTURE",null,"En cours",null,null,"En cours","30032","BEAUCAIRE","GARD","OCCITANIE","Polygone",4.6125,43.800266,"D3 - Chimie, phytosanitaire, pharmacie"]
["SSP000191301","29.0059","GARCIA",null,"En cours",null,null,"En cours","29254","SAINT MARTIN DES CHAMPS","FINISTERE","BRETAGNE","Polygone",-3.8511996,48.559986,"K5 - Récupération, dépôts de ferrailles"]
["SSP000191401","30.0006","NOBEL",null,"En cours",null,null,"En cours","30155","MANDUEL","GARD","OCCITANIE","Polygone",4.5271163,43.7975,null,"18.03 - Fabrication d'explosifs, d'accessoires de mise à feu et d'artifices"]
["SSP000191501","30.0008","CEAC",null,"En cours",null,null,"En cours","30189","NIMES","GARD","OCCITANIE","Polygone",4.310933,43.80771,null,"28.23 - Fabrication d'accumulateurs"]
["SSP000191601","30.0013","Ancienne usine à tubes",null,"En cours",null,null,"En cours","30037","BESSEGES","GARD","OCCITANIE","Polygone",4.092788,44.293198,"J53 - Travail des métaux, chaudronnerie, poudres"]
["SSP000192201","30.0016","Agence commerciale EDF GDF",null,"En cours",null,null,"En cours","30007","ALES","GARD","OCCITANIE","Polygone",4.086246,44.12184,"J1 - Cokéfaction, usines à gaz"]
["SSP000192301","30.0018","Ancienne usine à gaz",null,"En cours",null,null,"En cours","30321","SOMMIERES","GARD","OCCITANIE","Polygone",4.0922947,43.775627,"J1 - Cokéfaction, usines à gaz"]
["SSP000192401",null,"Ancienne décharge de Kreisker",null,"Clôturée",null,null,"Clôturée","29011","BOHARS","FINISTERE","BRETAGNE","Polygone",-4.512467,48.426033]
["SSP000192501",null,"Ancienne décharge de Coat Enez",null,"Clôturée",null,null,"Clôturée","29212","PLOUZANE","FINISTERE","BRETAGNE","Polygone",-4.594153,48.39135]
["SSP000192801","30.0022","Crassier de Tamaris",null,"En cours",null,null,"En cours","30007","ALES","GARD","OCCITANIE","Polygone",4.0765038,44.14748,"J51 - Fonderie des métaux ferreux"]
["SSP000193101","30.0026","BRUN D'ARRE",null,"En cours",null,null,"En cours","30016","ARRE","GARD","OCCITANIE","Polygone",3.517224,43.96687,"E13 - Blanchiment, teinture, impression"]
["SSP000193201","30.0027","SNCF Technicentre Languedoc-Roussillon",null,"En cours",null,null,"En cours","30189","NIMES","GARD","OCCITANIE","Polygone",4.3796945,43.844856,"L22 - Transports"]
["SSP000193301","09.0003","ALUMINIUM PECHINEY - USINE D'AUZAT",null,"En cours",null,null,"En cours","09030","AUZAT","ARIEGE","OCCITANIE","Polygone",1.4795092,42.762577,"J32 - Métallurgie de l'aluminium"]
["SSP000193401",null,"Ancienne décharge route de Dinan",null,"Clôturée",null,null,"Clôturée","29042","CROZON","FINISTERE","BRETAGNE","Polygone",-4.517108,48.24013]
["SSP000193901","09.0006","NESTOR SAS (ex AVELANA)",null,"En cours",null,null,"En cours","09336","VILLENEUVE D'OLMES","ARIEGE","OCCITANIE","Polygone",1.8353791,42.915054,"E13 - Blanchiment, teinture, impression"]
["SSP000194001","09.0007","C.M.T. FINITIONS (ex FITEX)",null,"En cours",null,null,"En cours","09336","VILLENEUVE D'OLMES","ARIEGE","OCCITANIE","Polygone",1.8292433,42.910477,"E13 - Blanchiment, teinture, impression"]
["SSP000194101","09.0010","MEYLAN 60 (ex PAPETERIES MATUSSIERE ET FOREST)",null,"En cours",null,null,"En cours","09261","SAINT GIRONS","ARIEGE","OCCITANIE","Polygone",1.1271857,42.977844,"C22 - Fabrication de papiers et carton"]
["SSP000194201","09.0013","SOCIETE NOUVELLE SAREM",null,"En cours",null,null,"En cours","09296","SINSAT","ARIEGE","OCCITANIE","Polygone",1.6635954,42.798,"H13 - Traitement de surface"]
["SSP000194301","09.0015","ORIZONA  ( ex SOCIETE CENTRALE D'ECLAIRAGE)",null,"En cours",null,null,"En cours","09167","LEZAT SUR LEZE","ARIEGE","OCCITANIE","Polygone",1.3462344,43.28006,"H13 - Traitement de surface"]
["SSP000194601","09.0016","CMT (CARREMAN MICHEL THIERRY FINITIONS)",null,"En cours",null,null,"En cours","09160","LAVELANET","ARIEGE","OCCITANIE","Polygone",1.8434504,42.92543,"E13 - Blanchiment, teinture, impression"]
["SSP000194701","09.0018","INCINERATEUR D'ORDURES MENAGERES DE TARASCON SUR ARIEGE",null,"En cours",null,null,"En cours","09306","TARASCON SUR ARIEGE","ARIEGE","OCCITANIE","Polygone",1.59377,42.832005,"K2 - Traitement de déchets urbains"]
["SSP000194801","09.0019","ALUMINIUM PECHINEY (DECHARGE INTERNE DE MASSADA)",null,"En cours",null,null,"En cours","09030","AUZAT","ARIEGE","OCCITANIE","Polygone",1.4672741,42.74638,"K36 - Mise en décharge"]
["SSP000194901",null,"Ancienne décharge de Kerbalannec",null,"Clôturée",null,null,"Clôturée","29074","GUIMILIAU","FINISTERE","BRETAGNE","Polygone",-4.00983,48.481915]
["SSP000195101","09.0024","ANCIENNE USINE A GAZ",null,"En cours",null,"2012-06-01","En cours","09261","SAINT GIRONS","ARIEGE","OCCITANIE","Polygone",1.13903,42.98461,"J1 - Cokéfaction, usines à gaz"]
["SSP000195201","09.0025","AGENCE COMMERCIALE D'EDF GDF (ANCIENNE USINE A GAZ)",null,"En cours",null,"2012-06-01","En cours","09225","PAMIERS","ARIEGE","OCCITANIE","Polygone",1.6135107,43.11207,"J1 - Cokéfaction, usines à gaz"]
["SSP000195601","09.0029","DECHARGE INTERNE \"D8\" DE L'USINE PECHINEY DE SABART",null,"En cours",null,null,"En cours","09306","TARASCON SUR ARIEGE","ARIEGE","OCCITANIE","Polygone",1.5985926,42.83427,"K36 - Mise en décharge"]
["SSP000195701","09.0031","RECYCARBO",null,"En cours",null,null,"En cours","09157","LAROQUE D'OLMES","ARIEGE","OCCITANIE","Polygone",1.8762455,42.982937,"K3 - Traitement de déchets industriels"]
["SSP000196101",null,"Stockage de déchets de marées noires de Port Yeusin",null,"Clôturée",null,null,"Clôturée","29155","OUESSANT","FINISTERE","BRETAGNE","Polygone",-5.1057363,48.47059]
["SSP000196401","69.0112","Agence d'exploitation EDF GDF Services",null,"En cours",null,null,"En cours","69243","TARARE","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.437608,45.89284,"J1 - Cokéfaction, usines à gaz"]
["SSP000198101",null,"Ancienne décharge de Kerlarret",null,"Clôturée",null,null,"Clôturée","29217","PONT AVEN","FINISTERE","BRETAGNE","Polygone",-3.7808769,47.87198]
["SSP000198201",null,"Ancienne décharge de Landédéo",null,"Clôturée",null,null,"Clôturée","29217","PONT AVEN","FINISTERE","BRETAGNE","Polygone",-3.7683249,47.898476]
["SSP000198301",null,"Ancienne décharge du Guilly",null,"Clôturée",null,null,"Clôturée","29217","PONT AVEN","FINISTERE","BRETAGNE","Polygone",-3.7556784,47.879795]
["SSP000198501",null,"Ancienne décharge du quai Botrel",null,"Clôturée",null,null,"Clôturée","29217","PONT AVEN","FINISTERE","BRETAGNE","Polygone",-3.748717,47.84903]
["SSP000198701","31.0003","EDF GDF SERVICES GRAND TOULOUSE (Ancienne usine à gaz)",null,"En cours",null,null,"En cours","31555","TOULOUSE","HAUTE-GARONNE","OCCITANIE","Polygone",1.4276766,43.61085,"J1 - Cokéfaction, usines à gaz"]
["SSP000198901",null,"Ancienne décharge de Bostaniec",null,"Clôturée",null,null,"Clôturée","29302","PONT DE BUIS LES QUIMERCH","FINISTERE","BRETAGNE","Polygone",-4.1127315,48.252815]
["SSP000199001",null,"Ancienne décharge de Goasseac'h",null,"Clôturée",null,null,"Clôturée","29302","PONT DE BUIS LES QUIMERCH","FINISTERE","BRETAGNE","Polygone",-4.1328917,48.293335]
["SSP000199101",null,"Ancienne décharge de Kermorvan",null,"Clôturée",null,null,"Clôturée","29302","PONT DE BUIS LES QUIMERCH","FINISTERE","BRETAGNE","Polygone",-4.1059027,48.25677]
["SSP000199601",null,"Ancienne décharge de Kerhomen",null,"Clôturée",null,null,"Clôturée","29224","POULDERGAT","FINISTERE","BRETAGNE","Polygone",-4.331856,48.043736]
["SSP000199701",null,"Ancienne décharge de Kerlivit",null,"Clôturée",null,null,"Clôturée","29224","POULDERGAT","FINISTERE","BRETAGNE","Polygone",-4.3322244,48.057884]
["SSP000199801",null,"Ancienne décharge de Kermenez",null,"Clôturée",null,null,"Clôturée","29226","POULLAN SUR MER","FINISTERE","BRETAGNE","Polygone",-4.4119086,48.086796]
["SSP000199901",null,"Ancienne décharge de Kerviny",null,"Clôturée",null,null,"Clôturée","29226","POULLAN SUR MER","FINISTERE","BRETAGNE","Polygone",-4.3833084,48.05415]
["SSP000200001",null,"Ancienne décharge de Ménez Lanergat",null,"Clôturée",null,null,"Clôturée","29226","POULLAN SUR MER","FINISTERE","BRETAGNE","Polygone",-4.4050083,48.085815]
["SSP000200101",null,"Ancienne décharge de Lestrivin",null,"Clôturée",null,null,"Clôturée","29226","POULLAN SUR MER","FINISTERE","BRETAGNE","Polygone",-4.385938,48.08721]
["SSP000200201","31.0004","SEUB (SOCIETE D'EXPLOITATION DE L'USINE DE BOUSSENS)",null,"En cours",null,null,"En cours","31084","BOUSSENS","HAUTE-GARONNE","OCCITANIE","Polygone",0.9643209,43.165943,"D31 - Industrie du chlore"]
["SSP000200301","31.0025","SIVOM DE CADOURS - INCINERATEUR D'ORDURES MENAGERES",null,"En cours",null,null,"En cours","31098","CADOURS","HAUTE-GARONNE","OCCITANIE","Polygone",1.062921,43.739243,"K2 - Traitement de déchets urbains"]
["SSP000200601","31.0037","BEZIAT CASTANET",null,"En cours",null,null,"En cours","31182","FENOUILLET","HAUTE-GARONNE","OCCITANIE","Polygone",1.3965738,43.68949,null,"59.06 - Commerce de produits chimiques industriels"]
["SSP000200701","31.0042","LAFITTE(ex AUGROS PACKAGING )",null,"En cours",null,null,"En cours","31433","PORTET SUR GARONNE","HAUTE-GARONNE","OCCITANIE","Polygone",1.3810159,43.52811,"H1 - Mécanique, électrique, traitement de surface"]
["SSP000201101","30.0017","Ancienne usine à gaz",null,"En cours",null,null,"En cours","30263","SAINT HIPPOLYTE DU FORT","GARD","OCCITANIE","Polygone",3.8540032,43.963802,"J1 - Cokéfaction, usines à gaz"]
["SSP000201301","31.0046","ETABLISSEMENTS FIDELLE",null,"En cours",null,null,"En cours","31483","SAINT GAUDENS","HAUTE-GARONNE","OCCITANIE","Polygone",0.6947744,43.11077,"K52 - Dépôts de ferraille"]
["SSP000201401",null,"Ancienne décharge de Kerampape",null,"Clôturée",null,null,"Clôturée","29229","QUEMENEVEN","FINISTERE","BRETAGNE","Polygone",-4.1204314,48.125732]
["SSP000201601","31.0050","INCINERATEUR DE CAZERES",null,"En cours",null,null,"En cours","31135","CAZERES","HAUTE-GARONNE","OCCITANIE","Polygone",1.1139704,43.214252,"K2 - Traitement de déchets urbains"]
["SSP000201701","31.0051","PECHINEY BATIMENTS",null,"En cours",null,null,"En cours","31316","MARIGNAC","HAUTE-GARONNE","OCCITANIE","Polygone",0.6524132,42.92191,"J4 - Electrométallurgie"]
["SSP000201801","31.0052","ANCIENNE USINE A GAZ",null,"En cours",null,"2012-06-01","En cours","31483","SAINT GAUDENS","HAUTE-GARONNE","OCCITANIE","Polygone",0.7311779,43.107677,"J1 - Cokéfaction, usines à gaz"]
["SSP000202101",null,"Ancien site de stockage de déchets de marées noire de Kercaradec",null,"Clôturée",null,null,"Clôturée","29232","QUIMPER","FINISTERE","BRETAGNE","Polygone",-4.1432314,47.990456]
["SSP000202301",null,"Ancienne décharge de Lez Steir",null,"Clôturée",null,null,"Clôturée","29232","QUIMPER","FINISTERE","BRETAGNE","Polygone",-4.12883,48.03179]
["SSP000202401","31.0067","ENTREPRISE  MALET",null,"En cours",null,null,"En cours","31555","TOULOUSE","HAUTE-GARONNE","OCCITANIE","Polygone",1.4141749,43.552963,"F - Industries extractives"]
["SSP000202501","31.0069","NADAL",null,"En cours",null,null,"En cours","31555","TOULOUSE","HAUTE-GARONNE","OCCITANIE","Polygone",1.412642,43.595287,null,null,null,"38.12Z - Collecte des déchets dangereux"]
["SSP000202601","31.0072","Société des PETROLES SHELL",null,"En cours",null,null,"En cours","31555","TOULOUSE","HAUTE-GARONNE","OCCITANIE","Polygone",1.4524148,43.615025,"L23 - Détail de carburants"]
["SSP000202701","31.0073","TOTAL RAFFINAGE MARKETING (J.RIEUX)",null,"En cours",null,null,"En cours","31555","TOULOUSE","HAUTE-GARONNE","OCCITANIE","Polygone",1.46733,43.59283,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000202801","31.0076","GERLERO ET FILS",null,"En cours",null,null,"En cours","31467","SAINT ALBAN","HAUTE-GARONNE","OCCITANIE","Polygone",1.4084707,43.691105,"K35 - Regroupement, reconditionnement de déchets"]
["SSP000202901",null,"Ancienne décharge de Kerjequel",null,"Clôturée",null,null,"Clôturée","29232","QUIMPER","FINISTERE","BRETAGNE","Polygone",-4.075559,47.97221]
["SSP000203001",null,"Ancienne décharge de Poulguinan",null,"Clôturée",null,null,"Clôturée","29232","QUIMPER","FINISTERE","BRETAGNE","Polygone",-4.114458,47.985294]
["SSP000203101","31.0079","BOOMERANG (BIS RECYCLAGE)",null,"En cours",null,null,"En cours","31490","SAINT JORY","HAUTE-GARONNE","OCCITANIE","Polygone",1.3769442,43.73108,"K35 - Regroupement, reconditionnement de déchets"]
["SSP000203201","32.0002","INCINERATEUR DE PAUILHAC / SIDEL",null,"En cours",null,null,"En cours","32306","PAUILHAC","GERS","OCCITANIE","Polygone",0.62145764,43.877327,"K2 - Traitement de déchets urbains"]
["SSP000203301","32.0003","AGENCE D'EDF GDF SERVICES (ANCIENNE USINE A GAZ)",null,"En cours",null,"2012-06-01","En cours","32013","AUCH","GERS","OCCITANIE","Polygone",0.5952241,43.64841,"J1 - Cokéfaction, usines à gaz"]
["SSP000203901","32.0009","Ancien site Colas Sud Ouest",null,"En cours",null,null,"En cours","32013","AUCH","GERS","OCCITANIE","Polygone",0.60050064,43.662773,"G22 - Centrales d'enrobés"]
["SSP000204101","34.0003","Ancien étang de Frontignan",null,"En cours",null,null,"En cours","34108","FRONTIGNAN","HERAULT","OCCITANIE","Polygone",3.7506752,43.43965]
["SSP000204301","34.0005","ESSENCES ET CARBURANTS DE FRANCE",null,"En cours",null,null,"En cours","34108","FRONTIGNAN","HERAULT","OCCITANIE","Polygone",3.7035975,43.424175,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000204401","34.0011","Ancienne usine à gaz de Bedarieux",null,"En cours",null,null,"En cours","34028","BEDARIEUX","HERAULT","OCCITANIE","Polygone",3.1515477,43.612186]
["SSP000204501","34.0012","Agence EDF / GDF",null,"En cours",null,null,"En cours","34145","LUNEL","HERAULT","OCCITANIE","Polygone",4.1320434,43.68131]
["SSP000204601","34.0013","Agence EDF / GDF Services","GDF","En cours",null,null,"En cours","34199","PEZENAS","HERAULT","OCCITANIE","Polygone",3.427456,43.45267,"J1 - Cokéfaction, usines à gaz"]
["SSP000204801","34.0015","Agence d'Exploitation d'EDF GDF",null,"En cours",null,null,"En cours","34172","MONTPELLIER","HERAULT","OCCITANIE","Polygone",3.8852332,43.603928,"J1 - Cokéfaction, usines à gaz"]
["SSP000204901","34.0016","ANCIENNE USINE A GAZ",null,"En cours",null,null,"En cours","34142","LODEVE","HERAULT","OCCITANIE","Polygone",3.3225887,43.725033,"J1 - Cokéfaction, usines à gaz"]
["SSP000205001","34.0017","Agence EDF GDF SERVICES de Frontignan-Sète la Peyrade",null,"En cours",null,null,"En cours","34108","FRONTIGNAN","HERAULT","OCCITANIE","Polygone",3.7258077,43.424164,"J1 - Cokéfaction, usines à gaz"]
["SSP000205101",null,"Ancienne décharge de Keryvon",null,"Clôturée",null,null,"Clôturée","29250","SAINT HERNIN","FINISTERE","BRETAGNE","Polygone",-3.6110373,48.220333]
["SSP000205201","34.0019","MOULIN DU CAPITOUL",null,"En cours",null,null,"En cours","34142","LODEVE","HERAULT","OCCITANIE","Polygone",3.340866,43.69585,"D3 - Chimie, phytosanitaire, pharmacie"]
["SSP000205401","34.0024","Canal de La Peyrade / pipeline GDH",null,"En cours",null,null,"En cours","34108","FRONTIGNAN","HERAULT","OCCITANIE","Polygone",3.7250717,43.41947,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000205601","34.0026","Gare de CEILHES ROQUEREDONDE",null,"En cours",null,null,"En cours","34233","ROQUEREDONDE","HERAULT","OCCITANIE","Polygone",3.157138,43.811474]
["SSP000205701","34.0027","cocon de la RD8",null,"En cours",null,null,"En cours","34019","AVENE","HERAULT","OCCITANIE","Polygone",3.0988748,43.793533]
["SSP000205801","34.0028","LA MEDITERRANEENNE",null,"En cours",null,null,"En cours","34003","AGDE","HERAULT","OCCITANIE","Polygone",3.464924,43.31858,"D36 - Fabrication des engrais"]
["SSP000205901","34.0030","SOTRAITAL II",null,"En cours",null,null,"En cours","34244","SAINT BRES","HERAULT","OCCITANIE","Polygone",4.034694,43.6572,"H1 - Mécanique, électrique, traitement de surface"]
["SSP000206001","34.0031","Raffinerie Mobil de Frontignan","Ancienne raffinerie Mobil","En cours",null,null,"En cours","34108","FRONTIGNAN","HERAULT","OCCITANIE","Polygone",3.757184,43.440434,"D12 - Raffinage de pétrole, carburants et lubrifiants"]
["SSP000206101","34.0034","SHELL avenue de Maurin",null,"En cours",null,null,"En cours","34172","MONTPELLIER","HERAULT","OCCITANIE","Polygone",3.8737538,43.580765,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000206201","34.0036","TOTAL",null,"En cours",null,null,"En cours","34301","SETE","HERAULT","OCCITANIE","Polygone",3.7085366,43.40568,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000206301","34.0047","SPINELLI",null,"En cours",null,null,"En cours","34301","SETE","HERAULT","OCCITANIE","Polygone",3.7071857,43.40892,"K5 - Récupération, dépôts de ferrailles"]
["SSP000206401","34.0048","Ancienne station service TOTAL - Pézenas - avenue de Verdun",null,"En cours",null,null,"En cours","34199","PEZENAS","HERAULT","OCCITANIE","Polygone",3.420669,43.453415]
["SSP000206501","46.0007","SOB S.A.",null,"En cours",null,null,"En cours","46038","BRETENOUX","LOT","OCCITANIE","Polygone",1.8318948,44.92042,"D42 - Fabrication de peintures"]
["SSP000206601","46.0008","PECHINEY ELECTROMETALLURGIE",null,"En cours",null,null,"En cours","46163","LAVAL DE CERE","LOT","OCCITANIE","Polygone",1.9294256,44.948174,"J4 - Electrométallurgie"]
["SSP000206801","46.0009","Parking  ESPACE JEAN JAURES (Ancienne usine à gaz)",null,"En cours",null,null,"En cours","46102","FIGEAC","LOT","OCCITANIE","Polygone",2.0305471,44.6065,"J1 - Cokéfaction, usines à gaz"]
["SSP000207401","46.0010","CENTRE EDF GDF SERVICES LOT (ancienne usine à gaz)",null,"En cours",null,null,"En cours","46042","CAHORS","LOT","OCCITANIE","Point",0.0,0.0,"J1 - Cokéfaction, usines à gaz"]
["SSP000207701","46.0012","SIDENERGIE S.A.",null,"En cours",null,null,"En cours","46163","LAVAL DE CERE","LOT","OCCITANIE","Polygone",1.9298276,44.94819,"C13 - Traitement du bois"]
["SSP000208001",null,"Ancienne décharge de Moguer Bian",null,"Clôturée",null,null,"Clôturée","29271","SAINT VOUGAY","FINISTERE","BRETAGNE","Polygone",-4.1411266,48.56491]
["SSP000208801",null,"Ancienne décharge de Menez Luz",null,"Clôturée",null,null,"Clôturée","29280","TELGRUC SUR MER","FINISTERE","BRETAGNE","Polygone",-4.353844,48.22734]
["SSP000209301",null,"Ancienne décharge de Lanenos",null,"Clôturée",null,null,"Clôturée","29293","TREGUNC","FINISTERE","BRETAGNE","Polygone",-3.854707,47.835243]
["SSP000209701","69.0158","Les émulsions de Feyzin",null,"Clôturée",null,"2002-08-15","Clôturée","69276","FEYZIN","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.8546557,45.674114]
["SSP000210101",null,"Ancienne décharge de Garzuel",null,"Clôturée",null,null,"Clôturée","29016","BRASPARTS","FINISTERE","BRETAGNE","Polygone",-3.961634,48.311897]
["SSP000211101",null,"Ancienne décharge de Lanouarzec",null,"Clôturée",null,null,"Clôturée","29241","ROSPORDEN","FINISTERE","BRETAGNE","Polygone",-3.7896636,47.957127]
["SSP000211201",null,"Ancienne décharge de Villeneuve Cadol",null,"Clôturée",null,null,"Clôturée","29241","ROSPORDEN","FINISTERE","BRETAGNE","Polygone",-3.8366637,47.953163]
["SSP000211601",null,"ancienne décharge de Kerguestoc",null,"Clôturée",null,null,"Clôturée","29280","TELGRUC SUR MER","FINISTERE","BRETAGNE","Polygone",-4.373871,48.24404]
["SSP000211701",null,"Ancienne décharge de Mané Lohac",null,"Clôturée",null,null,"Clôturée","56164","PLOEREN","MORBIHAN","BRETAGNE","Polygone",-2.8655064,47.63273]
["SSP000211801",null,"Ancienne décharge de la Grande Lande de la Haie",null,"Clôturée",null,null,"Clôturée","56053","ELVEN","MORBIHAN","BRETAGNE","Polygone",-2.581711,47.7191]
["SSP000211901",null,"Ancienne décharge de Gréavo",null,"Clôturée",null,null,"Clôturée","56088","ILE D'ARZ","MORBIHAN","BRETAGNE","Polygone",-2.8055916,47.5879]
["SSP000212001",null,"Ancienne décharge du Marais du Moulin",null,"Clôturée",null,null,"Clôturée","56088","ILE D'ARZ","MORBIHAN","BRETAGNE","Polygone",-2.8007395,47.595913]
["SSP000212101",null,"Ancienne décharge du stade",null,"Clôturée",null,null,"Clôturée","56259","LA TRINITE SURZUR","MORBIHAN","BRETAGNE","Polygone",-2.6010995,47.60905]
["SSP000212301",null,"Ancienne décharge de Saint Goustan",null,"Clôturée",null,null,"Clôturée","56251","THEIX","MORBIHAN","BRETAGNE","Polygone",-2.7099044,47.645874]
["SSP000212401",null,"Ancienne décharge de Bonnervo",null,"Clôturée",null,null,"Clôturée","56251","THEIX","MORBIHAN","BRETAGNE","Polygone",-2.682726,47.646908]
["SSP000212501","31.0030","LACROIX TOUS ARTIFICES SA",null,"En cours",null,null,"En cours","31395","MURET","HAUTE-GARONNE","OCCITANIE","Polygone",1.3389016,43.475395,"D8 - Poudres et explosifs"]
["SSP000212601",null,"Ancienne décharge communale",null,"Clôturée",null,null,"Clôturée","56254","TREDION","MORBIHAN","BRETAGNE","Polygone",-2.5913534,47.7928]
["SSP000212701","27.0034","Agence d'exploitation d'EDF / GDF",null,"En cours",null,null,"En cours","27375","LOUVIERS","EURE","NORMANDIE","Polygone",1.17655,49.21752]
["SSP000212801","27.0081","îlot Thorel ex-site Mennetrier Services Automobiles (MSA)",null,"En cours",null,null,"En cours","27375","LOUVIERS","EURE","NORMANDIE","Polygone",1.1676224,49.214752,"L2 - Transports, automobile, carburants"]
["SSP000212901","27.0093","LA PLAQUETTE",null,"En cours",null,null,"En cours","27375","LOUVIERS","EURE","NORMANDIE","Polygone",1.1789012,49.201527]
["SSP000213001","76.0036","ESSO RSAF - ancienne lagune MOBIL",null,"En cours",null,null,"En cours","76476","NOTRE DAME DE GRAVENCHON","SEINE-MARITIME","NORMANDIE","Polygone",0.57029253,49.47938,"D12 - Raffinage de pétrole, carburants et lubrifiants"]
["SSP000213101","76.0043","TERRAIN  C.B.L. JOUXTANT L'USINE ECO HUILE A LILLEBONNE",null,"En cours",null,null,"En cours","76384","LILLEBONNE","SEINE-MARITIME","NORMANDIE","Polygone",0.5288493,49.482395,"K41 - Régénération d'huiles"]
["SSP000213201","76.0060","Ancienne usine à gaz de Bolbec",null,"En cours",null,null,"En cours","76114","BOLBEC","SEINE-MARITIME","NORMANDIE","Polygone",0.46686324,49.572308,"J1 - Cokéfaction, usines à gaz"]
["SSP000213301","76.0101","Installation technique d'EDF",null,"En cours",null,null,"En cours","76164","CAUDEBEC EN CAUX","SEINE-MARITIME","NORMANDIE","Polygone",0.7218614,49.52778]
["SSP000213401","76.0120","TOTAL PETROCHEMICAL FRANCE - site de NDG",null,"En cours",null,null,"En cours","76476","NOTRE DAME DE GRAVENCHON","SEINE-MARITIME","NORMANDIE","Polygone",0.5576847,49.48847,"D33 - Pétrochimie carbochimie organique"]
["SSP000213501","76.0155","FRED AUTO (SARL)",null,"En cours",null,null,"En cours","76258","FAUVILLE EN CAUX","SEINE-MARITIME","NORMANDIE","Polygone",0.5930863,49.656338,"L23 - Détail de carburants"]
["SSP000213601","76.0208","UIOM Lillebonne (ancien site de l')",null,"En cours",null,null,"En cours","76384","LILLEBONNE","SEINE-MARITIME","NORMANDIE","Polygone",0.536821,49.497417]
["SSP000213701","76.0216","DUVAL",null,"En cours",null,null,"En cours","76494","PARC D'ANXTOT","SEINE-MARITIME","NORMANDIE","Polygone",0.4005609,49.583035]
["SSP000213801",null,"Ancienne décharge de Kermesquel",null,"Clôturée",null,null,"Clôturée","56260","VANNES","MORBIHAN","BRETAGNE","Polygone",-2.7750833,47.67082]
["SSP000213901",null,"Ancienne décharge de Kermain",null,"Clôturée",null,null,"Clôturée","56260","VANNES","MORBIHAN","BRETAGNE","Polygone",-2.7542868,47.633083]
["SSP000214001",null,"Ancienne décharge de la Zone Industrielle du Prat",null,"Clôturée",null,null,"Clôturée","56260","VANNES","MORBIHAN","BRETAGNE","Polygone",-2.7170177,47.652443]
["SSP000214201","56.0029","MANUFACTURE DES PNEUMATIQUES MICHELIN - PARTIE EN CESSATION",null,"En cours",null,null,"En cours","56260","VANNES","MORBIHAN","BRETAGNE","Polygone",-2.7095227,47.655224,"H13 - Traitement de surface"]
["SSP000214401",null,"Ancienne décharge de la ZA du Flachec",null,"Clôturée",null,null,"Clôturée","56015","BERRIC","MORBIHAN","BRETAGNE","Polygone",-2.531141,47.623363]
["SSP000214501",null,"Ancienne décharge de l'Epine",null,"Clôturée",null,null,"Clôturée","56111","LIMERZEL","MORBIHAN","BRETAGNE","Polygone",-2.3688166,47.672176]
["SSP000214601",null,"Ancienne décharge de Clergerel",null,"Clôturée",null,null,"Clôturée","56171","PLUHERLIN","MORBIHAN","BRETAGNE","Polygone",-2.4006128,47.691406]
["SSP000214701",null,"Ancienne décharge du Palud du Minlard",null,"Clôturée",null,null,"Clôturée","56002","AMBON","MORBIHAN","BRETAGNE","Polygone",-2.5615833,47.552654]
["SSP000214901",null,"Ancienne décharge de la route d'Arzal",null,"Clôturée",null,null,"Clôturée","56018","BILLIERS","MORBIHAN","BRETAGNE","Polygone",-2.4745913,47.527626]
["SSP000215001",null,"Ancienne décharge du Clos Hellec",null,"Clôturée",null,null,"Clôturée","56052","DAMGAN","MORBIHAN","BRETAGNE","Polygone",-2.5486045,47.531013]
["SSP000215101",null,"Ancienne décharge de Kerjanic",null,"Clôturée",null,null,"Clôturée","56126","MARZAN","MORBIHAN","BRETAGNE","Polygone",-2.354211,47.54083]
["SSP000215201",null,"Ancienne décharge de la Lande La Grée",null,"Clôturée",null,null,"Clôturée","56147","NIVILLAC","MORBIHAN","BRETAGNE","Polygone",-2.2798178,47.546833]
["SSP000215301",null,"Ancienne décharge de Bel Air",null,"Clôturée",null,null,"Clôturée","56149","NOYAL MUZILLAC","MORBIHAN","BRETAGNE","Polygone",-2.4609866,47.604424]
["SSP000215401",null,"Ancienne décharge de la Lande Rohelle",null,"Clôturée",null,null,"Clôturée","56149","NOYAL MUZILLAC","MORBIHAN","BRETAGNE","Polygone",-2.4845693,47.599575]
["SSP000215501",null,"Ancienne décharge de Cambony",null,"Clôturée",null,null,"Clôturée","56212","SAINT DOLAY","MORBIHAN","BRETAGNE","Polygone",-2.1669297,47.55533]
["SSP000215601","48.0002","Agence EDF / GDF Services",null,"En cours",null,"2010-10-20","En cours","48092","MARVEJOLS","LOZERE","OCCITANIE","Polygone",3.2921557,44.547382,"J1 - Cokéfaction, usines à gaz"]
["SSP000215701","48.0005","Mines du Mazel - Mas d'Orcières",null,"En cours",null,null,"En cours","48027","LE BLEYMARD","LOZERE","OCCITANIE","Polygone",3.728542,44.47303]
["SSP000215801","65.0002","SOULE \"Site principal\"",null,"En cours",null,null,"En cours","65059","BAGNERES DE BIGORRE","HAUTES-PYRENEES","OCCITANIE","Polygone",0.14236294,43.072014,"H - Mécanique, traitements des surfaces"]
["SSP000215901","65.0009","GIAT INDUSTRIES ( secteurs mécanique T68-2519 et pyrotechnique T68-xxxx)",null,"En cours",null,null,"En cours","65440","TARBES","HAUTES-PYRENEES","OCCITANIE","Polygone",0.07829867,43.24263,"H - Mécanique, traitements des surfaces"]
["SSP000216101","65.0012","INSTALLATION TECHNIQUE D'EDF GDF",null,"En cours",null,"2012-06-01","En cours","65059","BAGNERES DE BIGORRE","HAUTES-PYRENEES","OCCITANIE","Polygone",0.14705664,43.06951,"J1 - Cokéfaction, usines à gaz"]
["SSP000216201",null,"Ancienne décharge de la route de Tavardy",null,"Clôturée",null,null,"Clôturée","56040","CLEGUER","MORBIHAN","BRETAGNE","Polygone",-3.3840947,47.86212]
["SSP000216301","65.0013","CENTRE EDF GDF SERVICES",null,"En cours",null,null,"En cours","65440","TARBES","HAUTES-PYRENEES","OCCITANIE","Polygone",0.06407226,43.238487,"J1 - Cokéfaction, usines à gaz"]
["SSP000216501","65.0015","SOULE \"Site Egalité\"",null,"En cours",null,null,"En cours","65059","BAGNERES DE BIGORRE","HAUTES-PYRENEES","OCCITANIE","Polygone",0.15036942,43.07131,"H - Mécanique, traitements des surfaces"]
["SSP000216701","66.0001","Dynamiterie de PAULILLES",null,"En cours",null,null,"En cours","66148","PORT VENDRES","PYRENEES-ORIENTALES","OCCITANIE","Polygone",3.1227446,42.503563,"D81 - Poudres et explosifs (fabrication de)"]
["SSP000216801",null,"Ancienne décharge de la Route de Kerhierne",null,"Clôturée",null,null,"Clôturée","56063","GESTEL","MORBIHAN","BRETAGNE","Polygone",-3.4403539,47.819202]
["SSP000216901","66.0006","SNAG FRANCE TELECOM","SNAG FRANCE TELECOM","En cours",null,null,"En cours","66136","PERPIGNAN","PYRENEES-ORIENTALES","OCCITANIE","Polygone",2.8675423,42.685013,null,null,"50.2Z - Entretien et réparation de véhicules automobiles"]
["SSP000217001","66.0007","Centre EDF-GDF Services",null,"En cours",null,null,"En cours","66136","PERPIGNAN","PYRENEES-ORIENTALES","OCCITANIE","Polygone",2.8845572,42.688602,"J1 - Cokéfaction, usines à gaz"]
["SSP000217101","66.0019","SHELL Perpignan",null,"En cours",null,null,"En cours","66136","PERPIGNAN","PYRENEES-ORIENTALES","OCCITANIE","Polygone",2.9204915,42.696377,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000217201","66.0020","Station service Actif Autos",null,"En cours",null,null,"En cours","66008","ARGELES SUR MER","PYRENEES-ORIENTALES","OCCITANIE","Polygone",3.0180008,42.550064,"L2 - Transports, automobile, carburants"]
["SSP000217301","81.0001","SODAIN",null,"En cours",null,null,"En cours","81273","SAIX","TARN","OCCITANIE","Polygone",2.1421993,43.592598,"K42 - Régénération de solvants"]
["SSP000217401","82.0003","DELMAS LUMINAIRES",null,"En cours",null,null,"En cours","82121","MONTAUBAN","TARN-ET-GARONNE","OCCITANIE","Polygone",1.3739458,44.034576,"H13 - Traitement de surface"]
["SSP000217501","82.0004","CENTRE EDF GDF (ANCIENNE USINE A GAZ)",null,"En cours",null,null,"En cours","82186","VALENCE","TARN-ET-GARONNE","OCCITANIE","Polygone",0.89176947,44.104626,"J1 - Cokéfaction, usines à gaz"]
["SSP000217601","82.0009","INCINERATEUR DE NEGREPELISSE",null,"En cours",null,null,"En cours","82134","NEGREPELISSE","TARN-ET-GARONNE","OCCITANIE","Polygone",1.5244215,44.040344,"K2 - Traitement de déchets urbains"]
["SSP000217701","82.0010","INCINERATEUR D'AUVILLAR",null,"En cours",null,null,"En cours","82008","AUVILLAR","TARN-ET-GARONNE","OCCITANIE","Polygone",0.89532655,44.060207,"K2 - Traitement de déchets urbains"]
["SSP000217901",null,"Ancienne décharge de Beatus",null,"Clôturée",null,null,"Clôturée","56078","GUIDEL","MORBIHAN","BRETAGNE","Polygone",-3.4931827,47.802696]
["SSP000218101",null,"Ancienne décharge du Loch",null,"Clôturée",null,null,"Clôturée","56078","GUIDEL","MORBIHAN","BRETAGNE","Polygone",-3.5091472,47.754936]
["SSP000218201",null,"Ancienne décharge de La Becquerie",null,"Clôturée",null,null,"Clôturée","56083","HENNEBONT","MORBIHAN","BRETAGNE","Polygone",-3.2858276,47.79084]
["SSP000218401",null,"Ancienne décharge de Malachappe",null,"Clôturée",null,null,"Clôturée","56098","LANESTER","MORBIHAN","BRETAGNE","Polygone",-3.310576,47.780914]
["SSP000218701",null,"Ancienne décharge de Kermavic",null,"Clôturée",null,null,"Clôturée","56101","LANGUIDIC","MORBIHAN","BRETAGNE","Polygone",-3.1952217,47.80808]
["SSP000218901",null,"Ancienne décharge de Coet Megan",null,"Clôturée",null,null,"Clôturée","56101","LANGUIDIC","MORBIHAN","BRETAGNE","Polygone",-3.1628528,47.819794]
["SSP000219001",null,"Ancienne décharge de Kervern",null,"Clôturée",null,null,"Clôturée","56118","LOCMIQUELIC","MORBIHAN","BRETAGNE","Polygone",-3.3339076,47.732487]
["SSP000219101",null,"Ancienne décharge de Kerdual",null,"Clôturée",null,null,"Clôturée","56185","QUEVEN","MORBIHAN","BRETAGNE","Polygone",-3.3773396,47.769684]
["SSP000219201",null,"ETS - Collège et SEGPA Anita Conti",null,"Clôturée",null,null,"Clôturée","56121","LORIENT","MORBIHAN","BRETAGNE","Polygone",-3.3803735,47.73646]
["SSP000219301",null,"Ancienne décharge du Couregant",null,"Clôturée",null,null,"Clôturée","56162","PLOEMEUR","MORBIHAN","BRETAGNE","Polygone",-3.4657867,47.710575]
["SSP000219401",null,"Ancienne décharge de Kerham",null,"Clôturée",null,null,"Clôturée","56162","PLOEMEUR","MORBIHAN","BRETAGNE","Polygone",-3.481462,47.717983]
["SSP000219501",null,"Ancienne décharge du Roch",null,"Clôturée",null,null,"Clôturée","56162","PLOEMEUR","MORBIHAN","BRETAGNE","Polygone",-3.4546287,47.70897]
["SSP000219701",null,"Ancienne décharge de Toulgodo",null,"Clôturée",null,null,"Clôturée","56166","PLOUAY","MORBIHAN","BRETAGNE","Polygone",-3.285433,47.94245]
["SSP000219901",null,"Ancienne décharge des Deux Moulins",null,"Clôturée",null,null,"Clôturée","56193","RIANTEC","MORBIHAN","BRETAGNE","Polygone",-3.338731,47.709736]
["SSP000220001",null,"Ancienne décharge de Kerbillet",null,"Clôturée",null,null,"Clôturée","56014","BERNE","MORBIHAN","BRETAGNE","Polygone",-3.39704,47.985966]
["SSP000220101",null,"Ancienne décharge de la Grotte",null,"Clôturée",null,null,"Clôturée","56049","CROIXANVEC","MORBIHAN","BRETAGNE","Polygone",-2.857851,48.137085]
["SSP000220201",null,"Ancienne décharge de Pont Colin",null,"Clôturée",null,null,"Clôturée","56113","LOCMALO","MORBIHAN","BRETAGNE","Polygone",-3.1769037,48.05015]
["SSP000220301",null,"Ancienne décharge de Miné Nonnénou",null,"Clôturée",null,null,"Clôturée","56081","GUISCRIFF","MORBIHAN","BRETAGNE","Polygone",-3.612173,48.00827]
["SSP000220401",null,"Ancienne décharge de Guervillan",null,"Clôturée",null,null,"Clôturée","56093","KERGRIST","MORBIHAN","BRETAGNE","Polygone",-2.919276,48.139126]
["SSP000220501",null,"Ancienne décharge du Parc Ty Gadic Bihan",null,"Clôturée",null,null,"Clôturée","56105","LANVENEGEN","MORBIHAN","BRETAGNE","Polygone",-3.5391808,47.99429]
["SSP000220601",null,"Ancienne décharge de Plohair",null,"Clôturée",null,null,"Clôturée","56048","LE CROISTY","MORBIHAN","BRETAGNE","Polygone",-3.3610747,48.070282]
["SSP000220701",null,"Ancienne décharge de Kerbloch",null,"Clôturée",null,null,"Clôturée","56057","LE FAOUET","MORBIHAN","BRETAGNE","Polygone",-3.5059164,48.04289]
["SSP000220801",null,"Ancienne décharge du Parc-Lann-Bihan",null,"Clôturée",null,null,"Clôturée","56201","LE SAINT","MORBIHAN","BRETAGNE","Polygone",-3.5777564,48.09162]
["SSP000220901","56.0023","LE GALL",null,"Clôturée",null,null,"Clôturée","56246","LE SOURN","MORBIHAN","BRETAGNE","Polygone",-2.9624298,48.044403,"K52 - Dépôts de ferraille"]
["SSP000221101",null,"Ancienne décharge de Beg er Lann",null,"Clôturée",null,null,"Clôturée","56131","MESLAN","MORBIHAN","BRETAGNE","Polygone",-3.4412045,47.9913]
["SSP000221201",null,"Ancienne décharge de la Bechette",null,"Clôturée",null,null,"Clôturée","56047","CREDIN","MORBIHAN","BRETAGNE","Polygone",-2.7757556,48.036034]
["SSP000221301",null,"Ancienne décharge du Hinger",null,"Clôturée",null,null,"Clôturée","56110","LIGNOL","MORBIHAN","BRETAGNE","Polygone",-3.2720857,48.02385]
["SSP000221401",null,"Ancienne décharge de Poulvern",null,"Clôturée",null,null,"Clôturée","56151","NOYAL PONTIVY","MORBIHAN","BRETAGNE","Polygone",-2.8908234,48.008858]
["SSP000221501","54.0024","STATION SHELL","Pollution accidentelle aux hydrocarbures 1997","En cours",null,null,"En cours","54265","HOUDEMONT","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",6.183785,48.644215,"L23 - Détail de carburants"]
["SSP000221601","54.0004","Usine de la société MINES DE BOUXVILLER","Pollution accidentelle 1972","En cours",null,null,"En cours","54300","LANEUVEVILLE DEVANT NANCY","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",6.255804,48.64186]
["SSP000221701","54.0087","ALSTOM MOTEURS","Cessation d'activités 2001","En cours",null,null,"En cours","54395","NANCY","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",6.187248,48.702366,"H1 - Mécanique, électrique, traitement de surface"]
["SSP000221801",null,"Ancienne décharge sauvage de Quélloué",null,"Clôturée",null,null,"Clôturée","56151","NOYAL PONTIVY","MORBIHAN","BRETAGNE","Polygone",-2.9207275,48.06341]
["SSP000221901",null,"Ancienne décharge sauvage du Bourg",null,"Clôturée",null,null,"Clôturée","56160","PLEUGRIFFET","MORBIHAN","BRETAGNE","Polygone",-2.6894877,47.989166]
["SSP000222001","54.0116","Gare SNCF","Cessation d'activtés 2010","En cours",null,null,"En cours","54395","NANCY","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",6.1797256,48.68595,"L13 - Entrepôts de produits dangereux"]
["SSP000222101",null,"Ancienne décharge sauvage de la rue Henri Gaillard",null,"Clôturée",null,null,"Clôturée","56178","PONTIVY","MORBIHAN","BRETAGNE","Polygone",-2.976107,48.061504]
["SSP000222201","54.0123","ONYX EST/ SOULIER EST SNC","Cessation d'activités 2011","En cours",null,null,"En cours","54300","LANEUVEVILLE DEVANT NANCY","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",6.2234282,48.66203,"K - Déchets et traitements"]
["SSP000222301","54.0094","CALDIC","Cessation d'activités","Clôturée",null,null,"Clôturée","54328","LUDRES","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",6.192829,48.609684,"D3 - Chimie, phytosanitaire, pharmacie"]
["SSP000222401",null,"Ancienne décharge de la rue Jean Moulin",null,"Clôturée",null,null,"Clôturée","56178","PONTIVY","MORBIHAN","BRETAGNE","Polygone",-2.9581494,48.06267]
["SSP000222601","54.0005","ANCIEN DEPOT TOTAL, LOTISSEMENT DE REMENAUVILLE","Polution aux hydrocarbures","Clôturée",null,"2004-07-22","Clôturée","54395","NANCY","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",6.1991663,48.684532,null,null,"51.1C - Intermédiaires du commerce en combustibles, métaux, minéraux et produits chimiques"]
["SSP000222701",null,"Ancienne décharge de l'avenue Parmentier",null,"Clôturée",null,null,"Clôturée","56178","PONTIVY","MORBIHAN","BRETAGNE","Polygone",-2.9591928,48.06214]
["SSP000222801","54.0090","Ancienne Chaudronnerie Lorraine","Découverte terres polluées","En cours",null,null,"En cours","54395","NANCY","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",6.181261,48.705162,"J53 - Travail des métaux, chaudronnerie, poudres"]
["SSP000223001","54.0026","Ancienne usine à gaz NANCY ILE DE CORSE",null,"En cours",null,null,"En cours","54395","NANCY","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",6.1905484,48.694016,"J1 - Cokéfaction, usines à gaz"]
["SSP000223101","54.0041","Site RIMMA","Pollution découverte lors de travaux","En cours",null,null,"En cours","54395","NANCY","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",6.2035017,48.690693,"K2 - Traitement de déchets urbains"]
["SSP000223201","54.0099","STATION SERVICE TOTAL - RUE DE TOMBLAINE","Cessation d'activités 2004","Clôturée",null,"2008-12-18","Clôturée","54395","NANCY","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",6.202195,48.686718,"L23 - Détail de carburants"]
["SSP000223301","54.0074","Station TOTAL - LAROCHE",null,"En cours",null,null,"En cours","54395","NANCY","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",6.1918645,48.68932]
["SSP000223401","31.0026","FERRONNERIES DU MIDI Usine de l'Embouchure / ZAC des Ponts Jumeaux",null,"En cours",null,null,"En cours","31555","TOULOUSE","HAUTE-GARONNE","OCCITANIE","Polygone",1.4227895,43.612778,null,"20.01 - Fonderie de métaux ferreux"]
["SSP000223501","54.0136","Station TOTAL Jeanne d'Arc","Cessation d'activités 2010","En cours",null,null,"En cours","54395","NANCY","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",6.1759963,48.67928,null,null,"50.5Z - Commerce de détail de carburants"]
["SSP000223601","54.0111","Ancienne station-service OIL FRANCE","Cessation d'activités 2008","En cours",null,null,"En cours","54482","SAINT MAX","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",6.206114,48.7004,null,null,"50.5Z - Commerce de détail de carburants"]
["SSP000223701","54.0118","Garage DUROC - MARC ANGE",null,"En cours",null,null,"En cours","54547","VANDOEUVRE LES NANCY","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",6.1753626,48.67174]
["SSP000223801",null,"Ancienne décharge de Saint Michel",null,"Clôturée",null,null,"Clôturée","56178","PONTIVY","MORBIHAN","BRETAGNE","Polygone",-2.9680312,48.053642]
["SSP000223901",null,"Ancienne décharge de la Garenne",null,"Clôturée",null,null,"Clôturée","56189","RADENAC","MORBIHAN","BRETAGNE","Polygone",-2.6859236,47.94846]
["SSP000224001","88.0064","FAURECIA SIEGES D'AUTOMOBILE",null,"En cours",null,null,"En cours","88082","CELLES SUR PLAINE","VOSGES","GRAND EST","Polygone",6.942222,48.449116,"H1 - Mécanique, électrique, traitement de surface"]
["SSP000224101","88.0001","INTERNATIONAL DECOR (ex ALPHA DECORATION)",null,"En cours",null,null,"En cours","88082","CELLES SUR PLAINE","VOSGES","GRAND EST","Polygone",6.9526324,48.460167,"H1 - Mécanique, électrique, traitement de surface"]
["SSP000224201",null,"Ancienne décharge de canal de l'Oust",null,"Clôturée",null,null,"Clôturée","56198","ROHAN","MORBIHAN","BRETAGNE","Polygone",-2.7653856,48.077145]
["SSP000224301",null,"Ancienne carrière et décharge de Sylvestre",null,"Clôturée",null,null,"Clôturée","56242","SEGLIEN","MORBIHAN","BRETAGNE","Polygone",-3.1350477,48.113976]
["SSP000224401","88.0043","COVERIGHT SURFACES FRANCE SNC",null,"En cours",null,null,"En cours","88011","ARCHES","VOSGES","GRAND EST","Polygone",6.5356326,48.11545,"C23 - Transformation de papiers et carton"]
["SSP000224501","30.0020","Ancienne usine à gaz",null,"En cours",null,null,"En cours","30189","NIMES","GARD","OCCITANIE","Polygone",4.3669295,43.831234,"J1 - Cokéfaction, usines à gaz"]
["SSP000224701",null,"Ancienne décharge de la Tranchée d'Hilvern",null,"Clôturée",null,null,"Clôturée","56215","SAINT GONNERY","MORBIHAN","BRETAGNE","Polygone",-2.84052,48.11427]
["SSP000224801",null,"Ancien dépôt de mâchefers",null,"Clôturée",null,null,"Clôturée","56178","PONTIVY","MORBIHAN","BRETAGNE","Polygone",-2.965423,48.041367]
["SSP000224901","88.0050","Cartonnerie Jacquemin",null,"En cours",null,null,"En cours","88135","DOCELLES","VOSGES","GRAND EST","Polygone",6.621976,48.14532,"C2 - Industrie du papier et du carton"]
["SSP000225001",null,"Ancienne décharge des Grèves de Fontreven",null,"Clôturée",null,null,"Clôturée","22081","HILLION","COTES-D'ARMOR","BRETAGNE","Polygone",-2.6760128,48.51184]
["SSP000225101",null,"Ancienne décharge des Grèves du Pont du Gué Plat",null,"Clôturée",null,null,"Clôturée","22081","HILLION","COTES-D'ARMOR","BRETAGNE","Polygone",-2.6701539,48.49244]
["SSP000225301",null,"Ancienne décharge des Aubiers",null,"Clôturée",null,null,"Clôturée","22081","HILLION","COTES-D'ARMOR","BRETAGNE","Polygone",-2.6651018,48.49521]
["SSP000225401","88.0026","Ancienne usine à gaz d'Epinal",null,"En cours",null,null,"En cours","88160","EPINAL","VOSGES","GRAND EST","Polygone",6.446226,48.185043]
["SSP000225501",null,"Ancienne décharge du Fiche",null,"Clôturée",null,null,"Clôturée","22081","HILLION","COTES-D'ARMOR","BRETAGNE","Polygone",-2.6358976,48.475155]
["SSP000225601",null,"Ancienne décharge des Clos des Vergers",null,"Clôturée",null,null,"Clôturée","22144","LA MEAUGON","COTES-D'ARMOR","BRETAGNE","Polygone",-2.8418295,48.50471]
["SSP000225701","88.0002","CHARPENTE HOUOT SA",null,"En cours",null,null,"En cours","88196","GERARDMER","VOSGES","GRAND EST","Polygone",6.878579,48.07638,"C1 - Bois et de l'ameublement (industrie du)"]
["SSP000225801",null,"Ancienne décharge de Saint Barthélémy",null,"Clôturée",null,null,"Clôturée","22144","LA MEAUGON","COTES-D'ARMOR","BRETAGNE","Polygone",-2.8282504,48.51536]
["SSP000225901","88.0036","NP VOSGES (ex-FAURECIA SENONES)",null,"En cours",null,null,"En cours","88346","LA PETITE RAON","VOSGES","GRAND EST","Polygone",6.99784,48.40866,"D7 - Caoutchouc et matières plastiques"]
["SSP000226001","88.0044","Filature de Laveline",null,"En cours",null,null,"En cours","88262","LAVELINE DEVANT BRUYERES","VOSGES","GRAND EST","Polygone",6.7555003,48.182392,"E1 - Textile et habillement, teinture, impression"]
["SSP000226101","88.0010","YERAMEX INTERNATIONAL (ex COPLAC)",null,"En cours",null,null,"En cours","88444","LE SAULCY","VOSGES","GRAND EST","Polygone",7.056763,48.4185]
["SSP000226201","88.0068","SEB Le Syndicat",null,"En cours",null,null,"En cours","88462","LE SYNDICAT","VOSGES","GRAND EST","Polygone",6.6705146,48.01737,"H1 - Mécanique, électrique, traitement de surface"]
["SSP000226301","88.0015","Société SOVOS, ex-tanneries GROSJEAN",null,"En cours",null,"2008-05-28","En cours","88468","LE THILLOT","VOSGES","GRAND EST","Polygone",6.7671514,47.872818,"E21 - Tannerie, mégisserie"]
["SSP000226401","88.0059","SISOV Lerrain",null,"En cours",null,null,"En cours","88267","LERRAIN","VOSGES","GRAND EST","Polygone",6.153896,48.15278,"K31 - Incinération"]
["SSP000226501","88.0034","Founchot Ressa Industrie",null,"En cours",null,null,"En cours","88270","LIFFOL LE GRAND","VOSGES","GRAND EST","Polygone",5.5896626,48.31223]
["SSP000226601","88.0069","ABRAMANTE",null,"En cours",null,null,"En cours","88319","MOYENMOUTIER","VOSGES","GRAND EST","Polygone",6.8818464,48.375862]
["SSP000226701",null,"Ancienne décharge des Fontenelles",null,"Clôturée",null,null,"Clôturée","22106","LANGUEUX","COTES-D'ARMOR","BRETAGNE","Polygone",-2.7363274,48.49719]
["SSP000226801","88.0070","Founchot Nouvelle Industrie",null,"En cours",null,null,"En cours","88270","LIFFOL LE GRAND","VOSGES","GRAND EST","Polygone",5.5776944,48.31163]
["SSP000226901","88.0027","Ancienne usine à gaz de Neufchateau",null,"En cours",null,null,"En cours","88321","NEUFCHATEAU","VOSGES","GRAND EST","Polygone",5.697052,48.34977]
["SSP000227001","88.0020","COMPAGNIE DE DEVELOPPEMENT TEXTILE (CDT) - Usine de tissage",null,"En cours",null,null,"En cours","88327","NOMEXY","VOSGES","GRAND EST","Polygone",6.382727,48.311096]
["SSP000227101",null,"Ancienne décharge de Craffaud",null,"Clôturée",null,null,"Clôturée","22176","PLEDRAN","COTES-D'ARMOR","BRETAGNE","Polygone",-2.7833982,48.44786]
["SSP000227401","88.0045","COMPAGNIE DE DEVELOPPEMENT TEXTILE (CDT) - Usine de teinture",null,"En cours",null,null,"En cours","88327","NOMEXY","VOSGES","GRAND EST","Polygone",6.386935,48.303974,"E1 - Textile et habillement, teinture, impression"]
["SSP000227501","88.0055","Filature de Chenimenil",null,"En cours",null,null,"En cours","88327","NOMEXY","VOSGES","GRAND EST","Polygone",6.388557,48.303062,"E1 - Textile et habillement, teinture, impression"]
["SSP000227701","88.0004","Ancienne décharge de la verrerie-cristallerie de Portieux",null,"En cours",null,null,"En cours","88355","PORTIEUX","VOSGES","GRAND EST","Polygone",6.391921,48.348034]
["SSP000227801","88.0073","Equipement cuisine et bain (ECB)",null,"En cours",null,null,"En cours","88357","POUSSAY","VOSGES","GRAND EST","Polygone",6.126928,48.310177,"C12 - Produits en bois, ameublement (fabrication de)"]
["SSP000227901",null,"Ancienne décharge des Tronchets",null,"Clôturée",null,null,"Clôturée","22215","PLOUFRAGAN","COTES-D'ARMOR","BRETAGNE","Polygone",-2.8277059,48.47078]
["SSP000228001",null,"Ancienne décharge de La Ville au Beau",null,"Clôturée",null,null,"Clôturée","22215","PLOUFRAGAN","COTES-D'ARMOR","BRETAGNE","Polygone",-2.8214712,48.524216]
["SSP000228201",null,"Ancienne décharge du Haut de la Côte",null,"Clôturée",null,null,"Clôturée","22215","PLOUFRAGAN","COTES-D'ARMOR","BRETAGNE","Polygone",-2.8113804,48.51735]
["SSP000228301","88.0053","Compagnie Pétrolière de l'Est (CPE)",null,"En cours",null,null,"En cours","88372","RAON L'ETAPE","VOSGES","GRAND EST","Polygone",6.846503,48.408997,"L2 - Transports, automobile, carburants"]
["SSP000228501","88.0012","GRUPO ANTOLIN VOSGES (EX MERITOR LYS FRANCE, EX ROCKWELL)",null,"Clôturée",null,"2016-07-25","Clôturée","88408","RUPT SUR MOSELLE","VOSGES","GRAND EST","Polygone",6.6621404,47.923233,"H1 - Mécanique, électrique, traitement de surface"]
["SSP000228601",null,"Ancienne décharge du Pont de Pierre",null,"Clôturée",null,null,"Clôturée","22215","PLOUFRAGAN","COTES-D'ARMOR","BRETAGNE","Polygone",-2.8097682,48.50876]
["SSP000228701","88.0039","Ancienne Concession PEUGEOT",null,"En cours",null,null,"En cours","88413","SAINT DIE DES VOSGES","VOSGES","GRAND EST","Polygone",6.962116,48.277275,"D72 - Transformation des matières plastiques"]
["SSP000228801","88.0071","ESSO SAF",null,"En cours",null,null,"En cours","88413","SAINT DIE DES VOSGES","VOSGES","GRAND EST","Polygone",6.9558115,48.279667]
["SSP000228901",null,"Ancienne décharge du Terrain de Manoeuvre",null,"Clôturée",null,null,"Clôturée","22215","PLOUFRAGAN","COTES-D'ARMOR","BRETAGNE","Polygone",-2.789978,48.48091]
["SSP000229001","88.0054","Cartonnerie Jacquemin",null,"En cours",null,null,"En cours","88424","SAINTE MARGUERITE","VOSGES","GRAND EST","Polygone",6.9790406,48.27734,"C22 - Fabrication de papiers et carton"]
["SSP000229101","88.0023","CEF Sarl (Compagnie Européenne de Fonderie)",null,"En cours",null,null,"En cours","88442","SAPOIS","VOSGES","GRAND EST","Polygone",6.7482305,48.01549,"J5 - Fonderie et travail des métaux"]
["SSP000229301","88.0011","Anciennes lagunes de BLANCHISSERIE TEINTURERIE DE THAON (BTT)",null,"En cours",null,null,"En cours","88465","THAON LES VOSGES","VOSGES","GRAND EST","Polygone",6.430286,48.251656,"E13 - Blanchiment, teinture, impression"]
["SSP000229401","22.0002","ANCIENNE SAVONNERIE ETABLISSEMENTS RENAUD-LUCIENNE",null,"En cours",null,null,"En cours","22215","PLOUFRAGAN","COTES-D'ARMOR","BRETAGNE","Polygone",-2.7802513,48.503757,"D62 - Fabrication de détergents"]
["SSP000229501","88.0057","SEB",null,"En cours",null,null,"En cours","88498","VECOUX","VOSGES","GRAND EST","Polygone",6.647817,47.97681,"H1 - Mécanique, électrique, traitement de surface"]
["SSP000229601","88.0083","GERMAIN Frères (H3C)",null,"En cours",null,null,"En cours","88500","VENTRON","VOSGES","GRAND EST","Polygone",6.8781447,47.931355]
["SSP000229701","88.0077","YERAMEX - Décharge de VIEUX MOULIN",null,"En cours",null,null,"En cours","88506","VIEUX MOULIN","VOSGES","GRAND EST","Polygone",7.0022454,48.39991]
["SSP000229801",null,"Ancienne décharge de la Ville Gouault",null,"Clôturée",null,null,"Clôturée","22251","PORDIC","COTES-D'ARMOR","BRETAGNE","Polygone",-2.7885816,48.564053]
["SSP000229901","88.0060","SISOV Xertigny",null,"En cours",null,null,"En cours","88530","XERTIGNY","VOSGES","GRAND EST","Polygone",6.4092903,48.049706,"K31 - Incinération"]
["SSP000230001",null,"Ancienne décharge de Tournemine",null,"Clôturée",null,null,"Clôturée","22251","PORDIC","COTES-D'ARMOR","BRETAGNE","Polygone",-2.7779608,48.568382]
["SSP000230101","88.0100","SOUCHE PAPERS",null,"En cours",null,null,"En cours","88009","ANOULD","VOSGES","GRAND EST","Polygone",6.95177,48.195637]
["SSP000230201",null,"Ancienne décharge de Berrien",null,"Clôturée",null,null,"Clôturée","22278","SAINT BRIEUC","COTES-D'ARMOR","BRETAGNE","Polygone",-2.8069754,48.52685]
["SSP000230301",null,"Ancienne décharge de la place de la Liberté",null,"Clôturée",null,null,"Clôturée","22278","SAINT BRIEUC","COTES-D'ARMOR","BRETAGNE","Polygone",-2.7520251,48.509697]
["SSP000230401","22.0017","Ancienne usine à gaz",null,"En cours",null,null,"En cours","22278","SAINT BRIEUC","COTES-D'ARMOR","BRETAGNE","Polygone",-2.7565913,48.523525,"J1 - Cokéfaction, usines à gaz"]
["SSP000230501",null,"Ancienne décharge de L'Hôtel d'en Haut",null,"Clôturée",null,null,"Clôturée","22287","SAINT DONAN","COTES-D'ARMOR","BRETAGNE","Polygone",-2.876912,48.467236]
["SSP000230701",null,"Ancienne décharge de la Coudraie",null,"Clôturée",null,null,"Clôturée","22307","SAINT JULIEN","COTES-D'ARMOR","BRETAGNE","Polygone",-2.806115,48.442818]
["SSP000230801",null,"Ancienne décharge du Bois de Craffaut",null,"Clôturée",null,null,"Clôturée","22307","SAINT JULIEN","COTES-D'ARMOR","BRETAGNE","Polygone",-2.8012564,48.453575]
["SSP000230901","55.0040","SARAP Industrie et ANTHEA (ex-SME)",null,"En cours",null,null,"En cours","55009","ANCEMONT","MEUSE","GRAND EST","Polygone",5.4067855,49.06728]
["SSP000231001","55.0034","AIR LIQUIDE WELDING FRANCE",null,"En cours",null,null,"En cours","55122","COMMERCY","MEUSE","GRAND EST","Polygone",5.579079,48.77234,"H1 - Mécanique, électrique, traitement de surface"]
["SSP000231101","55.0028","ANCIENNE USINE AMSU",null,"En cours",null,null,"En cours","55132","COUSANCES LES FORGES","MEUSE","GRAND EST","Polygone",5.0789475,48.60814,"H1 - Mécanique, électrique, traitement de surface"]
["SSP000231201","55.0038","DUKER",null,"En cours",null,null,"En cours","55132","COUSANCES LES FORGES","MEUSE","GRAND EST","Polygone",5.081533,48.613396]
["SSP000231301","55.0017","Ancienne goudronnerie",null,"En cours",null,null,"En cours","55545","VERDUN","MEUSE","GRAND EST","Polygone",5.3633757,49.149628,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000231401","55.0029","Ancienne station-service OIL FRANCE",null,"En cours",null,null,"En cours","55545","VERDUN","MEUSE","GRAND EST","Polygone",5.396778,49.151493]
["SSP000231501","55.0035","Les Liants de L'Est",null,"En cours",null,null,"En cours","55545","VERDUN","MEUSE","GRAND EST","Polygone",5.38328,49.165943]
["SSP000231601","54.0028","Dépôt pétrolier BP Fuel Services (ex SSLC)","Pollution aux hydrocarbures","En cours",null,null,"En cours","54300","LANEUVEVILLE DEVANT NANCY","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",6.2251043,48.6617,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000231701","54.0072","Usine LA ROCHETTE","Pollution au Plomb et HAP","En cours",null,"2007-03-08","En cours","54300","LANEUVEVILLE DEVANT NANCY","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",6.22755,48.660023,"C - Bois, papier et carton"]
["SSP000231801","54.0020","ANCIEN DEPOT SHELL","Pollution aux hydrocarbures 1997","Clôturée",null,"2004-07-22","Clôturée","54395","NANCY","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",6.1684227,48.679306,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000231901","54.0092","Ancienne station-service Total - Relais du Charmois","Cessation d'activités de 2000","Clôturée",null,"2008-12-18","Clôturée","54547","VANDOEUVRE LES NANCY","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",6.168914,48.668358,"L23 - Détail de carburants"]
["SSP000232101","88.0005","Ancienne décharge de la papeterie ARJO-WIGGINS (devenu MUNKSJO)",null,"En cours",null,null,"En cours","88358","POUXEUX","VOSGES","GRAND EST","Polygone",6.549881,48.115124,"C22 - Fabrication de papiers et carton"]
["SSP000232201","88.0079","Station-service intermarché",null,"En cours",null,null,"En cours","88196","GERARDMER","VOSGES","GRAND EST","Polygone",6.8725405,48.074257]
["SSP000232301",null,"Ancienne décharge du Moulin Danguy",null,"Clôturée",null,null,"Clôturée","22001","ALLINEUC","COTES-D'ARMOR","BRETAGNE","Polygone",-2.8711514,48.30879]
["SSP000232401","57.0176","Garage de la vallée",null,"En cours",null,null,"En cours","57017","AMANVILLERS","MOSELLE","GRAND EST","Polygone",6.0502305,49.167717,"K5 - Récupération, dépôts de ferrailles"]
["SSP000232501","57.0037","Ancienne usine FORGES et BOULONNERIES",null,"En cours",null,null,"En cours","57032","ARS SUR MOSELLE","MOSELLE","GRAND EST","Polygone",6.085569,49.080822]
["SSP000232601",null,"Ancienne décharge des caves",null,"Clôturée",null,null,"Clôturée","22002","ANDEL","COTES-D'ARMOR","BRETAGNE","Polygone",-2.576494,48.494507]
["SSP000232701","57.0139","DECHARGE ESKA",null,"En cours",null,null,"En cours","57447","MARLY","MOSELLE","GRAND EST","Polygone",6.1475387,49.0782]
["SSP000232901","57.0119","Sotrameuse",null,"En cours",null,null,"En cours","57463","METZ","MOSELLE","GRAND EST","Polygone",6.2395983,49.10662,"L2 - Transports, automobile, carburants"]
["SSP000233001","57.0028","Anciens Ets. ZILHARDT et STAUB",null,"En cours",null,null,"En cours","57463","METZ","MOSELLE","GRAND EST","Polygone",6.162691,49.132454]
["SSP000233201","57.0102","Site SIGHI - BARADE",null,"En cours",null,null,"En cours","57463","METZ","MOSELLE","GRAND EST","Polygone",6.1604004,49.1299,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000233301","57.0019","ANCIENNE USINE A GAZ MONTIGNY",null,"En cours",null,null,"En cours","57480","MONTIGNY LES METZ","MOSELLE","GRAND EST","Polygone",6.161295,49.097485,"J1 - Cokéfaction, usines à gaz"]
["SSP000233401",null,"Ancienne décharge de la Roc'h Huon Vhelan",null,"Clôturée",null,null,"Clôturée","22004","BEGARD","COTES-D'ARMOR","BRETAGNE","Polygone",-3.2584755,48.625813]
["SSP000233501",null,"Ancienne décharge de Galvezan",null,"Clôturée",null,null,"Clôturée","22005","BELLE ISLE EN TERRE","COTES-D'ARMOR","BRETAGNE","Polygone",-3.3933005,48.531525]
["SSP000233601","57.0131","ROLANFER",null,"En cours",null,null,"En cours","57751","WOIPPY","MOSELLE","GRAND EST","Polygone",6.157292,49.150455,"J53 - Travail des métaux, chaudronnerie, poudres"]
["SSP000233801",null,"Ancienne décharge du marais de la Grande Motte",null,"Clôturée",null,null,"Clôturée","22007","BINIC","COTES-D'ARMOR","BRETAGNE","Polygone",-2.8386128,48.599026]
["SSP000234301",null,"Ancienne décharge du terrain de football",null,"Clôturée",null,null,"Clôturée","22008","BOBITAL","COTES-D'ARMOR","BRETAGNE","Polygone",-2.1043046,48.407303]
["SSP000234401",null,"Ancienne décharge du Rocher commun",null,"Clôturée",null,null,"Clôturée","22008","BOBITAL","COTES-D'ARMOR","BRETAGNE","Polygone",-2.105241,48.419296]
["SSP000234501",null,"Ancienne décharge de la Chapelle de la Pitié",null,"Clôturée",null,null,"Clôturée","22011","BOQUEHO","COTES-D'ARMOR","BRETAGNE","Polygone",-2.9848905,48.474167]
["SSP000234601",null,"Ancienne décharge des Forges",null,"Clôturée",null,null,"Clôturée","22013","BOURBRIAC","COTES-D'ARMOR","BRETAGNE","Polygone",-3.1763,48.48988]
["SSP000234701","57.0082","Train à fil de Rombas",null,"En cours",null,null,"En cours","57019","AMNEVILLE","MOSELLE","GRAND EST","Polygone",6.1391706,49.263916,"J23 - Première transformation de l'acier"]
["SSP000234801","57.0091","KORSEC INDUSTRIE",null,"En cours",null,null,"En cours","57287","BASSE HAM","MOSELLE","GRAND EST","Polygone",6.2183685,49.37594,"K52 - Dépôts de ferraille"]
["SSP000234901","57.0001","Société TRI",null,"En cours",null,null,"En cours","57073","BETTING","MOSELLE","GRAND EST","Polygone",6.8180175,49.140152,"K - Déchets et traitements"]
["SSP000235001",null,"Ancienne décharge de la Roblinais",null,"Clôturée",null,null,"Clôturée","22014","BOURSEUL","COTES-D'ARMOR","BRETAGNE","Polygone",-2.2638423,48.494526]
["SSP000235101","57.0145","Mayer et Fils",null,"En cours",null,null,"En cours","57134","CHATEL SAINT GERMAIN","MOSELLE","GRAND EST","Polygone",6.0825663,49.119873,"M1 - Industries diverses"]
["SSP000235201",null,"Ancienne décharge de la Ville Vain",null,"Clôturée",null,null,"Clôturée","22014","BOURSEUL","COTES-D'ARMOR","BRETAGNE","Polygone",-2.2379,48.489227]
["SSP000235401",null,"Ancienne décharge de La Croix Beauvais",null,"Clôturée",null,null,"Clôturée","22015","BREHAND","COTES-D'ARMOR","BRETAGNE","Polygone",-2.5786529,48.378963]
["SSP000235501",null,"Ancienne décharge de la Croix Launay",null,"Clôturée",null,null,"Clôturée","22015","BREHAND","COTES-D'ARMOR","BRETAGNE","Polygone",-2.5857158,48.38928]
["SSP000235601","57.0066","CRISTALLERIE DE HARTZVILLER",null,"En cours",null,null,"En cours","57299","HARTZVILLER","MOSELLE","GRAND EST","Polygone",7.081939,48.67248,"G15 - Industrie du verre"]
["SSP000235701","57.0132","La Platinerie",null,"En cours",null,null,"En cours","57306","HAYANGE","MOSELLE","GRAND EST","Polygone",6.0684185,49.328407,"J - Sidérurgie, métallurgie, coke"]
["SSP000235901","57.0093","Lorraine Zingage et Clemens",null,"En cours",null,null,"En cours","57200","LES ETANGS","MOSELLE","GRAND EST","Polygone",6.37887,49.142567,"H13 - Traitement de surface"]
["SSP000235902","57.0094","Lorraine Zingage et Clemens",null,"En cours",null,null,"En cours","57200","LES ETANGS","MOSELLE","GRAND EST","Polygone",6.37887,49.142567,"H13 - Traitement de surface"]
["SSP000236001","57.0053","MIM",null,"En cours",null,null,"En cours","57460","MERTEN","MOSELLE","GRAND EST","Polygone",6.662695,49.244694,"H13 - Traitement de surface"]
["SSP000236101","57.0044","SOCIETE NOUVELLE FONDERIE DE ZINC",null,"En cours",null,null,"En cours","57463","METZ","MOSELLE","GRAND EST","Polygone",6.1583014,49.131107,"J52 - Fonderie des métaux non ferreux"]
["SSP000236201","57.0227","SOTRALLE",null,"En cours",null,null,"En cours","57466","METZING","MOSELLE","GRAND EST","Polygone",6.9576354,49.088776]
["SSP000236301","57.0196","ALTIA Saint Hélène",null,"En cours",null,null,"En cours","57474","MONDELANGE","MOSELLE","GRAND EST","Polygone",6.1622853,49.256504]
["SSP000236401","57.0108","ANCIENNE USINE A GAZ MORHANGE",null,"En cours",null,null,"En cours","57483","MORHANGE","MOSELLE","GRAND EST","Polygone",6.634857,48.919846]
["SSP000236601","57.0218","Ancienne usine BATA (puis HELLO SA)",null,"Clôturée",null,"2015-04-17","Clôturée","57488","MOUSSEY","MOSELLE","GRAND EST","Polygone",6.808535,48.68313]
["SSP000236701","57.0075","Ancienne cokerie de Moyeuvre-Grande",null,"En cours",null,null,"En cours","57491","MOYEUVRE GRANDE","MOSELLE","GRAND EST","Polygone",6.062052,49.252514,"J1 - Cokéfaction, usines à gaz"]
["SSP000236801",null,"Ancienne décharge de Cambel",null,"Clôturée",null,null,"Clôturée","22020","BROONS","COTES-D'ARMOR","BRETAGNE","Polygone",-2.2511444,48.27972]
["SSP000236901",null,"Ancien dépôt de fioul",null,"Clôturée",null,null,"Clôturée","22020","BROONS","COTES-D'ARMOR","BRETAGNE","Polygone",-2.2592425,48.318848]
["SSP000237001","57.0076","Crassiers du Perotin et du Conroy et bassins à boues",null,"En cours",null,null,"En cours","57492","MOYEUVRE PETITE","MOSELLE","GRAND EST","Polygone",6.020558,49.266766,"K36 - Mise en décharge"]
["SSP000237101","57.0194","Faïencerie de Niderviller",null,"En cours",null,null,"En cours","57505","NIDERVILLER","MOSELLE","GRAND EST","Polygone",7.105357,48.71321,"G12 - Fabrication de produits céramiques"]
["SSP000237301","57.0084","Anciens Hauts-Fourneaux de Rombas",null,"En cours",null,null,"En cours","57591","ROMBAS","MOSELLE","GRAND EST","Polygone",6.1106153,49.259315,"J21 - Production de fontes (haut fourneau)"]
["SSP000237401","57.0101","Ancienne usine sidérurgique de Jamailles",null,"En cours",null,null,"En cours","57597","ROSSELANGE","MOSELLE","GRAND EST","Polygone",6.068837,49.254234,"J2 - Sidérurgie, première transformation"]
["SSP000237501","57.0018","Ancienne cokerie de Micheville",null,"En cours",null,null,"En cours","57603","RUSSANGE","MOSELLE","GRAND EST","Polygone",5.941875,49.48052]
["SSP000237601","57.0062","MIROITERIE DU PLAN INCLINE",null,"En cours",null,null,"En cours","57618","SAINT LOUIS","MOSELLE","GRAND EST","Polygone",7.221935,48.718235,"G15 - Industrie du verre"]
["SSP000237701","57.0167","ANCIENNE USINE A GAZ SARREBOURG",null,"En cours",null,null,"En cours","57630","SARREBOURG","MOSELLE","GRAND EST","Polygone",7.0442457,48.733303,"J1 - Cokéfaction, usines à gaz"]
["SSP000237801","57.0068","Ancienne usine SESA",null,"En cours",null,null,"En cours","57631","SARREGUEMINES","MOSELLE","GRAND EST","Polygone",7.076625,49.118896,"J52 - Fonderie des métaux non ferreux"]
["SSP000238001","57.0006","Dépôt de pneus et de RBA de la société TRI",null,"En cours",null,null,"En cours","57631","SARREGUEMINES","MOSELLE","GRAND EST","Polygone",7.077101,49.101887]
["SSP000238101","57.0043","Anciens crassier et laminoirs de TERVILLE",null,"En cours",null,null,"En cours","57666","TERVILLE","MOSELLE","GRAND EST","Polygone",6.1402016,49.339153]
["SSP000238301","31.0081","ALMAMET",null,"En cours",null,null,"En cours","31316","MARIGNAC","HAUTE-GARONNE","OCCITANIE","Polygone",0.65202993,42.9201]
["SSP000238401","57.0109","Ancienne usine à gaz de Thionville",null,"En cours",null,null,"En cours","57672","THIONVILLE","MOSELLE","GRAND EST","Polygone",6.157841,49.347122,"J1 - Cokéfaction, usines à gaz"]
["SSP000238501","57.0090","Ancienne usine sidérurgique de Thionville",null,"En cours",null,null,"En cours","57672","THIONVILLE","MOSELLE","GRAND EST","Polygone",6.1564713,49.337666]
["SSP000238701","57.0080","Crassier de Volkrange",null,"En cours",null,null,"En cours","57672","THIONVILLE","MOSELLE","GRAND EST","Polygone",6.08666,49.35115,"K36 - Mise en décharge"]
["SSP000238801",null,"Ancien stockage de déchets de marées noires de Caroual Ouest",null,"Clôturée",null,null,"Clôturée","22054","ERQUY","COTES-D'ARMOR","BRETAGNE","Polygone",-2.4825103,48.615715]
["SSP000238901","57.0070","ETILAM","ETILAM","En cours",null,null,"En cours","57672","THIONVILLE","MOSELLE","GRAND EST","Polygone",6.177423,49.365253]
["SSP000239001",null,"Ancien stockage de déchets de marées noires de La Lande Jual",null,"Clôturée",null,null,"Clôturée","22054","ERQUY","COTES-D'ARMOR","BRETAGNE","Polygone",-2.481056,48.61649]
["SSP000239101","57.0078","Crasier d'Uckange et ancien parc des matières premières","Ancien crassier d'Uckange","En cours",null,null,"En cours","57683","UCKANGE","MOSELLE","GRAND EST","Polygone",6.1626506,49.3149,"J - Sidérurgie, métallurgie, coke | K36 - Mise en décharge"]
["SSP000239102","57.0127","Crasier d'Uckange et ancien parc des matières premières",null,"En cours",null,null,"En cours","57683","UCKANGE","MOSELLE","GRAND EST","Polygone",6.1628265,49.315228,"J - Sidérurgie, métallurgie, coke | K36 - Mise en décharge"]
["SSP000239201","57.0079","Ancienne agglomération d'Uckange",null,"En cours",null,null,"En cours","57683","UCKANGE","MOSELLE","GRAND EST","Polygone",6.15858,49.303944,"J2 - Sidérurgie, première transformation"]
["SSP000239301","57.0125","Ancienne usine à cyanamide",null,"En cours",null,null,"En cours","57683","UCKANGE","MOSELLE","GRAND EST","Polygone",6.155389,49.313457,"D3 - Chimie, phytosanitaire, pharmacie"]
["SSP000239401","54.0001","CRASSIER DE LA SOCIETE C.F.C. DAUM","Cessation d'activités 1992","En cours",null,null,"En cours","54010","ALLAMPS","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",5.800368,48.540833,null,null,null,"38.11Z - Collecte des déchets non dangereux"]
["SSP000239501","54.0030","CRASSIER ET ANCIENNE USINE D'AUBOUE",null,"En cours",null,null,"En cours","54028","AUBOUE","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",5.9804,49.216553,"J21 - Production de fontes (haut fourneau)"]
["SSP000239601","65.0010","BOSTIK",null,"En cours",null,null,"En cours","65226","IBOS","HAUTES-PYRENEES","OCCITANIE","Polygone",-0.013647501,43.242,"D44 - Fabrication de colles et mastics"]
["SSP000239701","54.0101","PASEK France",null,"En cours",null,null,"En cours","54055","BAYONVILLE SUR MAD","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",5.999447,49.01521,"G12 - Fabrication de produits céramiques"]
["SSP000239801","82.0012","CIMENTERIE LAFARGE",null,"En cours",null,null,"En cours","82187","VAREN","TARN-ET-GARONNE","OCCITANIE","Polygone",1.8921019,44.145477,"G11 - Fabrication de chaux, ciment, plâtre"]
["SSP000239901","54.0031","CRASSIER et BASSIN à BOUES de MOULAINE",null,"En cours",null,null,"En cours","54254","HAUCOURT MOULAINE","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",5.8113856,49.513477,"K36 - Mise en décharge"]
["SSP000240201","54.0039","USINE de MOULAINE",null,"En cours",null,null,"En cours","54254","HAUCOURT MOULAINE","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",5.816245,49.506573,"J21 - Production de fontes (haut fourneau)"]
["SSP000240301","81.0007","ETERNIT ETABLISSEMENT D'ALBI-TERSSAC",null,"En cours",null,null,"En cours","81297","TERSSAC","TARN","OCCITANIE","Polygone",2.0769553,43.921116,"G13 - Fabrication de produits en amiante-ciment"]
["SSP000240401","81.0013","CRASSIER DU SAUT DU TARN",null,"En cours",null,null,"En cours","81257","SAINT JUERY","TARN","OCCITANIE","Polygone",2.2184408,43.95223,"J22 - Production d'acier brut, aciéries"]
["SSP000240501",null,"Ancien stockage de déchets de marées noires de la Roche Pilange",null,"Clôturée",null,null,"Clôturée","22054","ERQUY","COTES-D'ARMOR","BRETAGNE","Polygone",-2.479265,48.617844]
["SSP000240601","54.0017","COS-SIH",null,"En cours",null,null,"En cours","54261","HERSERANGE","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",5.803818,49.52232,"I - Energie"]
["SSP000240701","81.0017","MEGISSERIE GRAULHETOISE SA (Occupant du site : Les Plasticiens Volants)",null,"En cours",null,null,"En cours","81105","GRAULHET","TARN","OCCITANIE","Polygone",1.9751301,43.76575,"E21 - Tannerie, mégisserie"]
["SSP000240901","54.0035","Site du PYLONE - Crassier et bassin à boues d'HERSERANGE (AMREF)",null,"En cours",null,null,"En cours","54261","HERSERANGE","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",5.7875934,49.51176,"J2 - Sidérurgie, première transformation"]
["SSP000241001",null,"Ancien stockage de déchets de marées noires de Bon Abri",null,"Clôturée",null,null,"Clôturée","22081","HILLION","COTES-D'ARMOR","BRETAGNE","Polygone",-2.651665,48.524708]
["SSP000241101","54.0069","Train à fil (TAF) d'Herserange",null,"En cours",null,null,"En cours","54261","HERSERANGE","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",5.8109407,49.520676,"J21 - Production de fontes (haut fourneau)"]
["SSP000241301",null,"Ancien stockage de déchets de marées noires de la Pointe du Paon",null,"Clôturée",null,null,"Clôturée","22016","ILE DE BREHAT","COTES-D'ARMOR","BRETAGNE","Polygone",-2.9906256,48.863808]
["SSP000241501","54.0009","USINE DE SENELLE (AMF)",null,"En cours",null,null,"En cours","54261","HERSERANGE","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",5.780739,49.51448,"J2 - Sidérurgie, première transformation"]
["SSP000241601","81.0020","ANCIENNE MEGISSERIE AZAM ET CIE SARL",null,"Clôturée",null,"2017-04-04","Clôturée","81105","GRAULHET","TARN","OCCITANIE","Polygone",1.9994093,43.77158,"E21 - Tannerie, mégisserie"]
["SSP000241801","54.0120","ARCELORMITTAL - Crombillon - Crassier et Bassins à boues",null,"En cours",null,null,"En cours","54263","HOMECOURT","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",6.000133,49.22735]
["SSP000241901",null,"Ancien stockage de déchets de marées noires Ile à Poules",null,"Clôturée",null,null,"Clôturée","22085","KERBORS","COTES-D'ARMOR","BRETAGNE","Polygone",-3.1839032,48.841]
["SSP000242101","54.0014","Hauts Fourneaux Réunis de Saulnes et Uckange (HFRSU)",null,"En cours",null,null,"En cours","54270","HUSSIGNY GODBRANGE","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",5.8649154,49.49939,"J2 - Sidérurgie, première transformation"]
["SSP000242201","81.0024","MEGISSERIE DE BELLEVUE",null,"En cours",null,null,"En cours","81105","GRAULHET","TARN","OCCITANIE","Polygone",1.9990515,43.770885,"E21 - Tannerie, mégisserie"]
["SSP000242301",null,"Ancien stockage de déchets de marées noires de Truzugal",null,"Clôturée",null,null,"Clôturée","22134","LOUANNEC","COTES-D'ARMOR","BRETAGNE","Polygone",-3.4269845,48.79792]
["SSP000242401","81.0025","PEYRUSSE ET CIE",null,"En cours",null,"2005-05-27","En cours","81105","GRAULHET","TARN","OCCITANIE","Polygone",1.9996412,43.761017,"E21 - Tannerie, mégisserie"]
["SSP000242501","81.0031","AGENCE EDF GDF (ANCIENNE USINE A GAZ)",null,"En cours",null,"2012-06-01","En cours","81163","MAZAMET","TARN","OCCITANIE","Polygone",2.378,43.495785,"J1 - Cokéfaction, usines à gaz"]
["SSP000242601",null,"Ancien stockage de déchets de marées noires de Kerespert",null,"Clôturée",null,null,"Clôturée","22134","LOUANNEC","COTES-D'ARMOR","BRETAGNE","Polygone",-3.404724,48.796646]
["SSP000242701","54.0034","Ancienne usine de JOEUF",null,"En cours",null,null,"En cours","54280","JOEUF","MEURTHE-ET-MOSELLE","GRAND EST","Point",0.0,0.0,"J21 - Production de fontes (haut fourneau)"]
["SSP000242801","81.0032","AGENCES D'EXPLOITATION EDF ET GDF",null,"En cours",null,"2012-06-01","En cours","81004","ALBI","TARN","OCCITANIE","Polygone",2.141967,43.93556,"J1 - Cokéfaction, usines à gaz"]
["SSP000242901","81.0033","EDF - CENTRE DE PRODUCTION THERMIQUE",null,"En cours",null,null,"En cours","81004","ALBI","TARN","OCCITANIE","Polygone",2.1404397,43.95314,"I11 - Centrales électriques thermiques"]
["SSP000243001",null,"Ancien stockage de déchets de marées noires de Douar Autret",null,"Clôturée",null,null,"Clôturée","22134","LOUANNEC","COTES-D'ARMOR","BRETAGNE","Polygone",-3.408255,48.7752]
["SSP000243101","81.0034","POURSINES-AZALBERT",null,"En cours",null,null,"En cours","81005","ALBINE","TARN","OCCITANIE","Polygone",2.535191,43.459217,"E2 - Industrie des cuirs et peaux, tannerie"]
["SSP000243201","81.0037","SOCIETE NOUVELLE DES ETABLISSEMENTS SENAT",null,"En cours",null,null,"En cours","81105","GRAULHET","TARN","OCCITANIE","Polygone",1.9754118,43.75999,"E21 - Tannerie, mégisserie"]
["SSP000243301","81.0039","Moulin de la Resse (CARAYOL, CARA'S CUIR)",null,"En cours",null,null,"En cours","81163","MAZAMET","TARN","OCCITANIE","Polygone",2.37637,43.481598,"E21 - Tannerie, mégisserie"]
["SSP000243401","81.0040","MOLINA SARL (RENOV' EMBAL)",null,"En cours",null,null,"En cours","81244","SAINT BENOIT DE CARMAUX","TARN","OCCITANIE","Polygone",2.140593,44.054375,"K3 - Traitement de déchets industriels"]
["SSP000243501","81.0041","MOLINA (enseigne commerciale : RENOV'EMBAL SUD SARL)",null,"En cours",null,null,"En cours","81105","GRAULHET","TARN","OCCITANIE","Polygone",2.0074048,43.762856,"K3 - Traitement de déchets industriels"]
["SSP000243601",null,"Ancien stockage de déchets de marées noires de la Ville Neuve",null,"Clôturée",null,null,"Clôturée","22135","LOUARGAT","COTES-D'ARMOR","BRETAGNE","Polygone",-3.3594947,48.5556]
["SSP000243901","81.0042","GAUBIL & FILS",null,"En cours",null,null,"En cours","81315","VIELMUR SUR AGOUT","TARN","OCCITANIE","Polygone",2.085219,43.61924,"E1 - Textile et habillement, teinture, impression"]
["SSP000244001","81.0043","Mégisserie de MIQUELOU",null,"En cours",null,null,"En cours","81105","GRAULHET","TARN","OCCITANIE","Polygone",2.0045903,43.762184,"E21 - Tannerie, mégisserie"]
["SSP000244201","81.0045","SOGECUIR",null,"En cours",null,null,"En cours","81105","GRAULHET","TARN","OCCITANIE","Polygone",1.9954209,43.76851,"E21 - Tannerie, mégisserie"]
["SSP000244301","81.0046","FINA-ALBENQUE",null,"En cours",null,null,"En cours","81065","CASTRES","TARN","OCCITANIE","Polygone",2.2390947,43.60939,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000244401","54.0011","Ancienne Cokerie à LONGLAVILLE - Confinement cokerie - AMF",null,"En cours",null,null,"En cours","54321","LONGLAVILLE","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",5.8015714,49.536884]
["SSP000244501","54.0108","ARCELORMITTAL REF LONGLAVILLE Confinement Ouest",null,"En cours",null,null,"En cours","54321","LONGLAVILLE","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",5.7925587,49.5367]
["SSP000244601","54.0107","PIMEST SARL (ex EUROGEP)","Pollution accidentelle","En cours",null,null,"En cours","54321","LONGLAVILLE","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",5.7954674,49.535732,"H1 - Mécanique, électrique, traitement de surface"]
["SSP000244701","54.0050","SLR Longlaville (crassier)","Pollution due au fonctionnement de l'installation","En cours",null,null,"En cours","54321","LONGLAVILLE","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",5.8116994,49.537197,null,null,"37.1Z - Récupération de matières métalliques recyclables"]
["SSP000244901",null,"Ancien stockage de déchets de marées noires du Sémaphore",null,"Clôturée",null,null,"Clôturée","22166","PENVENAN","COTES-D'ARMOR","BRETAGNE","Polygone",-3.3040032,48.830074]
["SSP000245001","54.0045","BASSIN à BOUES et CRASSIER de la BANNIE",null,"En cours",null,null,"En cours","54382","MONT SAINT MARTIN","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",5.7784295,49.534855,"K36 - Mise en décharge"]
["SSP000245101",null,"Ancien stockage de déchets de marées noires de Bellevue",null,"Clôturée",null,null,"Clôturée","22166","PENVENAN","COTES-D'ARMOR","BRETAGNE","Polygone",-3.2825515,48.833584]
["SSP000245201",null,"Ancienne décharge de déchets verts et ancien stockage de déchets de marées noires de Kergastel",null,"Clôturée",null,null,"Clôturée","22166","PENVENAN","COTES-D'ARMOR","BRETAGNE","Polygone",-3.3183305,48.823414]
["SSP000245401","54.0067","ancienne cokerie",null,"En cours",null,null,"En cours","54397","NEUVES MAISONS","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",6.124175,48.61089,"J1 - Cokéfaction, usines à gaz"]
["SSP000245501",null,"Ancien stockage de déchets de marées noires de Ploumanac'h",null,"Clôturée",null,null,"Clôturée","22168","PERROS GUIREC","COTES-D'ARMOR","BRETAGNE","Polygone",-3.4784465,48.827953]
["SSP000245601",null,"Ancienne décharge et ancien stockage de déchets de marées noires de Kergadic",null,"Clôturée",null,null,"Clôturée","22168","PERROS GUIREC","COTES-D'ARMOR","BRETAGNE","Polygone",-3.4666197,48.811142]
["SSP000245701","54.0007","Ancien complexe sidérurgique (Pompey)",null,"En cours",null,null,"En cours","54430","POMPEY","MEURTHE-ET-MOSELLE","GRAND EST","Point",0.0,0.0,"J22 - Production d'acier brut, aciéries"]
["SSP000245702","54.0137","Ancien complexe sidérurgique (Pompey)",null,"En cours",null,null,"En cours","54150","CUSTINES","MEURTHE-ET-MOSELLE","GRAND EST","Point",0.0,0.0,"J22 - Production d'acier brut, aciéries"]
["SSP000245801","54.0102","ANCIEN SITE SUTE",null,"En cours",null,null,"En cours","54431","PONT A MOUSSON","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",6.057793,48.906757,"D72 - Transformation des matières plastiques"]
["SSP000246001","81.0047","MEGISSERIE OCCITANE",null,"En cours",null,null,"En cours","81105","GRAULHET","TARN","OCCITANIE","Polygone",1.9932793,43.767826,"E21 - Tannerie, mégisserie"]
["SSP000246201","54.0043","Crassier pôle nord (AMF)",null,"En cours",null,null,"En cours","54451","REHON","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",5.745004,49.50812,"K36 - Mise en décharge"]
["SSP000246301","54.0042","CRASSIER de PULVENTEUX",null,"En cours",null,null,"En cours","54451","REHON","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",5.7474327,49.504505,"K36 - Mise en décharge"]
["SSP000246401",null,"Ancienne décharge et ancien stockage de déchets de marées noires de Kerzinan",null,"Clôturée",null,null,"Clôturée","22168","PERROS GUIREC","COTES-D'ARMOR","BRETAGNE","Polygone",-3.4834194,48.798996]
["SSP000246501","54.0012","Usine La Providence (AMREF) - REHON CUTRY LEXY",null,"En cours",null,null,"En cours","54451","REHON","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",5.7462916,49.501446,"J2 - Sidérurgie, première transformation"]
["SSP000246601","54.0038","BASSIN à BOUES de Saulnes",null,"En cours",null,null,"En cours","54493","SAULNES","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",5.819708,49.52641,"K36 - Mise en décharge"]
["SSP000246801","54.0040","CARREAU de la MINE d'ANDERNY",null,"En cours",null,null,"En cours","54536","TUCQUEGNIEUX","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",5.908146,49.321148,null,"56.01 - Récupération de ferraille et vieux métaux non ferreux"]
["SSP000247001","81.0048","MEGISSERIE LAINIERE",null,"En cours",null,null,"En cours","81105","GRAULHET","TARN","OCCITANIE","Polygone",2.0188937,43.76465,"E21 - Tannerie, mégisserie"]
["SSP000247101","55.0024","ANCIENNE USINE A GAZ COMMERCY",null,"En cours",null,null,"En cours","55122","COMMERCY","MEUSE","GRAND EST","Polygone",5.5988846,48.762924,"J1 - Cokéfaction, usines à gaz"]
["SSP000247301","55.0015","LA FUSION ELECTRIQUE (ex FONDERIES D'ACIER DE LORRAINE)",null,"En cours",null,null,"En cours","55502","STENAY","MEUSE","GRAND EST","Polygone",5.1887617,49.484554,"J51 - Fonderie des métaux ferreux"]
["SSP000247401",null,"Ancien stockage de déchets de marées noires de Port Ploumanac'h",null,"Clôturée",null,null,"Clôturée","22168","PERROS GUIREC","COTES-D'ARMOR","BRETAGNE","Polygone",-3.488213,48.825645]
["SSP000247501","55.0027","ANCIENNE DECHARGE DES FONDERIES DE VAUCOULEURS",null,"En cours",null,null,"En cours","55533","VAUCOULEURS","MEUSE","GRAND EST","Polygone",5.6458406,48.601795,"J51 - Fonderie des métaux ferreux"]
["SSP000247701",null,"Ancien stockage de déchets de marées noires de Ploumanac'h - Saint Guirec",null,"Clôturée",null,null,"Clôturée","22168","PERROS GUIREC","COTES-D'ARMOR","BRETAGNE","Polygone",-3.479471,48.82498]
["SSP000247801","81.0049","Mégisserie Saint HILAIRE (Raison socialez : SCI DES MARCHES)",null,"En cours",null,null,"En cours","81105","GRAULHET","TARN","OCCITANIE","Polygone",2.0629551,43.770607,"E21 - Tannerie, mégisserie"]
["SSP000247901","81.0051","SA ESCAPAT et CIE",null,"En cours",null,null,"En cours","81105","GRAULHET","TARN","OCCITANIE","Polygone",1.9980707,43.76103,"E21 - Tannerie, mégisserie"]
["SSP000248001","57.0121","Ancienne usine sidérurgique de La Paix",null,"En cours",null,null,"En cours","57012","ALGRANGE","MOSELLE","GRAND EST","Polygone",6.0357046,49.349037,"J2 - Sidérurgie, première transformation"]
["SSP000248101",null,"Ancien stockage de déchets de marées noires du Sémaphore",null,"Clôturée",null,null,"Clôturée","22168","PERROS GUIREC","COTES-D'ARMOR","BRETAGNE","Polygone",-3.4734411,48.82742]
["SSP000248601",null,"Ancien stockage de déchets de marées noires Les Vallées",null,"Clôturée",null,null,"Clôturée","22186","PLENEUF VAL ANDRE","COTES-D'ARMOR","BRETAGNE","Polygone",-2.5310743,48.593918]
["SSP000248701",null,"Ancien stockage de déchets de marées noires de Tournemine",null,"Clôturée",null,null,"Clôturée","22187","PLERIN","COTES-D'ARMOR","BRETAGNE","Polygone",-2.769681,48.555393]
["SSP000248801","57.0010","Anciennes cokerie et usine d'Hagondange",null,"En cours",null,null,"En cours","57283","HAGONDANGE","MOSELLE","GRAND EST","Polygone",6.152544,49.232666]
["SSP000248802","57.0118","Anciennes cokerie et usine d'Hagondange",null,"En cours",null,null,"En cours","57283","HAGONDANGE","MOSELLE","GRAND EST","Polygone",6.152544,49.232666]
["SSP000249101",null,"Ancien stockage de déchets de marées noires de Port Béni",null,"Clôturée",null,null,"Clôturée","22195","PLEUBIAN","COTES-D'ARMOR","BRETAGNE","Polygone",-3.1703537,48.848278]
["SSP000249201",null,"Ancienne décharge et Ancien stockage de déchets de marées noires de Pen Crec'h",null,"Clôturée",null,null,"Clôturée","22195","PLEUBIAN","COTES-D'ARMOR","BRETAGNE","Polygone",-3.152794,48.831734]
["SSP000249301","57.0040","Friche de l'ancienne usine de MOYEUVRE GRANDE",null,"En cours",null,null,"En cours","57491","MOYEUVRE GRANDE","MOSELLE","GRAND EST","Polygone",6.0545535,49.24912,"J2 - Sidérurgie, première transformation"]
["SSP000249501","54.0044","BASSINS à BOUES de CUTRY - REHON",null,"En cours",null,null,"En cours","54151","CUTRY","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",5.742902,49.49463,"K36 - Mise en décharge"]
["SSP000249601","54.0003","ANCIENNE USINE UNION FRANÇAISE DES PETROLES (U.F.P.)",null,"En cours",null,null,"En cours","54157","DIEULOUARD","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",6.070996,48.847828,"K41 - Régénération d'huiles"]
["SSP000249701","12.0007","BLANC AERO INDUSTRIES",null,"En cours",null,null,"En cours","12300","VILLEFRANCHE DE ROUERGUE","AVEYRON","OCCITANIE","Polygone",2.030889,44.34566,"H13 - Traitement de surface"]
["SSP000249801","54.0129","SOCIETE DU TRAIN UNIVERSEL DE LONGWY",null,"En cours",null,null,"En cours","54261","HERSERANGE","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",5.7937374,49.519756,"J53 - Travail des métaux, chaudronnerie, poudres"]
["SSP000249901","54.0015","USINE DE LA CHIERS",null,"En cours",null,null,"En cours","54323","LONGWY","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",5.7777004,49.52429,"J2 - Sidérurgie, première transformation"]
["SSP000250001","12.0008","ASP",null,"En cours",null,null,"En cours","12254","SALLES LA SOURCE","AVEYRON","OCCITANIE","Polygone",2.4827523,44.40815,"H14 - Application de peinture"]
["SSP000250101","54.0016","ANCIEN COMPLEXE SIDERURGIQUE DE MICHEVILLE",null,"En cours",null,null,"En cours","54580","VILLERUPT","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",5.933569,49.477272,"J2 - Sidérurgie, première transformation"]
["SSP000250301","12.0011","DECHARGE DU RUAU",null,"En cours",null,null,"En cours","12013","AUBIN","AVEYRON","OCCITANIE","Polygone",2.2976058,44.547012,"J5 - Fonderie et travail des métaux"]
["SSP000250501","54.0093","ANCIENNE USINE A GAZ DES CRISTALLERIES","Pollution due au fonctionnement de l'installation","En cours",null,null,"En cours","54039","BACCARAT","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",6.7316213,48.44987,"J1 - Cokéfaction, usines à gaz"]
["SSP000250601","12.0014","SETCM - CENTRALE DE BOISSE PENCHOT",null,"En cours",null,null,"En cours","12028","BOISSE PENCHOT","AVEYRON","OCCITANIE","Polygone",2.204965,44.577427,"I11 - Centrales électriques thermiques"]
["SSP000250701","12.0017","ABC ex SPCV ex VIEILLE MONTAGNE et KUHLMAN",null,"En cours",null,null,"En cours","12305","VIVIEZ","AVEYRON","OCCITANIE","Polygone",2.218247,44.548088,"G - Industries minérales"]
["SSP000250901","12.0020","GRAVIERE DE GRANDCHAMP ET LA PAYSSIERE",null,"En cours",null,null,"En cours","12101","FLAGNAC","AVEYRON","OCCITANIE","Polygone",2.2372441,44.60399,"F - Industries extractives"]
["SSP000251101","54.0065","Crassier rive droite",null,"En cours",null,null,"En cours","54397","NEUVES MAISONS","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",6.11149,48.606213,"K36 - Mise en décharge"]
["SSP000251201","12.0022","AGENCE EDF GDF",null,"Clôturée",null,null,"Clôturée","12300","VILLEFRANCHE DE ROUERGUE","AVEYRON","OCCITANIE","Polygone",2.039789,44.349228,"J1 - Cokéfaction, usines à gaz"]
["SSP000251301","54.0066","Crassier rive gauche",null,"En cours",null,null,"En cours","54397","NEUVES MAISONS","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",6.1225376,48.60451,"K36 - Mise en décharge"]
["SSP000251401","12.0023","ETABLISSEMENTS DURAND",null,"En cours",null,null,"En cours","12264","SEBAZAC CONCOURES","AVEYRON","OCCITANIE","Polygone",2.5939496,44.415524,"K52 - Dépôts de ferraille"]
["SSP000251501","12.0027","UMICORE  LAUBAREDE",null,"En cours",null,null,"En cours","12305","VIVIEZ","AVEYRON","OCCITANIE","Polygone",2.2188435,44.559742,"J52 - Fonderie des métaux non ferreux"]
["SSP000251601","12.0030","Collège public Amans-Joseph Fabre n° 0120101V",null,"En cours",null,null,"En cours","12202","RODEZ","AVEYRON","OCCITANIE","Polygone",2.5756145,44.353104]
["SSP000251801","57.0105","Bassin à boues du haut de Micheville",null,"En cours",null,null,"En cours","57603","RUSSANGE","MOSELLE","GRAND EST","Polygone",5.9311748,49.48227,"K36 - Mise en décharge"]
["SSP000251901","57.0126","ANCIENS HAUTS-FOURNEAUX D'UCKANGE",null,"En cours",null,null,"En cours","57683","UCKANGE","MOSELLE","GRAND EST","Polygone",6.1575155,49.306995,"J21 - Production de fontes (haut fourneau)"]
["SSP000252001","57.0081","Acierie et laminoirs de Rombas",null,"En cours",null,null,"En cours","57019","AMNEVILLE","MOSELLE","GRAND EST","Polygone",6.122208,49.260536,"J22 - Production d'acier brut, aciéries"]
["SSP000252101",null,"Ancien stockage de déchets de marées noires du Rugno",null,"Clôturée",null,null,"Clôturée","22195","PLEUBIAN","COTES-D'ARMOR","BRETAGNE","Polygone",-3.1224053,48.862984]
["SSP000252201",null,"Ancien stockage de déchets de marées noires de Brestan",null,"Clôturée",null,null,"Clôturée","22195","PLEUBIAN","COTES-D'ARMOR","BRETAGNE","Polygone",-3.1574614,48.851856]
["SSP000252401",null,"Ancien stockage de déchets de marées noires de Yelog",null,"Clôturée",null,null,"Clôturée","22195","PLEUBIAN","COTES-D'ARMOR","BRETAGNE","Polygone",-3.149353,48.853043]
["SSP000252501",null,"Ancien stockage de déchets de marées noires de Porz Ran",null,"Clôturée",null,null,"Clôturée","22195","PLEUBIAN","COTES-D'ARMOR","BRETAGNE","Polygone",-3.107424,48.86524]
["SSP000252701",null,"Ancien stockage de déchets de marées noires de Landrellec 1",null,"Clôturée",null,null,"Clôturée","22198","PLEUMEUR BODOU","COTES-D'ARMOR","BRETAGNE","Polygone",-3.5359662,48.809547]
["SSP000253001",null,"Ancien stockage de déchets de marées noires de L'Ile Grande - 1",null,"Clôturée",null,null,"Clôturée","22198","PLEUMEUR BODOU","COTES-D'ARMOR","BRETAGNE","Polygone",-3.5794978,48.804688]
["SSP000253101",null,"Ancien stockage de déchets de marées noires de L'Ile Grande - Corps de Garde",null,"Clôturée",null,null,"Clôturée","22198","PLEUMEUR BODOU","COTES-D'ARMOR","BRETAGNE","Polygone",-3.5723963,48.805466]
["SSP000253701",null,"Ancien stockage de déchets de marées noires de Landrellec 3",null,"Clôturée",null,null,"Clôturée","22198","PLEUMEUR BODOU","COTES-D'ARMOR","BRETAGNE","Polygone",-3.5344777,48.807533]
["SSP000253801",null,"Ancien stockage de déchets de marées noires de L'île Grande - 2",null,"Clôturée",null,null,"Clôturée","22198","PLEUMEUR BODOU","COTES-D'ARMOR","BRETAGNE","Polygone",-3.576848,48.79836]
["SSP000253901",null,"Ancien stockage de déchets de marées noires de L'île Grande - Porz Gwen",null,"Clôturée",null,null,"Clôturée","22198","PLEUMEUR BODOU","COTES-D'ARMOR","BRETAGNE","Polygone",-3.5759637,48.80338]
["SSP000254001",null,"Ancienne décharge et ancien stockage de déchets de marées noires de L'île Grande",null,"Clôturée",null,null,"Clôturée","22198","PLEUMEUR BODOU","COTES-D'ARMOR","BRETAGNE","Polygone",-3.5740905,48.804592]
["SSP000254201",null,"Ancien stockage de déchets de marées noires de Cornec",null,"Clôturée",null,null,"Clôturée","22210","PLOUBAZLANEC","COTES-D'ARMOR","BRETAGNE","Polygone",-3.0197268,48.820717]
["SSP000254301",null,"Ancien stockage de déchets de marées noires de l'Anse de Gouern",null,"Clôturée",null,null,"Clôturée","22210","PLOUBAZLANEC","COTES-D'ARMOR","BRETAGNE","Polygone",-3.0515642,48.81548]
["SSP000254401",null,"Ancien stockage de déchets de marées noires de Launay Mal Nommé",null,"Clôturée",null,null,"Clôturée","22210","PLOUBAZLANEC","COTES-D'ARMOR","BRETAGNE","Polygone",-3.0164545,48.808865]
["SSP000254501",null,"Ancien stockage de déchets de marées noires de Lezvellec",null,"Clôturée",null,null,"Clôturée","22210","PLOUBAZLANEC","COTES-D'ARMOR","BRETAGNE","Polygone",-3.0406337,48.790226]
["SSP000254601",null,"Ancien stockage de déchets de marées noires de la Grève de Porz Dun",null,"Clôturée",null,null,"Clôturée","22210","PLOUBAZLANEC","COTES-D'ARMOR","BRETAGNE","Polygone",-3.0237086,48.79483]
["SSP000254701",null,"Ancienne décharge et ancien stockage de déchets de marées noires de Gouërmel",null,"Clôturée",null,null,"Clôturée","22218","PLOUGRESCANT","COTES-D'ARMOR","BRETAGNE","Polygone",-3.2687263,48.833298]
["SSP000254801",null,"Ancien stockage de déchets de marées noires du Buchu",null,"Clôturée",null,null,"Clôturée","22218","PLOUGRESCANT","COTES-D'ARMOR","BRETAGNE","Polygone",-3.2310922,48.866165]
["SSP000254901",null,"Ancien stockage de déchets de marées noires du Gouffre",null,"Clôturée",null,null,"Clôturée","22218","PLOUGRESCANT","COTES-D'ARMOR","BRETAGNE","Polygone",-3.2331626,48.864952]
["SSP000255001",null,"Ancien stockage de déchets de marées noires de Kergonnet",null,"Clôturée",null,null,"Clôturée","22218","PLOUGRESCANT","COTES-D'ARMOR","BRETAGNE","Polygone",-3.2553813,48.84272]
["SSP000255101",null,"Ancien stockage de déchets de marées noires de l'Ile Yvinec",null,"Clôturée",null,null,"Clôturée","22218","PLOUGRESCANT","COTES-D'ARMOR","BRETAGNE","Polygone",-3.2604294,48.854404]
["SSP000255301",null,"Ancien stockage de déchets de marées noires de Crec'h Guezennec",null,"Clôturée",null,null,"Clôturée","22218","PLOUGRESCANT","COTES-D'ARMOR","BRETAGNE","Polygone",-3.2558155,48.84775]
["SSP000255401",null,"Ancien stockage de déchets de marées noires de la pointe du Château (Porz Bugalé)",null,"Clôturée",null,null,"Clôturée","22218","PLOUGRESCANT","COTES-D'ARMOR","BRETAGNE","Polygone",-3.225146,48.86905]
["SSP000255701",null,"Ancien stockage de déchets de marées noires du Gouffre - Fosse n°4",null,"Clôturée",null,null,"Clôturée","22218","PLOUGRESCANT","COTES-D'ARMOR","BRETAGNE","Polygone",-3.2371097,48.866104]
["SSP000255801","57.0117","BOYON",null,"Clôturée",null,"2015-04-17","Clôturée","57447","MARLY","MOSELLE","GRAND EST","Polygone",6.1386395,49.058403,"K36 - Mise en décharge"]
["SSP000255901",null,"Ancien stockage de déchets de marées noires de Gouërmel Guermeur",null,"Clôturée",null,null,"Clôturée","22218","PLOUGRESCANT","COTES-D'ARMOR","BRETAGNE","Polygone",-3.2623749,48.83475]
["SSP000256001",null,"Ancien stockage de déchets de marées noires de la pointe du Château",null,"Clôturée",null,null,"Clôturée","22218","PLOUGRESCANT","COTES-D'ARMOR","BRETAGNE","Polygone",-3.2293656,48.866768]
["SSP000256101",null,"Ancien stockage de déchets de marées noires de Porz Bugalé",null,"Clôturée",null,null,"Clôturée","22218","PLOUGRESCANT","COTES-D'ARMOR","BRETAGNE","Polygone",-3.2228181,48.86677]
["SSP000256201",null,"Ancien stockage de déchets de marées noires de Kergadiou",null,"Clôturée",null,null,"Clôturée","22218","PLOUGRESCANT","COTES-D'ARMOR","BRETAGNE","Polygone",-3.2242122,48.84839]
["SSP000256401",null,"Ancien stockage de déchets de marées noires du Palud",null,"Clôturée",null,null,"Clôturée","22221","PLOUGUIEL","COTES-D'ARMOR","BRETAGNE","Polygone",-3.2031245,48.834892]
["SSP000256501",null,"Ancien stockage de déchets de marées noires de la Pointe Jaune (Beg Melen)",null,"Clôturée",null,null,"Clôturée","22221","PLOUGUIEL","COTES-D'ARMOR","BRETAGNE","Polygone",-3.2069213,48.81379]
["SSP000256601",null,"Ancien stockage de déchets de marées noires de Croaz Min",null,"Clôturée",null,null,"Clôturée","22224","PLOULEC'H","COTES-D'ARMOR","BRETAGNE","Polygone",-3.5200896,48.72772]
["SSP000257201",null,"Ancien stockage de déchets de marées noires du Marais de Notenno 1 et 3",null,"Clôturée",null,null,"Clôturée","22343","TREBEURDEN","COTES-D'ARMOR","BRETAGNE","Polygone",-3.5684302,48.793144]
["SSP000257601",null,"Ancien stockage de déchets de marées noires du Marais de Kellen",null,"Clôturée",null,null,"Clôturée","22343","TREBEURDEN","COTES-D'ARMOR","BRETAGNE","Polygone",-3.5773973,48.78304]
["SSP000257701",null,"Ancien stockage de déchets de marées noires de Penvern",null,"Clôturée",null,null,"Clôturée","22343","TREBEURDEN","COTES-D'ARMOR","BRETAGNE","Polygone",-3.562317,48.79506]
["SSP000258201",null,"Ancien stockage de déchets de marées noires de La Pointe de Séhar",null,"Clôturée",null,null,"Clôturée","22349","TREDREZ LOCQUEMEAU","COTES-D'ARMOR","BRETAGNE","Polygone",-3.583668,48.725155]
["SSP000258501",null,"Ancien stockage de déchets de marées noires de la Pointe de Dourven",null,"Clôturée",null,null,"Clôturée","22349","TREDREZ LOCQUEMEAU","COTES-D'ARMOR","BRETAGNE","Polygone",-3.5628943,48.72977]
["SSP000258601",null,"Ancien stockage de déchets de marées noires de Roc'h Loarn Kerougant",null,"Clôturée",null,null,"Clôturée","22353","TREGASTEL","COTES-D'ARMOR","BRETAGNE","Polygone",-3.4979708,48.796074]
["SSP000258701",null,"Ancien stockage de déchets de marées noires de Tremarc'h",null,"Clôturée",null,null,"Clôturée","22353","TREGASTEL","COTES-D'ARMOR","BRETAGNE","Polygone",-3.4966962,48.80169]
["SSP000258801",null,"Ancien stockage de déchets de marées noires de Poul Palud",null,"Clôturée",null,null,"Clôturée","22353","TREGASTEL","COTES-D'ARMOR","BRETAGNE","Polygone",-3.499611,48.824986]
["SSP000258901","84.0024","CEREALIS (Ex Engrais VITAL)",null,"En cours",null,null,"En cours","84043","ENTRAIGUES SUR LA SORGUE","VAUCLUSE","PROVENCE-ALPES-COTE D'AZUR","Polygone",4.9323325,44.015724,"D3 - Chimie, phytosanitaire, pharmacie"]
["SSP000259001",null,"Ancien stockage de déchets de marées noires de L'Ile Renote 1",null,"Clôturée",null,null,"Clôturée","22353","TREGASTEL","COTES-D'ARMOR","BRETAGNE","Polygone",-3.509598,48.834774]
["SSP000259301",null,"Ancien stockage de déchets de marées noires du Grannec",null,"Clôturée",null,null,"Clôturée","22353","TREGASTEL","COTES-D'ARMOR","BRETAGNE","Polygone",-3.5324018,48.823402]
["SSP000259401",null,"Ancien stockage de déchets de marées noires la Grève Blanche",null,"Clôturée",null,null,"Clôturée","22353","TREGASTEL","COTES-D'ARMOR","BRETAGNE","Polygone",-3.5221145,48.829433]
["SSP000260101",null,"Ancien stockage de déchets de marées noires du Royau",null,"Clôturée",null,null,"Clôturée","22379","TREVOU TREGUIGNEC","COTES-D'ARMOR","BRETAGNE","Polygone",-3.340844,48.827797]
["SSP000260501",null,"Ancienne décharge et ancien stockage de déchets de marées noires de Kerlivou",null,"Clôturée",null,null,"Clôturée","22210","PLOUBAZLANEC","COTES-D'ARMOR","BRETAGNE","Polygone",-3.0355847,48.817924]
["SSP000260601",null,"Ancienne décharge de La Croisel Lande",null,"Clôturée",null,null,"Clôturée","22021","BRUSVILY","COTES-D'ARMOR","BRETAGNE","Polygone",-2.1363497,48.389797]
["SSP000260701",null,"Ancienne décharge de la Petite Tournée",null,"Clôturée",null,null,"Clôturée","22390","YVIAS","COTES-D'ARMOR","BRETAGNE","Polygone",-3.028194,48.71108]
["SSP000260801","80.0006","SHELL / Jardin des Peintres",null,"En cours",null,null,"En cours","80021","AMIENS","SOMME","HAUTS-DE-FRANCE","Polygone",2.2670193,49.90613,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000261101",null,"Ancienne décharge de Kerdudy",null,"Clôturée",null,null,"Clôturée","29075","GUIPAVAS","FINISTERE","BRETAGNE","Polygone",-4.404265,48.4225]
["SSP000261601",null,"Ancienne décharge de Lannouzec",null,"Clôturée",null,null,"Clôturée","22023","BULAT PESTIVIEN","COTES-D'ARMOR","BRETAGNE","Polygone",-3.3355584,48.42411]
["SSP000261701",null,"Ancienne décharge de la Voie Romaine",null,"Clôturée",null,null,"Clôturée","22024","CALANHEL","COTES-D'ARMOR","BRETAGNE","Polygone",-3.503603,48.446922]
["SSP000261801",null,"Ancienne décharge de Ker ar Pont",null,"Clôturée",null,null,"Clôturée","22024","CALANHEL","COTES-D'ARMOR","BRETAGNE","Polygone",-3.481013,48.438587]
["SSP000262001",null,"Ancienne décharge de Kerdrequen",null,"Clôturée",null,null,"Clôturée","22025","CALLAC","COTES-D'ARMOR","BRETAGNE","Polygone",-3.4607327,48.428898]
["SSP000262101",null,"Ancienne décharge de Kerhuel",null,"Clôturée",null,null,"Clôturée","22028","CAMLEZ","COTES-D'ARMOR","BRETAGNE","Polygone",-3.301618,48.79216]
["SSP000262401",null,"Ancienne décharge du Guer",null,"Clôturée",null,null,"Clôturée","22033","CAUREL","COTES-D'ARMOR","BRETAGNE","Polygone",-3.0615678,48.216198]
["SSP000262501",null,"Ancienne décharge de Keriven",null,"Clôturée",null,null,"Clôturée","22033","CAUREL","COTES-D'ARMOR","BRETAGNE","Polygone",-3.0555408,48.211815]
["SSP000262601",null,"Ancienne décharge de Plas Kerouern",null,"Clôturée",null,null,"Clôturée","22034","CAVAN","COTES-D'ARMOR","BRETAGNE","Polygone",-3.3481727,48.686565]
["SSP000262801","57.0029","Ancien dépôt MARCHAL",null,"En cours",null,null,"En cours","57463","METZ","MOSELLE","GRAND EST","Polygone",6.1592007,49.13076,"K5 - Récupération, dépôts de ferrailles"]
["SSP000262901","57.0138","SOFFAB",null,"En cours",null,null,"En cours","57463","METZ","MOSELLE","GRAND EST","Polygone",6.160932,49.1342]
["SSP000263001","57.0174","GOERIG",null,"En cours",null,null,"En cours","57019","AMNEVILLE","MOSELLE","GRAND EST","Polygone",6.133827,49.261116]
["SSP000263101","57.0199","Société TEXTILOR",null,"En cours",null,null,"En cours","57287","BASSE HAM","MOSELLE","GRAND EST","Polygone",6.2296276,49.375553]
["SSP000263301",null,"Ancienne décharge des Aulnays",null,"Clôturée",null,null,"Clôturée","22056","EVRAN","COTES-D'ARMOR","BRETAGNE","Polygone",-1.9880934,48.38236]
["SSP000263401",null,"Ancienne décharge du Runiat",null,"Clôturée",null,null,"Clôturée","22063","GOMMENEC'H","COTES-D'ARMOR","BRETAGNE","Polygone",-3.0539854,48.63181]
["SSP000263501",null,"Ancienne décharge de Pen ar Lan",null,"Clôturée",null,null,"Clôturée","22067","GRACES","COTES-D'ARMOR","BRETAGNE","Polygone",-3.1683176,48.541656]
["SSP000263601",null,"Ancienne décharge de La Ville Blanche",null,"Clôturée",null,null,"Clôturée","22067","GRACES","COTES-D'ARMOR","BRETAGNE","Polygone",-3.1661289,48.544456]
["SSP000263701",null,"Ancienne décharge de Cadolan",null,"Clôturée",null,null,"Clôturée","22070","GUINGAMP","COTES-D'ARMOR","BRETAGNE","Polygone",-3.1456687,48.55387]
["SSP000263901","57.0140","Ancien incinérateur de Dieuze",null,"En cours",null,null,"En cours","57177","DIEUZE","MOSELLE","GRAND EST","Polygone",6.733528,48.820255,"K2 - Traitement de déchets urbains"]
["SSP000264001","57.0123","Ancien site de la société KOCH",null,"En cours",null,null,"En cours","57177","DIEUZE","MOSELLE","GRAND EST","Polygone",6.7210135,48.82465,"K5 - Récupération, dépôts de ferrailles"]
["SSP000264101",null,"Ancienne décharge de La Croix Faut",null,"Clôturée",null,null,"Clôturée","22072","GURUNHUEL","COTES-D'ARMOR","BRETAGNE","Polygone",-3.3082416,48.517174]
["SSP000264201","57.0092","Cedest Engrais",null,"En cours",null,null,"En cours","57179","DISTROFF","MOSELLE","GRAND EST","Polygone",6.261679,49.335136,"D36 - Fabrication des engrais"]
["SSP000264301","57.0009","TOTAL FINA (ex DEA-CALMES)",null,"En cours",null,null,"En cours","57221","FLORANGE","MOSELLE","GRAND EST","Polygone",6.1526914,49.321014]
["SSP000264401",null,"Ancienne décharge de Belno",null,"Clôturée",null,null,"Clôturée","22075","HEMONSTOIR","COTES-D'ARMOR","BRETAGNE","Polygone",-2.8341315,48.167046]
["SSP000264501",null,"Ancienne décharge de Ténoquevel",null,"Clôturée",null,null,"Clôturée","22075","HEMONSTOIR","COTES-D'ARMOR","BRETAGNE","Polygone",-2.816746,48.158363]
["SSP000264601",null,"Ancienne décharge du Nouette",null,"Clôturée",null,null,"Clôturée","22076","HENANBIHEN","COTES-D'ARMOR","BRETAGNE","Polygone",-2.3861613,48.574677]
["SSP000264801",null,"Ancienne décharge de Malingeais",null,"Clôturée",null,null,"Clôturée","22077","HENANSAL","COTES-D'ARMOR","BRETAGNE","Polygone",-2.4562933,48.506554]
["SSP000264901",null,"Ancienne décharge de Lanveac",null,"Clôturée",null,null,"Clôturée","22078","HENGOAT","COTES-D'ARMOR","BRETAGNE","Polygone",-3.2149415,48.74133]
["SSP000265001",null,"Ancienne décharge de La Brousse",null,"Clôturée",null,null,"Clôturée","22079","HENON","COTES-D'ARMOR","BRETAGNE","Polygone",-2.6871088,48.365604]
["SSP000265101","57.0099","CEDILOR",null,"En cours",null,null,"En cours","57350","JOUY AUX ARCHES","MOSELLE","GRAND EST","Polygone",6.0909805,49.069534,"K3 - Traitement de déchets industriels"]
["SSP000265201","57.0148","Dubois Matériaux",null,"En cours",null,null,"En cours","57350","JOUY AUX ARCHES","MOSELLE","GRAND EST","Polygone",6.0936594,49.074127,"C13 - Traitement du bois"]
["SSP000265401","57.0204","Cojeancy",null,"En cours",null,null,"En cours","57413","LONGEVILLE LES SAINT AVOLD","MOSELLE","GRAND EST","Polygone",6.6832795,49.10955]
["SSP000265601","57.0192","ESKA - rue de la gare",null,"En cours",null,null,"En cours","57427","LUTZELBOURG","MOSELLE","GRAND EST","Polygone",7.248838,48.728565]
["SSP000265701","57.0191","ESKA - rue Koeberlé",null,"En cours",null,null,"En cours","57427","LUTZELBOURG","MOSELLE","GRAND EST","Polygone",7.246208,48.72852]
["SSP000265801","57.0197","CEDEC",null,"En cours",null,null,"En cours","57433","MAIZIERES LES METZ","MOSELLE","GRAND EST","Polygone",6.151419,49.203465]
["SSP000266001","57.0124","Ancienne usine d'incinération de Metz",null,"En cours",null,null,"En cours","57463","METZ","MOSELLE","GRAND EST","Polygone",6.188069,49.128586,"K - Déchets et traitements"]
["SSP000266201","57.0162","Recyclage 2000 (ex POLDER)",null,"En cours",null,null,"En cours","57491","MOYEUVRE GRANDE","MOSELLE","GRAND EST","Polygone",6.0487947,49.247654,"K3 - Traitement de déchets industriels"]
["SSP000266301",null,"Ancienne décharge de la Route de Plourivo",null,"Clôturée",null,null,"Clôturée","22086","KERFOT","COTES-D'ARMOR","BRETAGNE","Polygone",-3.045269,48.74516]
["SSP000266401",null,"Ancienne décharge du Bourg",null,"Clôturée",null,null,"Clôturée","22086","KERFOT","COTES-D'ARMOR","BRETAGNE","Polygone",-3.0244398,48.739407]
["SSP000266501",null,"Ancienne décharge de Crec'h Quenez Braz",null,"Clôturée",null,null,"Clôturée","22088","KERIEN","COTES-D'ARMOR","BRETAGNE","Polygone",-3.2144463,48.396057]
["SSP000266601",null,"Ancienne décharge de La Villeneuve",null,"Clôturée",null,null,"Clôturée","22091","KERMOROC'H","COTES-D'ARMOR","BRETAGNE","Polygone",-3.204114,48.612267]
["SSP000266801",null,"Ancienne décharge de Crec'h Jolben",null,"Clôturée",null,null,"Clôturée","22092","KERPERT","COTES-D'ARMOR","BRETAGNE","Polygone",-3.129145,48.37178]
["SSP000266901",null,"Ancienne décharge du Bourgneuf",null,"Clôturée",null,null,"Clôturée","22080","L'HERMITAGE LORGE","COTES-D'ARMOR","BRETAGNE","Polygone",-2.8405485,48.33064]
["SSP000267001",null,"Ancienne décharge de la Route de la Folie",null,"Clôturée",null,null,"Clôturée","22012","LA BOUILLIE","COTES-D'ARMOR","BRETAGNE","Polygone",-2.4545608,48.576817]
["SSP000267101",null,"Ancienne décharge de Quenhuel",null,"Clôturée",null,null,"Clôturée","22037","LA CHAPELLE NEUVE","COTES-D'ARMOR","BRETAGNE","Polygone",-3.424063,48.46523]
["SSP000267201",null,"Ancienne décharge de La Valiette",null,"Clôturée",null,null,"Clôturée","22039","LA CHEZE","COTES-D'ARMOR","BRETAGNE","Polygone",-2.6748846,48.141525]
["SSP000267401",null,"Ancienne décharge de Placieux",null,"Clôturée",null,null,"Clôturée","22073","LA HARMOYE","COTES-D'ARMOR","BRETAGNE","Polygone",-2.962469,48.35484]
["SSP000267501",null,"Ancienne décharge des Rochettes",null,"Clôturée",null,null,"Clôturée","22097","LA LANDEC","COTES-D'ARMOR","BRETAGNE","Polygone",-2.1852403,48.425407]
["SSP000267601",null,"Ancienne décharge du vieux bourg",null,"Clôturée",null,null,"Clôturée","22097","LA LANDEC","COTES-D'ARMOR","BRETAGNE","Polygone",-2.1826952,48.44425]
["SSP000267701",null,"Ancienne décharge des Divisions",null,"Clôturée",null,null,"Clôturée","22140","LA MALHOURE","COTES-D'ARMOR","BRETAGNE","Polygone",-2.4937248,48.403355]
["SSP000267801",null,"Ancienne décharge de la Ville Es Maury",null,"Clôturée",null,null,"Clôturée","22155","LA MOTTE","COTES-D'ARMOR","BRETAGNE","Polygone",-2.737893,48.22096]
["SSP000267901",null,"Ancienne décharge des Prés Colins",null,"Clôturée",null,null,"Clôturée","22255","LA PRENESSAYE","COTES-D'ARMOR","BRETAGNE","Polygone",-2.658673,48.195873]
["SSP000268001","57.0207","STYRIA ELESFRANCE",null,"Clôturée",null,null,"Clôturée","57606","SAINT AVOLD","MOSELLE","GRAND EST","Polygone",6.725334,49.113934]
["SSP000268101","57.0183","Comptoir Général du Ressort",null,"En cours",null,null,"En cours","57630","SARREBOURG","MOSELLE","GRAND EST","Polygone",7.076081,48.741005]
["SSP000268201",null,"Ancienne décharge du Moulin du Vicomte",null,"Clôturée",null,null,"Clôturée","22255","LA PRENESSAYE","COTES-D'ARMOR","BRETAGNE","Polygone",-2.628003,48.19189]
["SSP000268301",null,"Ancienne décharge du Chemin de l'Ourmel",null,"Clôturée",null,null,"Clôturée","22093","LAMBALLE","COTES-D'ARMOR","BRETAGNE","Polygone",-2.514701,48.480537]
["SSP000268401","57.0172","EFKA",null,"En cours",null,null,"En cours","57712","VIC SUR SEILLE","MOSELLE","GRAND EST","Polygone",6.52653,48.77853]
["SSP000268501",null,"Ancienne décharge de Saint Aaron",null,"Clôturée",null,null,"Clôturée","22093","LAMBALLE","COTES-D'ARMOR","BRETAGNE","Polygone",-2.4909983,48.513096]
["SSP000268601","57.0024","Ancien site POLDER (ex-PINCK)",null,"En cours",null,null,"En cours","57757","YUTZ","MOSELLE","GRAND EST","Polygone",6.1935077,49.3635,"K52 - Dépôts de ferraille"]
["SSP000268701",null,"Ancienne décharge de la Roche",null,"Clôturée",null,null,"Clôturée","22094","LANCIEUX","COTES-D'ARMOR","BRETAGNE","Polygone",-2.1524212,48.5861]
["SSP000268801","57.0200","Prosimétal",null,"En cours",null,null,"En cours","57757","YUTZ","MOSELLE","GRAND EST","Polygone",6.2075315,49.370457,"K5 - Récupération, dépôts de ferrailles"]
["SSP000268901",null,"Ancienne décharge de la Touche",null,"Clôturée",null,null,"Clôturée","22094","LANCIEUX","COTES-D'ARMOR","BRETAGNE","Polygone",-2.1432495,48.6067]
["SSP000269001","57.0206","ROS CASARES FRANCE",null,"En cours",null,null,"En cours","57757","YUTZ","MOSELLE","GRAND EST","Polygone",6.2040825,49.366108]
["SSP000269101","57.0122","Société Métallurgique de la Moselle",null,"En cours",null,null,"En cours","57757","YUTZ","MOSELLE","GRAND EST","Polygone",6.19878,49.363888,"H11 - Usinage"]
["SSP000269201",null,"Ancienne décharge de Pen ar Crec'h",null,"Clôturée",null,null,"Clôturée","22095","LANDEBAERON","COTES-D'ARMOR","BRETAGNE","Polygone",-3.2116535,48.651688]
["SSP000269401",null,"Ancienne décharge du Moulin de l'Etoile",null,"Clôturée",null,null,"Clôturée","22101","LANGOAT","COTES-D'ARMOR","BRETAGNE","Polygone",-3.3158054,48.717342]
["SSP000269501",null,"Ancienne décharge des Quatre Vents",null,"Clôturée",null,null,"Clôturée","22101","LANGOAT","COTES-D'ARMOR","BRETAGNE","Polygone",-3.2859654,48.718807]
["SSP000269601",null,"Ancienne décharge de Saint Yves",null,"Clôturée",null,null,"Clôturée","22101","LANGOAT","COTES-D'ARMOR","BRETAGNE","Polygone",-3.2673073,48.739746]
["SSP000269801",null,"Ancienne décharge du Carrée",null,"Clôturée",null,null,"Clôturée","22102","LANGOURLA","COTES-D'ARMOR","BRETAGNE","Polygone",-2.4035208,48.29212]
["SSP000270101",null,"Ancienne décharge du Roudouer",null,"Clôturée",null,null,"Clôturée","22214","PLOUEZEC","COTES-D'ARMOR","BRETAGNE","Polygone",-2.971625,48.713856]
["SSP000270201",null,"Ancienne décharge de Arrhuniou",null,"Clôturée",null,null,"Clôturée","22222","PLOUHA","COTES-D'ARMOR","BRETAGNE","Polygone",-2.9644995,48.7194]
["SSP000270301",null,"Ancienne décharge de Rumolin",null,"Clôturée",null,null,"Clôturée","22110","LANMERIN","COTES-D'ARMOR","BRETAGNE","Polygone",-3.3532999,48.735332]
["SSP000270401",null,"Ancienne décharge de Saint Julien",null,"Clôturée",null,null,"Clôturée","22110","LANMERIN","COTES-D'ARMOR","BRETAGNE","Polygone",-3.3637269,48.745487]
["SSP000270501",null,"Ancienne décharge de Belle Fontaine",null,"Clôturée",null,null,"Clôturée","22110","LANMERIN","COTES-D'ARMOR","BRETAGNE","Polygone",-3.3452492,48.741413]
["SSP000270601",null,"Ancienne décharge de Brestan",null,"Clôturée",null,null,"Clôturée","22111","LANMODEZ","COTES-D'ARMOR","BRETAGNE","Polygone",-3.0984988,48.840168]
["SSP000270901",null,"LE CREUSET",null,"Clôturée",null,null,"Clôturée","55132","COUSANCES LES FORGES","MEUSE","GRAND EST","Polygone",5.087714,48.605743]
["SSP000271001","55.0016","Décharge de sables des fonderies et ateliers salin",null,"En cours",null,null,"En cours","55144","DAMMARIE SUR SAULX","MEUSE","GRAND EST","Polygone",5.25094,48.601704,"J5 - Fonderie et travail des métaux"]
["SSP000271101","55.0032","AS 24",null,"En cours",null,null,"En cours","55398","PAGNY SUR MEUSE","MEUSE","GRAND EST","Polygone",5.7210817,48.68691,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000271201","55.0007","SITE HOPPECKE",null,"En cours",null,null,"En cours","55514","TREMONT SUR SAULX","MEUSE","GRAND EST","Polygone",5.043795,48.744316,"H16 - Piles électriques et accumulateurs (fabrication de)"]
["SSP000271301",null,"Ancienne décharge de Poull Ar Garz",null,"Clôturée",null,null,"Clôturée","22113","LANNION","COTES-D'ARMOR","BRETAGNE","Polygone",-3.435318,48.750847]
["SSP000271401",null,"Ancienne décharge de Convenant Gloal",null,"Clôturée",null,null,"Clôturée","22113","LANNION","COTES-D'ARMOR","BRETAGNE","Polygone",-3.4259171,48.718777]
["SSP000271501",null,"Ancienne décharge de Buhulien",null,"Clôturée",null,null,"Clôturée","22113","LANNION","COTES-D'ARMOR","BRETAGNE","Polygone",-3.4207134,48.71526]
["SSP000271701",null,"Ancienne décharge du Rocher",null,"Clôturée",null,null,"Clôturée","22114","LANRELAS","COTES-D'ARMOR","BRETAGNE","Polygone",-2.2870424,48.252907]
["SSP000271901",null,"Ancienne décharge du Moulin de Doualan",null,"Clôturée",null,null,"Clôturée","22117","LANTIC","COTES-D'ARMOR","BRETAGNE","Polygone",-2.8709872,48.590084]
["SSP000272001",null,"Ancienne décharge du Warem",null,"Clôturée",null,null,"Clôturée","22119","LANVELLEC","COTES-D'ARMOR","BRETAGNE","Polygone",-3.526586,48.605885]
["SSP000272101",null,"Ancienne décharge de la Leffetière",null,"Clôturée",null,null,"Clôturée","22122","LAURENAN","COTES-D'ARMOR","BRETAGNE","Polygone",-2.521219,48.216774]
["SSP000272201",null,"Ancienne décharge de Cargouet",null,"Clôturée",null,null,"Clôturée","22122","LAURENAN","COTES-D'ARMOR","BRETAGNE","Polygone",-2.5163484,48.229584]
["SSP000272301",null,"Ancienne décharge de Jaumais",null,"Clôturée",null,null,"Clôturée","22122","LAURENAN","COTES-D'ARMOR","BRETAGNE","Polygone",-2.4933212,48.224907]
["SSP000272401","12.0024","FRICHE GUIBERT / PROJET CAUSSE-GANTIER Suivi depuis acquisition par Cté COMMUNES",null,"En cours",null,null,"En cours","12145","MILLAU","AVEYRON","OCCITANIE","Polygone",3.0839577,44.100838,"E21 - Tannerie, mégisserie"]
["SSP000272501",null,"Ancienne décharge du Beau Val",null,"Clôturée",null,null,"Clôturée","22027","LE CAMBOUT","COTES-D'ARMOR","BRETAGNE","Polygone",-2.6279614,48.077908]
["SSP000272701","81.0003","CENTRE EDF GDF SERVICES GARONNE ET TARN (Ancienne usine à gaz)",null,"En cours",null,null,"En cours","81065","CASTRES","TARN","OCCITANIE","Polygone",2.245506,43.607967,"J1 - Cokéfaction, usines à gaz"]
["SSP000273001","69.0377","Teinturerie Thivel (route de Paris)",null,"Clôturée",null,"2018-02-16","Clôturée","69243","TARARE","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.4217963,45.894054,"E13 - Blanchiment, teinture, impression"]
["SSP000273101",null,"Ancienne décharge du Bourg",null,"Clôturée",null,null,"Clôturée","22066","LE GOURAY","COTES-D'ARMOR","BRETAGNE","Polygone",-2.4953847,48.329132]
["SSP000273201",null,"Ancienne décharge du bourg",null,"Clôturée",null,null,"Clôturée","22126","LE LESLAY","COTES-D'ARMOR","BRETAGNE","Polygone",-2.9648795,48.428455]
["SSP000273301",null,"Ancienne décharge de Traou Guer",null,"Clôturée",null,null,"Clôturée","22150","LE MERZER","COTES-D'ARMOR","BRETAGNE","Polygone",-3.0944073,48.593082]
["SSP000273401",null,"Ancienne décharge de Stand ar Vran",null,"Clôturée",null,null,"Clôturée","22157","LE MOUSTOIR","COTES-D'ARMOR","BRETAGNE","Polygone",-3.507101,48.25697]
["SSP000273501",null,"Ancienne décharge de la Ville Gohen",null,"Clôturée",null,null,"Clôturée","22263","LE QUIOU","COTES-D'ARMOR","BRETAGNE","Polygone",-2.016511,48.354534]
["SSP000273601",null,"Ancienne décharge de La Croix Plate",null,"Clôturée",null,null,"Clôturée","22386","LE VIEUX BOURG","COTES-D'ARMOR","BRETAGNE","Polygone",-2.9882326,48.38069]
["SSP000273701",null,"Ancienne décharge de la Route de Kerboeuf",null,"Clôturée",null,null,"Clôturée","22386","LE VIEUX BOURG","COTES-D'ARMOR","BRETAGNE","Polygone",-3.004048,48.386307]
["SSP000273801",null,"Ancienne décharge de la route de Calorguen",null,"Clôturée",null,null,"Clôturée","22123","LEHON","COTES-D'ARMOR","BRETAGNE","Polygone",-2.0419383,48.437397]
["SSP000273901",null,"Ancienne décharge de La Fleurette",null,"Clôturée",null,null,"Clôturée","22035","LES CHAMPS GERAUX","COTES-D'ARMOR","BRETAGNE","Polygone",-1.9795891,48.42824]
["SSP000274001",null,"Ancienne décharge du Bois de Crénard",null,"Clôturée",null,null,"Clôturée","22124","LESCOUET GOUAREC","COTES-D'ARMOR","BRETAGNE","Polygone",-3.167314,48.174263]
["SSP000274101",null,"Ancienne décharge de Miville",null,"Clôturée",null,null,"Clôturée","22127","LEZARDRIEUX","COTES-D'ARMOR","BRETAGNE","Polygone",-3.1083007,48.799522]
["SSP000274201",null,"Anciennes décharges de Fin Véo Bian",null,"Clôturée",null,null,"Clôturée","22127","LEZARDRIEUX","COTES-D'ARMOR","BRETAGNE","Polygone",-3.1324892,48.78581]
["SSP000274301",null,"Ancienne décharge de La Roche Noire",null,"Clôturée",null,null,"Clôturée","22127","LEZARDRIEUX","COTES-D'ARMOR","BRETAGNE","Polygone",-3.0934343,48.80972]
["SSP000274401",null,"Ancienne décharge de Convenant Le Goff",null,"Clôturée",null,null,"Clôturée","22128","LOCARN","COTES-D'ARMOR","BRETAGNE","Polygone",-3.3726664,48.343437]
["SSP000274501",null,"Ancienne décharge de la route de la Forêt",null,"Clôturée",null,null,"Clôturée","22132","LOHUEC","COTES-D'ARMOR","BRETAGNE","Polygone",-3.5184484,48.460155]
["SSP000274601","54.0126","PROTECH'EST","Cessation d'activités","En cours",null,null,"En cours","54061","BENAMENIL","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",6.6714473,48.567055,"H13 - Traitement de surface"]
["SSP000274701",null,"Ancienne décharge de La Lande du Cosquer",null,"Clôturée",null,null,"Clôturée","22132","LOHUEC","COTES-D'ARMOR","BRETAGNE","Polygone",-3.5033236,48.455093]
["SSP000274801","54.0056","Cokerie de Pont à Mousson (Sté PONT A MOUSSON S.A.)","Polution due au fonctionnement de l'installation","En cours",null,null,"En cours","54079","BLENOD LES PONT A MOUSSON","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",6.061298,48.881077,"J1 - Cokéfaction, usines à gaz"]
["SSP000274901",null,"Ancienne décharge de l'Etang de Loscouet",null,"Clôturée",null,null,"Clôturée","22133","LOSCOUET SUR MEU","COTES-D'ARMOR","BRETAGNE","Polygone",-2.2528057,48.179184]
["SSP000275001","54.0085","PROMEDO","Pollution due au fonctionnement de l'installation","En cours",null,null,"En cours","54118","CHARENCY VEZIN","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",5.5153575,49.486362,"G24 - Produits à base d'amiante (fabrication de)"]
["SSP000275101",null,"Ancienne décharge de Pen Feunteun",null,"Clôturée",null,null,"Clôturée","22134","LOUANNEC","COTES-D'ARMOR","BRETAGNE","Polygone",-3.3791025,48.786167]
["SSP000275201","54.0052","Usine PONT A MOUSSON de LIVERDUN",null,"En cours",null,null,"En cours","54318","LIVERDUN","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",6.0647454,48.747528,"J51 - Fonderie des métaux ferreux"]
["SSP000275301","54.0135","ANDRIN G. ET FILS","Cessation d'activités 1976","En cours",null,null,"En cours","54323","LONGWY","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",5.770472,49.52385,null,null,"31.6C - Fabrication de matériel électromagnétique industriel"]
["SSP000275401",null,"Ancienne décharge de Lann Consortet",null,"Clôturée",null,null,"Clôturée","22135","LOUARGAT","COTES-D'ARMOR","BRETAGNE","Polygone",-3.3767087,48.611336]
["SSP000275501",null,"Ancienne décharge de Crec'h Merien",null,"Clôturée",null,null,"Clôturée","22135","LOUARGAT","COTES-D'ARMOR","BRETAGNE","Polygone",-3.3633292,48.572895]
["SSP000275601","54.0132","DIDIER SIPC","Cessation d'activités 1991","En cours",null,null,"En cours","54323","LONGWY","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",5.763055,49.509975,"G14 - Fabrication d'autres matériaux de construction"]
["SSP000275701",null,"Ancienne décharge de Pen ar Mene",null,"Clôturée",null,null,"Clôturée","22135","LOUARGAT","COTES-D'ARMOR","BRETAGNE","Polygone",-3.3474588,48.54202]
["SSP000275801",null,"Ancienne décharge de la Zone Artisanale",null,"Clôturée",null,null,"Clôturée","22135","LOUARGAT","COTES-D'ARMOR","BRETAGNE","Polygone",-3.349382,48.566288]
["SSP000275901","54.0119","BOIS FRANCE SCIAGE","Cessation d'activtés 2010","En cours",null,null,"En cours","54423","PEXONNE","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",6.8696156,48.488655,null,"59.07 - Commerce du bois"]
["SSP000276001","54.0049","FAURECIA","Cessation d'activités","En cours",null,null,"En cours","54428","PIERREPONT","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",5.7032976,49.419575,"D72 - Transformation des matières plastiques"]
["SSP000276101","54.0008","ANCIEN DEPOT D'HYDROCARBURES RAOULX & PETROLESSENCE","Cessation d'activités 1987","En cours",null,null,"En cours","54528","TOUL","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",5.8981166,48.681698,null,null,null,"46.12B - Autres intermédiaires du commerce en combustibles, métaux, minéraux et produits chimiques"]
["SSP000276201",null,"Ancienne décharge de Beslière",null,"Clôturée",null,null,"Clôturée","22136","LOUDEAC","COTES-D'ARMOR","BRETAGNE","Polygone",-2.7215216,48.183254]
["SSP000276301","54.0109","Pneumatiques Kleber","Cessation d'activités 2008","En cours",null,null,"En cours","54528","TOUL","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",5.9107747,48.695717,"D7 - Caoutchouc et matières plastiques"]
["SSP000276401","69.0159","THIVEL",null,"Clôturée",null,"2018-02-16","Clôturée","69243","TARARE","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.4347596,45.8995,"E13 - Blanchiment, teinture, impression"]
["SSP000276501",null,"Ancienne décharge des Poulhauts",null,"Clôturée",null,null,"Clôturée","22136","LOUDEAC","COTES-D'ARMOR","BRETAGNE","Polygone",-2.6944165,48.16741]
["SSP000276601",null,"Ancienne décharge de Kerlagan",null,"Clôturée",null,null,"Clôturée","22137","MAEL CARHAIX","COTES-D'ARMOR","BRETAGNE","Polygone",-3.4450145,48.28265]
["SSP000276701",null,"Ancienne décharge de L'Isle",null,"Clôturée",null,null,"Clôturée","22137","MAEL CARHAIX","COTES-D'ARMOR","BRETAGNE","Polygone",-3.3672864,48.27955]
["SSP000276801",null,"Ancienne décharge de Douar Constant",null,"Clôturée",null,null,"Clôturée","22138","MAEL PESTIVIEN","COTES-D'ARMOR","BRETAGNE","Polygone",-3.3046668,48.39057]
["SSP000276901",null,"Ancienne décharge de Goaz Ar Goff",null,"Clôturée",null,null,"Clôturée","22141","MANTALLOT","COTES-D'ARMOR","BRETAGNE","Polygone",-3.3015037,48.70477]
["SSP000277101",null,"Ancienne décharge du Pont Tainguy",null,"Clôturée",null,null,"Clôturée","22143","MATIGNON","COTES-D'ARMOR","BRETAGNE","Polygone",-2.2854671,48.60406]
["SSP000277201",null,"Ancienne décharge de Queriollon",null,"Clôturée",null,null,"Clôturée","22145","MEGRIT","COTES-D'ARMOR","BRETAGNE","Polygone",-2.2634635,48.3919]
["SSP000277301",null,"Ancienne décharge de L'Enseigne",null,"Clôturée",null,null,"Clôturée","22146","MELLIONNEC","COTES-D'ARMOR","BRETAGNE","Polygone",-3.2720125,48.16122]
["SSP000277401",null,"Ancienne décharge de Saint Brieuc des Bois",null,"Clôturée",null,null,"Clôturée","22147","MERDRIGNAC","COTES-D'ARMOR","BRETAGNE","Polygone",-2.347353,48.184322]
["SSP000277601",null,"Ancienne décharge du Rocher",null,"Clôturée",null,null,"Clôturée","22148","MERILLAC","COTES-D'ARMOR","BRETAGNE","Polygone",-2.40609,48.256577]
["SSP000277701",null,"Ancienne décharge de Poulfos",null,"Clôturée",null,null,"Clôturée","22149","MERLEAC","COTES-D'ARMOR","BRETAGNE","Polygone",-2.8683398,48.27455]
["SSP000277801",null,"Ancienne décharge de la Touche",null,"Clôturée",null,null,"Clôturée","22151","MESLIN","COTES-D'ARMOR","BRETAGNE","Polygone",-2.567883,48.441814]
["SSP000277901",null,"Ancienne décharge de Gaurebout",null,"Clôturée",null,null,"Clôturée","22158","MUR DE BRETAGNE","COTES-D'ARMOR","BRETAGNE","Polygone",-2.9806545,48.20714]
["SSP000278001",null,"Ancienne décharge du Lann",null,"Clôturée",null,null,"Clôturée","22161","PABU","COTES-D'ARMOR","BRETAGNE","Polygone",-3.1336675,48.591988]
["SSP000278101",null,"Ancienne décharge sauvage de Kerbiguet",null,"Clôturée",null,null,"Clôturée","22162","PAIMPOL","COTES-D'ARMOR","BRETAGNE","Polygone",-3.098545,48.769176]
["SSP000278201",null,"Ancienne décharge de Keramazec",null,"Clôturée",null,null,"Clôturée","22162","PAIMPOL","COTES-D'ARMOR","BRETAGNE","Polygone",-3.0719388,48.79477]
["SSP000278401",null,"Ancienne décharge de Kermin",null,"Clôturée",null,null,"Clôturée","22162","PAIMPOL","COTES-D'ARMOR","BRETAGNE","Polygone",-3.0506682,48.76073]
["SSP000278501",null,"Ancienne décharge de La Lande Blanche",null,"Clôturée",null,null,"Clôturée","22162","PAIMPOL","COTES-D'ARMOR","BRETAGNE","Polygone",-3.0411484,48.753143]
["SSP000278601",null,"Ancienne décharge du Billec",null,"Clôturée",null,null,"Clôturée","22162","PAIMPOL","COTES-D'ARMOR","BRETAGNE","Polygone",-3.027235,48.773045]
["SSP000278701",null,"Ancienne décharge du Vieux Bourg",null,"Clôturée",null,null,"Clôturée","22162","PAIMPOL","COTES-D'ARMOR","BRETAGNE","Polygone",-3.009874,48.755817]
["SSP000278801","31.0031","TOTAL MARKETING SERVICES",null,"En cours",null,null,"En cours","31169","ESCALQUENS","HAUTE-GARONNE","OCCITANIE","Polygone",1.5491694,43.508266,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000278901","31.0008","NXP SEMICONDUCTORS FRANCE SAS ex FREESCALE SEMI CONDUCTEURS FRANCE SAS",null,"En cours",null,null,"En cours","31555","TOULOUSE","HAUTE-GARONNE","OCCITANIE","Polygone",1.3905389,43.560123,"H18 - Composants électroniques (fabrication de)"]
["SSP000279001",null,"Ancienne décharge de Minez Kerriou",null,"Clôturée",null,null,"Clôturée","22163","PAULE","COTES-D'ARMOR","BRETAGNE","Polygone",-3.4700475,48.236225]
["SSP000279101",null,"Ancienne décharge du Quinquis",null,"Clôturée",null,null,"Clôturée","22164","PEDERNEC","COTES-D'ARMOR","BRETAGNE","Polygone",-3.317407,48.598316]
["SSP000279201","65.0005","ALCAN (ex Aluminium Pechiney)",null,"Clôturée",null,null,"Clôturée","65258","LANNEMEZAN","HAUTES-PYRENEES","OCCITANIE","Polygone",0.3769402,43.09413,"J32 - Métallurgie de l'aluminium"]
["SSP000279301",null,"Ancienne décharge de Squibernevez",null,"Clôturée",null,null,"Clôturée","22164","PEDERNEC","COTES-D'ARMOR","BRETAGNE","Polygone",-3.2454004,48.59485]
["SSP000279401","31.0001","SOFERTI",null,"En cours",null,null,"En cours","31182","FENOUILLET","HAUTE-GARONNE","OCCITANIE","Polygone",1.4051594,43.67995,"D36 - Fabrication des engrais"]
["SSP000279501",null,"Ancienne décharge de Goas Roux",null,"Clôturée",null,null,"Clôturée","22164","PEDERNEC","COTES-D'ARMOR","BRETAGNE","Polygone",-3.279446,48.602093]
["SSP000279601",null,"Ancienne décharge de Croaz Ar Rhun",null,"Clôturée",null,null,"Clôturée","22166","PENVENAN","COTES-D'ARMOR","BRETAGNE","Polygone",-3.319632,48.810326]
["SSP000279701","31.0012","TOLOCHIMIE",null,"En cours",null,null,"En cours","31555","TOULOUSE","HAUTE-GARONNE","OCCITANIE","Polygone",1.4316398,43.551273,"D3 - Chimie, phytosanitaire, pharmacie"]
["SSP000279901",null,"Ancienne décharge de Kergadic",null,"Clôturée",null,null,"Clôturée","22168","PERROS GUIREC","COTES-D'ARMOR","BRETAGNE","Polygone",-3.469401,48.809708]
["SSP000280001","31.0057","CARNAUD METAL BOX (groupe CROWN EUROPE)",null,"En cours",null,null,"En cours","31555","TOULOUSE","HAUTE-GARONNE","OCCITANIE","Polygone",1.5061063,43.56648,"H11 - Usinage"]
["SSP000280101","31.0075","SOCIETE DES PETROLES SHELL",null,"En cours",null,null,"En cours","31149","COLOMIERS","HAUTE-GARONNE","OCCITANIE","Polygone",1.3277549,43.609177,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000280201","65.0001","YARA",null,"En cours",null,null,"En cours","65362","PIERREFITTE NESTALAS","HAUTES-PYRENEES","OCCITANIE","Polygone",-0.06507896,42.96677,"D36 - Fabrication des engrais"]
["SSP000280401","12.0010","INCINERATION D'ORDURES MENAGERES - SICTOM D'ESPALION",null,"En cours",null,null,"En cours","12216","SAINT COME D'OLT","AVEYRON","OCCITANIE","Polygone",2.8075597,44.52533,"K2 - Traitement de déchets urbains"]
["SSP000280501",null,"Ancienne décharge du Tertre Cosson",null,"Clôturée",null,null,"Clôturée","22170","PLAINE HAUTE","COTES-D'ARMOR","BRETAGNE","Polygone",-2.874081,48.427517]
["SSP000280601","81.0054","ESSO S.A.F",null,"En cours",null,null,"En cours","81004","ALBI","TARN","OCCITANIE","Polygone",2.1416419,43.945347,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000280701",null,"Ancienne décharge des Madrais d'En Bas",null,"Clôturée",null,null,"Clôturée","22170","PLAINE HAUTE","COTES-D'ARMOR","BRETAGNE","Polygone",-2.8686843,48.44419]
["SSP000280801","81.0028","EDF (PARC A CENDRES DE LA MOULINE)",null,"En cours",null,null,"En cours","81048","CAGNAC LES MINES","TARN","OCCITANIE","Polygone",2.129141,43.969448,"K36 - Mise en décharge"]
["SSP000281001",null,"Ancienne décharge de Rochauland",null,"Clôturée",null,null,"Clôturée","22174","PLEBOULLE","COTES-D'ARMOR","BRETAGNE","Polygone",-2.3416853,48.606667]
["SSP000281101","81.0029","EDF (PARC A CENDRES DE REILLET)",null,"En cours",null,null,"En cours","81048","CAGNAC LES MINES","TARN","OCCITANIE","Polygone",2.1335633,43.96209,"K36 - Mise en décharge"]
["SSP000281201","81.0050","LIMES ET RAPES",null,"En cours",null,null,"En cours","81257","SAINT JUERY","TARN","OCCITANIE","Polygone",2.2208345,43.94665,"H1 - Mécanique, électrique, traitement de surface"]
["SSP000281301","09.0030","ALUMINIUM PECHINEY - DECHARGE INTERNE DU \"VILLAGE\"",null,"En cours",null,null,"En cours","09030","AUZAT","ARIEGE","OCCITANIE","Polygone",1.4845979,42.76529,"K36 - Mise en décharge"]
["SSP000281401","81.0004","AFELEC et GALVACIER (anciennement groupe Arçonnerie Française)",null,"En cours",null,null,"En cours","81271","SAINT SULPICE LA POINTE","TARN","OCCITANIE","Polygone",1.6858488,43.772095,"H13 - Traitement de surface"]
["SSP000281601",null,"Ancienne décharge de La Lande",null,"Clôturée",null,null,"Clôturée","22177","PLEGUIEN","COTES-D'ARMOR","BRETAGNE","Polygone",-2.9581218,48.622208]
["SSP000281701","31.0013","EPR (ENTREPÔTS PETROLIERS REGIONAUX) DEPÔT DE TOULOUSE",null,"En cours",null,null,"En cours","31555","TOULOUSE","HAUTE-GARONNE","OCCITANIE","Polygone",1.4223391,43.629074,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000281801","31.0014","SHELL (DEPÔT DE TOULOUSE)",null,"En cours",null,null,"En cours","31555","TOULOUSE","HAUTE-GARONNE","OCCITANIE","Polygone",1.4222966,43.63089,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000281901","31.0015","LEXSA (ex LABINAL et MOLEX)",null,"En cours",null,null,"En cours","31584","VILLEMUR SUR TARN","HAUTE-GARONNE","OCCITANIE","Polygone",1.4975742,43.860973,"H1 - Mécanique, électrique, traitement de surface"]
["SSP000282001","31.0036","ANCIEN UIOM - COMMUNAUTE DE COMMUNES DE VILLEFRANCHE DE LAURAGAIS",null,"En cours",null,null,"En cours","31582","VILLEFRANCHE DE LAURAGAIS","HAUTE-GARONNE","OCCITANIE","Polygone",1.704568,43.403385,"K31 - Incinération"]
["SSP000282101",null,"Ancienne décharge de Kerhir",null,"Clôturée",null,null,"Clôturée","22177","PLEGUIEN","COTES-D'ARMOR","BRETAGNE","Polygone",-2.9497373,48.639965]
["SSP000282201",null,"Ancienne décharge de Quehenic",null,"Clôturée",null,null,"Clôturée","22180","PLELAN LE PETIT","COTES-D'ARMOR","BRETAGNE","Polygone",-2.2101386,48.421265]
["SSP000282301",null,"Ancienne décharge de Belle Chasse",null,"Clôturée",null,null,"Clôturée","22181","PLELAUFF","COTES-D'ARMOR","BRETAGNE","Polygone",-3.2087977,48.213474]
["SSP000282401",null,"Carrosserie COROY",null,"Clôturée",null,null,"Clôturée","57487","MOULINS LES METZ","MOSELLE","GRAND EST","Polygone",6.13009,49.09227]
["SSP000282501","57.0219","TOTAL",null,"En cours",null,null,"En cours","57160","CREUTZWALD","MOSELLE","GRAND EST","Point",0.0,0.0]
["SSP000282601",null,"Ancienne décharge de Bel Air",null,"Clôturée",null,null,"Clôturée","22183","PLEMET","COTES-D'ARMOR","BRETAGNE","Polygone",-2.591803,48.167362]
["SSP000283601",null,"Ancienne décharge de La Tantouille",null,"Clôturée",null,null,"Clôturée","22184","PLEMY","COTES-D'ARMOR","BRETAGNE","Polygone",-2.6608605,48.3317]
["SSP000283701",null,"Ancienne décharge de Perdiel",null,"Clôturée",null,null,"Clôturée","22185","PLENEE JUGON","COTES-D'ARMOR","BRETAGNE","Polygone",-2.44799,48.32351]
["SSP000283801","31.0028","AIR FRANCE",null,"En cours",null,null,"En cours","31555","TOULOUSE","HAUTE-GARONNE","OCCITANIE","Polygone",1.4758264,43.575413,"H - Mécanique, traitements des surfaces"]
["SSP000284001",null,"Ancienne décharge du Pré de l'Aune",null,"Clôturée",null,null,"Clôturée","22188","PLERNEUF","COTES-D'ARMOR","BRETAGNE","Polygone",-2.8682055,48.507137]
["SSP000284101",null,"Ancienne décharge du Moulin du Roy",null,"Clôturée",null,null,"Clôturée","22189","PLESIDY","COTES-D'ARMOR","BRETAGNE","Polygone",-3.138753,48.446793]
["SSP000284201",null,"Ancienne décharge de La Vallée de Fontenelle",null,"Clôturée",null,null,"Clôturée","22209","PLOUBALAY","COTES-D'ARMOR","BRETAGNE","Polygone",-2.1449285,48.53749]
["SSP000284301",null,"Ancienne décharge du Bas Gray",null,"Clôturée",null,null,"Clôturée","22190","PLESLIN TRIGAVOU","COTES-D'ARMOR","BRETAGNE","Polygone",-2.0748515,48.53962]
["SSP000284401",null,"Ancienne décharge du Clos Meunier",null,"Clôturée",null,null,"Clôturée","22191","PLESSALA","COTES-D'ARMOR","BRETAGNE","Polygone",-2.611847,48.253242]
["SSP000284501",null,"Ancienne décharge de la Zone Artisanale",null,"Clôturée",null,null,"Clôturée","22191","PLESSALA","COTES-D'ARMOR","BRETAGNE","Polygone",-2.6055152,48.276962]
["SSP000284601",null,"Ancienne décharge de Calendrias",null,"Clôturée",null,null,"Clôturée","22193","PLESTAN","COTES-D'ARMOR","BRETAGNE","Polygone",-2.4732618,48.410793]
["SSP000284701","31.0017","SNPE Reconversion et Services",null,"En cours",null,null,"En cours","31555","TOULOUSE","HAUTE-GARONNE","OCCITANIE","Polygone",1.4354898,43.56662,"D8 - Poudres et explosifs"]
["SSP000285201","18.0014","Site BOUGAUL",null,"En cours",null,null,"En cours","18207","SAINT FLORENT SUR CHER","CHER","CENTRE-VAL DE LOIRE","Point",0.0,0.0,"H11 - Usinage"]
["SSP000285601",null,"Ancienne décharge de Keraliez",null,"Clôturée",null,null,"Clôturée","22199","PLEUMEUR GAUTIER","COTES-D'ARMOR","BRETAGNE","Polygone",-3.1740615,48.781723]
["SSP000285801",null,"Ancienne décharge de Duancre",null,"Clôturée",null,null,"Clôturée","22203","PLOEUC SUR LIE","COTES-D'ARMOR","BRETAGNE","Polygone",-2.801865,48.320854]
["SSP000286401",null,"Ancienne décharge du Runio d'en haut",null,"Clôturée",null,null,"Clôturée","22206","PLOUAGAT","COTES-D'ARMOR","BRETAGNE","Polygone",-3.0104702,48.50611]
["SSP000287001",null,"Ancienne décharge du Bourg",null,"Clôturée",null,null,"Clôturée","22208","PLOUASNE","COTES-D'ARMOR","BRETAGNE","Polygone",-2.0078127,48.301773]
["SSP000287401",null,"Ancienne décharge de Prat Saint Christophe",null,"Clôturée",null,null,"Clôturée","22211","PLOUBEZRE","COTES-D'ARMOR","BRETAGNE","Polygone",-3.4541094,48.72518]
["SSP000287601",null,"Ancienne décharge de Convenat Pichouron",null,"Clôturée",null,null,"Clôturée","22211","PLOUBEZRE","COTES-D'ARMOR","BRETAGNE","Polygone",-3.436945,48.676792]
["SSP000288001",null,"Ancienne décharge de Saint Colomban",null,"Clôturée",null,null,"Clôturée","22212","PLOUEC DU TRIEUX","COTES-D'ARMOR","BRETAGNE","Polygone",-3.223795,48.669735]
["SSP000288801",null,"Ancienne décharge de Boderin",null,"Clôturée",null,null,"Clôturée","56240","SARZEAU","MORBIHAN","BRETAGNE","Polygone",-2.7055926,47.524746]
["SSP000289601",null,"RB COMPAGNIE",null,"Clôturée",null,null,"Clôturée","92050","NANTERRE","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.2088568,48.88681]
["SSP000289801","68.0226","LIGIBELL",null,"En cours",null,null,"En cours","68374","WINTZENHEIM","HAUT-RHIN","GRAND EST","Polygone",7.3154078,48.080536]
["SSP000290501",null,"EFR",null,"Clôturée",null,null,"Clôturée","92048","MEUDON","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.2340214,48.78449]
["SSP000291001","35.0030","AUTOMAXI INTERNATIONAL",null,"En cours",null,null,"En cours","35288","SAINT MALO","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.9896691,48.650867,"H13 - Traitement de surface"]
["SSP000291801","92.0023","Anciennement STE IMPREGNA",null,"En cours",null,null,"En cours","92025","COLOMBES","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.2490127,48.933426,"C13 - Traitement du bois"]
["SSP000291901","92.0095","SMURFIT KAPPA (anciennes papeteries de Nanterre)",null,"En cours",null,null,"En cours","92050","NANTERRE","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.2025223,48.90468,"C2 - Industrie du papier et du carton"]
["SSP000292301",null,"Total Relais Principal Italie",null,"Clôturée",null,null,"Clôturée","75113","PARIS 13E ARRONDISSEMENT","PARIS","ILE-DE-FRANCE","Polygone",2.359411,48.81701]
["SSP000293101",null,"Hôpital Broussais",null,"Clôturée",null,null,"Clôturée","75114","PARIS 14E ARRONDISSEMENT","PARIS","ILE-DE-FRANCE","Polygone",2.3127136,48.82704]
["SSP000293401",null,"Ancien garage",null,"Clôturée",null,null,"Clôturée","22093","LAMBALLE","COTES-D'ARMOR","BRETAGNE","Polygone",-2.5106125,48.469086]
["SSP000293701","93.0027","IMCD (ex SPCI)","Réhabilitation","Clôturée",null,null,"Clôturée","93066","SAINT DENIS","SEINE-SAINT-DENIS","ILE-DE-FRANCE","Polygone",2.36225,48.91627,"D3 - Chimie, phytosanitaire, pharmacie"]
["SSP000294301","28.0025","Installations techniques de Gaz de France",null,"En cours",null,null,"En cours","28051","BONNEVAL","EURE-ET-LOIR","CENTRE-VAL DE LOIRE","Polygone",1.3897654,48.182926,"J1 - Cokéfaction, usines à gaz"]
["SSP000294601","28.0035","HUREL ARC",null,"En cours",null,null,"En cours","28394","TREON","EURE-ET-LOIR","CENTRE-VAL DE LOIRE","Polygone",1.3136908,48.673573,"D36 - Fabrication des engrais"]
["SSP000295101",null,"SARL Electricité Auto Radio",null,"Clôturée",null,null,"Clôturée","75056","PARIS","PARIS","ILE-DE-FRANCE","Polygone",2.3569868,48.88964]
["SSP000295201","92.0039","SOLVADIS (ex CLEMENT RPC)",null,"En cours",null,null,"En cours","92036","GENNEVILLIERS","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.3024576,48.948135,"D - Chimie, parachimie, pétrole"]
["SSP000295601",null,"SARL Courcelles Automobiles",null,"Clôturée",null,null,"Clôturée","75056","PARIS","PARIS","ILE-DE-FRANCE","Polygone",2.3001883,48.882954]
["SSP000296001",null,"Ancienne décharge de Boutill",null,"Clôturée",null,null,"Clôturée","22224","PLOULEC'H","COTES-D'ARMOR","BRETAGNE","Polygone",-3.502658,48.72899]
["SSP000296601",null,"Ancienne décharge de Run Dogan",null,"Clôturée",null,null,"Clôturée","22214","PLOUEZEC","COTES-D'ARMOR","BRETAGNE","Polygone",-2.9458075,48.748947]
["SSP000296701",null,"Ancienne décharge de Goas Froment",null,"Clôturée",null,null,"Clôturée","22214","PLOUEZEC","COTES-D'ARMOR","BRETAGNE","Polygone",-2.9741786,48.726414]
["SSP000297401",null,"KAUFMAN & BROAD",null,"Clôturée",null,null,"Clôturée","92062","PUTEAUX","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.2443678,48.88559]
["SSP000297901","92.0068","GDF DPT Région Ile-de-France et Magasin central de EDF-GDF Services",null,"En cours",null,null,"En cours","92050","NANTERRE","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.1883256,48.901226,"J1 - Cokéfaction, usines à gaz"]
["SSP000298101",null,"CONFIDENTIALYS",null,"Clôturée",null,null,"Clôturée","92036","GENNEVILLIERS","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.3140326,48.927864]
["SSP000298401","95.0052","société Pains Jacquet",null,"En cours",null,null,"En cours","95063","BEZONS","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.218344,48.92508,"B1 - Industrie agro-alimentaire"]
["SSP000298901","92.0087","EFR FRANCE",null,"En cours",null,null,"En cours","92050","NANTERRE","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.1945643,48.884556,"L23 - Détail de carburants"]
["SSP000299401","59.0084","ICI CORONA",null,"En cours",null,null,"En cours","59606","VALENCIENNES","NORD","HAUTS-DE-FRANCE","Polygone",3.5225313,50.37062,"D42 - Fabrication de peintures"]
["SSP000300001","59.0143","CIMT",null,"En cours",null,null,"En cours","59383","MARLY","NORD","HAUTS-DE-FRANCE","Polygone",3.541999,50.344807,"M - Divers et services"]
["SSP000300201","59.0169","MARAIS LES VIVIERS",null,"En cours",null,null,"En cours","59475","PROUVY","NORD","HAUTS-DE-FRANCE","Polygone",3.4701364,50.316586,"G13 - Fabrication de produits en amiante-ciment"]
["SSP000300901","59.0272","Magnesita (ex LWB REFRACTORIES (Loist Réfractaires))",null,"En cours",null,null,"En cours","59606","VALENCIENNES","NORD","HAUTS-DE-FRANCE","Polygone",3.5107133,50.346924,"D - Chimie, parachimie, pétrole"]
["SSP000301201","59.0401","Site DOMMERY",null,"En cours",null,null,"En cours","59475","PROUVY","NORD","HAUTS-DE-FRANCE","Polygone",3.4580808,50.3153,"G13 - Fabrication de produits en amiante-ciment"]
["SSP000301501","59.0033","ANCIENNES USINES ROUSSEAU",null,"En cours",null,null,"En cours","59491","RAISMES","NORD","HAUTS-DE-FRANCE","Polygone",3.53201,50.41372,"F11 - Houillères"]
["SSP000302101","59.0045","DESVRES (ex DOUZIES CARRELAGE)",null,"En cours",null,null,"En cours","59225","FEIGNIES","NORD","HAUTS-DE-FRANCE","Polygone",3.9226475,50.31038,"G12 - Fabrication de produits céramiques"]
["SSP000303001","59.0059","DECHARGE PREMINES",null,"En cours",null,null,"En cours","59165","CUINCY","NORD","HAUTS-DE-FRANCE","Polygone",3.040502,50.36982,"K36 - Mise en décharge"]
["SSP000303601",null,"CARRIERE DES PEUPLIERS BAIL",null,"Clôturée",null,null,"Clôturée","59002","ABSCON","NORD","HAUTS-DE-FRANCE","Polygone",3.305755,50.32395]
["SSP000304701","59.0094","VERRERIES DE BLANC-MISSERON",null,"En cours",null,null,"En cours","59484","QUIEVRECHAIN","NORD","HAUTS-DE-FRANCE","Polygone",3.6625311,50.399952,"M1 - Industries diverses"]
["SSP000305001","59.0103","ANCIENNE COKERIE DE WAZIERS CDF",null,"En cours",null,null,"En cours","59654","WAZIERS","NORD","HAUTS-DE-FRANCE","Polygone",3.1058722,50.378674,"F11 - Houillères"]
["SSP000305201","59.0117","DCA LESAGE",null,"En cours",null,null,"En cours","59136","LE CATEAU CAMBRESIS","NORD","HAUTS-DE-FRANCE","Polygone",3.5387344,50.105442,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000305801","59.0140","LAITERIE UCANEL",null,"En cours",null,null,"En cours","59177","DOMPIERRE SUR HELPE","NORD","HAUTS-DE-FRANCE","Polygone",3.8654308,50.14226,"B12 - Industrie laitière"]
["SSP000306101","59.0145","CHIMICOLOR",null,"En cours",null,null,"En cours","59064","BELLAING","NORD","HAUTS-DE-FRANCE","Polygone",3.4355428,50.363617,"H13 - Traitement de surface"]
["SSP000306401","59.0177","SARL DRT",null,"En cours",null,null,"En cours","59178","DOUAI","NORD","HAUTS-DE-FRANCE","Polygone",3.0900288,50.379826,"K52 - Dépôts de ferraille"]
["SSP000307001","59.0193","SIPC (Société Industrielle de produits chimique)",null,"En cours",null,null,"En cours","59156","COURCHELETTES","NORD","HAUTS-DE-FRANCE","Polygone",3.0549383,50.34461,"D - Chimie, parachimie, pétrole"]
["SSP000307401","59.0209","SAMBRE ET MEUSE",null,"En cours",null,null,"En cours","59225","FEIGNIES","NORD","HAUTS-DE-FRANCE","Polygone",3.917172,50.306545,"J51 - Fonderie des métaux ferreux"]
["SSP000308001","59.0226","GALVANISATION DU CAMBRAISIS",null,"En cours",null,null,"En cours","59311","HONNECHY","NORD","HAUTS-DE-FRANCE","Polygone",3.4584854,50.065968,"H13 - Traitement de surface"]
["SSP000308301","59.0250","Arcelor Construction France (ex PAB NORD)",null,"En cours",null,null,"En cours","59447","ONNAING","NORD","HAUTS-DE-FRANCE","Polygone",3.601863,50.393772,"D7 - Caoutchouc et matières plastiques"]
["SSP000308601","59.0258","SNT Société nouvelle de traitement",null,"En cours",null,null,"En cours","59519","RUMEGIES","NORD","HAUTS-DE-FRANCE","Polygone",3.346425,50.491695,"H13 - Traitement de surface"]
["SSP000309101","59.0269","LME (Laminés Marchands Européens)",null,"En cours",null,null,"En cours","59603","TRITH SAINT LEGER","NORD","HAUTS-DE-FRANCE","Polygone",3.492171,50.3374,"J - Sidérurgie, métallurgie, coke"]
["SSP000309301","59.0279","AFR TITAGARH",null,"En cours",null,null,"En cours","59178","DOUAI","NORD","HAUTS-DE-FRANCE","Polygone",3.0946972,50.36916,"H1 - Mécanique, électrique, traitement de surface"]
["SSP000309601","59.0290","AGENCE EDF / GDF",null,"En cours",null,null,"En cours","59178","DOUAI","NORD","HAUTS-DE-FRANCE","Polygone",3.0854187,50.379944,"J1 - Cokéfaction, usines à gaz"]
["SSP000310101","59.0303","ANCIENNE USINE A GAZ DE SAINT-AMAND-LES-EAUX  GDF",null,"En cours",null,null,"En cours","59526","SAINT AMAND LES EAUX","NORD","HAUTS-DE-FRANCE","Polygone",3.424175,50.44399,"J1 - Cokéfaction, usines à gaz"]
["SSP000310701","59.0430","TBN ( rue des capucins)",null,"En cours",null,null,"En cours","59122","CAMBRAI","NORD","HAUTS-DE-FRANCE","Polygone",3.2299824,50.179436,"E3 - Laveries, blanchisseries, pressing"]
["SSP000311301","59.0459","COFRADEC",null,"En cours",null,null,"En cours","59481","LE QUESNOY","NORD","HAUTS-DE-FRANCE","Polygone",3.6464648,50.24811,"H21 - Imprimerie, presse, édition"]
["SSP000311801","59.0185","VALLOUREC",null,"En cours",null,null,"En cours","59033","AULNOYE AYMERIES","NORD","HAUTS-DE-FRANCE","Polygone",3.824787,50.194893,"J - Sidérurgie, métallurgie, coke"]
["SSP000312001","59.0240","TATASTEEL (ex MYRIAD)",null,"En cours",null,null,"En cours","59365","LOUVROIL","NORD","HAUTS-DE-FRANCE","Polygone",3.9554796,50.267227,"J - Sidérurgie, métallurgie, coke"]
["SSP000312301","59.0456","MIROUX",null,"En cours",null,null,"En cours","59230","FERRIERE LA GRANDE","NORD","HAUTS-DE-FRANCE","Polygone",3.9954605,50.254528,"J5 - Fonderie et travail des métaux"]
["SSP000312901","59.0104","DUHEM",null,"En cours",null,null,"En cours","59008","ANICHE","NORD","HAUTS-DE-FRANCE","Polygone",3.266101,50.33778,"D - Chimie, parachimie, pétrole"]
["SSP000313001","59.0106","BRENNTAG",null,"En cours",null,null,"En cours","59616","VIEUX CONDE","NORD","HAUTS-DE-FRANCE","Polygone",3.5625124,50.45503,"D - Chimie, parachimie, pétrole"]
["SSP000313701","59.0230","SEA Société Exploitation Atomiseurs",null,"En cours",null,null,"En cours","59136","LE CATEAU CAMBRESIS","NORD","HAUTS-DE-FRANCE","Polygone",3.541786,50.0909,"G1 - Céramique, verre, matériaux de construction"]
["SSP000314301","59.0470","AXTER",null,"En cours",null,null,"En cours","59156","COURCHELETTES","NORD","HAUTS-DE-FRANCE","Polygone",3.0625768,50.346493,"D - Chimie, parachimie, pétrole"]
["SSP000315001","59.0069","DECHARGE DES PRES D'AINEAUX - BAIL",null,"En cours",null,null,"En cours","59361","LOURCHES","NORD","HAUTS-DE-FRANCE","Polygone",3.3660727,50.307426,"K - Déchets et traitements"]
["SSP000315401","59.0035","ANCIEN CRASSIER USINOR",null,"En cours",null,null,"En cours","59603","TRITH SAINT LEGER","NORD","HAUTS-DE-FRANCE","Polygone",3.4921584,50.337368,"J2 - Sidérurgie, première transformation"]
["SSP000315601","59.0054","FRICHE DAMETA BAIL",null,"En cours",null,null,"En cours","59627","VILLERS SIRE NICOLE","NORD","HAUTS-DE-FRANCE","Polygone",4.023249,50.34124,"H13 - Traitement de surface"]
["SSP000316001","59.0312","SOGESCAUT (ex ANCIENNE USINE ETERNIT)",null,"En cours",null,null,"En cours","59475","PROUVY","NORD","HAUTS-DE-FRANCE","Polygone",3.456688,50.313976,"G13 - Fabrication de produits en amiante-ciment"]
["SSP000316901","59.0565","Décharge carrière Mouche",null,"En cours",null,null,"En cours","59312","HONNECOURT SUR ESCAUT","NORD","HAUTS-DE-FRANCE","Polygone",3.2077525,50.025013]
["SSP000317001","59.0566","Plateau de l'Esperance (ex site de stockage USINOR)",null,"En cours",null,null,"En cours","59365","LOUVROIL","NORD","HAUTS-DE-FRANCE","Polygone",3.9505143,50.262863,"L - Entreposage, transport, commerce"]
["SSP000317701","59.0576","CEREC - ANTONIUS",null,"En cours",null,null,"En cours","59495","RECQUIGNIES","NORD","HAUTS-DE-FRANCE","Polygone",4.0418077,50.28243]
["SSP000318301",null,"PELISSIER METAUX",null,"Clôturée",null,null,"Clôturée","93070","SAINT OUEN","SEINE-SAINT-DENIS","ILE-DE-FRANCE","Polygone",2.325602,48.908833]
["SSP000318701","58.0003","DECHARGE DU NANTIN",null,"En cours",null,null,"En cours","58218","PREMERY","NIEVRE","BOURGOGNE-FRANCHE-COMTE","Polygone",3.3344464,47.186993,"D - Chimie, parachimie, pétrole"]
["SSP000318801","38.0186","TRAVEL Industries",null,"En cours",null,null,"En cours","38114","CLONAS SUR VAREZE","ISERE","AUVERGNE-RHONE-ALPES","Polygone",4.770985,45.41582,"M1 - Industries diverses"]
["SSP000319301",null,"RAFFINERIES DU MIDI ZONE SUD","Raffinerie du midi Zone Sud","Clôturée",null,null,"Clôturée","34023","BALARUC LES BAINS","HERAULT","OCCITANIE","Polygone",3.6928208,43.443707,null,"05.31 - Raffinage de pétrole"]
["SSP000319601",null,"Société des Pétroles Shell station Alésia",null,"Clôturée",null,null,"Clôturée","75056","PARIS","PARIS","ILE-DE-FRANCE","Polygone",2.3158054,48.83092]
["SSP000320201",null,"Citroën",null,"Clôturée",null,null,"Clôturée","75056","PARIS","PARIS","ILE-DE-FRANCE","Polygone",2.2941806,48.83103]
["SSP000320401",null,"EURO-CHIF ZELCER FRERES",null,"Clôturée",null,null,"Clôturée","93070","SAINT OUEN","SEINE-SAINT-DENIS","ILE-DE-FRANCE","Polygone",2.3502758,48.903625]
["SSP000320701","49.0039","VALEO EQUIPEMENTS ELECTRIQUES MOTEUR",null,"En cours",null,null,"En cours","49007","ANGERS","MAINE-ET-LOIRE","PAYS DE LA LOIRE","Polygone",-0.54380524,47.442726,"H1 - Mécanique, électrique, traitement de surface"]
["SSP000321301",null,"Fonderie BERNARD",null,"Clôturée",null,null,"Clôturée","95598","SOISY SOUS MONTMORENCY","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.2979527,48.98369]
["SSP000321801","49.0040","GALVANOTEC",null,"En cours",null,null,"En cours","49015","AVRILLE","MAINE-ET-LOIRE","PAYS DE LA LOIRE","Polygone",-0.61282045,47.518322,"H13 - Traitement de surface"]
["SSP000321901",null,"RENAULT CTR",null,"Clôturée",null,null,"Clôturée","92063","RUEIL MALMAISON","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.198673,48.873024]
["SSP000322401",null,"SATRE",null,"Clôturée",null,null,"Clôturée","93070","SAINT OUEN","SEINE-SAINT-DENIS","ILE-DE-FRANCE","Polygone",2.341097,48.913498]
["SSP000322901","78.0043","Ancienne usine à gaz de Rambouillet",null,"En cours",null,null,"En cours","78517","RAMBOUILLET","YVELINES","ILE-DE-FRANCE","Polygone",1.8294916,48.639603,"J1 - Cokéfaction, usines à gaz"]
["SSP000323901",null,"Aide sociale à l'enfance - Résidence jeunes",null,"Clôturée",null,null,"Clôturée","89387","SENS","YONNE","BOURGOGNE-FRANCHE-COMTE","Polygone",3.2835898,48.201767]
["SSP000324101",null,"Ecole primaire publique Charles Michels",null,"Clôturée",null,null,"Clôturée","89387","SENS","YONNE","BOURGOGNE-FRANCHE-COMTE","Polygone",3.2830505,48.193474]
["SSP000324501",null,"Lycée Mathias",null,"Clôturée",null,null,"Clôturée","71076","CHALON SUR SAONE","SAONE-ET-LOIRE","BOURGOGNE-FRANCHE-COMTE","Polygone",4.8621974,46.787643]
["SSP000325001","21.0062","Station service TOTAL Beaune-Merceuil",null,"En cours",null,null,"En cours","21405","MERCEUIL","COTE-D'OR","BOURGOGNE-FRANCHE-COMTE","Polygone",4.8392534,46.961407]
["SSP000325501",null,"Ancienne décharge du Cosquet",null,"Clôturée",null,null,"Clôturée","22228","PLOUNEVEZ MOEDEC","COTES-D'ARMOR","BRETAGNE","Polygone",-3.468935,48.54799]
["SSP000325601",null,"Total relais d'Austerlitz",null,"Clôturée",null,null,"Clôturée","75056","PARIS","PARIS","ILE-DE-FRANCE","Polygone",2.3717475,48.837994]
["SSP000326001",null,"Ancienne décharge de Toull ar Hoat",null,"Clôturée",null,null,"Clôturée","22231","PLOURAC'H","COTES-D'ARMOR","BRETAGNE","Polygone",-3.5357141,48.403797]
["SSP000326601","71.0009","Site Bitulac",null,"En cours",null,null,"En cours","71190","EPINAC","SAONE-ET-LOIRE","BOURGOGNE-FRANCHE-COMTE","Polygone",4.5208774,46.983543,"D42 - Fabrication de peintures"]
["SSP000327101","71.0044","TOTAL RAFFINAGE MARKETING (Chalon, ex ELF)",null,"En cours",null,null,"En cours","71076","CHALON SUR SAONE","SAONE-ET-LOIRE","BOURGOGNE-FRANCHE-COMTE","Polygone",4.867777,46.797203,"L23 - Détail de carburants"]
["SSP000327301","92.0010","ENGIE",null,"En cours",null,null,"En cours","92036","GENNEVILLIERS","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.3088965,48.941605,"J1 - Cokéfaction, usines à gaz"]
["SSP000327501","89.0019","Société GRAINDORGE",null,"En cours",null,null,"En cours","89387","SENS","YONNE","BOURGOGNE-FRANCHE-COMTE","Polygone",3.2818034,48.191833,"H13 - Traitement de surface"]
["SSP000328001",null,"Société Commerciale Automobile",null,"Clôturée",null,null,"Clôturée","75056","PARIS","PARIS","ILE-DE-FRANCE","Polygone",2.376909,48.862694]
["SSP000328501",null,"BP Porte de la Vilette",null,"Clôturée",null,null,"Clôturée","75056","PARIS","PARIS","ILE-DE-FRANCE","Polygone",2.3872342,48.899033]
["SSP000328601","78.0113","TOTAL RAFFINAGE MARKETING",null,"En cours",null,null,"En cours","78517","RAMBOUILLET","YVELINES","ILE-DE-FRANCE","Polygone",1.8304546,48.649937]
["SSP000329101",null,"Crèche collective Rouen",null,"Clôturée",null,null,"Clôturée","75056","PARIS","PARIS","ILE-DE-FRANCE","Polygone",2.374103,48.887474]
["SSP000329701","71.0071","GDF SUEZ ENERGIE SERVICES (ex COFATHEC)",null,"En cours",null,null,"En cours","71076","CHALON SUR SAONE","SAONE-ET-LOIRE","BOURGOGNE-FRANCHE-COMTE","Polygone",4.851482,46.81647,"I11 - Centrales électriques thermiques"]
["SSP000330201",null,"SHELL",null,"Clôturée",null,null,"Clôturée","92040","ISSY LES MOULINEAUX","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.2562325,48.8244]
["SSP000330401","21.0017","Ancienne usine à gaz",null,"En cours",null,null,"En cours","21054","BEAUNE","COTE-D'OR","BOURGOGNE-FRANCHE-COMTE","Polygone",4.846741,47.02242,"J1 - Cokéfaction, usines à gaz"]
["SSP000330701","58.0010","Ancienne usine à gaz",null,"Clôturée",null,"2010-09-30","Clôturée","58117","FOURCHAMBAULT","NIEVRE","BOURGOGNE-FRANCHE-COMTE","Polygone",3.087092,47.01777,"J1 - Cokéfaction, usines à gaz"]
["SSP000331501","71.0026","Ancienne usine à gaz",null,"Clôturée",null,"2010-09-30","Clôturée","71076","CHALON SUR SAONE","SAONE-ET-LOIRE","BOURGOGNE-FRANCHE-COMTE","Polygone",4.8476925,46.779808,"J1 - Cokéfaction, usines à gaz"]
["SSP000332101",null,"PSA VEUVE LACROIX",null,"Clôturée",null,null,"Clôturée","92035","LA GARENNE COLOMBES","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.2312512,48.903694]
["SSP000332201","71.0005","NFM technologies (Framatome)",null,"En cours",null,null,"En cours","71153","LE CREUSOT","SAONE-ET-LOIRE","BOURGOGNE-FRANCHE-COMTE","Polygone",4.4517064,46.792522,"J23 - Première transformation de l'acier"]
["SSP000332501","91.0079","Shell Athis mons",null,"En cours",null,null,"En cours","91027","ATHIS MONS","ESSONNE","ILE-DE-FRANCE","Polygone",2.391344,48.69647,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000333301",null,"TRW Lucas Aérospace",null,"Clôturée",null,null,"Clôturée","92004","ASNIERES SUR SEINE","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.3136196,48.918232]
["SSP000333801","59.0098","ETS WATTEL ET FILS",null,"En cours",null,null,"En cours","59609","VENDEVILLE","NORD","HAUTS-DE-FRANCE","Polygone",3.0904224,50.57917,"K52 - Dépôts de ferraille"]
["SSP000334001","49.0029","Thermoplastiques Cousin Tessier",null,"En cours",null,null,"En cours","49027","BEGROLLES EN MAUGES","MAINE-ET-LOIRE","PAYS DE LA LOIRE","Polygone",-0.9537911,47.138042,"D34 - Fabrication de matières plastiques de base"]
["SSP000334601","78.0112","Nouvelle APF",null,"En cours",null,null,"En cours","78358","MAISONS LAFFITTE","YVELINES","ILE-DE-FRANCE","Polygone",2.1374311,48.94839]
["SSP000335101","45.0016","Agence EDF / GDF Services",null,"En cours",null,null,"En cours","45208","MONTARGIS","LOIRET","CENTRE-VAL DE LOIRE","Polygone",2.7313938,47.990173,"J1 - Cokéfaction, usines à gaz"]
["SSP000335501","78.0038","EXPLOITATION DE L'ILE LABORDE",null,"En cours",null,null,"En cours","78358","MAISONS LAFFITTE","YVELINES","ILE-DE-FRANCE","Polygone",2.138461,48.934196]
["SSP000335801","59.0573","FUJIFILM",null,"En cours",null,null,"En cours","59009","VILLENEUVE D'ASCQ","NORD","HAUTS-DE-FRANCE","Polygone",3.1423926,50.64247,"D5 - Fabrication de produits photographiques"]
["SSP000336101","59.0579","BRAMPTON RENOLD",null,"En cours",null,null,"En cours","59560","SECLIN","NORD","HAUTS-DE-FRANCE","Polygone",3.0382478,50.566795]
["SSP000336701","59.0593","RHODIA OPERATIONS SAS – PARTIE MINERALE",null,"En cours",null,null,"En cours","59527","SAINT ANDRE LEZ LILLE","NORD","HAUTS-DE-FRANCE","Polygone",3.0606642,50.663067,"D - Chimie, parachimie, pétrole"]
["SSP000337001","78.0010","ANCIENNE USINE A GAZ DU PECQ",null,"En cours",null,null,"En cours","78481","LE PECQ","YVELINES","ILE-DE-FRANCE","Polygone",2.1062458,48.89993,"J1 - Cokéfaction, usines à gaz"]
["SSP000337201",null,"La Charbonnière",null,"Clôturée",null,null,"Clôturée","75056","PARIS","PARIS","ILE-DE-FRANCE","Polygone",2.377853,48.901333]
["SSP000338101","59.0587","ROZENDAAL",null,"En cours",null,null,"En cours","59368","LA MADELEINE","NORD","HAUTS-DE-FRANCE","Polygone",3.067996,50.664368]
["SSP000338601","59.0564","CARBONISAGE de MOUVAUX",null,"En cours",null,null,"En cours","59421","MOUVAUX","NORD","HAUTS-DE-FRANCE","Polygone",3.1361935,50.712257,"E13 - Blanchiment, teinture, impression"]
["SSP000339001","59.0548","Sodemeca",null,"En cours",null,null,"En cours","59437","NOYELLES LES SECLIN","NORD","HAUTS-DE-FRANCE","Polygone",3.0290053,50.572292,"D34 - Fabrication de matières plastiques de base"]
["SSP000339301",null,"Station service TOTAL (ex-ELF)",null,"Clôturée",null,null,"Clôturée","78545","SAINT CYR L'ECOLE","YVELINES","ILE-DE-FRANCE","Polygone",2.0731716,48.804417]
["SSP000339501","59.0158","LIBERTE EDITIONS",null,"En cours",null,null,"En cours","59350","LILLE","NORD","HAUTS-DE-FRANCE","Polygone",3.0973196,50.63456,"H21 - Imprimerie, presse, édition"]
["SSP000340001",null,"BOST Marcel (Ets)",null,"Clôturée",null,null,"Clôturée","60067","BETHISY SAINT MARTIN","OISE","HAUTS-DE-FRANCE","Polygone",2.803826,49.287098]
["SSP000340301",null,"Collège Albert Samain",null,"Clôturée",null,null,"Clôturée","59512","ROUBAIX","NORD","HAUTS-DE-FRANCE","Polygone",3.1863976,50.702087]
["SSP000340501",null,"Relais Total Rivesaltes",null,"Clôturée",null,null,"Clôturée","66164","RIVESALTES","PYRENEES-ORIENTALES","OCCITANIE","Polygone",2.871528,42.76923]
["SSP000342301",null,"College La Cerisaie",null,"Clôturée",null,null,"Clôturée","94018","CHARENTON LE PONT","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.4090588,48.82071]
["SSP000342701",null,"LES VANETTES",null,"Clôturée",null,null,"Clôturée","92026","COURBEVOIE","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.2672038,48.900387]
["SSP000343301","19.0025","VAURIE",null,"En cours",null,null,"En cours","19229","SAINT PANTALEON DE LARCHE","CORREZE","NOUVELLE-AQUITAINE","Polygone",1.4165696,45.132378,"K5 - Récupération, dépôts de ferrailles"]
["SSP000343401","19.0026","ALVEA",null,"En cours",null,null,"En cours","19031","BRIVE LA GAILLARDE","CORREZE","NOUVELLE-AQUITAINE","Polygone",1.505978,45.147675,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000344001",null,"SNCF La Plaine",null,"Clôturée",null,null,"Clôturée","93066","SAINT DENIS","SEINE-SAINT-DENIS","ILE-DE-FRANCE","Polygone",2.3522577,48.912407]
["SSP000344601","88.0098","Ancienne décharge INTERNATIONAL PAPER",null,"En cours",null,null,"En cours","88009","ANOULD","VOSGES","GRAND EST","Polygone",6.96358,48.186893]
["SSP000345001","19.0021","DECONS RECUPERATIONS",null,"En cours",null,null,"En cours","19279","VARS SUR ROSEIX","CORREZE","NOUVELLE-AQUITAINE","Polygone",1.3745937,45.25425,"K52 - Dépôts de ferraille"]
["SSP000345201","88.0084","Société Lorraine de Céramique",null,"En cours",null,null,"En cours","88046","BEAUMENIL","VOSGES","GRAND EST","Polygone",6.721131,48.182896]
["SSP000345901","25.0032","RAFFINERIE DU MIDI",null,"En cours",null,null,"En cours","25056","BESANCON","DOUBS","BOURGOGNE-FRANCHE-COMTE","Polygone",6.045374,47.227245,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000347001","25.0064","SODEX HUART ROLAND",null,"En cours",null,null,"En cours","25519","SAINT HIPPOLYTE","DOUBS","BOURGOGNE-FRANCHE-COMTE","Polygone",6.8153214,47.325497]
["SSP000347501","25.0088","CAGB BASSIN ACCOSTAGE (Deluz)",null,"En cours",null,null,"En cours","25197","DELUZ","DOUBS","BOURGOGNE-FRANCHE-COMTE","Polygone",6.2023935,47.29113,"C2 - Industrie du papier et du carton"]
["SSP000347601","39.0002","Ancienne usine à gaz",null,"En cours",null,null,"En cours","39300","LONS LE SAUNIER","JURA","BOURGOGNE-FRANCHE-COMTE","Polygone",5.543842,46.676163,"J1 - Cokéfaction, usines à gaz"]
["SSP000348101","39.0038","CASINO_Station Service",null,"En cours",null,null,"En cours","39097","CHAMPAGNOLE","JURA","BOURGOGNE-FRANCHE-COMTE","Polygone",5.916877,46.74299,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000348401","45.0042","Ex magasin Leclerc",null,"En cours",null,null,"En cours","45004","AMILLY","LOIRET","CENTRE-VAL DE LOIRE","Polygone",2.731914,47.973457,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000349201","78.0003","DECHARGE SOTRADEC",null,"En cours",null,null,"En cours","78238","FLINS SUR SEINE","YVELINES","ILE-DE-FRANCE","Polygone",1.8831173,48.951443,"F32 - Carrières"]
["SSP000349301","19.0024","VICHY",null,"En cours",null,null,"En cours","19273","TURENNE","CORREZE","NOUVELLE-AQUITAINE","Polygone",1.6019005,45.03694,"K5 - Récupération, dépôts de ferrailles"]
["SSP000349901",null,"Moulin des Ecluses Parcelle B253",null,"Clôturée",null,null,"Clôturée","59080","BEUVRY LA FORET","NORD","HAUTS-DE-FRANCE","Polygone",3.2716649,50.45656]
["SSP000350201","25.0037","WITTMER",null,"En cours",null,null,"En cours","25539","SELONCOURT","DOUBS","BOURGOGNE-FRANCHE-COMTE","Polygone",6.867269,47.459866,"H11 - Usinage"]
["SSP000350601","78.0082","METZELER",null,"En cours",null,null,"En cours","78124","CARRIERES SUR SEINE","YVELINES","ILE-DE-FRANCE","Polygone",2.2006428,48.916046,"D71 - Industrie du caoutchouc"]
["SSP000350801","25.0068","BOLLORE ENERGIE (ex. COMBUSTIBLES DE L'EST)",null,"En cours",null,null,"En cours","25388","MONTBELIARD","DOUBS","BOURGOGNE-FRANCHE-COMTE","Polygone",6.797622,47.51408,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000351301","39.0031","Scierie PERRIER SARL",null,"En cours",null,null,"En cours","39411","PERRIGNY","JURA","BOURGOGNE-FRANCHE-COMTE","Polygone",5.581834,46.666058,"C13 - Traitement du bois"]
["SSP000351601","59.0554","GTN (Groupement Textile du Nord)",null,"En cours",null,null,"En cours","59382","MARETZ","NORD","HAUTS-DE-FRANCE","Polygone",3.4239337,50.05017,"E13 - Blanchiment, teinture, impression"]
["SSP000352201","36.0015","Agence de Gaz de France",null,"En cours",null,null,"En cours","36044","CHATEAUROUX","INDRE","CENTRE-VAL DE LOIRE","Polygone",1.7014028,46.809464,"J1 - Cokéfaction, usines à gaz"]
["SSP000352301","36.0016","EDF/ GDF SERVICES INDRE EN BERRY",null,"En cours",null,null,"En cours","36088","ISSOUDUN","INDRE","CENTRE-VAL DE LOIRE","Polygone",1.9902972,46.951958,"J1 - Cokéfaction, usines à gaz"]
["SSP000353001","88.0105","Verrerie - Cristallerie de Portieux",null,"En cours",null,null,"En cours","88355","PORTIEUX","VOSGES","GRAND EST","Polygone",6.3922524,48.357044]
["SSP000353801","21.0033","VM Tubes (Ex-VALTUBES ) ancienne usine",null,"En cours",null,null,"En cours","21425","MONTBARD","COTE-D'OR","BOURGOGNE-FRANCHE-COMTE","Polygone",4.3318315,47.620487,"J23 - Première transformation de l'acier"]
["SSP000354201","21.0078","BOLLORE ENERGIE SA",null,"En cours",null,null,"En cours","21231","DIJON","COTE-D'OR","BOURGOGNE-FRANCHE-COMTE","Polygone",5.027276,47.30173]
["SSP000354301","88.0058","SISOV Contrexeville",null,"En cours",null,null,"En cours","88114","CONTREXEVILLE","VOSGES","GRAND EST","Polygone",5.8667393,48.18917,"K2 - Traitement de déchets urbains"]
["SSP000355301","55.0009","CRASSIER TREFILEUROPE ET BASSINS A BOUES DE MARNAVAL",null,"En cours",null,null,"En cours","55010","ANCERVILLE","MEUSE","GRAND EST","Polygone",4.9980755,48.619205,"J2 - Sidérurgie, première transformation"]
["SSP000355801","64.0140","TEPF puits Lacq 15 et manifold M3LS - LA015 et M3LS",null,"En cours",null,null,"En cours","64300","LACQ","PYRENEES-ATLANTIQUES","NOUVELLE-AQUITAINE","Polygone",-0.63377845,43.41793]
["SSP000356401","64.0149","TEPF puits Lacq 79 - LA079",null,"En cours",null,null,"En cours","64300","LACQ","PYRENEES-ATLANTIQUES","NOUVELLE-AQUITAINE","Polygone",-0.63391703,43.41497]
["SSP000356801","80.0077","BRICARD",null,"En cours",null,null,"En cours","80360","FRESSENNEVILLE","SOMME","HAUTS-DE-FRANCE","Polygone",1.578196,50.069878,"H1 - Mécanique, électrique, traitement de surface"]
["SSP000357101","80.0102","SARL BAILLEUL",null,"En cours",null,null,"En cours","80654","QUESNOY LE MONTANT","SOMME","HAUTS-DE-FRANCE","Polygone",1.6744571,50.103573]
["SSP000357601","40.0051","MIRAMBET",null,"En cours",null,null,"En cours","40058","CACHEN","LANDES","NOUVELLE-AQUITAINE","Polygone",-0.40288243,44.06278,"C13 - Traitement du bois"]
["SSP000358001","49.0037","SAI TS",null,"En cours",null,null,"En cours","49367","VERN D'ANJOU","MAINE-ET-LOIRE","PAYS DE LA LOIRE","Polygone",-0.8404638,47.59865,"H13 - Traitement de surface"]
["SSP000358101","49.0033","Guiet",null,"En cours",null,null,"En cours","49218","MONTREVAULT","MAINE-ET-LOIRE","PAYS DE LA LOIRE","Polygone",-1.1136283,47.280174,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000358501",null,"Ecole St Dominique",null,"Clôturée",null,null,"Clôturée","78481","LE PECQ","YVELINES","ILE-DE-FRANCE","Polygone",2.101839,48.887764]
["SSP000359001","80.0058","VALNOR SA",null,"En cours",null,null,"En cours","80274","EPPEVILLE","SOMME","HAUTS-DE-FRANCE","Polygone",3.033929,49.739056,"K31 - Incinération"]
["SSP000359701","36.0018","Friche Industrielle BALSAN",null,"En cours",null,null,"En cours","36044","CHATEAUROUX","INDRE","CENTRE-VAL DE LOIRE","Polygone",1.6756089,46.812363]
["SSP000360001","36.0018","Société Nouvelle Le Flockage",null,"En cours",null,null,"En cours","36044","CHATEAUROUX","INDRE","CENTRE-VAL DE LOIRE","Polygone",1.6765555,46.813217,"E1 - Textile et habillement, teinture, impression"]
["SSP000360401","90.0014","Ancienne usine à gaz",null,"Clôturée",null,"2012-09-04","Clôturée","90052","GIROMAGNY","TERRITOIRE DE BELFORT","BOURGOGNE-FRANCHE-COMTE","Polygone",6.8293524,47.735046,"J1 - Cokéfaction, usines à gaz"]
["SSP000361001","89.0036","SCHIEVER CARBURANT",null,"En cours",null,null,"En cours","89382","SEIGNELAY","YONNE","BOURGOGNE-FRANCHE-COMTE","Polygone",3.609277,47.903015,"L23 - Détail de carburants"]
["SSP000361401",null,"Stockage de broyats du Bélieu",null,"Clôturée",null,null,"Clôturée","25050","LE BELIEU","DOUBS","BOURGOGNE-FRANCHE-COMTE","Polygone",6.6459885,47.11675]
["SSP000361501","25.0041","LEVIER INDUSTRIES SAS COMPOSANTS MECANIQ",null,"En cours",null,null,"En cours","25334","LEVIER","DOUBS","BOURGOGNE-FRANCHE-COMTE","Polygone",6.129894,46.95622,"H15 - Assemblage, montage"]
["SSP000361901","70.0029","SICTOM",null,"En cours",null,null,"En cours","70339","MELISEY","HAUTE-SAONE","BOURGOGNE-FRANCHE-COMTE","Polygone",6.5884714,47.78609,"K31 - Incinération"]
["SSP000362801","24.0026","BOUCHILLOU ALKYA",null,"En cours",null,null,"En cours","24037","BERGERAC","DORDOGNE","NOUVELLE-AQUITAINE","Polygone",0.49842855,44.841694]
["SSP000363301","24.0059","SIMPLY MARKET",null,"En cours",null,null,"En cours","24547","TERRASSON LAVILLEDIEU","DORDOGNE","NOUVELLE-AQUITAINE","Polygone",1.3178864,45.12904]
["SSP000363601","24.0042","SVISN",null,"En cours",null,null,"En cours","24350","RAZAC SUR L'ISLE","DORDOGNE","NOUVELLE-AQUITAINE","Polygone",0.61537606,45.17525]
["SSP000364101",null,"DEA de Dijon K1",null,"Clôturée",null,null,"Clôturée","21355","LONGVIC","COTE-D'OR","BOURGOGNE-FRANCHE-COMTE","Polygone",5.081266,47.27425]
["SSP000364601","49.0026","Point P Trouillard",null,"En cours",null,null,"En cours","49099","CHOLET","MAINE-ET-LOIRE","PAYS DE LA LOIRE","Polygone",-0.86561084,47.075256,"C13 - Traitement du bois"]
["SSP000365201","39.0032","Station-service TOTAL Relais Rouget de Lisle",null,"En cours",null,null,"En cours","39362","MONTMOROT","JURA","BOURGOGNE-FRANCHE-COMTE","Polygone",5.527875,46.67147,"L23 - Détail de carburants"]
["SSP000365301",null,"DEA Toul Rosières",null,"Clôturée",null,null,"Clôturée","54463","ROSIERES EN HAYE","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",5.974359,48.793747]
["SSP000365701",null,"ETAMAT de Thouars Groupe 4",null,"Clôturée",null,null,"Clôturée","79329","THOUARS","DEUX-SEVRES","NOUVELLE-AQUITAINE","Polygone",-0.17832355,46.98407]
["SSP000366401",null,"Air Précision",null,"Clôturée",null,null,"Clôturée","92022","CHAVILLE","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.1889164,48.800255]
["SSP000366701",null,"Ancienne maison du directeur de la société YAB",null,"Clôturée",null,null,"Clôturée","94052","NOGENT SUR MARNE","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.4914248,48.834743]
["SSP000366901","62.0019","BP - USINE GERLAND",null,"En cours",null,null,"En cours","62240","CORBEHEM","PAS-DE-CALAIS","HAUTS-DE-FRANCE","Polygone",3.0504284,50.338177,"D - Chimie, parachimie, pétrole"]
["SSP000367401","62.0044","POLIMERI (ex ENICHEM)",null,"En cours",null,null,"En cours","62563","MAZINGARBE","PAS-DE-CALAIS","HAUTS-DE-FRANCE","Polygone",2.725377,50.470676,"D34 - Fabrication de matières plastiques de base"]
["SSP000367901","62.0007","COKERIE DE CHOCQUES",null,"En cours",null,null,"En cours","62224","CHOCQUES","PAS-DE-CALAIS","HAUTS-DE-FRANCE","Polygone",2.5725386,50.53373,"J1 - Cokéfaction, usines à gaz"]
["SSP000368301","62.0017","ANCIENS LAVOIRS ET COKERIE DE MAZINGARBE",null,"En cours",null,null,"En cours","62563","MAZINGARBE","PAS-DE-CALAIS","HAUTS-DE-FRANCE","Polygone",2.7260127,50.46484,"F11 - Houillères"]
["SSP000368401","62.0020","Terril 205 CDF et bassins à goudrons",null,"En cours",null,null,"En cours","62277","DROCOURT","PAS-DE-CALAIS","HAUTS-DE-FRANCE","Polygone",2.9335263,50.405968,"F11 - Houillères"]
["SSP000368801","62.0035","NORD HELIO SERVICE",null,"En cours",null,null,"En cours","62563","MAZINGARBE","PAS-DE-CALAIS","HAUTS-DE-FRANCE","Polygone",2.757978,50.464466,"H13 - Traitement de surface"]
["SSP000369301","62.0067","COKES DE DROCOURT",null,"En cours",null,null,"En cours","62277","DROCOURT","PAS-DE-CALAIS","HAUTS-DE-FRANCE","Polygone",2.9288108,50.40188,"F11 - Houillères"]
["SSP000369601","62.0083","NOROXO",null,"En cours",null,null,"En cours","62413","HARNES","PAS-DE-CALAIS","HAUTS-DE-FRANCE","Polygone",2.875331,50.447807,"D - Chimie, parachimie, pétrole"]
["SSP000369801","62.0090","VYNOVA (ex SAV)",null,"En cours",null,null,"En cours","62186","BULLY LES MINES","PAS-DE-CALAIS","HAUTS-DE-FRANCE","Polygone",2.7291698,50.473576,"D - Chimie, parachimie, pétrole"]
["SSP000370301","62.0106","EDF GDF AGENCE DE BETHUNE",null,"En cours",null,null,"En cours","62119","BETHUNE","PAS-DE-CALAIS","HAUTS-DE-FRANCE","Polygone",2.6350105,50.523678,"J1 - Cokéfaction, usines à gaz"]
["SSP000370801","62.0139","SUEZ RV NORD EST",null,"En cours",null,null,"En cours","62443","HERSIN COUPIGNY","PAS-DE-CALAIS","HAUTS-DE-FRANCE","Polygone",2.621674,50.433533,"K21 - Décharges d'ordures ménagères"]
["SSP000371401","62.0064","ARKEMA (ex CECA)",null,"En cours",null,null,"En cours","62753","SAINT LAURENT BLANGY","PAS-DE-CALAIS","HAUTS-DE-FRANCE","Polygone",2.8272007,50.297974,"D - Chimie, parachimie, pétrole"]
["SSP000371501","62.0086","Prefere Résins France SAS (ex DYNEA Resine France / ex PERSTOP)",null,"En cours",null,null,"En cours","62173","BREBIERES","PAS-DE-CALAIS","HAUTS-DE-FRANCE","Polygone",3.0198622,50.336216,"D - Chimie, parachimie, pétrole"]
["SSP000371901","62.0053","ARRAS MAXEI",null,"En cours",null,null,"En cours","62041","ARRAS","PAS-DE-CALAIS","HAUTS-DE-FRANCE","Polygone",2.7777743,50.297874,"H16 - Piles électriques et accumulateurs (fabrication de)"]
["SSP000372401","62.0012","ANCIENS LAVOIRS ET COKERIE DE LIEVIN CDF",null,"En cours",null,null,"En cours","62510","LIEVIN","PAS-DE-CALAIS","HAUTS-DE-FRANCE","Polygone",2.778517,50.4082,"F11 - Houillères"]
["SSP000372701","62.0153","SA H. LOYEZ",null,"En cours",null,null,"En cours","62907","LIBERCOURT","PAS-DE-CALAIS","HAUTS-DE-FRANCE","Polygone",3.007157,50.486195]
["SSP000373001",null,"MICHEL COMBUSTIBLES",null,"Clôturée",null,null,"Clôturée","78265","GARANCIERES","YVELINES","ILE-DE-FRANCE","Polygone",1.7500776,48.81908]
["SSP000373801",null,"CRE de Montbartier parc n°1",null,"Clôturée",null,null,"Clôturée","82123","MONTBARTIER","TARN-ET-GARONNE","OCCITANIE","Polygone",1.2607266,43.91992]
["SSP000374801","78.0069","OXYMINE",null,"En cours",null,null,"En cours","78498","POISSY","YVELINES","ILE-DE-FRANCE","Polygone",2.0496514,48.936455,"G - Industries minérales"]
["SSP000376101","53.0030","Godeloup (ex-Lory)",null,"Clôturée",null,null,"Clôturée","53096","ERNEE","MAYENNE","PAYS DE LA LOIRE","Polygone",-0.9339522,48.296288,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000376301","53.0040","ADONIAL ex-SINIAT",null,"En cours",null,null,"En cours","53014","AZE","MAYENNE","PAYS DE LA LOIRE","Polygone",-0.6931572,47.83814,"D34 - Fabrication de matières plastiques de base"]
["SSP000376701","53.0017","MANN-HUMMEL",null,"Clôturée",null,null,"Clôturée","53130","LAVAL","MAYENNE","PAYS DE LA LOIRE","Polygone",-0.7493391,48.055744,null,"31.13 - Fabrication de pièces et équipements spécifiques pour automobiles"]
["SSP000377201","53.0044","Ernedis",null,"En cours",null,null,"En cours","53096","ERNEE","MAYENNE","PAYS DE LA LOIRE","Polygone",-0.92629814,48.29631]
["SSP000377501",null,"DEA de Toulouse  Francazal",null,"Clôturée",null,null,"Clôturée","31157","CUGNAUX","HAUTE-GARONNE","OCCITANIE","Polygone",1.3623011,43.542046]
["SSP000377701","47.0022","INDOFURANE-AMENDOR Brimont",null,"En cours",null,null,"En cours","47031","BOE","LOT-ET-GARONNE","NOUVELLE-AQUITAINE","Polygone",0.6635516,44.175594,"D31 - Industrie du chlore"]
["SSP000378501","40.0085","BERNARD",null,"En cours",null,null,"En cours","40331","VILLENEUVE DE MARSAN","LANDES","NOUVELLE-AQUITAINE","Polygone",-0.31073388,43.88458]
["SSP000378801","40.0126","NICOLAS (ex LABEYRIE Jacques S.A.)",null,"En cours",null,null,"En cours","40175","MAURRIN","LANDES","NOUVELLE-AQUITAINE","Polygone",-0.37542385,43.8243,"C13 - Traitement du bois"]
["SSP000379301","54.0133","SA des anciens établissements XENARD","Cessation d'activités 2014","En cours",null,null,"En cours","54498","SEICHAMPS","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",6.2528563,48.710503,null,null,"28.5D - Mécanique générale"]
["SSP000379401","38.0017","Carrière du Lémand",null,"En cours",null,null,"En cours","38553","VILLEFONTAINE","ISERE","AUVERGNE-RHONE-ALPES","Polygone",5.1588416,45.62276]
["SSP000380001","47.0039","LESPARRE EURL",null,"En cours",null,null,"En cours","47302","SOS","LOT-ET-GARONNE","NOUVELLE-AQUITAINE","Polygone",0.15401825,44.0635]
["SSP000380401","54.0112","ex GOUVY (Forges de Dieulouard)","Cessation d'acitivités 2010","En cours",null,null,"En cours","54157","DIEULOUARD","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",6.074059,48.841488,"H13 - Traitement de surface"]
["SSP000380901","34.0020","Parc industriel de la Pompignane","IBM","En cours",null,null,"En cours","34172","MONTPELLIER","HERAULT","OCCITANIE","Polygone",3.905714,43.616295,"H18 - Composants électroniques (fabrication de)"]
["SSP000381101","54.0068","Zone des étangs Cogénor",null,"En cours",null,null,"En cours","54397","NEUVES MAISONS","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",6.106003,48.6058]
["SSP000381701","16.0020","AMCOR FLEXIBLES SITE DU CHEMIN LUSSAULT",null,"En cours",null,null,"En cours","16028","BARBEZIEUX SAINT HILAIRE","CHARENTE","NOUVELLE-AQUITAINE","Polygone",-0.15190008,45.47064,"D34 - Fabrication de matières plastiques de base"]
["SSP000382001","16.0028","Leroy Somer - Rousselot (La Forêt des Moines)",null,"En cours",null,null,"En cours","16113","LA COURONNE","CHARENTE","NOUVELLE-AQUITAINE","Polygone",0.092028536,45.631847,"K36 - Mise en décharge"]
["SSP000382501","80.0001","S.P.R.B. VYCONE",null,"En cours",null,null,"En cours","80186","CHAULNES","SOMME","HAUTS-DE-FRANCE","Polygone",2.7944393,49.806583,"D4 - Encres, vernis, peintures, colles (fabrication de)"]
["SSP000382601","17.0013","SOCOFER",null,"En cours",null,null,"En cours","17300","LA ROCHELLE","CHARENTE-MARITIME","NOUVELLE-AQUITAINE","Polygone",-1.1970415,46.157814,"D36 - Fabrication des engrais"]
["SSP000383001",null,"Rosenlew - Saint Frères",null,"Clôturée",null,null,"Clôturée","80071","BEAUVAL","SOMME","HAUTS-DE-FRANCE","Polygone",2.3428679,50.113712]
["SSP000383401","17.0024","SPIMEC-SPIRAL",null,"En cours",null,null,"En cours","17274","PERIGNY","CHARENTE-MARITIME","NOUVELLE-AQUITAINE","Polygone",-1.1126915,46.157112,"H1 - Mécanique, électrique, traitement de surface"]
["SSP000383901","17.0036","Zodiac",null,"En cours",null,null,"En cours","17299","ROCHEFORT","CHARENTE-MARITIME","NOUVELLE-AQUITAINE","Polygone",-0.9557925,45.930717,"M1 - Industries diverses"]
["SSP000384001","17.0038","SERGENT-PROLAC",null,"En cours",null,null,"En cours","17434","SURGERES","CHARENTE-MARITIME","NOUVELLE-AQUITAINE","Polygone",-0.7539557,46.105743,"D4 - Encres, vernis, peintures, colles (fabrication de)"]
["SSP000384701","79.0028","TOUCHARD",null,"En cours",null,null,"En cours","79179","MONCOUTANT","DEUX-SEVRES","NOUVELLE-AQUITAINE","Polygone",-0.59356415,46.73211,"C11 - Scierie, fabrication de panneaux"]
["SSP000385001","86.0011","TIMAC AGRO (ex INTERFERTIL ex AGRI POITOU)",null,"En cours",null,null,"En cours","86016","AVANTON","VIENNE","NOUVELLE-AQUITAINE","Polygone",0.2917626,46.66167,"B3 - Fabrication d'aliments pour animaux"]
["SSP000385201","86.0013","New Fabris",null,"En cours",null,null,"En cours","86066","CHATELLERAULT","VIENNE","NOUVELLE-AQUITAINE","Polygone",0.54446894,46.848]
["SSP000385501","86.0016","Cave du Haut Poitou - racheté par AMPELIDAE",null,"En cours",null,null,"En cours","86177","NEUVILLE DE POITOU","VIENNE","NOUVELLE-AQUITAINE","Polygone",0.2526739,46.683884,"B2 - Industrie des boissons"]
["SSP000386001",null,"FILLOUX",null,"Clôturée",null,null,"Clôturée","95598","SOISY SOUS MONTMORENCY","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.2998238,48.984276]
["SSP000386401","80.0107","SARL ECLACHROME",null,"En cours",null,null,"En cours","80368","FRIVILLE ESCARBOTIN","SOMME","HAUTS-DE-FRANCE","Polygone",1.5468739,50.085262]
["SSP000386901",null,"SDC",null,"Clôturée",null,null,"Clôturée","95351","LOUVRES","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.4962358,49.05012]
["SSP000387301",null,"Gravure Moderne",null,"Clôturée",null,null,"Clôturée","92063","RUEIL MALMAISON","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.189332,48.883286]
["SSP000387501","93.0073","L'Île-Saint-Denis - Site Charvet et ses abords",null,"En cours",null,null,"En cours","93039","L'ILE SAINT DENIS","SEINE-SAINT-DENIS","ILE-DE-FRANCE","Polygone",2.337959,48.931232,"M5 - Activités administratives, bureau"]
["SSP000388001","83.0035","DANNE - ancien site production",null,"En cours",null,null,"En cours","83009","BANDOL","VAR","PROVENCE-ALPES-COTE D'AZUR","Polygone",5.7645397,43.141697,"M - Divers et services"]
["SSP000388201",null,"Décharge de Gourlaine",null,"Clôturée",null,null,"Clôturée","42086","ECOCHE","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.2963834,46.156017]
["SSP000388601","83.0010","BRENNTAG (ex. ORCHIDIS)",null,"En cours",null,"1998-12-31","En cours","83085","LA MOTTE","VAR","PROVENCE-ALPES-COTE D'AZUR","Polygone",6.507691,43.4837,"L13 - Entrepôts de produits dangereux"]
["SSP000389101","83.0037","FIRMENICH GRASSE SAS",null,"En cours",null,null,"En cours","83124","SEILLANS","VAR","PROVENCE-ALPES-COTE D'AZUR","Polygone",6.639391,43.638805,"D6 - Parfumerie, produits savonniers, détergents"]
["SSP000389501","13.0124","Voisin et Pascal",null,"En cours",null,null,"En cours","13039","FOS SUR MER","BOUCHES-DU-RHONE","PROVENCE-ALPES-COTE D'AZUR","Polygone",4.944459,43.432915,"C2 - Industrie du papier et du carton"]
["SSP000390001","95.0070","AUTOSHOP",null,"En cours",null,null,"En cours","95487","PERSAN","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.2855473,49.15686]
["SSP000390701","13.0005","CRASSIER ALUSUISSE AYGALADES",null,"Clôturée",null,"2012-06-01","Clôturée","13055","MARSEILLE","BOUCHES-DU-RHONE","PROVENCE-ALPES-COTE D'AZUR","Polygone",5.364458,43.34076,"J31 - Fabrication d'alumine"]
["SSP000391001","13.0058","SEVIA (ex: SRRHU - Société de Récupération et Régénération des Huiles Usagées)",null,"En cours",null,null,"En cours","13055","MARSEILLE","BOUCHES-DU-RHONE","PROVENCE-ALPES-COTE D'AZUR","Polygone",5.4107356,43.277363,"K35 - Regroupement, reconditionnement de déchets"]
["SSP000391601",null,"Site Melodie7 (ex Collège St Eugène de Mazenod)",null,"Clôturée",null,null,"Clôturée","13055","MARSEILLE","BOUCHES-DU-RHONE","PROVENCE-ALPES-COTE D'AZUR","Polygone",5.388214,43.28193]
["SSP000391801","79.0022","Agence EDF / GDF Services",null,"Clôturée",null,"2015-03-24","Clôturée","79191","NIORT","DEUX-SEVRES","NOUVELLE-AQUITAINE","Polygone",-0.45359218,46.327007,"D21 - Stockage et conditionnement des gaz et liquéfiés"]
["SSP000392401",null,"Centre EDF  GDF Services",null,"Clôturée",null,null,"Clôturée","17300","LA ROCHELLE","CHARENTE-MARITIME","NOUVELLE-AQUITAINE","Polygone",-1.1486723,46.16613]
["SSP000393001",null,"MAGNETTI MARELLI (EX SOLEX)",null,"Clôturée",null,null,"Clôturée","78335","LIMAY","YVELINES","ILE-DE-FRANCE","Polygone",1.7439282,48.98528]
["SSP000393401","59.0498","Teinturerie de l'Erclin",null,"En cours",null,null,"En cours","59485","QUIEVY","NORD","HAUTS-DE-FRANCE","Polygone",3.4281113,50.160828,"E13 - Blanchiment, teinture, impression"]
["SSP000393901",null,"Ancienne société LA NOUVELLE SALVA",null,"Clôturée",null,null,"Clôturée","67365","OSTWALD","BAS-RHIN","GRAND EST","Polygone",7.7177434,48.551193]
["SSP000394201",null,"FONDERIE RENAULT",null,"Clôturée",null,null,"Clôturée","94033","FONTENAY SOUS BOIS","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.475415,48.847816]
["SSP000394401",null,"Décharge 2 Meistratzheim",null,"Clôturée",null,null,"Clôturée","67286","MEISTRATZHEIM","BAS-RHIN","GRAND EST","Polygone",7.549858,48.448357]
["SSP000394901","59.0497","comafer",null,"En cours",null,null,"En cours","59037","AVESNES LES AUBERT","NORD","HAUTS-DE-FRANCE","Polygone",3.3953488,50.193523,"K52 - Dépôts de ferraille"]
["SSP000395101","64.0100","Décharge de Larceveau",null,"En cours",null,null,"En cours","64314","LARCEVEAU ARROS CIBITS","PYRENEES-ATLANTIQUES","NOUVELLE-AQUITAINE","Polygone",-1.1077114,43.238]
["SSP000395401","64.0112","Décharge de Mongoy",null,"En cours",null,null,"En cours","64156","BUZIET","PYRENEES-ATLANTIQUES","NOUVELLE-AQUITAINE","Polygone",-0.47514477,43.130424]
["SSP000395901",null,"Voies Navigables de France",null,"Clôturée",null,null,"Clôturée","59178","DOUAI","NORD","HAUTS-DE-FRANCE","Polygone",3.0787988,50.38106]
["SSP000396301","33.0214","Ancienne décharge de Guillos",null,"En cours",null,null,"En cours","33197","GUILLOS","GIRONDE","NOUVELLE-AQUITAINE","Polygone",-0.5175702,44.55844,"K21 - Décharges d'ordures ménagères"]
["SSP000396801","33.0197","Décharge les cousteaux",null,"En cours",null,null,"En cours","33514","SOULAC SUR MER","GIRONDE","NOUVELLE-AQUITAINE","Polygone",-1.1095912,45.499325,"K21 - Décharges d'ordures ménagères"]
["SSP000397101","33.0281","Decharge de Queyrac \"Lassus\"",null,"En cours",null,null,"En cours","33348","QUEYRAC","GIRONDE","NOUVELLE-AQUITAINE","Polygone",-0.9827313,45.362385]
["SSP000397301","33.0468","SPARFLEX (ex-QUIBEL  S.A)",null,"En cours",null,null,"En cours","33001","ABZAC","GIRONDE","NOUVELLE-AQUITAINE","Polygone",-0.13713656,45.015965]
["SSP000397601","33.0464","Pollution Radium Bassins à Flots",null,"En cours",null,null,"En cours","33063","BORDEAUX","GIRONDE","NOUVELLE-AQUITAINE","Polygone",-0.5578509,44.861702]
["SSP000398201","33.0299","Ancienne décharge 'Lande de Tourneau'",null,"En cours",null,null,"En cours","33376","SAINT AUBIN DE MEDOC","GIRONDE","NOUVELLE-AQUITAINE","Polygone",-0.72981566,44.937267]
["SSP000398301","33.0292","Decharge 'La Cambette'",null,"En cours",null,null,"En cours","33316","PELLEGRUE","GIRONDE","NOUVELLE-AQUITAINE","Polygone",0.07939231,44.738544]
["SSP000398801","33.0279","Decharge de Grignols",null,"En cours",null,null,"En cours","33271","MARIONS","GIRONDE","NOUVELLE-AQUITAINE","Polygone",-0.08985968,44.345375]
["SSP000399201","33.0346","CET ARVEYRES",null,"En cours",null,null,"En cours","33015","ARVEYRES","GIRONDE","NOUVELLE-AQUITAINE","Polygone",-0.2571898,44.912075]
["SSP000399601",null,"RENAULAC",null,"Clôturée",null,null,"Clôturée","33039","BEGLES","GIRONDE","NOUVELLE-AQUITAINE","Polygone",-0.55668235,44.79947]
["SSP000399701","33.0317","Décharge de Pineuilh",null,"En cours",null,null,"En cours","33324","PINEUILH","GIRONDE","NOUVELLE-AQUITAINE","Polygone",0.24097599,44.85571,"K21 - Décharges d'ordures ménagères"]
["SSP000400201","33.0253","BLANCONNIER",null,"En cours",null,null,"En cours","33281","MERIGNAC","GIRONDE","NOUVELLE-AQUITAINE","Polygone",-0.61915237,44.821953,"K52 - Dépôts de ferraille"]
["SSP000400501","33.0362","Décharge de Lanton",null,"En cours",null,null,"En cours","33229","LANTON","GIRONDE","NOUVELLE-AQUITAINE","Polygone",-1.0060805,44.72721]
["SSP000401201","33.0335","TOTAL - Relais ELF Pont du Pas",null,"En cours",null,null,"En cours","33273","MARTIGNAS SUR JALLE","GIRONDE","NOUVELLE-AQUITAINE","Polygone",-0.7697692,44.84203,"L23 - Détail de carburants"]
["SSP000401301","33.0337","Décharge de Captieux St Blaise ou  Sauvagnon",null,"En cours",null,null,"En cours","33095","CAPTIEUX","GIRONDE","NOUVELLE-AQUITAINE","Polygone",-0.26673138,44.279133]
["SSP000401801","33.0429","Station service LISA MAXIMUM CARBURANT",null,"En cours",null,null,"En cours","33529","LA TESTE DE BUCH","GIRONDE","NOUVELLE-AQUITAINE","Polygone",-1.1355567,44.61625]
["SSP000402201","33.0206","Déposante de Biganos",null,"En cours",null,null,"En cours","33051","BIGANOS","GIRONDE","NOUVELLE-AQUITAINE","Polygone",-0.94839925,44.660122,"K2 - Traitement de déchets urbains"]
["SSP000402601","33.0041","Décharge ABCCD Martignas",null,"En cours",null,null,"En cours","33273","MARTIGNAS SUR JALLE","GIRONDE","NOUVELLE-AQUITAINE","Polygone",-0.7625331,44.855526,"K36 - Mise en décharge"]
["SSP000402701","33.0432","SNECMA",null,"En cours",null,null,"En cours","33281","MERIGNAC","GIRONDE","NOUVELLE-AQUITAINE","Polygone",-0.7236783,44.83387]
["SSP000403201","57.0020","Dépots de résidus d'épuration des gaz à Malancourt-la-Montagne",null,"En cours",null,null,"En cours","57019","AMNEVILLE","MOSELLE","GRAND EST","Polygone",6.061383,49.2221]
["SSP000403601","62.0119","Desseilles Textiles SA",null,"En cours",null,null,"En cours","62193","CALAIS","PAS-DE-CALAIS","HAUTS-DE-FRANCE","Polygone",1.8587335,50.938957,"E1 - Textile et habillement, teinture, impression"]
["SSP000404501","80.0009","Ancien site DEBOUVERIE (TOTAL)",null,"En cours",null,null,"En cours","80021","AMIENS","SOMME","HAUTS-DE-FRANCE","Polygone",2.2820315,49.88004,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000404701",null,"TETE NOIRE",null,"Clôturée",null,null,"Clôturée","33063","BORDEAUX","GIRONDE","NOUVELLE-AQUITAINE","Polygone",-0.56143206,44.848988]
["SSP000405001","59.0557","Engrais Battaille",null,"En cours",null,null,"En cours","59253","FRESNES SUR ESCAUT","NORD","HAUTS-DE-FRANCE","Polygone",3.5688472,50.4256,"L1 - Entreposage, manutention, commerces"]
["SSP000405701",null,"Décharge de Bourg Argental",null,"Clôturée",null,null,"Clôturée","42028","BURDIGNES","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.5842376,45.295074]
["SSP000406101","67.0142","ZH Industrie",null,"En cours",null,null,"En cours","67348","OBERNAI","BAS-RHIN","GRAND EST","Polygone",7.4904184,48.467793,"H - Mécanique, traitements des surfaces"]
["SSP000406201",null,"Décharge de Régny",null,"Clôturée",null,null,"Clôturée","42181","REGNY","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.2177453,46.00452]
["SSP000406801",null,"Ancienne décharge du Poëmen",null,"Clôturée",null,null,"Clôturée","22059","LE FOEIL","COTES-D'ARMOR","BRETAGNE","Polygone",-2.9408855,48.40812]
["SSP000407101",null,"Arc International - site ex MMV",null,"Clôturée",null,null,"Clôturée","62040","ARQUES","PAS-DE-CALAIS","HAUTS-DE-FRANCE","Polygone",2.2976832,50.731415]
["SSP000407601","33.0100","PASTORI",null,"Clôturée",null,"2016-12-09","Clôturée","33104","CASTELNAU DE MEDOC","GIRONDE","NOUVELLE-AQUITAINE","Polygone",-0.7858019,45.02974,"D37 - Phytosanitaires, pesticides (fabrication de)"]
["SSP000407801","33.0285","Ancienne décharge Calens Beautiran",null,"En cours",null,null,"En cours","33037","BEAUTIRAN","GIRONDE","NOUVELLE-AQUITAINE","Polygone",-0.4682446,44.702282]
["SSP000408101","33.0352","MAIRIE - Cantenac",null,"En cours",null,null,"En cours","33268","MARGAUX","GIRONDE","NOUVELLE-AQUITAINE","Polygone",-0.66342527,45.022015]
["SSP000408801","83.0022","Ancienne usine à gaz",null,"En cours",null,null,"En cours","83126","LA SEYNE SUR MER","VAR","PROVENCE-ALPES-COTE D'AZUR","Polygone",5.886951,43.099667,"J1 - Cokéfaction, usines à gaz"]
["SSP000409301",null,"AFOUD ex Aboulghazi",null,"Clôturée",null,null,"Clôturée","84092","LE PONTET","VAUCLUSE","PROVENCE-ALPES-COTE D'AZUR","Polygone",4.860164,43.97528]
["SSP000409401","02.0013","TMPE",null,"En cours",null,null,"En cours","02596","PAVANT","AISNE","HAUTS-DE-FRANCE","Polygone",3.2834017,48.953053,"H1 - Mécanique, électrique, traitement de surface"]
["SSP000409901","06.0005","RECUP'METAUX",null,"Clôturée",null,null,"Clôturée","06149","LA TRINITE","ALPES-MARITIMES","PROVENCE-ALPES-COTE D'AZUR","Polygone",7.316221,43.746944,"K5 - Récupération, dépôts de ferrailles"]
["SSP000410401","13.0156","Ponteau - port de Ponteau",null,"En cours",null,null,"En cours","13056","MARTIGUES","BOUCHES-DU-RHONE","PROVENCE-ALPES-COTE D'AZUR","Polygone",5.0096602,43.37112]
["SSP000411001","33.0300","Décharge VEOLIA \"La Rafette\" St Loubès",null,"En cours",null,null,"En cours","33433","SAINT LOUBES","GIRONDE","NOUVELLE-AQUITAINE","Polygone",-0.45153296,44.927555]
["SSP000411201","33.0419","Décharge de Captieux Maharan",null,"En cours",null,null,"En cours","33095","CAPTIEUX","GIRONDE","NOUVELLE-AQUITAINE","Polygone",-0.27349287,44.307446]
["SSP000411501","42.0014","CRASSIER ASCOMETAL, LE MARAIS",null,"En cours",null,null,"En cours","42218","SAINT ETIENNE","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.398301,45.45794,"J22 - Production d'acier brut, aciéries"]
["SSP000411901","33.0233","Ancienne station service MEYRE",null,"En cours",null,null,"En cours","33333","LE PORGE","GIRONDE","NOUVELLE-AQUITAINE","Polygone",-1.0913727,44.874,"L23 - Détail de carburants"]
["SSP000412501","68.0021","ANC. DECHARGE PCUK",null,"En cours",null,null,"En cours","68374","WINTZENHEIM","HAUT-RHIN","GRAND EST","Polygone",7.3219266,48.07798,"K36 - Mise en décharge"]
["SSP000412601","02.0043","S.A. MATROT à GOUY 02",null,"En cours",null,null,"En cours","02352","GOUY","AISNE","HAUTS-DE-FRANCE","Polygone",3.246758,50.00523,"J53 - Travail des métaux, chaudronnerie, poudres"]
["SSP000413001","02.0058","PECQUET TESSON",null,"En cours",null,null,"En cours","02243","CROUY","AISNE","HAUTS-DE-FRANCE","Polygone",3.3573973,49.40263,"J53 - Travail des métaux, chaudronnerie, poudres"]
["SSP000413601","13.0143","BONNA SABLA",null,"En cours",null,null,"En cours","13055","MARSEILLE","BOUCHES-DU-RHONE","PROVENCE-ALPES-COTE D'AZUR","Polygone",5.497938,43.284378,"G - Industries minérales"]
["SSP000413801","13.0145","Grandes Huilerie Métropolitaine (GHM)",null,"En cours",null,null,"En cours","13055","MARSEILLE","BOUCHES-DU-RHONE","PROVENCE-ALPES-COTE D'AZUR","Polygone",5.4063225,43.278625,"B13 - Huiles et graisses animales ou végétales (industrie de)"]
["SSP000414101","13.0155","CRASSIER MONTGRAND",null,"En cours",null,null,"En cours","13055","MARSEILLE","BOUCHES-DU-RHONE","PROVENCE-ALPES-COTE D'AZUR","Polygone",5.492671,43.28532]
["SSP000414601","13.0157","SARIA Industrie Sud Est",null,"En cours",null,null,"En cours","13055","MARSEILLE","BOUCHES-DU-RHONE","PROVENCE-ALPES-COTE D'AZUR","Polygone",5.302645,43.364082]
["SSP000415001","58.0001","SAS BAYER ( Ex RHONE POULENC AGROCHIMIE)",null,"En cours",null,null,"En cours","58194","NEVERS","NIEVRE","BOURGOGNE-FRANCHE-COMTE","Polygone",3.1804612,46.984093,"D - Chimie, parachimie, pétrole"]
["SSP000415501","89.0032","Compagnie Pétrolière de l'Est",null,"En cours",null,null,"En cours","89257","MIGENNES","YONNE","BOURGOGNE-FRANCHE-COMTE","Polygone",3.540879,47.9711,"L23 - Détail de carburants"]
["SSP000415601","89.0034","BP France- Trottier ESCRIBE. Ancien depôt pétrolier",null,"En cours",null,null,"En cours","89263","MONETEAU","YONNE","BOURGOGNE-FRANCHE-COMTE","Polygone",3.5797322,47.84751,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000416001","60.0128","Yoplait france SAS",null,"En cours",null,null,"En cours","60533","RESSONS SUR MATZ","OISE","HAUTS-DE-FRANCE","Polygone",2.7500434,49.54187]
["SSP000416601","62.0121","LU",null,"En cours",null,null,"En cours","62193","CALAIS","PAS-DE-CALAIS","HAUTS-DE-FRANCE","Polygone",1.8598686,50.952477,"B17 - Autres industries agro-alimentaires"]
["SSP000416801","62.0152","Teinturerie de Coquelles",null,"En cours",null,null,"En cours","62239","COQUELLES","PAS-DE-CALAIS","HAUTS-DE-FRANCE","Polygone",1.8551161,50.92463]
["SSP000417101","67.0068","Ancienne usine à gaz",null,"En cours",null,null,"En cours","67437","SAVERNE","BAS-RHIN","GRAND EST","Polygone",7.369635,48.745903]
["SSP000417601",null,"Résidus de fonderie",null,"Clôturée",null,null,"Clôturée","42295","LES SALLES","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",3.7912402,45.857224]
["SSP000418201",null,"Ancienne usine à gaz",null,"Clôturée",null,null,"Clôturée","67061","BOUXWILLER","BAS-RHIN","GRAND EST","Polygone",7.4738855,48.825058]
["SSP000418601","13.0161","ISDI CRMI de la Bayanne",null,"En cours",null,null,"En cours","13047","ISTRES","BOUCHES-DU-RHONE","PROVENCE-ALPES-COTE D'AZUR","Polygone",4.9567018,43.524364]
["SSP000418901","06.0013","Agence d'EDF / GDF de Cannes la Bocca",null,"En cours",null,null,"En cours","06029","CANNES","ALPES-MARITIMES","PROVENCE-ALPES-COTE D'AZUR","Polygone",6.959376,43.551487,"J1 - Cokéfaction, usines à gaz"]
["SSP000419101","06.0019","ZAC de Cap d'Ail",null,"En cours",null,null,"En cours","06032","CAP D'AIL","ALPES-MARITIMES","PROVENCE-ALPES-COTE D'AZUR","Polygone",7.412364,43.727154,"J1 - Cokéfaction, usines à gaz"]
["SSP000419601","27.0016","DECHARGE DE DECHETS INDUSTRIELS WONDER",null,"En cours",null,null,"En cours","27375","LOUVIERS","EURE","NORMANDIE","Polygone",1.1809744,49.206734,"H16 - Piles électriques et accumulateurs (fabrication de)"]
["SSP000419801","04.0011","ANCIENNE USINE à GAZ",null,"Clôturée",null,"2012-06-24","Clôturée","04070","DIGNE LES BAINS","ALPES-DE-HAUTE-PROVENCE","PROVENCE-ALPES-COTE D'AZUR","Polygone",6.2437353,44.09656,"J1 - Cokéfaction, usines à gaz"]
["SSP000420101",null,"CHARPENTES FRANCAISES EX CALONGE",null,"Clôturée",null,null,"Clôturée","64068","ASSON","PYRENEES-ATLANTIQUES","NOUVELLE-AQUITAINE","Polygone",-0.25833607,43.142494]
["SSP000420601",null,"SN PECI",null,"Clôturée",null,null,"Clôturée","22168","PERROS GUIREC","COTES-D'ARMOR","BRETAGNE","Polygone",-3.471656,48.804436]
["SSP000421101","67.0162","Ancien dépôt CTS de Neudorf",null,"En cours",null,null,"En cours","67482","STRASBOURG","BAS-RHIN","GRAND EST","Point",0.0,0.0,"L2 - Transports, automobile, carburants"]
["SSP000421601","33.0290","Décharge COVED",null,"En cours",null,null,"En cours","33193","GRAYAN ET L'HOPITAL","GIRONDE","NOUVELLE-AQUITAINE","Polygone",-1.1025397,45.422436]
["SSP000422001","87.0039","ANCIENNE STATION SERVICE RELAIS TOTAL",null,"En cours",null,null,"En cours","87154","SAINT JUNIEN","HAUTE-VIENNE","NOUVELLE-AQUITAINE","Polygone",0.91290075,45.895275,"L23 - Détail de carburants"]
["SSP000422201","62.0192","DMS (ex DCA)",null,"En cours",null,null,"En cours","62093","BEAULENCOURT","PAS-DE-CALAIS","HAUTS-DE-FRANCE","Polygone",2.8788779,50.07991,"L23 - Détail de carburants"]
["SSP000422701","62.0022","BP - GERLAND",null,"En cours",null,null,"En cours","62280","DURY","PAS-DE-CALAIS","HAUTS-DE-FRANCE","Polygone",2.996676,50.25349,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000423001","62.0024","DECHARGE S.A.N.E.T.",null,"En cours",null,null,"En cours","62864","VIS EN ARTOIS","PAS-DE-CALAIS","HAUTS-DE-FRANCE","Polygone",2.9464593,50.227024,"K3 - Traitement de déchets industriels"]
["SSP000423301",null,"SOFOMA",null,"Clôturée",null,null,"Clôturée","02691","SAINT QUENTIN","AISNE","HAUTS-DE-FRANCE","Polygone",3.3059533,49.841316]
["SSP000423801","67.0256","ERGE 2000",null,"En cours",null,null,"En cours","67216","HUTTENHEIM","BAS-RHIN","GRAND EST","Polygone",7.587471,48.359062]
["SSP000424201","60.0052","Société ST MEDARD ETERNUM ( anciennement société MARBA)",null,"En cours",null,null,"En cours","60088","BORNEL","OISE","HAUTS-DE-FRANCE","Polygone",2.1799557,49.191486,"H13 - Traitement de surface"]
["SSP000424701",null,"RECKHOLDERBERG",null,"Clôturée",null,null,"Clôturée","68056","BRUNSTATT","HAUT-RHIN","GRAND EST","Polygone",7.3293858,47.714985]
["SSP000425001",null,"Ancienne décharge de Kerandiot",null,"Clôturée",null,null,"Clôturée","56029","CALAN","MORBIHAN","BRETAGNE","Polygone",-3.302607,47.885246]
["SSP000425201","62.0181","Ancienne décharge de la Géôle",null,"En cours",null,null,"En cours","62753","SAINT LAURENT BLANGY","PAS-DE-CALAIS","HAUTS-DE-FRANCE","Polygone",2.7877219,50.29747,"K21 - Décharges d'ordures ménagères"]
["SSP000425501",null,"Ancienne décharge de Barge",null,"Clôturée",null,null,"Clôturée","56155","PENESTIN","MORBIHAN","BRETAGNE","Polygone",-2.4348345,47.47405]
["SSP000426201",null,"Ancienne décharge du Cormier",null,"Clôturée",null,null,"Clôturée","56154","PEILLAC","MORBIHAN","BRETAGNE","Polygone",-2.2310321,47.718082]
["SSP000426301",null,"Ancienne décharge de la Dutière",null,"Clôturée",null,null,"Clôturée","56154","PEILLAC","MORBIHAN","BRETAGNE","Polygone",-2.2192054,47.707047]
["SSP000427001","62.0099","CENTRE EDF / GDF",null,"En cours",null,null,"En cours","62041","ARRAS","PAS-DE-CALAIS","HAUTS-DE-FRANCE","Polygone",2.7781196,50.29679,"J1 - Cokéfaction, usines à gaz"]
["SSP000427401",null,"Ancienne décharge de La Colline",null,"Clôturée",null,null,"Clôturée","56220","SAINTE HELENE","MORBIHAN","BRETAGNE","Polygone",-3.1995306,47.713238]
["SSP000428001","71.0032","Ancienne Tuilerie de la Loire",null,"Clôturée",null,"2011-11-28","Clôturée","71012","ARTAIX","SAONE-ET-LOIRE","BOURGOGNE-FRANCHE-COMTE","Polygone",3.976611,46.269867,"D71 - Industrie du caoutchouc"]
["SSP000428301","64.0015","Ancienne usine à gaz - Centre EDF / GDF Services d'Anglet Blancpignon",null,"Clôturée",null,"2006-12-20","Clôturée","64024","ANGLET","PYRENEES-ATLANTIQUES","NOUVELLE-AQUITAINE","Polygone",-1.497706,43.521336,"J1 - Cokéfaction, usines à gaz"]
["SSP000428501",null,"AREVA Miramas zone Est",null,"Clôturée",null,null,"Clôturée","13063","MIRAMAS","BOUCHES-DU-RHONE","PROVENCE-ALPES-COTE D'AZUR","Polygone",4.9957776,43.5791]
["SSP000428801","83.0043","SIVED NG",null,"En cours",null,null,"En cours","83037","LA CELLE","VAR","PROVENCE-ALPES-COTE D'AZUR","Polygone",6.0069,43.398792]
["SSP000429301","06.0024","Station Service Corniglion Molinier",null,"En cours",null,null,"En cours","06088","NICE","ALPES-MARITIMES","PROVENCE-ALPES-COTE D'AZUR","Polygone",7.228966,43.67615,"L23 - Détail de carburants"]
["SSP000429401","06.0028","Travaux miniers Cimes de Raus",null,"En cours",null,null,"En cours","06132","SAORGE","ALPES-MARITIMES","PROVENCE-ALPES-COTE D'AZUR","Polygone",7.4280033,44.02919]
["SSP000429901","56.0027","Ancienne station service LE DOUARIN",null,"En cours",null,null,"En cours","56010","BAUD","MORBIHAN","BRETAGNE","Polygone",-3.017132,47.87591,"L23 - Détail de carburants"]
["SSP000430301",null,"Ancienne décharge de la Grande Borne",null,"Clôturée",null,null,"Clôturée","56172","PLUMELEC","MORBIHAN","BRETAGNE","Polygone",-2.6561966,47.838276]
["SSP000430701","64.0030","SCB",null,"En cours",null,null,"En cours","64407","MOUGUERRE","PYRENEES-ATLANTIQUES","NOUVELLE-AQUITAINE","Polygone",-1.4370859,43.486057]
["SSP000431001",null,"Ancienne décharge de la Corday",null,"Clôturée",null,null,"Clôturée","56174","PLUMELIN","MORBIHAN","BRETAGNE","Polygone",-2.8824682,47.858494]
["SSP000431501","33.0306","NAVARRA",null,"En cours",null,null,"En cours","33555","MARCHEPRIME","GIRONDE","NOUVELLE-AQUITAINE","Polygone",-0.84892327,44.6884]
["SSP000431801","59.0581","SAMBRE ENROBES",null,"En cours",null,null,"En cours","59291","HAUTMONT","NORD","HAUTS-DE-FRANCE","Polygone",3.9527228,50.241604,"G22 - Centrales d'enrobés"]
["SSP000432601",null,"Décharge de St-Galmier",null,"Clôturée",null,null,"Clôturée","42222","SAINT GALMIER","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.338447,45.59468]
["SSP000432801",null,"Ancienne décharge de la Justice",null,"Clôturée",null,null,"Clôturée","56064","GLENAC","MORBIHAN","BRETAGNE","Polygone",-2.137172,47.7332]
["SSP000433101","62.0148","TEREOS Sucrerie de Lillers",null,"En cours",null,null,"En cours","62516","LILLERS","PAS-DE-CALAIS","HAUTS-DE-FRANCE","Polygone",2.5093265,50.563065]
["SSP000433801","94.0037","USINE A GAZ",null,"En cours",null,null,"En cours","94071","SUCY EN BRIE","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.505771,48.77295,"J1 - Cokéfaction, usines à gaz"]
["SSP000434301","33.0093","Ancienne usine à gaz - Agence d'Exploitation de Ste Foy La Grande",null,"Clôturée",null,"2006-12-11","Clôturée","33324","PINEUILH","GIRONDE","NOUVELLE-AQUITAINE","Polygone",0.2108642,44.838654,"J1 - Cokéfaction, usines à gaz"]
["SSP000434401","33.0094","Ancienne usine à gaz - Agence EDF GDF Services du Bassin d'Arcachon",null,"Clôturée",null,"2006-06-15","Clôturée","33009","ARCACHON","GIRONDE","NOUVELLE-AQUITAINE","Polygone",-1.1637925,44.657272,"J1 - Cokéfaction, usines à gaz"]
["SSP000434901","47.0020","Ancienne usine à gaz - Agence d'exploitation d'EDF / GDF",null,"En cours",null,null,"En cours","47195","NERAC","LOT-ET-GARONNE","NOUVELLE-AQUITAINE","Polygone",0.33910903,44.13913,"J1 - Cokéfaction, usines à gaz"]
["SSP000435201",null,"STARLETTE",null,"Clôturée",null,null,"Clôturée","67482","STRASBOURG","BAS-RHIN","GRAND EST","Polygone",7.7837286,48.574265]
["SSP000436101",null,"Ancienne décharge de PARC ER HOET",null,"Clôturée",null,null,"Clôturée","56013","BELZ","MORBIHAN","BRETAGNE","Polygone",-3.1858392,47.661648]
["SSP000436301","56.0019","Centre de stockage de matériaux inertes d'Auray-Belz-Quiberon",null,"En cours",null,null,"En cours","56046","CRACH","MORBIHAN","BRETAGNE","Polygone",-2.9883735,47.650707,"K36 - Mise en décharge"]
["SSP000436701",null,"Ancienne décharge du Bego",null,"Clôturée",null,null,"Clôturée","56168","PLOUHARNEL","MORBIHAN","BRETAGNE","Polygone",-3.1369092,47.595013]
["SSP000438101",null,"Ecole maternelle publique Aulezy",null,"Clôturée",null,null,"Clôturée","83061","FREJUS","VAR","PROVENCE-ALPES-COTE D'AZUR","Polygone",6.7353,43.43422]
["SSP000440001","67.0023","Ancienne usine à gaz",null,"En cours",null,null,"En cours","67482","STRASBOURG","BAS-RHIN","GRAND EST","Polygone",7.771267,48.572525,"J1 - Cokéfaction, usines à gaz"]
["SSP000440101","67.0216","Ancienne décharge interne PRR",null,"En cours",null,null,"En cours","67389","REICHSTETT","BAS-RHIN","GRAND EST","Polygone",7.779949,48.650127]
["SSP000440601",null,"Crèche du Conseil Général du Vaucluse et EEAP Le Petit Jardin",null,"Clôturée",null,null,"Clôturée","84007","AVIGNON","VAUCLUSE","PROVENCE-ALPES-COTE D'AZUR","Polygone",4.816928,43.94497]
["SSP000441101",null,"Groupe scolaire Frédéric Mistral",null,"Clôturée",null,null,"Clôturée","84007","AVIGNON","VAUCLUSE","PROVENCE-ALPES-COTE D'AZUR","Polygone",4.8006897,43.94587]
["SSP000441601","25.0006","DORCY",null,"En cours",null,null,"En cours","25539","SELONCOURT","DOUBS","BOURGOGNE-FRANCHE-COMTE","Polygone",6.8669953,47.4595,"H13 - Traitement de surface"]
["SSP000441901","90.0006","BOLLORE ENERGIE",null,"En cours",null,null,"En cours","90010","BELFORT","TERRITOIRE DE BELFORT","BOURGOGNE-FRANCHE-COMTE","Polygone",6.853212,47.623272,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000442201","90.0027","MACPLUS ex. RUST",null,"En cours",null,null,"En cours","90075","OFFEMONT","TERRITOIRE DE BELFORT","BOURGOGNE-FRANCHE-COMTE","Polygone",6.8688293,47.66071,"H - Mécanique, traitements des surfaces"]
["SSP000442701",null,"Ancienne décharge de Kéréou",null,"Clôturée",null,null,"Clôturée","29262","SAINT SAUVEUR","FINISTERE","BRETAGNE","Polygone",-3.9824605,48.468296]
["SSP000443101","54.0083","ANCIENNE USINE A GAZ NANCY DE FOUCAULD","Protocole gaz de France","Clôturée",null,"2010-02-11","Clôturée","54395","NANCY","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",6.1832466,48.70192,"J1 - Cokéfaction, usines à gaz"]
["SSP000443201",null,"Atelier Bus",null,"Clôturée",null,null,"Clôturée","76259","FECAMP","SEINE-MARITIME","NORMANDIE","Polygone",0.38654235,49.757156]
["SSP000443601",null,"Ancienne décharge de la Billiais",null,"Clôturée",null,null,"Clôturée","35184","MONTAUBAN DE BRETAGNE","ILLE-ET-VILAINE","BRETAGNE","Polygone",-2.0840669,48.204765]
["SSP000444101","59.0096","ANCIENNE DECHARGE SNCF",null,"En cours",null,null,"En cours","59606","VALENCIENNES","NORD","HAUTS-DE-FRANCE","Polygone",3.5352552,50.37652,"K - Déchets et traitements"]
["SSP000445101","67.0049","ALBUS (anc. USINE KÖMMERLING)",null,"En cours",null,null,"En cours","67222","INGWILLER","BAS-RHIN","GRAND EST","Polygone",7.4842916,48.86399,"D44 - Fabrication de colles et mastics"]
["SSP000445301","76.0137","GALVANISATION FÉCAMPOISE",null,"En cours",null,null,"En cours","76259","FECAMP","SEINE-MARITIME","NORMANDIE","Polygone",0.38402835,49.759068,"H13 - Traitement de surface"]
["SSP000445601","59.0097","CHANTIER CFF",null,"En cours",null,null,"En cours","59092","BOUCHAIN","NORD","HAUTS-DE-FRANCE","Polygone",3.3476584,50.3022,"K5 - Récupération, dépôts de ferrailles"]
["SSP000446401","67.0025","ANC. MAAS",null,"En cours",null,null,"En cours","67222","INGWILLER","BAS-RHIN","GRAND EST","Polygone",7.4688897,48.863403]
["SSP000446801",null,"Garage du Calvaire (ex Ets Fradin)",null,"Clôturée",null,null,"Clôturée","60509","PONT SAINTE MAXENCE","OISE","HAUTS-DE-FRANCE","Polygone",2.6037912,49.29866]
["SSP000446901",null,"TOTAL Relais de la Scarpe",null,"Clôturée",null,null,"Clôturée","59178","DOUAI","NORD","HAUTS-DE-FRANCE","Polygone",3.063864,50.369232]
["SSP000447401",null,"Cité Brunet",null,"Clôturée",null,null,"Clôturée","42276","SAINT PRIEST LA PRUGNE","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",3.7528996,45.95779]
["SSP000447901","42.0199","SECMI-CHEUCLE",null,"En cours",null,null,"En cours","42218","SAINT ETIENNE","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.3975787,45.441612,"H14 - Application de peinture"]
["SSP000448301","67.0087","SICFO STANLEY",null,"En cours",null,null,"En cours","67302","MONSWILLER","BAS-RHIN","GRAND EST","Polygone",7.3803444,48.749493]
["SSP000448501",null,"Ancienne station-service ARAL",null,"Clôturée",null,null,"Clôturée","67482","STRASBOURG","BAS-RHIN","GRAND EST","Polygone",7.7744384,48.612545]
["SSP000449001","76.0212","EGNO CHIMIE",null,"En cours",null,null,"En cours","76684","TANCARVILLE","SEINE-MARITIME","NORMANDIE","Polygone",0.4673864,49.477898]
["SSP000449501","62.0193","DMS (ex Hantute - Toulemonde)",null,"En cours",null,null,"En cours","62473","ISBERGUES","PAS-DE-CALAIS","HAUTS-DE-FRANCE","Polygone",2.445701,50.632637,"L13 - Entrepôts de produits dangereux"]
["SSP000450101","59.0407","BP FRANCE (Station service)",null,"En cours",null,null,"En cours","59178","DOUAI","NORD","HAUTS-DE-FRANCE","Polygone",3.0825481,50.363785,"L23 - Détail de carburants"]
["SSP000450301",null,"Forage fuyard 3349 (Pechelbronn)",null,"Clôturée",null,null,"Clôturée","67359","OHLUNGEN","BAS-RHIN","GRAND EST","Polygone",7.7096987,48.81096]
["SSP000450701",null,"Forage fuyard 3969 (Pechelbronn)",null,"Clôturée",null,null,"Clôturée","67254","KUTZENHAUSEN","BAS-RHIN","GRAND EST","Polygone",7.8596926,48.934692]
["SSP000451201",null,"Forage fuyard 1050 (Pechelbronn)",null,"Clôturée",null,null,"Clôturée","67290","MERKWILLER PECHELBRONN","BAS-RHIN","GRAND EST","Polygone",7.834991,48.937103]
["SSP000451501",null,"Forage fuyard 459 (Pechelbronn)",null,"Clôturée",null,null,"Clôturée","67290","MERKWILLER PECHELBRONN","BAS-RHIN","GRAND EST","Polygone",7.835866,48.938133]
["SSP000451801","62.0005","FRICHE DU CARBURE (ATOFINA)",null,"En cours",null,null,"En cours","62895","WINGLES","PAS-DE-CALAIS","HAUTS-DE-FRANCE","Polygone",2.861374,50.48806,"D32 - Chimie minérale inorganique autre"]
["SSP000452401","62.0158","Courtaulds - Usine de production",null,"En cours",null,null,"En cours","62239","COQUELLES","PAS-DE-CALAIS","HAUTS-DE-FRANCE","Polygone",1.8495517,50.92907,"M1 - Industries diverses"]
["SSP000452901","68.0112","Site SACM-- secteur B (La Cathédrale et son parvis)",null,"En cours",null,null,"En cours","68224","MULHOUSE","HAUT-RHIN","GRAND EST","Polygone",7.3320646,47.738934]
["SSP000453301","27.0025","PROSYNTHO - STPC VITER",null,"En cours",null,null,"En cours","27003","ACQUIGNY","EURE","NORMANDIE","Polygone",1.1856083,49.16276,"D37 - Phytosanitaires, pesticides (fabrication de)"]
["SSP000453401","27.0071","POLMARG",null,"En cours",null,null,"En cours","27375","LOUVIERS","EURE","NORMANDIE","Polygone",1.1582619,49.213856]
["SSP000453801",null,"Décharge rue des vallots",null,"Clôturée",null,null,"Clôturée","27375","LOUVIERS","EURE","NORMANDIE","Polygone",1.1493081,49.20274]
["SSP000454301","25.0027","SOCIETE NOUVELLE L'EPEE",null,"Clôturée",null,"2012-09-03","Clôturée","25526","SAINTE SUZANNE","DOUBS","BOURGOGNE-FRANCHE-COMTE","Polygone",6.7720847,47.50226,"H - Mécanique, traitements des surfaces"]
["SSP000454701",null,"Chemin des Gadaillères",null,"Clôturée",null,null,"Clôturée","42276","SAINT PRIEST LA PRUGNE","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",3.781428,45.927345]
["SSP000454901",null,"Les Allognières",null,"Clôturée",null,null,"Clôturée","42314","LA TUILIERE","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",3.784901,45.964172]
["SSP000455401",null,"DME ALMY",null,"Clôturée",null,null,"Clôturée","62498","LENS","PAS-DE-CALAIS","HAUTS-DE-FRANCE","Polygone",2.8204987,50.448143]
["SSP000455801","62.0144","Laboratoire Mont Saint Eloi",null,"En cours",null,null,"En cours","62065","AVION","PAS-DE-CALAIS","HAUTS-DE-FRANCE","Polygone",2.8259912,50.39457,"D62 - Fabrication de détergents"]
["SSP000456301","67.0109","Terril De Chambrier",null,"En cours",null,null,"En cours","67254","KUTZENHAUSEN","BAS-RHIN","GRAND EST","Polygone",7.839105,48.95025]
["SSP000456401","67.0108","Terril Le Bel",null,"En cours",null,null,"En cours","67379","PREUSCHDORF","BAS-RHIN","GRAND EST","Polygone",7.814956,48.93169]
["SSP000456901","62.0190","SOTRENOR",null,"En cours",null,null,"En cours","62250","COURRIERES","PAS-DE-CALAIS","HAUTS-DE-FRANCE","Polygone",2.927901,50.451862,"K31 - Incinération"]
["SSP000457401","27.0107","Ralston Energy Systems",null,"En cours",null,null,"En cours","27681","VERNON","EURE","NORMANDIE","Polygone",1.4709029,49.09441,"J5 - Fonderie et travail des métaux"]
["SSP000457801","67.0146","TOTAL Relais du Frankenbourg",null,"En cours",null,null,"En cours","67462","SELESTAT","BAS-RHIN","GRAND EST","Polygone",7.448754,48.262897,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000458201",null,"Quartier Rendu",null,"Clôturée",null,null,"Clôturée","13209","MARSEILLE 9E ARRONDISSEMENT","BOUCHES-DU-RHONE","PROVENCE-ALPES-COTE D'AZUR","Polygone",5.4023004,43.27627]
["SSP000459201",null,"Friche LEBORNE",null,"Clôturée",null,null,"Clôturée","60063","BERNEUIL EN BRAY","OISE","HAUTS-DE-FRANCE","Polygone",2.0423799,49.356453]
["SSP000459501",null,"Ancienne décharge Plessis Macé",null,"Clôturée",null,null,"Clôturée","49242","LE PLESSIS MACE","MAINE-ET-LOIRE","PAYS DE LA LOIRE","Polygone",-0.6606332,47.54876]
["SSP000460001","76.0019","Agence EDF GDF Services de Grand Quevilly",null,"En cours",null,null,"En cours","76322","LE GRAND QUEVILLY","SEINE-MARITIME","NORMANDIE","Polygone",1.0223092,49.40765,"J1 - Cokéfaction, usines à gaz"]
["SSP000460101","76.0020","SITE MALETRA, SNPC, ORDURES SERVICES",null,"En cours",null,null,"En cours","76322","LE GRAND QUEVILLY","SEINE-MARITIME","NORMANDIE","Polygone",1.0412776,49.412746,"K21 - Décharges d'ordures ménagères"]
["SSP000460501","76.0024","ANCIENNE MARE",null,"En cours",null,null,"En cours","76498","LE PETIT QUEVILLY","SEINE-MARITIME","NORMANDIE","Polygone",1.0504371,49.43049,"K36 - Mise en décharge"]
["SSP000460901","76.0103","Usine à gaz d'Elbeuf Normande",null,"En cours",null,null,"En cours","76231","ELBEUF","SEINE-MARITIME","NORMANDIE","Polygone",1.0099143,49.28357]
["SSP000461401","76.0156","ORTEC Environnement",null,"En cours",null,null,"En cours","76498","LE PETIT QUEVILLY","SEINE-MARITIME","NORMANDIE","Polygone",1.0680919,49.433716]
["SSP000461501","76.0169","HB FULLER",null,"En cours",null,null,"En cours","76709","LE TRAIT","SEINE-MARITIME","NORMANDIE","Polygone",0.7940384,49.48416,"D4 - Encres, vernis, peintures, colles (fabrication de)"]
["SSP000462101","76.0309","COMMENTRY",null,"En cours",null,null,"En cours","76484","OISSEL","SEINE-MARITIME","NORMANDIE","Polygone",1.1014924,49.35261]
["SSP000462401","76.0282","SNAM - berges de l'Oison en aval du site",null,"En cours",null,null,"En cours","76640","SAINT PIERRE LES ELBEUF","SEINE-MARITIME","NORMANDIE","Polygone",1.0454748,49.27402]
["SSP000462601","76.0330","Ensemble immobilier LAFAYETTE - ROUEN - (ex SARL IMMODEL/AD ROUEN/SAAS et LEMERC",null,"En cours",null,null,"En cours","76540","ROUEN","SEINE-MARITIME","NORMANDIE","Polygone",1.0877666,49.431843]
["SSP000462901","76.0017","CARRIERE LIERA",null,"En cours",null,null,"En cours","76759","YVILLE SUR SEINE","SEINE-MARITIME","NORMANDIE","Polygone",0.89544183,49.423065,"K52 - Dépôts de ferraille"]
["SSP000463401","76.0080","SODIDRO",null,"En cours",null,null,"En cours","76231","ELBEUF","SEINE-MARITIME","NORMANDIE","Polygone",1.0047643,49.2849,"D62 - Fabrication de détergents"]
["SSP000463801","76.0140","CANTREL",null,"En cours",null,null,"En cours","76640","SAINT PIERRE LES ELBEUF","SEINE-MARITIME","NORMANDIE","Polygone",1.0509505,49.276245,"K52 - Dépôts de ferraille"]
["SSP000464301","76.0179","BITUMASTIC",null,"En cours",null,null,"En cours","76498","LE PETIT QUEVILLY","SEINE-MARITIME","NORMANDIE","Polygone",1.0509479,49.424732,"D4 - Encres, vernis, peintures, colles (fabrication de)"]
["SSP000464401","76.0191","SEPROM",null,"En cours",null,null,"En cours","76222","DUCLAIR","SEINE-MARITIME","NORMANDIE","Polygone",0.8700758,49.479782]
["SSP000465001","76.0262","ROBERT BLONDEL PRODUCTION",null,"En cours",null,null,"En cours","76599","SAINT LEGER DU BOURG DENIS","SEINE-MARITIME","NORMANDIE","Polygone",1.150832,49.435913,"E1 - Textile et habillement, teinture, impression"]
["SSP000465301",null,"Sources Maraini",null,"Clôturée",null,null,"Clôturée","06091","PEILLE","ALPES-MARITIMES","PROVENCE-ALPES-COTE D'AZUR","Polygone",7.409135,43.76952]
["SSP000465501","39.0010","S.A.R.L BOUVET BOIS",null,"En cours",null,null,"En cours","39101","CHAMPVANS","JURA","BOURGOGNE-FRANCHE-COMTE","Polygone",5.4446883,47.110023,"C13 - Traitement du bois"]
["SSP000465901","78.0047","Ancienne usine à gaz de Chevreuse",null,"En cours",null,null,"En cours","78160","CHEVREUSE","YVELINES","ILE-DE-FRANCE","Polygone",2.0460181,48.706264,"J1 - Cokéfaction, usines à gaz"]
["SSP000466401",null,"THALES OPTRONIQUE",null,"Clôturée",null,null,"Clôturée","78297","GUYANCOURT","YVELINES","ILE-DE-FRANCE","Polygone",2.0695367,48.758953]
["SSP000466801",null,"ZAE route de DUCLAIRE",null,"Clôturée",null,null,"Clôturée","76636","SAINT PIERRE DE VARENGEVILLE","SEINE-MARITIME","NORMANDIE","Polygone",0.9242612,49.49666]
["SSP000467301",null,"dépôt de voirie de la rue du docteur cauchois",null,"Clôturée",null,null,"Clôturée","76540","ROUEN","SEINE-MARITIME","NORMANDIE","Polygone",1.125202,49.449146]
["SSP000467601",null,"Ancien site SCHENKER",null,"Clôturée",null,null,"Clôturée","76540","ROUEN","SEINE-MARITIME","NORMANDIE","Polygone",1.0686046,49.43878]
["SSP000467801",null,"ancien site \"WEBERT et RICOEUR\"",null,"Clôturée",null,null,"Clôturée","76540","ROUEN","SEINE-MARITIME","NORMANDIE","Polygone",1.0958778,49.426598]
["SSP000468301",null,"subsistances militaire de Grand Quevilly",null,"Clôturée",null,null,"Clôturée","76322","LE GRAND QUEVILLY","SEINE-MARITIME","NORMANDIE","Polygone",1.0447501,49.420704]
["SSP000468501",null,"lot A2 et A3 place des chartreux",null,"Clôturée",null,null,"Clôturée","76498","LE PETIT QUEVILLY","SEINE-MARITIME","NORMANDIE","Polygone",1.0665135,49.423626]
["SSP000468801",null,"Prequ'ile Waddington",null,"Clôturée",null,null,"Clôturée","76540","ROUEN","SEINE-MARITIME","NORMANDIE","Polygone",1.0568548,49.444683]
["SSP000469401","49.0062","CHOLET BUS (ex Transports Publics du Choletais)",null,"En cours",null,null,"En cours","49099","CHOLET","MAINE-ET-LOIRE","PAYS DE LA LOIRE","Polygone",-0.8622437,47.072514]
["SSP000469801","68.0031","ANC. USINE A GAZ",null,"En cours",null,null,"En cours","68269","RIBEAUVILLE","HAUT-RHIN","GRAND EST","Polygone",7.3279324,48.192738,"J1 - Cokéfaction, usines à gaz"]
["SSP000470401","13.0164","Ancienne décharge - lotissement \"les mouettes\"",null,"En cours",null,null,"En cours","13004","ARLES","BOUCHES-DU-RHONE","PROVENCE-ALPES-COTE D'AZUR","Polygone",4.734218,43.40961]
["SSP000470801",null,"Ancienne décharge du Jeannay",null,"Clôturée",null,null,"Clôturée","22240","PLUMAUGAT","COTES-D'ARMOR","BRETAGNE","Polygone",-2.2281969,48.238705]
["SSP000471301",null,"Ancienne décharge du Tertre Renard",null,"Clôturée",null,null,"Clôturée","22280","SAINT CARNE","COTES-D'ARMOR","BRETAGNE","Polygone",-2.059556,48.41118]
["SSP000471901",null,"Ancienne décharge des Cloissiaux",null,"Clôturée",null,null,"Clôturée","22302","SAINT JACUT DE LA MER","COTES-D'ARMOR","BRETAGNE","Polygone",-2.18694,48.581112]
["SSP000472101",null,"Ancienne décharge du Feil",null,"Clôturée",null,null,"Clôturée","22306","SAINT JUDOCE","COTES-D'ARMOR","BRETAGNE","Polygone",-1.960506,48.375095]
["SSP000472601",null,"Ancienne décharge du Petit Clos",null,"Clôturée",null,null,"Clôturée","35050","CARDROC","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.898644,48.284492]
["SSP000473501",null,"Ancienne décharge des Fosses",null,"Clôturée",null,null,"Clôturée","22317","SAINT MELOIR DES BOIS","COTES-D'ARMOR","BRETAGNE","Polygone",-2.2640514,48.455498]
["SSP000474001","85.0031","MAIRIE Nesmy (ex froger)",null,"En cours",null,null,"En cours","85160","NESMY","VENDEE","PAYS DE LA LOIRE","Polygone",-1.380644,46.573437,"K21 - Décharges d'ordures ménagères"]
["SSP000474501",null,"Groupe scolaire Saint Joseph",null,"Clôturée",null,null,"Clôturée","13001","AIX EN PROVENCE","BOUCHES-DU-RHONE","PROVENCE-ALPES-COTE D'AZUR","Polygone",5.4535604,43.53099]
["SSP000474801",null,"Collège public « Ampère »",null,"Clôturée",null,null,"Clôturée","13004","ARLES","BOUCHES-DU-RHONE","PROVENCE-ALPES-COTE D'AZUR","Polygone",4.626582,43.673473]
["SSP000475001",null,"Ancienne décharge du Châtelier",null,"Clôturée",null,null,"Clôturée","22327","SAINT SAMSON SUR RANCE","COTES-D'ARMOR","BRETAGNE","Polygone",-2.0029707,48.49223]
["SSP000475701",null,"Ancienne décharge de Lan Charnel",null,"Clôturée",null,null,"Clôturée","22320","SAINT NICODEME","COTES-D'ARMOR","BRETAGNE","Polygone",-3.3399947,48.34624]
["SSP000476101",null,"Lycee public Frederic Joliot-Curie",null,"Clôturée",null,null,"Clôturée","13005","AUBAGNE","BOUCHES-DU-RHONE","PROVENCE-ALPES-COTE D'AZUR","Polygone",5.561271,43.29299]
["SSP000476201",null,"Groupe scolaire Parc Bellevue",null,"Clôturée",null,null,"Clôturée","13203","MARSEILLE 3E ARRONDISSEMENT","BOUCHES-DU-RHONE","PROVENCE-ALPES-COTE D'AZUR","Polygone",5.3736506,43.31757]
["SSP000476701",null,"Groupe scolaire Valmante",null,"Clôturée",null,null,"Clôturée","13209","MARSEILLE 9E ARRONDISSEMENT","BOUCHES-DU-RHONE","PROVENCE-ALPES-COTE D'AZUR","Polygone",5.4211435,43.24812]
["SSP000477101",null,"Ecole primaire Révolution",null,"Clôturée",null,null,"Clôturée","13203","MARSEILLE 3E ARRONDISSEMENT","BOUCHES-DU-RHONE","PROVENCE-ALPES-COTE D'AZUR","Polygone",5.379989,43.31585]
["SSP000477601",null,"Groupe scolaire privés Belsunce",null,"Clôturée",null,null,"Clôturée","13202","MARSEILLE 2E ARRONDISSEMENT","BOUCHES-DU-RHONE","PROVENCE-ALPES-COTE D'AZUR","Polygone",5.3720455,43.304302]
["SSP000477901",null,"Collège public Chape",null,"Clôturée",null,null,"Clôturée","13204","MARSEILLE 4E ARRONDISSEMENT","BOUCHES-DU-RHONE","PROVENCE-ALPES-COTE D'AZUR","Polygone",5.389771,43.299652]
["SSP000478101","72.0059","CLEMABA",null,"En cours",null,null,"En cours","72023","BALLON","SARTHE","PAYS DE LA LOIRE","Polygone",0.23763414,48.175472,"L2 - Transports, automobile, carburants"]
["SSP000478401","68.0027","ANC. USINE FROSSARD",null,"En cours",null,null,"En cours","68149","HUNINGUE","HAUT-RHIN","GRAND EST","Polygone",7.579153,47.593037,"D1 - Industrie pétrolière, gaz naturel"]
["SSP000479001",null,"Collège Public Henri Wallon",null,"Clôturée",null,null,"Clôturée","13214","MARSEILLE 14E ARRONDISSEMENT","BOUCHES-DU-RHONE","PROVENCE-ALPES-COTE D'AZUR","Polygone",5.3871126,43.319176]
["SSP000479101",null,"Collège Public R. Rolland et Collège et SEGPA V.SCOTTO",null,"Clôturée",null,null,"Clôturée","13210","MARSEILLE 10E ARRONDISSEMENT","BOUCHES-DU-RHONE","PROVENCE-ALPES-COTE D'AZUR","Polygone",5.4097686,43.276318]
["SSP000479601",null,"Groupe scolaire Ruffi",null,"Clôturée",null,null,"Clôturée","13203","MARSEILLE 3E ARRONDISSEMENT","BOUCHES-DU-RHONE","PROVENCE-ALPES-COTE D'AZUR","Polygone",5.3704534,43.313904]
["SSP000480001",null,"Crèche Petit Jardin des Aigues Douces",null,"Clôturée",null,null,"Clôturée","13077","PORT DE BOUC","BOUCHES-DU-RHONE","PROVENCE-ALPES-COTE D'AZUR","Polygone",4.979249,43.403522]
["SSP000480301",null,"Ecole élémentaire Guynemer",null,"Clôturée",null,null,"Clôturée","06004","ANTIBES","ALPES-MARITIMES","PROVENCE-ALPES-COTE D'AZUR","Polygone",7.122493,43.580875]
["SSP000480501",null,"Ecole élémentaire publique « Hélène Vagliano »/ Ecole maternelle publique « Ange-Marie Miniconi »",null,"Clôturée",null,null,"Clôturée","06029","CANNES","ALPES-MARITIMES","PROVENCE-ALPES-COTE D'AZUR","Polygone",7.026961,43.55471]
["SSP000481001",null,"Groupe Scolaire Fuon Cauda",null,"Clôturée",null,null,"Clôturée","06088","NICE","ALPES-MARITIMES","PROVENCE-ALPES-COTE D'AZUR","Polygone",7.2647853,43.712555]
["SSP000481301",null,"Collège « Jules Romains »",null,"Clôturée",null,null,"Clôturée","06088","NICE","ALPES-MARITIMES","PROVENCE-ALPES-COTE D'AZUR","Polygone",7.202352,43.67796]
["SSP000481901",null,"Ecole primaire privée Barsamian",null,"Clôturée",null,null,"Clôturée","06088","NICE","ALPES-MARITIMES","PROVENCE-ALPES-COTE D'AZUR","Polygone",7.2245383,43.714596]
["SSP000482001",null,"Ecole maternelle de la Plage",null,"Clôturée",null,null,"Clôturée","06104","ROQUEBRUNE CAP MARTIN","ALPES-MARITIMES","PROVENCE-ALPES-COTE D'AZUR","Polygone",7.47938,43.75913]
["SSP000482401","59.0302","CENTRE EDF GDF SERVICES HAINAULT-CAMBRESIS",null,"En cours",null,null,"En cours","59036","AVESNES SUR HELPE","NORD","HAUTS-DE-FRANCE","Polygone",3.9254432,50.12507,"J1 - Cokéfaction, usines à gaz"]
["SSP000482901","45.0023","CHAMPATAY",null,"En cours",null,null,"En cours","45248","PATAY","LOIRET","CENTRE-VAL DE LOIRE","Polygone",1.704787,48.04445,"D4 - Encres, vernis, peintures, colles (fabrication de)"]
["SSP000483301","45.0015","Installation technique de Gaz de France",null,"Clôturée",null,"2012-08-22","Clôturée","45203","MEUNG SUR LOIRE","LOIRET","CENTRE-VAL DE LOIRE","Polygone",1.7041869,47.833015,"J1 - Cokéfaction, usines à gaz"]
["SSP000483501","68.0169","NOUVELLE SABLIERE DE HUNINGUE",null,"En cours",null,null,"En cours","68149","HUNINGUE","HAUT-RHIN","GRAND EST","Polygone",7.5772276,47.583633]
["SSP000484001","45.0036","SARL CARLIER",null,"En cours",null,null,"En cours","45083","CHATEAU RENARD","LOIRET","CENTRE-VAL DE LOIRE","Polygone",2.934415,47.933704,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000484301",null,"MYRRA",null,"Clôturée",null,null,"Clôturée","77121","COLLEGIEN","SEINE-ET-MARNE","ILE-DE-FRANCE","Polygone",2.6744273,48.82991]
["SSP000485001","72.0063","ALMIRALL PRODUCTION",null,"En cours",null,null,"En cours","72071","CHATEAU DU LOIR","SARTHE","PAYS DE LA LOIRE","Polygone",0.42054564,47.691708,"D38 - Industrie pharmaceutique"]
["SSP000485101","37.0024","Arts et Meubles de France",null,"En cours",null,null,"En cours","37196","RICHELIEU","INDRE-ET-LOIRE","CENTRE-VAL DE LOIRE","Polygone",0.32309303,47.03163,"C1 - Bois et de l'ameublement (industrie du)"]
["SSP000485501","37.0030","PAL PACK",null,"En cours",null,null,"En cours","37150","MAZIERES DE TOURAINE","INDRE-ET-LOIRE","CENTRE-VAL DE LOIRE","Polygone",0.39952457,47.381104,"K35 - Regroupement, reconditionnement de déchets"]
["SSP000486001","36.0020","ancien dépôt BP d'Issoudun",null,"En cours",null,null,"En cours","36179","SAINT AOUSTRILLE","INDRE","CENTRE-VAL DE LOIRE","Polygone",1.9697447,46.939148,"L23 - Détail de carburants"]
["SSP000486501","49.0068","VETIR (groupe ERAM)",null,"En cours",null,null,"En cours","49125","DOUE LA FONTAINE","MAINE-ET-LOIRE","PAYS DE LA LOIRE","Polygone",-0.24920875,47.184998,"D7 - Caoutchouc et matières plastiques"]
["SSP000486901","13.0133","DEPOT DE LA PLAINE DE PECOUT",null,"En cours",null,null,"En cours","13112","VELAUX","BOUCHES-DU-RHONE","PROVENCE-ALPES-COTE D'AZUR","Polygone",5.228582,43.523224,"D12 - Raffinage de pétrole, carburants et lubrifiants"]
["SSP000487701",null,"NPC AUTOLIV",null,"Clôturée",null,null,"Clôturée","76165","CAUDEBEC LES ELBEUF","SEINE-MARITIME","NORMANDIE","Polygone",1.0245787,49.288757]
["SSP000488101","36.0013","EDF GDF SERVICES INDRE EN BERRY",null,"En cours",null,null,"En cours","36006","ARGENTON SUR CREUSE","INDRE","CENTRE-VAL DE LOIRE","Polygone",1.5256287,46.585846,"J1 - Cokéfaction, usines à gaz"]
["SSP000488601",null,"AIR LIQUIDE - USINE ACETYLENE",null,"Clôturée",null,null,"Clôturée","77294","MITRY MORY","SEINE-ET-MARNE","ILE-DE-FRANCE","Polygone",2.6409583,48.985157]
["SSP000488701","36.0005","Subdivision DDE",null,"En cours",null,null,"En cours","36046","LA CHATRE","INDRE","CENTRE-VAL DE LOIRE","Polygone",1.9905121,46.58667,"J1 - Cokéfaction, usines à gaz"]
["SSP000489101","28.0040","REVELEC",null,"En cours",null,null,"En cours","28015","AUNEAU","EURE-ET-LOIR","CENTRE-VAL DE LOIRE","Polygone",1.7655382,48.459225,"H1 - Mécanique, électrique, traitement de surface"]
["SSP000489501",null,"AUTELY",null,"Clôturée",null,null,"Clôturée","26362","VALENCE","DROME","AUVERGNE-RHONE-ALPES","Polygone",4.8865404,44.919155]
["SSP000490201","76.0009","Déposante du chene fourchu",null,"En cours",null,null,"En cours","76231","ELBEUF","SEINE-MARITIME","NORMANDIE","Polygone",1.0052307,49.265297,"K36 - Mise en décharge"]
["SSP000490401",null,"Ecole primaire Victor Hugo",null,"Clôturée",null,null,"Clôturée","76165","CAUDEBEC LES ELBEUF","SEINE-MARITIME","NORMANDIE","Polygone",1.0153728,49.282444]
["SSP000491001",null,"Bammeville",null,"Clôturée",null,null,"Clôturée","76540","ROUEN","SEINE-MARITIME","NORMANDIE","Polygone",1.0923442,49.431194]
["SSP000491501",null,"Ecole maternelle Gérard Philippe",null,"Clôturée",null,null,"Clôturée","76498","LE PETIT QUEVILLY","SEINE-MARITIME","NORMANDIE","Polygone",1.067688,49.413612]
["SSP000492101",null,"Ancienne décharge de la route Longeau",null,"Clôturée",null,null,"Clôturée","22290","SAINT GELVEN","COTES-D'ARMOR","BRETAGNE","Polygone",-3.1014497,48.223488]
["SSP000492301",null,"Société BP FIOUL SERVICES",null,"Clôturée",null,null,"Clôturée","77243","LAGNY SUR MARNE","SEINE-ET-MARNE","ILE-DE-FRANCE","Polygone",2.684553,48.871574]
["SSP000492601","13.0167","TRIEDEC",null,"En cours",null,null,"En cours","13043","GIGNAC LA NERTHE","BOUCHES-DU-RHONE","PROVENCE-ALPES-COTE D'AZUR","Polygone",5.2106028,43.39193]
["SSP000493101",null,"Ecole Pierre Curie",null,"Clôturée",null,null,"Clôturée","76217","DIEPPE","SEINE-MARITIME","NORMANDIE","Polygone",1.1027753,49.923626]
["SSP000493701","44.0076","Jules Olivier Distribution",null,"En cours",null,null,"En cours","44186","SAINTE PAZANNE","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Polygone",-1.242039,47.2635]
["SSP000493801","72.0028","ALLIAGES METALLURGIES LEBLOND",null,"Clôturée",null,"2013-04-17","Clôturée","72095","COULAINES","SARTHE","PAYS DE LA LOIRE","Polygone",0.19621518,48.027637]
["SSP000494401",null,"Caillaud Bois",null,"Clôturée",null,null,"Clôturée","49092","CHEMILLE MELAY","MAINE-ET-LOIRE","PAYS DE LA LOIRE","Polygone",-0.69529444,47.18307]
["SSP000494801","72.0008","LANGLOIS CHIMIE",null,"En cours",null,null,"En cours","72181","LE MANS","SARTHE","PAYS DE LA LOIRE","Polygone",0.18265428,47.966022,"L13 - Entrepôts de produits dangereux"]
["SSP000495001","72.0033","Station-service Shell",null,"En cours",null,null,"En cours","72181","LE MANS","SARTHE","PAYS DE LA LOIRE","Polygone",0.22644651,47.997253,"L23 - Détail de carburants"]
["SSP000495301",null,"IDEAL STANDARD FRANCE",null,"Clôturée",null,null,"Clôturée","08363","REVIN","ARDENNES","GRAND EST","Polygone",4.6469145,49.9375]
["SSP000497801",null,"Gascogne Laminates",null,"Clôturée",null,null,"Clôturée","08190","GIVET","ARDENNES","GRAND EST","Polygone",4.8342915,50.13531]
["SSP000499401","52.0036","VSA ex VOILLEQUIN",null,"En cours",null,null,"En cours","52353","NOGENT","HAUTE-MARNE","GRAND EST","Polygone",5.3492227,48.030422,"H13 - Traitement de surface"]
["SSP000502101",null,"IMMOBILIERE PARAGON FRANCE",null,"Clôturée",null,null,"Clôturée","77121","COLLEGIEN","SEINE-ET-MARNE","ILE-DE-FRANCE","Polygone",2.6696222,48.82816]
["SSP000502201","53.0041","Lycée Douanier Rousseau","Lycée Douanier Rousseau","En cours",null,null,"En cours","53130","LAVAL","MAYENNE","PAYS DE LA LOIRE","Polygone",-0.76137626,48.072132,null,null,null,"85.31Z - Enseignement secondaire général"]
["SSP000502901",null,"Ancienne décharge de La Chaussaire",null,"Clôturée",null,null,"Clôturée","49085","LA CHAUSSAIRE","MAINE-ET-LOIRE","PAYS DE LA LOIRE","Polygone",-1.1557939,47.203827]
["SSP000503301",null,"Ancienne décharge Saint Clément des Levées",null,"Clôturée",null,null,"Clôturée","49272","SAINT CLEMENT DES LEVEES","MAINE-ET-LOIRE","PAYS DE LA LOIRE","Polygone",-0.18416815,47.35733]
["SSP000503501",null,"Ancienne décharge de Turquant",null,"Clôturée",null,null,"Clôturée","49358","TURQUANT","MAINE-ET-LOIRE","PAYS DE LA LOIRE","Polygone",0.022824422,47.20815]
["SSP000503801",null,"Ancienne décharge du May sur Evre",null,"Clôturée",null,null,"Clôturée","49193","LE MAY SUR EVRE","MAINE-ET-LOIRE","PAYS DE LA LOIRE","Polygone",-0.88378704,47.14217]
["SSP000504301",null,"Ancienne décharge de Vivy",null,"Clôturée",null,null,"Clôturée","49378","VIVY","MAINE-ET-LOIRE","PAYS DE LA LOIRE","Polygone",-0.0707416,47.315197]
["SSP000504701",null,"Ancienne décharge Morannes",null,"Clôturée",null,null,"Clôturée","49220","MORANNES","MAINE-ET-LOIRE","PAYS DE LA LOIRE","Polygone",-0.42218626,47.745617]
["SSP000505301","45.0027","DIFFUSION EVL",null,"En cours",null,null,"En cours","45155","GIEN","LOIRET","CENTRE-VAL DE LOIRE","Polygone",2.628233,47.7075,"H - Mécanique, traitements des surfaces"]
["SSP000505701","91.0028","CABLERIE DE CROSNE",null,"En cours",null,"2005-01-26","En cours","91191","CROSNE","ESSONNE","ILE-DE-FRANCE","Polygone",2.4557428,48.719677,"J53 - Travail des métaux, chaudronnerie, poudres"]
["SSP000506001",null,"ancien dépôt d'engrais et de munition",null,"Clôturée",null,null,"Clôturée","13004","ARLES","BOUCHES-DU-RHONE","PROVENCE-ALPES-COTE D'AZUR","Polygone",4.608816,43.676094]
["SSP000507001","28.0012","Perferct Circle Europe",null,"En cours",null,null,"En cours","28134","DREUX","EURE-ET-LOIR","CENTRE-VAL DE LOIRE","Polygone",1.3675963,48.74712,"H11 - Usinage"]
["SSP000507201","28.0079","Stylewood",null,"En cours",null,null,"En cours","28373","SENONCHES","EURE-ET-LOIR","CENTRE-VAL DE LOIRE","Polygone",1.0243497,48.561543,"C1 - Bois et de l'ameublement (industrie du)"]
["SSP000507701","93.0057","Caldeo",null,"En cours",null,null,"En cours","93057","LES PAVILLONS SOUS BOIS","SEINE-SAINT-DENIS","ILE-DE-FRANCE","Polygone",2.4991462,48.914124,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000508401","72.0002","Ancien site usine à gaz ENGIE",null,"En cours",null,null,"En cours","72181","LE MANS","SARTHE","PAYS DE LA LOIRE","Polygone",0.18729721,47.99818,"J1 - Cokéfaction, usines à gaz"]
["SSP000508801","76.0138","Rue des chantiers - Ex ACH construction Navale GRAVILLE",null,"En cours",null,null,"En cours","76351","LE HAVRE","SEINE-MARITIME","NORMANDIE","Polygone",0.1608341,49.478302,"J53 - Travail des métaux, chaudronnerie, poudres"]
["SSP000509301","76.0154","Place Caillard - Ex site Caillard",null,"En cours",null,null,"En cours","76351","LE HAVRE","SEINE-MARITIME","NORMANDIE","Polygone",0.12883554,49.48494]
["SSP000509601","76.0291","Route de la Pointe du Hoc - Ex GLI Services",null,"En cours",null,null,"En cours","76351","LE HAVRE","SEINE-MARITIME","NORMANDIE","Polygone",0.1861047,49.48235,"H - Mécanique, traitements des surfaces"]
["SSP000509801","76.0243","ROUTE DU PONT VII - Ex MILLENIUM CHEMICALS SAS",null,"En cours",null,null,"En cours","76351","LE HAVRE","SEINE-MARITIME","NORMANDIE","Polygone",0.17657663,49.48802]
["SSP000510401","13.0012","SITE DE LA SOCIETE CHIMIQUE DE GERLAND",null,"En cours",null,null,"En cours","13078","PORT SAINT LOUIS DU RHONE","BOUCHES-DU-RHONE","PROVENCE-ALPES-COTE D'AZUR","Polygone",4.8092527,43.394352,"D33 - Pétrochimie carbochimie organique"]
["SSP000510601",null,"Bois \"Les carrières\"",null,"Clôturée",null,null,"Clôturée","77139","COURTRY","SEINE-ET-MARNE","ILE-DE-FRANCE","Polygone",2.5973463,48.921284]
["SSP000511501","93.0001","ex PROGIVEN",null,"En cours",null,null,"En cours","93001","AUBERVILLIERS","SEINE-SAINT-DENIS","ILE-DE-FRANCE","Polygone",2.367018,48.915726,"D3 - Chimie, phytosanitaire, pharmacie"]
["SSP000512501",null,"GARAGE COLLET",null,"Clôturée",null,null,"Clôturée","78168","COIGNIERES","YVELINES","ILE-DE-FRANCE","Polygone",1.9360216,48.753456]
["SSP000513001",null,"Ancienne décharge de l'ancien aérodrome",null,"Clôturée",null,null,"Clôturée","22215","PLOUFRAGAN","COTES-D'ARMOR","BRETAGNE","Polygone",-2.811015,48.511898]
["SSP000513501",null,"Ancienne décharge de la rue des Bosses",null,"Clôturée",null,null,"Clôturée","22215","PLOUFRAGAN","COTES-D'ARMOR","BRETAGNE","Polygone",-2.782284,48.48475]
["SSP000514101","72.0036","Point P (ex- COLWELL EUROPE SAS)",null,"En cours",null,null,"En cours","72035","BESSE SUR BRAYE","SARTHE","PAYS DE LA LOIRE","Polygone",0.7571818,47.83323,"C22 - Fabrication de papiers et carton"]
["SSP000514301",null,"Ancienne décharfge de Koatilan",null,"Clôturée",null,null,"Clôturée","22217","PLOUGRAS","COTES-D'ARMOR","BRETAGNE","Polygone",-3.5682049,48.503937]
["SSP000514601",null,"Ancienne décharge de Pont Men",null,"Clôturée",null,null,"Clôturée","22235","PLOUZELAMBRE","COTES-D'ARMOR","BRETAGNE","Polygone",-3.5396035,48.648064]
["SSP000515201",null,"Ancienne décharge de Rugoasvin",null,"Clôturée",null,null,"Clôturée","22254","PRAT","COTES-D'ARMOR","BRETAGNE","Polygone",-3.3080144,48.674957]
["SSP000515301",null,"Ancienne décharge de Kervocu",null,"Clôturée",null,null,"Clôturée","22254","PRAT","COTES-D'ARMOR","BRETAGNE","Polygone",-3.2758656,48.699303]
["SSP000515801","14.0020","Ex MOULINEX",null,"En cours",null,null,"En cours","14181","CORMELLES LE ROYAL","CALVADOS","NORMANDIE","Polygone",-0.3237145,49.155125]
["SSP000516301","14.0002","UNIMETAL NORMANDIE",null,"En cours",null,null,"En cours","14327","HEROUVILLE SAINT CLAIR","CALVADOS","NORMANDIE","Polygone",-0.30995426,49.18979,"J - Sidérurgie, métallurgie, coke"]
["SSP000516701",null,"SITREVA",null,"Clôturée",null,null,"Clôturée","78564","SAINT MARTIN DE BRETHENCOURT","YVELINES","ILE-DE-FRANCE","Polygone",1.9472759,48.519535]
["SSP000516801","72.0067","PIGEON BOIS 72",null,"En cours",null,null,"En cours","72243","PONTVALLAIN","SARTHE","PAYS DE LA LOIRE","Polygone",0.1900908,47.766766,"C1 - Bois et de l'ameublement (industrie du)"]
["SSP000517501","36.0027","YARA France",null,"En cours",null,null,"En cours","36088","ISSOUDUN","INDRE","CENTRE-VAL DE LOIRE","Polygone",1.9961702,46.95971,"D36 - Fabrication des engrais"]
["SSP000517901",null,"PMB Automobiles",null,"Clôturée",null,null,"Clôturée","78686","VIROFLAY","YVELINES","ILE-DE-FRANCE","Polygone",2.1609998,48.799675]
["SSP000519401",null,"Ancienne aire d'accueil",null,"Clôturée",null,null,"Clôturée","84007","AVIGNON","VAUCLUSE","PROVENCE-ALPES-COTE D'AZUR","Polygone",4.78667,43.938957]
["SSP000519501","95.0007","CPT EDF CHAMPAGNE SUR OISE",null,"En cours",null,null,"En cours","95134","CHAMPAGNE SUR OISE","VAL-D'OISE","ILE-DE-FRANCE","Point",0.0,0.0,"I11 - Centrales électriques thermiques"]
["SSP000520001",null,"Ancienne décharge des Caves des landelles",null,"Clôturée",null,null,"Clôturée","22246","POMMERET","COTES-D'ARMOR","BRETAGNE","Polygone",-2.6424263,48.467392]
["SSP000520401","94.0108","COMAU SCIAKY",null,"En cours",null,null,"En cours","94081","VITRY SUR SEINE","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.4072318,48.80411]
["SSP000521201",null,"PPC (ex. Freyssinet Industries)",null,"Clôturée",null,null,"Clôturée","71475","SAINT REMY","SAONE-ET-LOIRE","BOURGOGNE-FRANCHE-COMTE","Polygone",4.842792,46.77052]
["SSP000521301","53.0003","Ancienne mines de la Lucette",null,"En cours",null,null,"En cours","53103","LE GENEST SAINT ISLE","MAYENNE","PAYS DE LA LOIRE","Polygone",-0.91004676,48.096176,"F31 - Minerais non métalliques (extraction de)"]
["SSP000521901","44.0137","Garage Pluchon (ex-GARAGE BEAUCHENE)",null,"En cours",null,null,"En cours","44142","REMOUILLE","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Polygone",-1.3733306,47.057026,"L21 - Vente et réparation automobile"]
["SSP000522301",null,"Ancienne décharge du Val",null,"Clôturée",null,null,"Clôturée","22234","PLOUVARA","COTES-D'ARMOR","BRETAGNE","Polygone",-2.900798,48.504707]
["SSP000522901",null,"Ancienne décharge du Louch Vraz",null,"Clôturée",null,null,"Clôturée","22304","SAINT JEAN KERDANIEL","COTES-D'ARMOR","BRETAGNE","Polygone",-3.0367894,48.55127]
["SSP000523201",null,"Ancienne décharge d'ordures ménagères",null,"Clôturée",null,null,"Clôturée","53096","ERNEE","MAYENNE","PAYS DE LA LOIRE","Polygone",-0.9307127,48.327465]
["SSP000523501",null,"Ancienne décharge d'ordures ménagères",null,"Clôturée",null,null,"Clôturée","53029","BIERNE","MAYENNE","PAYS DE LA LOIRE","Polygone",-0.5133773,47.789856]
["SSP000524101",null,"Ancienne décharge d'ordures sauvages",null,"Clôturée",null,null,"Clôturée","53036","BOUERE","MAYENNE","PAYS DE LA LOIRE","Polygone",-0.46427286,47.85051]
["SSP000524501",null,"Entreprise Pautrel - Décharge d'ordures ménagères, dépot de vidange",null,"Clôturée",null,null,"Clôturée","53077","COSSE LE VIVIEN","MAYENNE","PAYS DE LA LOIRE","Polygone",-0.9462434,47.91415]
["SSP000524601",null,"Ancienne décharge de Malabry",null,"Clôturée",null,null,"Clôturée","22248","POMMERIT LE VICOMTE","COTES-D'ARMOR","BRETAGNE","Polygone",-3.090828,48.63642]
["SSP000525101",null,"Ancien dépôt d’ordures ménagères",null,"Clôturée",null,null,"Clôturée","53172","ORIGNE","MAYENNE","PAYS DE LA LOIRE","Polygone",-0.7390493,47.966545]
["SSP000525601",null,"Ancien dépôt d’ordures ménagères et de vidanges",null,"Clôturée",null,null,"Clôturée","53014","AZE","MAYENNE","PAYS DE LA LOIRE","Polygone",-0.6987299,47.83511]
["SSP000526601",null,"Ancienne décharge d'ordures ménagères",null,"Clôturée",null,null,"Clôturée","53004","AMPOIGNE","MAYENNE","PAYS DE LA LOIRE","Polygone",-0.8234137,47.808487]
["SSP000528101",null,"Ancienne décharge du Petit Village (secteur sud)",null,"Clôturée",null,null,"Clôturée","22241","PLUMIEUX","COTES-D'ARMOR","BRETAGNE","Polygone",-2.5788686,48.09188]
["SSP000528801",null,"VAYSSADE",null,"Clôturée",null,null,"Clôturée","95288","GROSLAY","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.352329,48.986443]
["SSP000529401",null,"Ancienne décharge d'ordures ménagères",null,"Clôturée",null,null,"Clôturée","53101","FROMENTIERES","MAYENNE","PAYS DE LA LOIRE","Polygone",-0.6843453,47.84834]
["SSP000529801",null,"Ancienne décharge d'ordures ménagères",null,"Clôturée",null,null,"Clôturée","53231","SAINT LAURENT DES MORTIERS","MAYENNE","PAYS DE LA LOIRE","Polygone",-0.5428073,47.767925]
["SSP000529901",null,"Ancienne décharge d'ordures ménagères",null,"Clôturée",null,null,"Clôturée","53231","SAINT LAURENT DES MORTIERS","MAYENNE","PAYS DE LA LOIRE","Polygone",-0.55134827,47.766376]
["SSP000530401",null,"PASQUIER (ex. AUGA PICARD)",null,"Clôturée",null,null,"Clôturée","95658","VIGNY","VAL-D'OISE","ILE-DE-FRANCE","Polygone",1.9192983,49.084976]
["SSP000531501",null,"panavi",null,"Clôturée",null,null,"Clôturée","14437","MONDEVILLE","CALVADOS","NORMANDIE","Polygone",-0.30801934,49.155838]
["SSP000532201","2B.0006","ESSO S.A.F. Aéroport Bastia Poretta",null,"En cours",null,null,"En cours","2B148","LUCCIANA","HAUTE-CORSE","CORSE","Polygone",9.482237,42.546253,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000532501",null,"EDF",null,"Clôturée",null,null,"Clôturée","94022","CHOISY LE ROI","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.4097147,48.768803]
["SSP000532801",null,"Ancienne décharge de Rochroy",null,"Clôturée",null,null,"Clôturée","22298","SAINT GUEN","COTES-D'ARMOR","BRETAGNE","Polygone",-2.9434254,48.22385]
["SSP000533301",null,"RECYCLAGE 94",null,"Clôturée",null,null,"Clôturée","94022","CHOISY LE ROI","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.4225562,48.75846]
["SSP000533701","72.0072","SABLE",null,"En cours",null,null,"En cours","72181","LE MANS","SARTHE","PAYS DE LA LOIRE","Polygone",0.17672917,47.958893,"H13 - Traitement de surface"]
["SSP000533901",null,"SCL (ex STREDO)",null,"Clôturée",null,null,"Clôturée","94022","CHOISY LE ROI","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.41437,48.757175]
["SSP000534901","93.0019","TFR (Toute la France pour la Route)",null,"En cours",null,null,"En cours","93027","LA COURNEUVE","SEINE-SAINT-DENIS","ILE-DE-FRANCE","Polygone",2.4105937,48.941494,"K4 - Activité de régénération"]
["SSP000536001","77.0035","CIPEL (ex HOLLANDER)","CIPEL (ex HOLLANDER)","En cours",null,null,"En cours","77243","LAGNY SUR MARNE","SEINE-ET-MARNE","ILE-DE-FRANCE","Polygone",2.694657,48.877613]
["SSP000536801",null,"MURE",null,"Clôturée",null,null,"Clôturée","94041","IVRY SUR SEINE","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.4015265,48.80659]
["SSP000537201",null,"DIA",null,"Clôturée",null,null,"Clôturée","94081","VITRY SUR SEINE","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.4050214,48.779778]
["SSP000537501",null,"COMPAGNIE PHILIPS ECLAIRAGE: Crèche",null,"Clôturée",null,null,"Clôturée","94041","IVRY SUR SEINE","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.4009564,48.81357]
["SSP000538101",null,"Casse DP Recyclage",null,"Clôturée",null,null,"Clôturée","2B042","BORGO","HAUTE-CORSE","CORSE","Polygone",9.440714,42.58478,"K52 - Dépôts de ferraille"]
["SSP000539801",null,"Centre EDF/GDF Services Cher en Berry",null,"Clôturée",null,null,"Clôturée","18033","BOURGES","CHER","CENTRE-VAL DE LOIRE","Polygone",2.3832545,47.078945]
["SSP000539901",null,"Ancien dépôt de fuel",null,"Clôturée",null,null,"Clôturée","56054","ERDEVEN","MORBIHAN","BRETAGNE","Polygone",-3.1885705,47.653927]
["SSP000540801","91.0100","Station-service Total",null,"En cours",null,null,"En cours","91659","VILLABE","ESSONNE","ILE-DE-FRANCE","Polygone",2.4426055,48.59379,"L23 - Détail de carburants"]
["SSP000541601","18.0065","Décharge Torteron",null,"En cours",null,null,"En cours","18265","TORTERON","CHER","CENTRE-VAL DE LOIRE","Polygone",2.9856632,47.016525,"K2 - Traitement de déchets urbains"]
["SSP000541901","77.0159","DIAL FONDERIE","DIAL FONDERIE","En cours",null,null,"En cours","77305","MONTEREAU FAULT YONNE","SEINE-ET-MARNE","ILE-DE-FRANCE","Polygone",2.965102,48.38574,"J5 - Fonderie et travail des métaux"]
["SSP000542201","77.0126","THEVENIN ET DUCROT DISTRIBUTION","THEVENIN ET DUCROT DISTRIBUTION","En cours",null,null,"En cours","77327","NANGIS","SEINE-ET-MARNE","ILE-DE-FRANCE","Polygone",3.0314672,48.5592,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000542901",null,"Ancienne décharge du Fort de Landaoudec",null,"Clôturée",null,null,"Clôturée","29042","CROZON","FINISTERE","BRETAGNE","Polygone",-4.4843125,48.270996]
["SSP000544801","94.0030","LIEU DIT \"LA POLOGNE\"",null,"En cours",null,null,"En cours","94078","VILLENEUVE SAINT GEORGES","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.4678843,48.737614,"K51 - Récupération non ferreux"]
["SSP000545301","15.0003","Ancienne usine à gaz",null,"En cours",null,null,"En cours","15138","MURAT","CANTAL","AUVERGNE-RHONE-ALPES","Polygone",2.8631766,45.10917]
["SSP000545601",null,"Dépôt minier",null,"Clôturée",null,null,"Clôturée","63023","AUZELLES","PUY-DE-DOME","AUVERGNE-RHONE-ALPES","Polygone",3.5002825,45.60648]
["SSP000546101","91.0023","USINE NEXANS (Ex ALCATEL CABLE ,ex FILOTEX)",null,"En cours",null,null,"En cours","91201","DRAVEIL","ESSONNE","ILE-DE-FRANCE","Polygone",2.427853,48.680058,"H18 - Composants électroniques (fabrication de)"]
["SSP000546901",null,"Dépôt minier",null,"Clôturée",null,null,"Clôturée","63132","CUNLHAT","PUY-DE-DOME","AUVERGNE-RHONE-ALPES","Polygone",3.5408933,45.64658]
["SSP000547201","91.0011","SOCIETE  FERELEC INDUSTRIES",null,"En cours",null,null,"En cours","91086","BONDOUFLE","ESSONNE","ILE-DE-FRANCE","Polygone",2.3771713,48.620926,"H13 - Traitement de surface"]
["SSP000547401",null,"Dépôt minier de Pratclos",null,"Clôturée",null,null,"Clôturée","43112","LANGEAC","HAUTE-LOIRE","AUVERGNE-RHONE-ALPES","Polygone",3.483914,45.045784]
["SSP000548001",null,"Dépôt minier du Cheylat",null,"Clôturée",null,null,"Clôturée","43182","SAINT ETIENNE SUR BLESLE","HAUTE-LOIRE","AUVERGNE-RHONE-ALPES","Polygone",3.1461952,45.299744]
["SSP000549201","03.0020","Ancienne usine BOSTIK",null,"En cours",null,"2011-07-07","En cours","03094","CREUZIER LE VIEUX","ALLIER","AUVERGNE-RHONE-ALPES","Polygone",3.4127574,46.16176,"D44 - Fabrication de colles et mastics"]
["SSP000549601",null,"décharge de Trelins",null,"Clôturée",null,null,"Clôturée","42313","TRELINS","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.004483,45.727657]
["SSP000549701",null,"Travaux miniers DEMARTY",null,"Clôturée",null,null,"Clôturée","63184","LACHAUX","PUY-DE-DOME","AUVERGNE-RHONE-ALPES","Polygone",3.5847905,45.99904]
["SSP000550301","03.0045","Anciens établissements BOURBON",null,"En cours",null,null,"En cours","03315","VILLEFRANCHE D'ALLIER","ALLIER","AUVERGNE-RHONE-ALPES","Polygone",2.853546,46.401054]
["SSP000550801",null,"Depôts miniers de la Gare",null,"Clôturée",null,null,"Clôturée","63165","GIAT","PUY-DE-DOME","AUVERGNE-RHONE-ALPES","Polygone",2.4730916,45.796967]
["SSP000551101",null,"Dépôts Miniers - Foirail",null,"Clôturée",null,null,"Clôturée","63165","GIAT","PUY-DE-DOME","AUVERGNE-RHONE-ALPES","Polygone",2.4688754,45.801067]
["SSP000551501","03.0021","ANCIENNES FONDERIES ST JACQUES",null,"En cours",null,null,"En cours","03185","MONTLUCON","ALLIER","AUVERGNE-RHONE-ALPES","Polygone",2.6076066,46.349228,"J22 - Production d'acier brut, aciéries"]
["SSP000552201",null,"Ancien site minier uranifère - POYET (LE)",null,"Clôturée",null,null,"Clôturée","63027","BAFFIE","PUY-DE-DOME","AUVERGNE-RHONE-ALPES","Polygone",3.8129003,45.487625]
["SSP000552501","72.0003","ANCIEN SITE \"USINE A GAZ\"",null,"En cours",null,null,"En cours","72039","BONNETABLE","SARTHE","PAYS DE LA LOIRE","Polygone",0.41789886,48.17293]
["SSP000553301","72.0022","Agence d'exploitation d'EDF / GDF (ex-USINE A GAZ)",null,"En cours",null,null,"En cours","72315","SAINT REMY DE SILLE","SARTHE","PAYS DE LA LOIRE","Polygone",-0.12250925,48.181454]
["SSP000553401",null,"Remblai uranifère",null,"Clôturée",null,null,"Clôturée","63173","GRANDRIF","PUY-DE-DOME","AUVERGNE-RHONE-ALPES","Polygone",3.808117,45.49362]
["SSP000553901","03.0031","Anciens  établissements  CABASSE  INDUSTRIE",null,"En cours",null,null,"En cours","03221","SAINT BONNET TRONCAIS","ALLIER","AUVERGNE-RHONE-ALPES","Polygone",2.7181132,46.642265,"C12 - Produits en bois, ameublement (fabrication de)"]
["SSP000554301",null,"Ancienne décharge de Saint Ouen-en-Belin",null,"Clôturée",null,null,"Clôturée","72306","SAINT OUEN EN BELIN","SARTHE","PAYS DE LA LOIRE","Polygone",0.19960429,47.845287]
["SSP000554801",null,"Ancien site minier uranifère - PEN AR RAN",null,"Clôturée",null,null,"Clôturée","44125","PIRIAC SUR MER","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Polygone",-2.5455008,47.372257]
["SSP000554901","03.0016","Centre EDF GDF SERVICES",null,"En cours",null,null,"En cours","03082","COMMENTRY","ALLIER","AUVERGNE-RHONE-ALPES","Polygone",2.7519336,46.289593]
["SSP000555501","03.0019","Ancien dépot d'hydrocarbures ELF",null,"En cours",null,null,"En cours","03321","YZEURE","ALLIER","AUVERGNE-RHONE-ALPES","Polygone",3.3485813,46.549793,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000555801",null,"Remblai uranifère",null,"Clôturée",null,null,"Clôturée","43048","LA CHAISE DIEU","HAUTE-LOIRE","AUVERGNE-RHONE-ALPES","Polygone",3.7002702,45.327488]
["SSP000556601",null,"ancienne décharge d'Allonnes",null,"Clôturée",null,null,"Clôturée","72003","ALLONNES","SARTHE","PAYS DE LA LOIRE","Polygone",0.15305415,47.94413]
["SSP000556701",null,"Ancienne décharge de Ruaudin",null,"Clôturée",null,null,"Clôturée","72260","RUAUDIN","SARTHE","PAYS DE LA LOIRE","Polygone",0.25975546,47.933006]
["SSP000557101",null,"Ancienne décharge de Ponvallain",null,"Clôturée",null,null,"Clôturée","72243","PONTVALLAIN","SARTHE","PAYS DE LA LOIRE","Polygone",0.18591776,47.737904]
["SSP000557501",null,"Activités minières",null,"Clôturée",null,null,"Clôturée","07090","FLAVIAC","ARDECHE","AUVERGNE-RHONE-ALPES","Polygone",4.6663694,44.75035]
["SSP000558001",null,"Ancienne décharge de Saint Vincent",null,"Clôturée",null,null,"Clôturée","72324","SAINT VINCENT DES PRES","SARTHE","PAYS DE LA LOIRE","Polygone",0.37142166,48.29267]
["SSP000558101",null,"Ancien dépôt de la roseraie",null,"Clôturée",null,null,"Clôturée","72316","SAINT REMY DES MONTS","SARTHE","PAYS DE LA LOIRE","Polygone",0.39886788,48.308323]
["SSP000558701","44.0136","la Bauloise Automobiles SA (ex-CHANARD AUTOMOBILE)",null,"En cours",null,null,"En cours","44069","GUERANDE","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Polygone",-2.3971298,47.292904,"L2 - Transports, automobile, carburants"]
["SSP000559001",null,"Ancienne décharge du Bourg",null,"Clôturée",null,null,"Clôturée","35256","SAINT BRIAC SUR MER","ILLE-ET-VILAINE","BRETAGNE","Polygone",-2.1186678,48.62054]
["SSP000559401","76.0003","USINE A GAZ DE DIEPPE (ex Lebon et compagnie)",null,"En cours",null,null,"En cours","76217","DIEPPE","SEINE-MARITIME","NORMANDIE","Polygone",1.0982559,49.91717,"J1 - Cokéfaction, usines à gaz"]
["SSP000559501","76.0063","VINCO",null,"Clôturée",null,null,"Clôturée","76414","MARTIN EGLISE","SEINE-MARITIME","NORMANDIE","Polygone",1.0998925,49.913017,"H14 - Application de peinture"]
["SSP000560001",null,"THOUMYRE",null,"Clôturée",null,null,"Clôturée","76026","ARQUES LA BATAILLE","SEINE-MARITIME","NORMANDIE","Polygone",1.133476,49.883488,null,null,"10.1Z - Extraction et agglomération de la houille"]
["SSP000560401","76.0106","Usine à gaz de Neufchâtel-en-Bray",null,"En cours",null,null,"En cours","76462","NEUFCHATEL EN BRAY","SEINE-MARITIME","NORMANDIE","Polygone",1.4331429,49.730125]
["SSP000560901","76.0355","Station-service TOTAL relais Saint Aubin",null,"En cours",null,null,"En cours","76312","GOURNAY EN BRAY","SEINE-MARITIME","NORMANDIE","Polygone",1.7074839,49.484287]
["SSP000561101","76.0051","Troussel",null,"En cours",null,null,"En cours","76255","EU","SEINE-MARITIME","NORMANDIE","Polygone",1.4215773,50.05534,"H13 - Traitement de surface"]
["SSP000561401","76.0298","VERSTRAETE",null,"En cours",null,null,"En cours","76255","EU","SEINE-MARITIME","NORMANDIE","Polygone",1.4159522,50.052483]
["SSP000561901","76.0228","Fonderie de la BRESLE",null,"En cours",null,null,"En cours","76101","BLANGY SUR BRESLE","SEINE-MARITIME","NORMANDIE","Polygone",1.6166543,49.93761,"J52 - Fonderie des métaux non ferreux"]
["SSP000562101","76.0007","Affinerie Cauchoise",null,"En cours",null,null,"En cours","76602","SAINT MACLOU DE FOLLEVILLE","SEINE-MARITIME","NORMANDIE","Polygone",1.1108754,49.67664,"K36 - Mise en décharge"]
["SSP000562401",null,"Ancienne décharge de Ballon",null,"Clôturée",null,null,"Clôturée","72023","BALLON","SARTHE","PAYS DE LA LOIRE","Polygone",0.24344647,48.16012]
["SSP000563001","95.0011","GAZ DE FRANCE à L'Isle-Adam",null,"En cours",null,null,"En cours","95313","L'ISLE ADAM","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.210406,49.106594,"J1 - Cokéfaction, usines à gaz"]
["SSP000563401","05.0001","CRASSIER RIO TINTO ALCAN (Ex Péchiney)",null,"En cours",null,null,"En cours","05006","L'ARGENTIERE LA BESSEE","HAUTES-ALPES","PROVENCE-ALPES-COTE D'AZUR","Polygone",6.5576587,44.784054,"J32 - Métallurgie de l'aluminium"]
["SSP000564101",null,"Ancien site minier uranifère - BOIS DES FAYES",null,"Clôturée",null,null,"Clôturée","63027","BAFFIE","PUY-DE-DOME","AUVERGNE-RHONE-ALPES","Polygone",3.8066568,45.49037]
["SSP000564701",null,"SHELL",null,"Clôturée",null,null,"Clôturée","95288","GROSLAY","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.3619998,48.985374]
["SSP000565401","63.0050","COUZON (site Chabreloche)",null,"En cours",null,null,"En cours","63072","CHABRELOCHE","PUY-DE-DOME","AUVERGNE-RHONE-ALPES","Polygone",3.705529,45.876324,"J53 - Travail des métaux, chaudronnerie, poudres"]
["SSP000565901",null,"Ancienne décharge de Lizimonic",null,"Clôturée",null,null,"Clôturée","29146","MELGVEN","FINISTERE","BRETAGNE","Polygone",-3.8748097,47.931026]
["SSP000566101","95.0061","ETAIN SOUDURE",null,"En cours",null,null,"En cours","95612","LE THILLAY","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.4777617,48.997826,"J5 - Fonderie et travail des métaux"]
["SSP000566701","63.0002","Ancienne Usine A Gaz",null,"En cours",null,null,"En cours","63040","BILLOM","PUY-DE-DOME","AUVERGNE-RHONE-ALPES","Polygone",3.332493,45.723186,"J1 - Cokéfaction, usines à gaz"]
["SSP000567101","63.0009","Ancienne décharge ROUSSEL UCLAF",null,"En cours",null,null,"En cours","63207","MARAT","PUY-DE-DOME","AUVERGNE-RHONE-ALPES","Polygone",3.700392,45.65768,"K36 - Mise en décharge"]
["SSP000567601","63.0062","ZAC de Claveloux",null,"En cours",null,null,"En cours","63113","CLERMONT FERRAND","PUY-DE-DOME","AUVERGNE-RHONE-ALPES","Polygone",3.1338708,45.77798]
["SSP000568301","63.0034","Anciens Ets MARCHEPOIL SA",null,"En cours",null,null,"En cours","63430","THIERS","PUY-DE-DOME","AUVERGNE-RHONE-ALPES","Polygone",3.552481,45.853516,"H13 - Traitement de surface"]
["SSP000568601","63.0042","Station service TOTAL \"Relais Anatole FRANCE\"",null,"Clôturée",null,"2016-10-13","Clôturée","63113","CLERMONT FERRAND","PUY-DE-DOME","AUVERGNE-RHONE-ALPES","Polygone",3.1070821,45.777832]
["SSP000568901","03.0058","SEP (décharge)",null,"En cours",null,null,"En cours","03098","DESERTINES","ALLIER","AUVERGNE-RHONE-ALPES","Polygone",2.6103625,46.35513]
["SSP000569501","76.0035","Ancienne usine à gaz d'Etretat",null,"En cours",null,null,"En cours","76254","ETRETAT","SEINE-MARITIME","NORMANDIE","Polygone",0.21176976,49.703644,"J1 - Cokéfaction, usines à gaz"]
["SSP000569701","76.0128","Ancienne décharge de Lanquetot",null,"En cours",null,null,"En cours","76382","LANQUETOT","SEINE-MARITIME","NORMANDIE","Polygone",0.5149646,49.57063,"K21 - Décharges d'ordures ménagères"]
["SSP000570201",null,"Ancienne décharge de Mez Gouëz",null,"Clôturée",null,null,"Clôturée","22168","PERROS GUIREC","COTES-D'ARMOR","BRETAGNE","Polygone",-3.476292,48.806316]
["SSP000570701",null,"Dépôt de scories de la centrale thermique",null,"Clôturée",null,null,"Clôturée","04197","SAINTE TULLE","ALPES-DE-HAUTE-PROVENCE","PROVENCE-ALPES-COTE D'AZUR","Polygone",5.7875338,43.77576]
["SSP000571601",null,"Ancienne décharge de Déhault",null,"Clôturée",null,null,"Clôturée","72114","DEHAULT","SARTHE","PAYS DE LA LOIRE","Polygone",0.5782752,48.210876]
["SSP000572101",null,"Ancienne décharge de CHASSILLE",null,"Clôturée",null,null,"Clôturée","72070","CHASSILLE","SARTHE","PAYS DE LA LOIRE","Polygone",-0.123619296,48.02118]
["SSP000572601",null,"Ancienne décharge de Luceau",null,"Clôturée",null,null,"Clôturée","72173","LUCEAU","SARTHE","PAYS DE LA LOIRE","Polygone",0.39447767,47.718834]
["SSP000572801",null,"Ancienne décharge du GRAND-LUCE",null,"Clôturée",null,null,"Clôturée","72143","LE GRAND LUCE","SARTHE","PAYS DE LA LOIRE","Polygone",0.46166578,47.880386]
["SSP000573301",null,"Ancienne décharge de BEAUMONT",null,"Clôturée",null,null,"Clôturée","72029","BEAUMONT SUR SARTHE","SARTHE","PAYS DE LA LOIRE","Polygone",0.11968245,48.218952]
["SSP000573701",null,"ancienne décharge de Livet",null,"Clôturée",null,null,"Clôturée","72164","LIVET EN SAOSNOIS","SARTHE","PAYS DE LA LOIRE","Polygone",0.20180207,48.360012]
["SSP000573801",null,"Ancienne décharge d'Asse",null,"Clôturée",null,null,"Clôturée","72011","ASSE LE BOISNE","SARTHE","PAYS DE LA LOIRE","Polygone",-0.017723069,48.31961]
["SSP000574201",null,"ancienne décharge de Chemiré",null,"Clôturée",null,null,"Clôturée","72075","CHEMIRE LE GAUDIN","SARTHE","PAYS DE LA LOIRE","Polygone",-0.016354073,47.932827]
["SSP000574701",null,"OIL FRANCE",null,"Clôturée",null,null,"Clôturée","95306","HERBLAY","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.1870117,49.00276]
["SSP000575601",null,"Ancien site minier uranifère - EMENTRUERE",null,"Clôturée",null,null,"Clôturée","85109","LES HERBIERS","VENDEE","PAYS DE LA LOIRE","Polygone",-1.0171729,46.88682]
["SSP000575901",null,"Ancien site minier uranifère - GODARDIERE (LA)",null,"Clôturée",null,null,"Clôturée","85017","BEAUREPAIRE","VENDEE","PAYS DE LA LOIRE","Polygone",-1.070008,46.906918]
["SSP000576601",null,"Ancienne Carrière d'Amiante Canari (1)",null,"Clôturée",null,null,"Clôturée","2B058","CANARI","HAUTE-CORSE","CORSE","Polygone",9.326436,42.819763,"F32 - Carrières"]
["SSP000577201",null,"Société Nouvelle du Radium (laboratoire d'essai)",null,"Clôturée",null,null,"Clôturée","91272","GIF SUR YVETTE","ESSONNE","ILE-DE-FRANCE","Polygone",2.1336684,48.69511]
["SSP000577901",null,"Quai transit SAN LORENZO",null,"Clôturée",null,null,"Clôturée","2B304","SAN LORENZO","HAUTE-CORSE","CORSE","Polygone",9.259463,42.40063,"K21 - Décharges d'ordures ménagères"]
["SSP000578001",null,"SCA UVIB - cave Aghione Samuletto",null,"Clôturée",null,null,"Clôturée","2B346","VESCOVATO","HAUTE-CORSE","CORSE","Polygone",9.463045,42.504025,null,null,"01.1G - Viticulture"]
["SSP000578601",null,"ancienne décharge de MAISONCELLES",null,"Clôturée",null,null,"Clôturée","72178","MAISONCELLES","SARTHE","PAYS DE LA LOIRE","Polygone",0.5761998,47.939514]
["SSP000579001",null,"ancienne décharge de SAINT-MICHEL-DE-CHAVAIGNES",null,"Clôturée",null,null,"Clôturée","72303","SAINT MICHEL DE CHAVAIGNES","SARTHE","PAYS DE LA LOIRE","Polygone",0.5842432,48.013332]
["SSP000579301",null,"ancienne décharge de SILLE-LE-GUILLAUME",null,"Clôturée",null,null,"Clôturée","72145","LE GREZ","SARTHE","PAYS DE LA LOIRE","Polygone",-0.16196063,48.177917]
["SSP000579501",null,"ancienne décharge de BERNAY",null,"Clôturée",null,null,"Clôturée","72033","BERNAY EN CHAMPAGNE","SARTHE","PAYS DE LA LOIRE","Polygone",-0.048229925,48.06912]
["SSP000580301",null,"ancienne décharge de Brûlon",null,"Clôturée",null,null,"Clôturée","72050","BRULON","SARTHE","PAYS DE LA LOIRE","Polygone",-0.23135678,47.97399]
["SSP000581201",null,"CET 2 Sari d'Orcino",null,"Clôturée",null,null,"Clôturée","2A270","SARI D'ORCINO","CORSE-DU-SUD","CORSE","Polygone",8.83617,42.053642,"K36 - Mise en décharge"]
["SSP000581601",null,"Stériles miniers (fiche 44A-114)",null,"Clôturée",null,null,"Clôturée","44211","LA TURBALLE","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Polygone",-2.4690342,47.358555]
["SSP000581801",null,"Stériles miniers (fiche 44A-175)",null,"Clôturée",null,null,"Clôturée","44069","GUERANDE","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Polygone",-2.4416637,47.35187]
["SSP000582201",null,"Stériles miniers (fiche 85A-L.A.19)",null,"Clôturée",null,null,"Clôturée","44100","MONNIERES","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Polygone",-1.3586496,47.113865]
["SSP000582701",null,"Stériles miniers (fiche 85A-L.A.238)",null,"Clôturée",null,null,"Clôturée","44063","GETIGNE","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Polygone",-1.2146525,47.08875]
["SSP000583001",null,"Stériles miniers (85A-L.A.261)",null,"Clôturée",null,null,"Clôturée","44063","GETIGNE","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Polygone",-1.2018347,47.08295]
["SSP000583201",null,"Stériles miniers (fiche 85A-L.A.264)",null,"Clôturée",null,null,"Clôturée","44063","GETIGNE","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Polygone",-1.1920362,47.078003]
["SSP000583801",null,"Stériles miniers (fiche 85A-M.L.155)",null,"Clôturée",null,null,"Clôturée","49273","SAINT CRESPIN SUR MOINE","MAINE-ET-LOIRE","PAYS DE LA LOIRE","Polygone",-1.1888758,47.106327]
["SSP000584201",null,"Stériles miniers (fiche 85A-M.L.172)",null,"Clôturée",null,null,"Clôturée","49273","SAINT CRESPIN SUR MOINE","MAINE-ET-LOIRE","PAYS DE LA LOIRE","Polygone",-1.2181952,47.10414]
["SSP000584701",null,"Stériles miniers (fiche 85A-M.L.22)",null,"Clôturée",null,null,"Clôturée","49285","SAINT GERMAIN SUR MOINE","MAINE-ET-LOIRE","PAYS DE LA LOIRE","Polygone",-1.1157435,47.133183]
["SSP000584801",null,"Stériles miniers (fiche 85A-M.L.267)",null,"Clôturée",null,null,"Clôturée","49260","LA ROMAGNE","MAINE-ET-LOIRE","PAYS DE LA LOIRE","Polygone",-1.0135106,47.056606]
["SSP000585201",null,"Stériles miniers (fiche 85A-M.L.400)",null,"Clôturée",null,null,"Clôturée","49099","CHOLET","MAINE-ET-LOIRE","PAYS DE LA LOIRE","Polygone",-0.8870597,47.010098]
["SSP000585701",null,"Stériles miniers (fiche 85A-V.21)",null,"Clôturée",null,null,"Clôturée","85151","MORTAGNE SUR SEVRE","VENDEE","PAYS DE LA LOIRE","Polygone",-0.9562672,46.98473]
["SSP000586001",null,"Stériles miniers (fiche 85A-V.81)",null,"Clôturée",null,null,"Clôturée","85296","TREIZE VENTS","VENDEE","PAYS DE LA LOIRE","Point",0.0,0.0]
["SSP000586301","69.0353","Station-service ELF à Tassin-la-Demi-Lune",null,"Clôturée",null,"2019-03-01","Clôturée","69244","TASSIN LA DEMI LUNE","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.771876,45.75533,"L23 - Détail de carburants"]
["SSP000587101","60.0086","Isollex",null,"En cours",null,null,"En cours","60508","PONTPOINT","OISE","HAUTS-DE-FRANCE","Polygone",2.6826928,49.310333,"G14 - Fabrication d'autres matériaux de construction"]
["SSP000587401",null,"MUSSO",null,"Clôturée",null,null,"Clôturée","2A271","SARROLA CARCOPINO","CORSE-DU-SUD","CORSE","Polygone",8.827173,41.975136,"K36 - Mise en décharge"]
["SSP000588301","72.0053","SOA - Société Orléanaise d'Assainissement (ex-SCC)",null,"En cours",null,null,"En cours","72181","LE MANS","SARTHE","PAYS DE LA LOIRE","Polygone",0.18714845,47.962013]
["SSP000588401","72.0044","Soufflet agriculture (ex-Hurel Arc)",null,"En cours",null,null,"En cours","72386","YVRE L'EVEQUE","SARTHE","PAYS DE LA LOIRE","Polygone",0.28369677,48.008255,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000589001",null,"Ets LINET (ex Société des Engrais de Roubaix)",null,"Clôturée",null,null,"Clôturée","80677","ROISEL","SOMME","HAUTS-DE-FRANCE","Polygone",3.0972822,49.950203]
["SSP000593801","69.0386","Le nouveau garage",null,"Clôturée",null,"2018-05-03","Clôturée","69152","PIERRE BENITE","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.8270407,45.69568]
["SSP000594601","76.0384","Station-service SARL DELABAR",null,"En cours",null,null,"En cours","76235","ENVERMEU","SEINE-MARITIME","NORMANDIE","Polygone",1.2636126,49.89584]
["SSP000595401","69.0325","Sylviana Lightning International (SLI France)",null,"En cours",null,null,"En cours","69123","LYON","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.798384,45.777737,"H1 - Mécanique, électrique, traitement de surface"]
["SSP000596801",null,"ZAC Lyon Confluence",null,"Clôturée",null,null,"Clôturée","69123","LYON","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.817115,45.74141,"J1 - Cokéfaction, usines à gaz"]
["SSP000596804","69.0334","ZAC Lyon Confluence",null,"En cours",null,null,"En cours","69123","LYON","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.8174067,45.742622,"J1 - Cokéfaction, usines à gaz"]
["SSP000597001",null,"Usine de Navarre",null,"Clôturée",null,null,"Clôturée","27229","EVREUX","EURE","NORMANDIE","Polygone",1.119754,49.015667]
["SSP000597301","27.0044","PERFECT CIRCLE EUROPE",null,"En cours",null,null,"En cours","27391","MARCILLY SUR EURE","EURE","NORMANDIE","Polygone",1.3412226,48.823334,"J35 - Autres métaux non ferreux (métallurgie des)"]
["SSP000597801","27.0105","HERISSEY",null,"En cours",null,null,"En cours","27229","EVREUX","EURE","NORMANDIE","Polygone",1.1435591,49.000835]
["SSP000598401","85.0021","ARB",null,"En cours",null,null,"En cours","85271","SAINT SULPICE EN PAREDS","VENDEE","PAYS DE LA LOIRE","Polygone",-0.8325772,46.607265]
["SSP000598901","54.0144","MC CHROMAGE",null,"En cours",null,null,"En cours","54395","NANCY","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",6.191564,48.689]
["SSP000599501",null,"ESSO S.A.F",null,"Clôturée",null,null,"Clôturée","91667","VILLEMOISSON SUR ORGE","ESSONNE","ILE-DE-FRANCE","Polygone",2.3382874,48.656303]
["SSP000601101",null,"SCA VALFRANCE",null,"Clôturée",null,null,"Clôturée","77131","COULOMMIERS","SEINE-ET-MARNE","ILE-DE-FRANCE","Polygone",3.0848026,48.80359,"B15 - Stockage de céréales"]
["SSP000601601","85.0042","BUTAGAZ TRANSITION",null,"En cours",null,null,"En cours","85108","L'HERBERGEMENT","VENDEE","PAYS DE LA LOIRE","Polygone",-1.3744425,46.90512]
["SSP000605201",null,"Ancienne décharge d'Apremont",null,"Clôturée",null,null,"Clôturée","85006","APREMONT","VENDEE","PAYS DE LA LOIRE","Polygone",-1.7721951,46.744633]
["SSP000606301",null,"Ancienne décharge de Mareuil-sur-Lay-Dissais",null,"Clôturée",null,null,"Clôturée","85135","MAREUIL SUR LAY DISSAIS","VENDEE","PAYS DE LA LOIRE","Polygone",-1.22281,46.54319]
["SSP000606801",null,"Ancienne décharge de Saint-Malô-du-Bois",null,"Clôturée",null,null,"Clôturée","85240","SAINT MALO DU BOIS","VENDEE","PAYS DE LA LOIRE","Polygone",-0.90335214,46.920624]
["SSP000607301",null,"Ancienne décharge de Sallertaine",null,"Clôturée",null,null,"Clôturée","85280","SALLERTAINE","VENDEE","PAYS DE LA LOIRE","Polygone",-1.9195384,46.886494]
["SSP000608301",null,"Décharge de Lugo di Nazza",null,"Clôturée",null,null,"Clôturée","2B149","LUGO DI NAZZA","HAUTE-CORSE","CORSE","Polygone",9.310258,42.09279,"K36 - Mise en décharge"]
["SSP000608801",null,"Décharge de Calenzana",null,"Clôturée",null,null,"Clôturée","2B049","CALENZANA","HAUTE-CORSE","CORSE","Polygone",8.825627,42.518425,"K36 - Mise en décharge"]
["SSP000609501",null,"Décharge d’Occhiatana",null,"Clôturée",null,null,"Clôturée","2B182","OCCHIATANA","HAUTE-CORSE","CORSE","Polygone",8.996407,42.60706,"K36 - Mise en décharge"]
["SSP000613401","77.0073","WEBERT (ex CHARGERAUD)","WEBERT (ex CHARGERAUD)","En cours",null,null,"En cours","77333","NEMOURS","SEINE-ET-MARNE","ILE-DE-FRANCE","Polygone",2.694725,48.270264]
["SSP000615001","77.0078","Scierie d'Ecuelle","SCIERIE d'ECUELLES","Clôturée",null,null,"Clôturée","77316","MORET SUR LOING","SEINE-ET-MARNE","ILE-DE-FRANCE","Polygone",2.8282342,48.369877,"C13 - Traitement du bois"]
["SSP000616901","77.0157","Société BRIE CHAMPAGNE ETHANOL Bassin de stockage",null,"Clôturée",null,null,"Clôturée","77379","PROVINS","SEINE-ET-MARNE","ILE-DE-FRANCE","Polygone",3.2252696,48.578285]
["SSP000618901","77.0082","Raffinerie de BOURRON","Raffinerie de BOURRON (ancien site et mare)","En cours",null,null,"En cours","77048","BOURRON MARLOTTE","SEINE-ET-MARNE","ILE-DE-FRANCE","Polygone",2.6906,48.33233]
["SSP000619801",null,"Ancienne décharge \"La Garenne\"",null,"Clôturée",null,null,"Clôturée","85042","CHAILLE LES MARAIS","VENDEE","PAYS DE LA LOIRE","Polygone",-1.0257748,46.408947]
["SSP000620701","85.0036","PROLIFER RECYCLING",null,"En cours",null,null,"En cours","85092","FONTENAY LE COMTE","VENDEE","PAYS DE LA LOIRE","Polygone",-0.7942122,46.44511,"K5 - Récupération, dépôts de ferrailles"]
["SSP000621001","85.0007","Agences clientèle et d'exploitation d'EDF / GDF (ex-USINE A GAZ)",null,"En cours",null,null,"En cours","85194","LES SABLES D'OLONNE","VENDEE","PAYS DE LA LOIRE","Polygone",-1.7784625,46.49843,"J1 - Cokéfaction, usines à gaz"]
["SSP000621301",null,"Ancienne décharge Le Tablier",null,"Clôturée",null,null,"Clôturée","85285","LE TABLIER","VENDEE","PAYS DE LA LOIRE","Polygone",-1.3179386,46.550106]
["SSP000621901",null,"Décharge de Peri",null,"Clôturée",null,null,"Clôturée","2A209","PERI","CORSE-DU-SUD","CORSE","Polygone",8.902493,42.00445,"K36 - Mise en décharge"]
["SSP000622201",null,"Décharge d’Evisa",null,"Clôturée",null,null,"Clôturée","2A108","EVISA","CORSE-DU-SUD","CORSE","Polygone",8.797328,42.24242,"K36 - Mise en décharge"]
["SSP000622501",null,"Décharge d’Orto",null,"Clôturée",null,null,"Clôturée","2A196","ORTO","CORSE-DU-SUD","CORSE","Polygone",8.927983,42.17826,"K36 - Mise en décharge"]
["SSP000623001",null,"Décharge de Grosseto",null,"Clôturée",null,null,"Clôturée","2A130","GROSSETO PRUGNA","CORSE-DU-SUD","CORSE","Polygone",8.961073,41.86814,"K21 - Décharges d'ordures ménagères"]
["SSP000623401",null,"Décharge de Tolla",null,"Clôturée",null,null,"Clôturée","2A326","TOLLA","CORSE-DU-SUD","CORSE","Polygone",8.990224,41.972885,"K36 - Mise en décharge"]
["SSP000624801",null,"CET 2 Zicavo (site 4)",null,"Clôturée",null,null,"Clôturée","2A359","ZICAVO","CORSE-DU-SUD","CORSE","Polygone",9.138978,41.928165,"K36 - Mise en décharge"]
["SSP000625901","85.0030","SACHADIS",null,"En cours",null,null,"En cours","85194","LES SABLES D'OLONNE","VENDEE","PAYS DE LA LOIRE","Polygone",-1.8030609,46.497494,"L13 - Entrepôts de produits dangereux"]
["SSP000626101",null,"Ancien CET \"La Loge\"",null,"Clôturée",null,null,"Clôturée","85178","LE POIRE SUR VIE","VENDEE","PAYS DE LA LOIRE","Polygone",-1.4378775,46.746696]
["SSP000628101","44.0138","TRANSPORTS BEZIAU",null,"En cours",null,null,"En cours","44114","ORVAULT","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Polygone",-1.6479381,47.260838]
["SSP000632301","44.0148","LAURY-CHALONGES DIS SAS",null,"En cours",null,null,"En cours","44009","BASSE GOULAINE","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Polygone",-1.4681658,47.18747,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000632501","44.0149","NORMINTER SNC",null,"En cours",null,null,"En cours","44212","VALLET","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Polygone",-1.2748914,47.16386,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000634901","57.0193","SIB ADR",null,"En cours",null,null,"En cours","57097","BOULAY MOSELLE","MOSELLE","GRAND EST","Polygone",6.488724,49.18103]
["SSP000635601",null,"Ancienne décharge de Chauche",null,"Clôturée",null,null,"Clôturée","85064","CHAUCHE","VENDEE","PAYS DE LA LOIRE","Polygone",-1.2424083,46.84706]
["SSP000636401",null,"Agence EDF-GDF Services de Vendée (ex-USINE A GAZ)",null,"Clôturée",null,null,"Clôturée","85222","SAINT GILLES CROIX DE VIE","VENDEE","PAYS DE LA LOIRE","Polygone",-1.9392862,46.69867]
["SSP000637701",null,"Ancien CET \"La pointe des corbeaux\"",null,"Clôturée",null,null,"Clôturée","85113","L'ILE D'YEU","VENDEE","PAYS DE LA LOIRE","Polygone",-2.289505,46.695427]
["SSP000638401","44.0081","COLARENA PRESQU'ILE",null,"En cours",null,null,"En cours","44021","BOURGNEUF EN RETZ","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Polygone",-1.8776503,47.022743]
["SSP000639301",null,"Ancienne décharge de La Planche",null,"Clôturée",null,null,"Clôturée","44127","LA PLANCHE","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Polygone",-1.4313987,47.010616]
["SSP000640001",null,"Ancienne décharge de Le Loroux-Botterau",null,"Clôturée",null,null,"Clôturée","44084","LE LOROUX BOTTEREAU","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Polygone",-1.360553,47.225742]
["SSP000640201",null,"Ancienne décharge de Boussay",null,"Clôturée",null,null,"Clôturée","44022","BOUSSAY","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Polygone",-1.138681,47.04992]
["SSP000641001","44.0053","TEINTURERIE RICHARD",null,"En cours",null,null,"En cours","44110","NORT SUR ERDRE","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Polygone",-1.4944972,47.439228,"E3 - Laveries, blanchisseries, pressing"]
["SSP000641401","44.0080","SARL BONAMY",null,"En cours",null,null,"En cours","44213","VARADES","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Polygone",-1.0268798,47.46716]
["SSP000641901","44.0105","SITA OUEST (DIB) (ex SEDIMO)",null,"En cours",null,null,"En cours","44089","MALVILLE","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Polygone",-1.8085318,47.33476,"K35 - Regroupement, reconditionnement de déchets"]
["SSP000642001","44.0106","FERS",null,"En cours",null,null,"En cours","44143","REZE","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Polygone",-1.5382181,47.158604,"K52 - Dépôts de ferraille"]
["SSP000642701","44.0128","Station ELF - Relais Caltex",null,"En cours",null,null,"En cours","44154","SAINT BREVIN LES PINS","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Polygone",-2.1682572,47.265995,"L23 - Détail de carburants"]
["SSP000643001","44.0100","POINT P TROUILLARD",null,"En cours",null,null,"En cours","44109","NANTES","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Polygone",-1.5355457,47.216938]
["SSP000643701","44.0152","ATELIERS BRETONS DE RÉALISATIONS FERROVIAIRES Industrie (ABRFi)",null,"En cours",null,null,"En cours","44036","CHATEAUBRIANT","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Polygone",-1.4010261,47.70444,"H - Mécanique, traitements des surfaces"]
["SSP000644001","94.0043","YOPLAIT - SODIAAL",null,"En cours",null,null,"En cours","94041","IVRY SUR SEINE","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.3908982,48.819523]
["SSP000644301","44.0082","LEDUC (Bazouin)",null,"En cours",null,null,"En cours","44186","SAINTE PAZANNE","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Polygone",-1.8084822,47.10604,"C13 - Traitement du bois"]
["SSP000644901","44.0124","ALSTOM (halls 7 à 10)",null,"En cours",null,null,"En cours","44109","NANTES","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Polygone",-1.5628825,47.206127]
["SSP000646701","69.0396","COVED",null,"En cours",null,null,"En cours","69100","IRIGNY","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.830632,45.68676,"K36 - Mise en décharge"]
["SSP000646801","27.0045","RUBBERIA",null,"En cours",null,null,"En cours","27438","NONANCOURT","EURE","NORMANDIE","Polygone",1.2118467,48.76419,"D72 - Transformation des matières plastiques"]
["SSP000647301","27.0040","Ancienne fonderie de Vernon",null,"En cours",null,null,"En cours","27681","VERNON","EURE","NORMANDIE","Polygone",1.4726604,49.10099,"J51 - Fonderie des métaux ferreux"]
["SSP000649201","80.0033","Centre EDF GDF Services - Pays de Somme",null,"En cours",null,null,"En cours","80368","FRIVILLE ESCARBOTIN","SOMME","HAUTS-DE-FRANCE","Polygone",1.5446745,50.08517,"J1 - Cokéfaction, usines à gaz"]
["SSP000651801","77.0145","ZAC de l'Ancre de Lune Site Saint-Fiacre / Verdun - Ancienne station service AVIA-ERG",null,"En cours",null,null,"En cours","77475","TRILPORT","SEINE-ET-MARNE","ILE-DE-FRANCE","Polygone",2.9546316,48.959343,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000652001","60.0043","Centre EDF GDF Services de Cergy",null,"En cours",null,null,"En cours","60176","CREPY EN VALOIS","OISE","HAUTS-DE-FRANCE","Polygone",2.8932889,49.232285,"J1 - Cokéfaction, usines à gaz"]
["SSP000657301",null,"ancienne décharge de Marillais",null,"Clôturée",null,null,"Clôturée","49190","LE MARILLAIS","MAINE-ET-LOIRE","PAYS DE LA LOIRE","Polygone",-1.073458,47.35869]
["SSP000658201","14.0041","Dépôt de résidus de broyage à Soumont Saint Quentin",null,"En cours",null,null,"En cours","14678","SOUMONT SAINT QUENTIN","CALVADOS","NORMANDIE","Polygone",-0.25532472,48.979515,"K3 - Traitement de déchets industriels"]
["SSP000658801","14.0025","Ancienne usine à gaz",null,"Clôturée",null,"2010-10-21","Clôturée","14333","HONFLEUR","CALVADOS","NORMANDIE","Polygone",0.24456921,49.41471,"J1 - Cokéfaction, usines à gaz"]
["SSP000658901","14.0058","La Maison du Pneu - Yann BOURQUIN",null,"En cours",null,null,"En cours","14762","VIRE","CALVADOS","NORMANDIE","Polygone",-0.88570166,48.837624,"L23 - Détail de carburants"]
["SSP000659401","59.0613","SN LADOE SAS",null,"En cours",null,null,"En cours","59599","TOURCOING","NORD","HAUTS-DE-FRANCE","Polygone",3.1407728,50.719734,"D72 - Transformation des matières plastiques"]
["SSP000660601","27.0076","BATA (UNIMARCEAU)",null,"En cours",null,null,"En cours","27562","SAINT MARCEL","EURE","NORMANDIE","Polygone",1.4609194,49.110943]
["SSP000661201",null,"LA SOIE",null,"Clôturée",null,null,"Clôturée","27016","LES ANDELYS","EURE","NORMANDIE","Polygone",1.4121495,49.248127]
["SSP000662001",null,"Site SNCF",null,"Clôturée",null,null,"Clôturée","76114","BOLBEC","SEINE-MARITIME","NORMANDIE","Polygone",0.46726835,49.57819]
["SSP000662401","59.0292","AGENCE D'EXPLOITATION GDF",null,"En cours",null,null,"En cours","59360","LOOS","NORD","HAUTS-DE-FRANCE","Polygone",3.003873,50.612072,"J1 - Cokéfaction, usines à gaz"]
["SSP000690001","44.0159","NLB AUTOMOBILES",null,"En cours",null,null,"En cours","44186","SAINTE PAZANNE","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Polygone",-1.8164008,47.098446,"L23 - Détail de carburants"]
["SSP000691001","44.0161","TROUILLARD POINT P - ancien site LAPEYRE",null,"En cours",null,null,"En cours","44190","SAINT SEBASTIEN SUR LOIRE","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Polygone",-1.496493,47.192677]
["SSP000691301","44.0162","SNCF",null,"En cours",null,null,"En cours","44109","NANTES","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Polygone",-1.5699708,47.203304,"L - Entreposage, transport, commerce"]
["SSP000691701",null,"Ancienne décharge des Piarmes",null,"Clôturée",null,null,"Clôturée","44020","BOUGUENAIS","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Polygone",-1.6121637,47.174145]
["SSP000692201",null,"Ancienne décharge de Vincent Gâche",null,"Clôturée",null,null,"Clôturée","44109","NANTES","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Polygone",-1.5371135,47.208534]
["SSP000692701",null,"CFTS",null,"Clôturée",null,null,"Clôturée","44143","REZE","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Polygone",-1.562282,47.196667]
["SSP000693101",null,"Ancien Centre d'Enfouissement Technique de la Tougas",null,"Clôturée",null,null,"Clôturée","44162","SAINT HERBLAIN","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Polygone",-1.6540468,47.20091]
["SSP000693701",null,"Ancienne décharge de Bouguenais",null,"Clôturée",null,null,"Clôturée","44020","BOUGUENAIS","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Polygone",-1.6127893,47.167606]
["SSP000694301","27.0068","CARTONNERIE DE PONT-AUDEMER (CPA)",null,"En cours",null,null,"En cours","27467","PONT AUDEMER","EURE","NORMANDIE","Polygone",0.50825053,49.359318,null,null,null,"17.21B - Fabrication de cartonnages"]
["SSP000694701",null,"Ancienne décharge de Saint-Michel-Chef-Chef",null,"Clôturée",null,null,"Clôturée","44182","SAINT MICHEL CHEF CHEF","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Polygone",-2.089303,47.190838]
["SSP000694801",null,"Ancienne décharge de Vue",null,"Clôturée",null,null,"Clôturée","44220","VUE","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Polygone",-1.8715429,47.205708]
["SSP000695201","44.0127","VIDIBO",null,"En cours",null,null,"En cours","44217","VIGNEUX DE BRETAGNE","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Polygone",-1.7378535,47.327938]
["SSP000695701","44.0042","Agence clientèle d'EDF / GDF Services (ex-USINE A GAZ)",null,"En cours",null,null,"En cours","44055","LA BAULE ESCOUBLAC","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Polygone",-2.3959434,47.287956,"J1 - Cokéfaction, usines à gaz"]
["SSP000696001","27.0066","COSTIL parcelle 141 (Maître Diesbecq)",null,"En cours",null,null,"En cours","27467","PONT AUDEMER","EURE","NORMANDIE","Polygone",0.49853292,49.360847,"E2 - Industrie des cuirs et peaux, tannerie"]
["SSP000696201","27.0067","COSTIL Maître HESS",null,"En cours",null,null,"En cours","27467","PONT AUDEMER","EURE","NORMANDIE","Polygone",0.5002734,49.36099,"E2 - Industrie des cuirs et peaux, tannerie"]
["SSP000696701","27.0020","Ancienne agence d'exploitation d'EDF / GDF",null,"En cours",null,null,"En cours","27116","BRIONNE","EURE","NORMANDIE","Polygone",0.7196339,49.208706]
["SSP000697201","27.0003","DEPOT C.B.L. (EX MATTHYS)",null,"En cours",null,null,"En cours","27493","ROMILLY SUR ANDELLE","EURE","NORMANDIE","Polygone",1.2592615,49.341717]
["SSP000697601","27.0069","Société des Carrières et Sablières HEROUARD",null,"En cours",null,null,"En cours","27599","SAINT PIERRE LA GARENNE","EURE","NORMANDIE","Polygone",1.384955,49.15712]
["SSP000697701","27.0068","CARTONNERIE DE PONT-AUDEMER (CPA)",null,"En cours",null,null,"En cours","27467","PONT AUDEMER","EURE","NORMANDIE","Polygone",0.5098933,49.359253,"C22 - Fabrication de papiers et carton"]
["SSP000698101","44.0165","MASUY",null,"En cours",null,null,"En cours","44047","COUERON","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Polygone",-1.675015,47.24252]
["SSP000698601","27.0036","Agence EDF-GDF de Verneuil-sur-Avre",null,"En cours",null,null,"En cours","27679","VERNEUIL SUR AVRE","EURE","NORMANDIE","Polygone",0.9453241,48.739853,"J1 - Cokéfaction, usines à gaz"]
["SSP000698901",null,"Ancien garage BILLAUD",null,"Clôturée",null,null,"Clôturée","85166","OLONNE SUR MER","VENDEE","PAYS DE LA LOIRE","Polygone",-1.8077742,46.550682]
["SSP000699501",null,"STOCKOUEST-ZONE C",null,"Clôturée",null,null,"Clôturée","44184","SAINT NAZAIRE","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Polygone",-2.2026892,47.282856]
["SSP000700001","14.0028","Ancienne usine à gaz",null,"Clôturée",null,"2010-10-21","Clôturée","14699","TOUQUES","CALVADOS","NORMANDIE","Polygone",0.09270164,49.354954,"J1 - Cokéfaction, usines à gaz"]
["SSP000700501","14.0040","Dépôt de pneumatiques usagés",null,"En cours",null,null,"En cours","14011","ANCTOVILLE","CALVADOS","NORMANDIE","Polygone",-0.6772297,49.111732]
["SSP000701001","44.0012","ANCIEN DEPOT SHELL",null,"En cours",null,null,"En cours","44184","SAINT NAZAIRE","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Polygone",-2.1978703,47.293144,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000701101","50.0016","Truffert Lepesant",null,"En cours",null,null,"En cours","50129","CHERBOURG OCTEVILLE","MANCHE","NORMANDIE","Polygone",-1.6440833,49.647503,"J21 - Production de fontes (haut fourneau)"]
["SSP000701701","76.0118","SOCIETE ORGACHIM",null,"En cours",null,null,"En cours","76484","OISSEL","SEINE-MARITIME","NORMANDIE","Polygone",1.1059991,49.343773,"D3 - Chimie, phytosanitaire, pharmacie"]
["SSP000702701","44.0033","EX DEPOT ELF",null,"En cours",null,null,"En cours","44162","SAINT HERBLAIN","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Polygone",-1.6298366,47.194557,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000703001","76.0324","Docks 76",null,"En cours",null,null,"En cours","76540","ROUEN","SEINE-MARITIME","NORMANDIE","Polygone",1.0650413,49.44607]
["SSP000703401",null,"Bourderies_Ilots B à D",null,"Clôturée",null,null,"Clôturée","44143","REZE","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Polygone",-1.5656296,47.18968]
["SSP000704001",null,"Ancienne décharge de La Landelle",null,"Clôturée",null,null,"Clôturée","22308","SAINT JUVAT","COTES-D'ARMOR","BRETAGNE","Polygone",-2.0775876,48.354458]
["SSP000704501","44.0120","STATION DE DEBALLASTAGE (GPMNSN)",null,"En cours",null,null,"En cours","44184","SAINT NAZAIRE","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Polygone",-2.1959093,47.277264,"M - Divers et services"]
["SSP000705201",null,"Ancienne décharge",null,"Clôturée",null,null,"Clôturée","22342","TREBEDAN","COTES-D'ARMOR","BRETAGNE","Polygone",-2.1656597,48.394142]
["SSP000705401",null,"Décharge d'ordures ménagères",null,"Clôturée",null,null,"Clôturée","53196","SAINT AIGNAN DE COUPTRAIN","MAYENNE","PAYS DE LA LOIRE","Polygone",-0.2710032,48.463196]
["SSP000706201","44.0002","ANCIENNE CARRIERE DE PONTPIERRE",null,"En cours",null,null,"En cours","44162","SAINT HERBLAIN","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Polygone",-1.6372554,47.20976,"F32 - Carrières"]
["SSP000706701","49.0072","GUERIF Père et Fils",null,"En cours",null,null,"En cours","49278","SAINTE GEMMES SUR LOIRE","MAINE-ET-LOIRE","PAYS DE LA LOIRE","Polygone",-0.59192365,47.42723,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000707101","44.0008","SITE DE LA SOCIETE SOAF UNIT",null,"Clôturée",null,"2012-06-01","Clôturée","44051","DERVAL","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Polygone",-1.6316086,47.685867,"K36 - Mise en décharge"]
["SSP000707401",null,"Stériles miniers (fiche 85A-L.A.173)",null,"Clôturée",null,null,"Clôturée","85076","CUGAND","VENDEE","PAYS DE LA LOIRE","Polygone",-1.2836753,47.076572]
["SSP000707901",null,"Ancienne décharge brute",null,"Clôturée",null,null,"Clôturée","44005","ARTHON EN RETZ","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Polygone",-1.9541377,47.136528]
["SSP000708301",null,"Poste source électrique \"le marais\"",null,"Clôturée",null,null,"Clôturée","27562","SAINT MARCEL","EURE","NORMANDIE","Polygone",1.4665291,49.10298]
["SSP000711201","44.0167","MENANT Yvon - ancienne station-service ELAN",null,"En cours",null,null,"En cours","44072","HERBIGNAC","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Polygone",-2.3723462,47.390076,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000711301","78.0030","REFINAL (ex APROMETAL)",null,"En cours",null,null,"En cours","78498","POISSY","YVELINES","ILE-DE-FRANCE","Polygone",2.0486953,48.935665,"J52 - Fonderie des métaux non ferreux"]
["SSP000711701",null,"Ancienne déchetterie",null,"Clôturée",null,null,"Clôturée","44186","SAINTE PAZANNE","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Polygone",-1.8172144,47.094196]
["SSP000712001","27.0012","ancienne décharge de déchets industriels",null,"En cours",null,null,"En cours","27275","GAILLON","EURE","NORMANDIE","Polygone",1.3691002,49.161667]
["SSP000712601",null,"Ancienne décharge de Saint-Mars-de-Coutais",null,"Clôturée",null,null,"Clôturée","44178","SAINT MARS DE COUTAIS","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Polygone",-1.7515603,47.087765]
["SSP000712701","76.0255","Plastic OMNIUM",null,"En cours",null,null,"En cours","76647","SAINT ROMAIN DE COLBOSC","SEINE-MARITIME","NORMANDIE","Polygone",0.35871026,49.536602,"D72 - Transformation des matières plastiques"]
["SSP000713401","61.0012","AMCOR FLEXIBLES (SPEED)",null,"En cours",null,null,"En cours","61006","ARGENTAN","ORNE","NORMANDIE","Polygone",-0.025198994,48.734016]
["SSP000713701","33.0136","RULLEAU",null,"En cours",null,null,"En cours","33228","LANSAC","GIRONDE","NOUVELLE-AQUITAINE","Polygone",-0.5185108,45.07067]
["SSP000714201","87.0036","EMULSIONS ROUTIERES DU LIMOUSIN (ERL)",null,"En cours",null,null,"En cours","87085","LIMOGES","HAUTE-VIENNE","NOUVELLE-AQUITAINE","Polygone",1.222772,45.8294,"G22 - Centrales d'enrobés"]
["SSP000714601","14.0062","LCL crédit lyonnais",null,"En cours",null,null,"En cours","14047","BAYEUX","CALVADOS","NORMANDIE","Polygone",-0.7225106,49.280197]
["SSP000715501","49.0081","MOULINS BROCHET (ex-Minoterie FOURNIER)",null,"En cours",null,null,"En cours","49331","SEGRE","MAINE-ET-LOIRE","PAYS DE LA LOIRE","Polygone",-0.8883534,47.678967,"B1 - Industrie agro-alimentaire"]
["SSP000715801","49.0086","BREHERET",null,"En cours",null,null,"En cours","49218","MONTREVAULT","MAINE-ET-LOIRE","PAYS DE LA LOIRE","Polygone",-1.0203788,47.268044,"C13 - Traitement du bois"]
["SSP000716401",null,"Ancienne décharge de Grand Champ",null,"Clôturée",null,null,"Clôturée","44214","VAY","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Polygone",-1.7459232,47.511024]
["SSP000716501",null,"Ancien dépôt sauvage",null,"Clôturée",null,null,"Clôturée","44145","ROUANS","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Polygone",-1.8285321,47.133816]
["SSP000728801","95.0016","COLSON RECYCLAGE",null,"En cours",null,null,"En cours","95018","ARGENTEUIL","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.2390966,48.95288,"K5 - Récupération, dépôts de ferrailles"]
["SSP000730601","44.0155","ATELIERS NORMANDS",null,"En cours",null,null,"En cours","44109","NANTES","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Polygone",-1.5553681,47.227573]
["SSP000733301","95.0067","BORGERS",null,"En cours",null,null,"En cours","95487","PERSAN","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.2874494,49.149395,"D72 - Transformation des matières plastiques"]
["SSP000734301","18.0048","TWO CAST BERRY",null,"En cours",null,null,"En cours","18233","SAINT SATUR","CHER","CENTRE-VAL DE LOIRE","Polygone",2.8591273,47.34795,"J - Sidérurgie, métallurgie, coke"]
["SSP000736101","76.0225","POLYVER",null,"En cours",null,null,"En cours","76528","RIEUX","SEINE-MARITIME","NORMANDIE","Polygone",1.5778042,49.925972,"G15 - Industrie du verre"]
["SSP000740201","69.0242","PIV",null,"Clôturée",null,null,"Clôturée","69266","VILLEURBANNE","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.8962464,45.785713,"H - Mécanique, traitements des surfaces"]
["SSP000741101","69.0071","ZI Collonges (à supprimer)","Société des Pétroles Shell","En cours",null,null,"En cours","69063","COLLONGES AU MONT D'OR","RHONE","AUVERGNE-RHONE-ALPES","Polygone",4.849927,45.82196,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000741801","42.0020","GFD",null,"En cours",null,null,"En cours","42305","LA TALAUDIERE","LOIRE","AUVERGNE-RHONE-ALPES","Point",4.42483,45.468395]
["SSP000742101","42.0024","SIRA spur",null,"En cours",null,null,"En cours","42305","LA TALAUDIERE","LOIRE","AUVERGNE-RHONE-ALPES","Point",4.431663,45.473297,"K35 - Regroupement, reconditionnement de déchets"]
["SSP000742601","67.0029","BÜRKERT",null,"En cours",null,null,"En cours","67493","TRIEMBACH AU VAL","BAS-RHIN","GRAND EST","Point",7.2513967,47.437748,"H13 - Traitement de surface"]
["SSP000743201","63.0004","Ancien dépôt ESSO",null,"En cours",null,null,"En cours","63113","CLERMONT FERRAND","PUY-DE-DOME","AUVERGNE-RHONE-ALPES","Point",3.1462448,45.75837,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000743301","24.0005","ALVEA",null,"En cours",null,null,"En cours","24037","BERGERAC","DORDOGNE","NOUVELLE-AQUITAINE","Point",0.48548663,44.85207,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000743801","33.0039","YARA",null,"En cours",null,null,"En cours","33004","AMBES","GIRONDE","NOUVELLE-AQUITAINE","Point",-0.54637706,45.007954,"D36 - Fabrication des engrais"]
["SSP000744301","33.0045","SIAP",null,"En cours",null,null,"En cours","33032","BASSENS","GIRONDE","NOUVELLE-AQUITAINE","Point",-0.52981645,44.905308,"K3 - Traitement de déchets industriels"]
["SSP000744801","55.0010","LA MEUSIENNE  (ex SMCM)",null,"En cours",null,null,"En cours","55010","ANCERVILLE","MEUSE","GRAND EST","Point",5.006695,48.6194,"H13 - Traitement de surface"]
["SSP000745901","33.0057","SAPESO",null,"Clôturée",null,"2005-08-29","Clôturée","33063","BORDEAUX","GIRONDE","NOUVELLE-AQUITAINE","Polygone",-0.55288,44.85368,"H21 - Imprimerie, presse, édition"]
["SSP000746501","40.0028","LBC",null,"En cours",null,null,"En cours","40312","TARNOS","LANDES","NOUVELLE-AQUITAINE","Point",-1.5063616,43.532005]
["SSP000747001","33.0068","Station TOTAL FINA",null,"En cours",null,null,"En cours","33159","ETAULIERS","GIRONDE","NOUVELLE-AQUITAINE","Point",-0.5851525,45.22162,"L23 - Détail de carburants"]
["SSP000747901","33.0077","MANUSTOCK",null,"Clôturée",null,"2006-12-08","Clôturée","33527","LE TEICH","GIRONDE","NOUVELLE-AQUITAINE","Point",-1.0210818,44.634544,"C13 - Traitement du bois"]
["SSP000748001","33.0078","SFCME",null,"En cours",null,null,"En cours","33243","LIBOURNE","GIRONDE","NOUVELLE-AQUITAINE","Point",-0.23551913,44.94337,"H1 - Mécanique, électrique, traitement de surface"]
["SSP000748701","40.0012","MLPC",null,"En cours",null,null,"En cours","40151","LESGOR","LANDES","NOUVELLE-AQUITAINE","Point",-0.9119081,43.862854,"D33 - Pétrochimie carbochimie organique"]
["SSP000749201","40.0018","Société Pétrolière de Dépôts",null,"En cours",null,null,"En cours","40192","MONT DE MARSAN","LANDES","NOUVELLE-AQUITAINE","Point",-0.4645511,43.903267,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000749801","40.0027","LABAT MERLE",null,"En cours",null,null,"En cours","40284","SAINT VINCENT DE TYROSSE","LANDES","NOUVELLE-AQUITAINE","Point",-1.3020394,43.66312,"C12 - Produits en bois, ameublement (fabrication de)"]
["SSP000750001","40.0029","TIMAC AGRO",null,"En cours",null,null,"En cours","40312","TARNOS","LANDES","NOUVELLE-AQUITAINE","Point",-1.5063616,43.532005]
["SSP000750301","47.0008","EUTICALS (ex ARCHIMICA)",null,"En cours",null,null,"En cours","47032","BON ENCONTRE","LOT-ET-GARONNE","NOUVELLE-AQUITAINE","Point",0.6498586,44.207806,"D - Chimie, parachimie, pétrole"]
["SSP000750801","26.0010","IN SITU (ex BOULONNERIE CALIBREE)",null,"En cours",null,null,"En cours","26362","VALENCE","DROME","AUVERGNE-RHONE-ALPES","Point",4.885848,44.914616]
["SSP000751201","47.0017","Verrerie de Vianne",null,"En cours",null,null,"En cours","47318","VIANNE","LOT-ET-GARONNE","NOUVELLE-AQUITAINE","Point",0.31776187,44.21235,"G15 - Industrie du verre"]
["SSP000751401","64.0019","BONNET NEVE",null,"En cours",null,null,"En cours","64260","HENDAYE","PYRENEES-ATLANTIQUES","NOUVELLE-AQUITAINE","Point",-1.7601254,43.36381,"H - Mécanique, traitements des surfaces"]
["SSP000751801","85.0003","DEFONTAINE (TRAVAIL DES METAUX)",null,"En cours",null,null,"En cours","85039","LA BRUFFIERE","VENDEE","PAYS DE LA LOIRE","Point",-1.1785138,47.015053,"H1 - Mécanique, électrique, traitement de surface"]
["SSP000752301","47.0003","Décharge de Cadamas",null,"En cours",null,null,"En cours","47185","MONTAYRAL","LOT-ET-GARONNE","NOUVELLE-AQUITAINE","Point",0.98812103,44.470222,"J52 - Fonderie des métaux non ferreux"]
["SSP000752801","88.0003","NOVACARE (ANCIENNE DECHARGE DE LA PAPETERIE MOUGEOT)",null,"En cours",null,null,"En cours","88261","LAVAL SUR VOLOGNE","VOSGES","GRAND EST","Point",6.69467,48.19266,"C22 - Fabrication de papiers et carton"]
["SSP000753001","58.0002"," TRANSUNEL",null,"En cours",null,null,"En cours","58117","FOURCHAMBAULT","NIEVRE","BOURGOGNE-FRANCHE-COMTE","Point",3.0929108,47.015923,"H1 - Mécanique, électrique, traitement de surface"]
["SSP000753401","10.0004","VAL DE VEINE",null,"En cours",null,null,"En cours","10070","CELLES SUR OURCE","AUBE","GRAND EST","Point",4.4201484,48.069473,"K36 - Mise en décharge"]
["SSP000754001","26.0004","SOCIETE VIGNAL ARTRU",null,"En cours",null,null,"En cours","26064","CHABEUIL","DROME","AUVERGNE-RHONE-ALPES","Point",5.013466,44.908417,"H1 - Mécanique, électrique, traitement de surface"]
["SSP000754601","26.0001","DEPOT PETROLIER DE PORTES LES VALENCE ( D.P.P.V. ) - Pollution",null,"En cours",null,null,"En cours","26252","PORTES LES VALENCE","DROME","AUVERGNE-RHONE-ALPES","Point",4.8694243,44.8797,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000754801","38.0002","ACIERIE DE BONPERTUIS",null,"En cours",null,null,"En cours","38013","APPRIEU","ISERE","AUVERGNE-RHONE-ALPES","Point",5.528347,45.395763,"J22 - Production d'acier brut, aciéries"]
["SSP000755201","69.0219","Eurométal",null,"En cours",null,null,"En cours","69266","VILLEURBANNE","RHONE","AUVERGNE-RHONE-ALPES","Point",4.898541,45.779964,"K35 - Regroupement, reconditionnement de déchets"]
["SSP000755701","38.0010","USINE RHODIA Chimie, ancien stockage fûts (Gringalet)",null,"En cours",null,null,"En cours","38317","LE PONT DE CLAIX","ISERE","AUVERGNE-RHONE-ALPES","Point",5.7059703,45.130615]
["SSP000756001","38.0013","BLUESTAR Silicones - Décharge MSC",null,"En cours",null,null,"En cours","38468","SALAISE SUR SANNE","ISERE","AUVERGNE-RHONE-ALPES","Point",4.787675,45.35386]
["SSP000756201","93.0002","RHODIA CHIMIE ex SOCIETE CHIMIQUE DE LA COURNEUVE",null,"Clôturée",null,null,"Clôturée","93001","AUBERVILLIERS","SEINE-SAINT-DENIS","ILE-DE-FRANCE","Polygone",2.3698125,48.913456,"D3 - Chimie, phytosanitaire, pharmacie"]
["SSP000757201","61.0002","USINE MOULINEX",null,"En cours",null,null,"En cours","61001","ALENCON","ORNE","NORMANDIE","Point",0.10016573,48.417843]
["SSP000758201","87.0004","ANCIENNE USINE WATTELEZ",null,"En cours",null,null,"En cours","87113","LE PALAIS SUR VIENNE","HAUTE-VIENNE","NOUVELLE-AQUITAINE","Polygone",1.3097906,45.8553,"D71 - Industrie du caoutchouc"]
["SSP000758701","78.0006","SANOFI  AVENTIS (ex : MARION MERREL DOW)",null,"En cours",null,null,"En cours","78335","LIMAY","YVELINES","ILE-DE-FRANCE","Point",1.7550397,48.99413,"D38 - Industrie pharmaceutique"]
["SSP000758801","52.0001","ANCIENNE DECHARGE DE CHANCENAY",null,"En cours",null,null,"En cours","52104","CHANCENAY","HAUTE-MARNE","GRAND EST","Point",4.976236,48.669964,"K36 - Mise en décharge"]
["SSP000759201","95.0001","NCS PYROTECHNIE ET TECHNOLOGIES",null,"En cours",null,null,"En cours","95604","SURVILLIERS","VAL-D'OISE","ILE-DE-FRANCE","Point",2.543567,49.09309]
["SSP000759801","43.0002","AUZON",null,"En cours",null,null,"En cours","43016","AUZON","HAUTE-LOIRE","AUVERGNE-RHONE-ALPES","Polygone",3.360427,45.387535,"D37 - Phytosanitaires, pesticides (fabrication de)"]
["SSP000760101","68.0102","ANC. EXPLOITATION PETROLIERE (Z.A. STAFFELFELDEN)",null,"En cours",null,null,"En cours","68321","STAFFELFELDEN","HAUT-RHIN","GRAND EST","Point",7.250813,47.82776]
["SSP000760301","51.0002","CALDIC (ex DUCANCEL ET HEBERT)",null,"En cours",null,null,"En cours","51474","SAINT BRICE COURCELLES","MARNE","GRAND EST","Point",4.000425,49.276325,"D3 - Chimie, phytosanitaire, pharmacie"]
["SSP000761101","57.0005","TOTAL PETROCHEMICAL FRANCE (TPF)",null,"En cours",null,null,"En cours","57606","SAINT AVOLD","MOSELLE","GRAND EST","Point",6.7258945,49.143772,"D33 - Pétrochimie carbochimie organique"]
["SSP000761801","57.0007","SOLVAY POLYOLEFINS EUROPE-FRANCE (ANCIENS BASSINS DE DECANTATION)",null,"En cours",null,null,"En cours","57628","SARRALBE","MOSELLE","GRAND EST","Point",7.043824,49.009583,"K36 - Mise en décharge"]
["SSP000762501","57.0016","Crassier du Veymerange",null,"En cours",null,null,"En cours","57672","THIONVILLE","MOSELLE","GRAND EST","Point",6.120301,49.37193]
["SSP000762701","69.0390","EGIC",null,"En cours",null,null,"En cours","69204","SAINT GENIS LAVAL","RHONE","AUVERGNE-RHONE-ALPES","Point",4.817968,45.695072,"H1 - Mécanique, électrique, traitement de surface"]
["SSP000763301","33.0297","Décharge du Lourtet",null,"En cours",null,null,"En cours","33348","QUEYRAC","GIRONDE","NOUVELLE-AQUITAINE","Point",-0.9881153,45.364624,"K21 - Décharges d'ordures ménagères"]
["SSP000764101","80.0005","ORSAN-AMYLUM",null,"En cours",null,null,"En cours","80585","NESLE","SOMME","HAUTS-DE-FRANCE","Point",2.9094307,49.76157,"B1 - Industrie agro-alimentaire"]
["SSP000764401","28.0097","BOUDEVILLE & FONTAINE",null,"En cours",null,null,"En cours","28007","ANET","EURE-ET-LOIR","CENTRE-VAL DE LOIRE","Point",1.455867,48.863308]
["SSP000764601","91.0008","CENTRE PENITENTIAIRE - MAISON D'ARRET",null,"En cours",null,null,"En cours","91235","FLEURY MEROGIS","ESSONNE","ILE-DE-FRANCE","Point",2.3786314,48.637924,"I21 - Chaufferies urbaines"]
["SSP000765401","68.0004","TERRIL  ALEX",null,"En cours",null,null,"En cours","68088","FELDKIRCH","HAUT-RHIN","GRAND EST","Polygone",7.277545,47.85471,"K36 - Mise en décharge"]
["SSP000765701","68.0007","ANC. DECHARGE DE MULHOUSE (Eselacker)",null,"En cours",null,null,"En cours","68166","KINGERSHEIM","HAUT-RHIN","GRAND EST","Polygone",7.3092165,47.786694,"K36 - Mise en décharge"]
["SSP000766201","68.0012","CARRIERE BCS (Béton Contrôle du Seeboden)",null,"En cours",null,null,"En cours","68270","RICHWILLER","HAUT-RHIN","GRAND EST","Point",7.290288,47.788628,"F32 - Carrières"]
["SSP000766301","68.0013","BOLLORE ENERGIE",null,"En cours",null,null,"En cours","68271","RIEDISHEIM","HAUT-RHIN","GRAND EST","Point",7.370126,47.757065,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000766701","68.0017","TERRIL MARIE LOUISE",null,"En cours",null,null,"En cours","68321","STAFFELFELDEN","HAUT-RHIN","GRAND EST","Point",7.2678633,47.828167,"K36 - Mise en décharge"]
["SSP000767101","32.0010","ESCUDERO Guy",null,"En cours",null,null,"En cours","32013","AUCH","GERS","OCCITANIE","Point",0.5699584,43.63812,"K5 - Récupération, dépôts de ferrailles"]
["SSP000767601","68.0025","TERRIL FERNAND",null,"En cours",null,null,"En cours","68376","WITTENHEIM","HAUT-RHIN","GRAND EST","Point",7.3253064,47.802628,"K36 - Mise en décharge"]
["SSP000767701","73.0004","Ancienne décharge \"Les Plaines\"",null,"En cours",null,null,"En cours","73253","SAINT MARCEL","SAVOIE","AUVERGNE-RHONE-ALPES","Point",6.566824,45.504475]
["SSP000768801","45.0081","TPLC",null,"En cours",null,null,"En cours","45284","SAINT JEAN DE BRAYE","LOIRET","CENTRE-VAL DE LOIRE","Point",1.974897,47.91767]
["SSP000769101","73.0003","Ancienne décharge de la société Métaux Spéciaux \"Plateau-Robert\"",null,"En cours",null,null,"En cours","73253","SAINT MARCEL","SAVOIE","AUVERGNE-RHONE-ALPES","Point",6.551282,45.491573]
["SSP000769601","73.0017","ANCIENS CRASSIERS DE L'USINE PECHINEY ELECTRO METALLURGIE",null,"En cours",null,null,"En cours","73226","SAINT BERON","SAVOIE","AUVERGNE-RHONE-ALPES","Point",5.7159348,45.494553,"J3 - Métallurgie des métaux non ferreux, affinage"]
["SSP000769701","73.0009","ALUMINIUM PECHINEY/La PRAZ",null,"Clôturée",null,null,"Clôturée","73119","FRENEY","SAVOIE","AUVERGNE-RHONE-ALPES","Point",6.591226,45.20177,"J3 - Métallurgie des métaux non ferreux, affinage"]
["SSP000770201","73.0014","Dépôts de déchets de Champagneux",null,"En cours",null,null,"En cours","73070","CHAMPAGNEUX","SAVOIE","AUVERGNE-RHONE-ALPES","Point",5.6790805,45.633976,"K36 - Mise en décharge"]
["SSP000770701","27.0006","SOCIETE FONDERIE DES ARDENNES",null,"En cours",null,null,"En cours","27467","PONT AUDEMER","EURE","NORMANDIE","Point",0.5156666,49.34968,"J5 - Fonderie et travail des métaux"]
["SSP000771201","74.0004","COMPAGNIE ALPINE D'ALUMINIUM (ex NOVELIS SPECIALITE FRANCE, ex USINE PECHINEY RH",null,"En cours",null,null,"En cours","74010","ANNECY","HAUTE-SAVOIE","AUVERGNE-RHONE-ALPES","Point",6.098343,45.90918,"J32 - Métallurgie de l'aluminium"]
["SSP000771301","74.0005","ENTREPRISE SADDIER DECOLLETAGE",null,"En cours",null,null,"En cours","74037","BOEGE","HAUTE-SAVOIE","AUVERGNE-RHONE-ALPES","Point",6.40403,46.20845,"H11 - Usinage"]
["SSP000772001","92.0002","EX SOCIETE FRANÇAISE DE MUNITIONS",null,"En cours",null,null,"En cours","92040","ISSY LES MOULINEAUX","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.2536066,48.819775,"D8 - Poudres et explosifs"]
["SSP000772401","34.0002","SOCIETE SOTRAITAL",null,"En cours",null,null,"En cours","34111","GANGES","HERAULT","OCCITANIE","Point",3.7175303,43.93917]
["SSP000772801","69.0003","S.A. BRUNNER",null,"Clôturée",null,"2017-01-13","Clôturée","69289","SAINT PIERRE DE CHANDIEU","RHONE","AUVERGNE-RHONE-ALPES","Point",5.009185,45.669327,"D42 - Fabrication de peintures"]
["SSP000773201","69.0010","PORT EDOUARD HERRIOT",null,"En cours",null,null,"En cours","69123","LYON","RHONE","AUVERGNE-RHONE-ALPES","Point",4.831435,45.71945,"D21 - Stockage et conditionnement des gaz et liquéfiés"]
["SSP000773701","69.0020","DEPOT DE CENDRES ET DE MACHEFERS  (SYTRAIVAL) D'ARNAS",null,"En cours",null,null,"En cours","69013","ARNAS","RHONE","AUVERGNE-RHONE-ALPES","Point",4.7210236,46.025425,"K36 - Mise en décharge"]
["SSP000774201","69.0028","CPT EDF LOIRE SUR RHONE - Dépôt cendres et mâchefers",null,"En cours",null,null,"En cours","69091","GIVORS","RHONE","AUVERGNE-RHONE-ALPES","Point",4.802702,45.568172,"I11 - Centrales électriques thermiques"]
["SSP000774701","09.0001","ANCIENNE CARRIERE \"LES PUJOLS\"",null,"En cours",null,null,"En cours","09238","LES PUJOLS","ARIEGE","OCCITANIE","Point",1.7256685,43.086685,"D42 - Fabrication de peintures"]
["SSP000774801","45.0110","garage du Cas Rouge",null,"En cours",null,null,"En cours","45067","CHAINGY","LOIRET","CENTRE-VAL DE LOIRE","Point",1.7992201,47.875256]
["SSP000776201","33.0017","VALORM",null,"Clôturée",null,"2006-12-01","Clôturée","33256","LUDON MEDOC","GIRONDE","NOUVELLE-AQUITAINE","Point",-0.5875061,44.98057,"K35 - Regroupement, reconditionnement de déchets"]
["SSP000776601","33.0021","SARP Industries",null,"En cours",null,null,"En cours","33314","PAUILLAC","GIRONDE","NOUVELLE-AQUITAINE","Point",-0.7661745,45.1984,"K31 - Incinération"]
["SSP000776801","23.0002","SITE PICOTY (ex SOLIC)",null,"En cours",null,"2006-01-24","En cours","23096","GUERET","CREUSE","NOUVELLE-AQUITAINE","Point",1.8803306,46.19409,"K3 - Traitement de déchets industriels"]
["SSP000777601","77.0009","DECHARGE DE FOUJU-MOISENAY","DECHARGE DE FOUJU-MOISENAY","En cours",null,null,"En cours","77195","FOUJU","SEINE-ET-MARNE","ILE-DE-FRANCE","Polygone",2.7528589,48.579456,null,null,null,"38.21Z - Traitement et élimination des déchets non dangereux"]
["SSP000778901","71.0004","ANCIEN SITE MINIER DE CHIZEUIL",null,"En cours",null,null,"En cours","71075","CHALMOUX","SAONE-ET-LOIRE","BOURGOGNE-FRANCHE-COMTE","Point",3.845044,46.597523,"F3 - Minerais non métalliques, carrières (extraction de)"]
["SSP000779301","30.0003","SYNGENTA","SYNGENTA","En cours",null,null,"En cours","30004","AIGUES VIVES","GARD","OCCITANIE","Polygone",4.194001,43.72798,null,"18.08 - Fabrication de produits phytosanitaires"]
["SSP000779801","49.0007","PARKING DU CENTRE COMMERCIAL CARREFOUR St SERGE",null,"En cours",null,null,"En cours","49007","ANGERS","MAINE-ET-LOIRE","PAYS DE LA LOIRE","Point",-0.53988385,47.487118,"L23 - Détail de carburants"]
["SSP000780301","44.0009","BERTON DEMANGEAU",null,"Clôturée",null,"2012-06-01","Clôturée","44212","VALLET","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Point",-1.2602992,47.162304,"C1 - Bois et de l'ameublement (industrie du)"]
["SSP000780601","67.0001","SOCOMEC",null,"En cours",null,null,"En cours","67028","BENFELD","BAS-RHIN","GRAND EST","Point",7.5934,48.372787,"H - Mécanique, traitements des surfaces"]
["SSP000781101","67.0007","INEOS (anciens bassins de décantation de SOLVAY)",null,"En cours",null,null,"En cours","67191","HERBITZHEIM","BAS-RHIN","GRAND EST","Point",7.0571303,49.019768,"K36 - Mise en décharge"]
["SSP000781301","80.0083","VALEO",null,"Clôturée",null,"2017-10-16","Clôturée","80021","AMIENS","SOMME","HAUTS-DE-FRANCE","Point",2.280058,49.935852]
["SSP000781601","67.0011","DOW / ROHM AND HAAS (anciennt DOW CHEMICALS-ROHM&HAAS)",null,"En cours",null,null,"En cours","67261","LAUTERBOURG","BAS-RHIN","GRAND EST","Point",8.187037,48.964508,"K36 - Mise en décharge"]
["SSP000782101","67.0017","DARAMIC",null,"En cours",null,null,"En cours","67462","SELESTAT","BAS-RHIN","GRAND EST","Point",7.4657645,48.282604,"D72 - Transformation des matières plastiques"]
["SSP000782601","08.0004","FAYNOT ex : GALVASEMOY",null,"En cours",null,null,"En cours","08448","THILAY","ARDENNES","GRAND EST","Point",4.808634,49.900116,"H13 - Traitement de surface"]
["SSP000783601","12.0002","UMICORE (ex UNION MINIERE, ex VIEILLE MONTAGNE)",null,"En cours",null,null,"En cours","12305","VIVIEZ","AVEYRON","OCCITANIE","Point",2.219439,44.557106]
["SSP000783901","79.0003","Communauté d'agglomération Niortaise (CAN)",null,"En cours",null,null,"En cours","79191","NIORT","DEUX-SEVRES","NOUVELLE-AQUITAINE","Point",-0.492805,46.35135,"K21 - Décharges d'ordures ménagères"]
["SSP000784101","971.0001","EDF centrale électrique Désirade",null,"En cours",null,null,"En cours","97110","LA DESIRADE","GUADELOUPE","GUADELOUPE","Point",4.593646,43.471367]
["SSP000784701","60.0014","ANCIENNE DECHARGE KELLER",null,"En cours",null,null,"En cours","60567","SAINT AUBIN EN BRAY","OISE","HAUTS-DE-FRANCE","Point",1.8867717,49.423615,"D44 - Fabrication de colles et mastics"]
["SSP000785001","89.0004","Déposante  Bertrand",null,"En cours",null,null,"En cours","89206","JOIGNY","YONNE","BOURGOGNE-FRANCHE-COMTE","Point",3.3848636,47.973717,"K - Déchets et traitements"]
["SSP000785301","37.0001","DECHARGE DU CHEVAL BLANC",null,"En cours",null,null,"En cours","37115","DESCARTES","INDRE-ET-LOIRE","CENTRE-VAL DE LOIRE","Point",0.6781831,46.994583,"K21 - Décharges d'ordures ménagères"]
["SSP000785901","31.0002","TSM",null,"En cours",null,null,"En cours","31555","TOULOUSE","HAUTE-GARONNE","OCCITANIE","Point",1.4502648,43.57786,"H13 - Traitement de surface"]
["SSP000786301","60.0006","DECHARGE SAINT GOBAIN",null,"En cours",null,null,"En cours","60119","CAMBRONNE LES RIBECOURT","OISE","HAUTS-DE-FRANCE","Point",2.8970506,49.509285]
["SSP000786801","60.0011","ANCIENNE DECHARGE RODANET",null,"En cours",null,null,"En cours","60447","NERY","OISE","HAUTS-DE-FRANCE","Point",2.7686107,49.276398,"K36 - Mise en décharge"]
["SSP000787101","60.0016","DECHARGE CLARIANT DE TROSLY BREUIL",null,"En cours",null,null,"En cours","60647","TROSLY BREUIL","OISE","HAUTS-DE-FRANCE","Point",2.9655945,49.39587,"K36 - Mise en décharge"]
["SSP000787301","60.0019","IEP (ex SABIC Innovative Plastics, ex General Electrics Plastics ABS)",null,"En cours",null,null,"En cours","60685","VILLERS SAINT SEPULCRE","OISE","HAUTS-DE-FRANCE","Point",2.2156737,49.37111,"D34 - Fabrication de matières plastiques de base"]
["SSP000788001","21.0007","AMCOR FLEXIBLES PACKAGING FRANCE",null,"En cours",null,null,"En cours","21231","DIJON","COTE-D'OR","BOURGOGNE-FRANCHE-COMTE","Point",5.0370545,47.302826,"H2 - Imprimerie, presse-édition, photographie"]
["SSP000788901","13.0010"," SOCIETE EUROPEENNE DE SOUFRES INDUSTRIELS. - S.E.S.I.",null,"En cours",null,null,"En cours","13055","MARSEILLE","BOUCHES-DU-RHONE","PROVENCE-ALPES-COTE D'AZUR","Point",5.3842793,43.332962,"D32 - Chimie minérale inorganique autre"]
["SSP000789001","13.0014","Sté ELECTROLYSE PHOCEENNE (EX site de l'ancienne Société SODEGA)",null,"En cours",null,null,"En cours","13117","VITROLLES","BOUCHES-DU-RHONE","PROVENCE-ALPES-COTE D'AZUR","Point",5.2458267,43.43074,"H13 - Traitement de surface"]
["SSP000789601","64.0004","ANCIENNE CENTRALE EDF",null,"Clôturée",null,"2012-03-23","Clôturée","64061","ARTIX","PYRENEES-ATLANTIQUES","NOUVELLE-AQUITAINE","Point",-0.568616,43.397026,"I11 - Centrales électriques thermiques"]
["SSP000790101","64.0009","Décharge de Lescar",null,"En cours",null,null,"En cours","64335","LESCAR","PYRENEES-ATLANTIQUES","NOUVELLE-AQUITAINE","Point",-0.43026882,43.34118,"K21 - Décharges d'ordures ménagères"]
["SSP000790501","62.0178","Ryssen Alcools",null,"En cours",null,null,"En cours","62447","HESDIN","PAS-DE-CALAIS","HAUTS-DE-FRANCE","Point",2.032282,50.3739,"B14 - Industrie du sucre"]
["SSP000790701","14.0007","Ancien dépôt MIROLINE",null,"En cours",null,null,"En cours","14333","HONFLEUR","CALVADOS","NORMANDIE","Point",0.24150254,49.4232]
["SSP000791301","45.0004","Vermilion (ex TOREADOR ENERGY FRANCE (ex SITE ELF AQUITAINE PRODUCTION)",null,"En cours",null,null,"En cours","45275","SAINT FIRMIN DES BOIS","LOIRET","CENTRE-VAL DE LOIRE","Point",2.9115188,47.967007,"D1 - Industrie pétrolière, gaz naturel"]
["SSP000791601","28.0002","LE FONVILLE ( ROUX)",null,"En cours",null,null,"En cours","28054","LE BOULLAY MIVOYE","EURE-ET-LOIR","CENTRE-VAL DE LOIRE","Point",1.4116719,48.66017,"D72 - Transformation des matières plastiques"]
["SSP000792201","76.0027","AREVA T&D : PARKING ET USINE ALSTHOM",null,"En cours",null,null,"En cours","76498","LE PETIT QUEVILLY","SEINE-MARITIME","NORMANDIE","Point",1.047388,49.429287,"K21 - Décharges d'ordures ménagères"]
["SSP000792301","76.0030","SITE DE LA SOCIETE HAVRAISE DE MANUTENTION DE PRODUITS PETROLIERS",null,"En cours",null,null,"En cours","76351","LE HAVRE","SEINE-MARITIME","NORMANDIE","Point",0.13085097,49.49102,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000792801","76.0014","SCO (ex Grande Paroisse Oissel ex SITE AZOLACQ)",null,"En cours",null,null,"En cours","76484","OISSEL","SEINE-MARITIME","NORMANDIE","Point",1.1105173,49.35044,"D36 - Fabrication des engrais"]
["SSP000793201","76.0006","RAFFINERIE DE PETIT COURONNE (ex Couronnaise de Raffinage)",null,"En cours",null,null,"En cours","76497","PETIT COURONNE","SEINE-MARITIME","NORMANDIE","Point",1.0154532,49.383057,"D12 - Raffinage de pétrole, carburants et lubrifiants"]
["SSP000793601","76.0028","Décharge interne de ISOVER SAINT GOBAIN",null,"En cours",null,null,"En cours","76575","SAINT ETIENNE DU ROUVRAY","SEINE-MARITIME","NORMANDIE","Point",1.1169043,49.389404,"G14 - Fabrication d'autres matériaux de construction"]
["SSP000793701","76.0010","DEPOT DE DECHETS \"LA FERME DU GRUCHET\"",null,"En cours",null,null,"En cours","76705","TOURVILLE LA RIVIERE","SEINE-MARITIME","NORMANDIE","Point",1.0666026,49.32093]
["SSP000794601","974.0005","SUCRERIE-DISTILLERIE DE SAVANNA",null,"En cours",null,null,"En cours","97415","SAINT-PAUL","LA REUNION","LA REUNION","Point",-3.4045606,27.140974,"B14 - Industrie du sucre"]
["SSP000794901","64.0127","Décharge de Lons",null,"En cours",null,null,"En cours","64348","LONS","PYRENEES-ATLANTIQUES","NOUVELLE-AQUITAINE","Point",-0.4148522,43.30006]
["SSP000795501","972.0006","SOCOMOR",null,"En cours",null,null,"En cours","97218","LE MORNE-ROUGE","MARTINIQUE","MARTINIQUE","Point",3.5728261,41.69196,"B23 - Fabrication d'autres boissons"]
["SSP000795701","973.0002","CENTRALE ELECTRIQUE EDF",null,"En cours",null,null,"En cours","97311","SAINT-LAURENT-DU-MARONI","GUYANE","GUYANE","Point",0.0,0.0]
["SSP000796001","45.0008","FORAGE AEP",null,"En cours",null,null,"En cours","45273","SAINT DENIS DE L'HOTEL","LOIRET","CENTRE-VAL DE LOIRE","Point",2.1286583,47.868687]
["SSP000796901","70.0005","BECK TECHNOLOGIES (anciennement Blanc Aéro Technologies)",null,"En cours",null,null,"En cours","70006","AILLEVILLERS ET LYAUMONT","HAUTE-SAONE","BOURGOGNE-FRANCHE-COMTE","Point",6.326007,47.948044,"H13 - Traitement de surface"]
["SSP000797301","18.0039","STROMAG France",null,"En cours",null,null,"En cours","18108","LA GUERCHE SUR L'AUBOIS","CHER","CENTRE-VAL DE LOIRE","Point",2.9414656,46.941967,"H11 - Usinage"]
["SSP000797401","63.0003","USINE MICHELIN DES CARMES",null,"En cours",null,null,"En cours","63113","CLERMONT FERRAND","PUY-DE-DOME","AUVERGNE-RHONE-ALPES","Point",3.0928597,45.783234,"D71 - Industrie du caoutchouc"]
["SSP000798101","95.0005","CHEMTURA (ex GREAT LAKES CHEMICAL)",null,"En cours",null,null,"En cours","95487","PERSAN","VAL-D'OISE","ILE-DE-FRANCE","Point",2.266904,49.151245,"D35 - Traitement chimique des corps gras"]
["SSP000798501","93.0022","Direction de la recherche ENGIE/ ex usine à gaz du LANDY",null,"En cours",null,null,"En cours","93066","SAINT DENIS","SEINE-SAINT-DENIS","ILE-DE-FRANCE","Point",2.353661,48.92007,"J1 - Cokéfaction, usines à gaz"]
["SSP000799101","18.0004","USINES DE ROSIERES",null,"En cours",null,null,"En cours","18133","LUNERY","CHER","CENTRE-VAL DE LOIRE","Point",2.2532096,46.960155,"J5 - Fonderie et travail des métaux"]
["SSP000799501","13.0015","Calanque SAMENA",null,"En cours",null,null,"En cours","13055","MARSEILLE","BOUCHES-DU-RHONE","PROVENCE-ALPES-COTE D'AZUR","Point",5.349408,43.22853,"K - Déchets et traitements"]
["SSP000799901","58.0005","Euro Auto Hose (Ancien site GATES SA)",null,"En cours",null,null,"En cours","58194","NEVERS","NIEVRE","BOURGOGNE-FRANCHE-COMTE","Point",3.176645,46.998726,"D7 - Caoutchouc et matières plastiques"]
["SSP000800401","10.0006","GARAGE FLIZOT",null,"En cours",null,null,"En cours","10233","MERY SUR SEINE","AUBE","GRAND EST","Point",3.8961875,48.505238,"L23 - Détail de carburants"]
["SSP000801001","62.0021","BP - GERLAND",null,"En cours",null,null,"En cours","62627","NOYELLES SOUS BELLONNE","PAS-DE-CALAIS","HAUTS-DE-FRANCE","Point",3.024394,50.307796,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000801101","28.0010","COULOMBS",null,"En cours",null,null,"En cours","28113","COULOMBS","EURE-ET-LOIR","CENTRE-VAL DE LOIRE","Point",1.5480821,48.649506,"D72 - Transformation des matières plastiques"]
["SSP000801501","59.0027","Befesa Valera",null,"En cours",null,null,"En cours","59273","GRAVELINES","NORD","HAUTS-DE-FRANCE","Point",2.1449258,51.002495,"D - Chimie, parachimie, pétrole"]
["SSP000802101","26.0009","STATION AUTOROUTIERE SHELL",null,"En cours",null,null,"En cours","26252","PORTES LES VALENCE","DROME","AUVERGNE-RHONE-ALPES","Point",4.8649035,44.867916,"L23 - Détail de carburants"]
["SSP000802701","78.0011","LABO SERVICES (RIC)",null,"En cours",null,null,"En cours","78062","BEYNES","YVELINES","ILE-DE-FRANCE","Point",48.86144,1.8754523,"D38 - Industrie pharmaceutique"]
["SSP000802901","78.0016","STATION CARREFOUR AUTOROUTE A13",null,"En cours",null,null,"En cours","78531","ROSNY SUR SEINE","YVELINES","ILE-DE-FRANCE","Point",1.6049458,48.99936,"L23 - Détail de carburants"]
["SSP000803501","12.0004","PLATE FORME DE DECAZEVILLE",null,"En cours",null,null,"En cours","12089","DECAZEVILLE","AVEYRON","OCCITANIE","Point",2.2563581,44.568657]
["SSP000803901","69.0032","TEINTURE ET IMPRESSION DE LYON (TIL)",null,"En cours",null,null,"En cours","69264","VILLEFRANCHE SUR SAONE","RHONE","AUVERGNE-RHONE-ALPES","Point",4.7438383,45.98321,"E13 - Blanchiment, teinture, impression"]
["SSP000804501","69.0037","ANCIEN ETABLISSEMENT PELLET",null,"Clôturée",null,"2015-04-13","Clôturée","69266","VILLEURBANNE","RHONE","AUVERGNE-RHONE-ALPES","Point",4.9063115,45.76078]
["SSP000804601","69.0039","TESTUT - TRAYVOU",null,"Clôturée",null,"1994-11-24","Clôturée","69142","LA MULATIERE","RHONE","AUVERGNE-RHONE-ALPES","Point",4.8158584,45.726757]
["SSP000805001","41.0003","ANCIENNE DECHARGE COMMUNALE D'OUZOUER LE DOYEN",null,"En cours",null,null,"En cours","41172","OUZOUER LE DOYEN","LOIR-ET-CHER","CENTRE-VAL DE LOIRE","Point",1.3477054,47.940845]
["SSP000805501","08.0008","METAL BLANC",null,"En cours",null,null,"En cours","08078","BOURG FIDELE","ARDENNES","GRAND EST","Point",4.551477,49.88979,"J52 - Fonderie des métaux non ferreux"]
["SSP000806201","64.0018","Ancienne décharge MESSIER-DOWTY",null,"En cours",null,null,"En cours","64245","GOES","PYRENEES-ATLANTIQUES","NOUVELLE-AQUITAINE","Point",-0.5760337,43.215034,"K36 - Mise en décharge"]
["SSP000806501","28.0062","Bio Cos Natura",null,"En cours",null,null,"En cours","28134","DREUX","EURE-ET-LOIR","CENTRE-VAL DE LOIRE","Point",1.368516,48.74976,"K35 - Regroupement, reconditionnement de déchets"]
["SSP000807001","38.0022","ANCIENNE USINE DYNASTAR",null,"Clôturée",null,"1996-03-22","Clôturée","38133","COUBLEVIE","ISERE","AUVERGNE-RHONE-ALPES","Point",5.6181474,45.356937]
["SSP000807801","68.0032","ANC. USINE BAUMGARTNER",null,"En cours",null,null,"En cours","68298","SAINTE MARIE AUX MINES","HAUT-RHIN","GRAND EST","Point",7.1824555,48.239307,"E13 - Blanchiment, teinture, impression"]
["SSP000808201","25.0007","AUTOMOBILES PEUGEOT",null,"En cours",null,null,"En cours","25043","BART","DOUBS","BOURGOGNE-FRANCHE-COMTE","Polygone",6.766263,47.481266,"H13 - Traitement de surface"]
["SSP000808301","35.0002","Station-service DALLE (ex OLLIVIER)",null,"Clôturée",null,"2016-12-01","Clôturée","35330","TAILLIS","ILLE-ET-VILAINE","BRETAGNE","Polygone",-1.2375088,48.190113,"L23 - Détail de carburants"]
["SSP000808701","76.0045","CHEVRON CHEMICAL - terres du sud",null,"En cours",null,null,"En cours","76305","GONFREVILLE L'ORCHER","SEINE-MARITIME","NORMANDIE","Point",0.21350822,49.488613,"D33 - Pétrochimie carbochimie organique"]
["SSP000809201","76.0050","YACCO S.A.",null,"En cours",null,null,"En cours","76165","CAUDEBEC LES ELBEUF","SEINE-MARITIME","NORMANDIE","Point",1.0186647,49.28647]
["SSP000809401","33.0015","SCIERIE LE FLAMAND SAINT ISIDORE",null,"En cours",null,"2006-12-04","En cours","33300","NAUJAC SUR MER","GIRONDE","NOUVELLE-AQUITAINE","Point",-1.0688081,45.255756,"C13 - Traitement du bois"]
["SSP000810401","33.0032","SREE",null,"En cours",null,null,"En cours","33063","BORDEAUX","GIRONDE","NOUVELLE-AQUITAINE","Point",-0.5502778,44.867,"M - Divers et services"]
["SSP000811201","42.0017","IMPHY UGINE PRECISION-Site de Firminy - APERAM",null,"En cours",null,null,"En cours","42316","UNIEUX","LOIRE","AUVERGNE-RHONE-ALPES","Point",4.2840967,45.39622,"J53 - Travail des métaux, chaudronnerie, poudres"]
["SSP000811701","18.0018","Etablissement Traction SNCF",null,"En cours",null,null,"En cours","18279","VIERZON","CHER","CENTRE-VAL DE LOIRE","Point",2.0531409,47.231834,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000812201","64.0025","TURBOMECA",null,"En cours",null,null,"En cours","64138","BORDES","PYRENEES-ATLANTIQUES","NOUVELLE-AQUITAINE","Point",-0.28537354,43.238564,"H1 - Mécanique, électrique, traitement de surface"]
["SSP000812501","01.0012","CARRIER - MONTLUEL",null,"En cours",null,null,"En cours","01262","MONTLUEL","AIN","AUVERGNE-RHONE-ALPES","Point",5.049798,45.84565,"H13 - Traitement de surface"]
["SSP000812701","64.0027","TANNERIE CARRIAT",null,"En cours",null,null,"En cours","64213","ESPELETTE","PYRENEES-ATLANTIQUES","NOUVELLE-AQUITAINE","Point",-1.4496465,43.321922]
["SSP000813301","64.0031","SAGEM",null,"En cours",null,null,"En cours","64407","MOUGUERRE","PYRENEES-ATLANTIQUES","NOUVELLE-AQUITAINE","Point",-1.4042917,43.458675]
["SSP000813501","64.0033","CHIMEX",null,"En cours",null,null,"En cours","64410","MOURENX","PYRENEES-ATLANTIQUES","NOUVELLE-AQUITAINE","Point",-0.6155075,43.373898,"D - Chimie, parachimie, pétrole"]
["SSP000813801","64.0035","SANOFI Chimie",null,"En cours",null,null,"En cours","64410","MOURENX","PYRENEES-ATLANTIQUES","NOUVELLE-AQUITAINE","Point",-0.6155075,43.373898,"D38 - Industrie pharmaceutique"]
["SSP000814301","33.0080","Fonderie PENA",null,"En cours",null,null,"En cours","33281","MERIGNAC","GIRONDE","NOUVELLE-AQUITAINE","Point",-0.72614044,44.812172,"J52 - Fonderie des métaux non ferreux"]
["SSP000814901","33.0086","AIRBUS SAFRAN LAUNCHERS",null,"En cours",null,null,"En cours","33449","SAINT MEDARD EN JALLES","GIRONDE","NOUVELLE-AQUITAINE","Point",-0.72917074,44.870335,"D8 - Poudres et explosifs"]
["SSP000815301","18.0015","Dépôt BP FIOUL SERVICES",null,"En cours",null,null,"En cours","18205","SAINT DOULCHARD","CHER","CENTRE-VAL DE LOIRE","Point",2.372935,47.09974,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000815601","31.0018","HYDRO BUILDEX TOULOUSE (ex SAPA BUILDEX TOULOUSE)",null,"En cours",null,null,"En cours","31555","TOULOUSE","HAUTE-GARONNE","OCCITANIE","Point",1.422431,43.552883,"H - Mécanique, traitements des surfaces"]
["SSP000815801","42.0032","CVI ex : FOREZ POIDS LOURD RECUPERATION",null,"En cours",null,null,"En cours","42211","SAINT CYPRIEN","LOIRE","AUVERGNE-RHONE-ALPES","Point",4.2433186,45.532227]
["SSP000816401","33.0089","SARIA Industries",null,"En cours",null,null,"En cours","33167","FLOIRAC","GIRONDE","NOUVELLE-AQUITAINE","Point",-0.5305836,44.818527,"B11 - Viande, abattoirs, équarrissage (industrie de la)"]
["SSP000816901","42.0033","HINDERCHIED",null,"En cours",null,null,"En cours","42175","POUILLY LES FEURS","LOIRE","AUVERGNE-RHONE-ALPES","Point",4.229841,45.7966]
["SSP000817101","78.0021","CARREFOUR",null,"En cours",null,null,"En cours","78418","MONTESSON","YVELINES","ILE-DE-FRANCE","Point",2.1456833,48.930737,"L23 - Détail de carburants"]
["SSP000817601","67.0034","HAGER (I et II)",null,"En cours",null,null,"En cours","67348","OBERNAI","BAS-RHIN","GRAND EST","Point",7.5005856,48.4726,"H13 - Traitement de surface"]
["SSP000818001","68.0038","EURO TF anciennement MANUFACTURES HARTMANN MUNSTER",null,"En cours",null,null,"En cours","68226","MUNSTER","HAUT-RHIN","GRAND EST","Point",7.139917,48.038445]
["SSP000818501","67.0039","TREDI",null,"En cours",null,null,"En cours","67482","STRASBOURG","BAS-RHIN","GRAND EST","Point",7.790112,48.590588,"K31 - Incinération"]
["SSP000818801","67.0041","SEW USOCOME",null,"En cours",null,null,"En cours","67180","HAGUENAU","BAS-RHIN","GRAND EST","Point",7.8005686,48.82444]
["SSP000819001","67.0044","CHAUDRONNERIE BIEBER",null,"En cours",null,null,"En cours","67105","DRULINGEN","BAS-RHIN","GRAND EST","Point",7.1886206,48.866886]
["SSP000819301","67.0047","DE DIETRICH THERMIQUE",null,"En cours",null,null,"En cours","67291","MERTZWILLER","BAS-RHIN","GRAND EST","Point",7.6778064,48.872005,"H - Mécanique, traitements des surfaces"]
["SSP000819901","67.0051","SELF (ex. SABOREC)",null,"En cours",null,null,"En cours","67482","STRASBOURG","BAS-RHIN","GRAND EST","Point",7.788804,48.56828,"C1 - Bois et de l'ameublement (industrie du)"]
["SSP000820001","67.0053","NIJHOF BAUMLIN",null,"En cours",null,null,"En cours","67547","WITTISHEIM","BAS-RHIN","GRAND EST","Point",7.582784,48.263924,"J53 - Travail des métaux, chaudronnerie, poudres"]
["SSP000820501","78.0023","ITON SEINE",null,"En cours",null,null,"En cours","78089","BONNIERES SUR SEINE","YVELINES","ILE-DE-FRANCE","Polygone",1.5574609,49.033905]
["SSP000820901","68.0044","BASF",null,"En cours",null,null,"En cours","68149","HUNINGUE","HAUT-RHIN","GRAND EST","Point",7.578909,47.58549,"D - Chimie, parachimie, pétrole"]
["SSP000821401","67.0057","HAGER (ex. FLASH)",null,"En cours",null,null,"En cours","67437","SAVERNE","BAS-RHIN","GRAND EST","Point",7.3714366,48.73451,"H13 - Traitement de surface"]
["SSP000821501","37.0005","GROUPEMENT PETROLIER DE SAINT PIERRE DES CORPS",null,"En cours",null,null,"En cours","37233","SAINT PIERRE DES CORPS","INDRE-ET-LOIRE","CENTRE-VAL DE LOIRE","Point",0.72275794,47.92517,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000821901","37.0007","S.A. CHROM'FLASH",null,"En cours",null,null,"En cours","37233","SAINT PIERRE DES CORPS","INDRE-ET-LOIRE","CENTRE-VAL DE LOIRE","Point",0.752212,47.38888,"H13 - Traitement de surface"]
["SSP000822301","78.0025","RENAULT FLINS",null,"En cours",null,null,"En cours","78029","AUBERGENVILLE","YVELINES","ILE-DE-FRANCE","Point",1.857114,48.977077,"H1 - Mécanique, électrique, traitement de surface"]
["SSP000822901","18.0021","Usine des ATELIERS D'ORVAL",null,"En cours",null,null,"En cours","18172","ORVAL","CHER","CENTRE-VAL DE LOIRE","Point",2.46482,46.73318,"H - Mécanique, traitements des surfaces"]
["SSP000823001","68.0057","PEUGEOT CITROEN MULHOUSE",null,"En cours",null,null,"En cours","68300","SAUSHEIM","HAUT-RHIN","GRAND EST","Point",7.403709,47.783543]
["SSP000823501","67.0061","BOLLORE ENERGIE",null,"En cours",null,null,"En cours","67482","STRASBOURG","BAS-RHIN","GRAND EST","Point",7.796305,48.59457,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000824101","51.0017","TI Fuel Systems (ex MARWAL SYSTEMS)",null,"En cours",null,null,"En cours","51108","CHALONS EN CHAMPAGNE","MARNE","GRAND EST","Point",4.3535056,48.973167,"H13 - Traitement de surface"]
["SSP000824501","67.0064","Société Européenne de Stockage - Dépôt 2",null,"En cours",null,null,"En cours","67482","STRASBOURG","BAS-RHIN","GRAND EST","Point",7.8002973,48.593067,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000824601","67.0065","BP",null,"En cours",null,null,"En cours","67482","STRASBOURG","BAS-RHIN","GRAND EST","Point",7.7973833,48.59107,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000825101","08.0011","EDF",null,"En cours",null,null,"En cours","08480","VILLERS SEMEUSE","ARDENNES","GRAND EST","Point",4.740585,49.74995,"M - Divers et services"]
["SSP000825401","08.0014","VALLOUREC",null,"En cours",null,null,"En cours","08194","GLAIRE","ARDENNES","GRAND EST","Point",4.907079,49.714928,"J53 - Travail des métaux, chaudronnerie, poudres"]
["SSP000826101","30.0010","SNER",null,"En cours",null,null,"En cours","30007","ALES","GARD","OCCITANIE","Point",4.089753,44.12585]
["SSP000826201","30.0011","Station Service ROLLIN",null,"En cours",null,null,"En cours","30010","ANDUZE","GARD","OCCITANIE","Point",3.9851599,44.051846]
["SSP000826701","52.0013","BOLLORE",null,"En cours",null,null,"En cours","52448","SAINT DIZIER","HAUTE-MARNE","GRAND EST","Point",4.9742413,48.633286,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000827101","78.0034","PEUGEOT CITROEN POISSY SNC (PSA)",null,"En cours",null,null,"En cours","78498","POISSY","YVELINES","ILE-DE-FRANCE","Point",2.0472364,48.93794,"H1 - Mécanique, électrique, traitement de surface"]
["SSP000827501","10.0009","NAPPE  ALLUVIALE",null,"Clôturée",null,"2005-01-28","Clôturée","10067","BUCHERES","AUBE","GRAND EST","Point",4.1111727,48.237015]
["SSP000827601","10.0010","DECHARGE DES CRISTALLERIES ROYALES DE CHAMPAGNE",null,"En cours",null,null,"En cours","10035","BAYEL","AUBE","GRAND EST","Point",4.79305,48.194267,"K36 - Mise en décharge"]
["SSP000828101","73.0025","LAGUNES AGRATI France Fastening Systems ex ACUMENT(ex PTB)",null,"En cours",null,null,"En cours","73058","LA BRIDOIRE","SAVOIE","AUVERGNE-RHONE-ALPES","Point",5.7316756,45.530663,"H11 - Usinage"]
["SSP000828401","70.0012","THEVENIN DUCROT (EX-SHELL DIRECT)",null,"En cours",null,null,"En cours","70388","NOIDANS LES VESOUL","HAUTE-SAONE","BOURGOGNE-FRANCHE-COMTE","Point",6.1273346,47.619114,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000829101","88.0018","T.S.A. INOX ( Techniques de Soudure Appliquée )",null,"En cours",null,null,"En cours","88317","MOUSSEY","VOSGES","GRAND EST","Point",7.029217,48.43202,"H13 - Traitement de surface"]
["SSP000829401","55.0013","Société Métallurgique de Revigny",null,"En cours",null,null,"En cours","55427","REVIGNY SUR ORNAIN","MEUSE","GRAND EST","Point",4.976362,48.81993,"H13 - Traitement de surface"]
["SSP000829701","25.0010","PEUGEOT JAPY",null,"En cours",null,null,"En cours","25580","VALENTIGNEY","DOUBS","BOURGOGNE-FRANCHE-COMTE","Point",6.8440256,47.463303,"H1 - Mécanique, électrique, traitement de surface"]
["SSP000830101","49.0010","PHYTEUROP",null,"En cours",null,null,"En cours","49215","MONTREUIL BELLAY","MAINE-ET-LOIRE","PAYS DE LA LOIRE","Point",-0.12506898,47.129616,"D37 - Phytosanitaires, pesticides (fabrication de)"]
["SSP000830501","82.0005","VILLEROY ET BOCH",null,"En cours",null,null,"En cours","82186","VALENCE","TARN-ET-GARONNE","OCCITANIE","Point",0.8930375,44.102123,"G12 - Fabrication de produits céramiques"]
["SSP000830601","07.0007","ORRION CHIMIE METALCHEM (ex PHARMACIE CENTRALE DE FRANCE)",null,"En cours",null,null,"En cours","07349","LA VOULTE SUR RHONE","ARDECHE","AUVERGNE-RHONE-ALPES","Point",4.7876225,44.80611]
["SSP000831001","82.0008","AUTONEUM FRANCE SASU",null,"En cours",null,null,"En cours","82112","MOISSAC","TARN-ET-GARONNE","OCCITANIE","Point",1.1024084,44.099987,"D71 - Industrie du caoutchouc"]
["SSP000831401","74.0019","USINE BAIKOWSKI CHIMIE",null,"En cours",null,null,"En cours","74213","POISY","HAUTE-SAVOIE","AUVERGNE-RHONE-ALPES","Point",6.067131,45.936394,"D32 - Chimie minérale inorganique autre"]
["SSP000831901","36.0007","Station service Elf Antar",null,"En cours",null,null,"En cours","36044","CHATEAUROUX","INDRE","CENTRE-VAL DE LOIRE","Point",1.6754298,46.806618,"L23 - Détail de carburants"]
["SSP000832101","73.0027","Entrepôt Pétrolier de Chambéry",null,"Clôturée",null,"2019-07-08","Clôturée","73084","CHIGNIN","SAVOIE","AUVERGNE-RHONE-ALPES","Point",5.999991,45.5181,"L13 - Entrepôts de produits dangereux"]
["SSP000832501","36.0010","Société des Condensateurs Records (SCR)",null,"En cours",null,null,"En cours","36044","CHATEAUROUX","INDRE","CENTRE-VAL DE LOIRE","Point",1.7307904,46.8071,"H18 - Composants électroniques (fabrication de)"]
["SSP000833001","10.0012","LARBALETIER",null,"En cours",null,null,"En cours","10151","FONTAINE LES GRES","AUBE","GRAND EST","Point",3.8824353,48.41087,"H13 - Traitement de surface"]
["SSP000833401","85.0005","SNAM-ANTIPOL",null,"En cours",null,null,"En cours","85092","FONTENAY LE COMTE","VENDEE","PAYS DE LA LOIRE","Point",-0.77707833,46.458733,"K3 - Traitement de déchets industriels"]
["SSP000833501","10.0015","Eiffage Travaux publics (Appia Liants Nord Est) (ex Ste Chimique de la route)",null,"En cours",null,null,"En cours","10387","TROYES","AUBE","GRAND EST","Point",4.0760565,48.292534,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000834001","28.0015","PAULSTRA",null,"En cours",null,null,"En cours","28088","CHATEAUDUN","EURE-ET-LOIR","CENTRE-VAL DE LOIRE","Point",1.3409714,48.079296,"D71 - Industrie du caoutchouc"]
["SSP000834701","54.0021","CRISTALLERIES DAUM","Cessation d'activités","Clôturée",null,"2004-07-22","Clôturée","54395","NANCY","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",6.1980333,48.69808,"G15 - Industrie du verre"]
["SSP000835201","54.0027","Ancien entrepôt pétrolier de NANCY","Cessation d'activités","Clôturée",null,"2004-09-07","Clôturée","54483","SAINT NICOLAS DE PORT","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",6.281838,48.61917,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000835401","54.0036","BASSINS à BOUES du PYLÔNE n°1 et 2 (AMREF)",null,"En cours",null,null,"En cours","54261","HERSERANGE","MEURTHE-ET-MOSELLE","GRAND EST","Point",5.787009,49.51325,"J2 - Sidérurgie, première transformation"]
["SSP000835701","54.0037","KLECK SA (DEPÔT de FOD KLECK)","Pollution accidentelle au fioul","Clôturée",null,"2008-05-16","Clôturée","54382","MONT SAINT MARTIN","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",5.7605524,49.55516,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000836201","42.0092","FIMA PRODUCTION",null,"Clôturée",null,"2015-10-12","Clôturée","42224","SAINT GENEST MALIFAUX","LOIRE","AUVERGNE-RHONE-ALPES","Point",4.4183364,45.34341,"C12 - Produits en bois, ameublement (fabrication de)"]
["SSP000836801","31.0029","GIAT INDUSTRIES",null,"En cours",null,null,"En cours","31555","TOULOUSE","HAUTE-GARONNE","OCCITANIE","Point",1.4549401,43.57643,"H - Mécanique, traitements des surfaces"]
["SSP000836901","57.0027","ANCIEN DEPOT BP - TOTAL",null,"En cours",null,null,"En cours","57463","METZ","MOSELLE","GRAND EST","Point",6.152944,49.133495,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000837701","35.0003","SAS Armoricaine de Fonderie du Châtelet (AFC)",null,"Clôturée",null,"2016-12-06","Clôturée","35236","REDON","ILLE-ET-VILAINE","BRETAGNE","Point",-2.0920367,47.645657,"J - Sidérurgie, métallurgie, coke"]
["SSP000838201","53.0005","QUALIPAC (ex LISI-COSMETICS ex ARTEM et ex SOGECAP)",null,"En cours",null,null,"En cours","53253","SAINT SATURNIN DU LIMET","MAYENNE","PAYS DE LA LOIRE","Point",-1.0970485,47.81478,"H13 - Traitement de surface"]
["SSP000838801","53.0006","DOMAINE DE ROCHEFORT",null,"En cours",null,null,"En cours","53005","ANDOUILLE","MAYENNE","PAYS DE LA LOIRE","Point",-0.745831,48.177574,"G24 - Produits à base d'amiante (fabrication de)"]
["SSP000839101","54.0053","Décharge interne de l'usine de Liverdun (Sté PONT A MOUSSON S.A.)",null,"En cours",null,null,"En cours","54318","LIVERDUN","MEURTHE-ET-MOSELLE","GRAND EST","Point",6.028752,48.75865,"K36 - Mise en décharge"]
["SSP000840201","57.0045","Station Service SHELL",null,"En cours",null,null,"En cours","57177","DIEUZE","MOSELLE","GRAND EST","Point",6.7154074,48.812576,"L23 - Détail de carburants"]
["SSP000840801","57.0047","ATELIER CENTRAL AC4 des Houillères du Bassin de Lorraine",null,"En cours",null,null,"En cours","57123","CARLING","MOSELLE","GRAND EST","Point",6.7093687,49.145203]
["SSP000841201","54.0061","Dépôt de pneus  MULTIPLUS, PREST SCOP, LIPS","Risque d'incendie","Clôturée",null,"2004-07-22","Clôturée","54397","NEUVES MAISONS","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",6.10888,48.616573,"D71 - Industrie du caoutchouc"]
["SSP000841301","54.0057","Usine de pont à Mousson (Société PONT A MOUSSON S.A.)","Pollution due au fonctionnement de l'installation","En cours",null,null,"En cours","54431","PONT A MOUSSON","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",6.0515366,48.895588,"J21 - Production de fontes (haut fourneau)"]
["SSP000841701","57.0203","Station-service Total - relais du Sablon",null,"En cours",null,null,"En cours","57463","METZ","MOSELLE","GRAND EST","Point",0.0,0.0]
["SSP000842201","54.0060","CRISTALLERIES DE BACCARAT","Pollution due au fonctionnement de l'installation","En cours",null,null,"En cours","54039","BACCARAT","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",6.7450986,48.447598,"G15 - Industrie du verre"]
["SSP000842601","57.0058","Centrale Emile Huchet",null,"En cours",null,null,"En cours","57606","SAINT AVOLD","MOSELLE","GRAND EST","Point",6.698931,49.15158,"I11 - Centrales électriques thermiques"]
["SSP000842801","67.0215","ECOMARCHE",null,"En cours",null,null,"En cours","67529","WEYERSHEIM","BAS-RHIN","GRAND EST","Point",7.8053617,48.70825]
["SSP000843501","90.0005","EUROCAST (ex RENCAST)",null,"En cours",null,null,"En cours","90033","DELLE","TERRITOIRE DE BELFORT","BOURGOGNE-FRANCHE-COMTE","Point",7.00972,47.50719,"H13 - Traitement de surface"]
["SSP000844001","54.0062","Société BRENNTAG LORRAINE","Pollution due au fonctionnement de l'installation","En cours",null,null,"En cours","54528","TOUL","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",5.9353986,48.700146,"L13 - Entrepôts de produits dangereux"]
["SSP000844401","44.0023","ARCELORMITTAL ATLANTIQUE ET LORRAINE (ex. USINOR PACKAGING BASSE-INDRE)",null,"En cours",null,null,"En cours","44074","INDRE","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Point",-1.670091,47.19969,"J23 - Première transformation de l'acier"]
["SSP000844501","44.0025","ANCIENNE USINE CHIMIQUE OCTEL-FRANCE",null,"En cours",null,null,"En cours","44116","PAIMBOEUF","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Polygone",-2.0135872,47.284714,"D3 - Chimie, phytosanitaire, pharmacie"]
["SSP000844901","57.0072","Société BOUR",null,"En cours",null,null,"En cours","57221","FLORANGE","MOSELLE","GRAND EST","Point",6.119638,49.328266,"K5 - Récupération, dépôts de ferrailles"]
["SSP000845401","90.0010","ARA",null,"En cours",null,null,"En cours","90022","CHATENOIS LES FORGES","TERRITOIRE DE BELFORT","BOURGOGNE-FRANCHE-COMTE","Point",6.8559127,47.560265,"H - Mécanique, traitements des surfaces"]
["SSP000845701","90.0012","LISI AUTOMOTIVE",null,"En cours",null,null,"En cours","90033","DELLE","TERRITOIRE DE BELFORT","BOURGOGNE-FRANCHE-COMTE","Point",7.000819,47.514633,"H13 - Traitement de surface"]
["SSP000845901","57.0083","Crassier et bassins à boues de Rombas",null,"En cours",null,null,"En cours","57019","AMNEVILLE","MOSELLE","GRAND EST","Point",6.1145096,49.24948]
["SSP000846701","09.0002","ALLIANCE MAESTRIA (ex PEINTURES MAESTRIA)",null,"En cours",null,null,"En cours","09225","PAMIERS","ARIEGE","OCCITANIE","Point",1.6195505,43.12091,"D42 - Fabrication de peintures"]
["SSP000847001","61.0016","SOFEDIT (ex Thyssenkrupp)",null,"En cours",null,null,"En cours","61484","LE THEIL","ORNE","NORMANDIE","Point",0.6818688,48.25856]
["SSP000847501","09.0012","ETIENNE LACROIX \"TOUS ARTIFICES\"",null,"En cours",null,null,"En cours","09185","MAZERES","ARIEGE","OCCITANIE","Point",1.6902838,43.212597,"D81 - Poudres et explosifs (fabrication de)"]
["SSP000847601","09.0014","SOTAP-CAROL",null,"En cours",null,null,"En cours","09206","MONTFERRIER","ARIEGE","OCCITANIE","Point",1.8003546,42.89929,"E13 - Blanchiment, teinture, impression"]
["SSP000848201","31.0022","STCM",null,"En cours",null,null,"En cours","31555","TOULOUSE","HAUTE-GARONNE","OCCITANIE","Polygone",1.4263686,43.636684,"J33 - Métallurgie du plomb et du zinc"]
["SSP000848701","37.0036","SANOFI WINTHROP INDUSTRIES",null,"En cours",null,null,"En cours","37261","TOURS","INDRE-ET-LOIRE","CENTRE-VAL DE LOIRE","Point",0.69535,47.429554]
["SSP000849101","57.0095","RETIA (ex ATOFINA, ex HGD)",null,"En cours",null,null,"En cours","57350","JOUY AUX ARCHES","MOSELLE","GRAND EST","Point",6.0924067,49.071674,"K41 - Régénération d'huiles"]
["SSP000849301","57.0096","DEPOT PETROLIER S.P.L.R.L.",null,"En cours",null,null,"En cours","57303","HAUCONCOURT","MOSELLE","GRAND EST","Point",6.190217,49.208893,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000850401","21.0010","DEPOT   THEVENIN  DUCROT",null,"En cours",null,null,"En cours","21577","SAINT USAGE","COTE-D'OR","BOURGOGNE-FRANCHE-COMTE","Point",5.2510056,47.111206,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000850701","91.0049","SARL ACE-BCI",null,"En cours",null,null,"En cours","91045","BALLANCOURT SUR ESSONNE","ESSONNE","ILE-DE-FRANCE","Polygone",2.3879104,48.52162,"H13 - Traitement de surface"]
["SSP000851301","69.0042","RHODIA OPERATIONS (ex. RHODIA SILICES)",null,"En cours",null,null,"En cours","69063","COLLONGES AU MONT D'OR","RHONE","AUVERGNE-RHONE-ALPES","Point",4.847806,45.8284,"D3 - Chimie, phytosanitaire, pharmacie"]
["SSP000851401","69.0045","CHIMIOTECHNIC",null,"En cours",null,null,"En cours","69259","VENISSIEUX","RHONE","AUVERGNE-RHONE-ALPES","Point",4.8836994,45.709026,"D62 - Fabrication de détergents"]
["SSP000851801","69.0051","SITA REKEM (ex LABO SERVICES)",null,"En cours",null,null,"En cours","69091","GIVORS","RHONE","AUVERGNE-RHONE-ALPES","Point",4.7982006,45.57094,"K35 - Regroupement, reconditionnement de déchets"]
["SSP000852501","69.0059","GIVAUDAN FRANCE FRAGRANCES (GFF)",null,"En cours",null,null,"En cours","69123","LYON","RHONE","AUVERGNE-RHONE-ALPES","Point",4.861105,45.73256,"D6 - Parfumerie, produits savonniers, détergents"]
["SSP000853001","61.0048","FRESNAU'TO CASSE",null,"En cours",null,null,"En cours","61015","AUNOU SUR ORNE","ORNE","NORMANDIE","Point",0.23198135,48.623917]
["SSP000853101","69.0063","SHC / AVISA",null,"En cours",null,null,"En cours","69297","TERNAY","RHONE","AUVERGNE-RHONE-ALPES","Point",4.7890673,45.591927,"J51 - Fonderie des métaux ferreux"]
["SSP000853701","69.0075","Societe du Depot de Saint Priest (SDSP)",null,"En cours",null,null,"En cours","69290","SAINT PRIEST","RHONE","AUVERGNE-RHONE-ALPES","Point",4.9156523,45.689453]
["SSP000854101","57.0104","RETIA - Site de Marienau",null,"En cours",null,null,"En cours","57227","FORBACH","MOSELLE","GRAND EST","Point",6.8677173,49.178616,"D33 - Pétrochimie carbochimie organique"]
["SSP000854601","69.0084","VALEO PARIS RHONE",null,"En cours",null,null,"En cours","69123","LYON","RHONE","AUVERGNE-RHONE-ALPES","Point",4.875171,45.734684]
["SSP000854701","69.0085","ACTIS",null,"En cours",null,null,"En cours","69063","COLLONGES AU MONT D'OR","RHONE","AUVERGNE-RHONE-ALPES","Point",4.8507833,45.8242,"K3 - Traitement de déchets industriels"]
["SSP000855101","54.0070","CENTRALE THERMIQUE EDF DE BLENOD LES PONT A MOUSSON","Pollution due au fonctionnement de l'installation","En cours",null,null,"En cours","54079","BLENOD LES PONT A MOUSSON","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",6.084757,48.86997,"I11 - Centrales électriques thermiques"]
["SSP000855501","10.0021","VALCO (ex CAUVAL INDUSTRIES, ex DUMESTE)",null,"En cours",null,null,"En cours","10033","BAR SUR AUBE","AUBE","GRAND EST","Point",4.7162714,48.232765,"C12 - Produits en bois, ameublement (fabrication de)"]
["SSP000856101","92.0102","TOTAL RAFFINAGE MARKETTING",null,"En cours",null,null,"En cours","92012","BOULOGNE BILLANCOURT","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.2384508,48.835907,"L23 - Détail de carburants"]
["SSP000856201","10.0024","Société Troyenne de Teinture",null,"En cours",null,null,"En cours","10387","TROYES","AUBE","GRAND EST","Point",4.0760565,48.292534,"E13 - Blanchiment, teinture, impression"]
["SSP000856801","65.0004","ALCAN ARC",null,"En cours",null,null,"En cours","65092","BEYREDE JUMET","HAUTES-PYRENEES","OCCITANIE","Point",0.32981992,42.955124,"J41 - Ferro-alliages, abrasifs (industrie des)"]
["SSP000857301","65.0007","ALSTOM TRANSPORT SA (ex ALSTOM ex GEC ALSTHOM)",null,"En cours",null,null,"En cours","65417","SEMEAC","HAUTES-PYRENEES","OCCITANIE","Point",0.10996968,43.22866,"H1 - Mécanique, électrique, traitement de surface"]
["SSP000857501","65.0008","EADS SOCATA (ex SOCATA)",null,"En cours",null,null,"En cours","65284","LOUEY","HAUTES-PYRENEES","OCCITANIE","Point",0.01750114,43.178783,"H1 - Mécanique, électrique, traitement de surface"]
["SSP000857901","76.0207","UIOM Le Havre (ancien site de l') / NOVERGIE CENTRE OUEST",null,"En cours",null,null,"En cours","76351","LE HAVRE","SEINE-MARITIME","NORMANDIE","Point",0.15471132,49.477516,"K31 - Incinération"]
["SSP000858401","73.0030","USINE CEZUS",null,"En cours",null,null,"En cours","73303","UGINE","SAVOIE","AUVERGNE-RHONE-ALPES","Point",6.4316664,45.749245,"J5 - Fonderie et travail des métaux"]
["SSP000858801","73.0031","UGITECH  (site d'exploitation) ex Société UGINE-SAVOIE IMPHY",null,"En cours",null,null,"En cours","73303","UGINE","SAVOIE","AUVERGNE-RHONE-ALPES","Point",6.42948,45.74742,"J22 - Production d'acier brut, aciéries"]
["SSP000859301","02.0011","Déposante de VILLENEUVE ST GERMAIN",null,"En cours",null,null,"En cours","02805","VILLENEUVE SAINT GERMAIN","AISNE","HAUTS-DE-FRANCE","Point",3.3598166,49.382404,"K36 - Mise en décharge"]
["SSP000859601","80.0013","Darkiewicz",null,"En cours",null,null,"En cours","80162","CAIX","SOMME","HAUTS-DE-FRANCE","Point",2.6515381,49.813477,"H13 - Traitement de surface"]
["SSP000859801","80.0012","EVONIK REXIM",null,"En cours",null,null,"En cours","80410","HAM","SOMME","HAUTS-DE-FRANCE","Point",3.0821517,49.74311]
["SSP000860301","68.0065","SASCA (AEROPORT BALE-MULHOUSE)",null,"En cours",null,null,"En cours","68297","SAINT LOUIS","HAUT-RHIN","GRAND EST","Point",7.555753,47.59345,"D1 - Industrie pétrolière, gaz naturel"]
["SSP000860501","81.0010","RIAL SAS",null,"En cours",null,null,"En cours","81039","BRIATEXTE","TARN","OCCITANIE","Point",1.9330953,43.760723,"E2 - Industrie des cuirs et peaux, tannerie"]
["SSP000860801","81.0014","SEPIPROD (ex SEPPIC)",null,"En cours",null,null,"En cours","81065","CASTRES","TARN","OCCITANIE","Point",2.229186,43.589836,"D3 - Chimie, phytosanitaire, pharmacie"]
["SSP000861301","31.0034","AIRBUS OPERATIONS - USINE DE SAINT MARTIN DU TOUCH",null,"En cours",null,null,"En cours","31555","TOULOUSE","HAUTE-GARONNE","OCCITANIE","Point",1.3550197,43.609505,"H1 - Mécanique, électrique, traitement de surface"]
["SSP000861701","95.0012","USINE VASSET",null,"En cours",null,null,"En cours","95229","EZANVILLE","VAL-D'OISE","ILE-DE-FRANCE","Point",2.365583,49.033504]
["SSP000862301","92.0094","CHIMICOLOR",null,"En cours",null,null,"En cours","92035","LA GARENNE COLOMBES","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.2527142,48.912018,"H13 - Traitement de surface"]
["SSP000862601","31.0044","ZINCAL",null,"En cours",null,null,"En cours","31555","TOULOUSE","HAUTE-GARONNE","OCCITANIE","Point",1.4086367,43.55237,"H13 - Traitement de surface"]
["SSP000862801","73.0033","FERROPEM - Usine de Château-Feuillet",null,"En cours",null,null,"En cours","73187","LA LECHERE","SAVOIE","AUVERGNE-RHONE-ALPES","Point",6.4851294,45.522816]
["SSP000863301","12.0009","INCINERATION D'ORDURES MENAGERES - SICTOM DE CAMARES",null,"En cours",null,null,"En cours","12044","CAMARES","AVEYRON","OCCITANIE","Point",2.9075556,43.83564,"K2 - Traitement de déchets urbains"]
["SSP000863501","74.0023","Site historique de Chedde – usine SGL Carbon",null,"En cours",null,null,"En cours","74208","PASSY","HAUTE-SAVOIE","AUVERGNE-RHONE-ALPES","Point",6.728631,45.92627,"J42 - Fabrication d'électrodes"]
["SSP000864001","74.0024","Site historique de Chedde – ancienne usine PEM",null,"En cours",null,null,"En cours","74208","PASSY","HAUTE-SAVOIE","AUVERGNE-RHONE-ALPES","Point",6.7282763,45.927135,"J42 - Fabrication d'électrodes"]
["SSP000864501","76.0061","ANCIENNE USINE BAYARD",null,"En cours",null,null,"En cours","76624","SAINT NICOLAS D'ALIERMONT","SEINE-MARITIME","NORMANDIE","Point",1.2417821,49.87691,"H13 - Traitement de surface"]
["SSP000864901","76.0067","ALSTHOM",null,"En cours",null,null,"En cours","76351","LE HAVRE","SEINE-MARITIME","NORMANDIE","Point",0.14681111,49.496174,"M1 - Industries diverses"]
["SSP000865401","52.0018","FORGES DE FRONCLES",null,"En cours",null,null,"En cours","52211","FRONCLES","HAUTE-MARNE","GRAND EST","Point",5.135759,48.298077,"J53 - Travail des métaux, chaudronnerie, poudres"]
["SSP000865701","16.0008","Leroy Somer - Fonderie de Rabion",null,"En cours",null,null,"En cours","16015","ANGOULEME","CHARENTE","NOUVELLE-AQUITAINE","Point",0.13189243,45.638336,"J5 - Fonderie et travail des métaux"]
["SSP000865901","03.0009","DUNLOP - Site de production",null,"En cours",null,null,"En cours","03185","MONTLUCON","ALLIER","AUVERGNE-RHONE-ALPES","Point",2.5888212,46.37041,"D71 - Industrie du caoutchouc"]
["SSP000866201","76.0081","RALSTON",null,"En cours",null,null,"En cours","76165","CAUDEBEC LES ELBEUF","SEINE-MARITIME","NORMANDIE","Point",1.026756,49.291824,"H16 - Piles électriques et accumulateurs (fabrication de)"]
["SSP000866801","12.0012","ROBERT BOSCH",null,"En cours",null,null,"En cours","12176","ONET LE CHATEAU","AVEYRON","OCCITANIE","Point",2.6001709,44.360203,"H1 - Mécanique, électrique, traitement de surface"]
["SSP000866901","76.0086","CHEVRON CHEMICAL \"Petit Canal\"",null,"En cours",null,null,"En cours","76305","GONFREVILLE L'ORCHER","SEINE-MARITIME","NORMANDIE","Point",0.21350822,49.488613,"D33 - Pétrochimie carbochimie organique"]
["SSP000867501","12.0015","ANCIENNE PLATEFORME D'ELECTROLYSE (ex site VIEILLE MONTAGNE)",null,"En cours",null,null,"En cours","12305","VIVIEZ","AVEYRON","OCCITANIE","Point",2.219439,44.557106]
["SSP000867901","12.0018","SOFT (SUD OUEST FIOUL TOTAL)",null,"En cours",null,null,"En cours","12083","CRANSAC","AVEYRON","OCCITANIE","Point",2.2709918,44.52369,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000868501","17.0010","DEPOT PORTUAIRE D'HYDROCARBURES LIQUIDES",null,"En cours",null,null,"En cours","17300","LA ROCHELLE","CHARENTE-MARITIME","NOUVELLE-AQUITAINE","Point",-1.2096738,46.16861,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000868901","974.0022","décharge d'ordures ménagères de la Route du Volcan",null,"En cours",null,null,"En cours","97422","LE TAMPON","LA REUNION","LA REUNION","Point",55.58498,-21.20585,"K21 - Décharges d'ordures ménagères"]
["SSP000869101","12.0019","ZI DU CENTRE",null,"En cours",null,null,"En cours","12089","DECAZEVILLE","AVEYRON","OCCITANIE","Point",2.2563581,44.568657,"J2 - Sidérurgie, première transformation"]
["SSP000869401","76.0098","ESSO PIPE 10 TJ",null,"En cours",null,null,"En cours","76305","GONFREVILLE L'ORCHER","SEINE-MARITIME","NORMANDIE","Point",0.22544405,49.501163]
["SSP000870201","38.0040","TECUMSEH EUROPE",null,"En cours",null,null,"En cours","38537","LA VERPILLIERE","ISERE","AUVERGNE-RHONE-ALPES","Point",5.1386814,45.63976]
["SSP000870401","02.0019","Ancien dépôt BP FRANCE",null,"En cours",null,null,"En cours","02168","CHATEAU THIERRY","AISNE","HAUTS-DE-FRANCE","Point",3.4001322,49.03872,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000870901","31.0049","BASF - HCP",null,"En cours",null,null,"En cours","31084","BOUSSENS","HAUTE-GARONNE","OCCITANIE","Point",0.9696379,43.170486,"D33 - Pétrochimie carbochimie organique"]
["SSP000871301","63.0045","Station TOTAL LAGARDE",null,"En cours",null,null,"En cours","63291","PUY GUILLAUME","PUY-DE-DOME","AUVERGNE-RHONE-ALPES","Point",3.4772308,45.95541,"L23 - Détail de carburants"]
["SSP000871701","02.0024","FISCHER SCIENTIFIC (ex OSI)",null,"En cours",null,null,"En cours","02580","OULCHY LE CHATEAU","AISNE","HAUTS-DE-FRANCE","Point",3.3818128,49.206276,"D - Chimie, parachimie, pétrole"]
["SSP000871901","03.0012","ERASTEEL COMMENTRY",null,"En cours",null,null,"En cours","03082","COMMENTRY","ALLIER","AUVERGNE-RHONE-ALPES","Point",2.743912,46.287506,"J23 - Première transformation de l'acier"]
["SSP000872601","27.0029","Société MSA Station TOTAL Relais de Saint Just",null,"En cours",null,null,"En cours","27554","SAINT JUST","EURE","NORMANDIE","Point",1.4504445,49.1115,"L23 - Détail de carburants"]
["SSP000873001","80.0015","PARICHE",null,"En cours",null,null,"En cours","80120","BOUILLANCOURT EN SERY","SOMME","HAUTS-DE-FRANCE","Point",1.6321532,49.964565,"H13 - Traitement de surface"]
["SSP000873801","80.0020","DEPA",null,"En cours",null,null,"En cours","80651","LE QUESNE","SOMME","HAUTS-DE-FRANCE","Point",1.7923337,49.862434]
["SSP000873901","59.0247","WOESTELANDT Tuiles-Bardages-Terre Cuite",null,"En cours",null,null,"En cours","59433","NIEURLET","NORD","HAUTS-DE-FRANCE","Point",2.2805169,50.793304,"G1 - Céramique, verre, matériaux de construction"]
["SSP000874601","83.0008","DPCA (Ex GPCA 1)",null,"En cours",null,null,"En cours","83099","PUGET SUR ARGENS","VAR","PROVENCE-ALPES-COTE D'AZUR","Point",6.6807847,43.44922,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000875201","83.0007","Entrepot Pétrolier de Puget sur Argens (EPPA)",null,"En cours",null,null,"En cours","83099","PUGET SUR ARGENS","VAR","PROVENCE-ALPES-COTE D'AZUR","Point",6.6942906,43.447975,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000875601","63.0008","Anciens Ets TEILHOL",null,"En cours",null,null,"En cours","63125","COURPIERE","PUY-DE-DOME","AUVERGNE-RHONE-ALPES","Point",3.539339,45.76627,"H14 - Application de peinture"]
["SSP000875701","60.0024","REGEAL (ex RECOVCO AFFIMET)",null,"En cours",null,null,"En cours","60159","COMPIEGNE","OISE","HAUTS-DE-FRANCE","Point",2.8396811,49.430588,"J3 - Métallurgie des métaux non ferreux, affinage"]
["SSP000876201","60.0030","DISFLEX FRANCE",null,"En cours",null,null,"En cours","60106","BREUIL LE SEC","OISE","HAUTS-DE-FRANCE","Point",2.4574978,49.381424,"H13 - Traitement de surface"]
["SSP000876601","03.0015","SAGEM",null,"En cours",null,null,"En cours","03101","DOMERAT","ALLIER","AUVERGNE-RHONE-ALPES","Point",2.5466585,46.370895,"H1 - Mécanique, électrique, traitement de surface"]
["SSP000877301","01.0018","SPEICHIM PROCESSING",null,"En cours",null,null,"En cours","01390","SAINT VULBAS","AIN","AUVERGNE-RHONE-ALPES","Point",5.2641025,45.835278,"K4 - Activité de régénération"]
["SSP000877401","01.0019","THEVENIN DUCROT DISTRIBUTION",null,"Clôturée",null,"2002-02-28","Clôturée","01283","OYONNAX","AIN","AUVERGNE-RHONE-ALPES","Point",5.6427226,46.253746]
["SSP000877801","67.0197","BARUCH & FISCH (Rue de Dorlisheim)",null,"En cours",null,null,"En cours","67411","ROSHEIM","BAS-RHIN","GRAND EST","Point",7.4876676,48.504707]
["SSP000878301","38.0032","HYDRA BOCOTON",null,"En cours",null,null,"En cours","38318","PONT EVEQUE","ISERE","AUVERGNE-RHONE-ALPES","Point",4.9027987,45.529465,"E11 - Peignage, cardage des fibres textiles"]
["SSP000878801","38.0035","TOTAL RAFFINAGE FRANCE",null,"En cours",null,null,"En cours","38215","LUZINAY","ISERE","AUVERGNE-RHONE-ALPES","Point",4.930884,45.573116]
["SSP000878901","26.0012","S.A CHEDDITE FRANCE",null,"En cours",null,null,"En cours","26058","BOURG LES VALENCE","DROME","AUVERGNE-RHONE-ALPES","Point",4.8909082,44.95305,"J53 - Travail des métaux, chaudronnerie, poudres"]
["SSP000879601","69.0095","BODYCOTE - HIT TS",null,"En cours",null,null,"En cours","69271","CHASSIEU","RHONE","AUVERGNE-RHONE-ALPES","Point",4.966708,45.732647,"H - Mécanique, traitements des surfaces"]
["SSP000880001","69.0091","ENTREPOT PETROLIER de LYON (EPL)",null,"En cours",null,null,"En cours","69123","LYON","RHONE","AUVERGNE-RHONE-ALPES","Point",4.8312235,45.71461,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000880501","38.0045","SCHNEIDER ELECTRIC TEC 38  (Ex. Usine A)",null,"En cours",null,null,"En cours","38185","GRENOBLE","ISERE","AUVERGNE-RHONE-ALPES","Point",5.7119055,45.203075,"H1 - Mécanique, électrique, traitement de surface"]
["SSP000880701","84.0005","Coopérative Agricole Provence Languedoc (CAPL)",null,"En cours",null,null,"En cours","84129","SORGUES","VAUCLUSE","PROVENCE-ALPES-COTE D'AZUR","Point",4.8759394,44.00257,"L13 - Entrepôts de produits dangereux"]
["SSP000881001","69.0096","GIVAUDAN LAVIROTTE",null,"En cours",null,null,"En cours","69123","LYON","RHONE","AUVERGNE-RHONE-ALPES","Point",4.8621483,45.73336]
["SSP000881601","38.0049","STEELMAG (ex. UGIMAG FRANCE)",null,"En cours",null,null,"En cours","38439","SAINT PIERRE D'ALLEVARD","ISERE","AUVERGNE-RHONE-ALPES","Point",6.047824,45.372173,"J53 - Travail des métaux, chaudronnerie, poudres"]
["SSP000882001","38.0053","FONDERIE BOT",null,"En cours",null,null,"En cours","38563","VOIRON","ISERE","AUVERGNE-RHONE-ALPES","Point",5.5972123,45.360817,"J51 - Fonderie des métaux ferreux"]
["SSP000882101","38.0054","ALUMINIUM PECHINEY - Usine de Rioupéroux",null,"En cours",null,null,"En cours","38212","LIVET ET GAVET","ISERE","AUVERGNE-RHONE-ALPES","Point",5.900939,45.08794,"J32 - Métallurgie de l'aluminium"]
["SSP000882701","69.0104","BAYER CROPSCIENCE - Centre de la Dargoire",null,"En cours",null,null,"En cours","69123","LYON","RHONE","AUVERGNE-RHONE-ALPES","Point",4.812307,45.79124,"D37 - Phytosanitaires, pesticides (fabrication de)"]
["SSP000883001","69.0101","SOLVAY usine SAINT-FONS CHIMIE (ex- RHODIA OPERATIONS (ex-Organique))",null,"En cours",null,null,"En cours","69199","SAINT FONS","RHONE","AUVERGNE-RHONE-ALPES","Point",4.8461604,45.70255,"D32 - Chimie minérale inorganique autre"]
["SSP000883501","69.0103","BAYER SAS (ex. BAYER CROPSCIENCE FRANCE)",null,"En cours",null,null,"En cours","69115","LIMAS","RHONE","AUVERGNE-RHONE-ALPES","Point",4.7227945,45.978363,"D37 - Phytosanitaires, pesticides (fabrication de)"]
["SSP000883801","69.0107","HUNTSMAN",null,"En cours",null,null,"En cours","69199","SAINT FONS","RHONE","AUVERGNE-RHONE-ALPES","Point",4.848414,45.706135,"D4 - Encres, vernis, peintures, colles (fabrication de)"]
["SSP000884101","69.0109","TOTAL station service autoroutière de DRACE (A6) ",null,"En cours",null,null,"En cours","69077","DRACE","RHONE","AUVERGNE-RHONE-ALPES","Point",4.7676296,46.143078,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000884901","84.0012","SNPE/EURENCO",null,"En cours",null,null,"En cours","84129","SORGUES","VAUCLUSE","PROVENCE-ALPES-COTE D'AZUR","Point",4.8581586,43.994675,"D8 - Poudres et explosifs"]
["SSP000885401","92.0044","TOTAL",null,"En cours",null,null,"En cours","92036","GENNEVILLIERS","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.2775016,48.9466,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000885501","13.0041","ARKEMA - St Menet",null,"En cours",null,null,"En cours","13055","MARSEILLE","BOUCHES-DU-RHONE","PROVENCE-ALPES-COTE D'AZUR","Point",5.5021114,43.284668,"D - Chimie, parachimie, pétrole"]
["SSP000886201","05.0004","OPTEX ",null,"En cours",null,null,"En cours","05164","SAVINES LE LAC","HAUTES-ALPES","PROVENCE-ALPES-COTE D'AZUR","Point",6.399068,44.523773,"H - Mécanique, traitements des surfaces"]
["SSP000886501","95.0020","TENCATE (ex BIDIM)",null,"En cours",null,null,"En cours","95063","BEZONS","VAL-D'OISE","ILE-DE-FRANCE","Point",2.2097356,48.919216,"D72 - Transformation des matières plastiques"]
["SSP000886801","73.0041","METALTEMPLE",null,"En cours",null,null,"En cours","73261","SAINT MICHEL DE MAURIENNE","SAVOIE","AUVERGNE-RHONE-ALPES","Point",6.4640017,45.220016]
["SSP000887201","59.0030","FRICHE THIERS  CdF",null,"En cours",null,null,"En cours","59207","ESCAUTPONT","NORD","HAUTS-DE-FRANCE","Point",3.5509193,50.42394,"F11 - Houillères"]
["SSP000887701","59.0039","FORCAST - BAIL",null,"En cours",null,null,"En cours","59068","BERLAIMONT","NORD","HAUTS-DE-FRANCE","Point",3.7958667,50.20528,"K - Déchets et traitements"]
["SSP000888101","62.0041","AFAM",null,"En cours",null,null,"En cours","62560","MARQUISE","PAS-DE-CALAIS","HAUTS-DE-FRANCE","Point",1.6962919,50.80924,"J5 - Fonderie et travail des métaux"]
["SSP000888701","62.0046","DMS (ex MORY COMBUSTIBLES) quai de la Meuse",null,"En cours",null,null,"En cours","62193","CALAIS","PAS-DE-CALAIS","HAUTS-DE-FRANCE","Point",1.8569921,50.95626,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000888801","59.0047","FONDERIE RICHARD",null,"En cours",null,null,"En cours","59230","FERRIERE LA GRANDE","NORD","HAUTS-DE-FRANCE","Point",3.9926598,50.256413,"K22 - Regroupement d'OM, DIB"]
["SSP000889201","62.0051","ROCADE PERIPHERIQUE DE SAINT OMER",null,"En cours",null,null,"En cours","62765","SAINT OMER","PAS-DE-CALAIS","HAUTS-DE-FRANCE","Point",2.2646792,50.767586,"K - Déchets et traitements"]
["SSP000889701","59.0060","ANCIENNE USINE D'AGGLOMERATION DU FORT DE SCARPE - ANTHRACINE 54",null,"En cours",null,null,"En cours","59178","DOUAI","NORD","HAUTS-DE-FRANCE","Point",3.0777402,50.380238,"F11 - Houillères"]
["SSP000889901","62.0061","OI MANUFACTURING FRANCE (ex  OI BSN GLASS PACK)",null,"En cours",null,null,"En cours","62895","WINGLES","PAS-DE-CALAIS","HAUTS-DE-FRANCE","Point",2.857463,50.494152,"G1 - Céramique, verre, matériaux de construction"]
["SSP000890301","59.0066","NORZINCO",null,"En cours",null,null,"En cours","59014","ANZIN","NORD","HAUTS-DE-FRANCE","Point",3.5270386,50.380596,"J33 - Métallurgie du plomb et du zinc"]
["SSP000890801","62.0075","INTEROR",null,"En cours",null,null,"En cours","62193","CALAIS","PAS-DE-CALAIS","HAUTS-DE-FRANCE","Point",1.8863169,50.966026,"D3 - Chimie, phytosanitaire, pharmacie"]
["SSP000891201","59.0081","ZONE 3 (SRD)",null,"En cours",null,null,"En cours","59183","DUNKERQUE","NORD","HAUTS-DE-FRANCE","Point",2.3600152,51.03063,"D12 - Raffinage de pétrole, carburants et lubrifiants"]
["SSP000891701","59.0089","MAUBEUGE CERAMIQUES",null,"En cours",null,null,"En cours","59392","MAUBEUGE","NORD","HAUTS-DE-FRANCE","Point",3.9616704,50.283623,"G12 - Fabrication de produits céramiques"]
["SSP000892001","59.0091","SCI BUREAUX DE L'ESPERANCE (ex USINOR)",null,"En cours",null,null,"En cours","59365","LOUVROIL","NORD","HAUTS-DE-FRANCE","Point",3.9464498,50.264584,"M - Divers et services"]
["SSP000892201","62.0096","UCAR",null,"En cours",null,null,"En cours","62193","CALAIS","PAS-DE-CALAIS","HAUTS-DE-FRANCE","Point",1.868174,50.952213,"D3 - Chimie, phytosanitaire, pharmacie"]
["SSP000892701","59.0111","NORDLYS",null,"En cours",null,null,"En cours","59043","BAILLEUL","NORD","HAUTS-DE-FRANCE","Point",2.7337792,50.7362,"E12 - Filtène, filature, tissage, tricotage"]
["SSP000893101","59.0120","STATION SERVICE TOTAL AUTOROUTE A2 TRITH",null,"En cours",null,null,"En cours","59603","TRITH SAINT LEGER","NORD","HAUTS-DE-FRANCE","Point",3.488314,50.32957,"I2 - Production de chaleur, chaufferies"]
["SSP000893401","59.0127","BORAX (ex SCI LE MANOIR)",null,"En cours",null,null,"En cours","59305","HERZEELE","NORD","HAUTS-DE-FRANCE","Point",2.5303702,50.87635,"K36 - Mise en décharge"]
["SSP000894001","59.0180","ANCIENNE DECHARGE GRAVELINES PORTE AUX BOULES",null,"En cours",null,null,"En cours","59273","GRAVELINES","NORD","HAUTS-DE-FRANCE","Point",2.1449258,51.002495,"K - Déchets et traitements"]
["SSP000894401","59.0191","BORAX FRANCAIS",null,"En cours",null,null,"En cours","59155","COUDEKERQUE BRANCHE","NORD","HAUTS-DE-FRANCE","Point",2.367628,51.01893,"D32 - Chimie minérale inorganique autre"]
["SSP000894901","76.0178","Ancien site NICAISE",null,"En cours",null,null,"En cours","76473","NOTRE DAME DE BLIQUETUIT","SEINE-MARITIME","NORMANDIE","Point",0.75148994,49.499874]
["SSP000895201","59.0208","Vale Manganèse (Ex RDME, es SEAS)",null,"En cours",null,null,"En cours","59271","GRANDE SYNTHE","NORD","HAUTS-DE-FRANCE","Point",2.3745432,51.028725,"J - Sidérurgie, métallurgie, coke"]
["SSP000895401","59.0218","Total Raffinage France - Appontements Pétroliers des Flandres",null,"En cours",null,null,"En cours","59273","GRAVELINES","NORD","HAUTS-DE-FRANCE","Point",2.1629865,51.010178,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000895901","59.0241","Total Raffinage marketing - Etablissement des Flandres (EF)",null,"En cours",null,null,"En cours","59359","LOON PLAGE","NORD","HAUTS-DE-FRANCE","Point",2.221827,51.000805,"D1 - Industrie pétrolière, gaz naturel"]
["SSP000896101","59.0248","TUILERIE DES FLANDRES",null,"En cours",null,null,"En cours","59433","NIEURLET","NORD","HAUTS-DE-FRANCE","Point",2.2805169,50.793304,"G1 - Céramique, verre, matériaux de construction"]
["SSP000896401","59.0266","DPC",null,"En cours",null,null,"En cours","59540","SAINT-POL-SUR-MER","NORD","HAUTS-DE-FRANCE","Point",2.3496797,51.03143,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000896901","95.0022","DASSAULT AVIATION",null,"En cours",null,null,"En cours","95018","ARGENTEUIL","VAL-D'OISE","ILE-DE-FRANCE","Point",2.2263966,48.933033]
["SSP000897501","92.0052","TRAPIL (ex SPI) TO1 NORD",null,"En cours",null,null,"En cours","92036","GENNEVILLIERS","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.2946177,48.947437,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000898201","92.0057","EDF",null,"En cours",null,null,"En cours","92036","GENNEVILLIERS","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.2598884,48.939667,"I11 - Centrales électriques thermiques"]
["SSP000898501","92.0059","ETG (ex CHAUSSON) Emboutissage Tôlerie Gennevilliers",null,"En cours",null,null,"En cours","92036","GENNEVILLIERS","HAUTS-DE-SEINE","ILE-DE-FRANCE","Point",2.2984035,48.920155,"H13 - Traitement de surface"]
["SSP000898701","26.0013","SOLYSTIC  (ex. MANNESMANN)",null,"En cours",null,null,"En cours","26058","BOURG LES VALENCE","DROME","AUVERGNE-RHONE-ALPES","Point",4.8974943,44.941536,"H - Mécanique, traitements des surfaces"]
["SSP000899001","92.0061","ex TCI",null,"En cours",null,null,"En cours","92050","NANTERRE","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.204105,48.88997,"H13 - Traitement de surface"]
["SSP000899601","06.0011","ALUCHROME","Plan de gestion - travaux","Clôturée",null,null,"Clôturée","06088","NICE","ALPES-MARITIMES","PROVENCE-ALPES-COTE D'AZUR","Polygone",7.29229,43.708443,"H13 - Traitement de surface"]
["SSP000899701","26.0017","SCAPA FRANCE",null,"En cours",null,null,"En cours","26362","VALENCE","DROME","AUVERGNE-RHONE-ALPES","Point",4.8957767,44.919617,"H12 - Traitement thermique"]
["SSP000900201","61.0013","FAURECIA - le Bois de Flers",null,"En cours",null,null,"En cours","61391","SAINT GEORGES DES GROSEILLERS","ORNE","NORMANDIE","Point",-0.56580806,48.770935,"H11 - Usinage"]
["SSP000900601","61.0018","TANNERIE DU PERCHE",null,"Clôturée",null,"2013-08-27","Clôturée","61491","TOUROUVRE","ORNE","NORMANDIE","Point",0.6567644,48.59916,"E2 - Industrie des cuirs et peaux, tannerie"]
["SSP000901201","51.0024","LE BRONZE INDUSTRIEL",null,"En cours",null,null,"En cours","51559","SUIPPES","MARNE","GRAND EST","Point",4.525059,49.125504,"J35 - Autres métaux non ferreux (métallurgie des)"]
["SSP000901301","14.0012","DPC",null,"En cours",null,null,"En cours","14437","MONDEVILLE","CALVADOS","NORMANDIE","Point",-0.3292432,49.182285,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000901801","14.0018","KNORR BREMSE",null,"En cours",null,null,"En cours","14366","LISIEUX","CALVADOS","NORMANDIE","Point",0.22152124,49.155987]
["SSP000902101","33.0435","PONTICELLI Frères",null,"En cours",null,null,"En cours","33004","AMBES","GIRONDE","NOUVELLE-AQUITAINE","Point",-0.5063211,45.00151]
["SSP000902701","77.0099","ROBBE Frères","ROBBE Frères","En cours",null,null,"En cours","77448","SEPT SORTS","SEINE-ET-MARNE","ILE-DE-FRANCE","Polygone",3.1067507,48.94711,"H1 - Mécanique, électrique, traitement de surface"]
["SSP000902801","92.0065","VLG CHEM (Ex AVENTIS PHARMA)",null,"En cours",null,null,"En cours","92078","VILLENEUVE LA GARENNE","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.3240364,48.93403,"D38 - Industrie pharmaceutique"]
["SSP000903501","51.0028","JEAN et CHAUMONT",null,"En cours",null,null,"En cours","51573","TINQUEUX","MARNE","GRAND EST","Point",3.983184,49.238865,"H13 - Traitement de surface"]
["SSP000903901","63.0017","AUBERT et DUVAL",null,"En cours",null,null,"En cours","63004","LES ANCIZES COMPS","PUY-DE-DOME","AUVERGNE-RHONE-ALPES","Point",2.807149,45.93787,"J23 - Première transformation de l'acier"]
["SSP000904401","51.0031","DOCHEX (ex Mac Dermid - ex SPCD - ex. FRAPPAZ)",null,"En cours",null,null,"En cours","51217","DORMANS","MARNE","GRAND EST","Point",3.6400385,49.063812,"H1 - Mécanique, électrique, traitement de surface"]
["SSP000904601","13.0026","RIO TINTO - ALCAN (Ex Aluminium Pechiney)",null,"En cours",null,null,"En cours","13041","GARDANNE","BOUCHES-DU-RHONE","PROVENCE-ALPES-COTE D'AZUR","Point",5.4919763,43.45296,"J31 - Fabrication d'alumine"]
["SSP000905101","71.0016","REXAM SMT",null,"En cours",null,null,"En cours","71543","TOURNUS","SAONE-ET-LOIRE","BOURGOGNE-FRANCHE-COMTE","Point",4.9138293,46.565296,"D72 - Transformation des matières plastiques"]
["SSP000905601","13.0032","EPC France (Ex NITROCHIMIE)",null,"En cours",null,null,"En cours","13097","SAINT MARTIN DE CRAU","BOUCHES-DU-RHONE","PROVENCE-ALPES-COTE D'AZUR","Polygone",4.779039,43.608925,"D81 - Poudres et explosifs (fabrication de)"]
["SSP000906401","51.0036","GANTOIS",null,"En cours",null,null,"En cours","51250","FISMES","MARNE","GRAND EST","Point",-132.84375,-88.279305,"H1 - Mécanique, électrique, traitement de surface"]
["SSP000906701","51.0039","VALEO THERMIQUE MOTEUR",null,"En cours",null,null,"En cours","51454","REIMS","MARNE","GRAND EST","Point",4.010589,49.27002,"H - Mécanique, traitements des surfaces"]
["SSP000907101","93.0034","VALEO",null,"En cours",null,null,"En cours","93008","BOBIGNY","SEINE-SAINT-DENIS","ILE-DE-FRANCE","Point",2.4242296,48.903557,"H1 - Mécanique, électrique, traitement de surface"]
["SSP000907701","13.0050","EIFFEL Industrie (Ex CAMOM, Ex SOPDECHIM)",null,"En cours",null,null,"En cours","13081","ROGNAC","BOUCHES-DU-RHONE","PROVENCE-ALPES-COTE D'AZUR","Point",5.2099013,43.49663,"K32 - Traitements physico-chimiques"]
["SSP000908101","13.0060","PROTEC METAUX ARENC - PMA",null,"En cours",null,null,"En cours","13055","MARSEILLE","BOUCHES-DU-RHONE","PROVENCE-ALPES-COTE D'AZUR","Polygone",5.3578544,43.346928,"H13 - Traitement de surface"]
["SSP000908201","13.0062","DAHER INTERNATIONAL (Ex PROVENCE STOCK SERVICE)",null,"En cours",null,null,"En cours","13004","ARLES","BOUCHES-DU-RHONE","PROVENCE-ALPES-COTE D'AZUR","Point",4.6316957,43.705494,"L13 - Entrepôts de produits dangereux"]
["SSP000908701","13.0069","CPB - DEPOT DU PORT DE LA POINTE",null,"En cours",null,null,"En cours","13014","BERRE L'ETANG","BOUCHES-DU-RHONE","PROVENCE-ALPES-COTE D'AZUR","Point",5.1487794,43.459995,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000909101","13.0073","CPB - UCB",null,"En cours",null,null,"En cours","13014","BERRE L'ETANG","BOUCHES-DU-RHONE","PROVENCE-ALPES-COTE D'AZUR","Point",5.1729436,43.49916,"D - Chimie, parachimie, pétrole"]
["SSP000909701","13.0080","AZUR CHIMIE (site entier)",null,"En cours",null,null,"En cours","13077","PORT DE BOUC","BOUCHES-DU-RHONE","PROVENCE-ALPES-COTE D'AZUR","Polygone",5.0009737,43.406094,"D - Chimie, parachimie, pétrole"]
["SSP000910101","77.0026","WIPELEC","WIPELEC","En cours",null,null,"En cours","77372","POMPONNE","SEINE-ET-MARNE","ILE-DE-FRANCE","Polygone",2.6966891,48.88103,"H1 - Mécanique, électrique, traitement de surface"]
["SSP000910501","13.0087","DEULEP",null,"En cours",null,null,"En cours","13078","PORT SAINT LOUIS DU RHONE","BOUCHES-DU-RHONE","PROVENCE-ALPES-COTE D'AZUR","Polygone",4.828587,43.38817,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000911101","13.0091","LEGRE   MANTE  Ancienne usine en activité (Partie C)",null,"En cours",null,null,"En cours","13055","MARSEILLE","BOUCHES-DU-RHONE","PROVENCE-ALPES-COTE D'AZUR","Point",5.357909,43.23207,"D - Chimie, parachimie, pétrole"]
["SSP000911701","13.0096","DEPOTS PETROLIERS DE FOS (DPF)",null,"En cours",null,null,"En cours","13039","FOS SUR MER","BOUCHES-DU-RHONE","PROVENCE-ALPES-COTE D'AZUR","Point",4.9160485,43.43512,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000911801","13.0097","L'ESCALETTE - Terrains Conseil Général",null,"En cours",null,null,"En cours","13055","MARSEILLE","BOUCHES-DU-RHONE","PROVENCE-ALPES-COTE D'AZUR","Point",5.3513865,43.22514,"J52 - Fonderie des métaux non ferreux"]
["SSP000912201","69.0113","Ancienne usine à gaz et Poste de détente de gaz de Lyon la Mouche",null,"En cours",null,null,"En cours","69123","LYON","RHONE","AUVERGNE-RHONE-ALPES","Point",4.8453536,45.726532,"J1 - Cokéfaction, usines à gaz"]
["SSP000913301","57.0129","SOCIETE CHRISTOPH",null,"En cours",null,null,"En cours","57618","SAINT LOUIS","MOSELLE","GRAND EST","Point",7.185388,48.71737,"L23 - Détail de carburants"]
["SSP000914601","59.0287","AGENCES CLIENTELE ET D'EXPLOITATION D'EDF / GDF",null,"En cours",null,null,"En cours","59155","COUDEKERQUE BRANCHE","NORD","HAUTS-DE-FRANCE","Point",2.3709238,51.016247,"J1 - Cokéfaction, usines à gaz"]
["SSP000914801","59.0284","AGENCES CLIENTELE ET D'EXPLOITATION D'EDF / GDF",null,"En cours",null,null,"En cours","59043","BAILLEUL","NORD","HAUTS-DE-FRANCE","Point",2.7178857,50.73886]
["SSP000915101","60.0031","Agence clientèle EDF-GDF Services",null,"En cours",null,null,"En cours","60581","SAINT JUST EN CHAUSSEE","OISE","HAUTS-DE-FRANCE","Point",2.416858,49.517982,"J1 - Cokéfaction, usines à gaz"]
["SSP000915601","26.0047","CNPE du Tricastin",null,"En cours",null,null,"En cours","26324","SAINT PAUL TROIS CHATEAUX","DROME","AUVERGNE-RHONE-ALPES","Point",4.729427,44.33063]
["SSP000916001","80.0025","Agence d'exploitation et agence clientèle d'EDF / GDF",null,"En cours",null,null,"En cours","80253","DOULLENS","SOMME","HAUTS-DE-FRANCE","Point",2.3398252,50.15971]
["SSP000916101","80.0026","Installation technique de Gaz de France",null,"En cours",null,null,"En cours","80410","HAM","SOMME","HAUTS-DE-FRANCE","Point",3.0700858,49.753036]
["SSP000916501","60.0033","Ancienne usine à gaz",null,"En cours",null,null,"En cours","60360","LIANCOURT","OISE","HAUTS-DE-FRANCE","Point",2.4630435,49.331192]
["SSP000917001","54.0127","Garage Peugeot, Réparation Automobile Nancéenne (RAN)","Cessation d'activités 2014","En cours",null,null,"En cours","54304","LAXOU","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",6.1250763,48.694065,null,null,null,"45.20B - Entretien et réparation d'autres véhicules automobiles"]
["SSP000917601","13.0103","Agence EDF / GDF Services",null,"En cours",null,null,"En cours","13005","AUBAGNE","BOUCHES-DU-RHONE","PROVENCE-ALPES-COTE D'AZUR","Point",5.5671635,43.293617]
["SSP000917801","80.0031","Centre EDF-GDF Services Pays de Somme",null,"En cours",null,null,"En cours","80021","AMIENS","SOMME","HAUTS-DE-FRANCE","Point",2.2815676,49.89117,"J1 - Cokéfaction, usines à gaz"]
["SSP000918101","89.0030","MATREX PRODUCTIONS ",null,"En cours",null,null,"En cours","89464","VILLENEUVE SUR YONNE","YONNE","BOURGOGNE-FRANCHE-COMTE","Point",3.32593,48.07795,"G14 - Fabrication d'autres matériaux de construction"]
["SSP000918701","33.0146","POUMEYRAU",null,"En cours",null,null,"En cours","33498","SALLES","GIRONDE","NOUVELLE-AQUITAINE","Point",-0.8779742,44.54602]
["SSP000919101","2A.0001","Ancienne usine à gaz",null,"En cours",null,"2012-09-04","En cours","2A004","AJACCIO","CORSE-DU-SUD","CORSE","Point",8.726014,41.912804,"J1 - Cokéfaction, usines à gaz"]
["SSP000919201","60.0039","Agence EDF GDF",null,"En cours",null,null,"En cours","60175","CREIL","OISE","HAUTS-DE-FRANCE","Point",2.4690225,49.261345,"J1 - Cokéfaction, usines à gaz"]
["SSP000919701","60.0042","Ancienne usine à gaz de Neuilly-en-Thelle (60)",null,"En cours",null,null,"En cours","60450","NEUILLY EN THELLE","OISE","HAUTS-DE-FRANCE","Point",2.2758222,49.229424,"J1 - Cokéfaction, usines à gaz"]
["SSP000920201","21.0022","SEB (site de la décharge de boues)",null,"En cours",null,null,"En cours","21317","IS SUR TILLE","COTE-D'OR","BOURGOGNE-FRANCHE-COMTE","Point",5.116898,47.53052,"K36 - Mise en décharge"]
["SSP000920501","62.0111","EDF GDF SERVICES - CÔTE D'OPALE",null,"En cours",null,null,"En cours","62160","BOULOGNE SUR MER","PAS-DE-CALAIS","HAUTS-DE-FRANCE","Point",1.6104518,50.718765,"J1 - Cokéfaction, usines à gaz"]
["SSP000920701","62.0112","EDF GDF SERVICES",null,"En cours",null,null,"En cours","62826","LE TOUQUET PARIS PLAGE","PAS-DE-CALAIS","HAUTS-DE-FRANCE","Point",1.5907217,50.523727,"J1 - Cokéfaction, usines à gaz"]
["SSP000921701","50.0014","Ancienne usine à gaz",null,"Clôturée",null,null,"Clôturée","50147","COUTANCES","MANCHE","NORMANDIE","Polygone",-1.4453841,49.034924,"J1 - Cokéfaction, usines à gaz"]
["SSP000922301","973.0005","ELA N°1",null,"En cours",null,null,"En cours","97304","KOUROU","GUYANE","GUYANE","Point",0.0,0.0]
["SSP000922701","14.0042","Dépôt de résidus de broyage à Fontenay le Pesnel",null,"En cours",null,null,"En cours","14278","FONTENAY LE PESNEL","CALVADOS","NORMANDIE","Point",-0.5912076,49.16366,"K3 - Traitement de déchets industriels"]
["SSP000922801","02.0033","Centre EDF GDF Services Pays de l'Aisne",null,"En cours",null,null,"En cours","02738","TERGNIER","AISNE","HAUTS-DE-FRANCE","Point",3.2948575,49.64957,"J1 - Cokéfaction, usines à gaz"]
["SSP000923301","13.0114","ESSO RAFFINERIE",null,"En cours",null,null,"En cours","13039","FOS SUR MER","BOUCHES-DU-RHONE","PROVENCE-ALPES-COTE D'AZUR","Point",4.9246883,43.445694,"D12 - Raffinage de pétrole, carburants et lubrifiants"]
["SSP000923801","08.0024","IDEAL STANDARD FRANCE (usine)",null,"En cours",null,null,"En cours","08363","REVIN","ARDENNES","GRAND EST","Point",4.6478915,49.936794,"G1 - Céramique, verre, matériaux de construction"]
["SSP000924101","08.0027","fonderie VAL THOME",null,"En cours",null,null,"En cours","08328","NOUZONVILLE","ARDENNES","GRAND EST","Point",4.763292,49.815025,"J51 - Fonderie des métaux ferreux"]
["SSP000924301","08.0029","BEROUDIAUX SA",null,"En cours",null,null,"En cours","08363","REVIN","ARDENNES","GRAND EST","Point",4.627513,49.937584,"J51 - Fonderie des métaux ferreux"]
["SSP000925101","77.0058","SICA de GOUAIX","SICA de GOUAIX","En cours",null,null,"En cours","77208","GOUAIX","SEINE-ET-MARNE","ILE-DE-FRANCE","Polygone",3.30985,48.47428,"D36 - Fabrication des engrais"]
["SSP000925601","77.0069","CORNING SA","CORNING SA","En cours",null,null,"En cours","77016","BAGNEAUX SUR LOING","SEINE-ET-MARNE","ILE-DE-FRANCE","Polygone",2.704617,48.230873,"G1 - Céramique, verre, matériaux de construction"]
["SSP000926101","973.0003","PRIPRIS DE LA CENTRALE EDF DE PARIACABO",null,"En cours",null,null,"En cours","97304","KOUROU","GUYANE","GUYANE","Point",0.0,0.0]
["SSP000926201","95.0031","CEFIVAL",null,"En cours",null,null,"En cours","95487","PERSAN","VAL-D'OISE","ILE-DE-FRANCE","Point",2.2863543,49.14727,"H - Mécanique, traitements des surfaces"]
["SSP000926601","38.0072","Société PROGIL (ferme Morel)",null,"Clôturée",null,"2015-06-17","Clôturée","38317","LE PONT DE CLAIX","ISERE","AUVERGNE-RHONE-ALPES","Point",5.712425,45.13381]
["SSP000927301","42.0056","Station service ELF",null,"Clôturée",null,"2014-07-21","Clôturée","42218","SAINT ETIENNE","LOIRE","AUVERGNE-RHONE-ALPES","Point",4.386829,45.412018]
["SSP000928101","26.0022","KARL",null,"En cours",null,null,"En cours","26039","BEAUREGARD BARET","DROME","AUVERGNE-RHONE-ALPES","Point",5.1441708,45.047604,"K22 - Regroupement d'OM, DIB"]
["SSP000928301","26.0025","GASCON",null,"En cours",null,null,"En cours","26362","VALENCE","DROME","AUVERGNE-RHONE-ALPES","Point",4.8813367,44.897247,"H15 - Assemblage, montage"]
["SSP000929001","2A.0006","CET CAPA Saint Antoine",null,"En cours",null,null,"En cours","2A004","AJACCIO","CORSE-DU-SUD","CORSE","Point",8.685957,41.930244]
["SSP000929301","69.0121","APPIA LIANTS EMULSIONS (ex LHYR)",null,"En cours",null,null,"En cours","69063","COLLONGES AU MONT D'OR","RHONE","AUVERGNE-RHONE-ALPES","Point",4.850695,45.825027,"G14 - Fabrication d'autres matériaux de construction"]
["SSP000929801","13.0119","SOREDEM",null,"En cours",null,null,"En cours","13106","SEPTEMES LES VALLONS","BOUCHES-DU-RHONE","PROVENCE-ALPES-COTE D'AZUR","Polygone",5.3751245,43.397434,"D32 - Chimie minérale inorganique autre"]
["SSP000929901","68.0104","ANC. GRAVIERE REMBLAYEE DURRENWAECHTER",null,"En cours",null,null,"En cours","68297","SAINT LOUIS","HAUT-RHIN","GRAND EST","Polygone",7.5495768,47.581303]
["SSP000930401","64.0043","HELIOPARC",null,"Clôturée",null,"2005-04-26","Clôturée","64445","PAU","PYRENEES-ATLANTIQUES","NOUVELLE-AQUITAINE","Point",-0.36737216,43.319344,"M4 - Enseignement"]
["SSP000931001","73.0060","TOTAL Relais de Maurienne",null,"Clôturée",null,"2015-05-13","Clôturée","73074","LA CHAPELLE","SAVOIE","AUVERGNE-RHONE-ALPES","Point",6.285699,45.440987,"L2 - Transports, automobile, carburants"]
["SSP000931301","01.0034","GPO",null,"Clôturée",null,"2006-12-31","Clôturée","01341","SAINT CHAMP","AIN","AUVERGNE-RHONE-ALPES","Point",5.7352,45.78331]
["SSP000931601","28.0028","REICO",null,"En cours",null,null,"En cours","28415","VILLEMEUX SUR EURE","EURE-ET-LOIR","CENTRE-VAL DE LOIRE","Point",1.4570049,48.6683,"D21 - Stockage et conditionnement des gaz et liquéfiés"]
["SSP000932201","91.0123","SEDV",null,"En cours",null,null,"En cours","91661","VILLEBON SUR YVETTE","ESSONNE","ILE-DE-FRANCE","Point",2.2538235,48.704273,"L23 - Détail de carburants"]
["SSP000932601","42.0117","BARRIOL ET DALLIERE INDUSTRIES","Barriol et Dallière","Clôturée",null,null,"Clôturée","42005","ANDREZIEUX BOUTHEON","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.2513037,45.52672,"H11 - Usinage"]
["SSP000933201","07.0014","TRIGANO INDUSTRIES",null,"En cours",null,null,"En cours","07324","TOURNON SUR RHONE","ARDECHE","AUVERGNE-RHONE-ALPES","Point",4.827059,45.071316,"H13 - Traitement de surface"]
["SSP000933301","74.0032","SARL PASTEUR Recyclage",null,"Clôturée",null,null,"Clôturée","74298","VETRAZ MONTHOUX","HAUTE-SAVOIE","AUVERGNE-RHONE-ALPES","Point",6.254015,46.17585]
["SSP000933801","25.0025","AFFINAL INDUSTRIE",null,"En cours",null,null,"En cours","25428","NOMMAY","DOUBS","BOURGOGNE-FRANCHE-COMTE","Point",6.8516383,47.539032,"J51 - Fonderie des métaux ferreux"]
["SSP000934301","76.0116","SANOFI CHIMIE",null,"En cours",null,null,"En cours","76561","SAINT AUBIN LES ELBEUF","SEINE-MARITIME","NORMANDIE","Point",1.0081563,49.30987,"D3 - Chimie, phytosanitaire, pharmacie"]
["SSP000934801","76.0122","Compagnie industrielle maritime (CIM)",null,"En cours",null,null,"En cours","76351","LE HAVRE","SEINE-MARITIME","NORMANDIE","Point",0.1444773,49.46775,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000934901","76.0123","SEREP (Société d'études et de réalisation pour l'environnement et le procédé)",null,"En cours",null,null,"En cours","76351","LE HAVRE","SEINE-MARITIME","NORMANDIE","Point",0.13179833,49.495926,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000935601","25.0030","ROMCHANT SA",null,"En cours",null,null,"En cours","25284","GRAND CHARMONT","DOUBS","BOURGOGNE-FRANCHE-COMTE","Point",6.827695,47.525967,"L23 - Détail de carburants"]
["SSP000936001","80.0037","A & G Lenne",null,"En cours",null,null,"En cours","80235","DARGNIES","SOMME","HAUTS-DE-FRANCE","Point",1.5315439,50.043037,"H13 - Traitement de surface"]
["SSP000936201","70.0018","CONFLANDEY INDUSTRIE (EX-TREFILERIES DE CONFLANDEY)",null,"En cours",null,null,"En cours","70167","CONFLANDEY","HAUTE-SAONE","BOURGOGNE-FRANCHE-COMTE","Point",6.0500712,47.732807,"H13 - Traitement de surface"]
["SSP000936501","02.0037","DMS (ex DCA)",null,"En cours",null,null,"En cours","02598","PERNANT","AISNE","HAUTS-DE-FRANCE","Point",3.2293255,49.376938,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000937001","25.0033","LISI AUTOMOTIVE",null,"En cours",null,null,"En cours","25196","DASLE","DOUBS","BOURGOGNE-FRANCHE-COMTE","Point",6.89813,47.4787,"J53 - Travail des métaux, chaudronnerie, poudres"]
["SSP000937501","974.0011","USINE DE LA MARE",null,"En cours",null,null,"En cours","97418","SAINTE-MARIE","LA REUNION","LA REUNION","Point",-3.4045606,27.140974,"B14 - Industrie du sucre"]
["SSP000938001","67.0073","AVIA (Ancien TOTAL)",null,"En cours",null,null,"En cours","67117","ECKARTSWILLER","BAS-RHIN","GRAND EST","Point",7.328781,48.77286,"L23 - Détail de carburants"]
["SSP000938101","67.0074","CARRIERE DE SAINT-NABOR",null,"En cours",null,null,"En cours","67368","OTTROTT","BAS-RHIN","GRAND EST","Point",7.4311643,48.461212,"F32 - Carrières"]
["SSP000938701","67.0082","STATION SERVICE EBERLE",null,"En cours",null,null,"En cours","67282","MARLENHEIM","BAS-RHIN","GRAND EST","Point",7.499972,48.61975,"L23 - Détail de carburants"]
["SSP000939001","67.0086","CERAMIQUES CULINAIRES DE FRANCE",null,"En cours",null,null,"En cours","67472","SOUFFLENHEIM","BAS-RHIN","GRAND EST","Point",7.9564023,48.829933,"G12 - Fabrication de produits céramiques"]
["SSP000939201","68.0071","USINE INERGY AUTOMOTIVE SYSTEMS (ex. SOLVAY)",null,"En cours",null,null,"En cours","68256","PFASTATT","HAUT-RHIN","GRAND EST","Point",7.297582,47.7637,"D72 - Transformation des matières plastiques"]
["SSP000939501","68.0074","MR  EQUIPEMENT",null,"En cours",null,null,"En cours","68224","MULHOUSE","HAUT-RHIN","GRAND EST","Point",7.3325825,47.76814,"H - Mécanique, traitements des surfaces"]
["SSP000940001","67.0090","OUTILS WOLF",null,"En cours",null,null,"En cours","67544","WISSEMBOURG","BAS-RHIN","GRAND EST","Point",7.9499345,49.029194,"H - Mécanique, traitements des surfaces"]
["SSP000940701","33.0101","Décharge du Bourgailh",null,"En cours",null,null,"En cours","33318","PESSAC","GIRONDE","NOUVELLE-AQUITAINE","Point",-0.6866323,44.804733,"K36 - Mise en décharge"]
["SSP000941201","68.0079","Stade de Huningue, ancienne gravière Gutknecht",null,"En cours",null,null,"En cours","68349","VILLAGE NEUF","HAUT-RHIN","GRAND EST","Polygone",7.5699797,47.59369]
["SSP000941501","33.0107","LAMECOL",null,"En cours",null,null,"En cours","33281","MERIGNAC","GIRONDE","NOUVELLE-AQUITAINE","Point",-0.64187056,44.831547,"C12 - Produits en bois, ameublement (fabrication de)"]
["SSP000941701","33.0109","Galva Sud-Ouest",null,"En cours",null,null,"En cours","33318","PESSAC","GIRONDE","NOUVELLE-AQUITAINE","Point",-0.6485872,44.791767,"H13 - Traitement de surface"]
["SSP000942301","33.0114","CISMATIC",null,"Clôturée",null,"2012-03-26","Clôturée","33012","ARSAC","GIRONDE","NOUVELLE-AQUITAINE","Point",-0.72404474,44.969753,"H13 - Traitement de surface"]
["SSP000942601","33.0116","Décharge de St Girons D'Ayguevives",null,"En cours",null,null,"En cours","33416","SAINT GIRONS D'AIGUEVIVES","GIRONDE","NOUVELLE-AQUITAINE","Point",-0.5431819,45.14377,"K36 - Mise en décharge"]
["SSP000943101","40.0040","SITCOM Côte Sud Des Landes",null,"En cours",null,null,"En cours","40181","MESSANGES","LANDES","NOUVELLE-AQUITAINE","Point",-1.3624829,43.80937,"K2 - Traitement de déchets urbains"]
["SSP000943501","47.0024","BRANGE",null,"En cours",null,null,"En cours","47027","BIAS","LOT-ET-GARONNE","NOUVELLE-AQUITAINE","Point",0.6705445,44.410324,"J53 - Travail des métaux, chaudronnerie, poudres"]
["SSP000944101","64.0045","Décharge de Bacheforès",null,"En cours",null,null,"En cours","64102","BAYONNE","PYRENEES-ATLANTIQUES","NOUVELLE-AQUITAINE","Point",-1.4607929,43.484825]
["SSP000944701","64.0050","Elf Antar France",null,"Clôturée",null,"2015-04-27","Clôturée","64549","UZEIN","PYRENEES-ATLANTIQUES","NOUVELLE-AQUITAINE","Point",-0.43149808,43.395725,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000945101","74.0033","S.A. PRODUITS CHIMIQUES PLATRET",null,"En cours",null,null,"En cours","74305","VILLE LA GRAND","HAUTE-SAVOIE","AUVERGNE-RHONE-ALPES","Point",6.282622,46.205536]
["SSP000945301","68.0082","TERRIL AMELIE EST",null,"En cours",null,null,"En cours","68375","WITTELSHEIM","HAUT-RHIN","GRAND EST","Point",7.2440176,47.798958,"K36 - Mise en décharge"]
["SSP000945801","68.0087","MARX SPAENLIN -SOMETALOR  (av. de Suisse)",null,"En cours",null,null,"En cours","68154","ILLZACH","HAUT-RHIN","GRAND EST","Point",7.377133,47.769115,"K52 - Dépôts de ferraille"]
["SSP000946001","68.0089","TERRIL JOSEPH ELSE OUEST",null,"En cours",null,null,"En cours","68375","WITTELSHEIM","HAUT-RHIN","GRAND EST","Point",7.2440176,47.798958,"K36 - Mise en décharge"]
["SSP000946301","76.0132","EADS REVIMA",null,"En cours",null,null,"En cours","76164","CAUDEBEC EN CAUX","SEINE-MARITIME","NORMANDIE","Point",0.74628115,49.522778,"H13 - Traitement de surface"]
["SSP000946701","38.0087","MINATEC (site GEG INPG)",null,"Clôturée",null,null,"Clôturée","38185","GRENOBLE","ISERE","AUVERGNE-RHONE-ALPES","Polygone",5.7092314,45.194344,"J1 - Cokéfaction, usines à gaz"]
["SSP000947401","67.0096","PUITS II ET V",null,"En cours",null,null,"En cours","67379","PREUSCHDORF","BAS-RHIN","GRAND EST","Point",7.812835,48.93133,"D11 - Extraction de pétrole et gaz naturel"]
["SSP000947901","67.0106","PUITS  III  et VII",null,"En cours",null,null,"En cours","67177","GUNSTETT","BAS-RHIN","GRAND EST","Point",7.7877264,48.91909,"D11 - Extraction de pétrole et gaz naturel"]
["SSP000948201","68.0170","GMR (EX-HUPFER A.G.)",null,"En cours",null,null,"En cours","68126","HEGENHEIM","HAUT-RHIN","GRAND EST","Point",7.535773,47.56231,"C - Bois, papier et carton"]
["SSP000948401","21.0030","TOTAL (ex SODIPLEC)",null,"En cours",null,null,"En cours","21111","BROGNON","COTE-D'OR","BOURGOGNE-FRANCHE-COMTE","Point",5.1711044,47.41175,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000949001","02.0038","VAN TEX",null,"En cours",null,null,"En cours","02361","GUISE","AISNE","HAUTS-DE-FRANCE","Point",3.6190877,49.891174,"E1 - Textile et habillement, teinture, impression"]
["SSP000949401","59.0346","PETITPREZ LAMBAERE",null,"En cours",null,null,"En cours","59512","ROUBAIX","NORD","HAUTS-DE-FRANCE","Point",3.1621482,50.685257,"E13 - Blanchiment, teinture, impression"]
["SSP000949501","74.0056","Ancien site de la société Dailloux Récupération",null,"Clôturée",null,"2018-01-09","Clôturée","74272","SILLINGY","HAUTE-SAVOIE","AUVERGNE-RHONE-ALPES","Point",6.0373654,45.95019,"K22 - Regroupement d'OM, DIB"]
["SSP000950101","89.0013","OXFORD AUTOMOTIVE MECANISMES  (OAM et OAMDF)  (Ex Ariès Industries)",null,"En cours",null,null,"En cours","89074","CHAMPIGNY","YONNE","BOURGOGNE-FRANCHE-COMTE","Point",3.1393995,48.30887,"H1 - Mécanique, électrique, traitement de surface"]
["SSP000950701","80.0045","A.F.R",null,"En cours",null,null,"En cours","80464","LANCHERES","SOMME","HAUTS-DE-FRANCE","Point",1.5493846,50.17571,"F2 - Minerais métalliques (extraction de)"]
["SSP000951001","44.0047","GROUPEMENT PETROLIER DE NANTES (GPN)",null,"En cours",null,null,"En cours","44162","SAINT HERBLAIN","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Point",-1.6359222,47.19458]
["SSP000951201","28.0034","SOUFFLET (ex - HUREL ARC)",null,"En cours",null,null,"En cours","28014","AUNAY SOUS CRECY","EURE-ET-LOIR","CENTRE-VAL DE LOIRE","Point",1.3039,48.673874,"D36 - Fabrication des engrais"]
["SSP000951701","60.0051","Saint Louis Sucre",null,"En cours",null,null,"En cours","60103","BRESLES","OISE","HAUTS-DE-FRANCE","Point",2.247375,49.41475,"B14 - Industrie du sucre"]
["SSP000952301","76.0142","E&SCHIMIE (ex IFRACHEM)",null,"En cours",null,null,"En cours","76640","SAINT PIERRE LES ELBEUF","SEINE-MARITIME","NORMANDIE","Point",1.0426171,49.267536]
["SSP000952701","76.0147","TCAR",null,"En cours",null,null,"En cours","76540","ROUEN","SEINE-MARITIME","NORMANDIE","Point",1.1231512,49.43948,"L1 - Entreposage, manutention, commerces"]
["SSP000952801","76.0148","MORPHO groupe SAFRAN (ex: SAGEM)",null,"En cours",null,null,"En cours","76575","SAINT ETIENNE DU ROUVRAY","SEINE-MARITIME","NORMANDIE","Point",1.1125336,49.37358,"H18 - Composants électroniques (fabrication de)"]
["SSP000953501","84.0018","SOCATRI",null,"En cours",null,null,"En cours","84019","BOLLENE","VAUCLUSE","PROVENCE-ALPES-COTE D'AZUR","Polygone",4.733559,44.318,"H13 - Traitement de surface"]
["SSP000954501","68.0101","ANC. BP (route de Bâle)",null,"En cours",null,null,"En cours","68066","COLMAR","HAUT-RHIN","GRAND EST","Point",7.3604245,48.067833]
["SSP000954801","68.0100","ANC. BP (rue du prunier)",null,"En cours",null,null,"En cours","68066","COLMAR","HAUT-RHIN","GRAND EST","Point",7.377876,48.08979]
["SSP000955001","74.0034","SARL DEFAGO Frères Technicdur",null,"En cours",null,null,"En cours","74124","FEIGERES","HAUTE-SAVOIE","AUVERGNE-RHONE-ALPES","Point",6.0630875,46.103542,"H13 - Traitement de surface"]
["SSP000955601","69.0135","JACQUI VALLET",null,"En cours",null,null,"En cours","69290","SAINT PRIEST","RHONE","AUVERGNE-RHONE-ALPES","Point",4.965007,45.716995,"L1 - Entreposage, manutention, commerces"]
["SSP000956101","18.0027","Station de transit de déchets ESTEVE",null,"En cours",null,null,"En cours","18033","BOURGES","CHER","CENTRE-VAL DE LOIRE","Point",2.355504,47.083214,"K3 - Traitement de déchets industriels"]
["SSP000956801","94.0045","BP-SAINT MAUR",null,"En cours",null,null,"En cours","94068","SAINT MAUR DES FOSSES","VAL-DE-MARNE","ILE-DE-FRANCE","Point",2.4909072,48.802765,"L23 - Détail de carburants"]
["SSP000956901","92.0069","Total Raffinage Marketing, ex FINA LUBRIFIANTS","Remise en état","En cours","2001-06-11",null,"En cours","92050","NANTERRE","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.1866362,48.898296,"D - Chimie, parachimie, pétrole"]
["SSP000957301","80.0048","FERINOX",null,"En cours",null,null,"En cours","80680","ROSIERES EN SANTERRE","SOMME","HAUTS-DE-FRANCE","Point",2.7074492,49.817757,"J5 - Fonderie et travail des métaux"]
["SSP000958301","42.0064","Teintures et Apprêts DANJOUX Usine pont du Rhins",null,"En cours",null,null,"En cours","42071","LE COTEAU","LOIRE","AUVERGNE-RHONE-ALPES","Point",4.093586,46.02544,"E13 - Blanchiment, teinture, impression"]
["SSP000958601","95.0036","MOBIL OIL",null,"En cours",null,null,"En cours","95395","LE MESNIL AUBRY","VAL-D'OISE","ILE-DE-FRANCE","Point",2.3916843,49.054844,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000958801","60.0055","ancien dépôt pétrolier TOTAL FINA ELF",null,"En cours",null,null,"En cours","60057","BEAUVAIS","OISE","HAUTS-DE-FRANCE","Point",2.1110094,49.42507,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000959301","27.0039","SOCIETE  BROGSER",null,"En cours",null,null,"En cours","27117","BROGLIE","EURE","NORMANDIE","Point",0.5282864,49.00867,"H13 - Traitement de surface"]
["SSP000959701","60.0058","Mueller (ex. Desnoyers)",null,"En cours",null,null,"En cours","60342","LAIGNEVILLE","OISE","HAUTS-DE-FRANCE","Point",2.429116,49.299015]
["SSP000960301","69.0140","TEINTURES ET APPRETS DANJOUX T.A.D.",null,"En cours",null,null,"En cours","69025","BOURG-DE-THIZY","RHONE","AUVERGNE-RHONE-ALPES","Point",4.294371,46.0339,"E13 - Blanchiment, teinture, impression"]
["SSP000960401","59.0384","BP WATTEAU",null,"En cours",null,null,"En cours","59606","VALENCIENNES","NORD","HAUTS-DE-FRANCE","Point",3.511888,50.358658,"L2 - Transports, automobile, carburants"]
["SSP000961001","10.0045","Teinturerie des Bas Trévois",null,"En cours",null,null,"En cours","10387","TROYES","AUBE","GRAND EST","Point",4.082011,48.290855,"E1 - Textile et habillement, teinture, impression"]
["SSP000961501","69.0142","CHARDON ET COUCHOUD",null,"En cours",null,null,"En cours","69266","VILLEURBANNE","RHONE","AUVERGNE-RHONE-ALPES","Point",4.8751907,45.761806,"H13 - Traitement de surface"]
["SSP000961801","67.0111","STOCKO CONTACT",null,"En cours",null,null,"En cours","67010","ANDLAU","BAS-RHIN","GRAND EST","Point",7.429806,48.387203,"H1 - Mécanique, électrique, traitement de surface"]
["SSP000962001","67.0113","SOGETEX",null,"En cours",null,null,"En cours","67130","ERSTEIN","BAS-RHIN","GRAND EST","Point",7.663043,48.42104,"E12 - Filtène, filature, tissage, tricotage"]
["SSP000962701","38.0093","ZAC Vigny Musset",null,"Clôturée",null,null,"Clôturée","38185","GRENOBLE","ISERE","AUVERGNE-RHONE-ALPES","Polygone",5.7288117,45.16733]
["SSP000963001","19.0004","EUROVIA à EYREIN",null,"Clôturée",null,"2019-09-11","Clôturée","19081","EYREIN","CORREZE","NOUVELLE-AQUITAINE","Point",1.9082001,45.33109,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000963601","76.0160","MULTISOL",null,"En cours",null,null,"En cours","76681","SOTTEVILLE LES ROUEN","SEINE-MARITIME","NORMANDIE","Point",1.1166449,49.402042,"D12 - Raffinage de pétrole, carburants et lubrifiants"]
["SSP000963701","76.0161","Et. LETELLIER",null,"En cours",null,null,"En cours","76255","EU","SEINE-MARITIME","NORMANDIE","Point",1.4238346,50.04508,"H1 - Mécanique, électrique, traitement de surface"]
["SSP000964201","67.0120","GARAGE SANDROCK",null,"En cours",null,null,"En cours","67405","ROESCHWOOG","BAS-RHIN","GRAND EST","Point",8.032413,48.82427,"L23 - Détail de carburants"]
["SSP000964701","59.0387","DSV bat C (ex LEPOUTRE TERNYNCK - TCM)",null,"En cours",null,null,"En cours","59650","WATTRELOS","NORD","HAUTS-DE-FRANCE","Point",3.1901765,50.714283,"E13 - Blanchiment, teinture, impression"]
["SSP000965301","28.0039","TOTAL Raffinage Distribution",null,"En cours",null,null,"En cours","28218","LUCE","EURE-ET-LOIR","CENTRE-VAL DE LOIRE","Point",1.4683856,48.43794,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000965401","73.0065","Société Métaux Spéciaux  - Ancienne décharge des tennis",null,"En cours",null,null,"En cours","73253","SAINT MARCEL","SAVOIE","AUVERGNE-RHONE-ALPES","Point",6.562201,45.50016]
["SSP000966001","67.0126","SETRAL",null,"En cours",null,null,"En cours","67408","ROMANSWILLER","BAS-RHIN","GRAND EST","Point",7.393238,48.643757,"D12 - Raffinage de pétrole, carburants et lubrifiants"]
["SSP000966301","26.0037","STATION SERVICE BP",null,"En cours",null,null,"En cours","26165","LIVRON SUR DROME","DROME","AUVERGNE-RHONE-ALPES","Point",4.8476677,44.777496]
["SSP000966801","69.0150","LENNE",null,"Clôturée",null,"2015-04-13","Clôturée","69266","VILLEURBANNE","RHONE","AUVERGNE-RHONE-ALPES","Point",4.906729,45.759098,"J52 - Fonderie des métaux non ferreux"]
["SSP000966901","69.0151","O-I MANUFACTURING (Ex. VMC)",null,"En cours",null,null,"En cours","69091","GIVORS","RHONE","AUVERGNE-RHONE-ALPES","Point",4.7636857,45.586525,"G15 - Industrie du verre"]
["SSP000967401","59.0400","Unité de traitement par inertage et stabilisation de poussières (SGTD)",null,"En cours",null,null,"En cours","59179","DOUCHY LES MINES","NORD","HAUTS-DE-FRANCE","Point",3.3882062,50.300438,"K35 - Regroupement, reconditionnement de déchets"]
["SSP000967801","60.0066","Ex FONDERIES LAFEUILLE",null,"En cours",null,null,"En cours","60463","NOGENT SUR OISE","OISE","HAUTS-DE-FRANCE","Point",2.4758265,49.269745]
["SSP000968401","57.0120","ANCIENNE STATION SERVICE MATCH",null,"En cours",null,null,"En cours","57474","MONDELANGE","MOSELLE","GRAND EST","Point",6.155568,49.256573,"L23 - Détail de carburants"]
["SSP000968501","78.0059","CARREFOUR",null,"En cours",null,null,"En cours","78418","MONTESSON","YVELINES","ILE-DE-FRANCE","Point",2.1426253,48.9286,"L23 - Détail de carburants"]
["SSP000969201","18.0031","Dépôt hydrocarbures WOREX",null,"En cours",null,null,"En cours","18137","MAREUIL SUR ARNON","CHER","CENTRE-VAL DE LOIRE","Point",2.1671646,46.881413]
["SSP000969601","86.0007","DECONS",null,"En cours",null,null,"En cours","86289","LE VIGEANT","VIENNE","NOUVELLE-AQUITAINE","Point",0.62094086,46.186394,"J52 - Fonderie des métaux non ferreux"]
["SSP000969801","73.0069","Ancienne UIOM de Sollières-Sardière",null,"En cours",null,null,"En cours","73290","TERMIGNON","SAVOIE","AUVERGNE-RHONE-ALPES","Point",6.816832,45.266266,"K31 - Incinération"]
["SSP000970101","59.0402","Recylex (ex Metaleurop Escaudoeuvres)",null,"En cours",null,null,"En cours","59206","ESCAUDOEUVRES","NORD","HAUTS-DE-FRANCE","Point",3.2662218,50.195633,"K51 - Récupération non ferreux"]
["SSP000970701","18.0032","KOYO (Anciennement TIMKEN)",null,"En cours",null,null,"En cours","18279","VIERZON","CHER","CENTRE-VAL DE LOIRE","Point",2.1123478,47.20516,"H1 - Mécanique, électrique, traitement de surface"]
["SSP000971201","73.0075","MERSEN ( EX CELLIER CHAUDRONNERIE 2C)",null,"Clôturée",null,null,"Clôturée","73128","GRESY SUR AIX","SAVOIE","AUVERGNE-RHONE-ALPES","Point",5.9209933,45.726013,"H - Mécanique, traitements des surfaces"]
["SSP000971801","76.0167","Grassin Delyle (secteur racheté par GALVANORM /SCI GRENA)",null,"En cours",null,null,"En cours","76402","MALAUNAY","SEINE-MARITIME","NORMANDIE","Point",1.0472633,49.525642,"M1 - Industries diverses"]
["SSP000972301","19.0010","Ateliers municipaux de la ville de Brive",null,"Clôturée",null,"2019-09-11","Clôturée","19031","BRIVE LA GAILLARDE","CORREZE","NOUVELLE-AQUITAINE","Point",1.481128,45.152332,"L23 - Détail de carburants"]
["SSP000972501","19.0013","FRANCE BOIS IMPREGNES (FBI)",null,"En cours",null,null,"En cours","19136","MEYMAC","CORREZE","NOUVELLE-AQUITAINE","Point",2.1621616,45.535275,"C13 - Traitement du bois"]
["SSP000973101","26.0041","FOUR INCINERATEUR LA CHAPELLE EN VERCORS",null,"En cours",null,null,"En cours","26074","LA CHAPELLE EN VERCORS","DROME","AUVERGNE-RHONE-ALPES","Point",5.3962584,44.98032]
["SSP000973401","34.0022","Station service Hyper U",null,"En cours",null,null,"En cours","34090","LE CRES","HERAULT","OCCITANIE","Point",3.9433594,43.642555,"L23 - Détail de carburants"]
["SSP000973701","95.0045","usine de traitement des ordures ménagères de Bessancourt",null,"En cours",null,null,"En cours","95060","BESSANCOURT","VAL-D'OISE","ILE-DE-FRANCE","Point",2.1995273,49.03643,"K2 - Traitement de déchets urbains"]
["SSP000974201","34.0025","Ancienne usine de Ceilhes et Rocozels",null,"En cours",null,null,"En cours","34019","AVENE","HERAULT","OCCITANIE","Point",3.0968554,43.797478,"D32 - Chimie minérale inorganique autre"]
["SSP000974601","39.0018","STATION BP LA MONTAGNE",null,"En cours",null,null,"En cours","39300","LONS LE SAUNIER","JURA","BOURGOGNE-FRANCHE-COMTE","Point",5.5704226,46.670776,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000975201","76.0168","ANTIGONE",null,"En cours",null,null,"En cours","76394","LONGROY","SEINE-MARITIME","NORMANDIE","Point",1.5475478,49.98289]
["SSP000975501","66.0012","UIOM de Lesquerde",null,"En cours",null,null,"En cours","66097","LESQUERDE","PYRENEES-ORIENTALES","OCCITANIE","Point",2.5363224,42.788696]
["SSP000975701","63.0026","TBI Vertaizon",null,"En cours",null,null,"En cours","63453","VERTAIZON","PUY-DE-DOME","AUVERGNE-RHONE-ALPES","Point",3.2955103,45.784306,"D72 - Transformation des matières plastiques"]
["SSP000976201","76.0171","BRENNTAG NORMANDIE",null,"En cours",null,null,"En cours","76452","MONTVILLE","SEINE-MARITIME","NORMANDIE","Point",1.0629472,49.541092,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000976501","69.0166","COLAS RHONE ALPES",null,"En cours",null,null,"En cours","69123","LYON","RHONE","AUVERGNE-RHONE-ALPES","Point",4.8174353,45.74007,"G22 - Centrales d'enrobés"]
["SSP000976801","42.0071","FERRAPIE  TRANSPORT AFFRETEMENT",null,"En cours",null,null,"En cours","42183","LA RICAMARIE","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.366486,45.409332,"L22 - Transports"]
["SSP000977401","60.0069","SAR",null,"En cours",null,null,"En cours","60007","AGNETZ","OISE","HAUTS-DE-FRANCE","Point",2.378269,49.395653]
["SSP000977801","76.0173","Site BOVIN",null,"En cours",null,null,"En cours","76498","LE PETIT QUEVILLY","SEINE-MARITIME","NORMANDIE","Point",1.0656694,49.424152,"K52 - Dépôts de ferraille"]
["SSP000978401","56.0013","Station-service ELF (PENVERN)",null,"Clôturée",null,"2006-12-01","Clôturée","56101","LANGUIDIC","MORBIHAN","BRETAGNE","Point",-3.16412,47.835526,"L23 - Détail de carburants"]
["SSP000978701","59.0434","Ancien site NORMED - UF ACIERS",null,"En cours",null,null,"En cours","59183","DUNKERQUE","NORD","HAUTS-DE-FRANCE","Point",2.3745432,51.028725,"J53 - Travail des métaux, chaudronnerie, poudres"]
["SSP000978901","64.0053","ARYSTA LIFESCIENCE",null,"En cours",null,null,"En cours","64418","NOGUERES","PYRENEES-ATLANTIQUES","NOUVELLE-AQUITAINE","Point",-0.6016442,43.371113,"D37 - Phytosanitaires, pesticides (fabrication de)"]
["SSP000979201","68.0116","MONTREUX PNEUS",null,"En cours",null,null,"En cours","68215","MONTREUX VIEUX","HAUT-RHIN","GRAND EST","Point",7.027168,47.618015]
["SSP000979901","33.0363","MAIRIE - Latresne",null,"En cours",null,null,"En cours","33234","LATRESNE","GIRONDE","NOUVELLE-AQUITAINE","Point",-0.5052461,44.7844]
["SSP000980001","68.0193","MITTELBUEHL",null,"En cours",null,null,"En cours","68051","BREITENBACH HAUT RHIN","HAUT-RHIN","GRAND EST","Point",7.106655,48.007893]
["SSP000980501","62.0120","DMS (Ex Mory Combustibles) rue beaumarais",null,"En cours",null,null,"En cours","62193","CALAIS","PAS-DE-CALAIS","HAUTS-DE-FRANCE","Point",1.868174,50.952213,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000981001","38.0108","ZAC Vigny Musset - Ilot N",null,"Clôturée",null,null,"Clôturée","38185","GRENOBLE","ISERE","AUVERGNE-RHONE-ALPES","Polygone",5.726024,45.167805,null,null,null,"38.32Z - Récupération de déchets triés"]
["SSP000981601","28.0043","FAPEC (EX IBP FRANCE)",null,"En cours",null,null,"En cours","28196","ILLIERS COMBRAY","EURE-ET-LOIR","CENTRE-VAL DE LOIRE","Point",1.2444862,48.305077,"C - Bois, papier et carton"]
["SSP000981901","42.0074","UIOM de NOIRETABLE",null,"En cours",null,null,"En cours","42159","NOIRETABLE","LOIRE","AUVERGNE-RHONE-ALPES","Point",3.746832,45.82353,"K - Déchets et traitements"]
["SSP000982301","69.0179","IPIF - International Paper Industrie France",null,"En cours",null,null,"En cours","69290","SAINT PRIEST","RHONE","AUVERGNE-RHONE-ALPES","Point",4.967466,45.68021,"C2 - Industrie du papier et du carton"]
["SSP000982701","38.0111","ZAC Vigny Musset   - Ilot M",null,"Clôturée",null,null,"Clôturée","38185","GRENOBLE","ISERE","AUVERGNE-RHONE-ALPES","Polygone",5.724965,45.167652,null,null,null,"38.32Z - Récupération de déchets triés"]
["SSP000983401","73.0085","PURFER  - division FONLUPT",null,"En cours",null,null,"En cours","73065","CHAMBERY","SAVOIE","AUVERGNE-RHONE-ALPES","Point",5.8998866,45.58487,"K5 - Récupération, dépôts de ferrailles"]
["SSP000983501","66.0015","Décharge d'Ille sur Têt",null,"En cours",null,null,"En cours","66088","ILLE SUR TET","PYRENEES-ORIENTALES","OCCITANIE","Point",2.616657,42.674755,"K2 - Traitement de déchets urbains"]
["SSP000984101","66.0018","UIOM de PERPIGNAN",null,"En cours",null,null,"En cours","66136","PERPIGNAN","PYRENEES-ORIENTALES","OCCITANIE","Point",2.90465,42.698666]
["SSP000984501","28.0044","VERBOOM",null,"En cours",null,null,"En cours","28404","VERNOUILLET","EURE-ET-LOIR","CENTRE-VAL DE LOIRE","Point",1.352283,48.71431,"H11 - Usinage"]
["SSP000984901","25.0036","Stockage de broyats du Bélieu",null,"En cours",null,null,"En cours","25050","LE BELIEU","DOUBS","BOURGOGNE-FRANCHE-COMTE","Point",6.6464267,47.115993]
["SSP000985001","38.0116","ALSTOM (ex NEYRTEC  ALSTOM  ATLANTIQUE)",null,"En cours",null,null,"En cours","38317","LE PONT DE CLAIX","ISERE","AUVERGNE-RHONE-ALPES","Point",5.711609,45.136124]
["SSP000985501","54.0095","FISCHER LORRAINE","Cessation d'activités 2000","Clôturée",null,"2004-09-10","Clôturée","54329","LUNEVILLE","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",6.518734,48.59067,"H11 - Usinage"]
["SSP000985901","974.0013","PIPE LINE SRE",null,"En cours",null,null,"En cours","97407","LE PORT","LA REUNION","LA REUNION","Point",0.0,0.0,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000986501","28.0046","CLAIRCELL",null,"En cours",null,null,"En cours","28061","BROU","EURE-ET-LOIR","CENTRE-VAL DE LOIRE","Point",1.1791747,48.21635,"C23 - Transformation de papiers et carton"]
["SSP000986601","69.0189","ENI FRANCE SARL  (ex. AGIP station service)",null,"En cours",null,null,"En cours","69123","LYON","RHONE","AUVERGNE-RHONE-ALPES","Point",4.8284883,45.778896,"L23 - Détail de carburants"]
["SSP000987101","08.0037","Société GODART Frères",null,"En cours",null,null,"En cours","08249","LAVAL MORENCY","ARDENNES","GRAND EST","Point",4.49128,49.833115,"H1 - Mécanique, électrique, traitement de surface"]
["SSP000987501","41.0018","DEC (Dépôts Electrolytiques et Chimiques)",null,"En cours",null,null,"En cours","41060","CORMENON","LOIR-ET-CHER","CENTRE-VAL DE LOIRE","Point",0.8922067,47.970222,"H13 - Traitement de surface"]
["SSP000987901","29.0025","STATION-SERVICE Interne SNCF",null,"Clôturée",null,"2006-07-31","Clôturée","29232","QUIMPER","FINISTERE","BRETAGNE","Point",-4.0883484,47.994717,"L23 - Détail de carburants"]
["SSP000988001","26.0045","BUBBLE et FOAM Industries S.A   (ex site  TARKETT SOMMER)",null,"En cours",null,null,"En cours","26325","SAINT RAMBERT D'ALBON","DROME","AUVERGNE-RHONE-ALPES","Point",4.8119383,45.281395,"D72 - Transformation des matières plastiques"]
["SSP000988601","73.0091","ANCIENNE USINE D'INCINERATION D'ENTREMONT LE VIEUX",null,"En cours",null,null,"En cours","73107","ENTREMONT LE VIEUX","SAVOIE","AUVERGNE-RHONE-ALPES","Point",5.878754,45.436703,"K2 - Traitement de déchets urbains"]
["SSP000989101","35.0015","TRIADIS Services (ex SPEICHIM Processing)",null,"En cours",null,null,"En cours","35281","SAINT JACQUES DE LA LANDE","ILLE-ET-VILAINE","BRETAGNE","Point",-1.726905,48.077934,"K42 - Régénération de solvants"]
["SSP000989801","60.0079","TREFIMETAUX SA",null,"En cours",null,null,"En cours","60616","SERIFONTAINE","OISE","HAUTS-DE-FRANCE","Point",1.7903126,49.36362,"J52 - Fonderie des métaux non ferreux"]
["SSP000990001","34.0029","Station Service SUPER U",null,"En cours",null,null,"En cours","34057","CASTELNAU LE LEZ","HERAULT","OCCITANIE","Polygone",3.8984995,43.62324,"L23 - Détail de carburants"]
["SSP000990401","10.0058","CYCLEUROPE",null,"En cours",null,null,"En cours","10323","ROMILLY SUR SEINE","AUBE","GRAND EST","Point",3.6974204,48.520206,"H13 - Traitement de surface"]
["SSP000991001","62.0128","E.G.E.F. Sénicourt (Groupe Forclum)",null,"En cours",null,null,"En cours","62896","WIRWIGNES","PAS-DE-CALAIS","HAUTS-DE-FRANCE","Point",1.7612017,50.680763,"H1 - Mécanique, électrique, traitement de surface"]
["SSP000991501","01.0059","EDF rue Marguerite d'Autriche",null,"Clôturée",null,"2019-04-02","Clôturée","01053","BOURG EN BRESSE","AIN","AUVERGNE-RHONE-ALPES","Point",5.2375174,46.198925,"K35 - Regroupement, reconditionnement de déchets"]
["SSP000991601","69.0196","CTM ENNOBLISSEMENT",null,"En cours",null,null,"En cours","69157","PONTCHARRA SUR TURDINE","RHONE","AUVERGNE-RHONE-ALPES","Point",4.499813,45.87387,"E1 - Textile et habillement, teinture, impression"]
["SSP000992001","01.0061","WEBER ET BROUTIN FRANCE",null,"En cours",null,null,"En cours","01405","SERVAS","AIN","AUVERGNE-RHONE-ALPES","Point",5.160811,46.126453,"G14 - Fabrication d'autres matériaux de construction"]
["SSP000992501","07.0015","CNPE de Cruas-Meysse",null,"En cours",null,null,"En cours","07076","CRUAS","ARDECHE","AUVERGNE-RHONE-ALPES","Point",4.7540054,44.63456]
["SSP000993001","59.0449","CET D' ONNAING",null,"En cours",null,null,"En cours","59447","ONNAING","NORD","HAUTS-DE-FRANCE","Point",3.5933833,50.403214,"K21 - Décharges d'ordures ménagères"]
["SSP000993201","59.0453","CET de FRESNES SUR ESCAUT",null,"En cours",null,null,"En cours","59253","FRESNES SUR ESCAUT","NORD","HAUTS-DE-FRANCE","Point",3.5721521,50.44599,"K21 - Décharges d'ordures ménagères"]
["SSP000993501","67.0174","REMEX Rosheim (ex CONTENEURS ENVIRON SCE (C.E.S. Ex. SABLIERE MAETZ Site de Grie",null,"En cours",null,null,"En cours","67411","ROSHEIM","BAS-RHIN","GRAND EST","Point",7.5298014,48.507736]
["SSP000994001","95.0055","site DUCO",null,"En cours",null,null,"En cours","95424","MONTIGNY LES CORMEILLES","VAL-D'OISE","ILE-DE-FRANCE","Point",2.2087047,48.99868,"D43 - Fabrication de vernis"]
["SSP000994401","28.0048","MEDICIS INDUSTRIE",null,"En cours",null,null,"En cours","28404","VERNOUILLET","EURE-ET-LOIR","CENTRE-VAL DE LOIRE","Point",1.332178,48.72682,"D38 - Industrie pharmaceutique"]
["SSP000994501","81.0036","ETERNIT DECHARGE DE RANTEIL",null,"En cours",null,null,"En cours","81004","ALBI","TARN","OCCITANIE","Point",2.128287,43.899197,"K36 - Mise en décharge"]
["SSP000994901","38.0121","TOTAL France A48",null,"En cours",null,null,"En cours","38565","VOREPPE","ISERE","AUVERGNE-RHONE-ALPES","Point",5.62422,45.278255,"L23 - Détail de carburants"]
["SSP000995501","41.0021","ENERFLUX",null,"En cours",null,null,"En cours","41018","BLOIS","LOIR-ET-CHER","CENTRE-VAL DE LOIRE","Point",1.3121859,47.584118,"H1 - Mécanique, électrique, traitement de surface"]
["SSP000996101","38.0125","ZAC Portes du Grésivaudan (ex DPG)",null,"En cours",null,null,"En cours","38421","SAINT MARTIN D'HERES","ISERE","AUVERGNE-RHONE-ALPES","Point",5.771623,45.183273,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP000996301","24.0019","GOUBIE",null,"En cours",null,null,"En cours","24340","PRIGONRIEUX","DORDOGNE","NOUVELLE-AQUITAINE","Point",0.41060123,44.87285]
["SSP000996601","71.0056","RECYPNEUS",null,"En cours",null,null,"En cours","71310","MONTCHANIN","SAONE-ET-LOIRE","BOURGOGNE-FRANCHE-COMTE","Point",4.482773,46.740147,"K3 - Traitement de déchets industriels"]
["SSP000997501","33.0122","LAFON",null,"En cours",null,null,"En cours","33051","BIGANOS","GIRONDE","NOUVELLE-AQUITAINE","Point",-0.9513834,44.664425]
["SSP000998001","33.0126","ROCHETTE",null,"En cours",null,null,"En cours","33097","CARCANS","GIRONDE","NOUVELLE-AQUITAINE","Point",-1.0412902,45.085453,"C13 - Traitement du bois"]
["SSP000998101","33.0127","SERVY",null,"En cours",null,null,"En cours","33104","CASTELNAU DE MEDOC","GIRONDE","NOUVELLE-AQUITAINE","Point",-0.81591654,45.007607]
["SSP000998501","33.0131","GUEDON",null,"En cours",null,null,"En cours","33151","DONNEZAC","GIRONDE","NOUVELLE-AQUITAINE","Point",-0.44663936,45.223957]
["SSP000999201","33.0139","MOURLAN",null,"En cours",null,null,"En cours","33235","LAVAZAN","GIRONDE","NOUVELLE-AQUITAINE","Point",-0.114707105,44.39551]
["SSP000999501","33.0141","HOSTEIN ET LAVAL",null,"En cours",null,null,"En cours","33248","LISTRAC MEDOC","GIRONDE","NOUVELLE-AQUITAINE","Point",-0.8511317,45.052868]
["SSP000999701","33.0143","LABROUSSE ET FILS",null,"En cours",null,null,"En cours","33336","PRECHAC","GIRONDE","NOUVELLE-AQUITAINE","Point",-0.3757258,44.392147]
["SSP001000301","33.0150","SOFA",null,"En cours",null,null,"En cours","33473","SAINT SAVIN","GIRONDE","NOUVELLE-AQUITAINE","Point",-0.07468135,44.85696]
["SSP001000801","40.0050","CASTAGNE",null,"Clôturée",null,"2014-01-06","Clôturée","40046","BISCARROSSE","LANDES","NOUVELLE-AQUITAINE","Point",-1.2229942,44.395657]
["SSP001001401","40.0056","NEURRISSE Bois et Dérivés",null,"En cours",null,null,"En cours","40075","CASTETS","LANDES","NOUVELLE-AQUITAINE","Point",-1.164872,43.860992]
["SSP001001501","40.0057","DACQUOISE ASSAINISSEMENT",null,"En cours",null,null,"En cours","40088","DAX","LANDES","NOUVELLE-AQUITAINE","Point",-1.0620881,43.704933]
["SSP001001901","40.0062","TECMA",null,"En cours",null,null,"En cours","40133","LABENNE","LANDES","NOUVELLE-AQUITAINE","Point",-1.4301388,43.584393]
["SSP001002401","40.0066","BOUGES",null,"En cours",null,null,"En cours","40155","LINXE","LANDES","NOUVELLE-AQUITAINE","Point",-1.2521158,43.92563]
["SSP001002701","40.0069","LARREILLET",null,"En cours",null,null,"En cours","40210","ONESSE LAHARIE","LANDES","NOUVELLE-AQUITAINE","Point",-1.0288886,44.072178]
["SSP001002901","36.0030","Intermarché FLAMA",null,"En cours",null,null,"En cours","36045","CHATILLON SUR INDRE","INDRE","CENTRE-VAL DE LOIRE","Point",1.1677439,46.98767,"L23 - Détail de carburants"]
["SSP001003401","40.0075","CHASTEL",null,"En cours",null,null,"En cours","40295","SAUGNACQ ET MURET","LANDES","NOUVELLE-AQUITAINE","Point",-0.8301489,44.390427]
["SSP001004001","40.0080","MIREMONT ETS",null,"En cours",null,null,"En cours","40285","SAINT YAGUEN","LANDES","NOUVELLE-AQUITAINE","Point",-0.7381625,43.905926,"C13 - Traitement du bois"]
["SSP001004501","40.0086"," BEYRIA  ETS (site Usine)",null,"En cours",null,null,"En cours","40333","YGOS SAINT SATURNIN","LANDES","NOUVELLE-AQUITAINE","Point",-0.71722436,44.00042]
["SSP001004601","40.0087","BEYRIA  ETS (site Scierie)",null,"En cours",null,null,"En cours","40333","YGOS SAINT SATURNIN","LANDES","NOUVELLE-AQUITAINE","Point",-0.71722436,44.00042]
["SSP001005001","47.0031","BRIOLANCE BOIS",null,"En cours",null,null,"En cours","47029","BLANQUEFORT SUR BRIOLANCE","LOT-ET-GARONNE","NOUVELLE-AQUITAINE","Point",0.96490306,44.61418]
["SSP001005601","47.0037","DE SANGOSSE",null,"En cours",null,null,"En cours","47209","PONT DU CASSE","LOT-ET-GARONNE","NOUVELLE-AQUITAINE","Point",0.67742544,44.229504]
["SSP001005901","24.0025","POLYREY",null,"En cours",null,null,"En cours","24023","BANEUIL","DORDOGNE","NOUVELLE-AQUITAINE","Point",0.71213984,44.83399]
["SSP001006101","64.0054","DMBP (ex DISPANO)",null,"En cours",null,null,"En cours","64102","BAYONNE","PYRENEES-ATLANTIQUES","NOUVELLE-AQUITAINE","Point",-1.4658142,43.489166]
["SSP001006801","95.0056","SIBAG",null,"En cours",null,null,"En cours","95219","ERMONT","VAL-D'OISE","ILE-DE-FRANCE","Point",2.2470152,48.993305,"D71 - Industrie du caoutchouc"]
["SSP001007401","87.0023","CHAMPEAU ",null,"En cours",null,null,"En cours","87064","EYMOUTIERS","HAUTE-VIENNE","NOUVELLE-AQUITAINE","Point",1.702765,45.735977,"C1 - Bois et de l'ameublement (industrie du)"]
["SSP001007901","87.0028","FCP (FONDERIE DE CUIVRE DU PALAIS)",null,"En cours",null,null,"En cours","87113","LE PALAIS SUR VIENNE","HAUTE-VIENNE","NOUVELLE-AQUITAINE","Point",1.3268468,45.87668,"J52 - Fonderie des métaux non ferreux"]
["SSP001008001","87.0029","Valdi (ex Valdi le Palais)",null,"En cours",null,null,"En cours","87113","LE PALAIS SUR VIENNE","HAUTE-VIENNE","NOUVELLE-AQUITAINE","Point",1.3252198,45.878338]
["SSP001008701","24.0023","BARBARIE",null,"En cours",null,null,"En cours","24107","LA CHAPELLE FAUCHER","DORDOGNE","NOUVELLE-AQUITAINE","Point",0.7611698,45.379078]
["SSP001009401","33.0160","SANITRA FOURRIER -Blaye",null,"Clôturée",null,"2015-04-27","Clôturée","33058","BLAYE","GIRONDE","NOUVELLE-AQUITAINE","Point",-0.6587351,45.118637,"K2 - Traitement de déchets urbains"]
["SSP001009701","33.0163","PBM IMPORT",null,"En cours",null,null,"En cours","33249","LORMONT","GIRONDE","NOUVELLE-AQUITAINE","Point",-0.51755077,44.8772]
["SSP001009901","33.0165","WORLD FUEL SERVICES anciennement ESSO SERVICE AVIATION",null,"En cours",null,null,"En cours","33281","MERIGNAC","GIRONDE","NOUVELLE-AQUITAINE","Point",-0.6668094,44.835457]
["SSP001010701","40.0090","FP BOIS",null,"En cours",null,null,"En cours","40184","MIMIZAN","LANDES","NOUVELLE-AQUITAINE","Point",-1.2241018,44.197372]
["SSP001011301","38.0202","GARAGE de L'OURSIERE",null,"En cours",null,null,"En cours","38421","SAINT MARTIN D'HERES","ISERE","AUVERGNE-RHONE-ALPES","Point",5.75527,45.186985,"L23 - Détail de carburants"]
["SSP001012001","64.0066","TOTAL FINA ELF FRANCE",null,"En cours",null,null,"En cours","64024","ANGLET","PYRENEES-ATLANTIQUES","NOUVELLE-AQUITAINE","Point",-1.5531998,43.4739]
["SSP001012101","38.0128","Station SHELL (ESMONIN)",null,"En cours",null,null,"En cours","38185","GRENOBLE","ISERE","AUVERGNE-RHONE-ALPES","Point",5.717659,45.16133,"L23 - Détail de carburants"]
["SSP001012701","24.0030","GASCOGNE WOOD PRODUCTS  ex CBP",null,"En cours",null,null,"En cours","24478","SAINT PARDOUX ET VIELVIC","DORDOGNE","NOUVELLE-AQUITAINE","Point",0.965731,44.77204]
["SSP001013301","33.0172","SOVAL",null,"En cours",null,null,"En cours","33032","BASSENS","GIRONDE","NOUVELLE-AQUITAINE","Point",-0.5303311,44.906204]
["SSP001014001","33.0185","Ancienne Station Service GARAGE LE CAM",null,"En cours",null,null,"En cours","33555","MARCHEPRIME","GIRONDE","NOUVELLE-AQUITAINE","Point",-0.84957546,44.70747]
["SSP001014101","38.0130","ZAC Vigny Musset  - Ilot H",null,"Clôturée",null,null,"Clôturée","38185","GRENOBLE","ISERE","AUVERGNE-RHONE-ALPES","Polygone",5.7274933,45.16688,null,null,null,"38.32Z - Récupération de déchets triés"]
["SSP001014901","03.0033","MANURHIN  DEFENSE",null,"En cours",null,null,"En cours","03023","BELLERIVE SUR ALLIER","ALLIER","AUVERGNE-RHONE-ALPES","Point",3.39276,46.147976,"D81 - Poudres et explosifs (fabrication de)"]
["SSP001015301","69.0210","TOTAL FRANCE - Station service ELF -A7 aire de Solaize",null,"En cours",null,null,"En cours","69296","SOLAIZE","RHONE","AUVERGNE-RHONE-ALPES","Point",4.8365216,45.651905,"L23 - Détail de carburants"]
["SSP001016001","73.0095","CAMIVA (Iveco Magirus Fire Fighting Camiva)",null,"En cours",null,null,"En cours","73222","SAINT ALBAN LEYSSE","SAVOIE","AUVERGNE-RHONE-ALPES","Point",5.9613276,45.57302,"H14 - Application de peinture"]
["SSP001016101","76.0188","ISOVER Saint-Gobain",null,"En cours",null,null,"En cours","76575","SAINT ETIENNE DU ROUVRAY","SEINE-MARITIME","NORMANDIE","Point",1.0911459,49.386875,"G14 - Fabrication d'autres matériaux de construction"]
["SSP001016601","51.0058","SNCF - Fagnières",null,"En cours",null,null,"En cours","51242","FAGNIERES","MARNE","GRAND EST","Point",4.330881,48.964012,"L2 - Transports, automobile, carburants"]
["SSP001016901","41.0024","PASSENAUD",null,"En cours",null,null,"En cours","41060","CORMENON","LOIR-ET-CHER","CENTRE-VAL DE LOIRE","Point",0.89125663,47.97389,"K52 - Dépôts de ferraille"]
["SSP001017501","63.0035","BP FRANCE",null,"En cours",null,null,"En cours","63164","GERZAT","PUY-DE-DOME","AUVERGNE-RHONE-ALPES","Point",3.1382575,45.815613,"D21 - Stockage et conditionnement des gaz et liquéfiés"]
["SSP001017701","64.0068","Parme Automobile",null,"Clôturée",null,"2013-03-29","Clôturée","64122","BIARRITZ","PYRENEES-ATLANTIQUES","NOUVELLE-AQUITAINE","Point",-1.5646642,43.47841,"K51 - Récupération non ferreux"]
["SSP001018701","33.0187","O.I. MANUFACTURING (ex BSN)",null,"En cours",null,null,"En cours","33539","VAYRES","GIRONDE","NOUVELLE-AQUITAINE","Point",-0.3280031,44.893528]
["SSP001019501","59.0462","AKERS",null,"En cours",null,null,"En cours","59068","BERLAIMONT","NORD","HAUTS-DE-FRANCE","Point",3.7953725,50.208984,"J51 - Fonderie des métaux ferreux"]
["SSP001020301","76.0296","THOMSON CUIVRE (Ex TREFIMETAUX)",null,"En cours",null,null,"En cours","76212","DARNETAL","SEINE-MARITIME","NORMANDIE","Point",1.1479335,49.436455]
["SSP001020401","76.0192","Compagnie Industrielle Maritime (CIM)",null,"En cours",null,null,"En cours","76595","SAINT JOUIN BRUNEVAL","SEINE-MARITIME","NORMANDIE","Point",0.15441637,49.657757,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP001021401","18.0037","MBDA - Bourges Aéroport",null,"En cours",null,null,"En cours","18033","BOURGES","CHER","CENTRE-VAL DE LOIRE","Point",2.3738952,47.066727,"H - Mécanique, traitements des surfaces"]
["SSP001022001","76.0357","CEPIC (compagnie des procédés industriels carbomeca)",null,"En cours",null,null,"En cours","76216","DEVILLE LES ROUEN","SEINE-MARITIME","NORMANDIE","Point",1.0444895,49.46854,"M1 - Industries diverses"]
["SSP001022701","67.0137","HAGER ELECTRO SAS",null,"En cours",null,null,"En cours","67046","BISCHWILLER","BAS-RHIN","GRAND EST","Point",7.870541,48.765453,"D72 - Transformation des matières plastiques"]
["SSP001022901","13.0126","AVITAIR SA (Ex SHELL AVITAIR - Dépôt aéroport)",null,"En cours",null,null,"En cours","13054","MARIGNANE","BOUCHES-DU-RHONE","PROVENCE-ALPES-COTE D'AZUR","Point",5.2133093,43.445477,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP001023201","13.0128","JEFCO",null,"En cours",null,null,"En cours","13055","MARSEILLE","BOUCHES-DU-RHONE","PROVENCE-ALPES-COTE D'AZUR","Point",5.424503,43.290882,"D42 - Fabrication de peintures"]
["SSP001023801","63.0036","O.I MANUFACTURING FRANCE ( ex: BSN GLASS PACK)",null,"En cours",null,null,"En cours","63291","PUY GUILLAUME","PUY-DE-DOME","AUVERGNE-RHONE-ALPES","Point",3.475345,45.95831,"G15 - Industrie du verre"]
["SSP001024201","76.0195","SEGAFREDO ZANETTI - ANCIEN SITE COLLET (ex MCF)",null,"En cours",null,null,"En cours","76681","SOTTEVILLE LES ROUEN","SEINE-MARITIME","NORMANDIE","Point",1.1058561,49.419064,"G22 - Centrales d'enrobés"]
["SSP001024401","24.0039"," Dépôt Pneus Usagés CONDAT PNEUMATIQUES",null,"En cours",null,"2006-12-12","En cours","24550","THENON","DORDOGNE","NOUVELLE-AQUITAINE","Point",1.0675492,45.139164,"K22 - Regroupement d'OM, DIB"]
["SSP001025101","61.0028","Usine FERODO/VALEO du Réservoir",null,"Clôturée",null,null,"Clôturée","61007","ATHIS DE L'ORNE","ORNE","NORMANDIE","Point",-0.50115186,48.799118]
["SSP001025801","59.0465","ASTRA ZENECA DUNKERQUE PRODUCTION",null,"En cours",null,null,"En cours","59183","DUNKERQUE","NORD","HAUTS-DE-FRANCE","Point",2.3511806,51.009274,"D38 - Industrie pharmaceutique"]
["SSP001026301","64.0116","Décharge communale de Saint-Jean-de-Luz",null,"En cours",null,null,"En cours","64483","SAINT JEAN DE LUZ","PYRENEES-ATLANTIQUES","NOUVELLE-AQUITAINE","Point",-1.6271539,43.392338]
["SSP001026501","28.0050","LATTY INTERNATIONAL",null,"En cours",null,null,"En cours","28061","BROU","EURE-ET-LOIR","CENTRE-VAL DE LOIRE","Point",1.1554229,48.20663]
["SSP001026801","59.0466","Inter Raccord, anciennement ",null,"En cours",null,null,"En cours","59053","BAVAY","NORD","HAUTS-DE-FRANCE","Point",3.7885144,50.29341,"H11 - Usinage"]
["SSP001027401","91.0093","ERICSSON",null,"En cours",null,null,"En cours","91377","MASSY","ESSONNE","ILE-DE-FRANCE","Polygone",2.2679722,48.728394,"H1 - Mécanique, électrique, traitement de surface"]
["SSP001027601","88.0051","COLAS EST",null,"En cours",null,null,"En cours","88209","GOLBEY","VOSGES","GRAND EST","Point",0.0,0.0]
["SSP001028101","45.0040","APM Group",null,"En cours",null,null,"En cours","45203","MEUNG SUR LOIRE","LOIRET","CENTRE-VAL DE LOIRE","Point",1.6922165,47.83127,"J35 - Autres métaux non ferreux (métallurgie des)"]
["SSP001028601","59.0471","SDME",null,"En cours",null,null,"En cours","59183","DUNKERQUE","NORD","HAUTS-DE-FRANCE","Point",2.3378794,51.002174,"G22 - Centrales d'enrobés"]
["SSP001029101","37.0015","Société Tourangelle de Matériaux Enrobés (STME)",null,"En cours",null,null,"En cours","37233","SAINT PIERRE DES CORPS","INDRE-ET-LOIRE","CENTRE-VAL DE LOIRE","Point",0.75514704,47.382324,"G22 - Centrales d'enrobés"]
["SSP001029601","01.0069","Le Joint Metalloplastique Français",null,"Clôturée",null,"2007-04-04","Clôturée","01034","BELLEY","AIN","AUVERGNE-RHONE-ALPES","Point",5.695181,45.757122]
["SSP001029801","91.0090","RMSP (Récupération métallurgique Sud Parisien)",null,"Clôturée",null,null,"Clôturée","91377","MASSY","ESSONNE","ILE-DE-FRANCE","Polygone",2.2720346,48.72615,"K52 - Dépôts de ferraille"]
["SSP001030201","47.0047","C2R",null,"En cours",null,"2014-09-03","En cours","47168","MIRAMONT DE GUYENNE","LOT-ET-GARONNE","NOUVELLE-AQUITAINE","Point",0.36127865,44.60165,"H1 - Mécanique, électrique, traitement de surface"]
["SSP001030801","25.0039","BORDY",null,"En cours",null,null,"En cours","25367","MANDEURE","DOUBS","BOURGOGNE-FRANCHE-COMTE","Point",6.811439,47.434402]
["SSP001031201","11.0018","EPPLN",null,"En cours",null,null,"En cours","11266","PORT LA NOUVELLE","AUDE","OCCITANIE","Point",3.0573545,43.02374,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP001031301","24.0040","CHROMADURLIN",null,"En cours",null,null,"En cours","24145","CREYSSE","DORDOGNE","NOUVELLE-AQUITAINE","Point",0.56682664,44.855625]
["SSP001031801","57.0151","Centrale EDF de Production Thermique Richemont",null,"En cours",null,null,"En cours","57582","RICHEMONT","MOSELLE","GRAND EST","Point",6.178676,49.282516,"I11 - Centrales électriques thermiques"]
["SSP001032801","61.0037","Usine FERODO/VALEO de La Planche",null,"Clôturée",null,null,"Clôturée","61007","ATHIS DE L'ORNE","ORNE","NORMANDIE","Point",-0.53405565,48.82149]
["SSP001033601","59.0477","CET Noyelles Sur Escaut Marcoing",null,"En cours",null,null,"En cours","59438","NOYELLES SUR ESCAUT","NORD","HAUTS-DE-FRANCE","Point",3.169356,50.133068,"K21 - Décharges d'ordures ménagères"]
["SSP001033901","45.0026","PROTIME",null,"En cours",null,null,"En cours","45082","CHATEAUNEUF SUR LOIRE","LOIRET","CENTRE-VAL DE LOIRE","Point",2.2064228,47.86896,"H - Mécanique, traitements des surfaces"]
["SSP001034401","79.0017","Paul Grandjouan Saco (ex ONYX TOP OUEST)",null,"En cours",null,null,"En cours","79048","LA CRECHE","DEUX-SEVRES","NOUVELLE-AQUITAINE","Point",-0.33284023,46.3446,"K21 - Décharges d'ordures ménagères"]
["SSP001035001","28.0054","CLIP",null,"En cours",null,null,"En cours","28387","THIRON GARDAIS","EURE-ET-LOIR","CENTRE-VAL DE LOIRE","Point",0.9887561,48.309334,"D33 - Pétrochimie carbochimie organique"]
["SSP001035501","76.0199","APS2 (Atelier Pièces Spéciales 2)",null,"En cours",null,null,"En cours","76255","EU","SEINE-MARITIME","NORMANDIE","Point",1.4327892,50.039352,"H11 - Usinage"]
["SSP001035601","33.0216","CUISINE AS Frimont",null,"Clôturée",null,"2015-04-27","Clôturée","33352","LA REOLE","GIRONDE","NOUVELLE-AQUITAINE","Point",-0.03549187,44.585915,"C12 - Produits en bois, ameublement (fabrication de)"]
["SSP001036001","64.0074","Station service SHELL",null,"Clôturée",null,"2013-03-08","Clôturée","64483","SAINT JEAN DE LUZ","PYRENEES-ATLANTIQUES","NOUVELLE-AQUITAINE","Point",-1.641449,43.399372,"L23 - Détail de carburants"]
["SSP001036901","33.0198","Décharge de Querquillas",null,"En cours",null,null,"En cours","33005","ANDERNOS LES BAINS","GIRONDE","NOUVELLE-AQUITAINE","Point",-1.0840966,44.752056,"K2 - Traitement de déchets urbains"]
["SSP001037401","33.0204","Fonderie Julien DESTANG",null,"Clôturée",null,"2015-04-27","Clôturée","33042","BELIN BELIET","GIRONDE","NOUVELLE-AQUITAINE","Point",-0.790018,44.50274,"J51 - Fonderie des métaux ferreux"]
["SSP001037801","42.0181","UGITECH",null,"En cours",null,null,"En cours","42218","SAINT ETIENNE","LOIRE","AUVERGNE-RHONE-ALPES","Point",4.433552,45.434883,"H13 - Traitement de surface"]
["SSP001038301","33.0211","SHELL Relais de Gazinet - A 63",null,"Clôturée",null,"2007-10-25","Clôturée","33122","CESTAS","GIRONDE","NOUVELLE-AQUITAINE","Point",-0.6847793,44.743156,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP001038801","38.0142","LECLERC ISERE DISTRIBUTION",null,"Clôturée",null,"2005-09-21","Clôturée","38416","SAINT MARCELLIN","ISERE","AUVERGNE-RHONE-ALPES","Point",5.316921,45.149696,"L23 - Détail de carburants"]
["SSP001039201","41.0037","Orléans Sud Auto (ex donadieu)",null,"En cours",null,null,"En cours","41256","THEILLAY","LOIR-ET-CHER","CENTRE-VAL DE LOIRE","Point",2.0348506,47.332115]
["SSP001039301","41.0038","POINT P",null,"En cours",null,null,"En cours","41018","BLOIS","LOIR-ET-CHER","CENTRE-VAL DE LOIRE","Point",1.316437,47.60507]
["SSP001039701","33.0218","FORD AQUITAINE INDUSTRIES",null,"En cours",null,null,"En cours","33056","BLANQUEFORT","GIRONDE","NOUVELLE-AQUITAINE","Point",-0.6095108,44.91491]
["SSP001041401","33.0220","Décharge d'Etauliers",null,"En cours",null,null,"En cours","33159","ETAULIERS","GIRONDE","NOUVELLE-AQUITAINE","Point",-0.57287073,45.22642,"K21 - Décharges d'ordures ménagères"]
["SSP001041801","42.0091","Alcoa Fastening System",null,"En cours",null,null,"En cours","42147","MONTBRISON","LOIRE","AUVERGNE-RHONE-ALPES","Point",4.0648046,45.619946,"H11 - Usinage"]
["SSP001042001","57.0152","CDF - EUROZONE - PUITS SIMON",null,"En cours",null,null,"En cours","57660","STIRING WENDEL","MOSELLE","GRAND EST","Point",6.9380555,49.20374]
["SSP001042601","33.0225","RABA - Pauillac",null,"En cours",null,null,"En cours","33314","PAUILLAC","GIRONDE","NOUVELLE-AQUITAINE","Point",-0.7488534,45.19856,"K21 - Décharges d'ordures ménagères"]
["SSP001043401","44.0052","SAH LEDUC",null,"En cours",null,null,"En cours","44205","LES TOUCHES","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Point",-1.4300557,47.440525]
["SSP001043901","33.0229","Décharge de Vendays Montalivet",null,"En cours",null,null,"En cours","33540","VENDAYS MONTALIVET","GIRONDE","NOUVELLE-AQUITAINE","Point",-1.0606474,45.356476,"K22 - Regroupement d'OM, DIB"]
["SSP001044001","33.0230","Décharge Rocanguille de Gensac",null,"En cours",null,null,"En cours","33186","GENSAC","GIRONDE","NOUVELLE-AQUITAINE","Point",0.068760246,44.80051,"K21 - Décharges d'ordures ménagères"]
["SSP001044401","73.0098","SONOCO ALCORE",null,"En cours",null,null,"En cours","73105","LES ECHELLES","SAVOIE","AUVERGNE-RHONE-ALPES","Point",5.7408457,45.442005,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP001044901","73.0100","PEDRETTI  Transports",null,"En cours",null,null,"En cours","73179","LA MOTTE SERVOLEX","SAVOIE","AUVERGNE-RHONE-ALPES","Point",5.8864465,45.599083,"L1 - Entreposage, manutention, commerces"]
["SSP001045701","26.0048","STATION SERVICE TOTAL - Garage Belotti",null,"En cours",null,null,"En cours","26324","SAINT PAUL TROIS CHATEAUX","DROME","AUVERGNE-RHONE-ALPES","Point",4.7677336,44.348763,"L23 - Détail de carburants"]
["SSP001046001","974.0015","Station-service CALTEX La Possession",null,"Clôturée",null,"2012-08-10","Clôturée","97408","LA POSSESSION","LA REUNION","LA REUNION","Point",55.329304,-20.94292,"L23 - Détail de carburants"]
["SSP001046701","31.0058","BOEHRINGER INGELHEIM (ex MERIAL)",null,"En cours",null,null,"En cours","31555","TOULOUSE","HAUTE-GARONNE","OCCITANIE","Point",1.3912262,43.59393,"D38 - Industrie pharmaceutique"]
["SSP001047001","57.0157","Station service TOTAL - Rue des alliés (Port Mazerolles)",null,"En cours",null,null,"En cours","57463","METZ","MOSELLE","GRAND EST","Point",6.1655583,49.12957,"L23 - Détail de carburants"]
["SSP001047601","33.0235","Shell Bordeaux Louis Barthou",null,"En cours",null,null,"En cours","33063","BORDEAUX","GIRONDE","NOUVELLE-AQUITAINE","Point",-0.6103604,44.85148,"L23 - Détail de carburants"]
["SSP001047701","92.0089","RUBIS TERMINAL PARTIE OUEST (SEPUR)",null,"En cours",null,null,"En cours","92078","VILLENEUVE LA GARENNE","HAUTS-DE-SEINE","ILE-DE-FRANCE","Point",2.311469,48.94679,"D3 - Chimie, phytosanitaire, pharmacie"]
["SSP001048101","59.0491","BRASSERIE BOUS",null,"En cours",null,null,"En cours","59359","LOON PLAGE","NORD","HAUTS-DE-FRANCE","Point",2.2186906,51.005302]
["SSP001048901","39.0024","CHARPENTES INDUSTRIELLES FRANCHE COMTE",null,"En cours",null,null,"En cours","39013","ARBOIS","JURA","BOURGOGNE-FRANCHE-COMTE","Point",5.765022,46.921658,"C13 - Traitement du bois"]
["SSP001049201","28.0076","SHELL (ex ESSO)",null,"En cours",null,null,"En cours","28173","GASVILLE OISEME","EURE-ET-LOIR","CENTRE-VAL DE LOIRE","Point",1.5776876,48.467945,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP001049401","68.0140","PEUGEOT MOTOCYCLES",null,"En cours",null,null,"En cours","68068","DANNEMARIE","HAUT-RHIN","GRAND EST","Point",7.126129,47.630898,"H13 - Traitement de surface"]
["SSP001050001","38.0155","TOTAL FRANCE Relais de Saint Quentin Fallavier",null,"En cours",null,null,"En cours","38449","SAINT QUENTIN FALLAVIER","ISERE","AUVERGNE-RHONE-ALPES","Point",5.12147,45.649734]
["SSP001050301","67.0144","TOTAL",null,"En cours",null,null,"En cours","67246","KOGENHEIM","BAS-RHIN","GRAND EST","Point",7.540721,48.338097,"L23 - Détail de carburants"]
["SSP001051001","42.0093","SAG FRANCE",null,"En cours",null,null,"En cours","42110","L'HORME","LOIRE","AUVERGNE-RHONE-ALPES","Point",4.556253,45.493362,"H11 - Usinage"]
["SSP001051101","24.0051","SIRMET SAS",null,"En cours",null,null,"En cours","24053","BOULAZAC","DORDOGNE","NOUVELLE-AQUITAINE","Point",0.77413267,45.179893]
["SSP001051601","82.0019","ANTAVIA",null,"En cours",null,null,"En cours","82048","DIEUPENTALE","TARN-ET-GARONNE","OCCITANIE","Point",1.2735332,43.85934,"H1 - Mécanique, électrique, traitement de surface"]
["SSP001052001","64.0093","TOTAL - Relais Marne Verdun",null,"En cours",null,null,"En cours","64122","BIARRITZ","PYRENEES-ATLANTIQUES","NOUVELLE-AQUITAINE","Point",-1.5569495,43.481792,"L23 - Détail de carburants"]
["SSP001052501","33.0242","VERMILION REP Lugos",null,"En cours",null,null,"En cours","33260","LUGOS","GIRONDE","NOUVELLE-AQUITAINE","Point",-0.9483378,44.45207,"D1 - Industrie pétrolière, gaz naturel"]
["SSP001052601","40.0120","LAMARQUE SOGY BOIS (usine CAVALIER)",null,"En cours",null,null,"En cours","40135","LABRIT","LANDES","NOUVELLE-AQUITAINE","Point",-0.5514162,44.108006,"C11 - Scierie, fabrication de panneaux"]
["SSP001053301","24.0049","Dépôt aéroportuaire de Bergerac",null,"En cours",null,null,"En cours","24037","BERGERAC","DORDOGNE","NOUVELLE-AQUITAINE","Point",0.48617738,44.85298,"L23 - Détail de carburants"]
["SSP001053601","57.0163","BRGM-DPSM (ex CDF)",null,"En cours",null,null,"En cours","57606","SAINT AVOLD","MOSELLE","GRAND EST","Point",6.6827736,49.166714]
["SSP001053801","33.0250","FORESTIER",null,"Clôturée",null,"2015-04-27","Clôturée","33114","CAVIGNAC","GIRONDE","NOUVELLE-AQUITAINE","Point",-0.38966122,45.101185,"C1 - Bois et de l'ameublement (industrie du)"]
["SSP001054101","33.0245","TERRALYS (ex GED)",null,"En cours",null,null,"En cours","33474","SAINT SELVE","GIRONDE","NOUVELLE-AQUITAINE","Point",-0.44885272,44.65071,"K35 - Regroupement, reconditionnement de déchets"]
["SSP001054701","33.0248","VEYNAT",null,"En cours",null,null,"En cours","33535","TRESSES","GIRONDE","NOUVELLE-AQUITAINE","Point",-0.47462082,44.83259,"M - Divers et services"]
["SSP001055201","01.0071","SNCF",null,"Clôturée",null,"2009-10-23","Clôturée","01033","BELLEGARDE SUR VALSERINE","AIN","AUVERGNE-RHONE-ALPES","Point",5.8265514,46.111603,"L - Entreposage, transport, commerce"]
["SSP001056001","47.0052","AFM RECYCLAGE",null,"En cours",null,null,"En cours","47157","MARMANDE","LOT-ET-GARONNE","NOUVELLE-AQUITAINE","Point",0.15935817,44.50812,"K52 - Dépôts de ferraille"]
["SSP001056101","47.0053","GARREAU Jean-Jacques -CASSE AUTOS 47",null,"En cours",null,null,"En cours","47171","MONBALEN","LOT-ET-GARONNE","NOUVELLE-AQUITAINE","Point",0.7296284,44.30488,"K52 - Dépôts de ferraille"]
["SSP001056701","33.0261","Dépôt  Pneus Gironde Environnement 2000 Marcheprime",null,"Clôturée",null,"2015-04-27","Clôturée","33555","MARCHEPRIME","GIRONDE","NOUVELLE-AQUITAINE","Point",-0.8467713,44.68908]
["SSP001057001","37.0018","Ile Balzac",null,"En cours",null,null,"En cours","37261","TOURS","INDRE-ET-LOIRE","CENTRE-VAL DE LOIRE","Point",0.7067802,47.37181,"K21 - Décharges d'ordures ménagères"]
["SSP001057201","95.0065","GATEFOSSE (EX-LIBIOL SA)",null,"En cours",null,null,"En cours","95598","SOISY SOUS MONTMORENCY","VAL-D'OISE","ILE-DE-FRANCE","Point",2.3000228,48.976585,"D38 - Industrie pharmaceutique"]
["SSP001057501","02.0055","SAICA VENIZEL (ex LA ROCHETTE VENIZEL)",null,"En cours",null,null,"En cours","02780","VENIZEL","AISNE","HAUTS-DE-FRANCE","Point",3.4100137,49.36781,"C22 - Fabrication de papiers et carton"]
["SSP001058401","64.0082","Station service LAMERAIN",null,"En cours",null,null,"En cours","64483","SAINT JEAN DE LUZ","PYRENEES-ATLANTIQUES","NOUVELLE-AQUITAINE","Point",-1.6589959,43.387157,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP001058801","39.0022","TEFAL",null,"En cours",null,null,"En cours","39190","DAMPIERRE","JURA","BOURGOGNE-FRANCHE-COMTE","Point",5.759984,47.158905,"M1 - Industries diverses"]
["SSP001059401","73.0108","Mecad Savoie Industrie",null,"Clôturée",null,"2015-05-11","Clôturée","73121","FRONTENEX","SAVOIE","AUVERGNE-RHONE-ALPES","Point",6.316943,45.62657,"H11 - Usinage"]
["SSP001059701","80.0092","VIDAM  (ex SEDIMEC)",null,"En cours",null,null,"En cours","80481","LIHONS","SOMME","HAUTS-DE-FRANCE","Point",2.7663066,49.82464,"K36 - Mise en décharge"]
["SSP001060001","64.0098","Décharge de Soeix",null,"En cours",null,null,"En cours","64422","OLORON SAINTE MARIE","PYRENEES-ATLANTIQUES","NOUVELLE-AQUITAINE","Point",-0.6313376,43.197353]
["SSP001060501","77.0125","JFCE","JFCE","En cours",null,null,"En cours","77284","MEAUX","SEINE-ET-MARNE","ILE-DE-FRANCE","Polygone",2.9095488,48.96118,"H13 - Traitement de surface"]
["SSP001060701","17.0028","TECHNICENTRE DE SAINTES (ex EIMM)",null,"En cours",null,null,"En cours","17415","SAINTES","CHARENTE-MARITIME","NOUVELLE-AQUITAINE","Point",-0.615668,45.746506,"H1 - Mécanique, électrique, traitement de surface"]
["SSP001061101","25.0044","SOTREFI",null,"En cours",null,null,"En cours","25228","ETUPES","DOUBS","BOURGOGNE-FRANCHE-COMTE","Point",6.8660526,47.51439,"K32 - Traitements physico-chimiques"]
["SSP001062401","84.0023","KSB service EITB-SITELC (Ex SITELEC)",null,"En cours",null,null,"En cours","84007","AVIGNON","VAUCLUSE","PROVENCE-ALPES-COTE D'AZUR","Point",4.8509727,43.938522,"H1 - Mécanique, électrique, traitement de surface"]
["SSP001062801","42.0099","Société Stéphanoise de Construction Mécanique",null,"En cours",null,null,"En cours","42218","SAINT ETIENNE","LOIRE","AUVERGNE-RHONE-ALPES","Point",4.391094,45.45116]
["SSP001063401","64.0092","SAS SADT",null,"En cours",null,null,"En cours","64348","LONS","PYRENEES-ATLANTIQUES","NOUVELLE-AQUITAINE","Point",-0.4237223,43.305767]
["SSP001063701","33.0270","SMICVAL",null,"En cours",null,null,"En cours","33393","SAINT DENIS DE PILE","GIRONDE","NOUVELLE-AQUITAINE","Point",-0.15564884,44.996704]
["SSP001063901","33.0274","GMTP - GIMENO",null,"En cours",null,null,"En cours","33358","ROMAGNE","GIRONDE","NOUVELLE-AQUITAINE","Point",-0.19653231,44.75985]
["SSP001064501","01.0074","TOTAL - site de La Chambière",null,"En cours",null,null,"En cours","01451","VIRIAT","AIN","AUVERGNE-RHONE-ALPES","Point",5.2126913,46.218002,"L23 - Détail de carburants"]
["SSP001064701","33.0280","Decharge de La Brède-Podensac",null,"En cours",null,null,"En cours","33552","VIRELADE","GIRONDE","NOUVELLE-AQUITAINE","Point",-0.42464513,44.644768]
["SSP001065001","33.0293","Décharge de Mariolan",null,"En cours",null,null,"En cours","33529","LA TESTE DE BUCH","GIRONDE","NOUVELLE-AQUITAINE","Point",-1.1567472,44.646805,"K21 - Décharges d'ordures ménagères"]
["SSP001065601","91.0097","Station service  SHELL",null,"En cours",null,null,"En cours","91471","ORSAY","ESSONNE","ILE-DE-FRANCE","Polygone",2.182043,48.693245,"L23 - Détail de carburants"]
["SSP001066101","40.0134","LAMARQUE SOGY BOIS (Castets)",null,"En cours",null,null,"En cours","40333","YGOS SAINT SATURNIN","LANDES","NOUVELLE-AQUITAINE","Point",-0.7411511,43.979897]
["SSP001066901","02.0060","F.E.E. (Flandres Economie Environnementale)",null,"En cours",null,null,"En cours","02014","AMIGNY ROUY","AISNE","HAUTS-DE-FRANCE","Polygone",3.3256147,49.619003,"K36 - Mise en décharge"]
["SSP001067201","64.0102","ALVEA Relais Gantois",null,"En cours",null,null,"En cours","64230","GAN","PYRENEES-ATLANTIQUES","NOUVELLE-AQUITAINE","Point",-0.3871829,43.229828]
["SSP001067401","76.0213","DMS Fécamp",null,"En cours",null,null,"En cours","76259","FECAMP","SEINE-MARITIME","NORMANDIE","Point",0.39501476,49.744675,"L23 - Détail de carburants"]
["SSP001067701","57.0179","LORCA Hauconcourt",null,"En cours",null,null,"En cours","57303","HAUCONCOURT","MOSELLE","GRAND EST","Point",6.1834803,49.205868,"L13 - Entrepôts de produits dangereux"]
["SSP001068301","57.0178","ESSO (La Maxe - A31 - ex TOTAL)",null,"En cours",null,null,"En cours","57452","LA MAXE","MOSELLE","GRAND EST","Point",6.184784,49.150112]
["SSP001068401","38.0278","ERDF",null,"En cours",null,null,"En cours","38544","VIENNE","ISERE","AUVERGNE-RHONE-ALPES","Point",4.874957,45.525097,"D - Chimie, parachimie, pétrole"]
["SSP001068901","02.0061","SANEL PLASTIMARNE - décharge de matière plastique",null,"En cours",null,null,"En cours","02250","CUIRY LES CHAUDARDES","AISNE","HAUTS-DE-FRANCE","Point",3.7690458,49.38568,"K36 - Mise en décharge"]
["SSP001069301","91.0103","CEA de Saclay",null,"En cours",null,null,"En cours","91534","SACLAY","ESSONNE","ILE-DE-FRANCE","Point",2.1567028,48.724125]
["SSP001069501","02.0082","DMS",null,"En cours",null,null,"En cours","02738","TERGNIER","AISNE","HAUTS-DE-FRANCE","Point",0.0,0.0]
["SSP001069901","27.0065","EUROFOIL ex NOVELIS FOIL France",null,"En cours",null,null,"En cours","27502","RUGLES","EURE","NORMANDIE","Point",0.70603466,48.804012,"J32 - Métallurgie de l'aluminium"]
["SSP001070101","33.0308","Station service Patrick SAGE",null,"Clôturée",null,"2013-04-02","Clôturée","33435","SAINT MACAIRE","GIRONDE","NOUVELLE-AQUITAINE","Point",-0.22793357,44.56448,"L23 - Détail de carburants"]
["SSP001070401","41.0042","Delphi Diesel Systems France SAS",null,"En cours",null,null,"En cours","41018","BLOIS","LOIR-ET-CHER","CENTRE-VAL DE LOIRE","Point",1.3248683,47.60304,"H - Mécanique, traitements des surfaces"]
["SSP001071101","31.0063","SIRIUS DEVELOPPEMENT (ex CIREP)",null,"En cours",null,null,"En cours","31555","TOULOUSE","HAUTE-GARONNE","OCCITANIE","Point",1.4003837,43.546154,"H13 - Traitement de surface"]
["SSP001071201","64.0103","THYSSENKRUPP",null,"En cours",null,null,"En cours","64062","ARUDY","PYRENEES-ATLANTIQUES","NOUVELLE-AQUITAINE","Point",-0.43603918,43.10924]
["SSP001071701","51.0063","BOLLORE ENERGIE SA",null,"En cours",null,null,"En cours","51454","REIMS","MARNE","GRAND EST","Point",4.000177,49.265266]
["SSP001072301","27.0064","STRATEC (ex FACOM)",null,"En cours",null,null,"En cours","27230","EZY SUR EURE","EURE","NORMANDIE","Point",1.397833,48.864544,"H11 - Usinage"]
["SSP001072801","76.0221","DANONE NEUFCHATEL « Garage »",null,"En cours",null,null,"En cours","76462","NEUFCHATEL EN BRAY","SEINE-MARITIME","NORMANDIE","Point",1.433705,49.736553,"B1 - Industrie agro-alimentaire"]
["SSP001072901","76.0222","DANONE NEUFCHATEL « Usine »",null,"En cours",null,null,"En cours","76462","NEUFCHATEL EN BRAY","SEINE-MARITIME","NORMANDIE","Point",1.433705,49.736553]
["SSP001073401","60.0100","Kohler France (ex Jacob Delafon)",null,"En cours",null,null,"En cours","60471","NOYON","OISE","HAUTS-DE-FRANCE","Point",3.0112293,49.57665,"J51 - Fonderie des métaux ferreux"]
["SSP001073901","51.0075","Morgan Cupex",null,"En cours",null,null,"En cours","51504","SAINT MARTIN SUR LE PRE","MARNE","GRAND EST","Point",4.362478,48.99237]
["SSP001075001","42.0102","FOREZ PEINTURES",null,"En cours",null,null,"En cours","42218","SAINT ETIENNE","LOIRE","AUVERGNE-RHONE-ALPES","Point",4.4036946,45.45358,"L1 - Entreposage, manutention, commerces"]
["SSP001075201","76.0227","SEA INVEST zone 2",null,"En cours",null,null,"En cours","76319","GRAND COURONNE","SEINE-MARITIME","NORMANDIE","Point",0.99521744,49.359608,"L13 - Entrepôts de produits dangereux"]
["SSP001075501","76.0229","GALVANORM",null,"En cours",null,null,"En cours","76366","LE HOULME","SEINE-MARITIME","NORMANDIE","Point",1.0349406,49.51448,"H13 - Traitement de surface"]
["SSP001076001","77.0129","ANCIENNE UIOM ","ANCIENNE UIOM ","En cours",null,null,"En cours","77487","VAUX LE PENIL","SEINE-ET-MARNE","ILE-DE-FRANCE","Polygone",2.691959,48.541958,"K2 - Traitement de déchets urbains"]
["SSP001076501","31.0061","ALQUIER ET FILS",null,"En cours",null,null,"En cours","31478","SAINT FELIX LAURAGAIS","HAUTE-GARONNE","OCCITANIE","Point",1.9458671,43.445568,"C13 - Traitement du bois"]
["SSP001076701","37.0020","AERAZUR",null,"En cours",null,null,"En cours","37020","BEAULIEU LES LOCHES","INDRE-ET-LOIRE","CENTRE-VAL DE LOIRE","Point",1.011266,47.12833,"D71 - Industrie du caoutchouc"]
["SSP001077201","42.0110","AUTOS DIFFUSION - (REGIE RENAULT)",null,"En cours",null,null,"En cours","42218","SAINT ETIENNE","LOIRE","AUVERGNE-RHONE-ALPES","Point",4.3834167,45.459385,"L21 - Vente et réparation automobile"]
["SSP001077501","42.0114","Total Raffinage-Marketing (ex :ELF ANTARGAZ)",null,"En cours",null,null,"En cours","42186","RIVE DE GIER","LOIRE","AUVERGNE-RHONE-ALPES","Point",4.6223416,45.53011,"L23 - Détail de carburants"]
["SSP001078101","59.0506","UIOM Petite-Synthe",null,"En cours",null,null,"En cours","59183","DUNKERQUE","NORD","HAUTS-DE-FRANCE","Point",2.3178308,51.002747,"K31 - Incinération"]
["SSP001078301","54.0113","Station-service Relais Trois Maisons","Pollution accidentelle 2007","En cours",null,null,"En cours","54395","NANCY","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",6.1695504,48.704903,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP001078601","24.0053","Domaine d'Essendieras",null,"En cours",null,null,"En cours","24463","SAINT MEDARD D'EXCIDEUIL","DORDOGNE","NOUVELLE-AQUITAINE","Point",1.0884188,45.34368]
["SSP001079301","33.0315","Station service ESSO Bel Air",null,"En cours",null,null,"En cours","33063","BORDEAUX","GIRONDE","NOUVELLE-AQUITAINE","Point",-0.60747206,44.839657]
["SSP001079701","70.0022","FAURECIA",null,"En cours",null,null,"En cours","70310","LURE","HAUTE-SAONE","BOURGOGNE-FRANCHE-COMTE","Point",6.4919596,47.681404,"D7 - Caoutchouc et matières plastiques"]
["SSP001079801","64.0107","Papeterie des Gaves",null,"En cours",null,null,"En cours","64430","ORTHEZ","PYRENEES-ATLANTIQUES","NOUVELLE-AQUITAINE","Point",-0.7799319,43.489616,"C22 - Fabrication de papiers et carton"]
["SSP001080201","45.0037","RIC ENVIRONNEMENT",null,"En cours",null,null,"En cours","45053","BRIARE","LOIRET","CENTRE-VAL DE LOIRE","Point",2.7701318,47.611084,"K52 - Dépôts de ferraille"]
["SSP001080801","31.0086","WOLSELEY France BOIS et Matériaux SA",null,"En cours",null,null,"En cours","31467","SAINT ALBAN","HAUTE-GARONNE","OCCITANIE","Point",1.4053227,43.69087,"C13 - Traitement du bois"]
["SSP001081401","94.0062","AIR FRANCE INDUSTRIES site ORLY",null,"En cours",null,null,"En cours","94054","ORLY","VAL-DE-MARNE","ILE-DE-FRANCE","Point",2.3740728,48.74557,"H - Mécanique, traitements des surfaces"]
["SSP001081601","76.0241","Renault",null,"En cours",null,null,"En cours","76178","CLEON","SEINE-MARITIME","NORMANDIE","Point",1.0479146,49.315792,"H15 - Assemblage, montage"]
["SSP001081901","45.0041","ARJOWIGGINS (ex COPIGRAPH)",null,"En cours",null,null,"En cours","45191","MALESHERBES","LOIRET","CENTRE-VAL DE LOIRE","Point",2.3862236,48.29836,"C22 - Fabrication de papiers et carton"]
["SSP001082501","44.0144","Fonderie Atlantique Industrie (FAI)",null,"En cours",null,null,"En cours","44109","NANTES","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Point",-1.5969585,47.194115,"J52 - Fonderie des métaux non ferreux"]
["SSP001083001","70.0023","SMG MAGYAR (Société Métallurgique de Gray )",null,"En cours",null,null,"En cours","70026","ARC LES GRAY","HAUTE-SAONE","BOURGOGNE-FRANCHE-COMTE","Point",5.6020956,47.459415]
["SSP001083101","90.0017","Ancienne usine d'incinération de Fêche l'Eglise",null,"En cours",null,null,"En cours","90045","FECHE L'EGLISE","TERRITOIRE DE BELFORT","BOURGOGNE-FRANCHE-COMTE","Point",6.9570475,47.50579,"K31 - Incinération"]
["SSP001083701","71.0084","MONCIA (Ex SOCCRAM)",null,"En cours",null,null,"En cours","71306","MONTCEAU LES MINES","SAONE-ET-LOIRE","BOURGOGNE-FRANCHE-COMTE","Point",4.349297,46.66453,"I21 - Chaufferies urbaines"]
["SSP001084301","37.0026","AUTO CAST",null,"En cours",null,null,"En cours","37027","BLERE","INDRE-ET-LOIRE","CENTRE-VAL DE LOIRE","Point",0.9890581,47.330185,"J51 - Fonderie des métaux ferreux"]
["SSP001084801","90.0022","CAB (UIOM BELFORT)",null,"En cours",null,null,"En cours","90010","BELFORT","TERRITOIRE DE BELFORT","BOURGOGNE-FRANCHE-COMTE","Point",6.859653,47.627678,"K2 - Traitement de déchets urbains"]
["SSP001085001","28.0058","SOMEL (ex-UIOM)",null,"En cours",null,null,"En cours","28280","NOGENT LE ROTROU","EURE-ET-LOIR","CENTRE-VAL DE LOIRE","Point",0.84520555,48.300343,"K31 - Incinération"]
["SSP001085301","28.0059","SOMEL (ex-UIOM)",null,"En cours",null,null,"En cours","28127","DANGEAU","EURE-ET-LOIR","CENTRE-VAL DE LOIRE","Point",1.303536,48.21733,"K36 - Mise en décharge"]
["SSP001086101","76.0246","GP Est",null,"En cours",null,null,"En cours","76322","LE GRAND QUEVILLY","SEINE-MARITIME","NORMANDIE","Point",1.0328822,49.42394,"D36 - Fabrication des engrais"]
["SSP001086501","10.0067","Autocasse Thiebault",null,"En cours",null,null,"En cours","10325","ROSIERES PRES TROYES","AUBE","GRAND EST","Point",4.0477786,48.26186]
["SSP001086601","18.0046","CHAMPION SUPERMARCHE FRANCE",null,"En cours",null,null,"En cours","18033","BOURGES","CHER","CENTRE-VAL DE LOIRE","Point",2.4028733,47.10611,"L23 - Détail de carburants"]
["SSP001087001","76.0249","Oissel remediation",null,"En cours",null,null,"En cours","76484","OISSEL","SEINE-MARITIME","NORMANDIE","Point",1.1134382,49.34396]
["SSP001087501","18.0047","SMURFIT KAPPA PAPIER RECYCLE FRANCE (ancienne papeterie)",null,"En cours",null,null,"En cours","18270","VALLENAY","CHER","CENTRE-VAL DE LOIRE","Point",2.3709905,46.80255]
["SSP001088701","41.0051","VALDEM - Lignières (décharge)",null,"En cours",null,null,"En cours","41115","LIGNIERES","LOIR-ET-CHER","CENTRE-VAL DE LOIRE","Point",1.1849726,47.88374,"K21 - Décharges d'ordures ménagères"]
["SSP001089101","93.0055","SOS TRAITEMENT DE SURFACE",null,"En cours",null,null,"En cours","93055","PANTIN","SEINE-SAINT-DENIS","ILE-DE-FRANCE","Point",2.4120615,48.88844,"H13 - Traitement de surface"]
["SSP001089601","93.0056","FAIVELEY (ex SAB WABCO)",null,"En cours",null,null,"En cours","93071","SEVRAN","SEINE-SAINT-DENIS","ILE-DE-FRANCE","Point",2.5201075,48.926582]
["SSP001090101","94.0066","ALKAN",null,"En cours",null,null,"En cours","94074","VALENTON","VAL-DE-MARNE","ILE-DE-FRANCE","Point",2.4716961,48.740112,"H - Mécanique, traitements des surfaces"]
["SSP001090501","42.0120","SOCIETE DENIS",null,"En cours",null,null,"En cours","42330","VILLARS","LOIRE","AUVERGNE-RHONE-ALPES","Point",4.356728,45.470123,"J53 - Travail des métaux, chaudronnerie, poudres"]
["SSP001090801","76.0261","LOZAÏ",null,"En cours",null,null,"En cours","76498","LE PETIT QUEVILLY","SEINE-MARITIME","NORMANDIE","Point",1.0470223,49.43232,"J53 - Travail des métaux, chaudronnerie, poudres"]
["SSP001091001","27.0079","HEMERY S.A.",null,"En cours",null,null,"En cours","27665","TROUVILLE LA HAULE","EURE","NORMANDIE","Point",0.556735,49.43581,"K5 - Récupération, dépôts de ferrailles"]
["SSP001091501","60.0106","Agora Ex Force 5",null,"En cours",null,null,"En cours","60395","MERU","OISE","HAUTS-DE-FRANCE","Point",2.131831,49.229256]
["SSP001091801","68.0146","LIEBHERR France",null,"En cours",null,null,"En cours","68066","COLMAR","HAUT-RHIN","GRAND EST","Point",7.366245,48.095062,"G14 - Fabrication d'autres matériaux de construction"]
["SSP001092101","77.0131","VOESTALPINE ROTEC France","VOESTALPINE ROTEC France","En cours",null,null,"En cours","77350","OZOIR LA FERRIERE","SEINE-ET-MARNE","ILE-DE-FRANCE","Polygone",2.6859019,48.768818,"J53 - Travail des métaux, chaudronnerie, poudres"]
["SSP001092801","88.0075","Station service - Rue de la Belle Orge",null,"En cours",null,null,"En cours","88372","RAON L'ETAPE","VOSGES","GRAND EST","Point",6.8354144,48.403282]
["SSP001093301","08.0060","Ateliers des Janves",null,"En cours",null,null,"En cours","08081","BOGNY SUR MEUSE","ARDENNES","GRAND EST","Point",4.745269,49.85924,"J5 - Fonderie et travail des métaux"]
["SSP001093701","37.0029","SNCF MAGASIN GENERAL",null,"En cours",null,null,"En cours","37233","SAINT PIERRE DES CORPS","INDRE-ET-LOIRE","CENTRE-VAL DE LOIRE","Point",0.7343458,47.38457,"L1 - Entreposage, manutention, commerces"]
["SSP001094001","19.0020","EDF - LES BORDES",null,"En cours",null,null,"En cours","19031","BRIVE LA GAILLARDE","CORREZE","NOUVELLE-AQUITAINE","Polygone",1.5502396,45.165066]
["SSP001094201","67.0151","Station service Total Wietrich",null,"En cours",null,null,"En cours","67101","DORLISHEIM","BAS-RHIN","GRAND EST","Point",7.498328,48.52544,"L23 - Détail de carburants"]
["SSP001094801","08.0066","FRICHE MANIL",null,"En cours",null,null,"En cours","08488","VIVIER AU COURT","ARDENNES","GRAND EST","Point",4.830184,49.736065,"J5 - Fonderie et travail des métaux"]
["SSP001095101","26.0052","RENCAST",null,"En cours",null,null,"En cours","26281","ROMANS SUR ISERE","DROME","AUVERGNE-RHONE-ALPES","Point",5.0890145,45.05475,"J52 - Fonderie des métaux non ferreux"]
["SSP001095301","94.0068","METAL COULEUR SYSTEMES",null,"En cours",null,null,"En cours","94011","BONNEUIL SUR MARNE","VAL-DE-MARNE","ILE-DE-FRANCE","Point",2.5025811,48.779865,"H13 - Traitement de surface"]
["SSP001096201","08.0067","BOLLORE ENERGIE ex : SHELL DIRECT",null,"En cours",null,null,"En cours","08190","GIVET","ARDENNES","GRAND EST","Point",4.8253546,50.155754,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP001096601","39.0025","CENEMAT_ CdC du COMTE DE GRIMONT",null,"En cours",null,null,"En cours","39354","MONTHOLIER","JURA","BOURGOGNE-FRANCHE-COMTE","Point",5.644939,46.895973]
["SSP001097201","38.0163","Gare de Jallieu",null,"En cours",null,null,"En cours","38053","BOURGOIN JALLIEU","ISERE","AUVERGNE-RHONE-ALPES","Point",5.2713437,45.601974,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP001097501","38.0164","Compagnie de Distribution des Hydrocarbures (CDH)",null,"En cours",null,null,"En cours","38558","VILLETTE DE VIENNE","ISERE","AUVERGNE-RHONE-ALPES","Point",4.916695,45.574123,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP001097701","74.0104","CAUX",null,"En cours",null,null,"En cours","74264","SCIONZIER","HAUTE-SAVOIE","AUVERGNE-RHONE-ALPES","Point",6.5498533,46.06634,"H13 - Traitement de surface"]
["SSP001098201","69.0229","DAFFOS ET BAUDASSE",null,"En cours",null,null,"En cours","69266","VILLEURBANNE","RHONE","AUVERGNE-RHONE-ALPES","Point",4.919422,45.76107,"K - Déchets et traitements"]
["SSP001098501","88.0078","Station service TOTAL - Relais du bois des Chênes - Vincey",null,"En cours",null,null,"En cours","88513","VINCEY","VOSGES","GRAND EST","Point",6.338451,48.331715]
["SSP001098701","88.0081","Papeterie GREGOIRE",null,"En cours",null,null,"En cours","88429","SAINT NABORD","VOSGES","GRAND EST","Point",6.5768723,48.02692]
["SSP001099201","38.0168","LAUZIER",null,"En cours",null,null,"En cours","38053","BOURGOIN JALLIEU","ISERE","AUVERGNE-RHONE-ALPES","Point",5.2739973,45.580326,"J5 - Fonderie et travail des métaux"]
["SSP001099601","77.0135","AMCOR FLEXIBLES SPS","AMCOR FLEXIBLES SPS","En cours",null,null,"En cours","77131","COULOMMIERS","SEINE-ET-MARNE","ILE-DE-FRANCE","Polygone",3.0958319,48.806293,"D72 - Transformation des matières plastiques"]
["SSP001100101","69.0233","DEL SIGNORE",null,"En cours",null,null,"En cours","69266","VILLEURBANNE","RHONE","AUVERGNE-RHONE-ALPES","Point",4.886528,45.78328,"H13 - Traitement de surface"]
["SSP001100201","38.0172","FOURNIER (ex CODIS)",null,"En cours",null,null,"En cours","38239","MOIRANS","ISERE","AUVERGNE-RHONE-ALPES","Point",5.5805264,45.323154,"L13 - Entrepôts de produits dangereux"]
["SSP001100801","89.0020","ESSO SAF (  ancienne usine Bitume et Emulsions d'Auxerre)",null,"En cours",null,null,"En cours","89024","AUXERRE","YONNE","BOURGOGNE-FRANCHE-COMTE","Point",3.580004,47.795483,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP001101101","89.0023"," POIDS LOURDS 2000",null,"En cours",null,null,"En cours","89433","VAULT DE LUGNY","YONNE","BOURGOGNE-FRANCHE-COMTE","Point",3.851364,47.498913,"L1 - Entreposage, manutention, commerces"]
["SSP001101701","974.0019","décharge d'ordures ménagères de la Ravine Cocâtre",null,"En cours",null,null,"En cours","97423","LES TROIS-BASSINS","LA REUNION","LA REUNION","Point",55.315292,-21.1167,"K21 - Décharges d'ordures ménagères"]
["SSP001101801","89.0026","Etablissements CHARLES GARNIER",null,"En cours",null,null,"En cours","89460","VILLENEUVE LA GUYARD","YONNE","BOURGOGNE-FRANCHE-COMTE","Point",3.060482,48.34005,"J34 - Métallurgie des métaux précieux"]
["SSP001102301","38.0174","BEAL Recyclage",null,"En cours",null,null,"En cours","38130","LA COTE SAINT ANDRE","ISERE","AUVERGNE-RHONE-ALPES","Point",5.2618556,45.386513,"K5 - Récupération, dépôts de ferrailles"]
["SSP001102701","22.0016","Centre Technique Départemental (CTD) / Le Légué",null,"En cours",null,null,"En cours","22278","SAINT BRIEUC","COTES-D'ARMOR","BRETAGNE","Point",-2.73785,48.527073,"G2 - Chantiers, construction, bitumes, enrobés"]
["SSP001103101","974.0023","décharge d'ordures ménagères de Bras-Creux",null,"En cours",null,null,"En cours","97422","LE TAMPON","LA REUNION","LA REUNION","Point",55.54226,-21.258547,"K21 - Décharges d'ordures ménagères"]
["SSP001103201","974.0024","décharge d'ordures ménagères de la Bergerie (Petit Tampon)",null,"En cours",null,null,"En cours","97422","LE TAMPON","LA REUNION","LA REUNION","Point",55.533836,-21.288889,"K21 - Décharges d'ordures ménagères"]
["SSP001103701","69.0339","PRECIAL CASTING",null,"Clôturée",null,"2013-01-16","Clôturée","69059","CIVRIEUX D'AZERGUES","RHONE","AUVERGNE-RHONE-ALPES","Point",4.7000446,45.85456,"J52 - Fonderie des métaux non ferreux"]
["SSP001104001","974.0026","décharge d'ordures ménagères de Vincendo",null,"En cours",null,null,"En cours","97412","SAINT-JOSEPH","LA REUNION","LA REUNION","Point",55.668964,-21.377926,"K21 - Décharges d'ordures ménagères"]
["SSP001104601","974.0032","décharge d'ordures ménagères de la Montagne",null,"En cours",null,null,"En cours","97411","SAINT-DENIS","LA REUNION","LA REUNION","Point",55.417747,-20.885952,"K21 - Décharges d'ordures ménagères"]
["SSP001104701","974.0033","décharge d'ordures ménagères de la Cressonnière",null,"En cours",null,null,"En cours","97409","SAINT-ANDRE","LA REUNION","LA REUNION","Point",55.664803,-20.981606,"K21 - Décharges d'ordures ménagères"]
["SSP001105301","64.0109","Décharge de Bénéjacq",null,"En cours",null,null,"En cours","64109","BENEJACQ","PYRENEES-ATLANTIQUES","NOUVELLE-AQUITAINE","Point",-0.21149951,43.18874]
["SSP001105601","08.0074","Fonte ardennaise FA3 - crassier",null,"En cours",null,null,"En cours","08491","VRIGNE AUX BOIS","ARDENNES","GRAND EST","Point",4.849085,49.73302,"K36 - Mise en décharge"]
["SSP001106401","67.0154","dépôt du Gressen",null,"En cours",null,null,"En cours","67212","HOLTZHEIM","BAS-RHIN","GRAND EST","Point",7.6636333,48.55083]
["SSP001106501","08.0081","Freddy Golinval Recyclage (FGR)",null,"En cours",null,null,"En cours","08081","BOGNY SUR MEUSE","ARDENNES","GRAND EST","Point",2.3452773,48.860832,"K5 - Récupération, dépôts de ferrailles"]
["SSP001107001","88.0082","Station-service TOTAL - Epinal - Rue Serot",null,"En cours",null,null,"En cours","88160","EPINAL","VOSGES","GRAND EST","Point",6.4499393,48.178867,"L2 - Transports, automobile, carburants"]
["SSP001107401","56.0018","PARKER HANNIFIN MANUFACTURING FRANCE SAS (ex LEGRIS)",null,"En cours",null,null,"En cours","56228","SAINT MARCEL","MORBIHAN","BRETAGNE","Point",-2.4057565,47.805454,"H - Mécanique, traitements des surfaces"]
["SSP001108301","42.0148","FIPROFIL SA GUILLAUMOND – SYSTEM PLUM",null,"En cours",null,null,"En cours","42237","SAINT JEAN BONNEFONDS","LOIRE","AUVERGNE-RHONE-ALPES","Point",4.4228754,45.44507,"J5 - Fonderie et travail des métaux"]
["SSP001108701","29.0058","COMBUSTIBLES DE L'OUEST (CPO)",null,"En cours",null,null,"En cours","29232","QUIMPER","FINISTERE","BRETAGNE","Point",-4.0217137,47.982533,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP001109001","38.0260","HENRY TIMBER (ex VALSCIUS)",null,"En cours",null,null,"En cours","38394","SAINT HILAIRE DU ROSIER","ISERE","AUVERGNE-RHONE-ALPES","Point",5.246926,45.071663,"C22 - Fabrication de papiers et carton"]
["SSP001109501","77.0139","METAUX OUVRES ET DECORES","METAUX OUVRES ET DECORES","En cours",null,null,"En cours","77284","MEAUX","SEINE-ET-MARNE","ILE-DE-FRANCE","Polygone",2.8761513,48.96705,"H13 - Traitement de surface"]
["SSP001109901","29.0063","VALCOR",null,"Clôturée",null,"2015-02-06","Clôturée","29046","DOUARNENEZ","FINISTERE","BRETAGNE","Point",-4.3197346,48.07955]
["SSP001110001","77.0140","Brodard Graphique",null,"En cours",null,null,"En cours","77131","COULOMMIERS","SEINE-ET-MARNE","ILE-DE-FRANCE","Polygone",3.090014,48.805973,"H21 - Imprimerie, presse, édition"]
["SSP001110401","76.0271","DESGENETAIS (friche) (ex. Société Lillebonnaise de Caoutchouc)",null,"En cours",null,null,"En cours","76114","BOLBEC","SEINE-MARITIME","NORMANDIE","Point",0.49223363,49.57693]
["SSP001111001","71.0040","POWERTRAIN (ex IVECO FRANCE)",null,"En cours",null,null,"En cours","71047","BOURBON LANCY","SAONE-ET-LOIRE","BOURGOGNE-FRANCHE-COMTE","Point",3.7475307,46.626587]
["SSP001111801","71.0043","THEVENIN & DUCROT (ex SHELL )",null,"En cours",null,null,"En cours","71269","LUX","SAONE-ET-LOIRE","BOURGOGNE-FRANCHE-COMTE","Point",4.84674,46.75416]
["SSP001112001","68.0150","TOTAL avenue de colmar",null,"En cours",null,null,"En cours","68224","MULHOUSE","HAUT-RHIN","GRAND EST","Point",7.326366,47.761738,"L2 - Transports, automobile, carburants"]
["SSP001112301","71.0046","TOTAL RAFFINAGE MARKETING (Tournus)",null,"En cours",null,null,"En cours","71543","TOURNUS","SAONE-ET-LOIRE","BOURGOGNE-FRANCHE-COMTE","Point",4.903879,46.572414,"L23 - Détail de carburants"]
["SSP001112901","52.0037","FONDERIE VIRY",null,"En cours",null,null,"En cours","52006","ALLICHAMPS","HAUTE-MARNE","GRAND EST","Point",4.892745,48.56069,"J35 - Autres métaux non ferreux (métallurgie des)"]
["SSP001113301","71.0053","TOTAL RAFFINAGE MARKETING (Autun)",null,"En cours",null,null,"En cours","71014","AUTUN","SAONE-ET-LOIRE","BOURGOGNE-FRANCHE-COMTE","Point",4.311801,46.95533,"L23 - Détail de carburants"]
["SSP001113401","59.0533","FLANDRIA ALUMINIUM",null,"En cours",null,null,"En cours","59643","WARNETON","NORD","HAUTS-DE-FRANCE","Point",2.9444644,50.745117,"J21 - Production de fontes (haut fourneau)"]
["SSP001113801","76.0272","Fourcin",null,"En cours",null,null,"En cours","76212","DARNETAL","SEINE-MARITIME","NORMANDIE","Point",1.2082741,49.440033]
["SSP001114301","84.0027","La Mure BIANCO",null,"En cours",null,null,"En cours","84053","GRILLON","VAUCLUSE","PROVENCE-ALPES-COTE D'AZUR","Polygone",4.934262,44.396675,"L23 - Détail de carburants"]
["SSP001114801","58.0018","POUGUES BAUDRAS SCI (Station-service)",null,"En cours",null,null,"En cours","58214","POUGUES LES EAUX","NIEVRE","BOURGOGNE-FRANCHE-COMTE","Point",0.0,0.0,"L23 - Détail de carburants"]
["SSP001115001","58.0021","SIOM de La Machine",null,"En cours",null,null,"En cours","58151","LA MACHINE","NIEVRE","BOURGOGNE-FRANCHE-COMTE","Point",0.0,0.0,"K - Déchets et traitements"]
["SSP001115301","77.0142","WIPELEC (ex CACI COMPAGNIE D'APPLICATIONS CHIMIQUES)","WIPELEC (ex CACI COMPAGNIE D'APPLICATIONS CHIMIQUES)","En cours",null,null,"En cours","77284","MEAUX","SEINE-ET-MARNE","ILE-DE-FRANCE","Polygone",2.9095511,48.96416,"D42 - Fabrication de peintures"]
["SSP001115801","83.0030","Station Service TOTAL Champs de Mars",null,"En cours",null,null,"En cours","83137","TOULON","VAR","PROVENCE-ALPES-COTE D'AZUR","Point",5.9379525,43.123116,"L23 - Détail de carburants"]
["SSP001116201","83.0031","Station Service de Bonnegrâce",null,"En cours",null,null,"En cours","83129","SIX FOURS LES PLAGES","VAR","PROVENCE-ALPES-COTE D'AZUR","Point",5.8131213,43.110092,"L23 - Détail de carburants"]
["SSP001116301","83.0032","Station Service AVIA - L'Esterel",null,"En cours",null,null,"En cours","83001","LES ADRETS DE L'ESTEREL","VAR","PROVENCE-ALPES-COTE D'AZUR","Point",6.785844,43.54164,"L23 - Détail de carburants"]
["SSP001116701","01.0084","SCHNEIDER ELECTRIC",null,"En cours",null,null,"En cours","01343","SAINT CYR SUR MENTHON","AIN","AUVERGNE-RHONE-ALPES","Point",4.955553,46.273285]
["SSP001117201","01.0089","Tissus Techniques de Trévoux",null,"En cours",null,null,"En cours","01427","TREVOUX","AIN","AUVERGNE-RHONE-ALPES","Point",4.7531767,45.945793]
["SSP001117501","69.0238","JST Transformateur",null,"En cours",null,null,"En cours","69123","LYON","RHONE","AUVERGNE-RHONE-ALPES","Point",4.8746557,45.730488,"M1 - Industries diverses"]
["SSP001117701","06.0026","PROMAROUTE",null,"En cours",null,null,"En cours","06088","NICE","ALPES-MARITIMES","PROVENCE-ALPES-COTE D'AZUR","Point",7.1900325,43.695415,"G22 - Centrales d'enrobés"]
["SSP001118401","27.0082","HENKEL France",null,"En cours",null,null,"En cours","27375","LOUVIERS","EURE","NORMANDIE","Point",1.1717424,49.231434,"D44 - Fabrication de colles et mastics"]
["SSP001119101","04.0020","ARKEMA - Electrolyse à Mercure",null,"En cours",null,null,"En cours","04049","CHATEAU ARNOUX SAINT AUBAN","ALPES-DE-HAUTE-PROVENCE","PROVENCE-ALPES-COTE D'AZUR","Point",6.000977,44.063953,"D31 - Industrie du chlore"]
["SSP001119501","90.0026","VMC Pêche",null,"En cours",null,null,"En cours","90072","MORVILLARS","TERRITOIRE DE BELFORT","BOURGOGNE-FRANCHE-COMTE","Point",6.933147,47.54654]
["SSP001119601","62.0156","Cuno France Filtration SAS",null,"En cours",null,null,"En cours","62043","LES ATTAQUES","PAS-DE-CALAIS","HAUTS-DE-FRANCE","Point",1.9665172,50.893936,"J53 - Travail des métaux, chaudronnerie, poudres"]
["SSP001120001","12.0026","UMICORE DECHETS (ex UNION MINIERE, ex VIEILLE MONTAGNE)",null,"En cours",null,null,"En cours","12305","VIVIEZ","AVEYRON","OCCITANIE","Point",2.2227128,44.5507,"J52 - Fonderie des métaux non ferreux"]
["SSP001120801","62.0163","MECCANO SA",null,"En cours",null,null,"En cours","62193","CALAIS","PAS-DE-CALAIS","HAUTS-DE-FRANCE","Point",2.15834,50.991703]
["SSP001121201","88.0087","MICHELIN",null,"En cours",null,null,"En cours","88209","GOLBEY","VOSGES","GRAND EST","Point",6.4335346,48.21051]
["SSP001121401","62.0165","Desvres SA (ancienne usine de carrelage)",null,"En cours",null,null,"En cours","62268","DESVRES","PAS-DE-CALAIS","HAUTS-DE-FRANCE","Point",1.8138555,50.66923]
["SSP001121901","42.0143","STATION SERVICE CASINO CARBURANTS",null,"En cours",null,null,"En cours","42275","SAINT PRIEST EN JAREZ","LOIRE","AUVERGNE-RHONE-ALPES","Point",4.3566823,45.479256,"L23 - Détail de carburants"]
["SSP001122401","62.0172","Station TOTAL SARL Lefebvre",null,"En cours",null,null,"En cours","62811","THEROUANNE","PAS-DE-CALAIS","HAUTS-DE-FRANCE","Point",2.2512426,50.63062]
["SSP001122801","59.0543","ISDND STR EUROVIA",null,"En cours",null,null,"En cours","59359","LOON PLAGE","NORD","HAUTS-DE-FRANCE","Point",2.2110481,51.001095]
["SSP001122901","62.0176","ISDND d'Ergny",null,"En cours",null,null,"En cours","62302","ERGNY","PAS-DE-CALAIS","HAUTS-DE-FRANCE","Point",1.9210085,50.569633,"K36 - Mise en décharge"]
["SSP001123301","33.0326","LIANTS DISTRIBUTION",null,"En cours",null,null,"En cours","33004","AMBES","GIRONDE","NOUVELLE-AQUITAINE","Point",-0.56241095,45.00738]
["SSP001123801","77.0144","STREL","STREL","En cours",null,null,"En cours","77320","MOUROUX","SEINE-ET-MARNE","ILE-DE-FRANCE","Polygone",3.074884,48.821896,"H1 - Mécanique, électrique, traitement de surface"]
["SSP001124101","45.0046","SRTM ( ex JAPOROP )",null,"En cours",null,null,"En cours","45036","BOISMORAND","LOIRET","CENTRE-VAL DE LOIRE","Point",2.7378118,47.76377,"L21 - Vente et réparation automobile"]
["SSP001124301","02.0076","SAINT LOUIS SUCRE",null,"En cours",null,null,"En cours","02211","CONDE SUR SUIPPE","AISNE","HAUTS-DE-FRANCE","Point",3.9615736,49.42553,"B14 - Industrie du sucre"]
["SSP001124801","59.0546","GlassDéco",null,"En cours",null,null,"En cours","59249","FOURMIES","NORD","HAUTS-DE-FRANCE","Point",4.030559,50.024483]
["SSP001125301","76.0284","WOREX",null,"En cours",null,null,"En cours","76638","SAINT PIERRE EN VAL","SEINE-MARITIME","NORMANDIE","Point",1.4431177,50.024044,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP001125701","63.0039","ZI de Cournon d'Auvergne (ex éts CAREL FOUCHE LANGUEPIN)",null,"En cours",null,null,"En cours","63124","COURNON D'AUVERGNE","PUY-DE-DOME","AUVERGNE-RHONE-ALPES","Point",3.1663702,45.738747,"K3 - Traitement de déchets industriels"]
["SSP001125801","64.0113","Décharge de Salies de Béarn",null,"En cours",null,null,"En cours","64499","SALIES DE BEARN","PYRENEES-ATLANTIQUES","NOUVELLE-AQUITAINE","Point",-0.92607766,43.470993]
["SSP001126301","33.0328","ICL France (ex PRIMALAB)",null,"En cours",null,null,"En cours","33200","LE HAILLAN","GIRONDE","NOUVELLE-AQUITAINE","Point",-0.67157763,44.869205,"D3 - Chimie, phytosanitaire, pharmacie"]
["SSP001126801","69.0239","SHELL Villeurbanne (Cours Emile Zola)",null,"En cours",null,null,"En cours","69266","VILLEURBANNE","RHONE","AUVERGNE-RHONE-ALPES","Point",4.8785696,45.769974,"L23 - Détail de carburants"]
["SSP001127101","33.0505","LAGARDE SA",null,"En cours",null,null,"En cours","33433","SAINT LOUBES","GIRONDE","NOUVELLE-AQUITAINE","Polygone",-0.46348614,44.922016,null,"23.03 - Fabrication d'outillage, outils pour machines"]
["SSP001127301","76.0287","CHAUFFERIE BOIS ENERGIE",null,"En cours",null,null,"En cours","76410","MAROMME","SEINE-MARITIME","NORMANDIE","Point",1.027388,49.487495]
["SSP001127901","60.0111","UMICORE (Vieille montagne)",null,"En cours",null,null,"En cours","60175","CREIL","OISE","HAUTS-DE-FRANCE","Point",2.4778793,49.257328]
["SSP001128201","69.0250","MAJ",null,"Clôturée",null,"2018-01-18","Clôturée","69266","VILLEURBANNE","RHONE","AUVERGNE-RHONE-ALPES","Point",4.8927374,45.755596]
["SSP001128701","67.0163","BRASSERIE KRONENBOURG",null,"En cours",null,null,"En cours","67348","OBERNAI","BAS-RHIN","GRAND EST","Point",7.4988236,48.470703]
["SSP001128801","67.0164","PUNCH Powerglide Strasbourg S.A.S.",null,"En cours",null,null,"En cours","67482","STRASBOURG","BAS-RHIN","GRAND EST","Point",7.7872024,48.537704]
["SSP001129201","69.0251","EDA GEORGES DAVID ex SCMP",null,"Clôturée",null,-687449.0351736111,"Clôturée","69275","DECINES CHARPIEU","RHONE","AUVERGNE-RHONE-ALPES","Point",4.9371676,45.762157,"D72 - Transformation des matières plastiques"]
["SSP001129601","67.0166","SAPLAST",null,"En cours",null,null,"En cours","67482","STRASBOURG","BAS-RHIN","GRAND EST","Point",7.787173,48.537678]
["SSP001130101","69.0271","Station-service Relais Felix Faure",null,"En cours",null,null,"En cours","69123","LYON","RHONE","AUVERGNE-RHONE-ALPES","Point",4.871742,45.755344]
["SSP001130201","77.0146","OFFREDY (site de la rue Lavoisier)","OFFREDY (site de la rue Lavoisier)","En cours","2006-06-27",null,"En cours","77350","OZOIR LA FERRIERE","SEINE-ET-MARNE","ILE-DE-FRANCE","Polygone",2.6804397,48.769665,"H13 - Traitement de surface"]
["SSP001130801","57.0222","CERTAS ENERGY France (ex ESSO - avenue de Strasbourg)",null,"En cours",null,null,"En cours","57463","METZ","MOSELLE","GRAND EST","Point",0.0,0.0]
["SSP001131201","26.0053","DROMENSEIGNE",null,"En cours",null,null,"En cours","26362","VALENCE","DROME","AUVERGNE-RHONE-ALPES","Point",4.9300046,44.93517,"K35 - Regroupement, reconditionnement de déchets"]
["SSP001131801","57.0211","RECORD (Hypermarché)",null,"En cours",null,null,"En cours","57606","SAINT AVOLD","MOSELLE","GRAND EST","Point",6.7206726,49.1093]
["SSP001131901","57.0212","Ancien gazomètre de Marienau - confinement des matières épurantes",null,"En cours",null,null,"En cours","57484","MORSBACH","MOSELLE","GRAND EST","Point",6.864582,49.173405]
["SSP001132301","69.0273","SOTRA SEPEREF",null,"En cours",null,null,"En cours","69163","QUINCIEUX","RHONE","AUVERGNE-RHONE-ALPES","Point",4.7829823,45.903294]
["SSP001133101","01.0091","TOTAL (Relais Elf Bd Ch de Gaulle, Bourg en Bresse)",null,"En cours",null,null,"En cours","01053","BOURG EN BRESSE","AIN","AUVERGNE-RHONE-ALPES","Point",5.241208,46.2013,"L23 - Détail de carburants"]
["SSP001133601","57.0215","PROFILEST",null,"En cours",null,null,"En cours","57529","OTTANGE","MOSELLE","GRAND EST","Point",6.2136006,49.142315]
["SSP001133701","57.0216","EUROMOSELLE- HAUCONCOURT",null,"En cours",null,null,"En cours","57303","HAUCONCOURT","MOSELLE","GRAND EST","Point",6.1527333,49.20585]
["SSP001134601","54.0131","SAS ADG BETON INDUSTRIEL","Cessation d'activités 2013.","En cours",null,null,"En cours","54339","MALZEVILLE","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",6.1945424,48.722008,"G23 - Centrales à béton"]
["SSP001134901","38.0183","Total Roussillon Station Service",null,"En cours",null,null,"En cours","38344","ROUSSILLON","ISERE","AUVERGNE-RHONE-ALPES","Point",4.8008947,45.369194,"L23 - Détail de carburants"]
["SSP001135101","38.0185","Rhod Peintures",null,"En cours",null,null,"En cours","38344","ROUSSILLON","ISERE","AUVERGNE-RHONE-ALPES","Point",4.8097396,45.38775]
["SSP001135401","67.0168","GAGGENAU Industrie",null,"En cours",null,null,"En cours","67268","LIPSHEIM","BAS-RHIN","GRAND EST","Point",7.672457,48.492584,"H1 - Mécanique, électrique, traitement de surface"]
["SSP001136001","38.0193","CONSTELLIUM PECHINEY  (ex ALCAN) Centre de Recherche de Voreppe (CRV)",null,"En cours",null,null,"En cours","38565","VOREPPE","ISERE","AUVERGNE-RHONE-ALPES","Point",5.6088862,45.312424,"J32 - Métallurgie de l'aluminium"]
["SSP001136401","38.0196","AUREUS",null,"En cours",null,null,"En cours","38184","GRENAY","ISERE","AUVERGNE-RHONE-ALPES","Point",5.078217,45.662186]
["SSP001137101","07.0019","Centre Hospitalier des Vals d'Ardèche",null,"En cours",null,null,"En cours","07349","LA VOULTE SUR RHONE","ARDECHE","AUVERGNE-RHONE-ALPES","Point",4.781511,44.806442,"M3 - Santé"]
["SSP001137401","69.0297","Beton Lyonnais",null,"En cours",null,null,"En cours","69275","DECINES CHARPIEU","RHONE","AUVERGNE-RHONE-ALPES","Point",4.954575,45.779114,"G23 - Centrales à béton"]
["SSP001137601","01.0096","AMF QSE (ex LCM)",null,"En cours",null,null,"En cours","01386","SAINT SORLIN EN BUGEY","AIN","AUVERGNE-RHONE-ALPES","Point",5.3611555,45.88892,"L1 - Entreposage, manutention, commerces"]
["SSP001138401","59.0569","AGC (ex Glaverbel Boussois)",null,"En cours",null,null,"En cours","59104","BOUSSOIS","NORD","HAUTS-DE-FRANCE","Point",4.033839,50.288036,"G15 - Industrie du verre"]
["SSP001138601","972.0008","Station-service TOTAL - Montgérald",null,"En cours",null,null,"En cours","97209","FORT-DE-FRANCE","MARTINIQUE","MARTINIQUE","Point",-61.04915,14.616257,"L23 - Détail de carburants"]
["SSP001138901","26.0059","Kalistrut Aerospace France",null,"En cours",null,null,"En cours","26333","SAINT VALLIER","DROME","AUVERGNE-RHONE-ALPES","Point",4.817755,45.166367,"H13 - Traitement de surface"]
["SSP001139401","69.0277","SAPRR",null,"En cours",null,null,"En cours","69242","TAPONAS","RHONE","AUVERGNE-RHONE-ALPES","Point",4.764953,46.13641]
["SSP001139801","61.0053","LUREM Machines à Bois",null,"En cours",null,null,"En cours","61145","DOMFRONT","ORNE","NORMANDIE","Point",-0.6501334,48.584995,"H - Mécanique, traitements des surfaces"]
["SSP001140301","38.0205","Groupe Bernard",null,"En cours",null,null,"En cours","38185","GRENOBLE","ISERE","AUVERGNE-RHONE-ALPES","Point",5.717712,45.197483,"L21 - Vente et réparation automobile"]
["SSP001140701","38.0211","Station BP Bir Hakeim",null,"En cours",null,null,"En cours","38185","GRENOBLE","ISERE","AUVERGNE-RHONE-ALPES","Point",5.735515,45.18867,"L23 - Détail de carburants"]
["SSP001140901","38.0212","ECTRA",null,"Clôturée",null,null,"Clôturée","38421","SAINT MARTIN D'HERES","ISERE","AUVERGNE-RHONE-ALPES","Polygone",5.754916,45.18425,null,null,null,"52.10B - Entreposage et stockage non frigorifique"]
["SSP001141401","76.0382","Pipe L12",null,"En cours",null,null,"En cours","76322","LE GRAND QUEVILLY","SEINE-MARITIME","NORMANDIE","Point",1.0160477,49.403328]
["SSP001141701","69.0282","DIVERSEY",null,"En cours",null,null,"En cours","69013","ARNAS","RHONE","AUVERGNE-RHONE-ALPES","Point",4.7251606,46.001095,"D62 - Fabrication de détergents"]
["SSP001142001","59.0574","TATA STEEL (ex Myriad, ex FFM)",null,"En cours",null,null,"En cours","59392","MAUBEUGE","NORD","HAUTS-DE-FRANCE","Point",3.9536464,50.266613,"J5 - Fonderie et travail des métaux"]
["SSP001142501","26.0063","NOVEX",null,"En cours",null,null,"En cours","26333","SAINT VALLIER","DROME","AUVERGNE-RHONE-ALPES","Point",4.8199105,45.17117,"G12 - Fabrication de produits céramiques"]
["SSP001142901","74.0054","Décharge de la Frasse",null,"En cours",null,null,"En cours","74208","PASSY","HAUTE-SAVOIE","AUVERGNE-RHONE-ALPES","Point",6.7310815,45.930595,"K21 - Décharges d'ordures ménagères"]
["SSP001143401","69.0284","ONTEX",null,"Clôturée",null,"2012-04-11","Clôturée","69013","ARNAS","RHONE","AUVERGNE-RHONE-ALPES","Point",4.730652,46.000626,"M - Divers et services"]
["SSP001143701","26.0064","Sté PETROLE SHELL (ex TOTAL RAFFINAGE MARKETING)",null,"En cours",null,null,"En cours","26005","ALLAN","DROME","AUVERGNE-RHONE-ALPES","Point",4.7799425,44.514885]
["SSP001143901","26.0065","SODIPLEC (exTOTAL RAFFINAGE MARKETING)",null,"En cours",null,null,"En cours","26325","SAINT RAMBERT D'ALBON","DROME","AUVERGNE-RHONE-ALPES","Point",4.8251443,45.27794,"D12 - Raffinage de pétrole, carburants et lubrifiants"]
["SSP001144401","73.0123","FOSECO",null,"En cours",null,null,"En cours","73065","CHAMBERY","SAVOIE","AUVERGNE-RHONE-ALPES","Point",5.908531,45.574997]
["SSP001144601","73.0124","ACIAL (ex. DUWIK)",null,"En cours",null,null,"En cours","73010","ALBENS","SAVOIE","AUVERGNE-RHONE-ALPES","Point",5.954694,45.783867]
["SSP001144901","972.0013","Station-service ESSO - Bas du Fort",null,"En cours",null,null,"En cours","97203","BASSE-POINTE","MARTINIQUE","MARTINIQUE","Point",-61.11942,14.868619,"L23 - Détail de carburants"]
["SSP001145401","972.0016","Station-service ESSO - Marin Bourg",null,"En cours",null,null,"En cours","97217","LE MARIN","MARTINIQUE","MARTINIQUE","Point",-60.87542,14.473386,"L23 - Détail de carburants"]
["SSP001145801","73.0127","Station ELAN (Mairie de la Valloire)",null,"En cours",null,null,"En cours","73306","VALLOIRE","SAVOIE","AUVERGNE-RHONE-ALPES","Point",6.4322467,45.1653,"L23 - Détail de carburants"]
["SSP001146301","74.0069","BOUVERAT INDUSTRIES  '' Site des Perrières ''",null,"Clôturée",null,null,"Clôturée","74169","MARNAZ","HAUTE-SAVOIE","AUVERGNE-RHONE-ALPES","Point",6.5296454,46.062817,"H11 - Usinage"]
["SSP001146701","74.0073","FAVRAT Paul SARL",null,"En cours",null,null,"En cours","74281","THONON LES BAINS","HAUTE-SAVOIE","AUVERGNE-RHONE-ALPES","Point",6.50897,46.39591,"C13 - Traitement du bois"]
["SSP001146901","972.0017","Station-service ESSO - Saint-Esprit",null,"En cours",null,null,"En cours","97223","SAINT-ESPRIT","MARTINIQUE","MARTINIQUE","Point",0.0,0.0,"L23 - Détail de carburants"]
["SSP001147201","74.0080","ANPER-RBDH",null,"En cours",null,null,"En cours","74169","MARNAZ","HAUTE-SAVOIE","AUVERGNE-RHONE-ALPES","Point",6.5242224,46.063255,"H11 - Usinage"]
["SSP001147901","60.0120","CONSTANT",null,"En cours",null,null,"En cours","60103","BRESLES","OISE","HAUTS-DE-FRANCE","Point",2.2502117,49.414547]
["SSP001148001","33.0340","EDITRANS Bassens",null,"En cours",null,null,"En cours","33032","BASSENS","GIRONDE","NOUVELLE-AQUITAINE","Point",-0.53847665,44.921703]
["SSP001148601","69.0289","Le Progrès",null,"Clôturée",null,"2005-03-01","Clôturée","69271","CHASSIEU","RHONE","AUVERGNE-RHONE-ALPES","Point",4.962797,45.725376]
["SSP001149101","38.0232","SICTOM des Terres Froides (zone ISDND/CET2)",null,"En cours",null,null,"En cours","38065","CHABONS","ISERE","AUVERGNE-RHONE-ALPES","Point",5.404353,45.428032,"K21 - Décharges d'ordures ménagères"]
["SSP001149501","68.0155","COCKROURI",null,"En cours",null,null,"En cours","68224","MULHOUSE","HAUT-RHIN","GRAND EST","Point",7.328923,47.73698]
["SSP001149601","26.0066","GERFLOR PROVENCE",null,"En cours",null,null,"En cours","26324","SAINT PAUL TROIS CHATEAUX","DROME","AUVERGNE-RHONE-ALPES","Point",4.741213,44.349854]
["SSP001150101","01.0105","DECHARGE de Neuville-les-Dames",null,"En cours",null,null,"En cours","01272","NEUVILLE LES DAMES","AIN","AUVERGNE-RHONE-ALPES","Point",4.9944386,46.14835,"K21 - Décharges d'ordures ménagères"]
["SSP001150401","01.0111","EMERY & Cie",null,"En cours",null,null,"En cours","01071","CESSY","AIN","AUVERGNE-RHONE-ALPES","Point",6.067258,46.32363,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP001151001","26.0067","CHARVET LA MURE BIANCO",null,"En cours",null,null,"En cours","26281","ROMANS SUR ISERE","DROME","AUVERGNE-RHONE-ALPES","Point",5.084314,45.053062,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP001151101","74.0088","PRECITURN (ex DEPOISIER-GERVEX)",null,"En cours",null,null,"En cours","74169","MARNAZ","HAUTE-SAVOIE","AUVERGNE-RHONE-ALPES","Point",6.51789,46.065273,"H11 - Usinage"]
["SSP001151801","38.0239","NORMABARRE - Usine SM2 (GROUPE SCHNEIDER ELECTRIC)",null,"En cours",null,null,"En cours","38416","SAINT MARCELLIN","ISERE","AUVERGNE-RHONE-ALPES","Point",5.312364,45.150307,"H1 - Mécanique, électrique, traitement de surface"]
["SSP001152201","74.0091","Savoies Enrobés",null,"En cours",null,null,"En cours","74019","ARGONAY","HAUTE-SAVOIE","AUVERGNE-RHONE-ALPES","Point",6.1655326,45.956047]
["SSP001152601","26.0068","THEVENIN DUCROT DISTRIBUTION - Ancien dépôt pétrolier AVIA",null,"Clôturée",null,"2006-01-05","Clôturée","26281","ROMANS SUR ISERE","DROME","AUVERGNE-RHONE-ALPES","Point",5.0752397,45.04857,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP001152701","67.0169","station-service CORA",null,"En cours",null,null,"En cours","67309","MUNDOLSHEIM","BAS-RHIN","GRAND EST","Point",7.724194,48.655193]
["SSP001153401","38.0242","SEMITAG",null,"En cours",null,null,"En cours","38474","SASSENAGE","ISERE","AUVERGNE-RHONE-ALPES","Point",5.67969,45.207882,"L - Entreposage, transport, commerce"]
["SSP001153701","38.0244","VIAL (station-service TOTAL FINA ELF)",null,"En cours",null,null,"En cours","38401","SAINT JEAN DE SOUDAIN","ISERE","AUVERGNE-RHONE-ALPES","Point",5.421636,45.567776,"L23 - Détail de carburants"]
["SSP001154601","64.0119","Station service LECLERC MILABIA (ex MIDIS)",null,"En cours",null,null,"En cours","64122","BIARRITZ","PYRENEES-ATLANTIQUES","NOUVELLE-AQUITAINE","Point",-1.558842,43.48218]
["SSP001154701","38.0249","Station Service TOTAL",null,"Clôturée",null,"2017-07-11","Clôturée","38544","VIENNE","ISERE","AUVERGNE-RHONE-ALPES","Point",4.8944836,45.527275,"L23 - Détail de carburants"]
["SSP001155201","74.0099","SICN",null,"En cours",null,null,"En cours","74010","ANNECY","HAUTE-SAVOIE","AUVERGNE-RHONE-ALPES","Point",6.12895,45.923275]
["SSP001155701","64.0120","AIROX (ex MMS)",null,"En cours",null,null,"En cours","64445","PAU","PYRENEES-ATLANTIQUES","NOUVELLE-AQUITAINE","Point",-0.35130763,43.317627]
["SSP001156101","69.0326","Nexans (ex Cables de Lyon)",null,"En cours",null,null,"En cours","69123","LYON","RHONE","AUVERGNE-RHONE-ALPES","Point",4.838869,45.739994,"H18 - Composants électroniques (fabrication de)"]
["SSP001156201","972.0023","ESSO Marin TigerMarket la Duprey",null,"En cours",null,null,"En cours","97217","LE MARIN","MARTINIQUE","MARTINIQUE","Point",-60.878983,14.472235,"L23 - Détail de carburants"]
["SSP001156901","60.0127","Garage du Calvaire",null,"En cours",null,null,"En cours","60509","PONT SAINTE MAXENCE","OISE","HAUTS-DE-FRANCE","Point",2.6103723,49.30785]
["SSP001157201","25.0054","Bernard Haenni SAS",null,"En cours",null,null,"En cours","25127","CHARQUEMONT","DOUBS","BOURGOGNE-FRANCHE-COMTE","Point",6.8197103,47.215645,"H14 - Application de peinture"]
["SSP001157901","972.0027","MétalCaraïb",null,"En cours",null,null,"En cours","97206","LE DIAMANT","MARTINIQUE","MARTINIQUE","Point",-60.98586,14.494573,"K5 - Récupération, dépôts de ferrailles"]
["SSP001158201","33.0354","Communauté de Communes-Cestas",null,"En cours",null,null,"En cours","33122","CESTAS","GIRONDE","NOUVELLE-AQUITAINE","Point",-0.68479526,44.743145]
["SSP001158801","33.0360","MAIRIE - La Sauve",null,"En cours",null,null,"En cours","33505","LA SAUVE","GIRONDE","NOUVELLE-AQUITAINE","Point",0.709091,7.574304]
["SSP001159601","33.0370","MAIRIE - Lugos",null,"En cours",null,null,"En cours","33260","LUGOS","GIRONDE","NOUVELLE-AQUITAINE","Point",-0.8818296,44.481075]
["SSP001160401","33.0379","SMICVAL",null,"En cours",null,null,"En cours","33374","SAINT AUBIN DE BLAYE","GIRONDE","NOUVELLE-AQUITAINE","Point",-0.5610221,45.267868]
["SSP001160501","76.0292","NOUVELLES SAVONNERIES DE FRANCE",null,"En cours",null,null,"En cours","76750","YAINVILLE","SEINE-MARITIME","NORMANDIE","Point",0.8187778,49.46305]
["SSP001161701","74.0102","DECHAMBOUX (Régénération)",null,"En cours",null,null,"En cours","74224","LA ROCHE SUR FORON","HAUTE-SAVOIE","AUVERGNE-RHONE-ALPES","Point",6.30134,46.069595,"K42 - Régénération de solvants"]
["SSP001162201","73.0134","ENI FRANCE - Station-service du Relais du Val Gelon",null,"En cours",null,null,"En cours","73079","CHATEAUNEUF","SAVOIE","AUVERGNE-RHONE-ALPES","Point",6.1544333,45.54725,"L23 - Détail de carburants"]
["SSP001163401","18.0054","CTSP  -Ancienne décharge Bourges",null,"En cours",null,null,"En cours","18033","BOURGES","CHER","CENTRE-VAL DE LOIRE","Point",2.439447,47.120617,"K21 - Décharges d'ordures ménagères"]
["SSP001163801","64.0122","SOGARA Station service Carrefour Lescar",null,"En cours",null,null,"En cours","64335","LESCAR","PYRENEES-ATLANTIQUES","NOUVELLE-AQUITAINE","Point",-0.42814475,43.315525]
["SSP001164101","73.0138","Décharge de Pussy (CCVA)",null,"En cours",null,null,"En cours","73187","LA LECHERE","SAVOIE","AUVERGNE-RHONE-ALPES","Point",6.46062,45.54307,"K21 - Décharges d'ordures ménagères"]
["SSP001164501","73.0140","Décharge de Terre Neuve (ancienne)",null,"En cours",null,null,"En cours","73124","GILLY SUR ISERE","SAVOIE","AUVERGNE-RHONE-ALPES","Point",6.353994,45.64997,"K21 - Décharges d'ordures ménagères"]
["SSP001165001","38.0255","CFF PURFER (ex PURMET)",null,"En cours",null,null,"En cours","38377","SAINT CLAIR DE LA TOUR","ISERE","AUVERGNE-RHONE-ALPES","Point",5.4656296,45.572926,"K52 - Dépôts de ferraille"]
["SSP001165101","33.0408","SODICAR Station service",null,"En cours",null,null,"En cours","33011","ARES","GIRONDE","NOUVELLE-AQUITAINE","Point",-1.0834441,44.790997,"L23 - Détail de carburants"]
["SSP001165501","45.0054","SERVAIS",null,"En cours",null,null,"En cours","45004","AMILLY","LOIRET","CENTRE-VAL DE LOIRE","Point",2.7841275,47.972565,"D4 - Encres, vernis, peintures, colles (fabrication de)"]
["SSP001166101","28.0067","Expanscience - (ancien site d'exploitation)",null,"En cours",null,null,"En cours","28140","EPERNON","EURE-ET-LOIR","CENTRE-VAL DE LOIRE","Point",1.67714,48.601387,"D63 - Fabrication de produits de parfumerie"]
["SSP001166301","45.0053","Olivet distribution (station service Leclerc)",null,"En cours",null,null,"En cours","45232","OLIVET","LOIRET","CENTRE-VAL DE LOIRE","Point",1.9178323,47.841805,"L23 - Détail de carburants"]
["SSP001166601","33.0409","LACROIX",null,"En cours",null,null,"En cours","33174","FRONSAC","GIRONDE","NOUVELLE-AQUITAINE","Point",-0.26695183,44.934536]
["SSP001167501","33.0420","SIBA - Le Teich",null,"Clôturée",null,"2015-04-27","Clôturée","33527","LE TEICH","GIRONDE","NOUVELLE-AQUITAINE","Point",-0.97527415,44.619976]
["SSP001167901","33.0423","Déposante NAUD Guy",null,"En cours",null,null,"En cours","33514","SOULAC SUR MER","GIRONDE","NOUVELLE-AQUITAINE","Point",-1.1101516,45.507706]
["SSP001168401","76.0303","D2T (ex ETS m ex ESSO S.A.F)",null,"En cours",null,null,"En cours","76451","MONT SAINT AIGNAN","SEINE-MARITIME","NORMANDIE","Point",1.0702432,49.46748,"L2 - Transports, automobile, carburants"]
["SSP001168501","76.0304","MAHIEU Maurice",null,"En cours",null,null,"En cours","76467","NEVILLE","SEINE-MARITIME","NORMANDIE","Point",0.7039712,49.82664]
["SSP001168901","45.0055","BRENNTAG",null,"En cours",null,null,"En cours","45272","SAINT CYR EN VAL","LOIRET","CENTRE-VAL DE LOIRE","Point",1.9521886,47.812843,"L13 - Entrepôts de produits dangereux"]
["SSP001169401","45.0057","LES CHARPENTIERS DE PARIS",null,"En cours",null,null,"En cours","45146","LA FERTE SAINT AUBIN","LOIRET","CENTRE-VAL DE LOIRE","Point",1.9362724,47.712696,"C12 - Produits en bois, ameublement (fabrication de)"]
["SSP001169801","45.0059","SIFA TECHNOLOGIES",null,"En cours",null,null,"En cours","45234","ORLEANS","LOIRET","CENTRE-VAL DE LOIRE","Point",1.9229906,47.868977,"J32 - Métallurgie de l'aluminium"]
["SSP001170301","69.0344","ANOFLEX CONTITECH",null,"En cours",null,null,"En cours","69286","RILLIEUX LA PAPE","RHONE","AUVERGNE-RHONE-ALPES","Point",4.8757534,45.81629,"H - Mécanique, traitements des surfaces"]
["SSP001170801","73.0146","UGITECH - centre de stockage de Montgombert",null,"En cours",null,null,"En cours","73303","UGINE","SAVOIE","AUVERGNE-RHONE-ALPES","Point",6.430956,45.743927,"J22 - Production d'acier brut, aciéries"]
["SSP001171301","69.0347","Eiffage (ex APPIA)",null,"En cours",null,null,"En cours","69123","LYON","RHONE","AUVERGNE-RHONE-ALPES","Point",4.8171964,45.790554,"G22 - Centrales d'enrobés"]
["SSP001171801","64.0124","Station service SOGARA Anglet",null,"En cours",null,null,"En cours","64024","ANGLET","PYRENEES-ATLANTIQUES","NOUVELLE-AQUITAINE","Point",-1.4996618,43.488407]
["SSP001172101","45.0061","JOHN DEERE",null,"En cours",null,null,"En cours","45302","SARAN","LOIRET","CENTRE-VAL DE LOIRE","Point",1.915879,47.952644,"H - Mécanique, traitements des surfaces"]
["SSP001172301","69.0348","KEOLIS à Oullins",null,"En cours",null,null,"En cours","69149","OULLINS","RHONE","AUVERGNE-RHONE-ALPES","Point",4.8079042,45.7183,"L2 - Transports, automobile, carburants"]
["SSP001172801","38.0268","VFT SARL",null,"En cours",null,null,"En cours","38562","VIZILLE","ISERE","AUVERGNE-RHONE-ALPES","Polygone",5.765326,45.074707,"H - Mécanique, traitements des surfaces"]
["SSP001173001","67.0170","relais Total de Keskastel",null,"En cours",null,null,"En cours","67234","KESKASTEL","BAS-RHIN","GRAND EST","Point",7.0466113,48.966682]
["SSP001173301","67.0171","TEREOS SYRAL",null,"En cours",null,null,"En cours","67281","MARCKOLSHEIM","BAS-RHIN","GRAND EST","Point",7.59507,48.168964]
["SSP001173901","74.0111","SPMR",null,"En cours",null,null,"En cours","74243","SAINT JULIEN EN GENEVOIS","HAUTE-SAVOIE","AUVERGNE-RHONE-ALPES","Point",6.090862,46.140556,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP001174401","08.0088","USINE DU PAQUIS",null,"En cours",null,null,"En cours","08328","NOUZONVILLE","ARDENNES","GRAND EST","Point",4.7469916,49.814705,"H - Mécanique, traitements des surfaces"]
["SSP001174901","08.0092","TARKETT FRANCE",null,"En cours",null,null,"En cours","08194","GLAIRE","ARDENNES","GRAND EST","Point",4.916203,49.705048,"D34 - Fabrication de matières plastiques de base"]
["SSP001175301","39.0030","Société Nouvelle REVETIS",null,"En cours",null,null,"En cours","39572","VILLETTE LES ARBOIS","JURA","BOURGOGNE-FRANCHE-COMTE","Point",5.74603,46.92494,"H13 - Traitement de surface"]
["SSP001175501","69.0358","SNCF - Ateliers Matériel Oullins Voitures",null,"En cours",null,"2017-10-27","En cours","69149","OULLINS","RHONE","AUVERGNE-RHONE-ALPES","Point",4.8148956,45.717793,"L22 - Transports"]
["SSP001176001","73.0150","PECHINEY BÂTIMENT - ancienne usine de La Pouille",null,"En cours",null,null,"En cours","73002","AIGUEBELLE","SAVOIE","AUVERGNE-RHONE-ALPES","Point",6.3123274,45.519783]
["SSP001176201","73.0152","Ancienne décharge de Rocher Blanc",null,"En cours",null,null,"En cours","73201","PLANAY","SAVOIE","AUVERGNE-RHONE-ALPES","Point",6.6666083,45.44337]
["SSP001176701","38.0272","CCPBL - Déchèterie des Meunières",null,"Clôturée",null,"2017-07-11","Clôturée","38130","LA COTE SAINT ANDRE","ISERE","AUVERGNE-RHONE-ALPES","Point",5.2507606,45.38844,"K22 - Regroupement d'OM, DIB"]
["SSP001177201","33.0434","SNC ALVEA",null,"Clôturée",null,"2015-04-27","Clôturée","33529","LA TESTE DE BUCH","GIRONDE","NOUVELLE-AQUITAINE","Point",0.02841013,43.238686]
["SSP001177901","37.0051","STATION SERVICE - VAULTIER",null,"En cours",null,null,"En cours","37014","AZAY LE RIDEAU","INDRE-ET-LOIRE","CENTRE-VAL DE LOIRE","Point",0.48934954,47.274246,"L23 - Détail de carburants"]
["SSP001178701","08.0108","UCANEL",null,"En cours",null,null,"En cours","08140","DOM LE MESNIL","ARDENNES","GRAND EST","Point",4.7889304,49.694023,"B12 - Industrie laitière"]
["SSP001179001","45.0063","LEGUAY EMBALLAGES",null,"En cours",null,null,"En cours","45147","FLEURY LES AUBRAIS","LOIRET","CENTRE-VAL DE LOIRE","Point",1.9043411,47.920982]
["SSP001179201","61.0043","SONOFOQUE - Blanchardière (la Banane)",null,"En cours",null,null,"En cours","61169","FLERS","ORNE","NORMANDIE","Point",-0.5600146,48.747868]
["SSP001179601","93.0072","Peugeot Citroën Aulnay",null,"En cours",null,null,"En cours","93005","AULNAY SOUS BOIS","SEINE-SAINT-DENIS","ILE-DE-FRANCE","Point",2.495045,48.965157,"H1 - Mécanique, électrique, traitement de surface"]
["SSP001180401","59.0583","ALURAL",null,"En cours",null,null,"En cours","59550","SALOME","NORD","HAUTS-DE-FRANCE","Point",2.8229332,50.53165]
["SSP001180501","13.0148","QUEYRAS ENVIRONNEMENT",null,"Clôturée",null,null,"Clôturée","13055","MARSEILLE","BOUCHES-DU-RHONE","PROVENCE-ALPES-COTE D'AZUR","Polygone",5.401061,43.279522,"K - Déchets et traitements"]
["SSP001181001","68.0157","STOCKMEIER UERETHANES",null,"En cours",null,null,"En cours","68063","CERNAY","HAUT-RHIN","GRAND EST","Point",7.197728,47.793434]
["SSP001181501","44.0062","LACTALIS La Chevrolière",null,"Clôturée",null,"2012-12-26","Clôturée","44041","LA CHEVROLIERE","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Point",-1.6145867,47.093678]
["SSP001182001","44.0065","TEREOS (ex BEGHIN SAY)",null,"En cours",null,null,"En cours","44109","NANTES","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Point",-1.5563734,47.19994]
["SSP001182401","59.0584","Yves LEMAIRE",null,"En cours",null,null,"En cours","59482","QUESNOY SUR DEULE","NORD","HAUTS-DE-FRANCE","Point",3.0103173,50.714207]
["SSP001182601","44.0070","MHS (ex ATMEL NANTES)",null,"En cours",null,null,"En cours","44109","NANTES","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Point",-1.5207232,47.28593]
["SSP001182901","44.0073","PEBECO (ex FOCAST)",null,"En cours",null,null,"En cours","44058","FERCE","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Point",-1.3466411,47.78883]
["SSP001183601","53.0020","Vishay MCB Industrie SA",null,"En cours",null,null,"En cours","53062","CHATEAU GONTIER","MAYENNE","PAYS DE LA LOIRE","Point",-0.6917382,47.832283,"H18 - Composants électroniques (fabrication de)"]
["SSP001183701","69.0364","IP3 LYON (ex. PROMENS COMPOSANTS)",null,"En cours",null,null,"En cours","69013","ARNAS","RHONE","AUVERGNE-RHONE-ALPES","Point",4.7251697,46.003025]
["SSP001184301","71.0064","ESSEX (NEXANS)",null,"En cours",null,null,"En cours","71270","MACON","SAONE-ET-LOIRE","BOURGOGNE-FRANCHE-COMTE","Point",4.8274703,46.287445,"H1 - Mécanique, électrique, traitement de surface"]
["SSP001184801","71.0067","SNDCE",null,"En cours",null,null,"En cours","71512","SENNECEY LE GRAND","SAONE-ET-LOIRE","BOURGOGNE-FRANCHE-COMTE","Point",4.875645,46.64264,"H13 - Traitement de surface"]
["SSP001185301","972.0040","COLAS",null,"En cours",null,null,"En cours","97209","FORT-DE-FRANCE","MARTINIQUE","MARTINIQUE","Point",-61.048405,14.597806]
["SSP001185401","33.0443","Station-service des Tourterelles - Patrick GOUMETTOU",null,"En cours",null,null,"En cours","33236","LEGE CAP FERRET","GIRONDE","NOUVELLE-AQUITAINE","Point",-1.2419428,44.67449]
["SSP001186001","33.0445","TOTAL - Relais Club",null,"En cours",null,null,"En cours","33249","LORMONT","GIRONDE","NOUVELLE-AQUITAINE","Point",-0.51676,44.865093,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP001186301","44.0084","BOBCAT",null,"En cours",null,null,"En cours","44129","PONTCHATEAU","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Point",-2.067537,47.428307,"G14 - Fabrication d'autres matériaux de construction"]
["SSP001186901","68.0183","Trois Maisons Ouest (dépôt Sud-Est)",null,"En cours",null,null,"En cours","68297","SAINT LOUIS","HAUT-RHIN","GRAND EST","Point",7.5297704,47.622185]
["SSP001187101","33.0446","SAS Financière et Commerciale FIB - BORIFER",null,"En cours",null,null,"En cours","33063","BORDEAUX","GIRONDE","NOUVELLE-AQUITAINE","Point",-0.5585073,44.852757,"H - Mécanique, traitements des surfaces"]
["SSP001187501","33.0447","SA SAGA (SHOPI)",null,"En cours",null,"2015-03-05","En cours","33019","AUDENGE","GIRONDE","NOUVELLE-AQUITAINE","Point",-1.0140072,44.682137]
["SSP001188001","33.0452","BM VO DISTRIBUTION - Station -service AVIA",null,"Clôturée",null,"2015-03-05","Clôturée","33069","LE BOUSCAT","GIRONDE","NOUVELLE-AQUITAINE","Point",-0.6010082,44.861324]
["SSP001188701","93.0078","THOMET",null,"En cours",null,null,"En cours","93006","BAGNOLET","SEINE-SAINT-DENIS","ILE-DE-FRANCE","Polygone",2.415531,48.858406,"H13 - Traitement de surface"]
["SSP001188901","64.0128","Décharge de Jurançon",null,"En cours",null,null,"En cours","64284","JURANCON","PYRENEES-ATLANTIQUES","NOUVELLE-AQUITAINE","Point",0.0,0.0]
["SSP001189601","44.0092","TOTAL RAFFINAGE MARKETING",null,"En cours",null,null,"En cours","44143","REZE","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Point",-1.5708717,47.192432]
["SSP001189901","76.0322","DEMOLITION AUTOMOBILE DU FOUR A CHAUX",null,"En cours",null,null,"En cours","76592","SAINT JEAN DE FOLLEVILLE","SEINE-MARITIME","NORMANDIE","Point",0.5350204,49.387035]
["SSP001190701","972.0043","TOTAL Sainte-Thérèse",null,"En cours",null,null,"En cours","97209","FORT-DE-FRANCE","MARTINIQUE","MARTINIQUE","Point",-61.05286,14.613107,"L23 - Détail de carburants"]
["SSP001190901","72.0031","Commune de la Bruère - dépôt de ferraille",null,"En cours",null,null,"En cours","72049","LA BRUERE SUR LOIR","SARTHE","PAYS DE LA LOIRE","Point",0.37759542,47.654118,"K5 - Récupération, dépôts de ferrailles"]
["SSP001191401","69.0369","KILERDJIAN AUTOMOBILES",null,"En cours",null,null,"En cours","69266","VILLEURBANNE","RHONE","AUVERGNE-RHONE-ALPES","Point",4.8750615,45.76407,"L23 - Détail de carburants"]
["SSP001191901","67.0178","SCHROLL",null,"En cours",null,null,"En cours","67482","STRASBOURG","BAS-RHIN","GRAND EST","Point",7.78495,48.542904]
["SSP001192301","67.0182","TIMMEL FRERES SAS",null,"En cours",null,null,"En cours","67025","BEINHEIM","BAS-RHIN","GRAND EST","Point",8.091961,48.85344]
["SSP001192401","77.0152","WABCO FRANCE SAS","WABCO FRANCE SAS","En cours",null,null,"En cours","77118","CLAYE SOUILLY","SEINE-ET-MARNE","ILE-DE-FRANCE","Polygone",2.6987054,48.945377,"H13 - Traitement de surface"]
["SSP001192801","67.0185","METALIFER",null,"En cours",null,null,"En cours","67482","STRASBOURG","BAS-RHIN","GRAND EST","Point",7.7851257,48.54349]
["SSP001193301","31.0082","Galvanoplastie Industrielle Toulousaine (GIT)",null,"En cours",null,null,"En cours","31157","CUGNAUX","HAUTE-GARONNE","OCCITANIE","Point",1.3695724,43.55461,"H13 - Traitement de surface"]
["SSP001194001","972.0046","Station-service TEXACO Place d'Armes",null,"Clôturée",null,"2014-12-30","Clôturée","97213","LE LAMENTIN","MARTINIQUE","MARTINIQUE","Point",-60.99256,14.620909,"L23 - Détail de carburants"]
["SSP001194201","34.0046","Ancienne école maternelle La Providence",null,"En cours",null,null,"En cours","34172","MONTPELLIER","HERAULT","OCCITANIE","Point",3.872618,43.60419]
["SSP001194601","03.0044","JPM",null,"En cours",null,null,"En cours","03013","AVERMES","ALLIER","AUVERGNE-RHONE-ALPES","Point",3.3208215,46.58123,"H13 - Traitement de surface"]
["SSP001195101","67.0198","SONOCO",null,"En cours",null,null,"En cours","67458","SCHWEIGHOUSE SUR MODER","BAS-RHIN","GRAND EST","Point",7.7371526,48.823326]
["SSP001195501","67.0201","FAURECIA",null,"En cours",null,null,"En cours","67281","MARCKOLSHEIM","BAS-RHIN","GRAND EST","Point",7.5566993,48.156048]
["SSP001195601","67.0202","BARUCH & FISCH (Avenue de la Gare)",null,"En cours",null,null,"En cours","67411","ROSHEIM","BAS-RHIN","GRAND EST","Point",7.4849305,48.500927]
["SSP001196001","67.0207","WIMETAL",null,"En cours",null,null,"En cours","67544","WISSEMBOURG","BAS-RHIN","GRAND EST","Point",7.987904,49.02282]
["SSP001196501","67.0214","SITE ETS JULES VERNE",null,"En cours",null,null,"En cours","67437","SAVERNE","BAS-RHIN","GRAND EST","Point",7.373591,48.736004]
["SSP001197001","76.0326","Fonderie SÉNARD",null,"En cours",null,null,"En cours","76410","MAROMME","SEINE-MARITIME","NORMANDIE","Point",1.0431963,49.47933,"J5 - Fonderie et travail des métaux"]
["SSP001197301","974.0042","ENGEN LAGON",null,"En cours",null,null,"En cours","97415","SAINT-PAUL","LA REUNION","LA REUNION","Point",55.230732,-21.082941,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP001197601","56.0028","Décharge de BRELEAU (aciérie de Ploërmel)",null,"En cours",null,null,"En cours","56165","PLOERMEL","MORBIHAN","BRETAGNE","Point",-2.4050186,47.908997]
["SSP001198101","16.0023","DCNS Equipements Navals",null,"En cours",null,null,"En cours","16291","RUELLE SUR TOUVRE","CHARENTE","NOUVELLE-AQUITAINE","Point",0.22351022,45.67916]
["SSP001198501","28.0071","Philips Automotive Lighting",null,"En cours",null,null,"En cours","28085","CHARTRES","EURE-ET-LOIR","CENTRE-VAL DE LOIRE","Point",1.4782939,48.437447]
["SSP001198601","974.0043","STATION TOTAL SAINT-PIERRE CENTRE",null,"Clôturée",null,"2019-02-04","Clôturée","97416","SAINT-PIERRE","LA REUNION","LA REUNION","Point",55.46908,-21.33588,"L23 - Détail de carburants"]
["SSP001199001","28.0072","EXPANSCIENCE Site 2",null,"En cours",null,null,"En cours","28140","EPERNON","EURE-ET-LOIR","CENTRE-VAL DE LOIRE","Point",1.6849327,48.595715]
["SSP001199501","42.0180","PEYRACHE",null,"En cours",null,null,"En cours","42218","SAINT ETIENNE","LOIRE","AUVERGNE-RHONE-ALPES","Point",4.425122,45.441357,"K - Déchets et traitements"]
["SSP001200001","25.0072","AUTO CASSE 21",null,"En cours",null,null,"En cours","25031","AUDINCOURT","DOUBS","BOURGOGNE-FRANCHE-COMTE","Point",6.835929,47.48816,"K52 - Dépôts de ferraille"]
["SSP001200301","21.0065","PR INDUSTRIE",null,"En cours",null,null,"En cours","21023","ARNAY LE DUC","COTE-D'OR","BOURGOGNE-FRANCHE-COMTE","Point",5.2274203,47.72713]
["SSP001201801","68.0163","La chaussée",null,"En cours",null,null,"En cours","68297","SAINT LOUIS","HAUT-RHIN","GRAND EST","Point",7.538096,47.612988]
["SSP001202301","67.0217","Forage 1318",null,"En cours",null,null,"En cours","67487","SURBOURG","BAS-RHIN","GRAND EST","Point",7.8237762,48.90866,"D11 - Extraction de pétrole et gaz naturel"]
["SSP001202701","67.0220","Forage 4661",null,"En cours",null,null,"En cours","67487","SURBOURG","BAS-RHIN","GRAND EST","Point",7.815317,48.90764,"D11 - Extraction de pétrole et gaz naturel"]
["SSP001202801","68.0168","Grande Sablière de Saint-Louis",null,"En cours",null,null,"En cours","68297","SAINT LOUIS","HAUT-RHIN","GRAND EST","Point",7.5446873,47.597397]
["SSP001203301","25.0079","Scierie FILISETTI",null,"En cours",null,null,"En cours","25173","COUR SAINT MAURICE","DOUBS","BOURGOGNE-FRANCHE-COMTE","Point",6.702234,47.25715,"C11 - Scierie, fabrication de panneaux"]
["SSP001203901","67.0226","Puits 8",null,"En cours",null,null,"En cours","67290","MERKWILLER PECHELBRONN","BAS-RHIN","GRAND EST","Point",7.8301425,48.929367,"K36 - Mise en décharge"]
["SSP001204201","68.0174","LOSGRABEN",null,"En cours",null,null,"En cours","68120","HAGENTHAL LE BAS","HAUT-RHIN","GRAND EST","Point",7.480159,47.530228]
["SSP001204401","67.0227","Forage 459",null,"En cours",null,null,"En cours","67290","MERKWILLER PECHELBRONN","BAS-RHIN","GRAND EST","Point",7.8358827,48.938156,"D11 - Extraction de pétrole et gaz naturel"]
["SSP001204901","67.0229","Puits 7",null,"En cours",null,null,"En cours","67177","GUNSTETT","BAS-RHIN","GRAND EST","Point",7.7883353,48.9186]
["SSP001205401","68.0179","GALGEN (dépôt centre)",null,"En cours",null,null,"En cours","68182","LEYMEN","HAUT-RHIN","GRAND EST","Point",7.4810314,47.503334]
["SSP001205801","68.0186","TOTAL, station des 3 sapins",null,"En cours",null,null,"En cours","68334","THANN","HAUT-RHIN","GRAND EST","Point",7.1076407,47.8084]
["SSP001205901","68.0182","MAISON ROUGE",null,"En cours",null,null,"En cours","68182","LEYMEN","HAUT-RHIN","GRAND EST","Point",7.49049,47.49714]
["SSP001206401","67.0235","Puits 2",null,"En cours",null,null,"En cours","67379","PREUSCHDORF","BAS-RHIN","GRAND EST","Point",7.8128376,48.931343,"K3 - Traitement de déchets industriels"]
["SSP001206901","67.0239","Forage 945",null,"En cours",null,null,"En cours","67254","KUTZENHAUSEN","BAS-RHIN","GRAND EST","Point",7.8389616,48.931713]
["SSP001207201","67.0242","Forage 3068",null,"En cours",null,null,"En cours","67254","KUTZENHAUSEN","BAS-RHIN","GRAND EST","Point",7.860302,48.929905]
["SSP001207401","974.0045","ANCIENNE CARRIERE COCO-FRANCOISE",null,"Clôturée",null,"2019-04-03","Clôturée","97414","SAINT-LOUIS","LA REUNION","LA REUNION","Point",0.0,0.0,"F32 - Carrières"]
["SSP001208101","68.0188","ANC. DECHARGE STEINACKER",null,"En cours",null,null,"En cours","68039","BISEL","HAUT-RHIN","GRAND EST","Point",7.2212896,47.540184]
["SSP001208501","68.0194","SEEBERG",null,"En cours",null,null,"En cours","68210","MITTLACH","HAUT-RHIN","GRAND EST","Point",7.023285,47.99207]
["SSP001209201","70.0026","Ancien parc de l'équipement",null,"En cours",null,null,"En cours","70188","CREVENEY","HAUTE-SAONE","BOURGOGNE-FRANCHE-COMTE","Point",6.287945,47.68212,"G22 - Centrales d'enrobés"]
["SSP001209801","33.0460","ARIANE GROUP ex HERAKLES",null,"En cours",null,null,"En cours","33417","SAINTE HELENE","GIRONDE","NOUVELLE-AQUITAINE","Polygone",-0.8500751,44.995438,"D - Chimie, parachimie, pétrole"]
["SSP001210901","91.0120","AIR FRANCE",null,"En cours",null,null,"En cours","91479","PARAY VIEILLE POSTE","ESSONNE","ILE-DE-FRANCE","Point",2.367094,48.74347,"L22 - Transports"]
["SSP001211401","68.0217","HOLCIM Granulats (Zone C)",null,"En cours",null,null,"En cours","68278","RIXHEIM","HAUT-RHIN","GRAND EST","Point",7.3961387,47.75608,"F - Industries extractives"]
["SSP001211701","67.0245","ISTRA",null,"En cours",null,null,"En cours","67447","SCHILTIGHEIM","BAS-RHIN","GRAND EST","Point",7.731655,48.611275,"H21 - Imprimerie, presse, édition"]
["SSP001212001","28.0082","CHAFFOTEAUX (ARISTON)",null,"En cours",null,null,"En cours","28218","LUCE","EURE-ET-LOIR","CENTRE-VAL DE LOIRE","Point",1.447793,48.426403,"M1 - Industries diverses"]
["SSP001212801","53.0035","POINT P TROUILLARD",null,"En cours",null,null,"En cours","53014","AZE","MAYENNE","PAYS DE LA LOIRE","Point",-0.690597,47.831264]
["SSP001213101","45.0075","LA GRANDE PAROISSE",null,"En cours",null,null,"En cours","45147","FLEURY LES AUBRAIS","LOIRET","CENTRE-VAL DE LOIRE","Point",1.8968636,47.93194]
["SSP001213701","45.0080","SCI BANNIER (ex FONDERIE DE L'ORLEANAIS)",null,"En cours",null,null,"En cours","45147","FLEURY LES AUBRAIS","LOIRET","CENTRE-VAL DE LOIRE","Point",1.9009156,47.922535]
["SSP001214101","49.0023","ERNAULT TOYODA",null,"En cours",null,null,"En cours","49099","CHOLET","MAINE-ET-LOIRE","PAYS DE LA LOIRE","Point",-0.8581717,47.059044]
["SSP001214701","08.0113","KME Crassier NORD",null,"En cours",null,null,"En cours","08183","FROMELENNES","ARDENNES","GRAND EST","Point",0.0,0.0,"J5 - Fonderie et travail des métaux"]
["SSP001215101","31.0083","CERTAS ENERGY FRANCE SAS",null,"En cours",null,null,"En cours","31433","PORTET SUR GARONNE","HAUTE-GARONNE","OCCITANIE","Point",1.4160582,43.543034,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP001215601","13.0150","Station INTERMARCHE St-Loup",null,"En cours",null,null,"En cours","13055","MARSEILLE","BOUCHES-DU-RHONE","PROVENCE-ALPES-COTE D'AZUR","Point",5.43488,43.283962,"L23 - Détail de carburants"]
["SSP001215701","45.0090","Etablissements ROBROLLE RECYCLAGE ENVIRONNEMENT (PARTIE OUEST)",null,"En cours",null,null,"En cours","45169","INGRE","LOIRET","CENTRE-VAL DE LOIRE","Point",16.096937,51.138268,"K5 - Récupération, dépôts de ferrailles"]
["SSP001216301","31.0084","RENAULT RETAIL GROUP SA",null,"En cours",null,null,"En cours","31555","TOULOUSE","HAUTE-GARONNE","OCCITANIE","Point",1.4979376,43.571594,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP001217101","42.0190","STRONGLIGHT SA",null,"En cours",null,null,"En cours","42218","SAINT ETIENNE","LOIRE","AUVERGNE-RHONE-ALPES","Point",4.4065633,45.44456]
["SSP001217501","44.0113","OLMIX",null,"En cours",null,null,"En cours","44024","BRAINS","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Point",-1.7121003,47.159187]
["SSP001218001","18.0059","BBES ancienne chaufferie urbaine",null,"En cours",null,null,"En cours","18033","BOURGES","CHER","CENTRE-VAL DE LOIRE","Point",2.4045458,47.11109,"I21 - Chaufferies urbaines"]
["SSP001218701","31.0092","Ecoles maternelle et élémentaire Notre Dame (N° 0311479P_P et 0311479P)",null,"En cours",null,null,"En cours","31555","TOULOUSE","HAUTE-GARONNE","OCCITANIE","Point",1.4479188,43.590923]
["SSP001219801","78.0118","CARREFOUR STATION-SERVICE",null,"En cours",null,null,"En cours","78586","SARTROUVILLE","YVELINES","ILE-DE-FRANCE","Point",2.1972356,48.94577,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP001220501","44.0116","LEROUX ET LOTZ",null,"En cours",null,null,"En cours","44109","NANTES","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Point",-1.5960121,47.19635,"D21 - Stockage et conditionnement des gaz et liquéfiés"]
["SSP001220601","28.0084","TSO - société traitements de surface de l'Ouest",null,"En cours",null,null,"En cours","28394","TREON","EURE-ET-LOIR","CENTRE-VAL DE LOIRE","Point",1.329937,48.677834,"H13 - Traitement de surface"]
["SSP001221301","28.0086","Foga",null,"En cours",null,null,"En cours","28168","GALLARDON","EURE-ET-LOIR","CENTRE-VAL DE LOIRE","Point",1.6973609,48.529545,"H - Mécanique, traitements des surfaces"]
["SSP001221801","45.0094","FAURECIA",null,"En cours",null,null,"En cours","45028","BEAUGENCY","LOIRET","CENTRE-VAL DE LOIRE","Point",1.6423516,47.790024,"H15 - Assemblage, montage"]
["SSP001222001","73.0160","ancienne station service AS24",null,"En cours",null,null,"En cours","73011","ALBERTVILLE","SAVOIE","AUVERGNE-RHONE-ALPES","Point",6.3876877,45.660652]
["SSP001222301","75.0025","REDELE RDL&Cie",null,"En cours",null,null,"En cours","75056","PARIS","PARIS","ILE-DE-FRANCE","Polygone",2.2877982,48.8838,"L23 - Détail de carburants"]
["SSP001222801","53.0038","RIVAIN",null,"Clôturée",null,null,"Clôturée","53062","CHATEAU GONTIER","MAYENNE","PAYS DE LA LOIRE","Point",-0.7133395,47.825455,"D62 - Fabrication de détergents"]
["SSP001223401","72.0035","RENOV'AUTO",null,"En cours",null,null,"En cours","72286","SAINT GERVAIS DE VIC","SARTHE","PAYS DE LA LOIRE","Point",0.74225056,47.881664]
["SSP001223901","94.0095","TOTAL - RELAIS DE LA MONTAGNE",null,"En cours",null,null,"En cours","94044","LIMEIL BREVANNES","VAL-DE-MARNE","ILE-DE-FRANCE","Point",2.5136049,48.741856,"L23 - Détail de carburants"]
["SSP001224201","28.0090","GRT gaz",null,"En cours",null,null,"En cours","28324","SAINT ARNOULT DES BOIS","EURE-ET-LOIR","CENTRE-VAL DE LOIRE","Point",1.23571,48.509075,"D2 - Industrie des gaz"]
["SSP001224501","72.0042","LEROY SOMER",null,"En cours",null,null,"En cours","72003","ALLONNES","SARTHE","PAYS DE LA LOIRE","Point",0.16122206,47.94649,"H1 - Mécanique, électrique, traitement de surface"]
["SSP001225501","38.0284","SCHNEIDER ELECTRIC USINE J",null,"En cours",null,null,"En cours","38185","GRENOBLE","ISERE","AUVERGNE-RHONE-ALPES","Point",5.698171,45.207634,"H18 - Composants électroniques (fabrication de)"]
["SSP001225801","16.0026","CORMENIER",null,"En cours",null,null,"En cours","16308","SAINT CLAUD","CHARENTE","NOUVELLE-AQUITAINE","Point",0.4602003,45.899952,"C13 - Traitement du bois"]
["SSP001226201","01.0123","OROSOLV (ex WOLFF)",null,"En cours",null,null,"En cours","01031","BELLIGNAT","AIN","AUVERGNE-RHONE-ALPES","Point",5.6345186,46.243523]
["SSP001226601","44.0122","NANTAISE DE GALVANISATION SOCIETE (SNG)",null,"En cours",null,null,"En cours","44026","CARQUEFOU","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Point",-1.5056388,47.26126,"H13 - Traitement de surface"]
["SSP001227401","31.0094","Airbus Opérations SAS site Louis Bréguet",null,"En cours",null,null,"En cours","31149","COLOMIERS","HAUTE-GARONNE","OCCITANIE","Point",1.3529215,43.614426,"H15 - Assemblage, montage"]
["SSP001227901","16.0032","SVDM - Rouzèdes - CET",null,"En cours",null,null,"En cours","16290","ROUZEDE","CHARENTE","NOUVELLE-AQUITAINE","Point",0.5812076,45.7231,"K21 - Décharges d'ordures ménagères"]
["SSP001228201","31.0096","Société CAMELEON PICTO SUD",null,"En cours",null,null,"En cours","31555","TOULOUSE","HAUTE-GARONNE","OCCITANIE","Polygone",1.4337733,43.62214,"H2 - Imprimerie, presse-édition, photographie"]
["SSP001228401","67.0249","GO'TRANS KREYDER",null,"En cours",null,null,"En cours","67010","ANDLAU","BAS-RHIN","GRAND EST","Point",7.4322767,48.38666,"D21 - Stockage et conditionnement des gaz et liquéfiés"]
["SSP001229401","76.0335","Rousseau",null,"En cours",null,null,"En cours","76482","OFFRANVILLE","SEINE-MARITIME","NORMANDIE","Point",1.0490968,49.865013,"M1 - Industries diverses"]
["SSP001229601","67.0253","OIL FRANCE",null,"En cours",null,null,"En cours","67462","SELESTAT","BAS-RHIN","GRAND EST","Point",7.456151,48.267464]
["SSP001229901","63.0043","YVAN BEAL - ISEKI",null,"En cours",null,null,"En cours","63113","CLERMONT FERRAND","PUY-DE-DOME","AUVERGNE-RHONE-ALPES","Point",3.1237185,45.781197]
["SSP001230601","31.0095","FONDERIES DECHAUMONT",null,"En cours",null,null,"En cours","31395","MURET","HAUTE-GARONNE","OCCITANIE","Point",1.3397199,43.485092,"J5 - Fonderie et travail des métaux"]
["SSP001231001","76.0337","Maillard Roues Elastomères (MRE)",null,"En cours",null,null,"En cours","76462","NEUFCHATEL EN BRAY","SEINE-MARITIME","NORMANDIE","Point",1.4343246,49.732067]
["SSP001231601","40.0141","SINIAT SA (anc. LAFARGE PLATRES)",null,"En cours",null,null,"En cours","40233","POUILLON","LANDES","NOUVELLE-AQUITAINE","Polygone",-1.0194323,43.642437,null,"15.05 - Fabrication de plâtres et de produits en plâtre"]
["SSP001232101","27.0106","EQIOM-SAPPHIRE",null,"En cours",null,null,"En cours","27537","SAINT ETIENNE DU VAUVRAY","EURE","NORMANDIE","Point",1.225393,49.238953,"K35 - Regroupement, reconditionnement de déchets"]
["SSP001232701","76.0342","ORIL Industrie",null,"En cours",null,null,"En cours","76114","BOLBEC","SEINE-MARITIME","NORMANDIE","Point",0.48705128,49.575745,"J - Sidérurgie, métallurgie, coke"]
["SSP001233401","69.0376","CRISCA-ex-SIRM",null,"En cours",null,null,"En cours","69123","LYON","RHONE","AUVERGNE-RHONE-ALPES","Point",4.841136,45.7196]
["SSP001233801","38.0285","FOURNETON",null,"En cours",null,null,"En cours","38239","MOIRANS","ISERE","AUVERGNE-RHONE-ALPES","Point",5.582476,45.32609,"K52 - Dépôts de ferraille"]
["SSP001234101","38.0287","ASCO INDUSTRIES - Lot 4",null,"En cours",null,null,"En cours","38100","LE CHEYLAS","ISERE","AUVERGNE-RHONE-ALPES","Point",5.9999275,45.38109,"J22 - Production d'acier brut, aciéries"]
["SSP001234701","18.0063","CALDEO EX MERCIER STATION SERVICE ELAN",null,"En cours",null,null,"En cours","18011","ARGENT SUR SAULDRE","CHER","CENTRE-VAL DE LOIRE","Point",2.4497159,47.553967,"L23 - Détail de carburants"]
["SSP001235201","34.0049","MIALANES",null,"En cours",null,null,"En cours","34123","JUVIGNAC","HERAULT","OCCITANIE","Point",3.7981439,43.618053]
["SSP001235701","61.0050","SUEZ-RV Grand-Ouest Métaux",null,"En cours",null,null,"En cours","61294","MORTREE","ORNE","NORMANDIE","Point",0.09753202,48.641712,"K52 - Dépôts de ferraille"]
["SSP001236001","61.0049","STYL'FER",null,"En cours",null,null,"En cours","61163","LA FERRIERE AUX ETANGS","ORNE","NORMANDIE","Point",-0.5097769,48.65898,"H13 - Traitement de surface"]
["SSP001236201","45.0109","Garage de l'Ouanne",null,"En cours",null,null,"En cours","45329","TRIGUERES","LOIRET","CENTRE-VAL DE LOIRE","Point",2.9871156,47.93961]
["SSP001236801","38.0292","PURFER (filiale du groupe DERICHEBOURG)",null,"En cours",null,null,"En cours","38185","GRENOBLE","ISERE","AUVERGNE-RHONE-ALPES","Point",5.727803,45.17296]
["SSP001237201","45.0111","ROBROLLE RECYCLAGE ENVIRONNEMENT ( PARTIE EST )",null,"En cours",null,null,"En cours","45169","INGRE","LOIRET","CENTRE-VAL DE LOIRE","Point",16.096937,51.138268,"K5 - Récupération, dépôts de ferrailles"]
["SSP001237301","79.0030","TGVD",null,"En cours",null,null,"En cours","79062","CERIZAY","DEUX-SEVRES","NOUVELLE-AQUITAINE","Point",-0.6968073,46.820087]
["SSP001238001","45.0122","Pithiviers Distribution ( ex station service leclerc )",null,"En cours",null,null,"En cours","45252","PITHIVIERS","LOIRET","CENTRE-VAL DE LOIRE","Point",0.0,0.0]
["SSP001238801","64.0135","TEPF puits Lacq LA23-90-404 manifold M5",null,"En cours",null,null,"En cours","64300","LACQ","PYRENEES-ATLANTIQUES","NOUVELLE-AQUITAINE","Point",-0.6243844,43.406773]
["SSP001239301","64.0138","TEPF manifold MC20 (connecté au puits d'Andoins 2 ADS2D-G3)",null,"En cours",null,null,"En cours","64419","NOUSTY","PYRENEES-ATLANTIQUES","NOUVELLE-AQUITAINE","Point",-0.2167112,43.280148]
["SSP001239901","19.0029","FRANCE JOUETS",null,"En cours",null,null,"En cours","19061","CORNIL","CORREZE","NOUVELLE-AQUITAINE","Point",1.6961167,45.215134,"D34 - Fabrication de matières plastiques de base"]
["SSP001240601","49.0053","ALTIA ex PMP (Précision Mécano-plastique)",null,"En cours",null,null,"En cours","49129","ECOUFLANT","MAINE-ET-LOIRE","PAYS DE LA LOIRE","Point",-0.5100487,47.50373,"D34 - Fabrication de matières plastiques de base"]
["SSP001240901","94.0106","TOTAL – RELAIS DU KREMLIN-BICETRE",null,"En cours",null,null,"En cours","94043","LE KREMLIN BICETRE","VAL-DE-MARNE","ILE-DE-FRANCE","Point",2.34885,48.80618,"L2 - Transports, automobile, carburants"]
["SSP001241801","38.0293","SCIERIE REY",null,"En cours",null,null,"En cours","38446","SAINT PIERRE D'ENTREMONT","ISERE","AUVERGNE-RHONE-ALPES","Point",5.8574543,45.407024,null,"48.01 - Scierie"]
["SSP001241901","45.0143","PRODEX (ex HACQUIN)",null,"En cours",null,null,"En cours","45282","SAINT HILAIRE SAINT MESMIN","LOIRET","CENTRE-VAL DE LOIRE","Point",1.8273396,47.863228,"H13 - Traitement de surface"]
["SSP001242701","64.0153","TEPF puits Lacq 71 - LA071",null,"En cours",null,null,"En cours","64300","LACQ","PYRENEES-ATLANTIQUES","NOUVELLE-AQUITAINE","Point",-0.6245613,43.404877]
["SSP001243301","64.0157","TEPF Puits Lacq 70 - LA070",null,"En cours",null,null,"En cours","64396","MONT","PYRENEES-ATLANTIQUES","NOUVELLE-AQUITAINE","Point",-0.6499514,43.41627]
["SSP001243601","64.0160","TEPF puits Lacq 73 - LA073",null,"En cours",null,null,"En cours","64300","LACQ","PYRENEES-ATLANTIQUES","NOUVELLE-AQUITAINE","Point",-0.62215173,43.409767]
["SSP001244001","40.0145","PERRON Aimé (station-service MARMELLO)",null,"En cours",null,null,"En cours","40001","AIRE SUR L'ADOUR","LANDES","NOUVELLE-AQUITAINE","Point",-0.27301693,43.6912]
["SSP001244601","38.0295","CARROSSERIE ALBERT",null,"En cours",null,null,"En cours","38185","GRENOBLE","ISERE","AUVERGNE-RHONE-ALPES","Point",5.721804,45.18472]
["SSP001244901","76.0349","LEGRAND NORMANDIE","Cessation d'activités","Clôturée","2013-10-30","2020-11-03","Clôturée","76452","MONTVILLE","SEINE-MARITIME","NORMANDIE","Polygone",1.0690696,49.545246]
["SSP001245901","17.0046","Coop Atlantique (super U) - station service",null,"En cours",null,null,"En cours","17397","SAINT SAVINIEN","CHARENTE-MARITIME","NOUVELLE-AQUITAINE","Point",-0.67364615,45.872936,"L23 - Détail de carburants"]
["SSP001246001","33.0472","SMAC",null,"En cours",null,null,"En cours","33063","BORDEAUX","GIRONDE","NOUVELLE-AQUITAINE","Point",-0.565558,44.86522]
["SSP001246401","38.0298","GME - Grenobloise des Matériaux Enrobés",null,"En cours",null,null,"En cours","38565","VOREPPE","ISERE","AUVERGNE-RHONE-ALPES","Point",5.6264744,45.29468]
["SSP001247601","69.0381","Renault Trucks Usine Pont et Essieux - ex Arvin Meritor",null,"En cours",null,null,"En cours","69290","SAINT PRIEST","RHONE","AUVERGNE-RHONE-ALPES","Point",4.9107924,45.69685,"H11 - Usinage"]
["SSP001248201","38.0299","PICHON",null,"En cours",null,null,"En cours","38034","BEAUREPAIRE","ISERE","AUVERGNE-RHONE-ALPES","Point",5.057083,45.3303,"J53 - Travail des métaux, chaudronnerie, poudres"]
["SSP001248401","26.0088","Société Charles JOURDAN International Paris",null,"En cours",null,null,"En cours","26281","ROMANS SUR ISERE","DROME","AUVERGNE-RHONE-ALPES","Point",5.057724,45.0432]
["SSP001249301","74.0127","Wirth et Gruffat",null,"En cours",null,null,"En cours","74019","ARGONAY","HAUTE-SAVOIE","AUVERGNE-RHONE-ALPES","Point",6.1325955,45.938976,"H11 - Usinage"]
["SSP001249701","28.0093","GUERLAIN",null,"En cours",null,null,"En cours","28085","CHARTRES","EURE-ET-LOIR","CENTRE-VAL DE LOIRE","Point",1.5168761,48.432255]
["SSP001250201","44.0139","DIFATLANTIC",null,"En cours",null,null,"En cours","44143","REZE","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Point",38.264816,41.399986,"L2 - Transports, automobile, carburants"]
["SSP001250301","53.0046","TERRENA (ex Coopérative des agriculteurs de la Mayenne (CAM))",null,"En cours",null,null,"En cours","53130","LAVAL","MAYENNE","PAYS DE LA LOIRE","Point",-0.74199444,48.079018,"L23 - Détail de carburants"]
["SSP001251001","33.0473","Station Service BP Fontet",null,"En cours",null,null,"En cours","33170","FONTET","GIRONDE","NOUVELLE-AQUITAINE","Point",-0.030786302,44.561832]
["SSP001252001","33.0475","AFM RECYCLAGE",null,"En cours",null,null,"En cours","33063","BORDEAUX","GIRONDE","NOUVELLE-AQUITAINE","Point",-0.56028455,44.864597,"K35 - Regroupement, reconditionnement de déchets"]
["SSP001252801","61.0072","FOSSE Florian",null,"En cours",null,null,"En cours","61507","VILLIERS SOUS MORTAGNE","ORNE","NORMANDIE","Point",0.57262653,48.545654,"K52 - Dépôts de ferraille"]
["SSP001252901","73.0161","station service Simply Market",null,"En cours",null,null,"En cours","73181","MOUTIERS","SAVOIE","AUVERGNE-RHONE-ALPES","Point",6.527662,45.488533,"L23 - Détail de carburants"]
["SSP001253801","61.0080","Imprimerie de Montligeon",null,"En cours",null,null,"En cours","61097","LA CHAPELLE MONTLIGEON","ORNE","NORMANDIE","Point",0.65466887,48.48207,"H21 - Imprimerie, presse, édition"]
["SSP001254301","61.0084","SFAR",null,"En cours",null,null,"En cours","61491","TOUROUVRE","ORNE","NORMANDIE","Point",0.67494625,48.64802,"J51 - Fonderie des métaux ferreux"]
["SSP001255401","76.0364","Art Média Graphic (AMG)",null,"En cours",null,null,"En cours","76312","GOURNAY EN BRAY","SEINE-MARITIME","NORMANDIE","Point",1.7303299,49.48701,"M1 - Industries diverses"]
["SSP001255501","61.0099","PASSENAUD RECYCLAGE",null,"En cours",null,null,"En cours","61508","VIMOUTIERS","ORNE","NORMANDIE","Point",0.21834572,48.930946,"K52 - Dépôts de ferraille"]
["SSP001256501","50.0020","SNCF",null,"En cours",null,null,"En cours","50129","CHERBOURG OCTEVILLE","MANCHE","NORMANDIE","Point",-1.6200967,49.633163,"L23 - Détail de carburants"]
["SSP001257401","14.0054","FAN TECHNOLOGY (Ex FAN EUROPE ex VAUJOIS)",null,"En cours",null,null,"En cours","14437","MONDEVILLE","CALVADOS","NORMANDIE","Point",-0.2976483,49.157795,"J52 - Fonderie des métaux non ferreux"]
["SSP001258201","67.0255","BOLLORE Energie SA",null,"Clôturée",null,null,"Clôturée","67180","HAGUENAU","BAS-RHIN","GRAND EST","Point",0.0,0.0,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP001258301","47.0067","TOTAL ancienne station service Villeneuve sur Lot",null,"En cours",null,null,"En cours","47323","VILLENEUVE SUR LOT","LOT-ET-GARONNE","NOUVELLE-AQUITAINE","Point",0.0,0.0,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP001258901","72.0052","OUEST RENOV SERVICE",null,"En cours",null,null,"En cours","72008","ARNAGE","SARTHE","PAYS DE LA LOIRE","Point",0.19462964,47.928898,"K35 - Regroupement, reconditionnement de déchets"]
["SSP001259301","72.0057","AUCHAN Carburant",null,"En cours",null,null,"En cours","72065","LA CHAPELLE SAINT AUBIN","SARTHE","PAYS DE LA LOIRE","Point",0.17854221,48.035114,"L2 - Transports, automobile, carburants"]
["SSP001259701","17.0052","PICOTY ATLANTIQUE SERVICES",null,"En cours",null,null,"En cours","17183","GREZAC","CHARENTE-MARITIME","NOUVELLE-AQUITAINE","Point",0.0,0.0,"L1 - Entreposage, manutention, commerces"]
["SSP001260501","45.0147","EIFFAGE  (ex APPIA, ex HELLEBOID)",null,"En cours",null,null,"En cours","45298","SAINT PRYVE SAINT MESMIN","LOIRET","CENTRE-VAL DE LOIRE","Point",1.8819648,47.877846]
["SSP001261201","03.0049","Ancienne Station Service ELF (devenue Ancienne Station Service Total France)",null,"En cours",null,null,"En cours","03013","AVERMES","ALLIER","AUVERGNE-RHONE-ALPES","Point",3.3048942,46.60075,"D1 - Industrie pétrolière, gaz naturel"]
["SSP001261701","72.0075","SALLE Béatrice",null,"Clôturée",null,null,"Clôturée","72054","CHAMPAGNE","SARTHE","PAYS DE LA LOIRE","Point",0.0,0.0]
["SSP001262801","63.0060","CAFES EXCELLA",null,"En cours",null,null,"En cours","63193","LEMPDES","PUY-DE-DOME","AUVERGNE-RHONE-ALPES","Point",3.1870313,45.775253,"B2 - Industrie des boissons"]
["SSP001263001","76.0377","Site des Hauts Fourneaux de Rouen - Parcelle BC41",null,"En cours",null,null,"En cours","76322","LE GRAND QUEVILLY","SEINE-MARITIME","NORMANDIE","Point",1.0251102,49.40449]
["SSP001263601","62.0198","SCHAEFFLER CHAIN DRIVE SYSTEMS",null,"En cours",null,null,"En cours","62193","CALAIS","PAS-DE-CALAIS","HAUTS-DE-FRANCE","Point",0.0,0.0,"H1 - Mécanique, électrique, traitement de surface"]
["SSP001263701","28.0100","SIDEL FILLING ASSEPTIC",null,"En cours",null,null,"En cours","28134","DREUX","EURE-ET-LOIR","CENTRE-VAL DE LOIRE","Point",1.3438188,48.740948]
["SSP001263801","62.0200","TOTAL MARKETING SERVICES",null,"En cours",null,null,"En cours","62193","CALAIS","PAS-DE-CALAIS","HAUTS-DE-FRANCE","Point",1.7447928,59.855392,"L23 - Détail de carburants"]
["SSP001263901","62.0201","GALLOO LITTORAL - DIVISION CONDETTE",null,"En cours",null,null,"En cours","62235","CONDETTE","PAS-DE-CALAIS","HAUTS-DE-FRANCE","Point",1.6448945,50.67312,"K5 - Récupération, dépôts de ferrailles"]
["SSP001264001","37.0048","ROTOS 8 VINCENT",null,"En cours",null,null,"En cours","37261","TOURS","INDRE-ET-LOIRE","CENTRE-VAL DE LOIRE","Point",0.6724021,47.375225]
["SSP001264101","72.0079","TUPI (ex-BARBIER, ex-BURNET)",null,"En cours",null,null,"En cours","72132","LA FERTE BERNARD","SARTHE","PAYS DE LA LOIRE","Point",0.64649,48.18897]
["SSP001264201","62.0202","SOCIETE MARITIME DE COMBUSTIBLES LIQUIDES (SMCL)",null,"En cours",null,null,"En cours","62160","BOULOGNE SUR MER","PAS-DE-CALAIS","HAUTS-DE-FRANCE","Point",0.0,0.0,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP001264301","62.0203","ARC INTERNATIONAL Arques (ex MMV)",null,"En cours",null,null,"En cours","62040","ARQUES","PAS-DE-CALAIS","HAUTS-DE-FRANCE","Point",0.0,0.0]
["SSP001264501","71.0074","MARVELL GLASS-NORDEON (Ex PHILIPS ECLAIRAGE et TGI)",null,"En cours",null,null,"En cours","71076","CHALON SUR SAONE","SAONE-ET-LOIRE","BOURGOGNE-FRANCHE-COMTE","Point",4.8604164,46.80679,"G15 - Industrie du verre"]
["SSP001264801","71.0077","SAONE AUTOS PIECES (Hautefond)",null,"En cours",null,null,"En cours","71232","HAUTEFOND","SAONE-ET-LOIRE","BOURGOGNE-FRANCHE-COMTE","Point",4.1465297,46.442326,"L2 - Transports, automobile, carburants"]
["SSP001264901","28.0101","HAMMEL",null,"En cours",null,null,"En cours","28120","CRUCEY VILLAGES","EURE-ET-LOIR","CENTRE-VAL DE LOIRE","Point",1.3444507,48.526226]
["SSP001265301","62.0205","ARC INTERNATIONAL Arques (ex atelier de composition - terrain du quai)",null,"En cours",null,null,"En cours","62040","ARQUES","PAS-DE-CALAIS","HAUTS-DE-FRANCE","Point",0.0,0.0,"G15 - Industrie du verre"]
["SSP001265401","16.0038","Ancien site SAFT LECLANCHE - rue Jules durandeau",null,"En cours",null,null,"En cours","16015","ANGOULEME","CHARENTE","NOUVELLE-AQUITAINE","Point",0.14988182,45.65843,"H16 - Piles électriques et accumulateurs (fabrication de)"]
["SSP001265501","75.0037","S.A.S Rouge Pullon",null,"En cours",null,null,"En cours","75056","PARIS","PARIS","ILE-DE-FRANCE","Polygone",2.3601396,48.8659,"H13 - Traitement de surface"]
["SSP001265701","71.0087","SCIERIE LAMURE",null,"En cours",null,null,"En cours","71428","SAINT IGNY DE ROCHE","SAONE-ET-LOIRE","BOURGOGNE-FRANCHE-COMTE","Point",4.314001,46.202793,"C11 - Scierie, fabrication de panneaux"]
["SSP001265801","75.0036","CPCU Bichat",null,"En cours",null,null,"En cours","75056","PARIS","PARIS","ILE-DE-FRANCE","Point",2.3072464,48.88455]
["SSP001265901","71.0088","SARP Mâcon",null,"En cours",null,null,"En cours","71270","MACON","SAONE-ET-LOIRE","BOURGOGNE-FRANCHE-COMTE","Point",4.8252277,46.28604,"K - Déchets et traitements"]
["SSP001266301","71.0090","MACON ENROBES",null,"En cours",null,null,"En cours","71270","MACON","SAONE-ET-LOIRE","BOURGOGNE-FRANCHE-COMTE","Point",4.8253613,46.286137,"G22 - Centrales d'enrobés"]
["SSP001266401","71.0096","SARL Benoit POINSOT",null,"En cours",null,null,"En cours","71545","TRAMAYES","SAONE-ET-LOIRE","BOURGOGNE-FRANCHE-COMTE","Point",4.6026626,46.30759,"L23 - Détail de carburants"]
["SSP001266501","71.0092","LABRUYERE DISTRIBUTION",null,"En cours",null,null,"En cours","71270","MACON","SAONE-ET-LOIRE","BOURGOGNE-FRANCHE-COMTE","Point",4.8280845,46.29027,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP001266601","71.0093","Co. de Co. de Gueugnon - Déchetterie du Sauze",null,"En cours",null,null,"En cours","71230","GUEUGNON","SAONE-ET-LOIRE","BOURGOGNE-FRANCHE-COMTE","Point",4.056986,46.585148,"K - Déchets et traitements"]
["SSP001266701","72.0077","Garage DELORME (ex-Casse Auto)",null,"En cours",null,null,"En cours","72110","CROSMIERES","SARTHE","PAYS DE LA LOIRE","Point",-0.16314204,47.747353,"K5 - Récupération, dépôts de ferrailles"]
["SSP001266801","72.0078","Ex Ets COSSON",null,"Clôturée",null,null,"Clôturée","72008","ARNAGE","SARTHE","PAYS DE LA LOIRE","Point",0.18471196,47.940304]
["SSP001267101","71.0095","Station service SIMPLY MARKET",null,"En cours",null,null,"En cours","71543","TOURNUS","SAONE-ET-LOIRE","BOURGOGNE-FRANCHE-COMTE","Point",4.9155893,46.55815,"L23 - Détail de carburants"]
["SSP001267201","71.0097","Ancienne décharge industrielle  Peugeot",null,"En cours",null,null,"En cours","71220","GILLY SUR LOIRE","SAONE-ET-LOIRE","BOURGOGNE-FRANCHE-COMTE","Point",3.7427456,46.549908,"K36 - Mise en décharge"]
["SSP001267301","59.0618","H2D ex S.A Heliogravure Didier-Quebecor ex S.A. HELIOGRAVURE Jean DIDIER, anc. H",null,"En cours",null,null,"En cours","59350","LILLE","NORD","HAUTS-DE-FRANCE","Point",0.0,0.0,"H21 - Imprimerie, presse, édition"]
["SSP001267401","71.0098","LAGARDE",null,"En cours",null,null,"En cours","71047","BOURBON LANCY","SAONE-ET-LOIRE","BOURGOGNE-FRANCHE-COMTE","Point",3.765484,46.63271,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP001267601","71.0099","TEREX CRANES",null,"En cours",null,null,"En cours","71486","SAINT VALLIER","SAONE-ET-LOIRE","BOURGOGNE-FRANCHE-COMTE","Point",4.3510604,46.651276,"H1 - Mécanique, électrique, traitement de surface"]
["SSP001267701","71.0100","RABOINE (Ex FORMAN)",null,"En cours",null,null,"En cours","71356","POUILLOUX","SAONE-ET-LOIRE","BOURGOGNE-FRANCHE-COMTE","Point",4.368288,46.603115,"K - Déchets et traitements"]
["SSP001267801","59.0620","FRANCODIM",null,"En cours",null,null,"En cours","59279","HALLUIN","NORD","HAUTS-DE-FRANCE","Point",0.0,0.0]
["SSP001267901","45.0156","PHOSCAO",null,"En cours",null,null,"En cours","45082","CHATEAUNEUF SUR LOIRE","LOIRET","CENTRE-VAL DE LOIRE","Point",0.0,0.0]
["SSP001268001","27.0109","GRANDS MOULINS DE PARIS",null,"En cours",null,null,"En cours","27051","BEAUMONT LE ROGER","EURE","NORMANDIE","Point",0.77143294,49.074116,"B17 - Autres industries agro-alimentaires"]
["SSP001268101","45.0162","SCA AXEREAL",null,"En cours",null,null,"En cours","45235","ORMES","LOIRET","CENTRE-VAL DE LOIRE","Point",1.8168741,47.947586]
["SSP001268201","45.0157","SAS DAVID (Coopérative Caproga La Meunière)",null,"En cours",null,null,"En cours","45083","CHATEAU RENARD","LOIRET","CENTRE-VAL DE LOIRE","Point",2.9353652,47.927765]
["SSP001268301","45.0158","Malteries Franco-Belges (MFB)",null,"En cours",null,null,"En cours","45253","PITHIVIERS LE VIEIL","LOIRET","CENTRE-VAL DE LOIRE","Point",0.0,0.0]
["SSP001268401","45.0159","Coopérative Caproga La Meunière",null,"En cours",null,null,"En cours","45307","LA SELLE SUR LE BIED","LOIRET","CENTRE-VAL DE LOIRE","Point",2.9045715,48.08197]
["SSP001268501","45.0160","Caproga La Meunière",null,"En cours",null,null,"En cours","45178","LADON","LOIRET","CENTRE-VAL DE LOIRE","Point",2.5455434,48.001556]
["SSP001268701","52.0041","DUSSAUSSAY GALLIER",null,"En cours",null,null,"En cours","52353","NOGENT","HAUTE-MARNE","GRAND EST","Point",5.3498144,48.03639,"H - Mécanique, traitements des surfaces"]
["SSP001268901","11.0025","EFISOL",null,"En cours",null,null,"En cours","11129","ESPERAZA","AUDE","OCCITANIE","Point",2.2253923,42.9337,"D34 - Fabrication de matières plastiques de base"]
["SSP001269001","37.0049","TOUR(S)PLUS (ex SMICTOM de la Billette)",null,"En cours",null,null,"En cours","37122","JOUE LES TOURS","INDRE-ET-LOIRE","CENTRE-VAL DE LOIRE","Point",0.6191115,47.30429,"K21 - Décharges d'ordures ménagères"]
["SSP001269101","37.0050","VILLERET Bernard",null,"En cours",null,null,"En cours","37132","LOCHES","INDRE-ET-LOIRE","CENTRE-VAL DE LOIRE","Point",0.983183,47.13438,"L21 - Vente et réparation automobile"]
["SSP001269201","37.0053","AUCHAN CARBURANT - La Petite Arche",null,"En cours",null,null,"En cours","37261","TOURS","INDRE-ET-LOIRE","CENTRE-VAL DE LOIRE","Point",0.7025632,47.39814,"L23 - Détail de carburants"]
["SSP001269301","37.0054","PLASTIVALOIRE",null,"En cours",null,null,"En cours","37072","CHINON","INDRE-ET-LOIRE","CENTRE-VAL DE LOIRE","Point",0.27209085,47.17856,"D34 - Fabrication de matières plastiques de base"]
["SSP001269401","45.0163","HITACHI COMPUTER PRODUCTS",null,"En cours",null,null,"En cours","45006","ARDON","LOIRET","CENTRE-VAL DE LOIRE","Point",1.9206288,47.819965,"H18 - Composants électroniques (fabrication de)"]
["SSP001269501","26.0092","COLAS RHONE ALPES AUVERGNE",null,"En cours",null,null,"En cours","26124","ETOILE SUR RHONE","DROME","AUVERGNE-RHONE-ALPES","Point",4.848905,44.85858,"G22 - Centrales d'enrobés"]
["SSP001269601","33.0479","PEUGEOT RETAIL",null,"En cours",null,null,"En cours","33281","MERIGNAC","GIRONDE","NOUVELLE-AQUITAINE","Polygone",-0.6452783,44.831272,null,null,"50.2Z - Entretien et réparation de véhicules automobiles"]
["SSP001269701","45.0166","ANCIENNE USINE A GAZ– Jargeau",null,"En cours",null,null,"En cours","45173","JARGEAU","LOIRET","CENTRE-VAL DE LOIRE","Point",2.1238053,47.864475,"J1 - Cokéfaction, usines à gaz"]
["SSP001269901","76.0379","Décharge GAILLIARD",null,"En cours",null,null,"En cours","76057","BARENTIN","SEINE-MARITIME","NORMANDIE","Point",0.9582739,49.554974,"E1 - Textile et habillement, teinture, impression"]
["SSP001270001","45.0165","DURALEX International",null,"En cours",null,null,"En cours","45075","LA CHAPELLE SAINT MESMIN","LOIRET","CENTRE-VAL DE LOIRE","Point",1.825603,47.895813,"G15 - Industrie du verre"]
["SSP001270101","42.0206","STAUB FONDERIE",null,"En cours",null,null,"En cours","42189","ROCHE LA MOLIERE","LOIRE","AUVERGNE-RHONE-ALPES","Point",4.3280525,45.43622,"G12 - Fabrication de produits céramiques"]
["SSP001270201","31.0097","AIRBUS OPERATIONS SAS Site Clément Ader",null,"En cours",null,null,"En cours","31149","COLOMIERS","HAUTE-GARONNE","OCCITANIE","Point",1.3474075,43.62524,"H15 - Assemblage, montage"]
["SSP001270301","42.0207","SAM OUTILLAGE",null,"En cours",null,null,"En cours","42218","SAINT ETIENNE","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.389837,45.454067,"J5 - Fonderie et travail des métaux"]
["SSP001270401","01.0128","CHROMECA",null,"En cours",null,null,"En cours","01043","BEYNOST","AIN","AUVERGNE-RHONE-ALPES","Point",4.991115,45.82355,"H13 - Traitement de surface"]
["SSP001270501","37.0055","Garage BLANCHET",null,"En cours",null,null,"En cours","37184","LE PETIT PRESSIGNY","INDRE-ET-LOIRE","CENTRE-VAL DE LOIRE","Point",0.91879034,46.922626,"L23 - Détail de carburants"]
["SSP001270601","28.0102","Société FAUCHEUX",null,"En cours",null,null,"En cours","28218","LUCE","EURE-ET-LOIR","CENTRE-VAL DE LOIRE","Point",1.4671104,48.43066,"H15 - Assemblage, montage"]
["SSP001270901","37.0059","CHROM'FLASH (ex METAL COLOR)",null,"En cours",null,null,"En cours","37233","SAINT PIERRE DES CORPS","INDRE-ET-LOIRE","CENTRE-VAL DE LOIRE","Point",0.7580369,47.389435,"H13 - Traitement de surface"]
["SSP001271001","18.0068","ROSINOX",null,"En cours",null,null,"En cours","18033","BOURGES","CHER","CENTRE-VAL DE LOIRE","Point",2.394231,47.09953,"M1 - Industries diverses"]
["SSP001271101","38.0305","Dauphinoise de Matériaux Enrobés",null,"Clôturée",null,"2018-10-10","Clôturée","38276","NIVOLAS VERMELLE","ISERE","AUVERGNE-RHONE-ALPES","Point",5.307129,45.565113,"G22 - Centrales d'enrobés"]
["SSP001271201","37.0058","LOISEAU TOURAINE",null,"En cours",null,null,"En cours","37195","LA RICHE","INDRE-ET-LOIRE","CENTRE-VAL DE LOIRE","Point",0.6370822,47.37914]
["SSP001271301","69.0397","TRACTEL SOLUTIONS",null,"En cours",null,null,"En cours","69204","SAINT GENIS LAVAL","RHONE","AUVERGNE-RHONE-ALPES","Point",4.810222,45.69602,"D4 - Encres, vernis, peintures, colles (fabrication de)"]
["SSP001271401","18.0069","Société LIOT",null,"En cours",null,null,"En cours","18220","SAINT LEGER LE PETIT","CHER","CENTRE-VAL DE LOIRE","Point",3.0077538,47.1092,"B3 - Fabrication d'aliments pour animaux"]
["SSP001271601","75.0038","CPCU VAUGIRARD Dépôt",null,"En cours",null,null,"En cours","75056","PARIS","PARIS","ILE-DE-FRANCE","Polygone",2.3091984,48.83306,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP001271701","45.0167","OTIS",null,"En cours",null,null,"En cours","45155","GIEN","LOIRET","CENTRE-VAL DE LOIRE","Point",2.6262984,47.70221,"M1 - Industries diverses"]
["SSP001271801","18.0070","NEXTER SYSTEMS - TERRAIN SUD",null,"En cours",null,null,"En cours","18033","BOURGES","CHER","CENTRE-VAL DE LOIRE","Point",2.4153187,47.0784,"H13 - Traitement de surface"]
["SSP001271901","18.0071","Société NEXTER MUNITIONS GUERRY (ex GIAT Guerry)",null,"En cours",null,null,"En cours","18033","BOURGES","CHER","CENTRE-VAL DE LOIRE","Point",2.4243593,47.071064,"D81 - Poudres et explosifs (fabrication de)"]
["SSP001272001","18.0072","NEXTER SYSTEMS - GUERRY (ex Giat guerry)",null,"En cours",null,null,"En cours","18033","BOURGES","CHER","CENTRE-VAL DE LOIRE","Point",2.4243593,47.071064,"H - Mécanique, traitements des surfaces"]
["SSP001272101","38.0309","ECOPLA FRANCE",null,"En cours",null,null,"En cours","38466","SAINT VINCENT DE MERCUZE","ISERE","AUVERGNE-RHONE-ALPES","Point",5.9599576,45.37197]
["SSP001272401","76.0380","station TOTAL- relais du Rouvray",null,"En cours",null,null,"En cours","76484","OISSEL","SEINE-MARITIME","NORMANDIE","Polygone",1.1011977,49.35883,"L23 - Détail de carburants"]
["SSP001272501","37.0060","STIN - NARDEUX",null,"En cours",null,null,"En cours","37132","LOCHES","INDRE-ET-LOIRE","CENTRE-VAL DE LOIRE","Point",0.9907988,47.140728]
["SSP001272601","85.0047","Incobois",null,"En cours",null,null,"En cours","85217","SAINT GEORGES DE MONTAIGU","VENDEE","PAYS DE LA LOIRE","Point",-1.281979,46.940556,"C13 - Traitement du bois"]
["SSP001272801","38.0310","SKIS ROSSIGNOL",null,"En cours",null,null,"En cours","38383","SAINT ETIENNE DE CROSSEY","ISERE","AUVERGNE-RHONE-ALPES","Point",5.64364,45.380703]
["SSP001272901","03.0059","DUNLOP - Pistes d'essais",null,"En cours",null,null,"En cours","03262","SAINT VICTOR","ALLIER","AUVERGNE-RHONE-ALPES","Point",2.5881512,46.37991]
["SSP001273001","69.0391","STATION SERVICE AUCHAN",null,"En cours",null,null,"En cours","69072","DARDILLY","RHONE","AUVERGNE-RHONE-ALPES","Point",4.766054,45.821114]
["SSP001273101","76.0391","EURL BLONDEL",null,"En cours",null,null,"En cours","76002","ALVIMARE","SEINE-MARITIME","NORMANDIE","Point",0.6299587,49.603615,"L23 - Détail de carburants"]
["SSP001273201","974.0053","STATION SERVICE CADIVEL Daniel",null,"En cours",null,null,"En cours","97402","BRAS-PANON","LA REUNION","LA REUNION","Point",0.0,0.0,"L23 - Détail de carburants"]
["SSP001273301","76.0381","Station-service Ex-Comptoirs Modernes",null,"Clôturée",null,"2019-01-15","Clôturée","76402","MALAUNAY","SEINE-MARITIME","NORMANDIE","Point",1.035119,49.52318,"L23 - Détail de carburants"]
["SSP001273701","974.0052","STATION SERVICE TOTAL GENERAL LAMBERT",null,"En cours",null,null,"En cours","97413","SAINT-LEU","LA REUNION","LA REUNION","Point",55.28806,-21.176907,"L23 - Détail de carburants"]
["SSP001273801","27.0111","RAS Environnement",null,"En cours",null,null,"En cours","27268","LE FRESNE","EURE","NORMANDIE","Point",0.96846795,48.937935,"K35 - Regroupement, reconditionnement de déchets"]
["SSP001273901","27.0112","LEPICARD Agriculture",null,"En cours",null,null,"En cours","27165","CONCHES EN OUCHE","EURE","NORMANDIE","Point",0.96653855,48.93664,"K52 - Dépôts de ferraille"]
["SSP001274001","974.0054","STATION TOTAL MENDES ST-SUZANNE",null,"En cours",null,null,"En cours","97420","SAINTE-SUZANNE","LA REUNION","LA REUNION","Point",55.609863,-20.90915,"L23 - Détail de carburants"]
["SSP001274201","84.0040","SOTRAMO-PAROLA",null,"En cours",null,null,"En cours","84089","PERTUIS","VAUCLUSE","PROVENCE-ALPES-COTE D'AZUR","Point",0.0,0.0]
["SSP001274401","973.0009","Ancien dépôt SARA du Larivot",null,"En cours",null,null,"En cours","97307","MATOURY","GUYANE","GUYANE","Point",-52.36006,4.901986,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP001274501","30.0033","GREIF","Greif","En cours",null,null,"En cours","30141","LAUDUN L'ARDOISE","GARD","OCCITANIE","Polygone",4.652651,44.087864,null,null,null,"25.91Z - Fabrication de fûts et emballages métalliques similaires"]
["SSP001274601","45.0174","COMTE",null,"En cours",null,null,"En cours","45098","CLERY SAINT ANDRE","LOIRET","CENTRE-VAL DE LOIRE","Point",1.746795,47.821133]
["SSP001274701","45.0173","SGA MEYER",null,"En cours",null,null,"En cours","45254","POILLY LEZ GIEN","LOIRET","CENTRE-VAL DE LOIRE","Point",2.5708992,47.663795]
["SSP001274801","19.0032","Ancien dépôt d'hydrocarbures ALVEA",null,"En cours",null,null,"En cours","19272","TULLE","CORREZE","NOUVELLE-AQUITAINE","Point",1.7429181,45.242126,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP001274901","57.0229","WERNER",null,"En cours",null,null,"En cours","57628","SARRALBE","MOSELLE","GRAND EST","Point",7.022051,48.976936]
["SSP001275001","27.0113","Fromagerie DI BENEDETTO",null,"En cours",null,null,"En cours","27504","SACQUENVILLE","EURE","NORMANDIE","Point",1.0787984,49.09347,"B12 - Industrie laitière"]
["SSP001275201","69.0394","SECOSAR ETIRAGE",null,"En cours",null,null,"En cours","69259","VENISSIEUX","RHONE","AUVERGNE-RHONE-ALPES","Point",4.898609,45.68793]
["SSP001275301","22.0018","LOUISIANE",null,"En cours",null,null,"En cours","22136","LOUDEAC","COTES-D'ARMOR","BRETAGNE","Point",-2.7544036,48.16132,"C13 - Traitement du bois"]
["SSP001275401","76.0388","BOLLORE ENERGY",null,"En cours",null,null,"En cours","76178","CLEON","SEINE-MARITIME","NORMANDIE","Point",1.0224755,49.31232]
["SSP001275501","03.0061","Fonderie R.BREA SA (stockage de déchets)",null,"En cours",null,null,"En cours","03301","VAUX","ALLIER","AUVERGNE-RHONE-ALPES","Point",2.6006248,46.4143,"J32 - Métallurgie de l'aluminium"]
["SSP001275601","49.0073","Ancien Centre d’Études et de Construction de Prototypes (CECP)- (Avenue Général ",null,"En cours",null,null,"En cours","49007","ANGERS","MAINE-ET-LOIRE","PAYS DE LA LOIRE","Polygone",-0.53137803,47.47871]
["SSP001275701","59.0621","SAS LOMME (MOSSLEY SARTEL ex FREMAUX)",null,"En cours",null,null,"En cours","59350","LILLE","NORD","HAUTS-DE-FRANCE","Point",0.0,0.0]
["SSP001275801","45.0170","SCHIEVER CARBURANT (ex ATAC)",null,"En cours",null,null,"En cours","45229","NOGENT SUR VERNISSON","LOIRET","CENTRE-VAL DE LOIRE","Point",0.0,0.0]
["SSP001275901","76.0389","Bois et Matériaux (ex WOLSELEY FRANCE)","Cessation partielle","En cours",null,null,"En cours","76599","SAINT LEGER DU BOURG DENIS","SEINE-MARITIME","NORMANDIE","Polygone",1.1518321,49.43442]
["SSP001276001","14.0057","Ancienne décharge communale",null,"En cours",null,null,"En cours","14467","NORON L'ABBAYE","CALVADOS","NORMANDIE","Point",-0.22760001,48.898888]
["SSP001276101","44.0154","AUTO GARAGE DE L'OUEST",null,"En cours",null,null,"En cours","44162","SAINT HERBLAIN","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Point",-1.6265537,47.253445,"L21 - Vente et réparation automobile"]
["SSP001276201","69.0395","STEF LOGISTIQUE",null,"En cours",null,null,"En cours","69123","LYON","RHONE","AUVERGNE-RHONE-ALPES","Point",4.835173,45.723976,"L12 - Entrepôts frigorifiques"]
["SSP001276301","19.0033","TOTAL MARKETING SERVICES - Dépôt pétrolier de Brive (EPC )",null,"En cours",null,null,"En cours","19031","BRIVE LA GAILLARDE","CORREZE","NOUVELLE-AQUITAINE","Point",0.0,0.0,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP001276401","44.0156","ATELIERS NANTAIS MOULAGE DECOR SOUS TRAITANCE (ANMDS)",null,"En cours",null,null,"En cours","44041","LA CHEVROLIERE","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Polygone",-1.5950034,47.10411]
["SSP001276601","49.0076","JULES OLIVIER DISTRIBUTION (ex CONSTANT BOCHEREAU)",null,"En cours",null,null,"En cours","49069","CHAMPTOCEAUX","MAINE-ET-LOIRE","PAYS DE LA LOIRE","Point",-1.2428871,47.2638,"B23 - Fabrication d'autres boissons"]
["SSP001276701","44.0157","station service AS 24",null,"Clôturée",null,null,"Clôturée","44109","NANTES","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Polygone",-1.5555001,47.201595,null,null,"50.5Z - Commerce de détail de carburants"]
["SSP001276901","76.0394","ESSITY",null,"En cours",null,null,"En cours","76575","SAINT ETIENNE DU ROUVRAY","SEINE-MARITIME","NORMANDIE","Point",1.1165216,49.398586,"C21 - Fabrication de pâte à papier"]
["SSP001277001","74.0130","Site historique de Chedde – ancienne usine de production de perchlorates (ARKEMA",null,"En cours",null,null,"En cours","74208","PASSY","HAUTE-SAVOIE","AUVERGNE-RHONE-ALPES","Point",6.729097,45.92609,"D31 - Industrie du chlore"]
["SSP001277301","76.0393","CASTRES EQUIPEMENT",null,"En cours",null,null,"En cours","76681","SOTTEVILLE LES ROUEN","SEINE-MARITIME","NORMANDIE","Point",1.0947064,49.421143]
["SSP001277401","01.0129","PHILLIPS",null,"En cours",null,null,"En cours","01249","MIRIBEL","AIN","AUVERGNE-RHONE-ALPES","Point",4.966813,45.823093]
["SSP001277501","95.0073","LIBIOL-GATEFOSSE",null,"En cours",null,null,"En cours","95598","SOISY SOUS MONTMORENCY","VAL-D'OISE","ILE-DE-FRANCE","Point",2.3000228,48.976585,"D38 - Industrie pharmaceutique"]
["SSP001277601","75.0041","AGIP KENNEDY",null,"En cours",null,null,"En cours","75056","PARIS","PARIS","ILE-DE-FRANCE","Polygone",2.2806818,48.852375,"L23 - Détail de carburants"]
["SSP001277701","69.0398","CROWN EMBALLAGE",null,"En cours",null,null,"En cours","69268","VOURLES","RHONE","AUVERGNE-RHONE-ALPES","Point",4.762489,45.657413,"H21 - Imprimerie, presse, édition"]
["SSP001277901","49.0078","CONSTRUCTIONS TRILLOT",null,"En cours",null,null,"En cours","49089","CHAZE SUR ARGOS","MAINE-ET-LOIRE","PAYS DE LA LOIRE","Point",0.0,0.0,"C13 - Traitement du bois"]
["SSP001278101","38.0307","ASCO INDUSTRIES - Lot 12",null,"En cours",null,null,"En cours","38100","LE CHEYLAS","ISERE","AUVERGNE-RHONE-ALPES","Point",5.9995103,45.382362,"J22 - Production d'acier brut, aciéries"]
["SSP001278201","973.0011","Ancienne Décharge de Rémire-Montjoly",null,"En cours",null,null,"En cours","97309","REMIRE-MONTJOLY","GUYANE","GUYANE","Polygone",-52.2861,4.8911467,"K21 - Décharges d'ordures ménagères"]
["SSP001278301","69.0399","THEVENIN DUCROT DISTRIBUTION",null,"En cours",null,null,"En cours","69161","PROPIERES","RHONE","AUVERGNE-RHONE-ALPES","Point",4.436853,46.192577,"L23 - Détail de carburants"]
["SSP001278401","69.0400","Station service CARREFOUR",null,"En cours",null,null,"En cours","69266","VILLEURBANNE","RHONE","AUVERGNE-RHONE-ALPES","Point",4.8844976,45.769436]
["SSP001278701","973.0013","STATION TOTAL COLLERY EST",null,"En cours",null,null,"En cours","97302","CAYENNE","GUYANE","GUYANE","Point",-52.324284,4.902881,"L23 - Détail de carburants"]
["SSP001278801","973.0012","Casse la LEVEE MATOURY",null,"En cours",null,"2015-12-31","En cours","97307","MATOURY","GUYANE","GUYANE","Polygone",-52.32549,4.832988,null,"65.03 - Vente et réparation de véhicules automobiles"]
["SSP001278901","31.0098","Société des Eaux Minérales de Luchon",null,"En cours",null,null,"En cours","31042","BAGNERES DE LUCHON","HAUTE-GARONNE","OCCITANIE","Point",0.5974046,42.806896,"B2 - Industrie des boissons"]
["SSP001279001","31.0099","GETINGE LANCER",null,"En cours",null,null,"En cours","31557","TOURNEFEUILLE","HAUTE-GARONNE","OCCITANIE","Point",1.3120089,43.591656,"H13 - Traitement de surface"]
["SSP001279201","44.0164","LE HESRAN",null,"En cours",null,null,"En cours","44187","SAINT PERE EN RETZ","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Point",-2.039302,47.21458]
["SSP001279301","76.0396","SA LEBOUCHER",null,"En cours",null,null,"En cours","76474","NOTRE DAME DE BONDEVILLE","SEINE-MARITIME","NORMANDIE","Point",1.0463715,49.486553]
["SSP001279601","33.0482","Grand chantier des prés salés",null,"En cours",null,null,"En cours","33529","LA TESTE DE BUCH","GIRONDE","NOUVELLE-AQUITAINE","Polygone",-1.1487494,44.649036,"K21 - Décharges d'ordures ménagères"]
["SSP001279801","33.0483","LAQ'AUTO",null,"En cours",null,null,"En cours","33063","BORDEAUX","GIRONDE","NOUVELLE-AQUITAINE","Point",115.36598,-75.25045]
["SSP001280001","14.0060","Ancienne décharge de Canvie (Saint Martin de Tallevende)",null,"En cours",null,null,"En cours","14762","VIRE","CALVADOS","NORMANDIE","Point",-0.9208793,48.828403,"K21 - Décharges d'ordures ménagères"]
["SSP001280101","33.0484","SDS - Sté de Signalisation",null,"En cours",null,null,"En cours","33013","ARTIGUES PRES BORDEAUX","GIRONDE","NOUVELLE-AQUITAINE","Polygone",-0.50024396,44.854412,"H1 - Mécanique, électrique, traitement de surface"]
["SSP001280301","33.0486","LAMOTHE ABIET PINOSA - Emile Counord",null,"En cours",null,null,"En cours","33063","BORDEAUX","GIRONDE","NOUVELLE-AQUITAINE","Polygone",-0.57465416,44.8596,"K3 - Traitement de déchets industriels"]
["SSP001280501","33.0488","AQUITAINE DECAPAGE",null,"En cours",null,null,"En cours","33434","SAINT LOUIS DE MONTFERRAND","GIRONDE","NOUVELLE-AQUITAINE","Polygone",-0.52612287,44.939953,"H13 - Traitement de surface"]
["SSP001280601","38.0308","SCHNEIDER ELECTRICS SA Usine B (ex-MERLIN GERIN)",null,"En cours",null,null,"En cours","38185","GRENOBLE","ISERE","AUVERGNE-RHONE-ALPES","Polygone",5.711341,45.200886,null,null,null,"27.11Z - Fabrication de moteurs, génératrices et transformateurs électriques"]
["SSP001280701","33.0489","ALLIANCE PISCINES EUROPE",null,"En cours",null,null,"En cours","33056","BLANQUEFORT","GIRONDE","NOUVELLE-AQUITAINE","Point",-0.6231987,44.919052]
["SSP001280801","33.0490","BORDEAUX METROPOLE Décharge de Labarde 2",null,"En cours",null,null,"En cours","33063","BORDEAUX","GIRONDE","NOUVELLE-AQUITAINE","Point",-0.55003154,44.895233,"K21 - Décharges d'ordures ménagères"]
["SSP001280901","33.0491","LABADIE",null,"En cours",null,null,"En cours","33119","CENON","GIRONDE","NOUVELLE-AQUITAINE","Polygone",-0.5373136,44.861053,"K5 - Récupération, dépôts de ferrailles"]
["SSP001281001","33.0502","TRANSGOURMET OPERATIONS (ex BOREHAL)",null,"En cours",null,null,"En cours","33433","SAINT LOUBES","GIRONDE","NOUVELLE-AQUITAINE","Polygone",-0.45531875,44.91903,null,"73.07 - Entrepôts autres que frigorifiques"]
["SSP001281201","69.0401","SAONE AZERGUES",null,"En cours",null,null,"En cours","69273","CORBAS","RHONE","AUVERGNE-RHONE-ALPES","Point",4.909301,45.68305]
["SSP001281401","44.0163","DEPANNAGE AUTOMOBILES PEROU (DAP)",null,"En cours",null,null,"En cours","44158","SAINT ETIENNE DE MONTLUC","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Point",-1.733938,47.282024]
["SSP001281501","14.0061","BLOC MIROIR",null,"En cours",null,null,"En cours","14371","LIVAROT","CALVADOS","NORMANDIE","Point",0.1509253,48.99593,"H14 - Application de peinture"]
["SSP001281601","69.0402","Raccords plastiques Nicoll",null,"En cours",null,null,"En cours","69288","SAINT LAURENT DE MURE","RHONE","AUVERGNE-RHONE-ALPES","Point",5.037362,45.690742]
["SSP001281701","69.0403","USICHROM",null,"En cours",null,null,"En cours","69266","VILLEURBANNE","RHONE","AUVERGNE-RHONE-ALPES","Point",4.8769784,45.771244,"H13 - Traitement de surface"]
["SSP001281801","33.0498","ECOGRAS",null,"En cours",null,null,"En cours","33032","BASSENS","GIRONDE","NOUVELLE-AQUITAINE","Point",-0.5434584,44.92225,"G24 - Produits à base d'amiante (fabrication de)"]
["SSP001282001","62.0206","NICOLAY FILS",null,"En cours",null,null,"En cours","62043","LES ATTAQUES","PAS-DE-CALAIS","HAUTS-DE-FRANCE","Point",0.0,0.0]
["SSP001282501","92.0109","SEVIA",null,"En cours",null,null,"En cours","92004","ASNIERES SUR SEINE","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.3141284,48.915695,"K35 - Regroupement, reconditionnement de déchets"]
["SSP001282801","03.0062","AGIS (Ex DIAMANTINE)",null,"En cours",null,null,"En cours","03185","MONTLUCON","ALLIER","AUVERGNE-RHONE-ALPES","Point",2.6199245,46.343044,"D42 - Fabrication de peintures"]
["SSP001282901","03.0064","JYS CHROME",null,"En cours",null,null,"En cours","03180","MONTBEUGNY","ALLIER","AUVERGNE-RHONE-ALPES","Point",3.490162,46.529232,"H13 - Traitement de surface"]
["SSP001283101","33.0503","DISTILLERIE Guy NEYRAC",null,"En cours",null,null,"En cours","33324","PINEUILH","GIRONDE","NOUVELLE-AQUITAINE","Polygone",0.20819026,44.821712,null,"41.01 - Distillation d'alcool"]
["SSP001283301","33.0506","PLACOPLATRE- Sadirac",null,"En cours",null,null,"En cours","33363","SADIRAC","GIRONDE","NOUVELLE-AQUITAINE","Polygone",-0.42538047,44.776283,null,"15.09 - Fabrication de matériaux de construction divers"]
["SSP001283401","33.0507","PERNAT SMJ",null,"En cours",null,null,"En cours","33449","SAINT MEDARD EN JALLES","GIRONDE","NOUVELLE-AQUITAINE","Polygone",-0.6921235,44.879585,null,"53.02 - Fabrication de pièces diverses pour l'industrie"]
["SSP001283801","33.0511","CHATEAU BATAILLEY",null,"En cours",null,null,"En cours","33314","PAUILLAC","GIRONDE","NOUVELLE-AQUITAINE","Polygone",-0.78454494,45.177017,"F32 - Carrières"]
["SSP001283901","33.0512","CHATEAU LYNCH MOUSSAS",null,"En cours",null,null,"En cours","33314","PAUILLAC","GIRONDE","NOUVELLE-AQUITAINE","Polygone",-0.7846103,45.17809,"F32 - Carrières"]
["SSP001284101","33.0515","MAIRIE - Soussans",null,"En cours",null,null,"En cours","33517","SOUSSANS","GIRONDE","NOUVELLE-AQUITAINE","Polygone",-0.719333,45.036003,"K21 - Décharges d'ordures ménagères"]
["SSP001284201","69.0406","Schulman",null,"En cours",null,null,"En cours","69175","SAVIGNY","RHONE","AUVERGNE-RHONE-ALPES","Point",4.5952225,45.824623]
["SSP001284801","14.0065","FRANCE CHAMPIGNON (ex. GANOT)",null,"En cours",null,null,"En cours","14258","FALAISE","CALVADOS","NORMANDIE","Point",-0.178775,48.895397,"B17 - Autres industries agro-alimentaires"]
["SSP001284901","33.0518","OCCAMAT-DELAIR",null,"En cours",null,null,"En cours","33496","SALLEBOEUF","GIRONDE","NOUVELLE-AQUITAINE","Polygone",-0.38543737,44.833138,"K3 - Traitement de déchets industriels"]
["SSP001285001","33.0519","LARRE Christian",null,"En cours",null,null,"En cours","33080","CADAUJAC","GIRONDE","NOUVELLE-AQUITAINE","Polygone",-0.53137285,44.738037,"K52 - Dépôts de ferraille"]
["SSP001285301","973.0014","RUBIS (ancien dépot de caburants Chevron, TEXACO Monnerville)",null,"En cours",null,null,"En cours","97311","SAINT-LAURENT-DU-MARONI","GUYANE","GUYANE","Point",-54.034058,5.494663,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP001285601","44.0168","CROWN EMBALLAGE FRANCE",null,"En cours",null,null,"En cours","44109","NANTES","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Point",-1.6006975,47.19761]
["SSP001285701","60.0138","sivia",null,"En cours",null,null,"En cours","60245","FORMERIE","OISE","HAUTS-DE-FRANCE","Point",0.0,0.0]
["SSP001286001","33.0522","CANTE Réhabilitation - ISDI",null,"En cours",null,null,"En cours","33213","LA BREDE","GIRONDE","NOUVELLE-AQUITAINE","Polygone",-0.56516767,44.68946,"K - Déchets et traitements"]
["SSP001286101","65.0017","ENSTO NOVEXIA PARAFOUDRES",null,"En cours",null,null,"En cours","65059","BAGNERES DE BIGORRE","HAUTES-PYRENEES","OCCITANIE","Point",0.15208648,43.0755]
["SSP001286201","42.0208","BEL MAILLE",null,"En cours",null,null,"En cours","42184","RIORGES","LOIRE","AUVERGNE-RHONE-ALPES","Point",4.04991,46.059753,"E13 - Blanchiment, teinture, impression"]
["SSP001286301","60.0132","DMS",null,"En cours",null,null,"En cours","60382","MARGNY LES COMPIEGNE","OISE","HAUTS-DE-FRANCE","Point",0.0,0.0,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP001286401","60.0133","saxid",null,"En cours",null,null,"En cours","60009","ALLONNE","OISE","HAUTS-DE-FRANCE","Point",0.0,0.0]
["SSP001286501","42.0209","Becker Industrie",null,"En cours",null,null,"En cours","42299","SAVIGNEUX","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.0907807,45.602207,"D42 - Fabrication de peintures"]
["SSP001286601","60.0134","Total relai franc marché",null,"En cours",null,null,"En cours","60057","BEAUVAIS","OISE","HAUTS-DE-FRANCE","Point",0.0,0.0]
["SSP001286701","60.0135","FRONERI","Cessation des activités Froneri","En cours",null,null,"En cours","60057","BEAUVAIS","OISE","HAUTS-DE-FRANCE","Polygone",2.1225207,49.419918]
["SSP001286801","60.0136","Total",null,"En cours",null,null,"En cours","60138","CHAMANT","OISE","HAUTS-DE-FRANCE","Point",0.0,0.0]
["SSP001286901","60.0137","Station service AS 24",null,"En cours",null,null,"En cours","60151","CHOISY AU BAC","OISE","HAUTS-DE-FRANCE","Point",0.0,0.0,"M1 - Industries diverses"]
["SSP001287001","60.0139","DMS",null,"En cours",null,null,"En cours","60513","PRECY SUR OISE","OISE","HAUTS-DE-FRANCE","Point",0.0,0.0]
["SSP001287101","60.0140","Oise enrobés",null,"En cours",null,null,"En cours","60584","SAINT LEU D'ESSERENT","OISE","HAUTS-DE-FRANCE","Point",0.0,0.0]
["SSP001287201","44.0169","DECODIS SAS",null,"En cours",null,null,"En cours","44023","BOUVRON","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Point",0.0,0.0,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP001287401","49.0082","SUEZ EAU FRANCE (ex- LYONNAISE DES EAUX)",null,"En cours",null,null,"En cours","49099","CHOLET","MAINE-ET-LOIRE","PAYS DE LA LOIRE","Point",-0.8484593,47.024242,"B4 - Production d'eau"]
["SSP001287501","49.0083","PACOBA ENERGIES SERVICES (Ex BAUDENS Louis)",null,"En cours",null,null,"En cours","49328","SAUMUR","MAINE-ET-LOIRE","PAYS DE LA LOIRE","Point",-0.07207361,47.270634,"D13 - Dépôts de pétrole, produits dérivés ou gaz naturel"]
["SSP001287601","72.0085","Ex PHILIPS",null,"En cours",null,null,"En cours","72181","LE MANS","SARTHE","PAYS DE LA LOIRE","Point",-1.3630812,-5.983856]
["SSP001287701","26.0094","ENROBES 26 - ENTREPRISE 26",null,"En cours",null,null,"En cours","26252","PORTES LES VALENCE","DROME","AUVERGNE-RHONE-ALPES","Point",4.887722,44.879147,"G2 - Chantiers, construction, bitumes, enrobés"]
["SSP001288001","94.0116","CHABANY","Cessation totale","En cours",null,null,"En cours","94081","VITRY SUR SEINE","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.4084268,48.791702,null,"59.05 - Commerce de métaux"]
["SSP001288101","44.0170","BOA (anciennement VRAI)",null,"En cours",null,null,"En cours","44192","SAINT VIAUD","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Polygone",-2.0121932,47.279175]
["SSP001288301","60.0141","SIADIS",null,"En cours",null,null,"En cours","60341","LAGNY LE SEC","OISE","HAUTS-DE-FRANCE","Point",0.0,0.0,"K - Déchets et traitements"]
["SSP001288401","60.0142","INTERMARCHE","Cessation des activités","En cours",null,null,"En cours","60103","BRESLES","OISE","HAUTS-DE-FRANCE","Polygone",2.2523031,49.416584]
["SSP001288501","02.0083","ARKEMA FRANCE",null,"En cours",null,null,"En cours","02173","CHAUNY","AISNE","HAUTS-DE-FRANCE","Point",0.0,0.0]
["SSP001288601","43.0018","Eurotransmission",null,"En cours",null,null,"En cours","43224","SAINTE SIGOLENE","HAUTE-LOIRE","AUVERGNE-RHONE-ALPES","Point",4.2298484,45.23551,"H11 - Usinage"]
["SSP001288801","42.0210","LEROY-SOMER SAMOV",null,"Clôturée",null,null,"Clôturée","42059","CHAZELLES SUR LYON","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",4.3900237,45.63583,"J - Sidérurgie, métallurgie, coke"]
["SSP001288901","18.0074","NEXTER Munitions",null,"En cours",null,null,"En cours","18050","LA CHAPELLE SAINT URSIN","CHER","CENTRE-VAL DE LOIRE","Point",2.300279,47.05046,"D8 - Poudres et explosifs"]
["SSP001289001","28.0105","ATELIER 28 - Tremblay les Villages",null,"Clôturée",null,"2020-09-07","Clôturée","28393","TREMBLAY LES VILLAGES","EURE-ET-LOIR","CENTRE-VAL DE LOIRE","Point",1.386998,48.592735]
["SSP001289101","37.0062","AFM RECYCLAGE",null,"En cours",null,null,"En cours","37172","NOTRE DAME D'OE","INDRE-ET-LOIRE","CENTRE-VAL DE LOIRE","Point",0.70619553,47.45955,"K5 - Récupération, dépôts de ferrailles"]
["SSP001289201","67.0257","SARL CHOUCROUTE HESS",null,"Clôturée",null,"2020-08-20","Clôturée","67223","INNENHEIM","BAS-RHIN","GRAND EST","Point",7.5737524,48.497646,"B1 - Industrie agro-alimentaire"]
["SSP001289301","44.0171","SODICHAR (SUPER U)",null,"En cours",null,null,"En cours","44158","SAINT ETIENNE DE MONTLUC","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Polygone",-1.7902745,47.27803,"L23 - Détail de carburants"]
["SSP001289601","67.0258","Transports WEBER","Transport WEBER","En cours",null,null,"En cours","67025","BEINHEIM","BAS-RHIN","GRAND EST","Polygone",8.078882,48.860435]
["SSP001289701","67.0259","Tuileries réunies du Bas-Rhin","Tuileries réunies du Bas-Rhin","En cours",null,null,"En cours","67400","RIEDSELTZ","BAS-RHIN","GRAND EST","Polygone",7.9644685,48.989544]
["SSP001289801","72.0086","M LEGO","Diagnostic","En cours","2020-01-01",null,"En cours","72038","BOESSE LE SEC","SARTHE","PAYS DE LA LOIRE","Polygone",0.57779336,48.124687,null,null,null,"24.44Z - Métallurgie du cuivre"]
["SSP040002301",null,"VEOLIA PROPRETE","Cessation d'activité VEOLIA PROPRETE","Clôturée",null,null,"Clôturée","92050","NANTERRE","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.2100253,48.90726,null,null,null,"38.32Z - Récupération de déchets triés"]
["SSP040003701",null,"AIRBUS GROUP","Cessation d'activité","En cours",null,null,"En cours","92073","SURESNES","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.223374,48.86046,null,null,null,"94.20Z - Activités des syndicats de salariés"]
["SSP040004701",null,"DODIN CAMPENON BERNARD","DODIN Cessation d'activité","Clôturée",null,null,"Clôturée","92050","NANTERRE","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.2306612,48.896908,null,null,"14.2A - Production de sables et de granulats"]
["SSP040004801",null,"RENAULT TRAPEZE ZONE BL1/BL2","Travaux de réhabilitation","En cours",null,null,"En cours","92012","BOULOGNE BILLANCOURT","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.2322438,48.82727,null,null,"34.1Z - Construction de véhicules automobiles"]
["SSP040004901",null,"COMBUSTIBLE DE BOULOGNE","Cessation d'activité","En cours",null,null,"En cours","92012","BOULOGNE BILLANCOURT","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.248725,48.839203,null,null,null,"47.30Z - Commerce de détail de carburants en magasin spécialisé"]
["SSP040005001",null,"SIAAP Usine de pré-traitement","Cessation partielle d'activité","Clôturée",null,null,"Clôturée","92024","CLICHY","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.2957966,48.905304,null,null,"90.0A - Collecte et traitement des eaux usées"]
["SSP040005101",null,"VINCI CONSTRUCTION GRAND PROJET","Cessation d'activité unité de dessablage","Clôturée",null,null,"Clôturée","92020","CHATILLON","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.3020446,48.8113,null,null,"14.2A - Production de sables et de granulats"]
["SSP040005301",null,"ESSO WOREX","WOREX Cessation d'activité","En cours",null,null,"En cours","92023","CLAMART","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.2584834,48.811646,null,null,"50.5Z - Commerce de détail de carburants"]
["SSP040006001",null,"SOLETANCHE BACHY","Cessation d'activité","Clôturée",null,null,"Clôturée","92023","CLAMART","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.2730446,48.813477,"K - Déchets et traitements"]
["SSP040006301",null,"AS24","AS24 Cessation d'activité","Clôturée",null,null,"Clôturée","92036","GENNEVILLIERS","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.2973647,48.940266,null,null,"50.5Z - Commerce de détail de carburants"]
["SSP040006901",null,"ALLO PARIS BENNE LOCATION","APBL Cessation d'activité","Clôturée",null,null,"Clôturée","92036","GENNEVILLIERS","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.316357,48.926556,"K35 - Regroupement, reconditionnement de déchets"]
["SSP040007601",null,"GEODIS ILE DE FRANCE SERVICES","Cessation d'activité partielle","Clôturée",null,null,"Clôturée","92036","GENNEVILLIERS","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.27262,48.937553,null,null,null,"70.22Z - Conseil pour les affaires et autres conseils de gestion"]
["SSP040007701",null,"COMBUSTIBLES MOISSET ET FILS","COMBUSTIBLES MOISSET ET FILS","En cours","2008-09-30",null,"En cours","93005","AULNAY SOUS BOIS","SEINE-SAINT-DENIS","ILE-DE-FRANCE","Polygone",2.4963775,48.927498,null,null,null,"70.10Z - Activités des sièges sociaux"]
["SSP040007801",null,"INOREC","INOREC","Clôturée","2013-07-22",null,"Clôturée","93008","BOBIGNY","SEINE-SAINT-DENIS","ILE-DE-FRANCE","Polygone",2.4250977,48.89899,null,null,null,"46.72Z - Commerce de gros (commerce interentreprises) de minerais et métaux"]
["SSP040007901",null,"PECHARM'","PECHARM'","Clôturée","2007-01-02",null,"Clôturée","93015","COUBRON","SEINE-SAINT-DENIS","ILE-DE-FRANCE","Polygone",2.5643096,48.91767,null,null,null,"47.78C - Autres commerces de détail spécialisés divers"]
["SSP040008201",null,"CIE BRIQUETAGE METALLIQUE POUR FONDERIES","Cessation définitive d'activité","Clôturée",null,null,"Clôturée","93029","DRANCY","SEINE-SAINT-DENIS","ILE-DE-FRANCE","Polygone",2.4594185,48.930565,null,null,null,"38.32Z - Récupération de déchets triés"]
["SSP040008301",null,"BENNES 93","BENNES 93","En cours","1997-05-12",null,"En cours","93057","LES PAVILLONS SOUS BOIS","SEINE-SAINT-DENIS","ILE-DE-FRANCE","Polygone",2.5004857,48.91514,null,null,null,"38.11Z - Collecte des déchets non dangereux"]
["SSP040008501",null,"CHALALA GROUPE","Cessation d'activité","Clôturée",null,null,"Clôturée","92020","CHATILLON","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.2974772,48.80535,null,null,null,"47.30Z - Commerce de détail de carburants en magasin spécialisé"]
["SSP040008801",null,"BP FRANCE","Station-service en activité","Clôturée",null,null,"Clôturée","92071","SCEAUX","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.2798414,48.774734,null,null,null,"46.71Z - Commerce de gros (commerce interentreprises) de combustibles et de produits annexes"]
["SSP040009101",null,"HERTZ FRANCE","HERTZ FRANCE Cessation d'activité","Clôturée",null,null,"Clôturée","92026","COURBEVOIE","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.2415304,48.897324,null,null,null,"77.11A - Location de courte durée de voitures et de véhicules automobiles légers"]
["SSP040009701",null,"Centre technique municipal","Cessation définitive d'activité","Clôturée",null,null,"Clôturée","93007","LE BLANC MESNIL","SEINE-SAINT-DENIS","ILE-DE-FRANCE","Polygone",2.4686363,48.942337,null,null,null,"33.17Z - Réparation et maintenance d'autres équipements de transport"]
["SSP040010001",null,"RESOCLEAN  EUROPE","CLEAN 92 Cessation d'activité","En cours",null,null,"En cours","92078","VILLENEUVE LA GARENNE","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.312208,48.945244,null,null,null,"81.29B - Autres activités de nettoyage n.c.a."]
["SSP040010201",null,"ECO PHU","ECO PHU Cessation d'activité","Clôturée",null,null,"Clôturée","92036","GENNEVILLIERS","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.2867393,48.949406,null,null,null,"38.22Z - Traitement et élimination des déchets dangereux"]
["SSP040010301",null,"SIT'ALTERNATIF","Cessation d'activité","Clôturée",null,null,"Clôturée","92036","GENNEVILLIERS","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.2857435,48.946068,null,null,null,"38.11Z - Collecte des déchets non dangereux"]
["SSP040010401",null,"SINOUHE IMMOBILIER","Cessation d'activité partielle","Clôturée",null,null,"Clôturée","92036","GENNEVILLIERS","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.315136,48.924076,null,null,null,"52.10B - Entreposage et stockage non frigorifique"]
["SSP040010501",null,"Etablissements CAUQUIL","Cessation d'activité","Clôturée",null,null,"Clôturée","92036","GENNEVILLIERS","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.3014152,48.916016,null,null,null,"10.89Z - Fabrication d'autres produits alimentaires n.c.a."]
["SSP040010601",null,"RATP Centre Bus","RATP Cesation d'activité","En cours",null,null,"En cours","92020","CHATILLON","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.302638,48.80381,null,null,"50.5Z - Commerce de détail de carburants"]
["SSP040010701",null,"ENGIE",null,"Clôturée",null,null,"Clôturée","92071","SCEAUX","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.29163,48.779636,null,null,"50.5Z - Commerce de détail de carburants"]
["SSP040010801",null,"Entrepôt HD ex-SOGIM","ENTREPÔT HD EX-SOGIM","Clôturée","2012-01-01",null,"Clôturée","93032","GAGNY","SEINE-SAINT-DENIS","ILE-DE-FRANCE","Polygone",2.5360389,48.880222,null,null,null,"52.10B - Entreposage et stockage non frigorifique"]
["SSP040010901",null,"SIDEC ex-Printemps","SIDEC EX-PRINTEMPS","En cours","1998-06-22",null,"En cours","93039","L'ILE SAINT DENIS","SEINE-SAINT-DENIS","ILE-DE-FRANCE","Polygone",2.3300085,48.922653,null,null,null,"52.10B - Entreposage et stockage non frigorifique"]
["SSP040011001",null,"AIR FRANCE INDUSTRIE","AIR FRANCE INDUSTRIE","En cours","2007-08-21",null,"En cours","93013","LE BOURGET","SEINE-SAINT-DENIS","ILE-DE-FRANCE","Polygone",2.4415178,48.954597,null,null,null,"33.16Z - Réparation et maintenance d'aéronefs et d'engins spatiaux"]
["SSP040011101",null,"Roto Press Numeris","ROTO PRESS NUMERIS","Clôturée","2002-01-14",null,"Clôturée","93046","LIVRY GARGAN","SEINE-SAINT-DENIS","ILE-DE-FRANCE","Polygone",2.54922,48.927185,null,null,"22.2A - Imprimerie de journaux"]
["SSP040011201",null,"FINANCIERE OUSTRY","FINANCIERE OUSTRY","Clôturée","2008-02-14",null,"Clôturée","93047","MONTFERMEIL","SEINE-SAINT-DENIS","ILE-DE-FRANCE","Polygone",2.5561345,48.891247,null,null,"50.5Z - Commerce de détail de carburants"]
["SSP040011301",null,"Hôpital de la maison blanche","HÔPITAL DE LA MAISON BLANCHE","En cours",null,null,"En cours","93050","NEUILLY SUR MARNE","SEINE-SAINT-DENIS","ILE-DE-FRANCE","Polygone",2.544259,48.862705,null,null,"85.1A - Activités hospitalières"]
["SSP040011501",null,"AIRBUS HELICOPTERS","AIRBUS HELICOPTERS","En cours","2017-01-01",null,"En cours","93027","LA COURNEUVE","SEINE-SAINT-DENIS","ILE-DE-FRANCE","Polygone",2.3985827,48.92787,"H13 - Traitement de surface"]
["SSP040011601",null,"TRADEMAT","TRADEMAT","Clôturée","1996-01-01",null,"Clôturée","93013","LE BOURGET","SEINE-SAINT-DENIS","ILE-DE-FRANCE","Polygone",2.420111,48.93053,"K35 - Regroupement, reconditionnement de déchets"]
["SSP040011701",null,"EUROGRAVURE","EUROGRAVURE","En cours","2005-10-24",null,"En cours","93048","MONTREUIL","SEINE-SAINT-DENIS","ILE-DE-FRANCE","Polygone",2.4333706,48.85352,"H21 - Imprimerie, presse, édition"]
["SSP040011801",null,"Carrefour station service","CARREFOUR STATION SERVICE","En cours","2019-08-12",null,"En cours","93048","MONTREUIL","SEINE-SAINT-DENIS","ILE-DE-FRANCE","Polygone",2.4173355,48.85554,null,null,"50.5Z - Commerce de détail de carburants"]
["SSP040011901",null,"OPESLIA","OPESLIA Cessation d'activité","Clôturée","2020-03-31","2021-01-11","Clôturée","92036","GENNEVILLIERS","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.299936,48.948532,null,null,null,"46.77Z - Commerce de gros (commerce interentreprises) de déchets et débris"]
["SSP040012301",null,"ZAC des Bruyères Sud","Réaménagement du site","Clôturée",null,null,"Clôturée","92009","BOIS COLOMBES","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.2631266,48.906315,null,null,null,"68.10Z - Activités des marchands de biens immobiliers"]
["SSP040012701",null,"Centre technique du Conseil Général n°2","Cessation d'activité","En cours",null,null,"En cours","92050","NANTERRE","HAUTS-DE-SEINE","ILE-DE-FRANCE","Polygone",2.1910386,48.894833,null,null,null,"47.30Z - Commerce de détail de carburants en magasin spécialisé"]
["SSP040019601",null,"SAFI","SAFI Cessation d'activité","En cours",null,null,"En cours","94028","CRETEIL","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.4583993,48.79527,null,null,null,"45.11Z - Commerce de voitures et de véhicules automobiles légers"]
["SSP040019701",null,"ESSO SOCIETE ANONYME FRANCAISE","ESSO SAF Cessation d'activité","Clôturée",null,null,"Clôturée","94068","SAINT MAUR DES FOSSES","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.5066898,48.796658,null,null,null,"19.20Z - Raffinage du pétrole"]
["SSP040019801",null,"SERVICE INCINERATION D'ANIMAUX FAMILIERS","SIAF Cessation d'activité","Clôturée",null,null,"Clôturée","94052","NOGENT SUR MARNE","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.4810858,48.8408,null,null,null,"96.03Z - Services funéraires"]
["SSP040020001",null,"ETABLISSEMENTS RENE RAOUX","RENE RAOUX Cessation","En cours",null,null,"En cours","94002","ALFORTVILLE","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.4284537,48.798443,null,null,null,"38.32Z - Récupération de déchets triés"]
["SSP040020401",null,"AFB ENTREPRISE FERNANDES","AFB ","En cours",null,null,"En cours","94078","VILLENEUVE SAINT GEORGES","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.4693458,48.737423,null,null,null,"77.32Z - Location et location-bail de machines et équipements pour la construction"]
["SSP040020501",null,"BANQUE DE FRANCE","Banque de France Cessation","Clôturée",null,null,"Clôturée","94041","IVRY SUR SEINE","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.3894207,48.823162,null,null,null,"64.11Z - Activités de banque centrale"]
["SSP040020801",null,"SOCIETE D'APPLICATIONS DE BREVETS","SAB Cessation d'activité","Clôturée",null,null,"Clôturée","94016","CACHAN","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.327413,48.79955,null,null,null,"25.61Z - Traitement et revêtement des métaux"]
["SSP040020901",null,"ACTIVITE VILLENEUVOISE DE RECUPERATION","AVIREC Cessation d'activité","En cours",null,null,"En cours","94077","VILLENEUVE LE ROI","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.427762,48.732502,null,null,null,"38.32Z - Récupération de déchets triés"]
["SSP040021001",null,"CASTEL FRERES","CASTEL FRERES Cessation d'activité","En cours",null,null,"En cours","94073","THIAIS","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.371135,48.750965,null,null,null,"46.34Z - Commerce de gros (commerce interentreprises) de boissons"]
["SSP040021101",null,"SOGARIS Paris Sud","SOGARIS Cessation partielle","En cours",null,null,"En cours","94028","CRETEIL","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.4311023,48.777607,"L23 - Détail de carburants"]
["SSP040021201",null,"BSPP","BSPP Cessation partielle","En cours",null,null,"En cours","94028","CRETEIL","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.4577682,48.786377,null,null,"50.5Z - Commerce de détail de carburants"]
["SSP040021301",null,"ERDF","ERDF acte de malveillance","En cours",null,null,"En cours","94017","CHAMPIGNY SUR MARNE","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.5289795,48.812008,"K35 - Regroupement, reconditionnement de déchets"]
["SSP040021401",null,"ENGELHARD","ENGHELHARD Cessation d'activité","Clôturée",null,null,"Clôturée","94041","IVRY SUR SEINE","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.3984063,48.816963,"J34 - Métallurgie des métaux précieux"]
["SSP040021501",null,"MONOPRIX EXPLOITATION, PAR ABREVIATION MPX",null,"En cours",null,null,"En cours","94071","SUCY EN BRIE","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.5181084,48.7725,null,null,null,"47.11E - Magasins multi-commerces"]
["SSP040021601",null,"APHP Jean Rostand","APHP Jean Rostand Cessation d'activité","Clôturée",null,null,"Clôturée","94041","IVRY SUR SEINE","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.3787827,48.813343,null,null,null,"86.10Z - Activités hospitalières"]
["SSP040021701",null,"Marie d'Ivry (ateliers municipaux)","Cessation d'activité","En cours",null,null,"En cours","94041","IVRY SUR SEINE","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.3983657,48.81324,null,null,"50.5Z - Commerce de détail de carburants"]
["SSP040021801",null,"RIVP-IVRY","RIVP-IVRY Cessation d'activité","Clôturée",null,null,"Clôturée","94041","IVRY SUR SEINE","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.380069,48.802277,"I21 - Chaufferies urbaines"]
["SSP040022601",null,"UNION DES COMPAGNONS PAVEURS  UCP","Cessation d'activité","En cours",null,null,"En cours","94011","BONNEUIL SUR MARNE","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.5009024,48.783447,null,null,null,"42.11Z - Construction de routes et autoroutes"]
["SSP040023001",null,"SUBURBAINE CANALISATIONS GRANDS TRAVAUX","SPAC Cessation d'activité","En cours",null,null,"En cours","94081","VITRY SUR SEINE","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.4067957,48.777576,null,null,null,"42.21Z - Construction de réseaux pour fluides"]
["SSP040023101",null,"DEPOTS ELECTROLYTIQUES DU CENTRE","DELCEN Cessation d'activité","Clôturée",null,null,"Clôturée","94081","VITRY SUR SEINE","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.4061193,48.806114,null,null,null,"25.61Z - Traitement et revêtement des métaux"]
["SSP040023501",null,"SUEZ RV ILE-DE-FRANCE","SUEZ RV Cessation d'activité","En cours",null,null,"En cours","94041","IVRY SUR SEINE","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.3891153,48.82163,null,null,null,"38.11Z - Collecte des déchets non dangereux"]
["SSP040023601",null,"E. LECLERC","Signalement d'une pollution","En cours",null,null,"En cours","94043","LE KREMLIN BICETRE","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.3620741,48.807537,null,null,"50.5Z - Commerce de détail de carburants"]
["SSP040023701",null,"Christian DUTEY","DUTEY Cessation d'activité","Clôturée",null,null,"Clôturée","94077","VILLENEUVE LE ROI","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.4281123,48.732147,"K35 - Regroupement, reconditionnement de déchets"]
["SSP040023801",null,"RFM 94","RFM 94 activité illégale","Clôturée",null,null,"Clôturée","94077","VILLENEUVE LE ROI","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.435794,48.7401,"K5 - Récupération, dépôts de ferrailles"]
["SSP040023901",null,"ABTP","ABTP Cessation d'activité","Clôturée",null,null,"Clôturée","94071","SUCY EN BRIE","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.5020678,48.76658,"K2 - Traitement de déchets urbains"]
["SSP040024001",null,"TOTAL - Relais de Rungis","Fuite de carburant","Clôturée",null,null,"Clôturée","94021","CHEVILLY LARUE","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.35868,48.76412,null,null,"50.5Z - Commerce de détail de carburants"]
["SSP040024101",null,"MANUFACTURE KERING EYEWEAR","Réhabilitation du site avant construction","Clôturée",null,null,"Clôturée","94071","SUCY EN BRIE","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.498955,48.7659,"H13 - Traitement de surface"]
["SSP040024201",null,"GBC ALTMAYER","Incident- Déversement","Clôturée",null,null,"Clôturée","94081","VITRY SUR SEINE","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.3753748,48.79831,null,null,"52.4Y - Commerce de détail de charbons et combustibles"]
["SSP040024301",null,"COVED POINT E","Cessation d'activité","En cours","2019-06-05",null,"En cours","94021","CHEVILLY LARUE","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.3471272,48.76484,null,null,null,"38.11Z - Collecte des déchets non dangereux"]
["SSP040024701",null,"PRIGENT TRANSPORTS","PRIGENT TRANSPORT Cessation d'activité","En cours",null,null,"En cours","94019","CHENNEVIERES SUR MARNE","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.543163,48.797855,null,null,null,"49.41A - Transports routiers de fret interurbains"]
["SSP040024901",null,"PECHAUD, MARCEL","PECHAUD","En cours",null,null,"En cours","94071","SUCY EN BRIE","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.5105565,48.77521,null,null,null,"68.20B - Location de terrains et d'autres biens immobiliers"]
["SSP040025001",null,"MANSO, JOSE","AUTO MANSO Cessation d'activité","En cours",null,null,"En cours","94017","CHAMPIGNY SUR MARNE","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.5463274,48.808556,null,null,null,"45.32Z - Commerce de détail d'équipements automobiles"]
["SSP040025101",null,"VALMAR",null,"En cours",null,null,"En cours","94022","CHOISY LE ROI","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.41384,48.770477,null,null,null,"45.11Z - Commerce de voitures et de véhicules automobiles légers"]
["SSP040025201",null,"SANOFI WINTHROP INDUSTRIE","SANOFI","En cours",null,null,"En cours","94046","MAISONS ALFORT","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.4332433,48.79456,null,null,null,"21.20Z - Fabrication de préparations pharmaceutiques"]
["SSP040025301",null,"ARGENTURE BELARBI",null,"En cours",null,null,"En cours","94076","VILLEJUIF","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.3648062,48.80031,null,null,null,"32.12Z - Fabrication d'articles de joaillerie et bijouterie"]
["SSP040025401",null,"SOCIETE DES ETABLISSEMENTS PIERRE ABATE","ABATE ","Clôturée",null,null,"Clôturée","94076","VILLEJUIF","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.3687527,48.793304,null,null,null,"46.73A - Commerce de gros (commerce interentreprises) de bois et de matériaux de construction"]
["SSP040025501",null,"ELIDEC","ELIDEC Cessation","En cours",null,null,"En cours","94070","SANTENY","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.566775,48.716602,null,null,null,"38.12Z - Collecte des déchets dangereux"]
["SSP040025601",null,"DEPARTEMENT DU VAL DE MARNE","Hotel du département du Val-de-Marne","En cours",null,null,"En cours","94028","CRETEIL","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.4512906,48.781693,null,null,null,"84.11Z - Administration publique générale"]
["SSP040025701",null,"EPOXY DE LA BRIE","EPOXY DE LA BRIE","En cours",null,null,"En cours","77193","FORFRY","SEINE-ET-MARNE","ILE-DE-FRANCE","Polygone",2.8547037,49.055508,null,null,null,"25.61Z - Traitement et revêtement des métaux"]
["SSP040026001",null,"OSBORN METALS SAS","OSBORN METALS SAS","En cours","1980-01-01",null,"En cours","77284","MEAUX","SEINE-ET-MARNE","ILE-DE-FRANCE","Polygone",2.9127808,48.960564,null,null,null,"24.20Z - Fabrication de tubes, tuyaux, profilés creux et accessoires correspondants en acier"]
["SSP040027901",null,"CPCU","Pollution historique ","Clôturée",null,null,"Clôturée","94081","VITRY SUR SEINE","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.4163182,48.78906,"I21 - Chaufferies urbaines"]
["SSP040028001",null,"RIVP-VITRY","Cessation d'activité","Clôturée",null,null,"Clôturée","94081","VITRY SUR SEINE","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.3822007,48.802273,null,null,null,"52.10B - Entreposage et stockage non frigorifique"]
["SSP040028101",null,"LGD Developpement","LGD Developpement ","Clôturée",null,null,"Clôturée","94044","LIMEIL BREVANNES","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.4731996,48.754013,"K2 - Traitement de déchets urbains"]
["SSP040028201",null,"Super U (ex-Atac)","SUPER U (EX ATAC)","Clôturée",null,null,"Clôturée","94044","LIMEIL BREVANNES","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.489182,48.75087,null,null,"50.5Z - Commerce de détail de carburants"]
["SSP040028301",null,"TOTAL AZUR","TOTAL AZUR ","Clôturée",null,null,"Clôturée","94017","CHAMPIGNY SUR MARNE","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.4926603,48.822994,null,null,"50.5Z - Commerce de détail de carburants"]
["SSP040028401",null,"EXTRACT ECOTERRES","EXTRACT-ECOTERRES Cessation","En cours",null,null,"En cours","94011","BONNEUIL SUR MARNE","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.4985762,48.778633,"K3 - Traitement de déchets industriels"]
["SSP040028501",null,"SOFRILOG RUNGIS","SOFRILOG Cessation","Clôturée",null,null,"Clôturée","94065","RUNGIS","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.3590117,48.751682,null,null,null,"52.10A - Entreposage et stockage frigorifique"]
["SSP040028601",null,"SETBO","SETBO Cessation partielle","Clôturée",null,null,"Clôturée","94011","BONNEUIL SUR MARNE","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.4824076,48.771633,"I21 - Chaufferies urbaines"]
["SSP040028701",null,"VELLARD","VELLARD","En cours",null,"2015-06-03","En cours","77053","BRIE COMTE ROBERT","SEINE-ET-MARNE","ILE-DE-FRANCE","Polygone",2.6092486,48.69087,"E3 - Laveries, blanchisseries, pressing"]
["SSP040028801",null,"ELIA Médical","ELIA Médical","Clôturée","2005-09-07","2015-12-15","Clôturée","77053","BRIE COMTE ROBERT","SEINE-ET-MARNE","ILE-DE-FRANCE","Polygone",2.6172774,48.70233,"D21 - Stockage et conditionnement des gaz et liquéfiés"]
["SSP040028901",null,"TOTAL","TOTAL","En cours","1984-11-05","1992-12-17","En cours","77118","CLAYE SOUILLY","SEINE-ET-MARNE","ILE-DE-FRANCE","Polygone",2.7068398,48.94817,null,null,"50.5Z - Commerce de détail de carburants"]
["SSP040029001",null,"WIPELEC","WIPELEC","En cours","2003-01-01","2012-01-01","En cours","77243","LAGNY SUR MARNE","SEINE-ET-MARNE","ILE-DE-FRANCE","Polygone",2.686973,48.87582,"H13 - Traitement de surface"]
["SSP040029101",null,"BP","BP","En cours","1973-01-01",null,"En cours","77284","MEAUX","SEINE-ET-MARNE","ILE-DE-FRANCE","Polygone",2.879253,48.946774,null,null,"50.5Z - Commerce de détail de carburants"]
["SSP040029201",null,"BP","BP","En cours",null,null,"En cours","77284","MEAUX","SEINE-ET-MARNE","ILE-DE-FRANCE","Polygone",2.8833437,48.957554,null,null,"50.5Z - Commerce de détail de carburants"]
["SSP040029301",null,"SGRO Tranding Franc (ex IPBM)","SEGRO TRADING FRANCE","En cours","2013-07-16","2015-11-04","En cours","77294","MITRY MORY","SEINE-ET-MARNE","ILE-DE-FRANCE","Polygone",2.6415296,48.98087,null,null,null,"52.10B - Entreposage et stockage non frigorifique"]
["SSP040029501",null,"ROSSI","ROSSI","En cours",null,null,"En cours","77305","MONTEREAU FAULT YONNE","SEINE-ET-MARNE","ILE-DE-FRANCE","Polygone",2.9728887,48.384285,null,null,null,"38.11Z - Collecte des déchets non dangereux"]
["SSP040029801",null,"EAUX de MELUN","EAUX de MELUN","En cours","1988-12-05","2015-03-01","En cours","77445","SAVIGNY LE TEMPLE","SEINE-ET-MARNE","ILE-DE-FRANCE","Polygone",2.580803,48.60582,null,null,null,"37.00Z - Collecte et traitement des eaux usées"]
["SSP040030001",null,"SOCAME (ex-BUDANT)","SOCAME","En cours","1973-01-01",null,"En cours","77495","VERT SAINT DENIS","SEINE-ET-MARNE","ILE-DE-FRANCE","Polygone",2.62524,48.58443,null,null,"24.3Z - Fabrication de peintures et vernis"]
["SSP040030601",null,"Décharge municipale","Décharge municpale","En cours","1975-01-10",null,"En cours","77312","MONTIGNY SUR LOING","SEINE-ET-MARNE","ILE-DE-FRANCE","Polygone",2.7506266,48.3455,"K21 - Décharges d'ordures ménagères"]
["SSP040030901",null,"SUCCESSIF","SUCCESSIF Cessation","En cours",null,null,"En cours","94073","THIAIS","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.369779,48.760952,null,null,null,"45.11Z - Commerce de voitures et de véhicules automobiles légers"]
["SSP040031001",null,"SABRIE SA",null,"En cours",null,null,"En cours","94080","VINCENNES","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.4337487,48.84465,null,null,null,"45.11Z - Commerce de voitures et de véhicules automobiles légers"]
["SSP040031101",null,"GIBERT FRERES","GIBERT FRERES Cessation","En cours",null,null,"En cours","94017","CHAMPIGNY SUR MARNE","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.5489485,48.81151,null,null,null,"47.78B - Commerces de détail de charbons et combustibles"]
["SSP040031201",null,"RECUP AUTO S A R L","RECUP AUTO Cessation","En cours",null,null,"En cours","94017","CHAMPIGNY SUR MARNE","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.536884,48.814228,null,null,null,"38.32Z - Récupération de déchets triés"]
["SSP040031301",null,"GROUPE SPR","Groupe SPR Cessation","En cours",null,null,"En cours","94041","IVRY SUR SEINE","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.3928185,48.82079,null,null,null,"70.10Z - Activités des sièges sociaux"]
["SSP040032201",null,"T.D-DISTRIBUTION THEVENIN-DUCROT-DISTRIBUTION","AVIA THEVENIN-DUCROT Cessation","En cours",null,null,"En cours","94077","VILLENEUVE LE ROI","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.4206154,48.731365,null,null,null,"46.71Z - Commerce de gros (commerce interentreprises) de combustibles et de produits annexes"]
["SSP040032401",null,"CHEVILLY AUTOS SPORTS","CHEVILLY AUTOS SPORT Cessation","En cours",null,null,"En cours","94021","CHEVILLY LARUE","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.3677793,48.761726,null,null,null,"45.11Z - Commerce de voitures et de véhicules automobiles légers"]
["SSP040032501",null,"REVIVAL ILE DE FRANCE FERS ET METAUX","REVIVAL Cessation","En cours",null,null,"En cours","94011","BONNEUIL SUR MARNE","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.490331,48.77841,null,null,null,"68.20B - Location de terrains et d'autres biens immobiliers"]
["SSP040032701",null,"RENNOTTE","RENNOTTE Cessation","En cours",null,null,"En cours","94018","CHARENTON LE PONT","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.403357,48.828487,null,null,null,"25.61Z - Traitement et revêtement des métaux"]
["SSP040032801",null,"FLOREAL","FLOREAL Cessation","En cours",null,null,"En cours","94004","BOISSY SAINT LEGER","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.5026894,48.752506,null,null,null,"47.30Z - Commerce de détail de carburants en magasin spécialisé"]
["SSP040032901",null,"RECUTIL","RECUTIL","En cours",null,null,"En cours","77390","ROISSY EN BRIE","SEINE-ET-MARNE","ILE-DE-FRANCE","Polygone",2.6825225,48.78334,"K52 - Dépôts de ferraille"]
["SSP040034001",null,"ELECTRICITE DE FRANCE","EDF CPT Cessation","En cours",null,null,"En cours","94081","VITRY SUR SEINE","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.415267,48.790756,null,null,null,"35.11Z - Production d'électricité"]
["SSP040034101",null,"TDR","TDR Cessation","Clôturée",null,null,"Clôturée","94081","VITRY SUR SEINE","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.4069636,48.780556,"L2 - Transports, automobile, carburants"]
["SSP040034201",null,"TOTAL SUCY","Cessation d'activité","Clôturée",null,null,"Clôturée","94071","SUCY EN BRIE","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.5046496,48.77304,null,null,"50.5Z - Commerce de détail de carburants"]
["SSP040034301",null,"DAVLI","DAVLI Cessation","En cours",null,null,"En cours","94081","VITRY SUR SEINE","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.4066234,48.779682,null,null,null,"52.10B - Entreposage et stockage non frigorifique"]
["SSP040034401",null,"EIFFAGE Fondations","EIFFAGE FONDATIONS Cessation","En cours",null,null,"En cours","94079","VILLIERS SUR MARNE","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.5289805,48.823498,"G14 - Fabrication d'autres matériaux de construction"]
["SSP040034501",null,"SOLETACNHE BACHY","Cessation d'activité","Clôturée",null,null,"Clôturée","94081","VITRY SUR SEINE","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.416165,48.785393,null,null,"29.5D - Fabrication de matériels de travaux publics"]
["SSP040034801",null,"ETABLISSEMENTS MARAIS","MARAIS Cessation","Clôturée",null,null,"Clôturée","94054","ORLY","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.3963335,48.741604,null,null,"50.2Z - Entretien et réparation de véhicules automobiles"]
["SSP040034901",null,"BRASSE DEMENAGEMENTS","Cessation d'activité","Clôturée",null,null,"Clôturée","94016","CACHAN","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.342719,48.79655,null,null,"50.5Z - Commerce de détail de carburants"]
["SSP040035001",null,"AUCHAN SUPERMARCHE","AUCHAN/ SIMPLY MARKET- Cessation","En cours",null,null,"En cours","94081","VITRY SUR SEINE","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.3922033,48.78422,null,null,null,"47.11D - Supermarchés"]
["SSP040035301",null,"WIAME VRD","WIAME VRD","En cours","2013-05-06",null,"En cours","77282","MAUREGARD","SEINE-ET-MARNE","ILE-DE-FRANCE","Polygone",2.5744557,49.023476,null,null,"14.2A - Production de sables et de granulats"]
["SSP040035601",null,"SNCF VOYAGEURS","SNCF COMBUSTIBLE Cessation station-service","En cours",null,null,"En cours","94078","VILLENEUVE SAINT GEORGES","VAL-DE-MARNE","ILE-DE-FRANCE","Polygone",2.4368527,48.75056,null,null,null,"49.10Z - Transport ferroviaire interurbain de voyageurs"]
["SSP040041101",null,"COLLECTES VALORISATION ENERGIE DECHETS - COVED","COVED Cessation","En cours",null,null,"En cours","95018","ARGENTEUIL","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.213035,48.946384,null,null,null,"38.11Z - Collecte des déchets non dangereux"]
["SSP040041601",null,"ORANGE FRANCE","FRANCE TELECOM Cessation","Clôturée",null,null,"Clôturée","95018","ARGENTEUIL","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.247444,48.952053,null,null,null,"61.20Z - Télécommunications sans fil"]
["SSP040044301",null,"MOUROT INDUSTRIE","MOUROT Cessation","En cours",null,null,"En cours","95018","ARGENTEUIL","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.2218463,48.93696,null,null,null,"25.62B - Mécanique industrielle"]
["SSP040044501",null,"PIONEER FRANCE","PIONEER","Clôturée",null,null,"Clôturée","95018","ARGENTEUIL","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.2368183,48.93234,null,null,null,"46.43Z - Commerce de gros (commerce interentreprises) d'appareils électroménagers"]
["SSP040044601",null,"RM DISTRIBUTION","RM Distribution Cessation","Clôturée",null,null,"Clôturée","95018","ARGENTEUIL","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.2206562,48.950428,null,null,null,"46.73B - Commerce de gros (commerce interentreprises) d'appareils sanitaires et de produits de décoration"]
["SSP040044801",null,"SESEM","SESEM Cessation","Clôturée",null,null,"Clôturée","95018","ARGENTEUIL","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.2302978,48.928955,null,null,"28.5A - Traitement et revêtement des métaux"]
["SSP040044901",null,"SARL SOVULREP","SOLVUREP Cessation","Clôturée",null,null,"Clôturée","95018","ARGENTEUIL","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.2405372,48.93614,null,null,"25.1C - Rechapage de pneumatiques"]
["SSP040045101",null,"SYNDICAT MIXTE POUR LA COLLECTE ET LE TRAITEMENT DES EAUX USEES DANS LES BASSINS DE THEVE ET DE L'YSIEUX (SICTEUB)","SICTEUB Déclassement","Clôturée",null,null,"Clôturée","95026","ASNIERES SUR OISE","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.3561628,49.139393,null,null,null,"84.11Z - Administration publique générale"]
["SSP040045201",null,"BERNES AUTOS PIECES","BERNES AUTOS PIECES Activité non autorisée","Clôturée",null,null,"Clôturée","95058","BERNES SUR OISE","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.292047,49.154472,null,null,null,"45.31Z - Commerce de gros d'équipements automobiles"]
["SSP040045401",null,"ETABLISSEMENTS G. FERRANT","Etablissements FERRANT Cessation","En cours",null,null,"En cours","95063","BEZONS","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.204398,48.927044,null,null,null,"25.61Z - Traitement et revêtement des métaux"]
["SSP040045501",null,"J.L.B. AUTOMOBILES","JLB AUTOMOBILES Cessation","En cours",null,null,"En cours","95063","BEZONS","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.213475,48.929012,null,null,null,"45.11Z - Commerce de voitures et de véhicules automobiles légers"]
["SSP040045601",null,"SOC EUROPEENNE DE PRODUITS DE BEAUTE","REVLON Cessation","Clôturée",null,null,"Clôturée","95063","BEZONS","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.2125719,48.917534,null,null,null,"46.45Z - Commerce de gros (commerce interentreprises) de parfumerie et de produits de beauté"]
["SSP040045701",null,"RIBER","RIBER Cessation","Clôturée",null,null,"Clôturée","95063","BEZONS","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.2117841,48.921032,null,null,null,"28.99B - Fabrication d'autres machines spécialisées"]
["SSP040045901",null,"SCANIA ILE DE FRANCE","SCANIA Cessation","En cours",null,null,"En cours","95063","BEZONS","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.2055097,48.91768,null,null,"70.2C - Location d'autres biens immobiliers"]
["SSP040046001",null,"ZEBRA APPLICATIONS","ZEBRA APPLICATIONS Cessation","Clôturée",null,null,"Clôturée","95063","BEZONS","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.2280974,48.929077,null,null,null,"42.11Z - Construction de routes et autoroutes"]
["SSP040046401",null,"GUIZIER RECYCLAGE","GUIZIER RECYCLAGE Cessation","Clôturée",null,null,"Clôturée","95078","BOISSY L'AILLERIE","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.0184333,49.07754,null,null,null,"46.69B - Commerce de gros (commerce interentreprises) de fournitures et équipements industriels divers"]
["SSP040047401",null,"PLANETE BOIS FRANCILIEN","PLANETE BOIS FRANCILIEN Cessation","Clôturée",null,null,"Clôturée","95116","BRUYERES SUR OISE","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.3314095,49.14917,null,null,null,"38.32Z - Récupération de déchets triés"]
["SSP040047501",null,"SCEA H LEVESQUE ET FILS","SCEA H LEVESQUES ET FILS Dépôts liquides inflammables","En cours",null,null,"En cours","95169","COMMENY","VAL-D'OISE","ILE-DE-FRANCE","Polygone",1.8923848,49.12767,null,null,null,"01.47Z - Élevage de volailles"]
["SSP040047601",null,"FROMAGERIES BEL PRODUCTION FRANCE","Diagnostic","Clôturée","2010-01-01",null,"Clôturée","72132","LA FERTE BERNARD","SARTHE","PAYS DE LA LOIRE","Polygone",0.6379579,48.185932,null,null,null,"10.51C - Fabrication de fromage"]
["SSP040047701",null,"PINEIX, BERNARD","BERNARD AUTO","En cours",null,null,"En cours","78073","BOIS D'ARCY","YVELINES","ILE-DE-FRANCE","Polygone",2.0380943,48.80222,null,null,null,"45.32Z - Commerce de détail d'équipements automobiles"]
["SSP040047801",null,"AUCHAN HYPERMARCHE","AUCHAN France","Clôturée","2002-10-31",null,"Clôturée","78118","BUCHELAY","YVELINES","ILE-DE-FRANCE","Polygone",1.6866537,48.97929,null,null,null,"47.11F - Hypermarchés"]
["SSP040047901",null,"D.B.P.A","D.B.P.A","En cours",null,null,"En cours","78124","CARRIERES SUR SEINE","YVELINES","ILE-DE-FRANCE","Polygone",2.1823869,48.906277,null,null,null,"45.11Z - Commerce de voitures et de véhicules automobiles légers"]
["SSP040048001",null,"STOJAKOVIC, MARKO","STOJAKOVIC pressing","Clôturée","2002-07-05",null,"Clôturée","78146","CHATOU","YVELINES","ILE-DE-FRANCE","Polygone",2.1488883,48.901142,null,null,null,"74.90B - Activités spécialisées, scientifiques et techniques diverses"]
["SSP040048101",null,"STE MAS","MAS Cessation","Clôturée",null,null,"Clôturée","95241","FONTENAY EN PARISIS","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.4517345,49.041718,null,null,null,"77.39Z - Location et location-bail d'autres machines, équipements et biens matériels n.c.a."]
["SSP040048201",null,"SYNDICAT MIXTE DE LA REGION DE RAMBOUILLET","Cessation d'activité","Clôturée",null,null,"Clôturée","78517","RAMBOUILLET","YVELINES","ILE-DE-FRANCE","Polygone",1.8244826,48.624195,null,null,null,"84.11Z - Administration publique générale"]
["SSP040048301",null,"BOUSTANY AUTOMOBILES","BOUSTANY AUTOMOBILES","En cours",null,null,"En cours","78311","HOUILLES","YVELINES","ILE-DE-FRANCE","Polygone",2.1875558,48.92907,null,null,null,"45.11Z - Commerce de voitures et de véhicules automobiles légers"]
["SSP040048401",null,"R.A.S.","RAS (Ex MOBIL OIL) Cessation","En cours",null,null,"En cours","95252","FRANCONVILLE","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.2257648,48.985264,null,null,null,"45.20A - Entretien et réparation de véhicules automobiles légers"]
["SSP040048501",null,"BAUMGARTHEN, JOSEPH","BAUMGARTHEN","En cours",null,null,"En cours","78327","JUZIERS","YVELINES","ILE-DE-FRANCE","Polygone",1.8339148,48.98926,null,null,null,"43.39Z - Autres travaux de finition"]
["SSP040048601",null,"PRESSING SAINTE CLAIRE","PRESSING SAINTE CLAIRE","En cours",null,null,"En cours","78126","LA CELLE SAINT CLOUD","YVELINES","ILE-DE-FRANCE","Polygone",2.1468732,48.852634,null,null,null,"96.01B - Blanchisserie-teinturerie de détail"]
["SSP040048701",null,"ELYSEE VILLAGE RETOUCHES ET PRESSING","ELYSEE VILLAGE RETOUCHES ET PRESSING","En cours",null,null,"En cours","78126","LA CELLE SAINT CLOUD","YVELINES","ILE-DE-FRANCE","Polygone",2.1488225,48.85985,null,null,null,"96.01B - Blanchisserie-teinturerie de détail"]
["SSP040048801",null,"PAREA","PAREA","En cours",null,null,"En cours","78486","LE PERRAY EN YVELINES","YVELINES","ILE-DE-FRANCE","Polygone",1.8464006,48.68417,null,null,null,"47.30Z - Commerce de détail de carburants en magasin spécialisé"]
["SSP040048901",null,"CMA CARBURANTS","CMA CARBURANTS","En cours","1989-05-29","2015-07-24","En cours","78650","LE VESINET","YVELINES","ILE-DE-FRANCE","Polygone",2.1241348,48.8998,null,null,null,"47.30Z - Commerce de détail de carburants en magasin spécialisé"]
["SSP040049001",null,"SARL RSA RELAIS SERVICES AUTOMOBILES","SARL RSA RELAIS SERVICES AUTOMOBILES","En cours",null,null,"En cours","78354","MAGNANVILLE","YVELINES","ILE-DE-FRANCE","Polygone",1.6923149,48.976784,null,null,null,"45.11Z - Commerce de voitures et de véhicules automobiles légers"]
["SSP040049101",null,"ALLO TRANSPRESSING","ALLO TRANSPRESSING","En cours",null,null,"En cours","78498","POISSY","YVELINES","ILE-DE-FRANCE","Polygone",2.0485778,48.92443,null,null,null,"96.01B - Blanchisserie-teinturerie de détail"]
["SSP040049301",null,"ASTON","ASTON","En cours",null,null,"En cours","78557","SAINT HILARION","YVELINES","ILE-DE-FRANCE","Polygone",1.6876019,48.613674,null,null,null,"47.30Z - Commerce de détail de carburants en magasin spécialisé"]
["SSP040049401",null,"CYCLADIS","CYCLADIS","Clôturée",null,null,"Clôturée","78586","SARTROUVILLE","YVELINES","ILE-DE-FRANCE","Polygone",2.1851199,48.945675,null,null,null,"38.32Z - Récupération de déchets triés"]
["SSP040049601",null,"BELLO AUTOMOBILES","BELLO AUTOMOBILES","Clôturée",null,null,"Clôturée","78586","SARTROUVILLE","YVELINES","ILE-DE-FRANCE","Polygone",2.164247,48.941307,null,null,null,"45.11Z - Commerce de voitures et de véhicules automobiles légers"]
["SSP040049701",null,"FREMIPRESS","FREMIPRESS","Clôturée",null,null,"Clôturée","95306","HERBLAY","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.165686,48.988537,null,null,null,"96.01A - Blanchisserie-teinturerie de gros"]
["SSP040049801",null,"IMPRESSIONS & SERVICES","IMPRESSIONS & SERVICES Cessation","En cours",null,null,"En cours","95306","HERBLAY","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.1184618,49.025883,null,null,null,"18.12Z - Autre imprimerie (labeur)"]
["SSP040049901",null,"SCI POTET","SCI POTET","En cours",null,null,"En cours","78586","SARTROUVILLE","YVELINES","ILE-DE-FRANCE","Polygone",2.2002735,48.941322,null,null,null,"68.20A - Location de logements"]
["SSP040050001",null,"CACHERA, JEAN","CACHERA","En cours","1989-09-27","2015-05-28","En cours","78591","SEPTEUIL","YVELINES","ILE-DE-FRANCE","Polygone",1.677697,48.897877,null,"65.02 - Commerce de détail de carburants et lubrifiants"]
["SSP040050101",null,"EADS ASTRIUM SAS","EADS ASTRIUM SAS","Clôturée",null,null,"Clôturée","78640","VELIZY VILLACOUBLAY","YVELINES","ILE-DE-FRANCE","Polygone",2.1796753,48.781612,null,null,"35.3C - Construction de lanceurs et engins spatiaux"]
["SSP040050201",null,"ALMA","BP","Clôturée",null,null,"Clôturée","78646","VERSAILLES","YVELINES","ILE-DE-FRANCE","Polygone",2.1528327,48.804573,null,null,null,"47.30Z - Commerce de détail de carburants en magasin spécialisé"]
["SSP040050301",null,"PRESSING GRAND SIECLE","PRESSING GRAND SIECLE","Clôturée",null,null,"Clôturée","78646","VERSAILLES","YVELINES","ILE-DE-FRANCE","Polygone",2.157156,48.80397,null,null,null,"96.01B - Blanchisserie-teinturerie de détail"]
["SSP040050401",null,"NEXTER SYSTEMS","NEXTER SYSTEMS","En cours",null,null,"En cours","78646","VERSAILLES","YVELINES","ILE-DE-FRANCE","Polygone",2.091713,48.78512,null,null,null,"30.40Z - Construction de véhicules militaires de combat"]
["SSP040050601",null,"GROUPAGE IMPORTATION PNEUMATIQUE","GIP Cessation","Clôturée",null,null,"Clôturée","95257","LA FRETTE SUR SEINE","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.1725292,48.971558,null,null,null,"45.31Z - Commerce de gros d'équipements automobiles"]
["SSP040050602",null,"GROUPAGE IMPORTATION PNEUMATIQUE","MEZIANE (Ex GIP) Activité illicite","Clôturée",null,null,"Clôturée","95257","LA FRETTE SUR SEINE","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.1801453,48.959446,null,null,null,"45.31Z - Commerce de gros d'équipements automobiles"]
["SSP040050701",null,"CAPA FRANCE","AGORA (Ex CAPA FRANCE) Cessation","Clôturée",null,null,"Clôturée","95351","LOUVRES","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.5012178,49.051056,null,null,null,"46.21Z - Commerce de gros (commerce interentreprises) de céréales, de tabac non manufacturé, de semences et d'aliments pour le bétail"]
["SSP040051001",null,"SITA","SITA","En cours",null,null,"En cours","78020","ARNOUVILLE LES MANTES","YVELINES","ILE-DE-FRANCE","Polygone",1.7168567,48.893864,"K - Déchets et traitements"]
["SSP040051101",null,"SITA","SITA","En cours",null,null,"En cours","78113","BRUEIL EN VEXIN","YVELINES","ILE-DE-FRANCE","Polygone",1.8060461,49.01771,"K - Déchets et traitements"]
["SSP040051201",null,"Garage Vincent Autos","Garage Vincent Autos","Clôturée","2005-11-01",null,"Clôturée","78217","EPONE","YVELINES","ILE-DE-FRANCE","Polygone",1.8114651,48.959633,null,"58.01 - Commerce de gros d'accessoires d'automobiles et de matériel de garage"]
["SSP040051301",null,"DM AUTO 78 (ex AUTO CHOC78)","DM AUTO régularisation","En cours","1996-07-03",null,"En cours","78683","VILLIERS SAINT FREDERIC","YVELINES","ILE-DE-FRANCE","Polygone",1.882043,48.81834,null,null,"50.1Z - Commerce de véhicules automobiles"]
["SSP040051501",null,"VAL D OISE RECUPER AUTOS","VORA Cessation","En cours",null,null,"En cours","95355","MAGNY EN VEXIN","VAL-D'OISE","ILE-DE-FRANCE","Polygone",1.7850713,49.14659,null,null,null,"45.32Z - Commerce de détail d'équipements automobiles"]
["SSP040051901",null,"FLEX-N-GATE FRANCE","FLEX N GATE Cessation partielle","Clôturée",null,null,"Clôturée","95370","MARINES","VAL-D'OISE","ILE-DE-FRANCE","Polygone",1.9709519,49.143642,null,null,null,"29.32Z - Fabrication d'autres équipements automobiles"]
["SSP040052301",null,"LPG FRANCE","LPG FRANCE Cessation","Clôturée",null,null,"Clôturée","95394","MERY SUR OISE","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.1659112,49.05335,null,null,null,"43.21A - Travaux d'installation électrique dans tous locaux"]
["SSP040052401",null,"VEOLIA EAU - COMPAGNIE GENERALE DES EAUX","VEOLIA Cessation partielle charbon actif","Clôturée",null,null,"Clôturée","95394","MERY SUR OISE","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.176236,49.065502,null,null,null,"36.00Z - Captage, traitement et distribution d'eau"]
["SSP040052601",null,"Centre technique municipal","Centre Technique Municipal Cessation","En cours",null,null,"En cours","95018","ARGENTEUIL","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.2572894,48.943794,"L23 - Détail de carburants"]
["SSP040052701",null,"Total Raffinage Marketing","TOTAL Raffinage Marketing Cessation","En cours",null,null,"En cours","95018","ARGENTEUIL","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.2541537,48.947445,"L23 - Détail de carburants"]
["SSP040052801",null,"TSMP (ex-BM)","TSMP Cessation","Clôturée",null,null,"Clôturée","95018","ARGENTEUIL","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.260544,48.958336,"H13 - Traitement de surface"]
["SSP040052901",null,"WRM","WRM Cessation d'activité","Clôturée",null,null,"Clôturée","95018","ARGENTEUIL","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.2178593,48.95161,null,null,null,"38.11Z - Collecte des déchets non dangereux"]
["SSP040053001",null,"ILLIADE Auto","Illiade Auto Cessation","Clôturée",null,null,"Clôturée","95088","BONNEUIL EN FRANCE","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.446985,48.957867,"K5 - Récupération, dépôts de ferrailles"]
["SSP040053101",null,"RAMERY - Travaux publics","RAMERY Cessation","Clôturée",null,null,"Clôturée","95116","BRUYERES SUR OISE","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.3356752,49.149204,"G2 - Chantiers, construction, bitumes, enrobés"]
["SSP040053201",null,"SADI","SADI Cessation","En cours",null,null,"En cours","95306","HERBLAY","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.127924,49.02144,"K35 - Regroupement, reconditionnement de déchets"]
["SSP040053301",null,"AB RECUP","AB RECUP Cessation","Clôturée",null,null,"Clôturée","95395","LE MESNIL AUBRY","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.3967104,49.054893,null,null,null,"38.11Z - Collecte des déchets non dangereux"]
["SSP040053401",null,"SCREG IDFN","SCREG IDFN Autorisation temporaire","Clôturée",null,null,"Clôturée","95394","MERY SUR OISE","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.1857493,49.049625,"G2 - Chantiers, construction, bitumes, enrobés"]
["SSP040054101",null,"SIRR","SIRR","Clôturée",null,null,"Clôturée","78269","GAZERAN","YVELINES","ILE-DE-FRANCE","Polygone",1.795946,48.638245,"K1 - Stations d'épuration"]
["SSP040054501",null,"PRESSTALIS","PRESSTALIS Cessation","Clôturée",null,null,"Clôturée","95527","ROISSY EN FRANCE","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.5234287,49.009754,null,null,null,"82.19Z - Photocopie, préparation de documents et autres activités spécialisées de soutien de bureau"]
["SSP040054701",null,"SITA","SITA","En cours",null,null,"En cours","78638","VAUX SUR SEINE","YVELINES","ILE-DE-FRANCE","Polygone",1.9595593,49.018703,null,null,null,"38.11Z - Collecte des déchets non dangereux"]
["SSP040054801",null,"SITA","SITA","En cours",null,null,"En cours","78239","FOLLAINVILLE DENNEMONT","YVELINES","ILE-DE-FRANCE","Polygone",1.6885018,49.013905,null,null,null,"38.11Z - Collecte des déchets non dangereux"]
["SSP040055201",null,"FRANQUET","SCEA FRANQUET Cessation","En cours",null,null,"En cours","95527","ROISSY EN FRANCE","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.5118806,48.99766,null,null,null,"41.10C - Promotion immobilière d'autres bâtiments"]
["SSP040055301",null,"BOISSONNADE ET FILS","BOISSONADE ET FILS Cessation","En cours",null,null,"En cours","95582","SANNOIS","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.2624557,48.973103,null,null,null,"47.78B - Commerces de détail de charbons et combustibles"]
["SSP040055401",null,"DACHA, GILBERT","DACHA Activité VHU illicite","Clôturée",null,null,"Clôturée","95582","SANNOIS","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.2427785,48.976864,null,null,null,"46.14Z - Intermédiaires du commerce en machines, équipements industriels, navires et avions"]
["SSP040055501",null,"HORIZON PRESSING","HORIZON PRESSING Cessation","En cours",null,null,"En cours","95585","SARCELLES","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.3758235,48.975975,null,null,null,"96.01B - Blanchisserie-teinturerie de détail"]
["SSP040055601",null,"SOC IMPRESSIONS PROF ROTATIVES OFFSET","SIPRO Cessation","Clôturée",null,null,"Clôturée","95476","OSNY","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.071563,49.04887,null,null,null,"18.12Z - Autre imprimerie (labeur)"]
["SSP040055801",null,"WERNER & MERTZ FRANCE PROFESSIONAL","WERNER & MERTZ Cessation","Clôturée",null,null,"Clôturée","95585","SARCELLES","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.3913932,48.996887,null,null,null,"46.44Z - Commerce de gros (commerce interentreprises) de vaisselle, verrerie et produits d'entretien"]
["SSP040056001",null,"VOLVO TRUCKS FRANCE","VOLVO TRUCKS FRANCE Cessation","Clôturée",null,null,"Clôturée","95585","SARCELLES","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.393717,48.99579,null,null,null,"45.20B - Entretien et réparation d'autres véhicules automobiles"]
["SSP040056101",null,"DANI-ALU","DANI ALU Cessation","Clôturée",null,null,"Clôturée","95598","SOISY SOUS MONTMORENCY","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.298209,48.995987,null,null,null,"25.99B - Fabrication d'autres articles métalliques"]
["SSP040056201",null,"ALLURE","ALLURE Cessation","Clôturée",null,null,"Clôturée","95555","SAINT GRATIEN","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.2846482,48.964687,null,null,null,"96.01B - Blanchisserie-teinturerie de détail"]
["SSP040056301",null,"ADS IDF NORD","ADS Pollution accidentelle","Clôturée",null,null,"Clôturée","95563","SAINT LEU LA FORET","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.2473073,49.003742,null,null,null,"38.11Z - Collecte des déchets non dangereux"]
["SSP040056401",null,"BGD","BGD Cessation","Clôturée",null,null,"Clôturée","95572","SAINT OUEN L'AUMONE","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.1303995,49.031166,null,null,null,"45.32Z - Commerce de détail d'équipements automobiles"]
["SSP040056501",null,"KAO CHIMIGRAF FRANCE SAS","CHIMIGRAF Cessation","Clôturée",null,null,"Clôturée","95572","SAINT OUEN L'AUMONE","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.1271465,49.05266,null,null,null,"46.73B - Commerce de gros (commerce interentreprises) d'appareils sanitaires et de produits de décoration"]
["SSP040056801",null,"OCP REPARTITION","OCP Répartition Cessation","Clôturée",null,null,"Clôturée","95018","ARGENTEUIL","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.2127545,48.952835,null,null,null,"46.46Z - Commerce de gros (commerce interentreprises) de produits pharmaceutiques"]
["SSP040057001",null,"BINEAU","GARAGE BINEAU Cessation","Clôturée",null,null,"Clôturée","95063","BEZONS","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.2260842,48.929108,null,null,"50.2Z - Entretien et réparation de véhicules automobiles"]
["SSP040057201",null,"ESPACE ST GERMAIN","ESPACE ST GERMAIN CESSATION","Clôturée",null,null,"Clôturée","95063","BEZONS","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.2122595,48.922726,null,null,null,"45.11Z - Commerce de voitures et de véhicules automobiles légers"]
["SSP040057401",null,"GARAGE BOIREAU ET FILS","BOIREAU & FILS Cessation","Clôturée",null,null,"Clôturée","95120","BUTRY SUR OISE","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.1971402,49.082283,null,null,null,"45.20A - Entretien et réparation de véhicules automobiles légers"]
["SSP040057501",null,"KM IMPRESSION","KM IMPRESSION Cessation","Clôturée",null,null,"Clôturée","95018","ARGENTEUIL","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.25088,48.951992,null,null,null,"18.12Z - Autre imprimerie (labeur)"]
["SSP040057601",null,"PEREIRA, ALCINO","MOB'OCCASE Activité illicite","Clôturée",null,null,"Clôturée","95018","ARGENTEUIL","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.2314672,48.9321,null,null,"50.4Z - Commerce et réparation de motocycles"]
["SSP040058201",null,"INERGENCE","INERGENCE Cessation","En cours",null,null,"En cours","95229","EZANVILLE","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.3715408,49.0342,null,null,null,"70.22Z - Conseil pour les affaires et autres conseils de gestion"]
["SSP040058301",null,"FRAN","FRAN (Ex OK'PRESS) Cessation","En cours",null,null,"En cours","95219","ERMONT","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.258289,48.98772,null,null,null,"96.01B - Blanchisserie-teinturerie de détail"]
["SSP040058501",null,"SARM","SARM Cessation","Clôturée",null,null,"Clôturée","95527","ROISSY EN FRANCE","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.5181983,49.00692,null,null,null,"45.20B - Entretien et réparation d'autres véhicules automobiles"]
["SSP040058601",null,"COSMOLYS","COSMOLYS Cessation","Clôturée",null,null,"Clôturée","95572","SAINT OUEN L'AUMONE","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.1396673,49.039616,null,null,null,"38.12Z - Collecte des déchets dangereux"]
["SSP040058701",null,"BETON DE PARIS","BETON DE PARIS Cessation","En cours",null,null,"En cours","95527","ROISSY EN FRANCE","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.5181904,49.008152,null,"25.01 - Fabrication de matériel de travaux publics"]
["SSP040058801",null,"STACEX AUTO","STACEX AUTO","Clôturée",null,null,"Clôturée","95555","SAINT GRATIEN","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.276948,48.96613,null,null,"50.1Z - Commerce de véhicules automobiles"]
["SSP040058901",null,"Compagnie des sablieres de la Seine","Cie SABLIERES DE LA SEINE Cessation","Clôturée",null,null,"Clôturée","95572","SAINT OUEN L'AUMONE","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.12849,49.062973,"H14 - Application de peinture"]
["SSP040059001",null,"COMECA","COMECA Cessation","En cours",null,null,"En cours","95572","SAINT OUEN L'AUMONE","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.1344626,49.05324,"H14 - Application de peinture"]
["SSP040059101",null,"Etablissements MABIT et POUILLE","MABIT ET POUILLE Cessation","Clôturée",null,null,"Clôturée","95395","LE MESNIL AUBRY","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.397765,49.05121,null,null,null,"38.12Z - Collecte des déchets dangereux"]
["SSP040059201",null,"IDF recyclage","IDF RECYCLAGE Cessation","Clôturée",null,null,"Clôturée","95370","MARINES","VAL-D'OISE","ILE-DE-FRANCE","Polygone",1.973885,49.14352,"K - Déchets et traitements"]
["SSP040059301",null,"FRIGERST","FRIGERST Cessation","Clôturée",null,null,"Clôturée","95199","DOMONT","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.3456059,49.026855,"H14 - Application de peinture"]
["SSP040059401",null,"Total marketing Services","TOTAL MARKETING Cessation","En cours",null,null,"En cours","95585","SARCELLES","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.377424,48.97819,null,null,"50.5Z - Commerce de détail de carburants"]
["SSP040059601",null,"TOTAL (ex CPGS)","TOTAL (Ex CPGS) Cessation","Clôturée",null,null,"Clôturée","95487","PERSAN","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.2619982,49.157818,null,null,"50.5Z - Commerce de détail de carburants"]
["SSP040059701",null,"CENERGY","CENERGIE Cessation partielle","En cours",null,null,"En cours","95572","SAINT OUEN L'AUMONE","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.1174037,49.03001,null,null,null,"35.30Z - Production et distribution de vapeur et d'air conditionné"]
["SSP040059801",null,"HABITAT FRANCE","HABITAT France Cessation","Clôturée",null,null,"Clôturée","95572","SAINT OUEN L'AUMONE","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.1192443,49.028336,null,null,null,"47.59A - Commerce de détail de meubles"]
["SSP040059901",null,"HELI INTER","HELI INTER Cessation","En cours",null,null,"En cours","95572","SAINT OUEN L'AUMONE","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.1447225,49.057514,null,null,"62.2Z - Transports aériens non réguliers"]
["SSP040060001",null,"HOUGHTON","HOUGHTON Cessation","Clôturée",null,null,"Clôturée","95572","SAINT OUEN L'AUMONE","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.144717,49.05554,null,null,null,"46.71Z - Commerce de gros (commerce interentreprises) de combustibles et de produits annexes"]
["SSP040060101",null,"SCANIA FRANCE","SCANIA France non classement","Clôturée",null,null,"Clôturée","95572","SAINT OUEN L'AUMONE","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.1339216,49.045567,null,null,null,"45.19Z - Commerce d'autres véhicules automobiles"]
["SSP040061001",null,"AERTEC","AERTEC Reprise d'exploitation de DELPHI","Clôturée",null,null,"Clôturée","95675","VILLERON","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.5257616,49.063663,null,null,null,"33.16Z - Réparation et maintenance d'aéronefs et d'engins spatiaux"]
["SSP040061401",null,"LPG FRANCE","LPG France Cessation ","Clôturée",null,null,"Clôturée","95572","SAINT OUEN L'AUMONE","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.1408498,49.04033,null,null,null,"43.21A - Travaux d'installation électrique dans tous locaux"]
["SSP040061501",null,"SCOTT BADER SAS","SCOTT BADER Cessation","Clôturée",null,null,"Clôturée","95572","SAINT OUEN L'AUMONE","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.1366186,49.050358,null,null,null,"20.16Z - Fabrication de matières plastiques de base"]
["SSP040061601",null,"CHIMIE RECHERCHE ENVIRONNEMENT EVOLUTION","CREE Cessation partielle","Clôturée",null,null,"Clôturée","95607","TAVERNY","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.1870518,49.024868,null,null,null,"20.59Z - Fabrication d'autres produits chimiques n.c.a."]
["SSP040061701",null,"SERVICES LOCATIONS DE BENNES","SLB Activité illicite et cessation","Clôturée",null,null,"Clôturée","95527","ROISSY EN FRANCE","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.4889789,49.00268,null,null,null,"77.32Z - Location et location-bail de machines et équipements pour la construction"]
["SSP040062301",null,"MAJ","MAJ LOVETRA Cessation","En cours",null,null,"En cours","95572","SAINT OUEN L'AUMONE","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.1294663,49.05359,null,null,null,"77.29Z - Location et location-bail d'autres biens personnels et domestiques"]
["SSP040062401",null,"EMI MUSIC (CLB) ","EMI MUSIC Cessation","Clôturée",null,null,"Clôturée","95572","SAINT OUEN L'AUMONE","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.1337738,49.04234,"L1 - Entreposage, manutention, commerces"]
["SSP040062601",null,"SCI HOLLAND","SCI HOLAND  Cessation JOUAS","Clôturée",null,null,"Clôturée","95018","ARGENTEUIL","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.2391841,48.933308,null,"65.01 - Commerce de détail d'accessoires et d'équipements automobiles"]
["SSP040062701",null,"ADP Aéroports de paris","ADP Cessation TAG","Clôturée",null,null,"Clôturée","95527","ROISSY EN FRANCE","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.538447,49.007328,"I14 - Autres centrales électriques"]
["SSP040062801",null,"ESSO SAF","ESSO SAF Cessation","En cours",null,null,"En cours","95271","GENICOURT","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.0413494,49.100178,"L2 - Transports, automobile, carburants"]
["SSP040062901",null,"PICCONI","PICCONI Activité non autorisée","En cours",null,null,"En cours","95678","VILLIERS ADAM","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.22517,49.073277,null,"15.02 - Production de matériaux concassés de roche et de laitier"]
["SSP040064401",null,"ACHATS VENTES AUTOMOBILES","AVA Cessation","Clôturée",null,null,"Clôturée","95580","SAINT WITZ","VAL-D'OISE","ILE-DE-FRANCE","Polygone",2.529765,49.090733,null,null,null,"45.11Z - Commerce de voitures et de véhicules automobiles légers"]
["SSP040066201",null,"DANZEL WORLD AUTOMOBILE","DWA Cessation","Clôturée",null,null,"Clôturée","75056","PARIS","PARIS","ILE-DE-FRANCE","Polygone",2.3259726,48.829536,null,null,null,"45.11Z - Commerce de voitures et de véhicules automobiles légers"]
["SSP040066501",null,"SNCF RESEAU","SNCF AUSTERLITZ Cessation installations de distribution de carburant","En cours",null,null,"En cours","75056","PARIS","PARIS","ILE-DE-FRANCE","Polygone",2.3653142,48.840797,null,null,null,"52.21Z - Services auxiliaires des transports terrestres"]
["SSP040066801",null,"GARAGE DE LA PLACE DE COLOMBIE","Garage de la Combie (GTF Immobilier) Cessation","Clôturée",null,null,"Clôturée","75056","PARIS","PARIS","ILE-DE-FRANCE","Polygone",2.2668407,48.86222,null,null,null,"45.11Z - Commerce de voitures et de véhicules automobiles légers"]
["SSP040066901",null,"BP FRANCE","BP France Cessation","En cours",null,null,"En cours","75056","PARIS","PARIS","ILE-DE-FRANCE","Polygone",2.3618255,48.900036,null,null,null,"46.71Z - Commerce de gros (commerce interentreprises) de combustibles et de produits annexes"]
["SSP040067001",null,"TOP EDS","EDS Cessation","Clôturée",null,null,"Clôturée","75056","PARIS","PARIS","ILE-DE-FRANCE","Polygone",2.3608491,48.86879,null,null,null,"45.11Z - Commerce de voitures et de véhicules automobiles légers"]
["SSP040067101",null,"DELWAULLE CARBURANTS","DELWAULLE CARBURANTS Cessation","Clôturée",null,null,"Clôturée","75056","PARIS","PARIS","ILE-DE-FRANCE","Polygone",2.3848693,48.849255,null,null,"50.5Z - Commerce de détail de carburants"]
["SSP040067201",null,"Total Marketing Service – Porte de Saint-Ouen","BNP Parisbas projet immobilier","En cours",null,null,"En cours","75056","PARIS","PARIS","ILE-DE-FRANCE","Polygone",2.3290932,48.899723,null,null,"50.5Z - Commerce de détail de carburants"]
["SSP040067601",null,"Taysse","TAYSSE","Clôturée","1975-01-01","1986-08-01","Clôturée","91044","BALLAINVILLIERS","ESSONNE","ILE-DE-FRANCE","Polygone",2.2780929,48.661938,null,null,"50.2Z - Entretien et réparation de véhicules automobiles"]
["SSP040067701",null,"MECABALAYAGE","MECABALAYAGE","Clôturée","2008-01-01",null,"Clôturée","91086","BONDOUFLE","ESSONNE","ILE-DE-FRANCE","Polygone",2.3833096,48.621365,null,null,null,"81.22Z - Autres activités de nettoyage des bâtiments et nettoyage industriel"]
["SSP040067801",null,"SOREDIV FRANCE","SOREDIV FRANCE","Clôturée",null,"2001-06-06","Clôturée","91103","BRETIGNY SUR ORGE","ESSONNE","ILE-DE-FRANCE","Polygone",2.3007295,48.59155,"K35 - Regroupement, reconditionnement de déchets"]
["SSP040067901",null,"JOSSE","JOSSE","Clôturée",null,null,"Clôturée","91223","ETAMPES","ESSONNE","ILE-DE-FRANCE","Polygone",2.1448164,48.45242,"L2 - Transports, automobile, carburants"]
["SSP040068001",null,"CRUBILE","CRUBILE","En cours",null,null,"En cours","91122","BURES SUR YVETTE","ESSONNE","ILE-DE-FRANCE","Polygone",2.1595738,48.69219,null,null,null,"52.10B - Entreposage et stockage non frigorifique"]
["SSP040068101",null,"EVRY ENVIRONNEMENT SERVICES (EES)","EVRY ENVIRONNEMENT SERVICES (EES)","Clôturée",null,null,"Clôturée","91228","EVRY","ESSONNE","ILE-DE-FRANCE","Polygone",2.4625564,48.62841,"K35 - Regroupement, reconditionnement de déchets"]
["SSP040068301",null,"Garage EUROPA","Garage EUROPA","En cours",null,null,"En cours","91339","LINAS","ESSONNE","ILE-DE-FRANCE","Polygone",2.251945,48.61525,null,null,"50.2Z - Entretien et réparation de véhicules automobiles"]
["SSP040068401",null,"POINT P","POINT P","Clôturée",null,null,"Clôturée","91377","MASSY","ESSONNE","ILE-DE-FRANCE","Polygone",2.2598681,48.72835,null,null,null,"52.10B - Entreposage et stockage non frigorifique"]
["SSP040068501",null,"AUTODISTRIBUTION","AUTODISTRIBUTION","Clôturée",null,null,"Clôturée","91377","MASSY","ESSONNE","ILE-DE-FRANCE","Polygone",2.3007078,48.720367,null,null,"50.2Z - Entretien et réparation de véhicules automobiles"]
["SSP040068601",null,"SOFRAP","SOFRAP","En cours",null,null,"En cours","91589","SAVIGNY SUR ORGE","ESSONNE","ILE-DE-FRANCE","Polygone",2.3523371,48.69078,"D61 - Fabrication de produits savonniers"]
["SSP040068701",null,"CATHIER","CATHIER","Clôturée","1968-12-30",null,"Clôturée","91657","VIGNEUX SUR SEINE","ESSONNE","ILE-DE-FRANCE","Polygone",2.4144466,48.697567,"K52 - Dépôts de ferraille"]
["SSP040068801",null,"GARNIFER","GARNIFER","Clôturée","1991-01-01",null,"Clôturée","91687","VIRY CHATILLON","ESSONNE","ILE-DE-FRANCE","Polygone",2.3860395,48.677364,"K52 - Dépôts de ferraille"]
["SSP040068901",null,"GARNIFER","GARNIFER","Clôturée",null,null,"Clôturée","91687","VIRY CHATILLON","ESSONNE","ILE-DE-FRANCE","Polygone",2.394217,48.673565,"K52 - Dépôts de ferraille"]
["SSP040069001",null,"SPECIAL EMAIL","SPECIAL EMAIL","En cours",null,null,"En cours","91687","VIRY CHATILLON","ESSONNE","ILE-DE-FRANCE","Polygone",2.379687,48.68434,"H13 - Traitement de surface"]
["SSP040069101",null,"FRANCE TELECOM","FRANCE TELECOM","Clôturée",null,null,"Clôturée","91421","MONTGERON","ESSONNE","ILE-DE-FRANCE","Polygone",2.441931,48.710342,null,null,null,"27.11Z - Fabrication de moteurs, génératrices et transformateurs électriques"]
["SSP040069201",null,"DEVERGEZ","DEVERGEZ","En cours","1965-09-15",null,"En cours","91421","MONTGERON","ESSONNE","ILE-DE-FRANCE","Polygone",2.4412997,48.707424,null,null,"50.5Z - Commerce de détail de carburants"]
["SSP040069301",null,"SCOTTI AUTO","SCOTTI AUTO","En cours",null,null,"En cours","91339","LINAS","ESSONNE","ILE-DE-FRANCE","Polygone",2.260564,48.621452,null,null,"50.2Z - Entretien et réparation de véhicules automobiles"]
["SSP040069401",null,"WIENERBERGER","WIENERBERGER","Clôturée","1989-05-22",null,"Clôturée","91017","ANGERVILLIERS","ESSONNE","ILE-DE-FRANCE","Polygone",2.0134764,47.999817,null,null,null,"23.32Z - Fabrication de briques, tuiles et produits de construction, en terre cuite"]
["SSP040069601",null,"FAURECIA SIEGES D'AUTOMOBILE","FAURECIA SIEGES D'AUTOMOBILE","Clôturée",null,null,"Clôturée","91223","ETAMPES","ESSONNE","ILE-DE-FRANCE","Polygone",2.1514342,48.454613,null,null,null,"29.32Z - Fabrication d'autres équipements automobiles"]
["SSP040069701",null,"OLEO RECYCLING","OLEO RECYCLING","Clôturée",null,"2011-03-22","Clôturée","91294","GUILLERVAL","ESSONNE","ILE-DE-FRANCE","Polygone",2.0794234,48.371517,null,null,null,"38.11Z - Collecte des déchets non dangereux"]
["SSP040069801",null,"RAMOS, DENIS","RAMOS","En cours",null,null,"En cours","91332","LEUDEVILLE","ESSONNE","ILE-DE-FRANCE","Polygone",2.3279512,48.570175,null,null,null,"77.12Z - Location et location-bail de camions"]
["SSP040070001",null,"LEAPOL","LEAPOL","Clôturée",null,null,"Clôturée","91347","LONGPONT SUR ORGE","ESSONNE","ILE-DE-FRANCE","Polygone",2.274711,48.65306,null,null,null,"47.11F - Hypermarchés"]
["SSP040070201",null,"UNIVERSITE DE PARIS XI PARIS SUD","UNIVERSITE DE PARIS XI PARIS SUD","Clôturée",null,null,"Clôturée","91471","ORSAY","ESSONNE","ILE-DE-FRANCE","Polygone",2.1747382,48.70283,null,null,null,"85.42Z - Enseignement supérieur"]
["SSP040070401",null,"ADP INTERNATIONAL","ADP INTERNATIONAL","Clôturée",null,null,"Clôturée","91479","PARAY VIEILLE POSTE","ESSONNE","ILE-DE-FRANCE","Polygone",2.3636913,48.73236,null,null,null,"70.22Z - Conseil pour les affaires et autres conseils de gestion"]
["SSP040070601",null,"DEPANN SERVICE","DEPANN SERVICE","Clôturée",null,null,"Clôturée","91339","LINAS","ESSONNE","ILE-DE-FRANCE","Polygone",2.2544613,48.61669,null,null,null,"46.77Z - Commerce de gros (commerce interentreprises) de déchets et débris"]
["SSP040071501",null,"SIORAT","SIORAT","Clôturée","2013-05-21","2013-10-30","Clôturée","91204","ECHARCON","ESSONNE","ILE-DE-FRANCE","Polygone",2.3968594,48.58455,"G22 - Centrales d'enrobés"]
["SSP040071801",null,"Atelier du pneu","Atelier du pneu","Clôturée",null,null,"Clôturée","91174","CORBEIL ESSONNES","ESSONNE","ILE-DE-FRANCE","Polygone",2.4626503,48.612656,null,"58.02 - Commerce de gros de pneumatiques, cycles et motocycles"]
["SSP040077001",null,"ETS GOUTORBE","Inspection du 13/02/2020","Clôturée","2020-02-13",null,"Clôturée","42339","CHAUSSETERRE","LOIRE","AUVERGNE-RHONE-ALPES","Polygone",3.8014438,45.91049,null,null,null,"31.09B - Fabrication d'autres meubles et industries connexes de l'ameublement"]
["SSP040084301",null,"SODENA","Plan de Gestion ","En cours",null,null,"En cours","59172","DENAIN","NORD","HAUTS-DE-FRANCE","Polygone",3.3732476,50.325073,null,null,"50.1Z - Commerce de véhicules automobiles"]
["SSP040088901",null,"FROGER BERNARD","Froger- Le coteau","Clôturée","2004-05-17","2020-11-02","Clôturée","85191","LA ROCHE SUR YON","VENDEE","PAYS DE LA LOIRE","Polygone",-1.4191384,46.658627,null,null,"37.1Z - Récupération de matières métalliques recyclables"]
["SSP040095301",null,"Ancienne décharge du lieu-dit Kirchbaumacker",null,"Clôturée",null,null,"Clôturée","68166","KINGERSHEIM","HAUT-RHIN","GRAND EST","Polygone",7.3085475,47.793987,"K36 - Mise en décharge"]
["SSP040095401",null,"Ancienne décharge de Thann",null,"Clôturée",null,null,"Clôturée","68012","ASPACH LE HAUT","HAUT-RHIN","GRAND EST","Polygone",7.14921,47.79074,"K36 - Mise en décharge"]
["SSP040106601",null,"SOCIETE D'EXPLOITATION GAMBINO ET FILS","Cessation d'activité","Clôturée",null,null,"Clôturée","13100","SAINT REMY DE PROVENCE","BOUCHES-DU-RHONE","PROVENCE-ALPES-COTE D'AZUR","Polygone",4.803494,43.77738,null,null,null,"08.12Z - Exploitation de gravières et sablières, extraction d'argiles et de kaolin"]
["SSP040109201",null,"ETS ROENFANTZ-MARTZOLFF","","En cours",null,null,"En cours","67520","WASSELONNE","BAS-RHIN","GRAND EST","Polygone",7.449979,48.63918,null,null,null,"25.61Z - Traitement et revêtement des métaux"]
["SSP069312501",null,"COMMUNE DE STRASBOURG","Ecole des Romains","En cours",null,null,"En cours","67482","STRASBOURG","BAS-RHIN","GRAND EST","Polygone",7.715388,48.578556,null,null,null,"84.11Z - Administration publique générale"]
["SSP069322602",null,"LES LIANTS ROUTIERS VENDEENS","Diagnostic pollution","En cours",null,null,"En cours","85191","LA ROCHE SUR YON","VENDEE","PAYS DE LA LOIRE","Polygone",-1.4368954,46.67065,null,null,null,"23.99Z - Fabrication d'autres produits minéraux non métalliques n.c.a."]
["SSP069323401",null,"Ancien Garage FORD",null,"Clôturée",null,"2021-04-22","Clôturée","53130","LAVAL","MAYENNE","PAYS DE LA LOIRE","Polygone",-0.7496657,48.057228,null,null,"50.2Z - Entretien et réparation de véhicules automobiles"]
["SSP069323801",null,"POITIER, JEAN","Cessation d'activité POITIER Jean","En cours",null,null,"En cours","44070","LA HAIE FOUASSIERE","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Polygone",-1.3958354,47.151863,null,null,"60.2L - Transports routiers de marchandises de proximité"]
["SSP069323802",null,"POITIER, JEAN","Cessation d'activité POITIER Emile","En cours",null,null,"En cours","44070","LA HAIE FOUASSIERE","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Polygone",-1.398866,47.151737,null,null,"60.2L - Transports routiers de marchandises de proximité"]
["SSP069619301",null,"SERVICES AUTO 53 (GARAGE PREMIER)","SERVICES AUTO 53 (GARAGE PREMIER)","En cours",null,null,"En cours","53094","ENTRAMMES","MAYENNE","PAYS DE LA LOIRE","Polygone",-0.7203966,47.999626,null,null,"50.2Z - Entretien et réparation de véhicules automobiles"]
["SSP069663402",null,"Ancien site d'enfouissement de déchets","Ancien site d'enfouissement de déchets","En cours",null,null,"En cours","53130","LAVAL","MAYENNE","PAYS DE LA LOIRE","Polygone",-0.79274756,48.06606,"K21 - Décharges d'ordures ménagères"]
["SSP40592301",null,"CHARRIAUD",null,"Clôturée",null,null,"Clôturée","33080","CADAUJAC","GIRONDE","NOUVELLE-AQUITAINE","Polygone",-0.5522723,44.755627]
["SSP40715502",null,"RAMI Jérôme","Suspicion de pollution","En cours","2021-03-26",null,"En cours","33493","SAINT YZANS DE MEDOC","GIRONDE","NOUVELLE-AQUITAINE","Polygone",-0.82454556,45.324432]
["SSP40906101",null,"ORNECQ Jean-Luc","SUP","Clôturée","2021-05-27","2021-05-27","Clôturée","33162","EYSINES","GIRONDE","NOUVELLE-AQUITAINE","Polygone",-0.66193235,44.863773]
["SSP41294001",null,"FRANCE AUTO PIECES",null,"Clôturée",null,null,"Clôturée","33088","CAMPS SUR L'ISLE","GIRONDE","NOUVELLE-AQUITAINE","Polygone",-0.038350828,45.014683]
["SSP41702001",null,"QUANTIN MARC",null,"En cours","1959-10-31","1983-12-07","En cours","33063","BORDEAUX","GIRONDE","NOUVELLE-AQUITAINE","Polygone",-0.5615706,44.86567]
["SSP41830801",null,"ROULAUD ET FILS (ex-COOP ATLANTIQUE)","Mesures de suivi de pollution","En cours",null,null,"En cours","87048","CONDAT SUR VIENNE","HAUTE-VIENNE","NOUVELLE-AQUITAINE","Polygone",1.2474082,45.797016]
["SSP44363501",null,"COOP ATLANTIQUE","Mesures suivi de pollution","En cours",null,null,"En cours","87048","CONDAT SUR VIENNE","HAUTE-VIENNE","NOUVELLE-AQUITAINE","Polygone",1.2474946,45.797024]
["SSP50548401",null,"LAFARGEHOLCIM CIMENTS","LAFARGEHOLCIM CIMENTS","En cours","2021-09-06",null,"En cours","76657","SAINT VIGOR D'YMONVILLE","SEINE-MARITIME","NORMANDIE","Polygone",0.3190509,49.46721]
["SSP52189001",null,"DECHARGE PRESQU'ILE GRENOBLE",null,"Clôturée",null,null,"Clôturée","38185","GRENOBLE","ISERE","AUVERGNE-RHONE-ALPES","Polygone",5.683992,45.21006]
["SSP52619301",null,"RODIER",null,"Clôturée",null,null,"Clôturée","38027","BARRAUX","ISERE","AUVERGNE-RHONE-ALPES","Polygone",5.9997625,45.43393]
["SSP52626901",null,"CLEAN 38 SOCIETE NOUVELLE","","Clôturée",null,null,"Clôturée","38169","FONTAINE","ISERE","AUVERGNE-RHONE-ALPES","Polygone",5.674385,45.197407]
["SSP52647402",null,"SULPICE",null,"En cours",null,null,"En cours","38146","DIZIMIEU","ISERE","AUVERGNE-RHONE-ALPES","Polygone",5.2630115,45.714886]
["SSP52715701",null,"BRAND PASCAL","Cessation d'activité","En cours","2020-02-28",null,"En cours","74094","CRANVES SALES","HAUTE-SAVOIE","AUVERGNE-RHONE-ALPES","Polygone",6.283144,46.184505]
["SSP53656202",null,"RECTIPHASE","Cessation d'activité","En cours","2018-04-13",null,"En cours","74010","ANNECY","HAUTE-SAVOIE","AUVERGNE-RHONE-ALPES","Polygone",6.1259933,45.938873]
["SSP55011401",null,"Celluloïd Emminence","","Clôturée",null,null,"Clôturée","67462","SELESTAT","BAS-RHIN","GRAND EST","Polygone",7.45625,48.25408]
["SSP55300901",null,"HOPITAL JEANNE D'ARC","Cessation activité","En cours","2017-03-03","2021-10-26","En cours","54167","DOMMARTIN LES TOUL","MEURTHE-ET-MOSELLE","GRAND EST","Polygone",5.932541,48.67474]
["SSP56156301",null,"DIDIER STE INDUS. DE PRODUC. & DE CONSTR",null,"Clôturée",null,null,"Clôturée","67472","SOUFFLENHEIM","BAS-RHIN","GRAND EST","Polygone",7.9657454,48.825752]
["SSP57105301",null,"ROSEO (SOCCRAM)",null,"En cours",null,null,"En cours","49278","SAINTE GEMMES SUR LOIRE","MAINE-ET-LOIRE","PAYS DE LA LOIRE","Polygone",-0.5556439,47.443287]
["SSP57138401",null,"AUTO CASSE 72 SARL","AUTO CASSE 72 SARL","En cours",null,null,"En cours","72058","CHANGE","SARTHE","PAYS DE LA LOIRE","Polygone",0.27112457,47.97933]
["SSP57201401",null,"GUY DAUPHIN ENVIRONNEMENT (métaux)","Réhabilitation","En cours",null,null,"En cours","44109","NANTES","LOIRE-ATLANTIQUE","PAYS DE LA LOIRE","Polygone",-1.5280354,47.253]
["SSP64023502",null,"DEULEP",null,"En cours",null,null,"En cours","30258","SAINT GILLES","GARD","OCCITANIE","Polygone",4.4358516,43.672874]
["SSP64518301",null,"CARRION JEAN-MARIE",null,"En cours",null,null,"En cours","31541","SEILH","HAUTE-GARONNE","OCCITANIE","Polygone",1.3504208,43.694294,null,null,null,"45.32Z - Commerce de détail d'équipements automobiles"]
["SSP65124501",null,"ROBATEL INDUSTRIES SA","Robatel","En cours",null,null,"En cours","30141","LAUDUN L'ARDOISE","GARD","OCCITANIE","Polygone",4.691859,44.10886,null,null,"27.5G - Fonderie d'autres métaux non ferreux"]
["SSP68835001",null,"Commune d'Arles","Stockage de déchets non autorisé dans l'enceinte de la déchetterie","En cours","2020-08-03",null,"En cours","13004","ARLES","BOUCHES-DU-RHONE","PROVENCE-ALPES-COTE D'AZUR","Polygone",4.742492,43.412113]
["SSP69143301",null,"Sté d'Exploitation du Plateau de la Mure","ancienne décharge de déchets inertes et amiantés","Clôturée",null,null,"Clôturée","13055","MARSEILLE","BOUCHES-DU-RHONE","PROVENCE-ALPES-COTE D'AZUR","Polygone",5.375565,43.361217]
["SSP69248101",null,"FBTP","station de transit, regroupement ou tri de produits minéraux ou de déchets non dangereux inertes","Clôturée","2019-01-03","2021-07-30","Clôturée","13081","ROGNAC","BOUCHES-DU-RHONE","PROVENCE-ALPES-COTE D'AZUR","Polygone",5.240096,43.47678]

{"sheet":"Actions","index":1,"n_rows":19800,"n_cols":15,"rows_kept":4500,"cut":true,"hidden":false,"merged":[],"bounds":{"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0}}
["Code métier","Action","Date début","Date fin","Description","Milieu","Etude","Fréquence surveillance (nombre par an)","Nom paramètre SANDRE","Nom groupe SANDRE","Mesure de gestion","Mesure de sécurité","Traitement sur site / hors site","Traitement in situ","Traitement rejets"]
["SSP000000101","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Piège hydraulique ou Confinement hydraulique"]
["SSP000000101","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000000201","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"Un diagnostic initial suivi d'un diagnostic approfondi ont été réalisés  en raison d'un réaménagement pour les besoins internes de l'entreprise.","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000000201","Exécution des travaux de réhabilitation",null,null," Travaux de dépollution","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000000701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000000701","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Piège hydraulique ou Confinement hydraulique"]
["SSP000000701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000000701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000000701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage","N/A","N/A","N/A"]
["SSP000001701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000001701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000001901","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Barbotage in situ (sparging) | Ventilation de la zone non saturée (venting)"]
["SSP000001901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)","Ventilation de la zone non saturée (venting)"]
["SSP000001901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000002301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000002301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000002301","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)","Confinement par couverture et étanchéification"]
["SSP000002501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000002501","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000002501","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000002501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000002601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"COHV, solvants chlorés, fréons | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000002601","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification","Filtration"]
["SSP000002601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"COHV, solvants chlorés, fréons | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000002601","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)","Confinement par couverture et étanchéification"]
["SSP000002601","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000002601","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols","Confinement par couverture et étanchéification"]
["SSP000002601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Pompage de rabattement ou de récupération","N/A","N/A","N/A"]
["SSP000002801","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Ventilation de la zone non saturée (venting)"]
["SSP000002901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de gestion","N/A","Trichloroéthylène","COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP000002901","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2017-06-16 : LA SITUATION S'AMELIORE\n","Eaux souterraines","N/A","3",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000002901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A","Trichloroéthylène","COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP000002901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols","Ventilation de la zone non saturée (venting)"]
["SSP000003001","Etude SSP et ingénierie des travaux de réhabilitation","1995-02-15",null," En 1995, la société Gaz de France a remis un audit environnemental regroupant les recherches historiques et documentaires ainsi que l'ensemble des travaux effectués, les résultats d'analyses et leur interprétation. Ce document indiquait que, dans son état actuel, le site (sols et eaux souterraines) ne présentait pas de risques pour la santé humaine et son environnement. Il formulait également des recommandations en cas de réaménagement du site.\n","Eaux souterraines","Diagnostic et Analyse","N/A","Cyanures libres | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Autres éléments minéraux | Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés)","N/A","N/A","N/A","N/A","N/A"]
["SSP000003001","Etude SSP et ingénierie des travaux de réhabilitation","1996-04-25",null," L'application de cette méthode a abouti à l'établissement de 5 classes de priorité, la classe 1 étant jugée la plus sensible. Les engagements de la société Gaz de France ont fait l'objet d'un protocole d'accord relatif à la maîtrise et au suivi de la réhabilitation des anciens terrains d'usines à gaz entre le Ministère de l'Environnement et Gaz de France, signé le 25 avril 1996.",null,"Analyse des enjeux sanitaires (EQRS, ARR)","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000003001","Etude SSP et ingénierie des travaux de réhabilitation","1999-04-01",null,"Aussi, dans le cadre d'un projet immobilier, une étude détaillée des risques a été réalisée en 1999 sous la responsabilité de la société Gaz de France. L'inspection des installations classées a demandé que cette étude soit reprise, les résultats étant incompatibles avec les critères de la circulaire du 10 décembre 1999 du Ministère de l'Aménagement du Territoire et de l'Environnement. Ce projet immobilier ayant été abandonné, cette étude n'est plus d'actualité.",null,"Analyse des enjeux sanitaires (EQRS, ARR)","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000003001","Surveillance environnementale","2006-03-29","2011-04-01","L'arrêté de prescriptions complémentaires imposant à la société Gaz de France la réalisation d'un réseau piézométrique et la surveillance semestrielle des eaux souterraines au droit du site a été signé par Monsieur le Préfet de Seine et Marne le 29 mars 2006. Les paramètres suivis sont les suivants : BTEX, HAP, ammonium, cyanures totaux et cyanures libres.\n\nLes résultats des analyses du suivi de 2008 et 2009 de la nappe des eaux souterraines ont mis en évidence des teneurs élevées pour les paramètres benzène et HAP au droit de 2 ouvrages (PZ2 et PZ4). Des teneurs plus faibles en benzène ont été retrouvées en PZ3.\n\nPour répondre à la demande de la DRIEE, des analyses de la qualité de l'air du sol ont été réalisées en avril 2011. Ces analyses ont mis en évidence des teneurs faibles en BTEX et des teneurs plus élevées en HAP, notamment en naphtalène, en un piézair.",null,"N/A","1",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000003301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000003301","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000003301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000003401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Ammonium","Paramètres azotés","N/A","N/A","N/A","N/A","N/A"]
["SSP000003401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés)","N/A","N/A","N/A","N/A","N/A"]
["SSP000003401","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000003501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Cyanures libres","Autres éléments minéraux | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés)","N/A","N/A","N/A","N/A","N/A"]
["SSP000003501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés)","N/A","N/A","N/A","N/A","N/A"]
["SSP000003501","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)","Confinement par couverture et étanchéification"]
["SSP000003501","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols","Confinement par couverture et étanchéification"]
["SSP000003501","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération","Confinement par couverture et étanchéification"]
["SSP000003501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000003601","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Biodégradation dynamisée (ou atténuation naturelle dynamisée) | Confinement par couverture et étanchéification | Ventilation de la zone non saturée (venting)"]
["SSP000003601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000003602","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Arsenic | Chrome | Mercure | Nickel | Plomb | Trichloroéthylène","COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000003602","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Cadmium | Chrome | Cuivre | Mercure | Nickel | Plomb | Zinc","COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000003602","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols","Confinement par couverture et étanchéification | Ventilation de la zone non saturée (venting)"]
["SSP000003602","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique","Confinement par couverture et étanchéification | Ventilation de la zone non saturée (venting)"]
["SSP000003602","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000003701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de conception des travaux (PCT)","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000003701","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique","Piège hydraulique ou Confinement hydraulique"]
["SSP000003701","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du : 2015-12-15\nRésultat de la surveillance eaux souterraines : 1\nLes épaisseurs de flottants sont stables où en diminution en périphérie du site.\n","Eaux souterraines","N/A","1",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000003701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de conception des travaux (PCT)","N/A","Arsenic | Chrome | Cuivre | Nickel | Plomb","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000003701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Pompage de rabattement ou de récupération","N/A","N/A","N/A"]
["SSP000003801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"COHV, solvants chlorés, fréons | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000003801","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Ventilation de la zone non saturée (venting)"]
["SSP000003801","Surveillance environnementale","2004-03-01",null,"Résultat de la surveillance à la date du 2017-04-24 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","1",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000003801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000003801","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)","Confinement par couverture et étanchéification"]
["SSP000003801","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)","Confinement par couverture et étanchéification"]
["SSP000003801","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols","Confinement par couverture et étanchéification"]
["SSP000003801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000003901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000003901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000003901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000004001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," Investigations préliminaires EXCIPE en 2004\n– 40 sondages (S1 à S13, TP1 à TP29)\n– 5 piézomètres\n• Etude historique et documentaire ANTEA en 2005\n(Rapport A39314/A)\n• Diagnostic Environnemental ANTEA en 2006\n(Rapport A40390/B)\n45 sondages (tarière – et pelle mécanique)\n– 6 piézomètres\n– 6 prélèvements d’eaux de surface et de sédiments\n– 5 prélèvements de sédiments dans les carnaux\n– 14 carottages de béton dont 5 échantillons analysés\n• Diagnostic complémentaire ANTEA en 2006\n(Rapport A44328/A)\n– 30 fouilles à la pelle mécanique\n– 15 piézomètres gaz\n• Diagnostic complémentaire ANTEA en 2007\n(Rapport A47817/E)\n– 25 piézomètres gaz dont 10 avec prélèvements de sols","Sol - Sous-sol","Plan de gestion","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000004001","Exécution des travaux de réhabilitation",null,null," cf aménagement de la friche en 2010","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000004001","Exécution des travaux de réhabilitation",null,null," cf aménagement de la friche en 2010","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000004001","Exécution des travaux de réhabilitation",null,null," cf travaux de l'ADEME en 2003",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000004101","Exécution des travaux de réhabilitation",null,null,"   ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000004101","Exécution des travaux de réhabilitation",null,null,"  ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000004101","Exécution des travaux de réhabilitation",null,null,"   ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000004201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP000004201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000004301","Exécution des travaux de réhabilitation",null,null,"2 900 tonnes de terres ont été excavées. Les terres polluées ont fait l'objet d'un traitement hors site sur un biocentre. Les excavations ont atteint plus de 4 m de profondeur au maximum.","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000004301","Exécution des travaux de réhabilitation",null,null," site requalifié",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000004401","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"  arrêté préfectoral notifié le 11 juillet 2008.","Eaux souterraines","Diagnostic et Analyse","N/A","Arsenic | Cuivre | Plomb","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000004401","Surveillance environnementale","2008-08-11","2010-12-31","Résultat de la surveillance à la date du 2010-02-18 : LA SITUATION S'AMELIORE\nCommentaire : les teneurs sont passées sous les valeurs de référence retenues.\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000004401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," Une première campagne d'investigations a eu lieu en novembre 2004, la seconde en août 2007","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Cuivre | Molybdène | Plomb","COHV, solvants chlorés, fréons | Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000004401","Exécution des travaux de réhabilitation",null,null," La majorité de la pollution est confinée (par des matériaux inertes sur un mètre d'épaisseur pour la pollution aux PCB et par une dalle de 20 cm d'épaisseur ou par de l'enrobé pour les autre pollutions.","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000004401","Exécution des travaux de réhabilitation",null,null," site en activité",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000004501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Chrome | Nickel","COHV, solvants chlorés, fréons | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000004501","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2013-09-23 : LA SITUATION RESTE STABLE\nCommentaire : Présence significative de tétrachloroéthylène dans les eaux de nappe au droit du site.\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000004501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Chrome","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000004501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000004601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000004601","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000004601","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000004601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000004701","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2014-12-17 : LA SITUATION RESTE STABLE\nCommentaire : la concentration en 1-1-1-trichloroéthane au piézomètre n°2 reste stable\nInformations complémentaires : Conformément à son arrêté préfectoral du 26 février 2013, l'exploitant doit réaliser annuellement 4 campagnes d'analyses sur différents paramètres en indiquant le sens d'écoulement des eaux souterraines. Ces analyses permettront de mieux appréhender le comportement des polluants dans les eaux souterraines. \n\nAprès plusieurs relances, l'exploitant a été mis en demeure par arrêté du 13 avril 2017 de procéder à la réalisation de ces analyses annuelles et de transmettre ces résultats à l'inspection. \n\nL'exploitant a transmis en février 2018 les résultats des campagnes de suivi de la qualité des eaux souterraines pour la période 2013 à 2017. Pour cette période, la fréquence des mesures imposées par l'arrêté préfectoral de 2013 n'est pas respectée.\n\nEn février 2018 une campagne de suivi de la qualité de la nappe d'eau souterraine a été réalisée au travers des onze piézomètres présents : quatre en amont et sept en aval hydraulique du site.\n\nIl est noté que sur les campagnes précédentes, le piézomètre amont PZ8 présentait des teneurs en HCT non négligeable plus ou moins marquées tout au long des campagnes de 2013 à 2017. La campagne de 2018 révèle une nette amélioration de la teneur en HCT dans les eaux souterraines.\n\nIl est relevé un impact des eaux souterraines en ce qui concerne les composés organo halogénés volatils. Ce sont le 1,1 dichloroéthène et le 1,1,1-trichloroéthane qui présentent les teneurs les plus élevées notamment au droit des piézomètres PZ9, PZ2,PZ10 et PZ11 qui sont en aval hydraulique du site.\nLes campagnes de surveillance des eaux souterraines ont repris en 2021.","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000004701","Etude SSP et ingénierie des travaux de réhabilitation","2012-10-01","2012-11-01"," IEM","Sol - Sous-sol","Interprétation de l''état des milieux (IEM)","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000004801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de gestion","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000004801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000004801","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000004801","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000004801","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000004801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000005001","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2015-07-01 : LA SITUATION S'AMELIORE\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000005001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000005001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000005001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000005401","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000005501","Etude SSP et ingénierie des travaux de réhabilitation","1975-01-01","1975-01-01"," Diag","Eaux souterraines","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000005501","Exécution des travaux de réhabilitation","1975-01-01","1975-01-01"," Dépollution","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique","Piège hydraulique ou Confinement hydraulique"]
["SSP000005501","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du : 2015-01-15\nRésultat de la surveillance eaux souterraines : 2\nIl n'y a pratiquement plus d'hydrocarbures détectés dans les trois puits extérieurs au site ainsi que sur le site.\n","Eaux souterraines","N/A","1",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000005501","Etude SSP et ingénierie des travaux de réhabilitation","1975-01-01","1975-01-01"," Diag","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000005501","Exécution des travaux de réhabilitation","1975-01-01","1975-01-01"," mise en sécurité",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000005801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Nickel | Plomb","COHV, solvants chlorés, fréons | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000005801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Arsenic | Plomb","COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000005801","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000005801","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000005801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000006201","Etude SSP et ingénierie des travaux de réhabilitation","2002-01-01","2002-01-01"," Diag","Eaux souterraines","Diagnostic et Analyse","N/A","Ammonium | Fer | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Trichloroéthylène","Benzène et dérivés | COHV, solvants chlorés, fréons | Metaux et métalloïdes | Paramètres azotés","N/A","N/A","N/A","N/A","N/A"]
["SSP000006201","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2016-12-31 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000006201","Etude SSP et ingénierie des travaux de réhabilitation","2002-01-01","2002-01-01"," diagnostic","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cadmium | Chrome | Cuivre | Mercure | Nickel | Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Trichloroéthylène","Benzène et dérivés | COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000006201","Exécution des travaux de réhabilitation","2002-01-01","2002-01-01","Dépollution","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000006201","Exécution des travaux de réhabilitation","2002-01-01","2002-01-01","Dépollution","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000006201","Exécution des travaux de réhabilitation","2002-01-01","2002-01-01"," Mise en sécurité",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage","N/A","N/A","N/A"]
["SSP000006301","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,null,"Filtration"]
["SSP000006301","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2016-12-05 : LA SITUATION RESTE STABLE\nCommentaire : Traitement ayant permis une réduction des concentrations en hydrocarbures.\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000006301","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000006301","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000006301","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Ventilation de la zone non saturée (venting)"]
["SSP000006601","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000006601","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique"]
["SSP000006801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés)","N/A","N/A","N/A","N/A","N/A"]
["SSP000006801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés)","N/A","N/A","N/A","N/A","N/A"]
["SSP000006801","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000006801","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000006801","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique"]
["SSP000006801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000006901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Analyse des enjeux sanitaires (EQRS, ARR)","N/A",null,"COHV, solvants chlorés, fréons | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000006901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000006901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000006901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000007001","Etude SSP et ingénierie des travaux de réhabilitation","2005-08-10","2005-08-10"," Diag","Eaux souterraines","Diagnostic et Analyse","N/A","Aluminium | Ammonium | Arsenic | Cadmium | Sélénium","Hydrocarbures et indices liés | Metaux et métalloïdes | Paramètres azotés","N/A","N/A","N/A","N/A","N/A"]
["SSP000007001","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2014-03-11 : LA SITUATION RESTE STABLE\nAutomne 2021: actualisation des modalités de surveillance.\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000007001","Etude SSP et ingénierie des travaux de réhabilitation","2005-08-10","2005-08-10"," Diag","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Chrome | Cuivre | Mercure | Nickel","COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000007001","Exécution des travaux de réhabilitation","2005-08-10","2005-08-10"," Mise en sécurité",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000007201","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000007201","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000007201","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique","Confinement par couverture et étanchéification"]
["SSP000007201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000007401","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"  mémoire de cessation d'activités remis à l'inspection en mars 2004\n diagnostic détaillé réalisé en novembre 2004","Eaux souterraines","Diagnostic et Analyse","N/A","Nickel","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000007401","Surveillance environnementale",null,"2008-05-31","Résultat de la surveillance à la date du 2008-05-31 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000007401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," mémoire de cessation d'activités remis à l'inspection en mars 2004\n diagnostic détaillé réalisé en novembre 2004\nbilan sur la surveillance de la qualité des eaux souterraines  mai 2008","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cuivre","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000007401","Exécution des travaux de réhabilitation",null,null," site réaménagé",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000007601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," Investigations préliminaires EXCIPE en 2004\n– 40 sondages (S1 à S13, TP1 à TP29)\n– 5 piézomètres\n• Etude historique et documentaire ANTEA en 2005\n(Rapport A39314/A)\n• Diagnostic Environnemental ANTEA en 2006\n(Rapport A40390/B)\n45 sondages (tarière – et pelle mécanique)\n– 6 piézomètres\n– 6 prélèvements d’eaux de surface et de sédiments\n– 5 prélèvements de sédiments dans les carnaux\n– 14 carottages de béton dont 5 échantillons analysés\n• Diagnostic complémentaire ANTEA en 2006\n(Rapport A44328/A)\n– 30 fouilles à la pelle mécanique\n– 15 piézomètres gaz\n• Diagnostic complémentaire ANTEA en 2007\n(Rapport A47817/E)\n– 25 piézomètres gaz dont 10 avec prélèvements de sols","Sol - Sous-sol","Plan de gestion","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000007601","Exécution des travaux de réhabilitation",null,null,"cf études précitées","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000007601","Exécution des travaux de réhabilitation",null,null," cf études précitées",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000007801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Interprétation de l''état des milieux (IEM)","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP000007801","Surveillance environnementale","2005-12-13",null,"Résultat de la surveillance à la date du 2016-04-15 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000007801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Interprétation de l''état des milieux (IEM)","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP000007801","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols","Ventilation de la zone non saturée (venting)"]
["SSP000007801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000007901","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Piège hydraulique ou Confinement hydraulique"]
["SSP000007901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Lavage à l'eau"]
["SSP000007901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Pompage de rabattement ou de récupération","N/A","N/A","N/A"]
["SSP000008101","Exécution des travaux de réhabilitation",null,null,"traitement des sols","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique","Ventilation de la zone non saturée (venting)"]
["SSP000008501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Trichloroéthylène","COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP000008501","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Piège hydraulique ou Confinement hydraulique"]
["SSP000008501","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2017-12-31 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000008501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Trichloroéthylène","COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP000008501","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000008501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000008601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," suivi","Eaux souterraines","Plan de gestion","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000008601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," excavation des terres impactées","Sol - Sous-sol","Plan de gestion","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000008601","Exécution des travaux de réhabilitation",null,null," site clôturé avant et pendant le chantier\nsite encours de requalification",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000009101","Exécution des travaux de réhabilitation",null,null," Le site a été mis en sécurité par l'exploitant.",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000009101","Surveillance environnementale","2017-10-31",null,"Le 31 octobre 2017 le Préfet a pris un arrêté préfectoral complémentaire demandant la surveillance des milieux.  (eaux souterraines, gaz de sols, air ambiant des habitations hors site). Durée 4 ans, fréquence semestrielle.",null,"N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000010101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000010101","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Oxydation chimique | Piège hydraulique ou Confinement hydraulique"]
["SSP000010101","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2016-11-24 : LA SITUATION S'AMELIORE\nCommentaire : Mais les piézomètres les plus impactés n'ont pas été analysés en 2016.\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000010101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000010101","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000010101","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000010201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000010301","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2018-12-01 : LA SITUATION SE DEGRADE\nInformations complémentaires : Les piézomètres comprenant les teneurs en polluant les plus élevées (principalement hydrocarbures totaux et benzène) se retrouvent situés en aval du site, depuis la modification du sens d’écoulement de la nappe.\nA noter, pour le 1er trimestre 2013, la disparition de la phase flottante sur les PZ1, PZ4 et PZ9 ainsi que la diminution des teneurs en xylènes et éthylbenzène.\nDe nombreux ouvrages ont été supprimés à cause des travaux. Seuls ceux situés en périphérie du site ont été conservés et font l'objet d'un suivi.\n\nA la date du 09/02/2021, la situation s'améliore avec une forte diminution des concentrations en polluants dans l’eau de la nappe souterraine, en mars 2020.\nDes hydrocarbures ont été mesurés dans les gaz du sol en mars 2020 au droit du piézomètre PG2, implanté près du piézomètre PZ9, dans la zone actuellement en traitement par sparging et venting : 50,31 mg/m³ en hydrocarbures C5-C12. Le rapport précise que la présence d’hydrocarbures dans les gaz du sol est vraisemblablement en lien avec les actions de traitement.\nLes résultats des analyses dans les gaz du sol, de la campagne de juillet 2020 permettront de conclure quant au fait de savoir si les teneurs en hydrocarbures mesurées en mars 2020 au droit du piézair PG2 étaient dues au traitement en cours.","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000010301","Etude SSP et ingénierie des travaux de réhabilitation","2016-05-04",null," Les mesures de gestion prévues sont les suivantes :\n- excavation de la zone du poste de déchargement\n- excavation de la zone déchets\n- excavation de la zone du parc à cuves\n- traitement des terres in-situ par biopiles\n- traitement de la nappe dans la zone du parc à cuves par venting\n\nLa durée du chantier est estimée à 23 mois.\nLes travaux ont débuté en avril 2017.","Sol - Sous-sol","Plan de gestion","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000010301","Exécution des travaux de réhabilitation","2017-04-01",null,"Les travaux se poursuivent.","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols","Confinement par couverture et étanchéification | Ventilation de la zone non saturée (venting)"]
["SSP000010301","Exécution des travaux de réhabilitation","2017-04-01",null,"Les travaux se poursuivent.","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique","Confinement par couverture et étanchéification | Ventilation de la zone non saturée (venting)"]
["SSP000010401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP000010401","Surveillance environnementale","2004-06-23","2011-12-31","Résultat de la surveillance à la date du 2011-12-31 : LA SITUATION RESTE STABLE\nDate de fin envisagée de la surveillance : 2011-12-31","Eaux souterraines","N/A","1",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000010501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de gestion","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | COHV, solvants chlorés, fréons | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000010501","Surveillance environnementale","2005-06-01",null,"Résultat de la surveillance à la date du 2019-05-15 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000010501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | COHV, solvants chlorés, fréons | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000010501","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Ventilation de la zone non saturée (venting)"]
["SSP000010501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000010701","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2019-07-01 : LA SITUATION S'AMELIORE\nInformations complémentaires : Présence de chlorure de vinyle et de trichloroéthylène\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000010701","Etude SSP et ingénierie des travaux de réhabilitation","2015-11-04",null," AIR LIQUIDE a transmis, par courrier du 04/11/2015 complété le 23/03/2016, un plan de gestion de la pollution. Les techniques de dépollutions retenues sont les suivantes :\n- zone lot 1 – IDF HABITAT, sous le bâtiment : mise en place d’un système de venting sur une période de 6 mois et réalisation d’une ARR (Analyse du risque résiduel) pour valider l’arrêt du traitement ;\n- zone lots 1 et 2 – Nappe : injection d’oxydant ou pompage-traitement au droit des deux piézomètres déjà installés, pendant 1 an avec un bilan en fin de période pour valider l’arrêt du traitement ;\n- zone Nord - parking de débordement : excavation des terres et traitement en biotertre sur le site pendant 8 à 12 mois.\n\nAinsi, pour chaque zone traitée, une durée minimale de traitement a été définie, puis à l’issue de la période, le traitement sera poursuivi jusqu’à ce que l’abattement des concentrations en polluants soit inférieur à 10 % entre deux campagnes de mesures. De plus, un descriptif des différents équipements de traitement a été intégré au plan de gestion.","Sol - Sous-sol","Plan de gestion","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000010701","Exécution des travaux de réhabilitation","2017-12-04","2019-07-29","Sur proposition de l'inspection des installations classées, les travaux de dépollution ont été encadrés par l'arrêté préfectoral du 23/05/2016.\n\nUne inspection du site, le 30/05/2018, a permis de constater que les travaux d'excavation, au niveau du parking, avaient été réalisés en décembre 2017. Les terres excavées étaient en cours de traitement sur le site, dans 2 biotertres. Le traitement de la nappe a débuté en octobre 2017 et celui des gaz du sol en mai 2018.\nLes travaux de dépollution se poursuivent. Les concentrations en polluant dans la nappe sont stables, mais une diminution des teneurs en solvants chlorés a été constatée dans les gaz du sol.\n\nPar courrier du 24/01/2019, complété le 06/03/2019, l'exploitant a transmis le rapport de fin de travaux relatif aux travaux de dépollution de la zone du parking. L'inspection du 29/01/2019 a permis de constater que les fouilles avaient été remblayées et  que les biotertres avaient été supprimées. Les concentrations résiduelles dans les sols sont de 1,55 mg/kg en solvants chlorés et de 160 mg/kg en hydrocarbures. Dans les gaz du sol, la concentration maximale en trichloréthylène est de 140 µg/m³ et de 310 µg/m³ pour le perchloréthylène.\n\nLe rapport de fin de travaux relatif au traitement des gaz du sol au droit du lot 1 a été transmis par courrier du 03/05/2019. Le traitement par venting a été réalisé entre le 16/05/2018 et le 22/11/2018. Le taux d'abattement des polluants est compris entre 75 et 93 %. Les concentrations résiduelles en solvants chlorés, mesurées le 10/12/2018 étaient comprises entre 200 et 800 µg/m³.\nL'inspection du 23/10/2019 a permis de constater que l'installation de venting avait été supprimée et que le traitement des eaux de la nappe avait été arrêté fin juillet 2019.\n\nPar courrier du 05/03/2020, AIR LIQUIDE a transmis le rapport de fin de travaux pour la réhabilitation du lot 2. Le traitement par pompage de la nappe a été réalisé entre le 18/10/2017 et le 29/07/2019. Les concentrations en solvants, observées en septembre 2019 étaient de 21 µg/l en tétrachloroéthylène et de 11 µg/l en trichloréthylène.\n\nL'analyse des risques résiduels, transmise par courrier du10/03/2020, \n\n\nPar ailleurs, le suivi semestriel des milieux doit être poursuivi sur une durée d'au moins 4 ans, et fera l'objet d'un bilan quadriennal.","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000010701","Exécution des travaux de réhabilitation","2017-12-04","2019-07-29","Sur proposition de l'inspection des installations classées, les travaux de dépollution ont été encadrés par l'arrêté préfectoral du 23/05/2016.\n\nUne inspection du site, le 30/05/2018, a permis de constater que les travaux d'excavation, au niveau du parking, avaient été réalisés en décembre 2017. Les terres excavées étaient en cours de traitement sur le site, dans 2 biotertres. Le traitement de la nappe a débuté en octobre 2017 et celui des gaz du sol en mai 2018.\nLes travaux de dépollution se poursuivent. Les concentrations en polluant dans la nappe sont stables, mais une diminution des teneurs en solvants chlorés a été constatée dans les gaz du sol.\n\nPar courrier du 24/01/2019, complété le 06/03/2019, l'exploitant a transmis le rapport de fin de travaux relatif aux travaux de dépollution de la zone du parking. L'inspection du 29/01/2019 a permis de constater que les fouilles avaient été remblayées et  que les biotertres avaient été supprimées. Les concentrations résiduelles dans les sols sont de 1,55 mg/kg en solvants chlorés et de 160 mg/kg en hydrocarbures. Dans les gaz du sol, la concentration maximale en trichloréthylène est de 140 µg/m³ et de 310 µg/m³ pour le perchloréthylène.\n\nLe rapport de fin de travaux relatif au traitement des gaz du sol au droit du lot 1 a été transmis par courrier du 03/05/2019. Le traitement par venting a été réalisé entre le 16/05/2018 et le 22/11/2018. Le taux d'abattement des polluants est compris entre 75 et 93 %. Les concentrations résiduelles en solvants chlorés, mesurées le 10/12/2018 étaient comprises entre 200 et 800 µg/m³.\nL'inspection du 23/10/2019 a permis de constater que l'installation de venting avait été supprimée et que le traitement des eaux de la nappe avait été arrêté fin juillet 2019.\n\nPar courrier du 05/03/2020, AIR LIQUIDE a transmis le rapport de fin de travaux pour la réhabilitation du lot 2. Le traitement par pompage de la nappe a été réalisé entre le 18/10/2017 et le 29/07/2019. Les concentrations en solvants, observées en septembre 2019 étaient de 21 µg/l en tétrachloroéthylène et de 11 µg/l en trichloréthylène.\n\nL'analyse des risques résiduels, transmise par courrier du10/03/2020, \n\n\nPar ailleurs, le suivi semestriel des milieux doit être poursuivi sur une durée d'au moins 4 ans, et fera l'objet d'un bilan quadriennal.","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000010801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Interprétation de l''état des milieux (IEM)","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000010801","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique","Piège hydraulique ou Confinement hydraulique"]
["SSP000010801","Surveillance environnementale","2004-04-23",null,"Résultat de la surveillance à la date du 2018-01-09 : LA SITUATION S'AMELIORE\nCommentaire : Déplacement de la pollution vers des habitations\nInformations complémentaires : Des teneurs importantes en hydrocarbures et en benzène sont toujours présentes sur les piézomètres aval et sur le PZ4 situé en amont de la station service\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000010801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Interprétation de l''état des milieux (IEM)","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000010801","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000010901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000010901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000010901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000011001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de gestion","N/A",null,"COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP000011001","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Oxydation chimique"]
["SSP000011001","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2018-09-01 : LA SITUATION RESTE STABLE\nCommentaire : Les concentrations sont du même ordre de grandeur que celles observées depuis le début du suivi.\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000011001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A",null,"COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP000011001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Ventilation de la zone non saturée (venting)"]
["SSP000011001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000011101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000011101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000011101","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000011101","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000011201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000011201","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Ventilation de la zone non saturée (venting)"]
["SSP000011201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000011201","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique","Ventilation de la zone non saturée (venting)"]
["SSP000011201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Pompage de rabattement ou de récupération","N/A","N/A","N/A"]
["SSP000011501","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000011501","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2016-05-27 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000011501","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols","Biodégradation dynamisée (ou atténuation naturelle dynamisée)"]
["SSP000011501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...) | Pompage de rabattement ou de récupération","N/A","N/A","N/A"]
["SSP000011701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000011701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000011701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000011701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000011701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000011801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Chrome | Cuivre | Nickel | Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000011801","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Oxydation chimique"]
["SSP000011801","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2010-11-01 : LA SITUATION S'AMELIORE\nCommentaire : Il reste un impact résiduel essentiellement en chlorure de vinyle.\nDate de fin envisagée de la surveillance : 2010-11-01","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000011801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Chrome | Cuivre | Nickel | Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000011801","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000011801","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000011901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000011901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000012001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000012001","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000012001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000012001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000012201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cuivre | Plomb | Zinc","HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000012201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000012301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de gestion","N/A",null,"COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP000012301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A","Cuivre | Plomb | Zinc","HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000012301","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000012301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000012401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de gestion","N/A",null,"COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP000012401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A",null,"COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP000012501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A","Cadmium | Plomb","HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000012501","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000012601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000012701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP000012701","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Piège hydraulique ou Confinement hydraulique | Ventilation de la zone non saturée (venting)"]
["SSP000012701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Chrome | Cuivre | Plomb | Zinc","COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000012701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000012701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000012701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000012701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000012801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cuivre | Plomb","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000012901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Chrome | Nickel | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000012901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Chrome | Cuivre | Nickel | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000012901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000013101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000013101","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique","Ventilation de la zone non saturée (venting)"]
["SSP000013101","Surveillance environnementale","2010-07-06",null,"Résultat de la surveillance à la date du 2017-11-28 : LA SITUATION S'AMELIORE\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000013101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000013101","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000013101","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000013101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000013201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés","N/A","N/A","N/A","N/A","N/A"]
["SSP000013201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000013201","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000013201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000013301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000013301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000013301","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000013301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000013401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000013401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000013401","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000013401","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000013601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de gestion","N/A","Arsenic | Chrome | Nickel | Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Trichloroéthylène","Benzène et dérivés | COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000013601","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Piège hydraulique ou Confinement hydraulique"]
["SSP000013601","Surveillance environnementale","2013-11-06",null,"Résultat de la surveillance à la date du 2012-08-01 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000013601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A","Arsenic | Chlorures | Chrome | Cuivre | Nickel | Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Trichloroéthylène | Zinc","Autres éléments minéraux | Benzène et dérivés | COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000013601","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000013601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage | Interdiction d'accès (clôture...) | Pompage de rabattement ou de récupération | Reconditionnement de produits dangereux, Reconditionnement de déchets","N/A","N/A","N/A"]
["SSP000014601","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000014601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000014801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000014801","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000014801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000015201","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)","Ventilation de la zone non saturée (venting)"]
["SSP000015201","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols","Ventilation de la zone non saturée (venting)"]
["SSP000015201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000015301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000015301","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000015301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000015401","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000015501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | COHV, solvants chlorés, fréons | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000015501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | COHV, solvants chlorés, fréons | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000015501","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000016001","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000016001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000016001","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000016001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000016801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de gestion","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000016801","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2016-07-11 : LA SITUATION S'AMELIORE\nCommentaire : Une nette amélioration de la qualité des eaux de la nappe est à noter, suite au traitement de la nappe mais les concentrations restent importantes\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000016801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000016801","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000016801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000016901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Interprétation de l''état des milieux (IEM)","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000016901","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2018-06-20 : LA SITUATION RESTE STABLE\nCommentaire : 6.4 μg/l en benzène\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000016901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Interprétation de l''état des milieux (IEM)","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000016901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000016901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000017001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000017201","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2015-06-01 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000017201","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000017501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Chrome | Cuivre | Mercure | Zinc","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000017801","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2017-01-01 : LA SITUATION RESTE STABLE\nCommentaire : Il est toujours constaté des concentrations élevées en sels sur les piézométres avals\nInformations complémentaires : En 2015, des paramètres supplémentaires sont suivis :Chlorures, Bromures, Fluorures, Calcium, Magnésium, Potassium et Sodium. Pour ces paramètres la concentration en aval est supérieure à celle mesurée en amont.\n","Eaux souterraines","N/A","1",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000017801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000017801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000018101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000018101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000018101","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000018101","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000018501","Etude SSP et ingénierie des travaux de réhabilitation","2005-09-01","2005-09-01"," Dignostic","Eaux souterraines","Diagnostic et Analyse","N/A","Chrome | Molybdène | Nickel | Trichloroéthylène | Zinc","COHV, solvants chlorés, fréons | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000018501","Etude SSP et ingénierie des travaux de réhabilitation","2005-09-01","2005-09-01"," Diagnostic","Sol - Sous-sol","Diagnostic et Analyse","N/A","Plomb","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000018501","Exécution des travaux de réhabilitation","2005-09-01","2005-09-01"," Dépollution","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000018501","Exécution des travaux de réhabilitation","2005-09-01","2005-09-01"," Dépollution","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000018501","Exécution des travaux de réhabilitation","2005-09-01","2005-09-01","Dépollution","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000018501","Exécution des travaux de réhabilitation","2005-09-01","2005-09-01"," Mise en sécurité",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000018601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Cadmium | Cuivre | Mercure | Sélénium | Sulfates | Zinc","Autres éléments minéraux | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000018601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000018801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000018801","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Oxydation chimique | Piège hydraulique ou Confinement hydraulique"]
["SSP000018801","Surveillance environnementale","2001-03-01",null,"Résultat de la surveillance à la date du 2014-11-30 : LA SITUATION RESTE STABLE\nCommentaire : Par rapport daté d'octobre 2016, il est demandé à l'exploitant de poursuivre la surveillance de la nappe pendant 2 années supplémentaires.\nInformations complémentaires : Les résultats des dernières campagnes réalisées en 2014 ont permis de mettre en évidence :\r\n*la présence de la nappe alluviale à une profondeur d'environ 5 à 7 mètres au droit du site ;\r\n*un sens d'écoulement globalement dirigé vers le sud-est en période de hautes eaux et vers le sud sud-est en période de basses eaux comme lors des campagnes précédentes ;\r\n*la présence d'une phase surnageante en mars 2014 au droit de PZ13 (7 cm) ;\r\n*un fort impact en benzène (jusqu'à 37mg/l), hydrocarbures C10-C40 (jusqu'à 54 mg/l) et HAP (jusqu'à 34,3 mg/l pour la somme des 6 HAP) au droit des piézomètres PZ13 et PZ15 (zone ayant fait l'objet d'un traitement par écrémage jusqu'aux limites techniques de la méthode et où historiquement de fortes teneurs sont mesurées (anciennement PZ3, PZ3bis, PZ8 et PZ5).\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000018801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Chrome | Mercure | Plomb | Zinc","COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000018801","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Ventilation de la zone non saturée (venting)"]
["SSP000018801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000018901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000018901","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Piège hydraulique ou Confinement hydraulique"]
["SSP000018901","Surveillance environnementale","2000-08-24",null,"Commentaire : La surveillance est réalisée par :\r\n- l'exploitant actuel sur la partie Sud\r\n- l'ancien exploitant sur la partie Nord.\nInformations complémentaires : Présence de Benzène a des teneurs significatives dans la nappe au sud du site.\r\nImportantes fluctuations des teneurs en hydrocarbures sur l'ensemble des piézomètres du site, et des teneurs en éthylbenzène et xylène sur le piézomètre au centre de la parcelle.\r\nLe sens d'écoulement de la nappe déterminé dirigé vers le sud- sud-est.\r\nAbsence de flottant dans la nappe au nord du site.\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000018901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique","Ventilation de la zone non saturée (venting)"]
["SSP000018901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000019201","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000019201","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique"]
["SSP000019301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A","Plomb | Zinc","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000019301","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000019301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...) | Reconditionnement de produits dangereux, Reconditionnement de déchets","N/A","N/A","N/A"]
["SSP000019401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Chrome","HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000019401","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000019601","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000019601","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000019601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000019701","Surveillance environnementale","2007-08-07",null,"Informations complémentaires : Nette amélioration sur HCT et cuivre (2 polluants les plus présents)\r\nEvolution défavorable sur l'arsenic à suivre\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000019701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000019801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," Une évaluation de l'état des sols a été réalisée le 03/09/1992.","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cyanures libres | Mercure | Plomb","Autres éléments minéraux | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000020101","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000020101","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000020101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000020201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000020301","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000020301","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000020301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000020401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000020401","Surveillance environnementale","2004-01-01",null,"Résultat de la surveillance à la date du 2016-03-24 : LA SITUATION SE DEGRADE\nInformations complémentaires : - confirmation de la présence d’une couche de 0,5 cm de flottant sur le Pi11, ayant empêché la réalisation du prélèvement,\r\n- impact majeur en hydrocarbures, en particulier par les BTEX, au niveau des piézomètres Pz1, Pi5, Pi8  (nappe superficielle) présentant un fort dépassement des valeurs de référence, mais en baisse par rapport à la campagne de janvier 2016,\r\n- impact moindre en BTEX au niveau de Pz3 (nappe profonde), présentant un dépassement des valeurs de référence,\r\n- impact en benzène au droit de PZ6 implanté hors du site (en aval / latéral hydraulique de l’ancienne station), présentant un dépassement des valeurs de référence,\r\n- l’absence d’impact en Pz4 (nappe superficielle) et au puits Templier (nappe profonde) en aval du site,\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000020401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000020401","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000020401","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000020401","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000020501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000020501","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000020501","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000020501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000020701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000020701","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000020701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000020901","Etude SSP et ingénierie des travaux de réhabilitation","1999-02-04",null," Au regard du contexte environnemental du site, de la nature de ses activités et de la mauvaise gestion des produits, la DRIRE a demandé à la société MEURANT d’établir un diagnostic initial et une évaluation simplifiée des risques par arrêté préfectoral en date du 04 février 1999. L’examen de ces études n’appelait pas de remarques de la part de l'inspection des installations classées. Ce site relevait de la classe 2, impliquant la mise en place d'une surveillance des eaux souterraines.","Sol - Sous-sol","Diagnostic et Analyse","N/A","Chrome | Nickel | Zinc","COHV, solvants chlorés, fréons | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000020901","Etude SSP et ingénierie des travaux de réhabilitation","1999-02-02",null,"Au regard du contexte environnemental du site, de la nature de ses activités et de la mauvaise gestion des produits, la DRIRE a demandé à la société MEURANT d’établir un diagnostic initial et une évaluation simplifiée des risques par arrêté préfectoral en date du 04 février 1999. L’examen de ces études n’appelait pas de remarques de la part de l'inspection des installations classées. Ce site relevait de la classe 2, impliquant la mise en place d'une surveillance des eaux souterraines.",null,"Analyse des enjeux sanitaires (EQRS, ARR)","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000020901","Surveillance environnementale",null,null,"L'arrêté préfectoral n°07 DAIDD 1IC 173 du 13 juin 2007 prévoyait la mise en place de 3 piézomètres (1 en amont et 2 en aval), la réalisation de 2 campagnes de mesures (périodes de basses eaux et hautes eaux), le suivi des paramètres niveau de la nappe, hydrocarbures totaux, HAP, métaux lourds (As, Cd, Cr, Cu, Fe, Ni, Pb et Zn) et les composés organohalogénés volatils. A l'issue de ces deux campagnes de mesures, l'arrêté préfectoral a imposé à la société MEURANT de fournir un bilan sur l'évolution annuelle des concentrations mesurées et de se positionner sur la poursuite des mesures.",null,"N/A","1",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000021001","Exécution des travaux de réhabilitation","1998-11-05","2003-05-01","L'arrêté préfectoral du 5 novembre 1998 a imposé l'excavation des terres polluées autour des anciennes cuves et a prescrit la réalisation d'une surveillance de la nappe.","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000021001","Etude SSP et ingénierie des travaux de réhabilitation",null,"1993-01-01","En 1993, un audit environnement a été réalisé, révélant une pollution du sol superficiel. Des investigations complémentaires sur la pollution des sols ont été menées en octobre 1998 dans le cadre d'une expertise judiciaire. Ces investigations ont montré une pollution des sols aux BTEX, chrome, plomb, hydrocarbure et chlorobenzène.",null,"Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000021001","Etude SSP et ingénierie des travaux de réhabilitation","2004-07-07",null,"Conformément aux dispositions de l'arrêté préfectoral complémentaire du 7 juillet 2004, l'exploitant a transmis un mémoire de cessation d’activité accompagné d’un diagnostic initial et d’une évaluation simplifiée des risques (ESR) qui conduit à classer le site en classe 2 (site à surveiller).\n\nL'étude de ces documents a amené l'inspection des installations classées à demander à l'exploitant d'indiquer les mesures qu'il comptait mettre en œuvre compte tenu de la pollution résiduelle présente dans les différents milieux et, le cas échéant, de proposer les usages du sol et des eaux à proscrire. Il lui a également été demandé de compléter le programme de surveillance de la qualité des eaux souterraines mis en place au droit du site en l'élargissant à d'autres paramètres.",null,"Analyse des enjeux sanitaires (EQRS, ARR)","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000021001","Surveillance environnementale","2008-07-02","2009-09-01","L'arrêté préfectoral complémentaire n° 08 DAIDD IC 225 du 2 juillet 2008 impose à l'exploitant de proposer un plan de gestion du site, ainsi qu'un contrôle semestriel de la qualité des eaux souterraines au moyen de 3 piézomètres.\n\nMonsieur le Préfet de Seine-et-Marne a mis en demeure, par arrêté du 5 août 2009, l'exploitant de fournir un plan de gestion et de transmettre les résultats des campagnes d'analyses des eaux souterraines au titre de l'année 2008.",null,"N/A","1",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000021101","Exécution des travaux de réhabilitation",null,"2006-06-01","En juin 2005, des travaux d'excavation de la zone polluée par des hydrocarbures ont été réalisés : 700 tonnes de terres ont été évacuées en centre de traitement autorisé. La pollution résiduelle paraît compatible avec l'usage de cette partie du site (future voirie).","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique","Confinement par couverture et étanchéification"]
["SSP000021101","Etude SSP et ingénierie des travaux de réhabilitation","2001-02-08","2001-10-19","Un diagnostic initial réalisé par la société SOLER ENVIRONNEMENT (oct 2001) avait mis en évidence :\n- une pollution des sols par hydrocarbures au droit d'un ancien stockage d'huile\n- des teneurs anormalement élevées en métaux lourds dans les remblais,\nla présence d'hydrocarbures et de HAP (hydrocarbures aromatique polycyclique) à des concentrations supérieures à la VCI (valeur constat d'impact) \"usage sensible voire \"non sensible\" sur deux échantillons d'eau de nappe.\nLa cotation de l'étude simplifiée des risque, réalisé pour le site en état, c'est à dire sans activité, recouvert de dalle de béton et à usage industriel non fréquenté) a conduit à classer le site en classe 2 (site à surveiller) pour le milieu \"eau souterraine\".",null,"Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000021101","Etude SSP et ingénierie des travaux de réhabilitation",null,"2003-02-07","Une étude détaillée des risques (février 2003) a donc été menée en considérant l'utilisation du site en lieu de résidence et de travail pour des adultes et des enfants. Les voies d'exposition qui ont été retenues sont l'ingestion des sols, l'inhalation de poussières, le contact cutané et l'ingestion de végétaux cultivés sur le site. En raison des faibles teneurs de polluants mesurés\ndans la nappe à l'exception de la particularité d'un point en arsenic, celle-ci n'a pas été prise en compte dans l'EDR.\nLes composés considérés pour la quantification des risques sanitaires sont l'arsenic, le mercure, le plomb, la naphtalène, le benzo[a]pyrène, le fluoranthène et le pyrène.\nLe résultat du calcul des expositions montre que l'exposition étudiée est susceptible d'entraîner un risque pour la santé, principalement par le biais :\n- ingestion des sols pour les enfants (benzo[a]pyrène),\n- contact cutané (benzo[a]pyrène)\n- ingestion de végétaux cultivés sur le site (arsenic, benzo[a]pyrène, pyrène, plomb).",null,"Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000021101","Etude SSP et ingénierie des travaux de réhabilitation","2003-02-07",null,"Une étude détaillée des risques (février 2003) a donc été menée en considérant l'utilisation du site en lieu de résidence et de travail pour des adultes et des enfants. Les voies d'exposition qui ont été retenues sont l'ingestion des sols, l'inhalation de poussières, le contact cutané et l'ingestion de végétaux cultivés sur le site. En raison des faibles teneurs de polluants mesurés\ndans la nappe à l'exception de la particularité d'un point en arsenic, celle-ci n'a pas été prise en compte dans l'EDR.\nLes composés considérés pour la quantification des risques sanitaires sont l'arsenic, le mercure, le plomb, la naphtalène, le benzo[a]pyrène, le fluoranthène et le pyrène.\nLe résultat du calcul des expositions montre que l'exposition étudiée est susceptible d'entraîner un risque pour la santé, principalement par le biais :\n- ingestion des sols pour les enfants (benzo[a]pyrène),\n- contact cutané (benzo[a]pyrène)\n- ingestion de végétaux cultivés sur le site (arsenic, benzo[a]pyrène, pyrène, plomb).",null,"Analyse des enjeux sanitaires (EQRS, ARR)","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000021201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Arsenic | Nickel | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000021201","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Piège hydraulique ou Confinement hydraulique | Ventilation de la zone non saturée (venting)"]
["SSP000021201","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2016-04-14 : LA SITUATION S'AMELIORE\nInformations complémentaires : Les résultats du deuxième bilan quadriennal 2012-2016 montrent que :\r\n- pour la surveillance de la pollution résiduelle et d'un éventuel impact au niveau du centre commercial (piézomètres PZ2', PZ3' et PZ4') : une diminution importante de l'ensemble des composés toxiques organiques et métalliques depuis le début du suivi en 2008, ainsi qu'une améliorarion constante de la qualité de la nappe d'eau souterraine ;\r\n- pour la surveillance d'un éventuel impact au niveau de la station-service (PZ5') : aucun impact significatif en composés toxiques organiques ou métalliques en lien avec un éventuel impact de la station-service sur la qualité de la nappe d'eau souterraine n'a été mis en évidence depuis 2008. Les concentrations en composés toxiques recherchés sont systématiquement inférieures au seuil de quantification, voire de détection.\r\n\r\nLa surveillance se poursuit. L'ensemble des résultats du suivi devra être présenté à l'inspection à l'issue d'une période d'un an pour statuer sur les modalités de la surveillance de la qualité des eaux souterraines.\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000021201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Nickel | Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000021201","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000021201","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000021201","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000021201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000021301","Exécution des travaux de réhabilitation",null,null," D’après le mémoire de cessation d’activité, des travaux de remise en état du site ont été poursuivis depuis novembre 2003, date de la dernière transmission de SA ARLEQUIN relative à l’avancement des travaux de dépollution du site susvisé. Il a donc été demandé par lettre préfectorale du 31 août 2006 au mandataire judiciaire de décrire de façon plus précise le traitement en place sur le site et de se positionner sur l’évolution de ce traitement en vue de rendre le site compatible avec l’usage futur qui par défaut reste un usage industriel. En effet, les dernières valeurs mesurées en août 2005 dans les eaux souterraines révèlent pour certains polluants des teneurs supérieures aux seuils autorisés pour un usage industriel et le traitement par «venting» des terres prévu pour compléter les travaux de pompage effectués depuis 2000 ne semble pas avoir été réalisé.","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Piège hydraulique ou Confinement hydraulique"]
["SSP000021301","Etude SSP et ingénierie des travaux de réhabilitation","2015-10-16",null,"Une Interprétation de l'Etats des Milieux -IEM- et une Evaluation Quantitative des risques Sanitaires -EQRS- (sur site et sur les sites PRB, GRAPHIC SB) ont été réalisées en 2013. Elles concluent à la compatibilité de l’état des milieux avec un usage de bureaux (usage actuel des trois bâtiments hors site contrairement au site ARLEQUIN qui n’a pas d’usage).",null,"Interprétation de l''état des milieux (IEM)","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000021301","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"L’étude simplifiée des risques transmise par la SA ARLEQUIN en août 2002 conclut à un classement du site en classe 2, nécessitant une surveillance en raison de la présence de polluants (COHV, BTEX, acétate d’éthyle et hydrocarbures totaux) dans la première nappe rencontrée au droit du site, la nappe des calcaires de Saint Ouen, située à une dizaine de mètre de profondeur.",null,"Analyse des enjeux sanitaires (EQRS, ARR)","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000021301","Exécution des travaux de réhabilitation",null,null,"L’ADEME a été chargée de la réalisation d’une étude environnementale afin d’évaluer la qualité chimique des milieux sur site et hors site. Des investigations des milieux des sols (sur site uniquement), eaux souterraines (sur site et hors site), air du sol (sur site et hors site) et air intérieur (sur site et hors site) ont été menées. Cette étude a été confiée à la société BURGEAP.\nLes investigations ont mis en évidence la présence de quatre sources de pollution, aux solvants principalement, au sein des sols (zone de dépotage au nord, zone de fuite des canalisations, zone de fuite de l’atelier et zone de stockage des fûts au sud). Il a été mis en évidence qu’au moins deux des sources de pollutions atteignent la nappe des eaux souterraines.\nUne phase flottante a été mise en évidence au droit du site sur une surface au sol d’environ 700 m². Il a également été mis en évidence qu’un panache de composés dissous se développe en direction du sud est à l’extérieur de l’emprise du site.\nLes investigations sur les gaz mettent en avant une forte dégradation de la qualité de ce milieu au droit de la zone de fuite des canalisations et de la zone de fuite de l’atelier.",null,"N/A","N/A","N/A","N/A","Travaux de dépollution"]
["SSP000021301","Exécution des travaux de réhabilitation",null,null," Compte tenu des niveaux de pollution mesurés, un arrêté préfectoral complémentaire du 15 janvier 2008 a été pris à l'encontre des mandataires. Cet arrêté préfectoral impose au représentant de l'exploitant de:\n- caractériser l'état des milieux et des risques potentiels (délai : 3 mois);\n- proposer des mesures afin de restaurer des usages compatibles avec les niveaux de pollutions en présence (délai : 3 mois);\n- mettre en place une surveillance des eaux souterraines sur site et hors site (1er rapport à remettre dans un délai de 2 mois).\n",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage | Interdiction d'accès (clôture...) | Pompage de rabattement ou de récupération","N/A","N/A","N/A"]
["SSP000021301","Surveillance environnementale","2015-10-16","2016-01-01","Dans le cadre de l'intervention de l'ADEME, les arrêtés suivants ont été pris:\n- arrêté préfectoral n°15 DCSE SERV 03 du 27 mai 2015 prescrivant l'exécution de travaux d'office sur le site ayant été exploité par la société SA ARLEQUIN sur le territoire de la commune de Mitry-Mory et confiant la maîtrise d'ouvrage desdits travaux à 'Agence de l'Environnement et de la Maîtrise de l’Énergie (ADEME) ;\n- arrêté préfectoral n°15 DCSE SERV 09 du 16 octobre 2015 modifiant l'arrêté préfectoral n° 15 DCSE SERV 03 du 27 mai 2015 autorisant les agents de l'ADEME et le personnel des entreprises auxquelles elle délègue ses droits à occuper temporairement la parcelle de terrain située sur le site anciennement exploité par la SA ARLEQUIN sur le territoire de la commune de MITRY-MORY en vue d'effectuer des opérations de surveillance du site.\n\nLe rapport de l'ADEME présentant la campagne d'investigations de janvier 2016 pour les eaux souterraines et de janvier et mars 2016 pour le milieu air du sol confirme l'existence d'une lentille de phase flottante au droit du site. La nappe est fortement impactée en BTEX, hydrocarbures, HAP, COHV et acétates. Cette campagne confirme également la migration de la pollution sous forme dissoute en dehors du site en direction du Sud-Ouest.\nCe rapport confirme la dégradation significative de la qualité de ce milieu par les COHV, BTEX, hydrocarbures et acétates au droit du site et notamment au niveau de l'ancien atelier. Hors site, cette campagne montre une amélioration de la qualité de l'air du sol par rapport à novembre 2012.\n\nLa surveillance des milieux eaux souterraines et gaz du sol sur site et hors site se poursuit.\n\nCompte tenu du fort impact mis en évidence dans les sols, la nappe et les gaz de sols au droit des zones sources (situées en partie sous le bâtiment principal), l’ADEME rappelle qu’il appartiendra à tout nouvel acquéreur ou utilisateur de consolider ce constat par de nouvelles campagnes de mesures dont a minima l’analyse de l’eau du robinet et de nouvelles analyses de la qualité de l’air intérieur. Un plan de gestion devra aussi être réalisé en cas de travaux sur les sols (en cas de démolition ou de nouvelle construction) ou de modification de l’usage du site et/ou du bâtiment.\nDe plus, même si la compatibilité des milieux avec leur usage est avérée, et la source de pollution relativement stabilisée, compte tenu de la présence de cette source de pollution concentrée au droit du site (sous forme de lentille de flottant à la surface de la nappe et de sols imprégnés au droit des canalisations et de l’atelier) et conformément à la politique de gestion des sites et sols pollués, la réalisation d’un plan de gestion dédié à une intervention sur cette source de pollution concentrée serait souhaitable en vue de la résorber à terme.\nUn plan de gestion pourrait être incluse dans le projet d’aménagement du futur exploitant sachant qu’une bonne partie de la source est localisée sous le bâtiment principal du site et donc difficilement accessible à l’heure actuelle. Une attention particulière devra être portée sur la nature des polluants (mélange de solvants fortement corrosif) et des sols (peu perméables) qui peuvent rendre difficile le traitement. Il est à noter que les travaux menés entre 1998 et 2002 ont rencontré des difficultés opérationnelles pour ces raisons.",null,"N/A","1",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000021401","Etude SSP et ingénierie des travaux de réhabilitation","2004-02-03","2007-03-15","Les mesures de remise en état du site ont été demandées par arrêté préfectoral du 03 février 2004.\nLes déchets ont été éliminés,les 12 cuves dégazées et inertés, et les puits rebouchés.\nSur la totalité du site ont été réalisés : un diagnostic initial des sols et une évaluation simplifiée des risques, ainsi qu'une investigation des eaux souterraines avec évaluation simplifiée des risques.\n\nDeux zones de pollution des sols ont été mises en évidence :\n- une zone estimée de 100 m2 autour d'une ancienne cuve à colle située à l'angle Sud-Est du bâtiment principal DEVOISSELLE,où des concentrations de chloroforme de 0,5 &#956;g/kg MS ont été relevées, ainsi que du tétrachlorométhane, du trichloréthylène, du tetrachloroéthylène. L'ensemble de tous ces éléments représentant une concentration totale en Composés Organiques Volatils de 1,34 &#956;g/kg MS.\n- une zone estimée de 3000 m2 dans la partie SIDEV, impactée par des xylènes, ethylbenzène, tétrachlorométhane, trichloréthylène, tétrachloroéthylène.",null,"Analyse des enjeux sanitaires (EQRS, ARR)","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000021501","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000021501","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000021501","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000021501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000021601","Etude SSP et ingénierie des travaux de réhabilitation",null,"2000-09-01","La SNCF a répondu par courrier du 04 septembre 2000, portant sur la cession d'une partie des terrains de 900 m2, qu'elle n'envisageait aucune action corrective, eu égard aux teneurs en polluants dans les sols.\n\nEn effet, les hydrocarbures absorbés dans le sol et les métaux lourds (cadmium, nickel, plomb, zinc), présentaient des teneurs inférieures aux valeurs de définition de source-sol utilisées dans le guide technique du ministère de l'environnement relatif à l'évaluation simplifiée des risques sur les sites pollués.",null,"Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000021601","Exécution des travaux de réhabilitation",null,"2012-06-01","En 2010, l'inspection des installations classées a été informée par l'inspection du travail de la réalisation d'un projet immobilier par la construction de logements sociaux, qui a donné lieu à une nouvelle étude de risque sanitaire pour le compte de l'aménageur proposant une excavation des terres polluées, des précautions pour les personnels lors de la phase de travaux et des dispositions constructives pour limiter l'impact d'une pollution résiduelle dans les locaux en sous-sol (ventilation).",null,"N/A","N/A","N/A","N/A","Travaux de dépollution"]
["SSP000021601","Exécution des travaux de réhabilitation",null,null,"Les déchets métalliques présents en surface ont été évacués du site.",null,"N/A","N/A","N/A","N/A","Travaux de dépollution"]
["SSP000021601","Exécution des travaux de réhabilitation",null,"2000-09-04"," Les déchets métalliques présents en surface ont été évacués du site.",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000021701","Exécution des travaux de réhabilitation","2007-08-02","2009-09-14"," • du 2 août 2007 au 22 août 2007 : dépollution du site hors emprise des talus\n- décapage des terres sur 1 m d'épaisseur,\n- dépollution de la zone hors emprise des talus,\n- pompage et écrémage des eaux souterraines avec traitement des hydrocarbures récupérés,\n- remblaiement de la zone avec les terres issues du décapage après avoir vérifié leur acceptabilité.\n• du 26 février 2008 au 11 mars 2008 : excavation des talus résiduels périphériques.\nA l'issue des opérations d'excavation, les résultats d'analyse des terres restant en place et des remblais ont été jugés, par la société SOCOTEC, conformes aux objectifs de dépollution fixés dans l'EDR.\nEnviron 1020 tonnes de terres souillées ont été envoyées dans un biocentre et 1632 m3 dans un centre d'enfouissement technique de classe 3.","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique","Piège hydraulique ou Confinement hydraulique"]
["SSP000022101","Etude SSP et ingénierie des travaux de réhabilitation","2004-01-27","2006-12-14","L'arrêté préfectoral n° 04DAI 2IC 029 du 27 janvier 2004 impose un diagnostic initial, une évaluation simplifiée des risques et une surveillance des eaux souterraines .\nUne étude de pollution, ESR a été transmise en février 2006. Les résultats mettent en évidence une pollution importante avec produits phytosanitaires dans les sols et la nappe.",null,"Analyse des enjeux sanitaires (EQRS, ARR)","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000022101","Exécution des travaux de réhabilitation","2002-04-09",null," Mise en sécurité du site par interdiction d'accès, gardiennage, évacuation de produits ou de déchets.",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000022301","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000022301","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000022301","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000022301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000022401","Exécution des travaux de réhabilitation",null,"2008-11-28"," Suite à la découverte de cette pollution, la société COOPER a engagé en 2008 de sa propre initiative des travaux de dépollution.\nCes travaux comprenaient l’installation d'un système de pompage et d’écrémage des hydrocarbures surnageant et de l'eau la plus impactée, ainsi que la mise en place d’une unité pilote de traitement des eaux. Ces travaux ont duré 9 mois.","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification | Ventilation de la zone non saturée (venting)"]
["SSP000022401","Etude SSP et ingénierie des travaux de réhabilitation",null,"2007-11-29","La société COOPER a fait réaliser en 2007 avant la réalisation de travaux, un diagnostic de l’état des sols et des eaux souterraines du site ; Ce diagnostic a mis en évidence une pollution notamment en hydrocarbures totaux, des eaux souterraines qui se situent à environ 3-5 m de profondeur.",null,"Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000022401","Etude SSP et ingénierie des travaux de réhabilitation",null,"2012-10-23","L’étude d’octobre 2012 comprend une analyse des risques résiduels afin de vérifier la compatibilité des mesures de gestion. Les voies de transfert par ingestion des sols, inhalation de vapeur de polluants issues de la nappe et inhalation de vapeurs de polluants présents dans les sols ont été considérées dans les calculs de risques.\n\nCette analyse a mis en évidence pour les futurs employés du site des risques inférieurs à 1 et des excès de risque individuel inférieurs à 10-5.\nAinsi, l’étude conclut que la qualité environnementale des sols et des eaux souterraines du site est compatible avec un usage industriel et de poursuivre la surveillance des eaux souterraines sur les 3 piézomètres actuellement suivis. Les paramètres à analyser restent les mêmes : indice hydrocarbures, BTEX, COHV, HAP et 8 métaux toxiques.\n\nL'exploitant a transmis en octobre 2015 une mise à jour de l'analyse des risques résiduels. L'étude conclut que la qualité environnementale des sols, des gaz des sols et des eaux souterraines du site est compatible avec un usage industriel des terrains sous réserve de l'absence d'utilisation de l'eau souterraine. ",null,"Analyse des enjeux sanitaires (EQRS, ARR)","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000022401","Etude SSP et ingénierie des travaux de réhabilitation",null,"2009-10-01","Lors de cette phase pilote en 2009, une nouvelle campagne d’analyses de sol a été réalisée et a mis en évidence une pollution des sols. Les teneurs en hydrocarbures totaux s'élèvent à 1 750 mg/kg entre 1,7 et 3 m et croissent avec la profondeur pour atteindre 6 420 mg/kg à 5 m de profondeur, dans la zone de battement de la nappe. Cette pollution aux hydrocarbures est accompagnée de concentrations en toluène (1,38 mg/kg), éthylbenzène (12,2 mg/kg), xylènes (65,3 mg/kg) et naphtalène (24 mg/kg) significatives (concentrations maximales observées dans la zone de battement de la nappe).",null,"Plan de gestion","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000022401","Exécution des travaux de réhabilitation",null,"2012-10-23","Suite à cela, depuis août 2011 l’exploitant a décidé de mettre en œuvre un traitement des terres polluées du site par excavation et ensemencement biologique. A ce traitement s’ajoute une opération de récupération des hydrocarbures surnageant sur la nappe.",null,"N/A","N/A","N/A","N/A","Travaux de dépollution"]
["SSP000022401","Exécution des travaux de réhabilitation",null,"2015-05-28","restrictions d'usage prises afin notamment de conserver la mémoire des pollutions résiduelles présentes sur le site compatibles avec un usage industriel et de garantir la mise en œuvre d’un plan de gestion en cas de changement d’usage. D’après l’exploitant, ces restrictions d’usage prendront la forme de restrictions d’usage entre parties lors de la vente des terrains.",null,"N/A","N/A","N/A","N/A","Restriction d'usage proposée",null,"N/A","N/A","N/A"]
["SSP000022501","Etude SSP et ingénierie des travaux de réhabilitation",null,"2011-01-10"," L'exploitant a transmis en janvier 2011 un diagnostic environnemental du site.\nDeux captages d'alimentation ont été identifiés à proximité du site, en amont hydraulique de celui-ci. Le site se trouve également dans la zone ZICO \"BASSE ET PLAINES ADJACENTES\", à 500m d'un site NATURA 2000 et 500m de plusieurs ZNIEFF.\n\nLes sondages de sol effectués montrent la présence :\n- de composés azotés (ammonium, nitrates).\n- de métaux lourds, notamment en chrome ;\n- d'indices hydrocarbures totaux ;\n- de HAP ;\n- d'une légère contamination au PCB au niveau du transformateur ;\n\nL'étude recommande la surveillance semestrielle des eaux de la nappe par prélèvements d'eau souterraine dans les 3 piézomètres. Le schéma conceptuel fait apparaître les eaux souterraines et les eaux de surface comme des milieux d'expositions pertinents.\n","Eaux souterraines","Diagnostic et Analyse","N/A","Ammonium","Paramètres azotés","N/A","N/A","N/A","N/A","N/A"]
["SSP000022601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000022901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000023201","Surveillance environnementale","2004-03-01",null,"","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000023701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000023701","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000023701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000023801","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique","Piège hydraulique ou Confinement hydraulique"]
["SSP000023801","Surveillance environnementale","1998-02-01","2011-10-03","Résultat de la surveillance à la date du 2011-02-01 : LA SITUATION RESTE STABLE\nCommentaire : Le dispositif de surveillance est levé\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000023801","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000023801","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000023801","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Lavage à l'eau"]
["SSP000023801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Pompage de rabattement ou de récupération","N/A","N/A","N/A"]
["SSP000023901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000023901","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000023901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000023901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000024001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Cuivre | Plomb | Zinc","HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000024001","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000024001","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000024001","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000024001","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000024001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage | Interdiction d'accès (clôture...) | Pompage de rabattement ou de récupération | Reconditionnement de produits dangereux, Reconditionnement de déchets","N/A","N/A","N/A"]
["SSP000024201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Cyanures libres","Autres éléments minéraux","N/A","N/A","N/A","N/A","N/A"]
["SSP000024201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cyanures libres","Autres éléments minéraux","N/A","N/A","N/A","N/A","N/A"]
["SSP000024201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000024401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Arsenic | Chrome","COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000024401","Surveillance environnementale","2008-01-26",null,"Résultat de la surveillance à la date du : 2014-11-17\nRésultat de la surveillance eaux souterraines : 2\nréaparition du benzène sur tous les piézomètres sauf PZ44\r\nstabilité des xylènes totaux et de l'éthylbenzène en PZ44\r\nDiminution des hydrocarbures totaux \r\nstabilité de l'arsenic\r\ndiminution des COHV\n","Eaux souterraines","N/A","1",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000024401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Cuivre | Plomb","COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000025001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | COHV, solvants chlorés, fréons | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000025001","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Ventilation de la zone non saturée (venting)"]
["SSP000025001","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2018-09-04 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000025001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Arsenic | Cadmium | Plomb","COHV, solvants chlorés, fréons | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000025001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000025001","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000025001","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000025001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000025001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique"]
["SSP000025001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000025301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000025401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Chrome","COHV, solvants chlorés, fréons | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000025401","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification","Filtration"]
["SSP000025401","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du : 2017-06-30\nRésultat de la surveillance eaux souterraines : 1\n","Eaux souterraines","N/A","1",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000025401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Chrome","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000025401","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Ventilation de la zone non saturée (venting)"]
["SSP000025401","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage","N/A","N/A","N/A"]
["SSP000025501","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Piège hydraulique ou Confinement hydraulique"]
["SSP000025501","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000025501","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000025601","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Ventilation de la zone non saturée (venting)"]
["SSP000025601","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Solidification/stabilisation","Ventilation de la zone non saturée (venting)"]
["SSP000025601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...) | Pompage de rabattement ou de récupération","N/A","N/A","N/A"]
["SSP000025701","Surveillance environnementale",null,null,"surveillance effectuée","Eaux superficielles - Sédiments","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000025701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," plan de gestion","Sol - Sous-sol","Plan de gestion","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000025701","Exécution des travaux de réhabilitation",null,null," réhabilitation",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000025801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000026101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Chrome","COHV, solvants chlorés, fréons | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000026101","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Piège hydraulique ou Confinement hydraulique","Filtration"]
["SSP000026101","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2017-03-01 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000026101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cadmium | Chrome","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000026201","Etude SSP et ingénierie des travaux de réhabilitation","2000-10-01","2000-10-01"," Diagnostic","Eaux souterraines","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000026201","Surveillance environnementale","2000-10-01","2000-10-01","Arrêt de la surveillance.","Eaux souterraines","N/A","1",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000026201","Etude SSP et ingénierie des travaux de réhabilitation","2000-10-01","2000-10-01"," Diagnostic","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000026201","Exécution des travaux de réhabilitation","2000-10-01","2000-10-01","Dépollution","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols","Ventilation de la zone non saturée (venting)"]
["SSP000026201","Exécution des travaux de réhabilitation","2000-10-01","2000-10-01","Dépollution","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique","Ventilation de la zone non saturée (venting)"]
["SSP000026301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Arsenic | Trichloroéthylène","COHV, solvants chlorés, fréons | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000026301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Trichloroéthylène","COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000026301","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000026301","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000026301","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000026301","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000026301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000027201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Arsenic | Cadmium | Chrome | Cuivre | Fer | Nickel | Plomb | Zinc","COHV, solvants chlorés, fréons | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000027201","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2013-05-23 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","1",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000027201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Zinc","HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000027301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Arsenic | Cadmium | Chrome | Cuivre | Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Trichloroéthylène","Benzène et dérivés | COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000027301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Chrome | Cuivre | Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000027301","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000027301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000027501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | COHV, solvants chlorés, fréons | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000027501","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Ventilation de la zone non saturée (venting)"]
["SSP000027501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A",null,"COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés)","N/A","N/A","N/A","N/A","N/A"]
["SSP000027501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage","N/A","N/A","N/A"]
["SSP000027701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de gestion","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000027701","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Oxydation chimique"]
["SSP000027701","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2019-03-01 : LA SITUATION S'AMELIORE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000027701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000027701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000027701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000027801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de gestion","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000027801","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2011-10-12 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000027801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000027801","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000027801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000027901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000027901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000028101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000028101","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique","Ventilation de la zone non saturée (venting)"]
["SSP000028101","Surveillance environnementale","2008-01-01",null,"Résultat de la surveillance à la date du 2017-09-01 : LA SITUATION RESTE STABLE\nCommentaire : Teneurs en hydrocarbures et BTEX (Benzène, toluène, éthylbenzène et xylènes) élevées, mais relativement stable.\nInformations complémentaires : Les campagnes de surveillance de qualité des eaux souterraines ont permis de mettre en évidence un impact significatif en hydrocarbures C5-C40 et en BTEX dans les eaux souterraines en aval de l’emprise de l’ancienne station-service avec une migration des teneurs vers le sud-est, bien qu’une atténuation soit constatée dans les ouvrages les plus en aval.\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000028101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000028101","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000028101","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000028101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...) | Reconditionnement de produits dangereux, Reconditionnement de déchets","N/A","N/A","N/A"]
["SSP000028601","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"  Diagnostics et ARR réalisés","Eaux souterraines","Analyse des enjeux sanitaires (EQRS, ARR)","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000028601","Exécution des travaux de réhabilitation",null,null,"Excavation des terres impactées au niveau des anciennes cuves de stockage et du séparateur à hydrocarbures, et traitement de l’air du sol (par un procédé de venting) et des eaux souterraines (par des procédés de décantation et de stripping).","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Piège hydraulique ou Confinement hydraulique | Ventilation de la zone non saturée (venting)"]
["SSP000028601","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2017-03-13 : la situation reste stable (sauf au pz3 bis).\n","Eaux souterraines","N/A","1",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000028601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," Diagnostics et ARR réalisés","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000028601","Exécution des travaux de réhabilitation",null,null,"Excavation des terres impactées au niveau des anciennes cuves de stockage et du séparateur à hydrocarbures, et traitement de l’air du sol (par un procédé de venting) et des eaux souterraines (par des procédés de décantation et de stripping).","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols","Ventilation de la zone non saturée (venting)"]
["SSP000028601","Exécution des travaux de réhabilitation",null,null," Mesure de sécurité du site",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000028701","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"Diagnostic sols et nappe BURGEAP 02/08/2000\n ESR (2000)","Eaux souterraines","Diagnostic et Analyse","N/A",null,"COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP000028701","Exécution des travaux de réhabilitation",null,null,"  rapport fin de travaux ANTEA septembre 2005","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Piège hydraulique ou Confinement hydraulique | Ventilation de la zone non saturée (venting)"]
["SSP000028701","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"Diagnostic sols et nappe BURGEAP 02/08/2000\n ESR (2000)\n","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP000028701","Exécution des travaux de réhabilitation",null,null," rapport fin de travaux ANTEA septembre 2005","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000028701","Exécution des travaux de réhabilitation",null,null," rapport fin de travaux ANTEA septembre 2005","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000028701","Exécution des travaux de réhabilitation",null,null,"Mesure de mise en sécurité",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Pompage de rabattement ou de récupération","N/A","N/A","N/A"]
["SSP000028801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A","Arsenic | Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Zinc","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000028801","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000028801","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000028801","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000028801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...) | Reconditionnement de produits dangereux, Reconditionnement de déchets","N/A","N/A","N/A"]
["SSP000028901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000028901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000028901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000028901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000029201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cyanures libres","Autres éléments minéraux | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés)","N/A","N/A","N/A","N/A","N/A"]
["SSP000029501","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"  diagnostics en 1994 et 2000","Eaux souterraines","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000029501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," diagnostics en 1994 et 2000","Sol - Sous-sol","Diagnostic et Analyse","N/A","Plomb","COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000029501","Exécution des travaux de réhabilitation",null,null,"Des travaux de réhabilitation, comprenant notamment l’élimination de 500 m3 de terres polluées et un drainage passif sous les bâtiments, sont donc réalisés.","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000029501","Exécution des travaux de réhabilitation",null,null,"Des travaux de réhabilitation, comprenant notamment l’élimination de 500 m3 de terres polluées et un drainage passif sous les bâtiments, sont donc réalisés.","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000029701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Arsenic | Chrome | Cuivre | Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Trichloroéthylène | Zinc","Benzène et dérivés | COHV, solvants chlorés, fréons | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000029701","Surveillance environnementale","2006-11-29",null,"Résultat de la surveillance à la date du 2017-04-05 : LA SITUATION RESTE STABLE\nCommentaire : les teneurs en tétrachloroéthylène et trichloroéthylène sont en légère augmentation par rapport à la campagne précédente, mais reste inférieures aux valeurs retenues dans l'évaluation des risques sanitaires.\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000029701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Chrome | Cuivre | Mercure | Nickel | Plomb","COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000029701","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000029701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols","Confinement par couverture et étanchéification"]
["SSP000029701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000029801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP000029801","Surveillance environnementale","2006-03-15",null,"Résultat de la surveillance à la date du 2013-04-01 : LA SITUATION RESTE STABLE\nCommentaire : Impact en PCE sur l'ensemble des piézomètres (sauf Pz1 en aval, lors des 2 précédentes campagnes de 2012).\r\nAbsence d'impact en HCT et HAP confirmé\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000029801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000029801","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000029801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000029901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP000029901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cadmium | Cuivre | Cyanures libres | Mercure | Plomb","Autres éléments minéraux | COHV, solvants chlorés, fréons | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000029901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000029901","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000029901","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000029901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000030001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000030001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000030001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000030001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000030101","Etude SSP et ingénierie des travaux de réhabilitation","2014-01-01","2017-01-01"," IEM","Eaux souterraines","Interprétation de l''état des milieux (IEM)","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000030101","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2017-10-16 : LA SITUATION RESTE STABLE\nDate de fin envisagée de la surveillance : 2022-04-16","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000030101","Etude SSP et ingénierie des travaux de réhabilitation","2014-01-01","2017-01-01"," IEM","Sol - Sous-sol","Interprétation de l''état des milieux (IEM)","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000030201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de conception des travaux (PCT)","N/A",null,"COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP000030201","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000030201","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000030201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000030801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," Suivi des eaux souterraines sur le site interrompu.","Eaux souterraines","Interprétation de l''état des milieux (IEM)","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000030801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," Impacts dans les gaz des sols. Mesures dans l'air intérieur de certain riverains.","Sol - Sous-sol","Interprétation de l''état des milieux (IEM)","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000030801","Exécution des travaux de réhabilitation",null,null,"Travaux de dépollution (venting) de 2008 à 2011.","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Ventilation de la zone non saturée (venting)"]
["SSP000030801","Exécution des travaux de réhabilitation",null,null," Site propriété de l'établissement Plaine Commune.",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000031001","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Ventilation de la zone non saturée (venting)"]
["SSP000031001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Ventilation de la zone non saturée (venting)"]
["SSP000031001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000031401","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique"]
["SSP000031401","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000031501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés","N/A","N/A","N/A","N/A","N/A"]
["SSP000031501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés","N/A","N/A","N/A","N/A","N/A"]
["SSP000031501","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000031501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000031601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Trichloroéthylène","Benzène et dérivés | COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés)","N/A","N/A","N/A","N/A","N/A"]
["SSP000031601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000031601","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique"]
["SSP000031601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000031701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000031701","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Piège hydraulique ou Confinement hydraulique"]
["SSP000031701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000031701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000031701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000031701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Pompage de rabattement ou de récupération","N/A","N/A","N/A"]
["SSP000031801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000031901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Arsenic | Cuivre | Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Zinc","Benzène et dérivés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000031901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000031901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000032001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000032001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000032101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Ammonium | Cyanures libres","Autres éléments minéraux | Paramètres azotés","N/A","N/A","N/A","N/A","N/A"]
["SSP000032101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés)","N/A","N/A","N/A","N/A","N/A"]
["SSP000032101","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols","Confinement par couverture et étanchéification"]
["SSP000032101","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000032101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000032201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Cadmium | Nickel","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000032201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000032301","Surveillance environnementale",null,null,"","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000032301","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000032301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000032401","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000032401","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000032401","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000032501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000032601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Chrome | Plomb | Zinc","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000032601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Chrome | Plomb | Zinc","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000032601","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000032601","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000032701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000032701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000032701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000032801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000032801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Cuivre | Mercure | Plomb","COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000032801","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000032801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...) | Pompage de rabattement ou de récupération","N/A","N/A","N/A"]
["SSP000033401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés)","N/A","N/A","N/A","N/A","N/A"]
["SSP000033401","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000033701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Trichloroéthylène","COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP000033701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cuivre | Mercure | Plomb | Trichloroéthylène","COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000033701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000033901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A","Mercure | Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000033901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000033901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique"]
["SSP000033901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000034101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," En 1999 2001 et 2003 :diagnostics","Eaux souterraines","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000034101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," En 1999, 2001 et 2003 : diagnostics","Sol - Sous-sol","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000034101","Exécution des travaux de réhabilitation",null,null,"extraction de 200 m3 de terres polluées et le traitement biologique sur site de ces terres.","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000034101","Exécution des travaux de réhabilitation",null,null," Extraction de 200 m3 de terres polluées et le traitement biologique sur site de ces terres (2003)","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000034101","Exécution des travaux de réhabilitation",null,null,"extraction de 200 m3 de terres polluées et le traitement biologique sur site de ces terres.","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000034101","Exécution des travaux de réhabilitation",null,null," mise en sécurité",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000034201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Chrome | Cuivre | Nickel | Zinc","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000034201","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000034201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000034401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cyanures libres","Autres éléments minéraux","N/A","N/A","N/A","N/A","N/A"]
["SSP000034401","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000035001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique","Confinement par couverture et étanchéification"]
["SSP000035001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000035101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Arsenic | Baryum | Cadmium | Mercure | Plomb","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000035101","Surveillance environnementale","2001-03-27",null,"","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000035101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000035101","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000035101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000035201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Arsenic | Baryum | Cadmium | Mercure | Plomb","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000035201","Surveillance environnementale","2001-03-27",null,"","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000035201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000035201","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000035201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000035301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Plomb","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000035301","Surveillance environnementale",null,null,"","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000035301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Plomb","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000035301","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000035301","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000035301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000035401","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000035401","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000035401","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage","N/A","N/A","N/A"]
["SSP000035501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Arsenic","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000035501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Chrome | Plomb | Zinc","COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000035501","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000035501","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique","Confinement par couverture et étanchéification"]
["SSP000035501","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000035501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000035601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000035601","Surveillance environnementale","2002-06-04",null,"","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000035601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000035601","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Ventilation de la zone non saturée (venting)"]
["SSP000035601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000035701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de gestion","N/A","Chrome | Plomb | Trichloroéthylène","COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000035701","Surveillance environnementale",null,null,"","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000035701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A","Chrome | Cuivre | Plomb","COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000035701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000035701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000035801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Trichloroéthylène","COHV, solvants chlorés, fréons | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000035801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000035901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000035901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000035901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000036001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000036001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000036101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP000036101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Chlorures | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Autres éléments minéraux | Benzène et dérivés | COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP000036101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000036201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Ammonium | Chlorures | Fer | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Autres éléments minéraux | Benzène et dérivés | COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | Metaux et métalloïdes | Paramètres azotés","N/A","N/A","N/A","N/A","N/A"]
["SSP000036201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Chlorures | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Autres éléments minéraux | Benzène et dérivés | COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP000036201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000036301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Interprétation de l''état des milieux (IEM)","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP000036301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Interprétation de l''état des milieux (IEM)","N/A","Chlorures | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Autres éléments minéraux | Benzène et dérivés | COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP000036301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000036501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de gestion","N/A","Chlorures","Autres éléments minéraux | COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP000036501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A","Arsenic | Cadmium | Chrome | Cuivre | Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Zinc","Benzène et dérivés | COHV, solvants chlorés, fréons | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000036501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage | Interdiction d'accès (clôture...) | Reconditionnement de produits dangereux, Reconditionnement de déchets","N/A","N/A","N/A"]
["SSP000036502","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000036701","Exécution des travaux de réhabilitation",null,null,"Mise en sécurité du site par interdiction d'accès.",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000036801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Chrome | Cyanures libres","Autres éléments minéraux | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000036801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cadmium | Chrome | Cyanures libres | Plomb","Autres éléments minéraux | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000036801","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000036801","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000036801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000037001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000037201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A","Chrome","HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000037201","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000037201","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000037201","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000037201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000037301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000037401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Trichloroéthylène","COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP000037401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Chrome | Cuivre | Nickel | Trichloroéthylène | Zinc","COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000037401","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000037401","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000037401","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000037501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP000037501","Surveillance environnementale","2004-11-19",null,"Résultat de la surveillance à la date du 2006-10-01 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000037501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Cuivre | Nickel | Plomb","HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000037501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000037601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000037601","Surveillance environnementale","2004-11-01",null,"Résultat de la surveillance à la date du 2006-09-01 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000037601","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000037601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000037601","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000037601","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique","Ventilation de la zone non saturée (venting)"]
["SSP000037601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage | Interdiction d'accès (clôture...) | Reconditionnement de produits dangereux, Reconditionnement de déchets","N/A","N/A","N/A"]
["SSP000037701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Chrome | Cuivre | Nickel","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000037701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000037701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000037801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000037801","Surveillance environnementale","2006-07-01",null,"Résultat de la surveillance à la date du 2007-11-01 : LA SITUATION RESTE STABLE\nCommentaire : variations différentes selons les polluants\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000037801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | COHV, solvants chlorés, fréons | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000037801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000038001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A","Cadmium | Cuivre | Nickel | Plomb | Zinc","HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000038101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000038201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cadmium | Cuivre | Nickel | Plomb | Zinc","HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000038201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000038501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Trichloroéthylène","COHV, solvants chlorés, fréons | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000038501","Surveillance environnementale","2010-05-05",null,"Résultat de la surveillance à la date du 2012-04-02 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000038501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage","N/A","N/A","N/A"]
["SSP000038601","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000038601","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000038801","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000038801","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000038901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000038901","Surveillance environnementale","2001-06-29",null,"Résultat de la surveillance à la date du 2012-06-01 : LA SITUATION SE DEGRADE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000038901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés","N/A","N/A","N/A","N/A","N/A"]
["SSP000038901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique","Ventilation de la zone non saturée (venting)"]
["SSP000038901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000039301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Chrome | Trichloroéthylène","COHV, solvants chlorés, fréons | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000039301","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Piège hydraulique ou Confinement hydraulique"]
["SSP000039301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cadmium | Chrome | Cuivre | Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Trichloroéthylène","Benzène et dérivés | COHV, solvants chlorés, fréons | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000039301","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000039601","Surveillance environnementale",null,null,"","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000039601","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Biodégradation dynamisée (ou atténuation naturelle dynamisée) | Confinement par couverture et étanchéification"]
["SSP000039701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Arsenic | Cadmium | Chrome | Nickel | Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000039701","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Barbotage in situ (sparging)"]
["SSP000039701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Arsenic | Cadmium | Cuivre | Cyanures libres | Mercure | Nickel | Plomb | Zinc","Autres éléments minéraux | COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000039701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000039701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000039701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Pompage de rabattement ou de récupération","N/A","N/A","N/A"]
["SSP000039801","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000039801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000039901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de conception des travaux (PCT)","N/A","Chrome | Nickel","COHV, solvants chlorés, fréons | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000039901","Surveillance environnementale",null,null,"","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000039901","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","1",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000039901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de conception des travaux (PCT)","N/A","Chrome | Nickel","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000039901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000040001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP000040001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Plomb","COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000040001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000040101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Chrome","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000040101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000040201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000040201","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2012-09-07 : LA SITUATION RESTE STABLE\nInformations complémentaires : Le sens d’écoulement de la nappe est orienté vers le Sud-Est.\r\n\r\nIl existe 4 piézomètres :\r\n- Pz1 : le plus proche du puits Couchoud,\r\n- Pz2 : à l'amont hydraulique de tous les piézomètres,\r\n- Pz3 : à l'aval hydraulique et topographique des anciennes cuves du dépôt pétrolier,\r\n- Pz4 : à l'aval hydraulique de Pz1.\r\n\r\nLa côte de la nappe phréatique, en m NGF est d'environ 96.\r\n\r\nLes informations ci-dessous résument le nombre de dépassements observés sur les 3 dernières campagnes par rapport aux critères de qualité définis à l'annexe 1 de la circulaire du 23/10/2012 :\r\n- Dichloroéthène-1,1 : 30 µg/L - Pas de suivi qualité des eaux pour ce contaminant,\r\n- Trichloroéthane-1,1,1 : 200 µg/L - Pas de suivi qualité des eaux pour ce contaminant,\r\n- Trichloroéthylène : 10 µg/L - 3 dépassements (aout 2011, mars 2012, aout 2012) max 250 µg/l,\r\n- Chlorure de vinyle : 0,5 µg/L - Pas de suivi qualité des eaux pour ce contaminant,\r\n- Benzène : 1 µg/L - 3 dépassements (aout 2011, mars 2012, aout 2012) max 180 µg/l,\r\n- Toluène : 0,7 µg/L - Pas de suivi qualité des eaux pour ce contaminant,\t\r\n- Xylène ortho + méta + para : 0,5 µg/L - Pas de suivi qualité des eaux pour ce contaminant.\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000040201","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000040201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000040201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000040301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Arsenic | Cuivre | Nickel | Zinc","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000040301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cuivre | Mercure | Zinc","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000040401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000040401","Surveillance environnementale",null,"2016-04-01","Résultat de la surveillance à la date du : 2016-04-01\nRésultat de la surveillance eaux souterraines : 2\nUne légère pollution  aux COHV est présente au droit du site avec des teneurs du même ordre de grandeur entre l'amont et l'aval ne mettant pas en avant un impact du site.\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000040401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Cuivre | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000040401","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)","Confinement par couverture et étanchéification"]
["SSP000040401","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000040501","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2009-05-26 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000040501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Plomb","Hydrocarbures et indices liés | Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000040501","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000040501","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000040501","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000040501","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000040501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000040601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Chrome | Cuivre | Nickel | Zinc","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000040601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000040701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Chrome","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000040701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Chrome","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000040701","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000040701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000040801","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du : 2004-04-20\nRésultat de la surveillance eaux souterraines : 1\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000040801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Cadmium | Cuivre | Mercure | Plomb","HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000040801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000040901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP000040901","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2003-04-09 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000040901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP000040901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000040901","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000041001","Surveillance environnementale","2012-01-01",null,"Résultat de la surveillance à la date du 2004-11-04 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000041001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000041401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic","HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000041501","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique"]
["SSP000041601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Ammonium | Cyanures libres","Autres éléments minéraux | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Paramètres azotés","N/A","N/A","N/A","N/A","N/A"]
["SSP000041601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000041601","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000041601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000041701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000041701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000041701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000041701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique"]
["SSP000041701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000041801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Arsenic | Cobalt | Nickel","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000041801","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2001-02-26 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000041801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Cobalt | Nickel","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000041801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000041901","Surveillance environnementale","2004-04-05",null,"Résultat de la surveillance à la date du : 2012-01-01\nRésultat de la surveillance eaux souterraines : 1\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000041901","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000041901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000041901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000041901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000042001","Surveillance environnementale","2004-04-05",null,"Résultat de la surveillance à la date du 2016-03-30 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000042001","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000042001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000042001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000042101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000042101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic","COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000042101","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000042101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000042201","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","1",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000042301","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2015-04-01 : LA SITUATION RESTE STABLE\nDate de fin envisagée de la surveillance : 2015-08-01","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000042301","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000042301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000042401","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","1",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000042401","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000042501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Nickel","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000042501","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2005-10-01 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000042501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Chrome | Cuivre | Nickel | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000042601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A","Chrome | Cuivre | Plomb","COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000042601","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000042601","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique"]
["SSP000042601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000042701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"COHV, solvants chlorés, fréons | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000042701","Surveillance environnementale","2004-12-02",null,"Résultat de la surveillance à la date du 2017-09-01 : LA SITUATION S'AMELIORE\nInformations complémentaires : Le sens d’écoulement de la nappe est orienté du Sud – Sud/Ouest vers le Nord - Nord/Est.\r\nIl existe 3 piézomètres :\r\n- le piézomètre Pz1 en aval,\r\n- les piézomètres Pz2 et PZ3 en amont.\r\n\r\nla côte de la nappe phréatique, en m NGF est d'environ 92\r\n\r\nLes informations ci-dessous résument le nombre de dépassements observés sur les 3 dernières campagnes par rapport aux critères de qualité définis à l'annexe 1 de la circulaire du 23/10/2012.\r\nTetrachloroéthylène : 10 µg/L - 0 dépassement (03/2009, 08/2010 et 10/2010)\r\nTrichloroéthylène : 10 µg/L - 0 dépassement  (03/2009, 08/2010 et 10/2010)\r\nHCT  : 1000 µg/L - 0 dépassement  (03/2009, 08/2010 et 10/2010)\r\n\r\nLes résultats de la surveillance des eaux souterraines sur les paramètres hydrocarbures totaux (C10-C40), HAP et COHV ne mettent pas en avant d’impacts des activités ICPE exercées au droit du site sur la qualité des eaux souterraines incompatibles avec l’usage du site de type « commercial_industriel_artisanal ».\r\nAu regard des résultats obtenus lors des campagnes de surveillance des eaux souterraines et particulièrement ceux obtenus au cours des années 2016 et 2017, la surveillance des eaux souterraines au droit du site industriel exploité par la société Peyraverney au lieu dit « La Bascule » à Saint-Pierre-de-Boeuf peut être arrêtée.\r\nL’inspection demande de procéder à la neutralisation des ouvrages de surveillance des eaux souterraines selon les règles de l’art afin de garantir l'absence de circulation d'eau et l'absence de transfert de pollution. Il doit être transmis, dans un délai de 2 mois après les travaux de neutralisation, le compte rendu des travaux réalisés. Cette formalité met fin aux obligations d’entretien et de surveillance de l’ouvrage.\nDate de fin envisagée de la surveillance : 2017-09-01","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000042701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000042701","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000042701","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000042701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique"]
["SSP000042701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...) | Pompage de rabattement ou de récupération","N/A","N/A","N/A"]
["SSP000042801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP000042801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cadmium | Chrome | Cuivre | Cyanures libres | Nickel | Plomb","Autres éléments minéraux | COHV, solvants chlorés, fréons | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000042801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000042802","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP000042802","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000042901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000042901","Surveillance environnementale","2004-03-02",null,"Résultat de la surveillance à la date du 2004-07-22 : LA SITUATION S'AMELIORE\nCommentaire : teneur en hydrocarbures reste supérieure à la VCI\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000042901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000042901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000042901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000043001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic","HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000043001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique","Ventilation de la zone non saturée (venting)"]
["SSP000043101","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)","Ventilation de la zone non saturée (venting)"]
["SSP000043101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000043201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000043301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de gestion","N/A","Arsenic | Nickel | Plomb","COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000043301","Surveillance environnementale","2010-07-01",null,"Résultat de la surveillance à la date du 2013-02-01 : LA SITUATION RESTE STABLE\nInformations complémentaires : Le sens d’écoulement de la nappe est orienté du Nord-Ouest vers le Sud-Est.\r\n\r\nIl existe 5 piézomètres :\r\n- PZA est positionné en amont latéral hydraulique,\r\n- PZB est positionné en aval latéral hydraulique,\r\n- PZC est positionné en aval hydraulique,\r\n- PZD se situe en amont hydraulique,\r\n- PZE se situe en aval hydraulique.\r\n\r\nLes informations ci-dessous résument le nombre de dépassements observés sur les 3 dernières campagnes par rapport aux critères de qualité définis à l'annexe 1 de la circulaire du 23/10/2012 :\r\n- Hydrocarbures dissous : 1000 µg/L - non prescrit mais analyses réalisées par la mairie à fréquence semestrielle – 1 dépassement (07/2012 : 3700 µg/l),\r\n- TCA : 200 µg/L - non prescrit mais analyses réalisées par la mairie à fréquence semestrielle - 3 dépassements (07/2012, 11/2012, 02/2013 : 700 µg/l),\r\n- TCE : 10  µg/L - non prescrit mais analyses réalisées par la mairie à fréquence semestrielle – 1 dépassement (07/2012 : 10 µg/l),\r\n- Nickel : 20 µg/l - non prescrit mais analyses réalisées par la mairie à fréquence semestrielle – 3 dépassements (07/2012, 11/2012, 02/2013 : 700 µg/l).\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000043301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A","Arsenic","COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000043301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000043401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Mercure","HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000043401","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2011-10-01 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000043401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Cuivre | Mercure","COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000043501","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000043501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000043601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de gestion","N/A","Arsenic | Cadmium | Chrome | Cuivre | Mercure | Nickel | Plomb | Zinc","HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000043601","Surveillance environnementale","2009-08-20",null,"Résultat de la surveillance à la date du 2011-08-31 : LA SITUATION S'AMELIORE\nInformations complémentaires : Le sens d’écoulement de la nappe est orienté du Sud-Ouest vers le Nord-Est.\r\n\r\nIl existe 5 piézomètres :\r\n- Pz2,\r\n- Pz3,\r\n- Pz4,\r\n- Pz6 : hors site à l'aval hydraulique de la zone dite \"des fosses rondes\", \r\n- PZ7 : hors site à l'aval hydraulique de la zone dite \"des fosses rondes\", \r\n\r\nLa côte de la nappe phréatique, en m NGF est d'environ 98.\r\n\r\nLes informations ci-dessous résument le nombre de dépassements observés sur les 3 dernières campagnes par rapport aux critères de qualité définis à l'annexe 1 de la circulaire du 23/10/2012 :\r\n- Hydrocarbures dissous : 1000 µg/L – Pas de suivi de qualité des eaux prescrit pour ce contaminant- 1 dépassement (03/2011 : 1810 µg/l hors site).\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000043601","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000043601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A","Arsenic | Cadmium | Cuivre | Plomb | Zinc","HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000043601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000043701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de gestion","N/A",null,"COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000043701","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,null,"Filtration"]
["SSP000043701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A","Trichloroéthylène","COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000043701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols","Confinement par couverture et étanchéification"]
["SSP000043701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Lavage à l'eau","Confinement par couverture et étanchéification"]
["SSP000043701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique","Confinement par couverture et étanchéification"]
["SSP000043701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000043801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000043901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols","Confinement par couverture et étanchéification"]
["SSP000043901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique","Confinement par couverture et étanchéification"]
["SSP000043901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000044001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Cuivre | Plomb","COHV, solvants chlorés, fréons | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000044101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000044101","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,null,"Filtration"]
["SSP000044101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000044101","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000044101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000044201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Cadmium | Cuivre | Nickel","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000044201","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000044201","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000044201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000044301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cyanures libres","Autres éléments minéraux","N/A","N/A","N/A","N/A","N/A"]
["SSP000044301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000044401","Exécution des travaux de réhabilitation",null,null,"Travaux dépolllution","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols","Confinement par couverture et étanchéification"]
["SSP000044401","Exécution des travaux de réhabilitation",null,null,"Travaux dépolllution","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Lavage à l'eau","Confinement par couverture et étanchéification"]
["SSP000044401","Exécution des travaux de réhabilitation",null,null," Evacuation déchets",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000044501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000044601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de gestion","N/A","Nickel | Trichloroéthylène","COHV, solvants chlorés, fréons | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000044601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A","Arsenic | Nickel | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000044701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Chrome | Cuivre | Nickel | Plomb","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000044801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés | Phytosanitaires","N/A","N/A","N/A","N/A","N/A"]
["SSP000044801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Chrome | Nickel | Plomb | Zinc","Hydrocarbures et indices liés | Metaux et métalloïdes | Phytosanitaires","N/A","N/A","N/A","N/A","N/A"]
["SSP000044801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000044901","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000044901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000045001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000045001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000045101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Cuivre | Plomb","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000045201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Cadmium | Nickel","COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000045201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cuivre | Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000045501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cuivre | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000045601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Chrome | Cuivre | Mercure | Plomb | Zinc","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000045601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000045701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000045801","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000045901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A","Arsenic | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000046001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Arsenic | Chrome | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | COHV, solvants chlorés, fréons | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000046001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Chrome | Mercure | Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Zinc","Benzène et dérivés | COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000046101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Aluminium | Arsenic","HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000046101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Mercure | Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000046101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000046201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000046201","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000046201","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000046201","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000046201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000046301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," Réception du plan de gestion","Sol - Sous-sol","Plan de gestion","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000046301","Exécution des travaux de réhabilitation",null,null,"Travaux de dépollution","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000046401","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000046401","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000046501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de gestion","N/A","Arsenic","Hydrocarbures et indices liés | Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000046501","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2016-01-01 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000046501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A","Cuivre | Plomb","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000046601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000046601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000046701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Chrome | Mercure | Nickel | Plomb","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000046701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000046701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000046801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000046801","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2007-07-23 : LA SITUATION S'AMELIORE\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000046801","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000046801","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)","Confinement par couverture et étanchéification"]
["SSP000046801","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000046801","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000046801","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000046801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000046901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés)","N/A","N/A","N/A","N/A","N/A"]
["SSP000046901","Surveillance environnementale",null,null,"","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000046901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000046901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000046901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000046901","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000046901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Lavage à l'eau"]
["SSP000046901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000046901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique"]
["SSP000046901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Solidification/stabilisation"]
["SSP000046901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000047001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés)","N/A","N/A","N/A","N/A","N/A"]
["SSP000047001","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000047001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique"]
["SSP000047101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Ammonium | Chrome | Cyanures libres | Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Autres éléments minéraux | Benzène et dérivés | Metaux et métalloïdes | Paramètres azotés","N/A","N/A","N/A","N/A","N/A"]
["SSP000047101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés)","N/A","N/A","N/A","N/A","N/A"]
["SSP000047101","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique"]
["SSP000047101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000047102","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Arsenic | Cyanures libres | Nickel","Autres éléments minéraux | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000047102","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Cyanures libres | Nickel | Plomb","Autres éléments minéraux | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000047201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Cadmium | Chrome | Cuivre | Cyanures libres | Nickel | Plomb | Zinc","Autres éléments minéraux | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000047201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000047301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Arsenic | Chrome | Mercure | Nickel | Plomb","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000047301","Surveillance environnementale","2004-04-30",null,"Résultat de la surveillance à la date du 2013-04-30 : LA SITUATION RESTE STABLE\nCommentaire : Les résultats des analyses réalisées sur les eaux souterraines montrent ponctuellement des concentrations qui dépassent certains seuils de la circulaire du 23/10/2012 (prise en application de l'arrêté du 17 décembre 2008 établissant les critères d’évaluation et les modalités de détermination de l’état des eaux souterraines et des tendances significatives et durables de dégradation de l’état chimique des eaux souterraines) ; La dernière campagne où sont observés des dépassements est celle du 10/03/2011 :\r\n- pour l’arsenic : au droit de PZ STEP 4, 13 µg/L, pour une valeur-limite de 10 µg/L ;\r\n- pour le chrome : au droit de PZ STEP 4, 78 µg/L, pour une valeur-limite de 50 µg/L\r\n- pour le mercure : au droit de PZ1, 2,1 µg/L pour une valeur-limite de 1 µg/L ;\r\n- pour le nickel : au droit de PZ1, 60 µg/L, au droit de PZ STEP 4, 53 µg/L, pour une valeur-limite de 20 µg/L ;\r\n- pour le plomb : au droit de PZ1, 91 µg/L, au droit de PZ STEP 4, 81 µg/L, pour une valeur-limite de 10 µg/L.\r\n\r\nLe PZ1 est situé en amont supposé de l’ancienne usine d’incinération, PZ2 en aval direct supposé et PZ4 en aval supposé.\r\n\r\nLes analyses d’eaux superficielles (prélevées dans un petit cours d’eau longeant le site côté autoroute) ne montrent pas d’impact en amont (dernière quantification le 10/03/2011 : 16 µg/L de nickel et 170 µg/l de zinc) ni en aval (concentrations inférieures aux seuils de quantification du laboratoire pour tous les paramètres recherchés).\r\n\r\nLes analyses de sédiments réalisées depuis le 09/12/2010 montrent souvent un impact en hydrocarbures en aval par rapport aux teneurs observées en amont (ce qui n'est pas le cas pour la campagne du 30/04/2013). Concernant les métaux, les teneurs sont sensiblement les mêmes en amont et en aval.\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000047301","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000047301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Cadmium | Chrome | Cuivre | Nickel | Plomb","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000047301","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000047301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000047401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000047401","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000047401","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000047501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000047501","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2007-10-01 : LA SITUATION S'AMELIORE\nCommentaire : plus de trace d'HC dans la nappe\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000047501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000047501","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000047501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000047601","Surveillance environnementale","2009-07-01",null,"Résultat de la surveillance à la date du 2011-12-13 : LA SITUATION S'AMELIORE\nCommentaire : hydrocarbures ne sont plus quantifiés.\r\nteneur en Nickel stable\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000047601","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)","Confinement par couverture et étanchéification"]
["SSP000047601","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)","Confinement par couverture et étanchéification"]
["SSP000047601","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)","Confinement par couverture et étanchéification"]
["SSP000047601","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)","Confinement par couverture et étanchéification"]
["SSP000047601","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique","Confinement par couverture et étanchéification"]
["SSP000047601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Reconditionnement de produits dangereux, Reconditionnement de déchets","N/A","N/A","N/A"]
["SSP000047701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Trichloroéthylène","Benzène et dérivés | COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP000047701","Surveillance environnementale","2009-04-06",null,"Résultat de la surveillance à la date du 2012-02-01 : LA SITUATION RESTE STABLE\nCommentaire : L'arrêté préfectoral du 23/04/2010 prescrit la surveillance trimestrielle des eaux souterraines, pour recherche des hydrocarbures totaux, BTEX et COHV. Lors de la campagne du 01/02/2012, les seuils réglementaires sont dépassés pour le chlorure de vinyle (seuil = 0,5 µg/L) au droit de PZ3 (0,77 µg/L) et le benzène (seuil = 1 µg/L) au droit de PZ1 (1,04 µg/L) et de PZ2 (1,81 µg/L).\nInformations complémentaires : Les eaux souterraines sont présentes à faible profondeur, qui peuvent être en contact avec le réservoir karstique sous-jacent.\r\n\r\nLe réseau de surveillance est constitué comme suit : en amont PZ3 et en aval PZ1 et PZ2 ; Il est à noter que PZ3 a été implanté à l'amont immédiat de l'ancienne zone extérieure de stockage de bennes de déchets et de vernis et solvants.\r\n\r\nDepuis l'implantation des piézomètres, quatre campagnes de surveillance ont eu lieu : le 06/04/2009, le 26/05/2010, le 30/08/2010 et le 01/02/2012.\r\nLes seuils réglementaires sont dépassés pour le chlorure de vinyle (seuil = 0,5 µg/L) uniquement au droit de PZ3 (teneur maximum de 2,82 µg/l le 30/08/2010) et pour le benzène (seuil = 1 µg/L) au droit de PZ1 (maximum de 1,09 µg/L le 26/05/2010), de PZ2 (maximum de 2,27 µg/L le 06/04/2009)et de PZ3 (maximum de 1,9 µg/L le 06/04/2009).\r\n\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000047701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Trichloroéthylène","Benzène et dérivés | COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP000047801","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000047801","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000047801","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000047801","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique"]
["SSP000047801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000048001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Cuivre | Mercure | Plomb","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000048101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000048201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000048301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Chrome","HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000048301","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Piège hydraulique ou Confinement hydraulique"]
["SSP000048301","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2010-08-25 : LA SITUATION S'AMELIORE\nCommentaire : Absence de polluant dans la nappe depuis plusieurs années.\nInformations complémentaires : La surveillance est suspendue mais le dispositif reste en place.\r\nIl y a lieu de noter qu'une surveillance de la nappe est permanente par le gestionnaire du captage AEP qui n'a signalé aucune anomalie depuis plusieurs années.\r\n\n","Eaux souterraines","N/A","1",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000048301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Chrome | Cuivre","HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000048301","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique","Confinement par couverture et étanchéification"]
["SSP000048301","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Solidification/stabilisation","Confinement par couverture et étanchéification"]
["SSP000048301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Pompage de rabattement ou de récupération","N/A","N/A","N/A"]
["SSP000048601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Plomb | Zinc","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000048601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000048701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Arsenic | Mercure | Nickel | Plomb","HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000048701","Surveillance environnementale","2011-07-31",null,"Résultat de la surveillance à la date du 2011-07-31 : LA SITUATION RESTE STABLE\nInformations complémentaires : Les analyses des eaux souterraines réalisées en juillet 2011 sur 3 piézomètres ont mis en évidence les contaminations suivantes :\r\n- benzo(a)pyrène (0,08 µg/L sur PZ3) ;\r\n- HAP somme 4 (0,23 µg/L sur PZ3) ;\r\n- arsenic (37 µg/L sur PZ2) ;\r\n- nickel (36 µg/L sur PZ1) ;\r\n- plomb (85 µg/L sur PZ1 ; 91 µg/L sur PZ2 ; 88 µg/L sur PZ3) ;\r\n- mercure (1,39 µg/L sur PZ2) ;\r\n- PCB (0,11 µg/L sur PZ1 ; 0,27 µg/L sur PZ2 ; 0,1 µg/L sur PZ3) ;\r\n- HCT (0,06 mg/L sur PZ1 ; 0,04 mg/L sur PZ2 ; 0,15 mg/L sur PZ3).\r\n\r\nPar courrier du 19 juin 2013, il est demandé à M. DESGRAND de procéder à la surveillance semestrielle des eaux souterraines sur une période de 4 ans, comme il s’y est engagé.\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000048701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Cadmium | Cuivre | Mercure | Nickel | Plomb | Sulfates | Zinc","Autres éléments minéraux | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000048701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000048801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP000048801","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Piège hydraulique ou Confinement hydraulique | Ventilation de la zone non saturée (venting)"]
["SSP000048801","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2012-11-14 : LA SITUATION S'AMELIORE\nCommentaire : Résultats en amélioration constante dans les 2 points de mesure depuis le relargage ponctuel de 2006.\n","Eaux souterraines","N/A","1",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000048801","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000048801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Pompage de rabattement ou de récupération","N/A","N/A","N/A"]
["SSP000048901","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Piège hydraulique ou Confinement hydraulique"]
["SSP000048901","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000048901","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000048901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Lavage à l'eau","Ventilation de la zone non saturée (venting)"]
["SSP000048901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique","Ventilation de la zone non saturée (venting)"]
["SSP000048901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000049101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Chrome | Cuivre | Nickel | Plomb | Zinc","COHV, solvants chlorés, fréons | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000049101","Surveillance environnementale","2002-06-24",null,"Résultat de la surveillance à la date du 2012-09-24 : LA SITUATION RESTE STABLE\nCommentaire : Augmentation des teneurs en métaux (notamment cuivre, plomb et zinc sur le piézomètre 1).\r\nDiminution des solvants chlorés, notamment sur les piézomètres 2 et 3 (sauf trichlorotrifluoréthane sur le piézomètre 1)\nInformations complémentaires : Les analyses trimestrielles sur les piézomètres sont bien réalisées depuis 2008.\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000049101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Chrome | Cuivre | Mercure | Molybdène | Plomb | Sélénium | Zinc","COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000049101","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000049101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000049301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Chrome","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000049301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cadmium | Chrome | Trichloroéthylène | Zinc","COHV, solvants chlorés, fréons | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000049301","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000049301","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000049301","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000049301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000049501","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2015-09-14 : LA SITUATION S'AMELIORE\nCommentaire : Les éléments recueillis indiquent que les concentrations en BTEX et HCT au niveau des trois piézomètres sont inférieures aux seuils de détection du laboratoire. De plus, suite aux récents travaux effectués sur le site, un nivellement des piézomètres est à prévoir lors de la prochaine campagne de suivi de la qualité des eaux souterraines.\nInformations complémentaires : pas d'HCT présence de Toluène\r\nCampagne de juin & septembre 2015 : Les 2 campagnes de suivis de la qualité de la nappe, réalisées en juin et septembre 2015 montrent que les concentrations en BTEX et Hydrocarbures Totaux sont inférieurs aux seuils de détection du laboratoire. Un bilan quadriennal de la surveillance doit être adressé prochainement à l'inspection qui statuera sur le maintien ou non de cette surveillance.\r\n\r\nA la date du 7 juin 2016 : Lettre d'information du préfet actant la fin de la surveillance suite au bilan quadriennal.\nDate de fin envisagée de la surveillance : 2016-06-07","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000049501","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique"]
["SSP000049601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de gestion","N/A","Nickel | Plomb","HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000049601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A",null,"HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000049601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000049701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cadmium | Cuivre | Mercure | Plomb | Zinc","Hydrocarbures et indices liés | Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000049701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000049801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cadmium | Cuivre | Plomb | Zinc","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000049801","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000049801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000049901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000049901","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2011-02-28 : LA SITUATION RESTE STABLE\nInformations complémentaires : Présence de PCB (0,842 μg/L) et HAP (0,08 μg/L) dans la nappe située à une profondeur de 4 m au niveau du piézomètre Pz1.\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000049901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Cuivre | Plomb | Sulfates | Zinc","Autres éléments minéraux | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000049901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000050001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cadmium | Cuivre | Mercure | Plomb | Zinc","HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000050001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000050101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000050101","Surveillance environnementale","2011-05-31","2015-12-10","Résultat de la surveillance à la date du 2015-03-31 : LA SITUATION RESTE STABLE\nInformations complémentaires : L'arrêté préfectoral du 28 novembre 2011 a imposé à l'exploitant la surveillance trimestrielle des eaux souterraines via 3 piézomètres sur les HCT, les COHV et les BTEX durant au moins 4 ans.\r\n\r\nLa surveillance des eaux souterraines réalisée via 3 piézomètres de mai 2011 à septembre 2013 (9 campagnes) a mis en évidence les contaminations suivantes :\r\n- benzène sur MW1 : 2,3 µg/L en mai 2011, 1,4 µg/L en mars 2012 et 1 µg/L en septembre 2013 ;\r\n- BTEX totaux sur MW1 : entre 80 et 220 µg/L sur chaque campagne ;\r\n- HCT C10-C40 sur Mw1 : entre 1 000 et 1 600 µg/L sur chaque campagne sauf en mai 2011 (95 µg/L) et juin 2012 (520 µg/L).\r\n16/7/2014\r\nLa surveillance trimestrielle est effectué conformément à l' AP du 28/11/2011. Cette surveillance montre que les concentrations sur les paramètres HCT et BTEX sont faibles (quelques µg/L) et présente une stabilité dans le temps. Aucune anomalie n'a été mis en évidence à ce stade. Par ailleurs aucune trace d'HCT n'est retrouvée dans les piézomètres aval ce qui caractérise une pollution faible et très localisée.\r\n12/9/14\r\nLa Sté ENVIRON a réalisé une douzième campagne de surveillance environnementale le 20/6/14 afin d'observer l'évolution de la qualité des eaux souterraines depuis mai 2011. La qualité des eaux souterraines en aval du site reste compatible avec les limites de l'arrêté ministériel du 11 janvier 2007 relatif aux eaux de boisson, pour les paramètres recherchés.\r\nLa Sté ENVIRON a réalisé une treizième campagne de surveillance environnementale le 25/9/14 afin d'observer l'évolution de la qualité des eaux souterraines depuis mai 2011. Le niveau de la nappe a légèrement augmenté par rapport à juin 2014. Le sens d'écoulement est orienté sud et reste inchangé par rapport aux campagnes précédentes. La concentration en hydrocarbures totaux mesurée dans les eaux prélevées au droit de MW1 (170 µg/L) est inférieure à la limite de qualité des eaux brutes. La concentration en benzène dans les eaux prélevées au droit de MW1 est inférieure au seuil de détection analytique. La concentration en COHV est inférieure aux seuils de détection analytique.\r\nLa Sté ENVIRON a réalisé une quatorzième campagne de surveillance environnementale le 10/12/14 qui a pu mettre en évidence les points suivants :\r\n- Le niveau de la nappe a augmenté par rapport à septembre 2014. Le sens d'écoulement est orienté vers le sud et reste inchangé par rapport aux campagnes précédentes.\r\n- La concentration en hydrocarbures totaux mesurée dans les eaux prélevées au droit de MW1 (850 µg/L) est inférieure à la limite de qualité des eaux brutes utilisées pour la production d'eau destinée à la consommation humaine (1 000 µg/L).\r\n- La concentration en benzène dans les eaux prélevées au droit de MW1 (0,94 µg/L) est inférieure à la limite de qualité des eaux brutes utilisées pour la production d'eau destinée à la consommation humaine (1 µg/L).\r\n- Les concentration en COHV sont inférieures aux seuils de détection analytique pour les eaux prélevées dans les trois piézomètres lors de cette campagne.\r\nLes résultats analytiques indiquent l'absence de migration des impacts en HCT et BTEX observés au droit de MW1 vers les piézomètres en aval du site (MW2 & MW3).\r\nLa qualité des eaux souterraines en aval du site reste compatible avec les limites de l'arrêté ministériel du 11 janvier 2007 relatif aux eaux destinées à la consommation humaine et aux eaux brutes, pour les paramètres recherchés.\r\nLa Sté ENVIRON a réalisé une quinzième campagne de surveillance environnementale le 31/03/15 qui a pu mettre en évidence les points suivants :\r\nLes concentrations en HCT et BTEX mesurées au droit de MW1 lors de la présente campagne sont inférieures à celles mesurées lors de la précédente campagne (décembre 2014) et à celles mesurées lors des deux premières campagnes de 2014 (mars & juin). Elles restent toutefois supérieures aux concentrations mesurées lors de la campagne de septembre 2014.\r\nLes résultats analytiques indiquent l'absence de migration des impacts en HCT & BTEX observés au droit de MW1 vers les piézomètres en aval du site (MW2 & MW3).\r\nLa qualité des eaux souterraines en aval du site reste compatibles avec les valeurs limites de l'arrêté ministériel du 11 janvier 2007 relatif aux eaux respectivement destinées à la consommation humaine (COHV & BTEX) et aux eaux brutes (HCT).\r\nCampagne de Juin 2015 :\r\nRamboll Environ a réalisé une seizième campagne de surveillance environnementale le 4 juin 2015, afin de poursuivre l'observation de l'évolution de la qualité des eaux souterraine depuis mai 2011. Il s'agit également de la dernière campagne du suivi quadriennal de la qualité des eaux souterraines.\r\nLes concentrations en HCT & BTEX  mesurées au droit de MW1 lors de la présente campagne sont supérieures  celles mesurées lors de la précédente campagne (mars 2015). La concentration en BTEX mesurée au droit de MW1 est du même ordre de grandeur que celles mesurées lors des campagnes de mars, juin et décembre 2014. La concentration en HCT mesurée au droit de MW1 est du même ordre de grandeur que celles mesurées lors des campagnes de mars & juin 2014 et supérieure à celles mesurées lors des trois dernières campagnes (septembre 2014, décembre 2014 & mars 2015). Les résultats analytiques indiquent l'absence de migration des impacts en HCT & BTEX observés au droit de MW1 vers les piézomètres en aval du site (MW2 & MW3). La qualité des eaux souterraines en aval du site compatible avec les limites de l'arrêté ministériel du 11 janvier 2007 relatif aux eaux destinées à la consommation humaine et aux eaux brutes, pour les paramètres recherchés. Ramboll Environ propose de réaliser un bilan quadriennal afin de déterminer la nécessité ou non de poursuivre la surveillance de la qualité des eaux souterraines du site.\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000050101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Sulfates","Autres éléments minéraux","N/A","N/A","N/A","N/A","N/A"]
["SSP000050101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000050201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A","Cadmium | Cuivre | Mercure | Nickel | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Zinc","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000050201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000050301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A","Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Zinc","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000050301","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000050301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000050401","Surveillance environnementale","2008-11-01",null,"Résultat de la surveillance à la date du 2015-07-16 : LA SITUATION RESTE STABLE\nCommentaire : Des analyses sur la paramètres cuivre et PCB sont faites semestriellement depuis 2008 dans les sédiments :\r\n- au droit du stockage de DIB en niveau haut (7I) et niveau bas (7H) ;\r\n- en aval du stockage de DB en niveau haut (13D) et niveau bas (13C)\r\n\r\nL’exploitant compare les concentrations mesurées aux VDSS (valeur pouvant permettre de définir si un sol est une source de pollution), aux VCI (valeurs de constat impact usage sensible et usage non sensible).\r\n\r\nLes résultats de surveillance de juillet 2015 montrent que :\r\n- pour le cuivre, que ce soit au droit du stockage DIB ou en aval, les concentrations sont inférieures à la VDSS et aux VCI u.s et n.u.s (concentration max = 47 mg/kg MS contre une VDSS à 95 mg/kg MS).\r\n\r\n-pour les PCB au droit du stockage DIB niveau haut, les concentrations en PCB 101, 138, 153, 180 sont supérieures aux VCI u.s (concentrations respectivement à 0,180 / 0,77 / 0,93 / 0,75 mg/kg MS\r\n\r\n- pour les PCB en aval du stockage DIB niveau haut, des PCB 101, 118, 138, 153, 180 sont décelés mais les concentrations sont nettement inférieures à la VDSS (Cmax à 0,0058 mg/kg MS pour le PCB 138 pour une VDSS à 0,05).\r\n\r\n- pour les PCB au droit du stockage DIB et en aval niveau bas, les concentrations sont inférieures à la limite de quantification depuis 2008\r\n\r\nLes valeurs restent globalement assez stables depuis 2008 pour tous les paramètres sur tous les points de mesures.\nInformations complémentaires : Des analyses sur la paramètres cuivre et PCB sont faites semestriellement depuis 2008 dans les sédiments :\r\n- au droit du stockage de DIB en niveau haut (7I) et niveau bas (7H) ;\r\n- en aval du stockage de DB en niveau haut (13D) et niveau bas (13C)\r\n\r\nL’exploitant compare les concentrations mesurées aux VDSS (valeur pouvant permettre de définir si un sol est une source de pollution), aux VCI (valeurs de constat impact usage sensible et usage non sensible).\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000050401","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000050401","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000050501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Cadmium","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000050501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cadmium | Cuivre | Plomb | Zinc","Hydrocarbures et indices liés | Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000050501","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000050501","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000050601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cuivre | Plomb | Zinc","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000050601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000050701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000050801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Ammonium | Arsenic | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Metaux et métalloïdes | Paramètres azotés","N/A","N/A","N/A","N/A","N/A"]
["SSP000051001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Nickel | Plomb","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000051101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Cadmium | Chrome | Cuivre | Mercure | Plomb | Zinc","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000051101","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000051101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...) | Reconditionnement de produits dangereux, Reconditionnement de déchets","N/A","N/A","N/A"]
["SSP000051201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000051201","Surveillance environnementale","2004-01-22",null,"Résultat de la surveillance à la date du 2006-06-30 : LA SITUATION RESTE STABLE\nInformations complémentaires : Présence de HCT au droit de PZ1 à 380 µg/L.\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000051201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Chrome | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Trichloroéthylène","Benzène et dérivés | COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000051201","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000051201","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000051201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000051301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000051301","Surveillance environnementale","2004-04-21","2006-03-21","Résultat de la surveillance à la date du 2006-03-21 : LA SITUATION RESTE STABLE\nCommentaire : Compte tenu du fait que les teneurs en HCT, PCB, phénols et métaux n'ont pas dépassé les valeurs seuils en vigueur lors des 9 campagnes d'analyses, le cabinet Blondel a conclu qu'il n'était pas nécessaire de poursuivre le suivi dans un courrier à l'inspection des installations classées daté du 21/04/2006.\r\n\r\nUn courrier préfectoral a été envoyé au maire de la commune le 18 août 2006 stipulant les points suivants :\r\n\r\n- Les eaux souterraines amont et aval du site sont exemptes de toute pollution ;\r\n- Le suivi de la qualité des eaux souterraines peut être suspendu.\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000051301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic","Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000051301","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000051301","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000051301","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000051301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000051401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de gestion","N/A","Trichloroéthylène","COHV, solvants chlorés, fréons | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000051401","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2008-05-26 : LA SITUATION RESTE STABLE\nCommentaire : Pollution au TCE toujours présente sur le site. Les valeurs sont constantes aux voisinages de 95 µg/l. Aucune étude de la qualité des eaux souterraines n'a été réalisée depuis le 26/05/2008.\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000051401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A","Arsenic | Baryum | Cadmium | Chrome | Cuivre | Mercure | Nickel | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Trichloroéthylène | Zinc","Benzène et dérivés | COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000051401","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000051401","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000051501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Arsenic | Baryum | Plomb","COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes | Phytosanitaires","N/A","N/A","N/A","N/A","N/A"]
["SSP000051501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cuivre | Plomb","HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000051501","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000051501","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000051501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000051601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000051601","Surveillance environnementale","2004-05-01","2008-03-31","Résultat de la surveillance à la date du 2008-03-31 : LA SITUATION S'AMELIORE\nCommentaire : La surveillance de la qualité des eaux souterraines a été prescrite par l'arrêté préfectoral du 03/09/2003. \r\n\r\nEntre les mois d'aout 2002 et mars 2008, 13 campagnes de suivi de la qualité des eaux souterraines ont été réalisés sur le site. Ces dernières ont été effectuées sur un total de 4 puits. \r\nElles ont décelées une contamination des eaux souterraines en HCT entre février 2005 et aout 2006 avec une concentration maximale observée à 5 700 µg/l en aout 2005.\r\n\r\nAucune contamination n'a été détectée depuis aout 2006.\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000051601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Baryum","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000051601","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000051601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000051701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A","Arsenic | Cadmium | Chrome | Cuivre | Mercure | Molybdène | Nickel | Plomb | Zinc","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000051701","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000051701","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000051701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000051701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000051901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000051901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Cadmium | Chrome | Cuivre | Nickel | Zinc","COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000051901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000051901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000052001","Surveillance environnementale","2005-04-06","2005-12-20","Résultat de la surveillance à la date du 2005-12-20 : LA SITUATION RESTE STABLE\nInformations complémentaires : Les campagnes de surveillance de 2005 n'ont montré aucun impact avéré.\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000052001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A",null,"PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000052001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000052001","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000052001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique"]
["SSP000052001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000052101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A",null,"COHV, solvants chlorés, fréons | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000052101","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols","Ventilation de la zone non saturée (venting)"]
["SSP000052101","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique","Ventilation de la zone non saturée (venting)"]
["SSP000052101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000052201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000052201","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000052201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000052301","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","1",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000052301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000052301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000052401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000052401","Surveillance environnementale","2008-04-16",null,"Résultat de la surveillance à la date du : 2011-07-21\nRésultat de la surveillance eaux souterraines : 1\n","Eaux souterraines","N/A","1",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000052401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Zinc","Benzène et dérivés | Hydrocarbures et indices liés | Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000052401","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000052501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000052601","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000052601","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000052601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...) | Reconditionnement de produits dangereux, Reconditionnement de déchets","N/A","N/A","N/A"]
["SSP000052701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Arsenic | Plomb | Zinc","HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000052701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Mercure | Sulfates","Autres éléments minéraux | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000052701","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000052701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000052701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000052801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000052801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000052901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de gestion","N/A",null,"COHV, solvants chlorés, fréons | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000052901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Trichloroéthylène","Benzène et dérivés | COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000052901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000052901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000053001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de gestion","N/A","Arsenic | Molybdène","COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000053001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A","Arsenic | Baryum | Cadmium | Cuivre | Mercure | Plomb | Zinc","HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000053101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Nickel","COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000053101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Plomb","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000053101","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000053101","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000053101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000053201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cadmium | Cuivre | Mercure","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000053201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000053301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Cadmium | Chrome | Cuivre | Mercure | Molybdène | Nickel | Plomb | Zinc","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000053301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000053401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP000053401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000053401","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000053501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Trichloroéthylène","COHV, solvants chlorés, fréons | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000053501","Surveillance environnementale","2006-05-24",null,"Résultat de la surveillance à la date du 2009-05-20 : LA SITUATION RESTE STABLE\nCommentaire : La dernière campagne ayant été transmise à l'inspection des installations classées date du 20/05/2009. A cette date, 7 campagnes avaient été effectuées.\r\nSeules deux campagnes ont montré une contamination des eaux souterraines au droit du site. Le paramètre impactant était les COHV (PCE+TCE) et la concentration maximale a été observée le 20/11/2007 à 50.8 µg/l.\r\nAucune contamination n'a été détectée lors de la dernière campagne de suivi.\n","Eaux souterraines","N/A","3",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000053501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Chrome | Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Zinc","Benzène et dérivés | COHV, solvants chlorés, fréons | Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000053601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP000053601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cadmium | Chrome | Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Trichloroéthylène","Benzène et dérivés | COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000053601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000053701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique"]
["SSP000053801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Chrome | Cuivre | Nickel | Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Zinc","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000053801","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000053801","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique"]
["SSP000053801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000053901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Fer","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000053901","Surveillance environnementale","2002-03-14",null,"Résultat de la surveillance à la date du 2007-10-31 : LA SITUATION RESTE STABLE\nInformations complémentaires : Résultats de la campagne du 31/10/2007 :\r\nTétrachlorométhane : 0,8 µg/L au droit de PZ2 et 4 µg/L au droit de PZ3.\r\nFer : 1,4 mg/L au droit de PZ2 et 1,9 mg/L au droit de PZ3.\r\nPCE: traces (0,9 µg/L au droit de PZ2 et 5,9 µg/L au droit de PZ3).\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000053901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Chrome | Plomb","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000053901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000054001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000054001","Surveillance environnementale","2005-11-24",null,"Résultat de la surveillance à la date du 2006-03-14 : LA SITUATION RESTE STABLE\nInformations complémentaires : Absence d'eaux au droit de PZ1.\r\nDes traces de naphtalène ont été trouvées au droit de PZ2 et PZ3 (0,5 et 0,8 µg/L)\n","Eaux souterraines","N/A","1",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000054001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Plomb","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000054001","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000054001","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000054001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000054001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000054101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cuivre | Mercure | Plomb","Hydrocarbures et indices liés | Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000054101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000054201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000054301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000054301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000054401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Trichloroéthylène","COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP000054401","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2011-04-21 : LA SITUATION RESTE STABLE\nInformations complémentaires : Des prélèvements ont été effectués sur PZ1, PZ2, PZ3 et le drain de la station de traitement (21/04/2011).\r\n- du TCE a été trouvé au droit de PZ2 à 68,9 µg/L, de PZ3 à 4,3 µg/L et 10,8 µg/L au niveau du drain ;\r\n- du PCE a été trouvé au droit de PZ2 à 50,9 µg/L, de PZ3 à 5,6 µg/L et 24,6 µg/L au niveau du drain ;\r\n- du chlorure de vinyle a été détecté au droit de PZ1 à 2,24 µg/L, PZ2 à 37,5 µg/L, PZ3 à 779 µg/L et du drain à 16,1 µg/L ;\r\n- du cis-1,2-dichloroéthane a été détecté au droit de PZ2 à 192 µg/L, de PZ3 à 746 µg/L et 30,6 µg/L au niveau du drain ;\r\n- des traces de trans-1,2-dichloroéthane à 3,8 µg/L au droit de PZ3 ;\r\n- des traces d'arsenic ont été décelées au droit de PZ1, PZ3 et du drain ;\r\n- des traces d'HCT au droit de PZ1, PZ2 et PZ3 ;\r\n- des traces de mercure au droit de PZ2 ;\r\n- des traces de nickel ont été trouvées au droit de PZ2 et PZ3.\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000054401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cadmium | Chrome | Cuivre | Cyanures libres | Mercure | Nickel | Trichloroéthylène | Zinc","Autres éléments minéraux | COHV, solvants chlorés, fréons | Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000054401","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000054501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cadmium","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000054501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000054601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000054601","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000054601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000054701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de gestion","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000054701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A",null,"HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000054701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000054701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000054801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000054801","Surveillance environnementale","2011-10-06",null,"Résultat de la surveillance à la date du 2011-10-06 : LA SITUATION RESTE STABLE\nCommentaire : Seules des traces d'HCT sont trouvées au droit de PZ1 bis.\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000054801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000054801","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000054801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000054901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000054901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000054901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000054901","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000054901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000055001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A","Cuivre | Mercure | Nickel | Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Zinc","Benzène et dérivés | COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000055101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Chrome | Cuivre | Mercure | Plomb | Zinc","HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000055301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," .","Eaux souterraines","Diagnostic et Analyse","N/A","Aluminium | Nickel | Zinc","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000055301","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"  .","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Chrome | Cuivre | Mercure | Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000055301","Exécution des travaux de réhabilitation",null,null,"  . ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000055301","Exécution des travaux de réhabilitation",null,null,"  .",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000055401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Cadmium | Nickel","COHV, solvants chlorés, fréons | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000055401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cadmium | Cyanures libres | Zinc","Autres éléments minéraux | COHV, solvants chlorés, fréons | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000055401","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000055401","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000055501","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du : 2002-01-04\nRésultat de la surveillance eaux souterraines : 2\nles prélévements et analyses faite par Ate-Geoclean démontrent l'absence d'impact sur la nappe en benzéne,toluéne, ethyl-benzéne,Xyléne\nDate de fin envisagée de la surveillance : 2002-11-04","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000055501","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Ventilation de la zone non saturée (venting)"]
["SSP000055501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000055601","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000055601","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000055601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000055701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Trichloroéthylène","COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP000055701","Surveillance environnementale",null,"2006-06-30","Résultat de la surveillance à la date du 2006-06-30 : LA SITUATION S'AMELIORE\nInformations complémentaires : Les analyses des eaux souterraines ont été effectuées entre 28/06/2006 et le 30/06/2006, sur l'ensemble du site (ancienne station-service TOTAL et la société CHIMICOLOR). \r\nLes résultats montrent :\r\n- au niveau de PZ1 : 0,06 µg/L de naphtalène ;\r\n- au niveau de PZ2 : 300 µg/L d'HCT ;\n","Eaux souterraines","N/A","1",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000055701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cyanures libres | Plomb","Autres éléments minéraux | COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000055701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000055701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000055701","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000055701","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000055701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique"]
["SSP000055701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000055801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Fer","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000055801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Cuivre | Molybdène | Plomb","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000055801","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000055801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000055901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Baryum | Nickel | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Zinc","Benzène et dérivés | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000055901","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2012-05-23 : LA SITUATION RESTE STABLE\nCommentaire : Trace ou absence de l'ensemble des éléments recherchés sauf pour le nickel.\nInformations complémentaires : Résultats en nickel : mars 2012, 170 µg/L ; mai 2012, 160 µg/L au droit de CA-1 PZ en aval.\r\nUn suivi sur les 6 piézomètres (2 existants+4 nouveaux) a été réalisés, avec 6 analyses de novembre à octobre 2013. Ce suivi ne met en évidence aucune dégradation de la qualité de la nappe entre l'amont et l'aval hydraulique du site, avant et après excavations des terrains sur la partie sud. Un seul piézomètre montre de légers dépassements par rapport aux valeurs réglementaires « eaux potables », avec toutefois le respect des valeurs guide OMS « eau potable »le piézomètre F, en amont du site, pour les paramètres antimoine, sulfate. Les remblais au droit de ce piézomètres présentant également des contaminations  en antimoine ont pu influer sur la qualité de la nappe.\r\nAu final, la nappe au droit du site ne montre pas de source significative de pollution.\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000055901","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","1",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000055901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Cadmium | Chrome | Cuivre | Cyanures libres | Mercure | Molybdène | Nickel | Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Sulfates","Autres éléments minéraux | Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000055901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000055901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000055901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Reconditionnement de produits dangereux, Reconditionnement de déchets","N/A","N/A","N/A"]
["SSP000056001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Cuivre | Plomb","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000056001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000056101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cadmium | Cuivre | Plomb | Zinc","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000056101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000056201","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000056201","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000056201","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000056201","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000056201","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique"]
["SSP000056301","Exécution des travaux de réhabilitation",null,null,". ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)","Confinement par couverture et étanchéification"]
["SSP000056301","Exécution des travaux de réhabilitation",null,null," . ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000056301","Exécution des travaux de réhabilitation",null,null," . ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000056301","Exécution des travaux de réhabilitation",null,null,". ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique","Confinement par couverture et étanchéification"]
["SSP000056301","Exécution des travaux de réhabilitation",null,null," . ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000056401","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000056401","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000056401","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique","Biodégradation dynamisée (ou atténuation naturelle dynamisée)"]
["SSP000056401","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000056501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Cyanures libres","Autres éléments minéraux","N/A","N/A","N/A","N/A","N/A"]
["SSP000056501","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique"]
["SSP000056501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000056601","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000056601","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique"]
["SSP000056601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000056701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000056701","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000056701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000056801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000056901","Surveillance environnementale","2001-08-31",null,"Résultat de la surveillance à la date du 2013-03-31 : LA SITUATION S'AMELIORE\nInformations complémentaires : L'arrêté préfectoral du 9 décembre 2002 a imposé la surveillance trimestrielle des eaux souterraines sur les paramètres suivants : biphényle et oxyde de biphényle.\r\n\r\nLa surveillance effective du site a débuté en avril 2003. De octobre 2006 à octobre 2010 (13 campagnes) il a été constaté :\r\n- que les teneurs en polluants ont été relativement faibles (<100 µg/L, sauf une valeur de 300 µg/L en août 2007) ou la plupart inférieures au seuil de détection, en amont comme en aval ;\r\n- une réduction notable des teneurs en polluants sur les piézomètres, alors qu'il avait été mesuré jusqu'à 10 000 µg/L d'oxyde de biphényle en juillet 2006.\r\n\r\nPar courrier du 26 janvier 2011, SEMCODA a sollicité un allégement de la surveillance des eaux souterraines à une fréquence semestrielle. Par courrier du 19 avril 2011, l'inspection des installations classées a réservé une suite favorable à cette demande compte tenu que les résultats des analyses montrent notamment une stabilité au niveau de la nappe et une réduction notable des teneurs en polluant sur les piézomètres.\r\n\r\nDe janvier 2011 à mars 2013 (5 campagnes) :\r\n- diphényléther : maximum à 130 µg/L en janvier 2011 et en juin 2011 ;\r\n- biphényl : maximum à 41 µg/L en juin 2011.\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000056901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000057001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000057101","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000057101","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000057101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000057201","Surveillance environnementale","1978-01-01",null,"Résultat de la surveillance à la date du 2009-11-01 : LA SITUATION RESTE STABLE\nCommentaire : Une surveillance pièzométrique globale de la zone pétrolière est en place depuis 1978. Elle a fait l'objet d'une modification en 1999 afin de tenir compte des résultats acquis et de l'évolution prévisible du site. 2 groupes d'ouvrages sont analysés:\r\n- 5 ouvrages sont suivis à un rythme mensuel ;\r\n- 9 ouvrages sont suivi à fréquence trimestrielle.\r\n\r\nDepuis le début de la mise en place de ce suivi, 28 rapports ont été remis à l'administration. Le dernier en date a été rédigé au mois de février 2008. Sur l'ensemble des 29 dernières années, la pollution en Hydrocarbures totaux a été observée. La concentration maximale a été atteinte le 31/01/1990 sur le PZ1 (situé au nord du port), elle était alors de 64 260 mg/l. La concentration a ensuite progressivement diminué jusqu'au 09/06/2005 où elle atteignait 3,5 mg/l.\r\n\r\nDepuis cette date, 3 concentrations supérieures à 1 mg/l ont été notées sur des ouvrages différents (1,1 mg/l sur le Pz 8 le 08/12/2005, 2 mg/l et 1,7 mg/l sur le Pz 5 le 07/09/2006 et le 08/03/2007).\r\n\r\n\r\nLe site est également suivi dans le cadre de la surveillance de la qualité de la nappe alluviale de la zone industrielle au sud de Lyon. La dernière campagne renseigné de ce suivi (ayant eu lieu en novembre 2009) fait état d'une concentration en HCT inférieure à 0,03 mg/l. Aucun dépassements des valeurs seuils fixés par l'arrêté préfectoral du 17/12/2008 n'a été détecté.\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000057201","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols","Ventilation de la zone non saturée (venting)"]
["SSP000057201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000057301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Cyanures libres | Zinc","Autres éléments minéraux | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000057301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cuivre | Cyanures libres | Nickel | Zinc","Autres éléments minéraux | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000057301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000057401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000057401","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000057401","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000057401","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000057401","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique"]
["SSP000057401","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000057501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Plomb","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000057501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Chrome","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000057501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000057701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP000057701","Surveillance environnementale","2002-09-20",null,"Résultat de la surveillance à la date du 2007-03-28 : LA SITUATION RESTE STABLE\nCommentaire : L'arrêté préfectoral du 23 août 2004 impose à la société GECINA la réalisation du suivi de la qualité des eaux souterraines. Les campagnes sont réalisées à fréquence trimestrielle. La dernière campagne renseignée à l'Inspection des Installations Classées est celle du mois de mars 2007. 4 campagnes avaient été réalisées avant elle. \r\n\r\nPour chacune des campagnes effectuées, une pollution en PCE a été décelée, atteignant même 41 µg/l en mars 2007. Il s'agit cependant du seul paramètre impactant la nappe au vu des campagnes renseignées.\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000057701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Baryum | Cadmium | Chrome | Cuivre | Plomb","COHV, solvants chlorés, fréons | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000057701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000057701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000057801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000057801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000057901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés)","N/A","N/A","N/A","N/A","N/A"]
["SSP000057901","Surveillance environnementale","2004-11-01",null,"Résultat de la surveillance à la date du 2009-12-31 : LA SITUATION RESTE STABLE\nCommentaire : Au total, 5 campagnes de surveillance de la qualité des eaux souterraines ont été renseignées à l'Inspection des Installations Classées entre 2004 et 2006 puis trois autres à fréquence annuelle entre 2007 et 2009 (novembre).\r\nLors de ces campagnes, des dépassements permanent des valeurs guides dictées par l'arrêté du 17/12/2008 ont été observées en :\r\n- Tétrachloréthylène (maximum à 56 µg/l en novmebre 2004, 39 µg/l en mai 2006) ;\r\n- HCT (maximum à 80 mg/l en mai 2006).\r\n\r\nDes dépassements occasionnels ont également été notés en Benzo(a)pyrène (0,02 µg/l en septembre 2005).\r\nLa dernière mesure de 2009 faisait toujours état d'une contamination de la nappe au tétrachloroéthylène (57 µg/l).\nDate de fin envisagée de la surveillance : 2011-01-01","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000057901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Cuivre | Mercure | Plomb | Trichloroéthylène | Zinc","COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000057901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols","Confinement par couverture et étanchéification"]
["SSP000057901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000058001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Analyse des enjeux sanitaires (EQRS, ARR)","N/A",null,"PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000058001","Surveillance environnementale","2006-07-11",null,"Résultat de la surveillance à la date du 2010-09-15 : LA SITUATION SE DEGRADE\nCommentaire : Les teneurs anormales (selon les Normes de Qualité Environnementales provisoires)en PCB dans les eaux souterraines ont été constatées pour a première fois, lors de la campagnes du 15 septembre 2010.\r\n\r\nIl est tout de même à noter que l'arrêté du 11/01/07 relatif aux limites et références de qualité des eaux brutes et des eaux destinées à la consommation humaines ne présente pas encore de valeur guide pour les PCB.\nInformations complémentaires : Des PCB ont été quantifiés au droit de PZ1, pour la première fois, lors de la campagne de septembre 2010 à 0,015 µg/l (PCB-101) et 0,014 µg/l (PCB-118).\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000058001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Arsenic | Cadmium | Chrome | Cuivre | Nickel | Plomb","Hydrocarbures et indices liés | Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000058001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)","Biodégradation dynamisée (ou atténuation naturelle dynamisée)"]
["SSP000058001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols","Biodégradation dynamisée (ou atténuation naturelle dynamisée)"]
["SSP000058001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique","Biodégradation dynamisée (ou atténuation naturelle dynamisée)"]
["SSP000058001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique","Biodégradation dynamisée (ou atténuation naturelle dynamisée)"]
["SSP000058101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Chrome","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000058101","Surveillance environnementale","2007-10-10",null,"Résultat de la surveillance à la date du 2007-10-10 : LA SITUATION RESTE STABLE\nInformations complémentaires : Les résultats d'analyses des eaux souterraines montrent :\r\n- la présence de chrome dans les trois piézomètres, jusqu'à 76 µg/L au droit de PZ3 ;\r\n- la présence de potassium jusqu'à 6 ,7 mg/L au droit de PZ3.\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000058101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Baryum | Cadmium | Chrome | Cobalt | Cuivre | Nickel | Plomb | Trichloroéthylène | Zinc","COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000058101","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000058101","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000058101","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique"]
["SSP000058101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000058201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Trichloroéthylène","COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP000058201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Baryum | Chrome | Cuivre | Plomb","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000058201","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)","Confinement par couverture et étanchéification"]
["SSP000058201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000058301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Trichloroéthylène","Benzène et dérivés | COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés)","N/A","N/A","N/A","N/A","N/A"]
["SSP000058301","Surveillance environnementale","2005-09-29","2007-08-08","Résultat de la surveillance à la date du 2007-08-08 : LA SITUATION RESTE STABLE\nInformations complémentaires : Au 08/08/2007 :\r\nPZ1 : 2,4 µg/L de tétrachloréthène, 1,4 µg/L de trichloroéthène, 110 µg/L de plomb.\r\nPZ3 : 1,7 µg/L de cis-dichloroéthène.\n","Eaux souterraines","N/A","1",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000058301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Chrome | Cuivre | Mercure | Plomb | Zinc","HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000058301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000058401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Chrome","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000058401","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000058401","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000058401","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000058501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Ammonium | Arsenic","Metaux et métalloïdes | Paramètres azotés","N/A","N/A","N/A","N/A","N/A"]
["SSP000058501","Surveillance environnementale","2004-04-13",null,"Résultat de la surveillance à la date du 2006-03-31 : LA SITUATION S'AMELIORE\nInformations complémentaires : Aucun impact en HCT, nitrates, nitrites, ammonium et en arsenic n'a été mis en évidence.\nDate de fin envisagée de la surveillance : 2006-07-24","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000058501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000058601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000058601","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification | Ventilation de la zone non saturée (venting)","Filtration"]
["SSP000058601","Surveillance environnementale","2004-12-01",null,"Résultat de la surveillance à la date du 2013-02-07 : LA SITUATION S'AMELIORE\nCommentaire : Les résultats présentés par la société SERPOL montrent une diminution globale de la teneur en BTEX (principalement Benzène) et en hydrocarbures dans les eaux souterraines.\r\n\r\nLes teneurs observées restent cependant au dessus des valeurs seuils requises dans les eaux souterraines.\r\n\r\nLe dernier rapport de suivi de la nappe phréatique et de suivi du traitement a été remis à l'Inspection des Installations Classées le 2 mai 2013. \r\n\r\nLa campagne de suivi de la qualité de la nappe fait toujours état d'une pollution aux: \r\n- HCT (1 570 µg/l) ;\r\n- Benzène (748 µg/l). \nInformations complémentaires : Actuellement, des échantillons d'eaux sont prélevés dans 11 ouvrages en dehors et sur le site.\r\n\r\nNeuf piézomètres implantés à l'aval hydraulique sont étudiés ainsi que deux ouvrages situés à l'amont. \r\n\r\nLes piézomètres sont tous implantés dans la nappe du talus (dont le niveau statique varie entre 2.4 et 3.9 mètres de profondeur) à l'exception du Pz15 et du puits agricole implantés dans la nappe d'accompagnement du Gier à l'aval du site (le puits agricole est situé en dehors du site).\r\n\r\nL'écoulement des deux nappes se fait en direction du nord-est.\r\n\r\n\r\n\r\nLes résultats du suivi des eaux souterraines sont les suivants :\r\n\r\n1.  Impact en Benzène :\r\n\r\n\r\n- Pz6 : 8 fois entre décembre 2008 et juin 2011, un maximum de 150 µg/l en mai 2010 ;\r\n\r\n- Pz7 : 23 fois sur 61 campagnes avec un maximum a 40 µg/l en décembre 2004 ;\r\n\r\n- Pz2 : 32 fois sur 61 campagnes avec un maximum a 260 µg/l en octobre 2007 ;\r\n\r\n- Pz5 : 22 fois sur 37 campagnes, max= 58 µg/l en mai 2008 ;\r\n\r\n- Pz20 : 7 fois sur 10, max=480 µg/l en septembre 2011 ;\r\n\r\n- Pz16 : valeurs dépassées pour chaque campagne avec un maximum observé à 4100 µg/l en mai 2010. \r\n\r\n\r\n2. Impact en Hydrocarbures Totaux (HT) et Aliphatiques (HA) :\r\n\r\n- Pz6 : \r\n      HT = 3 fois avec un maximum de 1700 µg/l en juillet 2006 ;\r\n\r\n- Pz7 :\r\n      HT = 3 fois, max à 4700 µg/l en décembre 2007) ;\r\n      HA = 1 fois en décembre 2007, 530 µg/l ;\r\n\r\n- Pz2 : \r\n      HT = 4 fois entre août 2005 et avril 2006, (max à 2200 µg/l en janvier 2006) ;\r\n      HA = 3 fois de février (max 2700 µg/l) à avril 2006 ;\r\n\r\n- Pz5 : \r\n      HT = 24 fois sur 37 campagnes, (max à 160 000 µg/l en septembre 2008) ;\r\n      HA = 4 fois de février 2007 à janvier 2008 (max = 4100 µg/l en août 2007) ;\r\n\r\n- Pz20 : \r\n      HA = en mai 2010, 12 000 µg/l ;\r\n\r\n- Pz16 : \r\n      HT = 5 fois sur 10 campagnes, (max à 2300 µg/l en mai 2010) ;\r\n      HA = 5 fois sur 10 campagnes, (max à 140 000 µg/l en septembre 2010) ;\r\n\r\n\r\nLes eaux du puits agricole, ainsi que les eaux des ouvrages situés en amont du site, n'ont à ce jour pas présentées de teneurs en BTEX, hydrocarbures totaux et hydrocarbures aliphatique supérieures aux seuils requis pour les eaux souterraines.\r\n\r\nLes eaux du Pz15, piézomètre situé le plus à l'aval sur le site, ont atteint une fois la valeur de 1 mg/l en hydrocarbure totaux au mois de décembre 2010.\r\n\r\nCompte tenu de son implantation récente, le Pz22 n'a fait l'objet que d'un seule campagne et présente des valeurs supérieures aux seuils requis en Benzène, HT et HA.\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000058601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000058601","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)","Ventilation de la zone non saturée (venting)"]
["SSP000058601","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique","Ventilation de la zone non saturée (venting)"]
["SSP000058601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage | Pompage de rabattement ou de récupération","N/A","N/A","N/A"]
["SSP000058701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Trichloroéthylène","COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000058701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000058701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique"]
["SSP000058701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000058801","Surveillance environnementale","2009-03-01",null,"Résultat de la surveillance à la date du 2010-05-31 : LA SITUATION S'AMELIORE\nCommentaire : Le suivi de la qualité de la nappe d'au souterraine a été initié sur le site au mois de mars 2009, après réalisation des travaux. 6 campagnes ont été renseignées à l'inspection des installations classées (la dernière ayant eu lieu au mois de mai 2010). \r\n\r\nUn impact a été observée sur le site en Arsenic (maximum à 670 µg/l au mois d'aout 2009), en Plomb (100µg/l au mois de mars 2009) et en Nickel (33 µg/l en décembre 2009). Aucune contamination n'a été remarqué après la campagne de décembre 2009. \n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000058801","Exécution des travaux de réhabilitation",null,null,". ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000058801","Exécution des travaux de réhabilitation",null,null,". ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000058801","Exécution des travaux de réhabilitation",null,null," .",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000058901","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"      ","Eaux souterraines","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000058901","Exécution des travaux de réhabilitation",null,null,"    ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique","Oxydation chimique"]
["SSP000058901","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"    ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000058901","Exécution des travaux de réhabilitation",null,null,"   ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000058901","Exécution des travaux de réhabilitation",null,null,"   ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...) | Reconditionnement de produits dangereux, Reconditionnement de déchets","N/A","N/A","N/A"]
["SSP000059001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de gestion","N/A","Chrome","COHV, solvants chlorés, fréons | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000059001","Surveillance environnementale","2011-11-15","2017-11-30","Résultat de la surveillance à la date du 2018-05-24 : LA SITUATION RESTE STABLE\nInformations complémentaires : Dernières campagnes de surveillance réalisées par l'ADEME en 2017.\r\nPas d'impact significatif hors site.\nDate de fin envisagée de la surveillance : 2017-11-30","Eaux souterraines","N/A","1",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000059001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A","Arsenic | Chrome | Cuivre | Nickel","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000059001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000059001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Solidification/stabilisation"]
["SSP000059001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000059101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Analyse des enjeux sanitaires (EQRS, ARR)","N/A",null,"COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP000059101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Arsenic | Cadmium | Chrome | Cuivre | Cyanures libres | Plomb","Autres éléments minéraux | COHV, solvants chlorés, fréons | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000059101","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000059101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...) | Pompage de rabattement ou de récupération | Reconditionnement de produits dangereux, Reconditionnement de déchets","N/A","N/A","N/A"]
["SSP000059201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Trichloroéthylène","Benzène et dérivés | COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000059201","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique"]
["SSP000059201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000059301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Interprétation de l''état des milieux (IEM)","N/A","Cadmium | Chrome | Plomb | Trichloroéthylène","COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000059301","Surveillance environnementale","2008-12-12",null,"Résultat de la surveillance à la date du 2010-09-22 : LA SITUATION S'AMELIORE\nInformations complémentaires : Comparatif par rapport aux résultats obtenus lors des diagnostics (en 2002 et 2009):\r\nL'analyse des eaux souterraines sur les trois puits accessibles, le puits n°1 étant situé en amont hydraulique des infrastructures et les puits 2 et 3 en aval, a permis d'observer des concentrations supérieures aux valeurs de potabilité :\r\n- en HCT au niveau des trois ouvrages (puits 1 : 280 &#956;g/l, puits 2 : 2800 &#956;g/l et puits 3 : 4100 &#956;g/l)\r\n- en TCE et PCE au niveau du puits 1 (8,8 et 41 &#956;g/l)\r\n- en antimoine et plomb au niveau des puits 2 et 3 (Pb :60 et 70 &#956;g/l, Sb : 70 &#956;g/l au niveau du puits 3) \r\n\r\nLors de la seconde campagne de mesures de 2009, seuls les puits P2 et P3 ont pu faire l'objet d'un suivi, et les résultats indiquent que :\r\n- le puits P2 est impacté par le PCE (31,5  &#956;g/l)\r\n- le puits P3 est impacté par le cadmium, le chrome et le plomb (respectivement 6 &#956;g/l, 80 &#956;g/l, et 5320 &#956;g/l) et par des HCT (0,14 mg/l)\r\nLes analyses qui ont suivi les travaux ont été effectuées le 22 septembre 2010 sur le nouveau piézomètre implanté au droit du site, il en résulte :\r\n- l'absence ou faibles traces de BTEX;\r\n- une concentration en HAP 10 fois supérieures au seuil de qualité des eaux destinées à la consommation; humaine;\r\n- l'absence ou faibles traces de COHV;\r\n- une concentration en HCT de 1000 µg/l (valeur seuil : 1000 µg/l).\r\n\r\nUne surveillance de la qualité des eaux souterraines a été effectuée enter 2011 et 2015 par la société ENVISOL, pour le compte de BNP PARIBAS IMMOBILIER. Cette surveillance met principalement en évidence les éléments suivants :\r\n- des concentrations en trichloroéthylène et cis-1.2-dichloroéthène supérieures aux seuil définis dans l'ARR;\r\n- des concentrations en somme TCE+PCE supérieures à la limite de qualité des eaux destinées à la consommation humaine;\r\n- l'impact en COHV vient de l'amont et n'est pas attribuable au site;\r\n- les concentrations mesurées en hydrocarbures sont supérieures au seuil fixé dans l'ARR au droit d'un piézomètre (PZ4). On note cependant une diminution de ces valeurs lors des deux derniers suivis.\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000059301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Interprétation de l''état des milieux (IEM)","N/A","Arsenic | Cadmium | Cuivre | Nickel | Plomb | Trichloroéthylène | Zinc","COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000059301","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000059301","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000059301","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000059301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...) | Pompage de rabattement ou de récupération","N/A","N/A","N/A"]
["SSP000059401","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000059401","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000059401","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000059501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000059501","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000059501","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000059501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000059601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000059601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cadmium | Cuivre | Plomb | Zinc","Hydrocarbures et indices liés | Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000059601","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000059601","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000059601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000059701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Analyse des enjeux sanitaires (EQRS, ARR)","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000059701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Arsenic | Cadmium | Cuivre | Plomb | Zinc","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000059701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000059701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000059801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000059801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Reconditionnement de produits dangereux, Reconditionnement de déchets","N/A","N/A","N/A"]
["SSP000059901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Trichloroéthylène","COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP000059901","Surveillance environnementale","2006-01-01","2010-04-16","Résultat de la surveillance à la date du 2010-04-16 : LA SITUATION RESTE STABLE\nCommentaire : Ont été recherchés 17 COHV au droit des PZ2 et PZ3.\r\nOnt été détectés (à des teneurs inférieures aux valeurs limites de l'annexe II de la circulaire du 23 octobre 2012 ou dans le cas où il n'existe pas de valeur-limite) :\r\n* du cis 1,2-dichloroéthylène au droit de PZ2 (0,43 µg/L inférieure à 50 µg/L) ;\r\n* du 1,1,1-Trichloroéthane (il n'existe pas de valeur limite pour ce composé) au droit de PZ2 (2,5 µg/L) et de PZ3 (0,32 µg/L) ;\r\n* du trichloroéthylène en 2010 au droit de PZ2 (1,6 µg/L), au droit de PZ3 (0,49 µg/L).\r\n\r\nOnt été détectés à des concentrations supérieures aux valeurs limites de l'annexe II de la circulaire du 23 octobre 2012 :\r\n* du tétrachloroéthylène (valeur limite PCE = 10 µg/L) au droit de PZ2 (16 µg/L) et de PZ3 (15 µg/L) ;\r\n* la valeur limite pour la somme PCE + TCE est dépassée en conséquence.\nInformations complémentaires : Entre 2006 et 2010 (3 campagnes), sont détectés systématiquement du TCE (de l'ordre du µg/L), du PCE (de l'ordre de 20 µg/L). Les critères de qualité du PCE et de la somme de TCE+PCE (10 µg/L) sont dépassés dans le puits en 2006 et 2007, au droit de PZ2 en mars 2007 et avril 2010 et au droit de PZ3 en avril 2010.\n","Eaux souterraines","N/A","1",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000059901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Trichloroéthylène","COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000060001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Cadmium | Cuivre | Mercure | Plomb | Zinc","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000060001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000060101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Cuivre | Nickel","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000060101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000060201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Cuivre","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000060301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000060401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Arsenic | Plomb","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000060401","Surveillance environnementale","2008-04-15",null,"Résultat de la surveillance à la date du 2012-07-18 : LA SITUATION SE DEGRADE\nCommentaire : Les eaux souterraines au droit du site, ne présentent pas d'impact vis-àvis des HCT et arsenic.\r\nCependant, une pollution en plomb (11 µg/L) a été décelée au niveau de PZ3, selon les valeurs seuils en rigueur de l'époque.\n","Eaux souterraines","N/A","3",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000060401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000060401","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000060401","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique"]
["SSP000060501","Surveillance environnementale","2011-11-16",null,"Résultat de la surveillance à la date du 2013-05-31 : LA SITUATION RESTE STABLE\nInformations complémentaires : L'arrêté préfectoral du 29/07/2011 impose la surveillance semestrielle de la nappe en amont et aval via 3 piézomètres sur les paramètres suivants : pH, température, DCO, HCT, BTEX, HAP (16), PCE, TCE, trichloréthane, zinc.\r\n\r\n\r\nLa surveillance des eaux souterraines de novembre 2011 à mai 2013 (4 campagnes) via 3 piézomètres ne met pas en évidence de contaminations dépassant les seuils fixés par la circulaire du 23 octobre 2012 relative à l'application de l'arrêté du 17 décembre 2008 établissant les critères d’évaluation et les modalités de détermination de l’état des eaux souterraines et des tendances significatives et durables de dégradation de l’état chimique des eaux souterraines.\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000060501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A",null,"HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000060501","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000060501","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000060501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000060701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP000060701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Chrome | Cuivre | Molybdène | Nickel","COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000060801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Trichloroéthylène","COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP000060801","Surveillance environnementale","2006-02-07","2015-07-10","Résultat de la surveillance à la date du 2015-07-01 : LA SITUATION S'AMELIORE\nCommentaire : En 2015, suite à des mesures par le propriétaire, il a été constaté à l'état de trace (2,4ug/l) du tétrachloroéthylène en aval hydraulique du site.\nInformations complémentaires : Du fait que l'exploitant est radié, plus aucune surveillance n'est réalisée.\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000060801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Chrome | Trichloroéthylène","COHV, solvants chlorés, fréons | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000060801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000060901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Arsenic | Nickel | Plomb | Trichloroéthylène","COHV, solvants chlorés, fréons | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000060901","Surveillance environnementale","2005-05-02",null,"Résultat de la surveillance à la date du 2012-07-10 : LA SITUATION RESTE STABLE\nCommentaire : Au niveau de la nappe superficielle (PZ2, PZ101 et PZ3), la concentration mesurée en PCE (14,9 µg/L) est supérieure à la valeur seuil en vigueur à l'époque.\r\n\r\nAu niveau de la nappe profonde (PZ5, PZ1002 et PZ103), la concentration mesurée en PCE (14,9 µg/L) est supérieure à la valeur seuil en vigueur à l'époque.\nInformations complémentaires : Depuis mai 2005, on constate une diminution des concentration en TCE, PCE et 1,2-dichloroéthylène.\r\n\r\nDes teneurs en benzène ont été détectées pour la première fois en juillet 2012 (1,82 et 9,58 µg/L) dans les deux nappes.\n","Eaux souterraines","N/A","3",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000060901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000060901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000061001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000061001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000061101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000061101","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols","Ventilation de la zone non saturée (venting)"]
["SSP000061101","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique","Ventilation de la zone non saturée (venting)"]
["SSP000061101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000061201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP000061201","Surveillance environnementale","2012-10-17",null,"Résultat de la surveillance à la date du 2012-10-17 : LA SITUATION RESTE STABLE\nInformations complémentaires : Présence de TCE et PCE, à des concentrations de 17.2 µg/L au droit de PZ1bis, 17.2 µg/L au droit de PZ2bis et 18.1 µg/L au droit de PZ3.\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000061201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Cadmium | Cuivre | Mercure | Nickel | Plomb | Zinc","Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000061201","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000061201","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000061201","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique"]
["SSP000061301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"COHV, solvants chlorés, fréons | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000061301","Surveillance environnementale","2002-01-18",null,"Résultat de la surveillance à la date du 2004-12-16 : LA SITUATION S'AMELIORE\nInformations complémentaires : Le rapport  du suivi de la qualité des eaux souterraines (campagne de décembre 2004) montre :\r\n- que les concentrations en HCT sont maintenant inférieures à 50 µg/L ;\r\n- que les concentrations en PCE sont baisses avec 18 µg/L au droit de PZ1, 20 µg/L au droit de PZ2 et 46 µg/L au droit de PZ3.\r\n\r\n\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000061301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Trichloroéthylène","COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP000061301","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000061301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000061401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Arsenic | Nickel | Plomb","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000061401","Surveillance environnementale","2007-11-07",null,"Résultat de la surveillance à la date du 2016-11-10 : LA SITUATION S'AMELIORE\nCommentaire : Plus d'impact significatif en nappe depuis juillet 2013.\r\nLes polluants ne sont plus détectables ou à l'état de traces.\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000061401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Cadmium | Chrome | Cuivre | Mercure | Plomb | Zinc","COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000061401","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000061401","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols","Confinement par couverture et étanchéification"]
["SSP000061401","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Reconditionnement de produits dangereux, Reconditionnement de déchets","N/A","N/A","N/A"]
["SSP000061501","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000061601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Arsenic | Trichloroéthylène","COHV, solvants chlorés, fréons | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000061601","Surveillance environnementale","2007-01-09",null,"Résultat de la surveillance à la date du 2008-11-26 : LA SITUATION RESTE STABLE\nCommentaire : Un suivi de la qualité des eaux souterraines a début sur le site au mois de janvier 2007. Ce suivi a fait l'objet d'un arrêté préfectoral signé en date du 28/02/2007 et imposant des campagnes bimestrielles sur 3 ouvrages jusqu'à la fin des travaux de construction du Centre Pénitentiaire.\r\n\r\n12 campagnes ont été réalisées dont la dernière a eu lieu au mois de novembre 2008. les analyses ont montrés des contaminations ponctuels en :\r\n- PCE (sur 4 campagnes avec un maximum de 51 µg/l le 30/07/2007) ;\r\n- Arsenic (une fois à 31 µg/l le 26/11/2008) ;\r\n- TCE (une fois à 1,3 µg/l le 29/09/2008). \n","Eaux souterraines","N/A","6",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000061601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Cuivre | Trichloroéthylène","COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000061601","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000061601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000061701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Arsenic","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000061701","Surveillance environnementale","2007-11-19",null,"Résultat de la surveillance à la date du 2010-03-16 : LA SITUATION RESTE STABLE\nInformations complémentaires : La surveillance de la nappe est régulièrement réalisée depuis fin 2007 à l'aide de 3 piézomètres (PZ1 : en amont et PZ2 et PZ3 : en aval). La nappe est entre -5 et -8 m, avec une remontée dans les ouvrages à environ – 3 m du niveau du sol car la nappe est captive.\r\n\r\nLes composés relevés dans la nappe sont :\r\n- à l'aval, des hydrocarbures (3,8 à 400 mg/L) avec une phase de flottant au PZ2 de type huile ;\r\n- à l'amont comme à l'aval, de l'arsenic (75 µg/L) ;\r\n- à l'amont, du trichloréthylène (0,5 à 1,8 µg/L observée avant août 2008) ;\r\n- à l'aval mais aussi à l'amont, du 1,2-dichloroéthylène (0,5 à 9,6 µg/L) ;\r\n- à l'aval, du chlorure de vinyle (0,7 à 2,4 µg/L depuis 2008).\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000061701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Arsenic | Mercure | Plomb | Trichloroéthylène","COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000061801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cadmium | Cuivre | Plomb | Zinc","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000061801","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000061801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000061901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés","N/A","N/A","N/A","N/A","N/A"]
["SSP000061901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000061901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000062001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Plomb","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000062001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000062101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cuivre | Zinc","HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000062101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000062201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de gestion","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000062201","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Piège hydraulique ou Confinement hydraulique","Filtration"]
["SSP000062201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000062201","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000062201","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique"]
["SSP000062201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000062301","Surveillance environnementale","2005-06-01",null,"Résultat de la surveillance à la date du 2011-06-10 : LA SITUATION S'AMELIORE\nInformations complémentaires : Prélèvement au 10/06/2011 : \r\n- 0,25 µg/L de TCE au droit de PZ4 ; \r\n- PCE à 1,1 µg/L au droit de PZ4 et 0,6 µg/L au droit de PZ5.\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000062301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Chrome | Cuivre | Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000062301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000062401","Surveillance environnementale","2005-10-27","2006-11-20","Résultat de la surveillance à la date du 2006-11-20 : LA SITUATION S'AMELIORE\nInformations complémentaires : Prélèvements effectués sur 4 piézomètres : PZ3 (au nord du site \"marchandises sud\"), PZ7 (au nord du site), PZ14 (au sud-est du site), PZ16 (au nord du site).\r\nAu 20/11/2006, il n'est pas possible de définir une direction globale d'écoulement de la nappe, les gradients étant très faibles.\r\n\r\nPZ3 : 10 µg/L de cyanures totaux\r\nPZ7 : 10 µg/L de cuivre\r\nPZ16 : 12 µg/L de cyanures totaux\r\n\r\nLe suivi de la qualité des eaux souterraines a été effectué avant et après travaux.\r\n\r\nLes résultats montrent :\r\nAvant travaux (juin 2005) :\r\n0,05 mg/L de cyanures totaux, 0,17 µg/L de 16 HAP et 2,7 µg/L de COHV au droit de l'ouvrage en amont du site  PZ5bis.\r\n82,13 µg/L de 16 HAP et 0,6 µg/L de COHV au droit de l'ouvrage en aval du site PZ5.\r\n\r\nAprès travaux (avril 2006) :\r\n0,07 mg/L de cyanures totaux, 0,97 µg/L de 16 HAP et 2,4 µg/L de COHV au droit de l'ouvrage en amont du site  PZ5bis.\r\n251,3 µg/L de 16 HAP, 0,6 µg/L de CAV et 0,8 µg/L de COHV au droit de l'ouvrage en aval du site PZ5.\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000062401","Exécution des travaux de réhabilitation",null,null,".","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000062401","Exécution des travaux de réhabilitation",null,null,".","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique"]
["SSP000062401","Exécution des travaux de réhabilitation",null,null," .",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000062501","Exécution des travaux de réhabilitation",null,null,". ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000062501","Exécution des travaux de réhabilitation",null,null,". ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique"]
["SSP000062601","Exécution des travaux de réhabilitation",null,null,".","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000062601","Exécution des travaux de réhabilitation",null,null,".","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique"]
["SSP000062701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000062801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Analyse des enjeux sanitaires (EQRS, ARR)","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000062801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Arsenic | Mercure | Plomb | Trichloroéthylène | Zinc","COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000062801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000062901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A","Arsenic | Baryum | Cadmium | Chrome | Cuivre | Mercure | Molybdène | Nickel | Plomb | Sélénium | Zinc","COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000063001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000063001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000063101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000063101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000063201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000063201","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000063201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000063301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000063301","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000063301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000063301","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000063301","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000063301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000063401","Surveillance environnementale","1992-07-31",null,"Résultat de la surveillance à la date du 2012-11-30 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000063401","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000063401","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000063401","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000063501","Surveillance environnementale","2003-04-15",null,"Résultat de la surveillance à la date du : 2011-09-24\nRésultat de la surveillance eaux souterraines : 1\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000063501","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000063601","Surveillance environnementale",null,null,"","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000063601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cadmium | Chrome | Cuivre | Nickel | Plomb | Trichloroéthylène | Zinc","COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000063601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000063701","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2003-07-03 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000063701","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","3",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000063801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Fer","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000063801","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2012-06-30 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000063801","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000063801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Baryum | Chrome | Cuivre | Nickel","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000063801","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000063801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000063901","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000063901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000064001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Plomb","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000064001","Surveillance environnementale","2003-01-29",null,"Résultat de la surveillance à la date du 2006-03-22 : LA SITUATION S'AMELIORE\nInformations complémentaires : L'AP du 17/10/2002 impose une surveillance semestrielle de la qualité des eaux souterraines et des eaux de surface (l'Arc) sur les éléments suivant : HCT, HAP, BTEX, plomb, chrome et manganèse.\r\n\r\nLa surveillance des eaux souterraines effectuée par un piézomètre (dernière analyse le 22 mars 2006) montre :\r\n- des contaminations en manganèse (valeur seuil de 50 µg/L) : 160 µg/L en janvier 2003, 430 µg/L en septembre 2003, 350 µg/L en décembre 2003 et 66 µg/L en mars 2006 ;\r\n- que le plomb, le chrome, les HCT et les BTEX ne dépassent pas leurs valeurs seuils.\r\n\r\nLa 8ème campagne de prélèvement du 22 mars 2006  pour la surveillance des eaux souterraines a été effectuée quelques semaines après la fin des travaux de déconstruction du site.\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000064001","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000064001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Baryum | Chrome | Cuivre | Nickel | Plomb | Zinc","HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000064001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000064101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Ammonium | Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes | Paramètres azotés","N/A","N/A","N/A","N/A","N/A"]
["SSP000064101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000064101","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000064101","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique"]
["SSP000064101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000064201","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2012-12-31 : LA SITUATION RESTE STABLE\nInformations complémentaires : Les résultats de la surveillance des eaux souterraines pour le suivi 2013 - 2014 montrent une quasi stabilité de la qualité des eaux (absence d'anomalies pour les HCT, les HAP et le toluène sur l'ensemble des ouvrages; présence de PCB sur le piézomètre au droit de la pollution à des concentrations comprises entre 0,022 et 0,030 µg/l, absence de PCB pour les 2 autres piézomètres, à l'aval). La teneur en PCB sur le piézomètre au droit de la zone polluée semble orientée à la baisse avec une une stabilisation de la teneur entre 0,002 et 0,034 µg/l sur les 6 dernières campagne.\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000064201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000064201","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000064301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000064301","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000064301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Baryum | Chrome | Nickel","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000064301","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000064301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000064401","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000064501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Aluminium","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000064501","Surveillance environnementale","2006-06-19",null,"Résultat de la surveillance à la date du 2006-12-07 : LA SITUATION S'AMELIORE\nInformations complémentaires : L'arrêté préfectoral du 15 novembre 2004 impose à l'exploitant la surveillance trimestrielle des eaux souterraines via un point de contrôle au droit du captage de la source de Fontaine Froide sur les paramètres suivants : pH, conductivité, aluminium, manganèse et zinc.\r\n\r\nPar courrier du 12 février 2007, l'exploitant transmet à l'inspection de l'environnement les résultats de 2 campagnes d'analyses des eaux souterraines effectuées en 2006 : aucune contamination mise en évidence.\r\n\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000064501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000064601","Surveillance environnementale","2005-08-26",null,"Résultat de la surveillance à la date du 2012-02-14 : LA SITUATION RESTE STABLE\nInformations complémentaires : Depuis fin 2009, les teneurs en hydrocarbures totaux, BTEX et métaux sont inférieures aux limites de quantification analytique du laboratoire, à l'exception d'une anomalie en chrome et zinc détectés en juin 2010 (piézomètres amont et aval) non retrouvée ensuite.\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000064701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de gestion","N/A","Arsenic | Chrome | Mercure | Nickel | Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000064701","Surveillance environnementale","2009-11-01",null,"Résultat de la surveillance à la date du 2012-07-30 : LA SITUATION RESTE STABLE\nInformations complémentaires : Le 29 août 2008, un arrêté préfectoral prescrit une surveillance semestrielle de la qualité des eaux souterraines.\r\n\r\nLes analyses des eaux souterraines montrent, sur la base de la circulaire du 23 octobre 2012, des contaminations :\r\n- en novembre 2009 en HCT (5 120 mg/L pour une valeur seuil fixée à 1 mg/L),  benzène (5,60 µg/L pour une valeur seuil fixée à 1 µg/L), xylènes (2 496 µg/L pour une valeur seuil fixée à 500 µg/L), arsenic (65 µg/L pour une valeur seuil fixée à 10 µg/L), nickel (121 µg/L pour une valeur seuil fixée à 20 µg/L), plomb (97 µg/L pour une valeur seuil fixée à 10 µg/L) ;\r\n- le 22 juillet 2011 en HCT (453 mg/L), benzène (6,47 µg/L), arsenic (22  µg/L), chrome (114 µg/L pour une valeur seuil fixée à 50 µg/L), nickel (69 µg/L), plomb (436 µg/L), HAP somme 6 (4,1 µg/L pour une valeur seuil fixée à 1 µg/L) ;\r\n- le 11 janvier 2012 en HCT (145 mg/L), benzène (4,15 µg/L), arsenic (12 µg/L), nickel (23 µg/L), plomb (97 µg/L), HAP somme 6 (1,85 µg/L) ;\r\n- le 30 juillet 2012 en HCT (135 mg/L), benzène (2,14  µg/L), arsenic (57 µg/L), nickel (28 µg/L), plomb (117 µg/L), mercure (6,99 µg/L pour une valeur seuil fixée à 1 µg/L), HAP somme 6 (4,9 µg/L).\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000064701","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000064701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000064701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Pompage de rabattement ou de récupération","N/A","N/A","N/A"]
["SSP000064801","Surveillance environnementale",null,null,"","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000064901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cuivre | Plomb | Zinc","COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000065001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000065001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000065001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000065101","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000065101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000065201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Baryum | Chrome | Cuivre | Nickel | Plomb | Zinc","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000065201","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000065201","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000065201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000065301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cadmium | Cuivre | Plomb | Zinc","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000065401","Surveillance environnementale","1999-10-07","2000-06-13","Résultat de la surveillance à la date du 2000-06-13 : LA SITUATION RESTE STABLE\nInformations complémentaires : Suite à la visite du 8 septembre 1999, l'inspection de l'environnement demande par courrier du  9 septembre 1999 à l'exploitant d'effectuer une première campagne de deux mesures sur deux piézomètres sur les paramètres suivants : conductivité, pH, DCO, DBO5, indice phénol, cyanures, HCT, zinc, plomb, nickel, chrome total, mercure, aluminium, cadmium.\r\n\r\nPar courrier du 16 novembre 1999, l'exploitant transmet à l'inspection de l'environnement les résultats des premières analyses des eaux souterraines qui ne mettent pas en évidence de pollution particulière.\r\n\r\nSuite aux résultats satisfaisants de la première campagne d'analyse des eaux souterraines, l'inspection de l'environnement demande à l'exploitant par courrier du 11 janvier 2000 de réaliser une deuxième campagne simplifiée effectuée mensuellement pendant 6 mois sur les paramètres suivants : conductivité, pH, DCO et indice phénol.\r\n\r\nCette deuxième campagne, réalisée de décembre 1999 à juin 2000 ne met pas en évidence de pollution particulière.\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000065401","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000065401","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000065401","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...) | Reconditionnement de produits dangereux, Reconditionnement de déchets","N/A","N/A","N/A"]
["SSP000065501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Arsenic | Chrome | Fer | Molybdène | Plomb","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000065501","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000065501","Surveillance environnementale","1994-02-16",null,"Résultat de la surveillance à la date du 2012-06-01 : LA SITUATION RESTE STABLE\nInformations complémentaires : L'AP du 28/10/1993, rappelé dans l'AP du 09/10/1996, impose la surveillance semestrielle des eaux souterraines sur un nombre minimum de 10 piézomètres, pour les paramètres suivants : pH, DCO, arsenic, cadmium, chlorures, chrome VI, chrome total, cobalt, cuivre, cyanures, étain, fer, manganèse, mercure, molybdène, nickel, PCB, plomb, rhénium, titane, tungstène, vanadium et zinc.\r\n\r\nLe 13 février 2002, suite aux analyses pratiquées sur l'eau souterraine depuis plus de 5 ans, PEM demande une modification des dispositions prescrites par les AP suscités. \r\n\r\nSur avis de l'inspection le 08/07/2003 et l'avis du Conseil Départemental d'Hygiène le 30/07/2003, l'AP du 28/08/2003 allège la surveillance : \r\n- analyses semestrielles des eaux souterraines sur les paramètres pH, conductivité, arsenic, chrome hexavalent, chrome total, cobalt, cuivre, rhénium, titane, tungstène, fer total, manganèse, molybdène, plomb, vanadium, zinc, DCO et chlorures ;\r\n- une fois tous les 5 ans, analyses des eaux souterraines sur les paramètres pH, DCO, arsenic, cadmium, chlorures, chrome 6, chrome total, cobalt, cuivre, cyanures, étain, fer, manganèse, mercure, molybdène, nickel, PCB, plomb, rhénium, titane, tungstène, vanadium, zinc ;\r\n- le nombre de piézomètres sera au minimum de 8.\r\n\r\nLes derniers résultats des analyses des eaux souterraines mettent en évidence (de juin 2006 à juin 2012) :\r\n- une contamination régulière depuis novembre 2006 en arsenic : maximum à 230 µg/L en novembre 2007 (valeur seuil de 10 µg/L), 60 µg/L en juin 2012 ;\r\n- une contamination régulière depuis juin 2006 en chrome total : maximum à 220 µg/L en novembre 2007 et 2008 (valeur seuil de 50 µg/L), 160 µg/L en juin 2012 ;\r\n- une contamination régulière depuis novembre 2006 en chrome hexavalent : maximum à 220 µg/L en novembre 2008 (valeur seuil de 50 µg/L), 160 µg/L en juin 2012 ;\r\n- une contamination en fer depuis juin 2006 jusqu'en novembre 2008 avec un maximum à 590 µg/L en novembre 2007 (valeur seuil de 200 µg/L), 20 µg/L en juin 2012 ;\r\n- une contamination régulière depuis juin 2006 en manganèse : maximum à 510 µg/L en novembre 2007 (valeur seuil de 50 µg/L), 70 µg/L en juin 2012 ;\r\n- une forte contamination régulière depuis juin 2006 en molybdène : maximum à 19 000 µg/L en mai 2010 (valeur seuil de 70 µg/L), 10 700 µg/L en juin 2012 ;\r\n- une contamination régulière depuis juin 2006 en plomb : maximum à 30 µg/L en juin 2006 (valeur seuil de 10 µg/L), 20 µg/L en juin 2012 ;\r\n- que les paramètres chlorures, cuivre et zinc ne présentent pas de valeurs supérieures à leurs valeurs seuils ;\r\n- que les valeurs maximum pour les paramètres n'ayant pas de valeurs seuils sont : cobalt 10  µg/L (juin 2006 à décembre 2011), rhénium 400 µg/L (juin 2012), titane 20 µg/L (juin 2006), tungstène 240 µg/L (juin 2006) et vanadium 20 µg/L (juin 2012).\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000065501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Chrome | Molybdène","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000065501","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000065501","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000065501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000065601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Trichloroéthylène","Benzène et dérivés | COHV, solvants chlorés, fréons | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000065601","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000065601","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000065601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000065701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Aluminium | Fer","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000065701","Surveillance environnementale","2006-03-01",null,"Résultat de la surveillance à la date du 2013-08-01 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000065701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Chrome | Cuivre","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000065701","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000065701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000065701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000065801","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2013-11-18 : LA SITUATION RESTE STABLE\nCommentaire : absence d'impact\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000065801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000065801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000065901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cadmium | Chrome | Cyanures libres | Mercure | Nickel | Plomb","Autres éléments minéraux | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000065901","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000065901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique"]
["SSP000066101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Trichloroéthylène","COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000066101","Surveillance environnementale","2004-12-29",null,"Résultat de la surveillance à la date du : 2013-06-18\nRésultat de la surveillance eaux souterraines : 1\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000066101","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000066101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000066201","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2010-01-22 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000066201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cadmium | Mercure","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000066201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000066301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP000066301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cuivre | Plomb","COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000066301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000066401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Arsenic | Mercure","COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000066401","Surveillance environnementale","2010-09-03",null,"Résultat de la surveillance à la date du 2015-12-18 : LA SITUATION RESTE STABLE\nInformations complémentaires : La surveillance a été suspendue pendant l'année 2016 notamment du fait du chantier de construction des bâtiments d'habitations. Elle reprendra en 2017.\nDate de fin envisagée de la surveillance : 2017-12-31","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000066401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Cobalt | Molybdène | Plomb | Trichloroéthylène","COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000066401","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000066401","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000066401","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000066401","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000066401","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000066501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Chrome | Cuivre | Plomb","HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000066601","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000066601","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000066601","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000066601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000066701","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Ventilation de la zone non saturée (venting)"]
["SSP000066701","Surveillance environnementale","2001-01-12",null,"Résultat de la surveillance à la date du 2011-10-03 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000066701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000066701","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000066701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000066701","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000066701","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000066701","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000066701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Pompage de rabattement ou de récupération | Reconditionnement de produits dangereux, Reconditionnement de déchets","N/A","N/A","N/A"]
["SSP000066801","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000066801","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000066801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000066901","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000066901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000066901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000067001","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000067001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000067001","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000067001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000067101","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000067101","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000067101","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000067101","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000067101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000067201","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000067201","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000067201","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000067201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000067301","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000067301","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000067301","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000067301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000067401","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000067401","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000067401","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000067401","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000067501","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000067501","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000067501","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000067501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000067601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Chrome | Nickel | Trichloroéthylène","COHV, solvants chlorés, fréons | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000067601","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique"]
["SSP000067601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000067701","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000067701","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000067701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000067701","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000067701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000067801","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000067801","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000067801","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000067801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000067901","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000067901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000067901","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000067901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000068001","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000068001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000068001","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000068001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000068101","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000068101","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000068101","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000068101","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000068201","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000068201","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000068201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000068301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Arsenic | Plomb | Trichloroéthylène","COHV, solvants chlorés, fréons | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000068301","Surveillance environnementale","2009-01-31",null,"Résultat de la surveillance à la date du 2016-01-01 : LA SITUATION S'AMELIORE\nCommentaire : Depuis juin 2013, on observe une tendance générale orientée vers une nette baisse des concentrations en Trichloréthylène, Cis-1,2 Dichloroéthylène et 1,1-Dichloroéthane. Cette tendance est aussi observée pour le chlorure de vinyle, même si elle doit être néanmoins nuancée, compte tenu de la fluctuation des concentrations mesurées sur ce paramètre. LA SITUATION SEMBLE S ‘AMELIORER.\nInformations complémentaires : La surveillance de la qualité des eaux souterraines, à l'amont et à l'aval du site, a été poursuivie (6 campagnes entre 2010 et 2012). Des dépassements ont été observés :\r\n- en chlorure de vinyle en août 2010 (8,9 µg/L), en septembre 2011 (13 µg/L), en décembre 2011 (17 µg/L), en mars 2012 (7,2 µg/L) et en juin 2012 (14µg/L) ;\r\n- en 1,2-dichloroéthylène en août 2010 (320 µg/L), en septembre 2011 (270 µg/L), en décembre 2011 (1 800 µg/L), en mars 2012 (120 µg/L), en juin 2012 (170 µg/L), en août 2012 (57 µg/L) et en décembre 2012 (120 µg/L) ;\r\n - en trichloroéthylène en août 2010 (11 µg/L), en décembre 2011 (58 µg/L) et en décembre 2012 (47 µg/L).\r\n\r\nLes campagnes de surveillance de la qualité des eaux souterraines réalisées en 2013, 2014 et 2015 ont montré des dépassements des valeurs seuils sur les paramètres suivants:\r\n\r\n- Trichloréthylène ( 120 µg/l en mars 2013).\r\n\r\n- Cis-1,2 Dichloroéthylène ( 390 µg/l en mars 2013 et 110 µg/l en juin 2013).\r\n\r\n- Chlorure de vinyle  ( 3,2 µg/l en mars 2013, 6,2 µg/l en juin 2013, 3,6 µg/l en avril 2014, 7,2 µg/l en septembre 2014 et 1,9 µg/l en juin 2015).\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000068301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic","COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000068301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000068401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Ammonium | Arsenic | Trichloroéthylène | Zinc","COHV, solvants chlorés, fréons | Metaux et métalloïdes | Paramètres azotés","N/A","N/A","N/A","N/A","N/A"]
["SSP000068401","Surveillance environnementale","2003-02-21",null,"Résultat de la surveillance à la date du 2012-11-16 : LA SITUATION RESTE STABLE\nInformations complémentaires : L'arrêté préfectoral du 27 décembre 2001 impose la surveillance de la nappe phréatique sur 9 piézomètres de 3 à 6 fois par an pour les paramètres suivants : température, conductivité, azote total, nitrates, ammoniaque, chlorures, oxygène dissous, arsenic, chrome, nickel, plomb et trichloroéthylène.\r\n\r\n\r\nDes dépassements en ammonium sont observés de manière régulière sur les différentes campagnes de surveillances des eaux souterraines depuis 2002. Des concentrations légèrement supérieures aux valeurs seuils (circulaire du 23 octobre 2012) sont également observées de manière régulière en  trichloroéthylène. A noter un dépassement en arsenic en 2008.\n","Eaux souterraines","N/A","6",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000068401","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000068401","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000068501","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000068501","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000068501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000068601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Arsenic | Cadmium | Chrome | Cyanures libres | Nickel | Plomb | Trichloroéthylène","Autres éléments minéraux | COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000068601","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique",null,"Filtration"]
["SSP000068601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Cadmium | Chrome | Cuivre | Cyanures libres | Mercure | Nickel | Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Trichloroéthylène | Zinc","Autres éléments minéraux | Benzène et dérivés | COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000068601","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols","Confinement par couverture et étanchéification"]
["SSP000068701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Nickel","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000068701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Cuivre | Cyanures libres | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Trichloroéthylène | Zinc","Autres éléments minéraux | Benzène et dérivés | COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000068701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000068801","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2011-09-01 : LA SITUATION S'AMELIORE\nCommentaire : Après le travaux de dépollution du site intervenus au premier semestre 2011, aucune pollution en hydrocarbures n'est plus quantifiable au droit ni en aval hydraulique du site lors des campagnes d'avril, de juin ni de septembre 2011.\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000068801","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000068801","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000068801","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique"]
["SSP000068801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...) | Reconditionnement de produits dangereux, Reconditionnement de déchets","N/A","N/A","N/A"]
["SSP000068901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000068901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000069001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Chrome","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000069001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000069101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Aluminium | Fer","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000069101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000069201","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000069201","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000069201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000069301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Plomb","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000069301","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000069301","Surveillance environnementale","2001-05-16",null,"Résultat de la surveillance à la date du 2005-10-14 : LA SITUATION RESTE STABLE\nInformations complémentaires : L'arrêté du 6 octobre 1998 a imposé une surveillance semestrielle des eaux souterraines via 3 piézomètres (Pz 24, Pz Décharge et Pz Bénit) sur les paramètres suivants : conductivité, azote total, nitrates, ammoniaque, chlorures, phosphore ainsi qu'uniquement sur Pz Bénit une analyse bactériologique de type B3 et le plomb.\r\n\r\nLa surveillance des eaux souterraines s'est déroulée de mai 2001 à octobre 2005 (8 campagnes) sur 3 piézomètres. Elle met en évidence les contaminations suivantes :\r\n- phosphore total sur Pz Bénit (maximum à 3,41 mg/L en octobre 2001) ;\r\n- plomb sur Pz Bénit (maximum à 310 µg/L en octobre 2001) ;\r\n- germes aérobies revivifiables (maximum à 500/ml en septembre 2002) ;\r\n- coliformes totaux à 37 °C (maximum à 400/100 ml en septembre 2002) ;\r\n- coliformes thermotolérants à 44 °C (maximum à 2/100 ml en octobre 2001 et mars 2005) ;\r\n- entérocoques (maximum à 20/100 ml en octobre 2001) ;\r\n- spores de bactéries sulfito-réductrices (maximum à 9/20 ml en septembre 2002).\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000069301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000069401","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000069401","Surveillance environnementale","2010-01-01",null,"Résultat de la surveillance à la date du 2013-07-01 : LA SITUATION S'AMELIORE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000069401","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000069401","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000069401","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000069501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Analyse des enjeux sanitaires (EQRS, ARR)","N/A",null,"COHV, solvants chlorés, fréons | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000069501","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique","Confinement par couverture et étanchéification | Oxydation chimique | Ventilation de la zone non saturée (venting)"]
["SSP000069501","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2014-11-24 : LA SITUATION S'AMELIORE\nInformations complémentaires : Teneur résiduelle en COHV sur piézomètres situés en aval du bâtiment (30 à 1300 µg/l), non détectée sur les 2 puits privés situés en aval. PCB non détectés, sur piézomètre aval comme sur puits privés.\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000069501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A",null,"COHV, solvants chlorés, fréons | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000069501","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000069501","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000069501","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000069501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000069601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000069601","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Piège hydraulique ou Confinement hydraulique","Filtration"]
["SSP000069601","Surveillance environnementale","2012-01-23",null,"","Eaux souterraines","N/A","1",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000069601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000069601","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000069601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...) | Pompage de rabattement ou de récupération","N/A","N/A","N/A"]
["SSP000069901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés","N/A","N/A","N/A","N/A","N/A"]
["SSP000069901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Zinc","Benzène et dérivés | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000070001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000070101","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)","Confinement par couverture et étanchéification"]
["SSP000070101","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)","Confinement par couverture et étanchéification"]
["SSP000070101","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)","Confinement par couverture et étanchéification"]
["SSP000070101","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique","Confinement par couverture et étanchéification"]
["SSP000070101","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique","Confinement par couverture et étanchéification"]
["SSP000070101","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Solidification/stabilisation","Confinement par couverture et étanchéification"]
["SSP000070101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000070501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Cuivre | Plomb | Zinc","COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000070501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000070601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000070601","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000070701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Arsenic | Zinc","HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000070701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000072201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000072201","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000072201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000072201","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000072301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000072301","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2003-12-05 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000072301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000072301","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Biodégradation dynamisée (ou atténuation naturelle dynamisée)"]
["SSP000072301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Pompage de rabattement ou de récupération","N/A","N/A","N/A"]
["SSP000072401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Nickel | Plomb","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000072401","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000072501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000072501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000072701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de gestion","N/A",null,"Hydrocarbures et indices liés | Phytosanitaires","N/A","N/A","N/A","N/A","N/A"]
["SSP000072701","Surveillance environnementale","2011-04-20",null,"Résultat de la surveillance à la date du 2013-04-19 : LA SITUATION S'AMELIORE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000072701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A",null,"Hydrocarbures et indices liés | Phytosanitaires","N/A","N/A","N/A","N/A","N/A"]
["SSP000072701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols","Confinement par couverture et étanchéification"]
["SSP000072701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique","Confinement par couverture et étanchéification"]
["SSP000072701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000072801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000072801","Surveillance environnementale","2005-07-28",null,"Résultat de la surveillance à la date du 2011-03-30 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000072801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000072901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000072901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000072901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000073001","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000073001","Surveillance environnementale","2001-02-20",null,"Résultat de la surveillance à la date du 2015-08-18 : LA SITUATION RESTE STABLE\nCommentaire : Inférieur aux seuils autorisés dans l'AP.\n","Eaux souterraines","N/A","1",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000073001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Molybdène | Nickel","HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000073001","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique","Confinement par couverture et étanchéification"]
["SSP000073001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000073001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000073101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000073101","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000073101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000073201","Surveillance environnementale","2007-01-15",null,"Résultat de la surveillance à la date du 2015-09-22 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000073201","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000073201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Mercure","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000073201","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000073201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000073301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000073301","Surveillance environnementale","2003-01-08",null,"Résultat de la surveillance à la date du 2006-06-13 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","1",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000073301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cuivre | Plomb | Zinc","Hydrocarbures et indices liés | Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000073301","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000073301","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000073301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000073401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Chlorures | Sulfates","Autres éléments minéraux","N/A","N/A","N/A","N/A","N/A"]
["SSP000073401","Surveillance environnementale","2003-06-23",null,"Résultat de la surveillance à la date du 2014-09-01 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000073401","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000073401","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000073501","Surveillance environnementale","2006-10-31","2016-02-05","Résultat de la surveillance à la date du 2012-01-30 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000073501","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000073601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Cadmium | Nickel","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000073601","Surveillance environnementale","2003-01-08",null,"Résultat de la surveillance à la date du 2006-06-13 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","1",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000073601","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","1",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000073601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cuivre | Plomb | Zinc","COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000073601","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000073601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000073701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000073701","Surveillance environnementale","2008-10-03",null,"Résultat de la surveillance à la date du 2015-03-19 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000073701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000073701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000073701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000073801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Nickel | Plomb","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000073801","Surveillance environnementale","2005-09-29",null,"Résultat de la surveillance à la date du 2008-06-25 : LA SITUATION S'AMELIORE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000073801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic","HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000073801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage | Interdiction d'accès (clôture...) | Reconditionnement de produits dangereux, Reconditionnement de déchets","N/A","N/A","N/A"]
["SSP000073901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000073901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000073901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000074001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de gestion","N/A","Arsenic | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000074001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Trichloroéthylène","Benzène et dérivés | COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000074001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000074001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000074101","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2015-06-03 : LA SITUATION RESTE STABLE\nCommentaire : Atténuation naturelle des phénols confirmée.\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000074101","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000074101","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Biodégradation dynamisée (ou atténuation naturelle dynamisée)"]
["SSP000074101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000074201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Arsenic | Chrome | Nickel | Plomb","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000074201","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2010-10-05 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000074201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000074801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Nickel | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Trichloroéthylène","Benzène et dérivés | COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000074801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000074801","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000074801","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000074801","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique"]
["SSP000074801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000086401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Trichloroéthylène","COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP000086401","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2010-06-29 : LA SITUATION RESTE STABLE\nCommentaire : Bien que de même ordre de grandeur que la précédente campagne de 2008, les teneurs PCE et TCE augmentent légèrement en latéral hydraulique au site. Situation conforme en aval hydraulique.\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000086401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cadmium | Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Trichloroéthylène","Benzène et dérivés | COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000086401","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000086401","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000086401","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000086401","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000123201","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000123201","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000123201","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000123201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...) | Reconditionnement de produits dangereux, Reconditionnement de déchets","N/A","N/A","N/A"]
["SSP000124001","Surveillance environnementale","2001-07-24",null,"Résultat de la surveillance à la date du 2007-06-14 : LA SITUATION RESTE STABLE\nCommentaire : Satisfaisant amont\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000124001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000124201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Cadmium | Chrome | Plomb","HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000124201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000125001","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 1991-07-25 : LA SITUATION S'AMELIORE\nDate de fin envisagée de la surveillance : 1991-07-25","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000125001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique","Biodégradation dynamisée (ou atténuation naturelle dynamisée)"]
["SSP000125101","Surveillance environnementale","2007-09-14",null,"Résultat de la surveillance à la date du 2008-07-07 : LA SITUATION RESTE STABLE\nCommentaire : pas d'impact constaté\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000125101","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000125101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000125301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Arsenic","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000125301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cuivre | Plomb","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000125401","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"Les analyses effectuées avant travaux, de 2006 à 2018 rapportent des pollutions aux hydrocarbures ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000125401","Exécution des travaux de réhabilitation",null,null," 3 phases de travaux de dépollution par excavation des terres et traitement in situ ou dans des filières ad hoc, remblaiement par terres saines, traitement des eaux de remblais saturés et traitement des eaux profondes","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique","Confinement par couverture et étanchéification | Piège hydraulique ou Confinement hydraulique"]
["SSP000125401","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"Les diagnostics réalisés de 2007 à 2018 rapportent un miliue sol pollué par des hydrocarbures (HCT, FAP) et des solvants (BTEX, COHV).","Sol - Sous-sol","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000125401","Exécution des travaux de réhabilitation",null,null,"Les mesures prises sont le démantèlement et l'enlèvement des installations du site, l'excavation des terres polluées et le traitement de la nappe alluviale ainsi que la surveillance périodique des eaux souterraines.",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000125501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Ammonium | Sulfates","Autres éléments minéraux | Hydrocarbures et indices liés | Paramètres azotés","N/A","N/A","N/A","N/A","N/A"]
["SSP000125501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Ammonium | Plomb | Sulfates","Autres éléments minéraux | Metaux et métalloïdes | Paramètres azotés","N/A","N/A","N/A","N/A","N/A"]
["SSP000125501","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000125501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000127801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Sulfates","Autres éléments minéraux | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000127801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Sulfates","Autres éléments minéraux","N/A","N/A","N/A","N/A","N/A"]
["SSP000127801","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000128401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Trichloroéthylène","COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP000128501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000128501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000128601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000128801","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000128901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000128901","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000128901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000128901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique","Ventilation de la zone non saturée (venting)"]
["SSP000128901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000129001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000129001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000129001","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000129001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000129101","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 1993-10-15 : LA SITUATION RESTE STABLE\nInformations complémentaires : 0.26µg/L de pcb dans les eaux de la nappe.\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000129101","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000129101","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique"]
["SSP000129101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Pompage de rabattement ou de récupération","N/A","N/A","N/A"]
["SSP000129201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de conception des travaux (PCT)","N/A","Chrome | Nickel","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000129201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000129301","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000129301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de conception des travaux (PCT)","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000129301","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique","Ventilation de la zone non saturée (venting)"]
["SSP000129401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de gestion","N/A","Ammonium | Chlorures | Chrome | Sulfates | Zinc","Autres éléments minéraux | Metaux et métalloïdes | Paramètres azotés","N/A","N/A","N/A","N/A","N/A"]
["SSP000129401","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Piège hydraulique ou Confinement hydraulique"]
["SSP000129401","Surveillance environnementale","1998-04-01",null,"Résultat de la surveillance à la date du 2012-03-01 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","3",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000129401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A","Arsenic | Baryum | Cadmium | Cuivre | Mercure | Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Sulfates | Zinc","Autres éléments minéraux | Benzène et dérivés | COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000129501","Surveillance environnementale",null,null,"Commentaire : L'exploitant doit réaliser un bilan de la surveill\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000129501","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000129501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000129701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Nickel","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000129701","Surveillance environnementale","1995-11-01",null,"Résultat de la surveillance à la date du 2000-06-01 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000129701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000129701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000129801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage","N/A","N/A","N/A"]
["SSP000129901","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2012-07-23 : LA SITUATION RESTE STABLE\nInformations complémentaires : LMCU a sollicité en 2012 un allègement du programme de la surveillance des eaux souterraines notamment pour le xylène et l'arsenic qui sont inférieurs aux valeurs guides sur l'ensemble des ouvrages suivis.\r\nLa DREAL a demandé à LMCU d'établir un bilan de la surveillance réalisée depuis 2002 afin de proposer une stratégie globale d'évolution de la surveillance réalisée sur ce site. Ce bilan pourra reprendre les principes du bilan quadriennal prévu au chapitre 4.3 de la circulaire du 08/02/07 relative aux sites et sols pollués - Modalités de gestion et de réaménagement des sites pollués. \n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000130001","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2013-09-05 : LA SITUATION S'AMELIORE\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000130001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000130101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000130101","Surveillance environnementale","2002-04-17",null,"Résultat de la surveillance à la date du 2014-05-01 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000130101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000130201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000130201","Surveillance environnementale",null,null,"Résultat de la surveillance eaux souterraines : 1\n","Eaux souterraines","N/A","1",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000130201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000130201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000130301","Surveillance environnementale","2002-12-01",null,"Résultat de la surveillance à la date du 2014-05-01 : LA SITUATION RESTE STABLE\nCommentaire : Absence de détection des COHV, absence de détection des BTEX, absence de détection des hydrocarbures totaux (résultats similaires aux campagnes précédentes\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000130401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Arsenic","HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000130401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cuivre | Mercure | Plomb","COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000130501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000130501","Surveillance environnementale","2003-08-18",null,"Résultat de la surveillance à la date du 2005-12-31 : LA SITUATION S'AMELIORE\nInformations complémentaires : 2015 :la situation est stable, Teneurs en hydrocarbures et BTEX sont toutes inférieures aux seuils de quantification du laboratoire à l’exception d’un piézomètre qui présente une teneur en hydrocarbures totaux de 44 µg/L.\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000130501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000130501","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Lavage à l'eau","Ventilation de la zone non saturée (venting)"]
["SSP000130501","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique","Ventilation de la zone non saturée (venting)"]
["SSP000130601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Nickel","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000130601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Cadmium | Cuivre | Cyanures libres | Mercure | Nickel | Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Zinc","Autres éléments minéraux | Benzène et dérivés | COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000130801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000130801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000130801","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000130801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000130901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)","Confinement par couverture et étanchéification | Ventilation de la zone non saturée (venting)"]
["SSP000130901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)","Confinement par couverture et étanchéification | Ventilation de la zone non saturée (venting)"]
["SSP000131001","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2002-02-27 : LA SITUATION RESTE STABLE\nCommentaire : sauf augmentation du plomb et du sodium\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000131101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000131101","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique","Piège hydraulique ou Confinement hydraulique","Filtration"]
["SSP000131101","Surveillance environnementale","2002-01-02",null,"Résultat de la surveillance à la date du 2013-04-12 : LA SITUATION S'AMELIORE\nCommentaire : : Phase de surnageant de 1 cm seulement, avec une absence de migration de la pollution en dehors du site.\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000131101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000131101","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Ventilation de la zone non saturée (venting)"]
["SSP000131101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000131201","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000131201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000131301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP000131301","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2013-10-29 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000131301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000131401","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000131401","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000131401","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Lavage à l'eau"]
["SSP000131401","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000131501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de gestion","N/A","Aluminium | Arsenic | Chrome | Nickel | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Sulfates","Autres éléments minéraux | Benzène et dérivés | COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000131501","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000131501","Surveillance environnementale","2005-04-13",null,"Commentaire : La surveillance a montré une pollution de la nappe en hydrocarbures au niveau d’un piézomètre du réseau sur la parcelle 7282.\nInformations complémentaires : Des investigations supplémentaires sont nécessaires afin de : \r\n-diagnostiquer l’état de pollution du sol du site de l’ancien parc à charbon\r\n-diagnostiquer l’origine de la pollution de la nappe sur un piézomètre de la parcelle 7282 et d’en supprimer les causes.\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000131501","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000131501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A","Mercure","COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000131501","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000131501","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000131501","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000131501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000131601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Arsenic | Chlorures | Sélénium | Sulfates","Autres éléments minéraux | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000131601","Surveillance environnementale","2004-11-10",null,"Résultat de la surveillance à la date du 2012-03-01 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000131601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000131701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Arsenic | Cadmium | Chrome | Cuivre | Mercure | Nickel | Plomb | Zinc","COHV, solvants chlorés, fréons | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000131701","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Piège hydraulique ou Confinement hydraulique"]
["SSP000131701","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2001-09-01 : LA SITUATION SE DEGRADE\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000131701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Pompage de rabattement ou de récupération","N/A","N/A","N/A"]
["SSP000131801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Chlorures | Sulfates","Autres éléments minéraux","N/A","N/A","N/A","N/A","N/A"]
["SSP000131801","Surveillance environnementale","2001-05-03",null,"Résultat de la surveillance à la date du 2002-12-05 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000131801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Baryum | Cuivre | Cyanures libres | Zinc","Autres éléments minéraux | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000131801","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000131801","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000132001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000132201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000132501","Surveillance environnementale","2002-07-01",null,"Résultat de la surveillance à la date du 2010-03-08 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000132901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000133201","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000133201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage","N/A","N/A","N/A"]
["SSP000133801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000134301","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2010-12-12 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000134601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000135101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Chrome","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000135301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Chrome","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000135801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP000135801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000136401","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2012-04-11 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000136501","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique"]
["SSP000136701","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000137101","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000137601","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000137701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage","N/A","N/A","N/A"]
["SSP000138201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000138601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000139101","Surveillance environnementale",null,null,"Commentaire : la dégradation n'est pas significative mais il con\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000139401","Surveillance environnementale","2003-05-01",null,"Résultat de la surveillance à la date du 2005-02-01 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000139801","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000140201","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000140801","Surveillance environnementale","2003-01-01","2011-12-31","Commentaire : Pas d'impact sur les eaux souterraines \n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000141101","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000141701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Fer | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés | Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000141901","Surveillance environnementale",null,null,"","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000142001","Surveillance environnementale","2003-06-10",null,"Résultat de la surveillance à la date du 2013-10-11 : LA SITUATION S'AMELIORE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000142301","Surveillance environnementale","2003-01-01",null,"Résultat de la surveillance à la date du 2011-11-15 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000142501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000143301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Chrome | Cuivre | Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000143501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage","N/A","N/A","N/A"]
["SSP000144201","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2013-02-18 : LA SITUATION S'AMELIORE\nCommentaire : amélioration sensible de la situation\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000144401","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Pompage de rabattement ou de récupération","N/A","N/A","N/A"]
["SSP000144901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Trichloroéthylène","COHV, solvants chlorés, fréons | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000145001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"COHV, solvants chlorés, fréons | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000145301","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000145401","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000145601","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000158601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000159201","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000173901","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000179701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000181501","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","9",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000183901","Surveillance environnementale","2004-02-01",null,"Résultat de la surveillance à la date du 2015-06-01 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000187201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000189701","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)","Confinement par couverture et étanchéification"]
["SSP000190401","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000191301","Surveillance environnementale","2010-03-23",null,"Résultat de la surveillance à la date du 2010-04-30 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000193301","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols","Confinement par couverture et étanchéification"]
["SSP000194101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Chrome | Plomb","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000194701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cuivre | Plomb | Zinc","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000194801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000195601","Surveillance environnementale","2003-03-13",null,"Résultat de la surveillance à la date du 2018-06-05 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000196401","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique"]
["SSP000200601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000201601","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)","Confinement par couverture et étanchéification"]
["SSP000202401","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000202501","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique","Confinement par couverture et étanchéification"]
["SSP000202801","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000204301","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique","Confinement par couverture et étanchéification | Ventilation de la zone non saturée (venting)"]
["SSP000204301","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000205401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de gestion","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000205801","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Biodégradation dynamisée (ou atténuation naturelle dynamisée)"]
["SSP000206301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000206801","Surveillance environnementale","1998-08-18",null,"Résultat de la surveillance à la date du 2005-11-17 : LA SITUATION RESTE STABLE\nCommentaire : présence de  cyanures, de HAP\n","Eaux souterraines","N/A","1",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000212501","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000212501","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000212901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Chrome | Mercure","Hydrocarbures et indices liés | Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000213001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000213501","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000214201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A",null,"COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000217101","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique","Barbotage in situ (sparging) | Ventilation de la zone non saturée (venting)"]
["SSP000217201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000217401","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000217501","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000222201","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"Le diagnostic des sols et des eaux souterraines  a révélé une pollution aux hydrocarbures. Des investigations complémentaires ont été nécessaires afin de déterminer l’extension de la pollution. Les analyses réalisées ont mis en évidence une anomalie de la teneur en huiles minérales, pollution confirmée par une teneur en hydrocarbures dans les eaux souterraines et en composés organiques volatils (COV) totaux dans les gaz des sols. Cette pollution est très localisée, dans l’environnement immédiat de l’ancienne cuve d’hydrocarbures. La présence d’hydrocarbures est estimée couvrir environ 600 m², dont 100 m² très pollués. \n\nPar ailleurs, un autre sondage a montré une pollution des sols par les métaux suivants : baryum, cuivre, chrome. Les analyses des eaux souterraines prélevées au même endroit n’ont cependant montré aucun dépassement des normes de potabilité de l’eau concernant les polluants métalliques détectés dans les sols. \n\nL’analyse des gaz des sols au droit d'un autre sondage a permis de détecter une légère concentration en COV totaux, qui est interprétée comme une suspicion de contamination par des hydrocarbures à proximité (en effet une station de distribution d’hydrocarbures est présente). Cependant les mesures dans les sols et dans les eaux, au piézomètre le plus proche, n’ont révélé aucune anomalie.","Eaux souterraines","Diagnostic et Analyse","N/A",null,"HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000222201","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"Au vu du bilan coûts/avantages des différentes solutions techniques envisageables, l’exploitant a retenu : - l’évacuation vers une installation de stockage de déchets dangereux des sols pollués par des pollutions métalliques. - le traitement sur place, par biopile, des sols pollués par des hydrocarbures puis leur stockage dans un merlon paysager recouvert de 30 cm de terres propres. ","Sol - Sous-sol","Plan de gestion","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000222801","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"Dans le cadre d'une démarche de requalification urbaine, l'Etablissement Public Foncier de Lorraine(EPFl) a fait réaliser une Evaluation Simplifiée des Risques qui a été remise à l'inspection le 01 août 2002.\nDes sondages et analyses de sols ont été effectués et plusieurs sources de pollutions ont été recensées :\n- Une zone correspondant à l'ancien hall de fabrication constitue une source de pollution en Cuivre et Hydrocarbures Aromatiques Polycycliques (HAP).\n- L'emplacement des transformateurs et l'ancien atelier d'usinage constituent une source de pollution en PCB et cuivre.\n- L'ancien atelier de peinture et le parc à fer constituent une source de pollution en arsenic, chrome, cuivre, nickel, plomb et zinc.\n- Le secteur de l'ancienne décharge interne constitue une source de pollution en arsenic, chrome et cuivre.  \n\nL'ESR, réalisée dans le cadre d'un usage sensible, classe le site en 1, nécessitant des investigations approfondies, pour l'impact du cuivre et du plomb sur le sol. L'ESR classe également le site en 2, site à surveiller, pour son impact sur les eaux souterraines pour les autres métaux dosés et les PCB.","Eaux souterraines","Analyse des enjeux sanitaires (EQRS, ARR)","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000223101","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"Une étude environnementale est réalisée en février 1999, suite à la démolition du site en juin 1998. Pour cette étude, neuf sondages de sols et des analyses des sédiments en bordure amont et aval de la Meurthe sont réalisés.","Eaux superficielles - Sédiments","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000223401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Baryum | Cadmium | Chrome | Cuivre | Plomb","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000223501","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"Le diagnostic environnemental réalisé par la société TOTAL et remis en 2010 met en évidence principalement un impact du site sur les eaux souterraines aux hydrocarbures totaux ( de l'ordre de 3/4000 µg/l) et BTEX (de l'ordre de 100-300 µg/l). Le piézomètre situé à l'aval latéral du site ne montre pas d'impact.\n\nDes mesures de qualité de l’air intérieur de l’ancienne boutique ont également été menées. Elles ont montré des teneurs en BTEX inférieures aux limites de quantification et des teneurs en hydrocarbures de l’ordre de grandeur des limites de quantification. \n\nL’ancien exploitant conclut à une absence d’impact sur le site et à un impact potentiel hors site via un transfert de la pollution par la nappe phréatique, un dégazage et l’inhalation de vapeurs dans des locaux fermés.","Air","Diagnostic et Analyse","N/A","Indice hydrocarbures totaux - produits pétroliers | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000224101","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000224101","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000226001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000226301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Chrome | Cuivre | Plomb | Zinc","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000227401","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000228501","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000229401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Trichloroéthylène","Benzène et dérivés | COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000229901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000231501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000231701","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"En 2010, un aménageur a porté à la connaissance du Préfet son projet de reconversion du site (futur usage avec habitats, commerces et locaux professionnels).\nL'étude menée dans le cadre du projet a mis en évidence des pollutions des sols par des métaux (exemple : plomb jusque 6000 mg/kg de matière sèche sur un point), la présence de composés organiques dans les sols à des teneurs faibles, et un impact en Hydrocarbures Aromatiques Polycycliques (HAP) au niveau des eaux souterraines (jusque 20µg/l).","Eaux souterraines","Diagnostic et Analyse","N/A","Plomb","HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000231801","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"En février 1998, une Evaluation Simplifiée des Risques a été réalisée (ESR). \nCette étude classait le site en 2, \"à surveiller\" pour son impact sur les eaux souterraines. Dans le cadre de l'ESR, une évaluation des volumes de terres à traiter a été réalisée, cette étude proposait de traiter par lagunage un volume de terres estimé à 1000 m3 et dont la teneur en hydrocarbures est supérieur à 800 ppm.","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000231901","Surveillance environnementale",null,null,"Un suivi de la qualité des eaux a été réalisé au cours du mois de novembre 2001. Ce dernier conclut que les teneurs en HCT et BTEX dissous dans les eaux sont inférieurs au seuil de référence.","Eaux souterraines","N/A","1","Indice hydrocarbures totaux - produits pétroliers | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000232701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000233001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000233601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000234901","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000236001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Aluminium","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000237101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de gestion","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000237501","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000237601","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000238001","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000238301","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000239401","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"L'étude environnementale réalisée en 2006 a démontré la présence de boues de neutralisation (environ 4 000 m3) au sein du crassier. Les analyses réalisées confirment un potentiel polluant important.","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000239801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000240601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Cyanures libres","Autres éléments minéraux","N/A","N/A","N/A","N/A","N/A"]
["SSP000240901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000241501","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000242101","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000242901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique"]
["SSP000243201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000244201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000244601","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"Les investigations menées lors de la réalisation du diagnostic de la qualité des sols en février 2007 ont montré des teneurs en COHV toutes inférieures à la limite de quantification de l'analyse, la détection de teneurs en BTEX et la présence de HAP (dont benzoapyrène) dans les sols dans des teneurs significatives (dans la partie superficielle des remblais). Les concentrations en benzoapyrène mesurées sont susceptibles d'engendrer un risque sanitaire pour la population cible (travailleurs). Ce risque est lié à la possibilité d'être en contact direct avec ces terres, et les voies de transfert considérées sont le contact cutané, l'inhalation de vapeurs et l'ingestion de terres polluées.\n\nL'arrêté préfectoral autorisant la société PIMEST à reprendre une partie des activités exercées par EUROGEP (30 novembre 2007) a donc prescrit la réalisation d'analyses de sols pour délimiter la zone de pollution. ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Benzo(a)pyrène | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés)","N/A","N/A","N/A","N/A","N/A"]
["SSP000245401","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000245801","Surveillance environnementale","2005-04-01",null,"Résultat de la surveillance à la date du 2014-05-26 : LA SITUATION RESTE STABLE\nCommentaire : Depuis le début de la surveillance, la situation reste stable. \r\nDes HAP sont détectés dans les eaux souterraines au droit du site. \r\nLes teneurs en TCE, PCE et en chlorure de vinyle sont supérieures aux valeurs de gestion réglementaires en aval du site.\nInformations complémentaires : Surveillance de l'air intérieur d'habitations riveraines (fréquence semestrielle)\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000246501","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2012-09-26 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000246501","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)","Confinement par couverture et étanchéification"]
["SSP000248802","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000249501","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000249701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000250001","Surveillance environnementale","2004-08-01",null,"Résultat de la surveillance à la date du 2004-08-31 : LA SITUATION RESTE STABLE\nInformations complémentaires : Les analyses d'août 2004 ont permis de confirmer l'absence d'impact du site sur les eaux souterraines.\r\n\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000250501","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"La DRIRE a proposé des prescriptions visant des investigations complémentaires afin de préciser l'étendue de la zone polluée avant traitement. Ces mesures ont été prescrites par arrêté préfectoral du 23 octobre 2003.\nL'exploitant a remis à la DRIRE le 17 mars 2004, un diagnostic complémentaire sur la pollution des sols. Pour la réalisation de ce diagnostic des sondages supplémentaires ont été effectuées. Ces sondages ont permis de cerner une zone polluée sur une profondeur maximale de 2.5 m correspondant à l'emplacement d'anciens gazomètres. ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés)","N/A","N/A","N/A","N/A","N/A"]
["SSP000250701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Baryum | Cadmium | Sulfates | Zinc","Autres éléments minéraux | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000251301","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000251301","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000251501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...) | Pompage de rabattement ou de récupération | Reconditionnement de produits dangereux, Reconditionnement de déchets","N/A","N/A","N/A"]
["SSP000251801","Surveillance environnementale",null,null,"","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000260801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cuivre | Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000262901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000264301","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2007-11-13 : LA SITUATION SE DEGRADE\nCommentaire : Résultats d'analyses de mai 2008 attendus\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000266001","Surveillance environnementale",null,null,"","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000268101","Surveillance environnementale",null,null,"","Eaux souterraines","N/A","1",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000268101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000269101","Surveillance environnementale","2004-07-17",null,"Résultat de la surveillance à la date du 2010-05-20 : LA SITUATION RESTE STABLE\nCommentaire : détection d'hydrocarbures\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000271201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...) | Reconditionnement de produits dangereux, Reconditionnement de déchets","N/A","N/A","N/A"]
["SSP000272401","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000274801","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"Une Evaluation Simplifiée des Risques a été remise le 27 juillet 2001, et validé par l'inspection des installations classées le 13 juillet 2001. Ces études mettent en évidence une pollution des sols essentiellement par les HAP (Hydrocarbures Aromatiques Polycycliques). L'ESR classe le site en catégorie 1 nécessitant des investigations approfondies pour les sols (étude détaillée des risques (EDR)) et classe le site à surveiller pour son impact sur les eaux souterraines.","Eaux souterraines","Analyse des enjeux sanitaires (EQRS, ARR)","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000275001","Surveillance environnementale",null,null,"Par arrêté préfectoral du 18 juin 2003, la surveillance des eaux souterraines par prélèvements semestriels ainsi que des analyses des eaux du Dorlon en amont et aval du site ont été prescrit.","Eaux superficielles - Sédiments","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000275201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A","Cuivre | Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Zinc","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000275601","Exécution des travaux de réhabilitation",null,null,"L'exploitant a fourni un rapport présentant les travaux effectués sur la partie haute du site. En effet, afin de rendre l'état du site compatible avec un usage industriel, l'exploitant a réalisé les mesures de gestion suivantes : \n\n- élimination des infrastructures industrielles (deux cuves et un séparateur d'hydrocarbures)\n\n- traitement de la pollution sur trois secteurs (casiers, ancienne déchèterie et anciennes cuves de carburants) par excavation de 148 tonnes de terres contaminées et élimination dans des filières appropriées\n\n- confinement par 30cm de matériaux sains du secteur de la partie basse du site contaminé afin de couper toute voie de transfert de la pollution.","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)","Confinement par couverture et étanchéification"]
["SSP000275901","Exécution des travaux de réhabilitation",null,null,"Le mandataire liquidateur de la société BOIS FRANCE SCIAGE a mis en place les mesures de mise en sécurité suivantes :\n- nettoyage du bâtiment et évacuation des déchets\n- cuve à fioul vidée\n- installations de l'ancienne chaufferie de biomasse démantelées\n- retrait de  matériel et de matières combustibles au niveau du hangar et des lignes de production\n- les fosses ont été comblées\n- les sciures de bois non traitées ont été collectées et étalées sur une zone enherbée du site","Sol - Sous-sol","N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000276001","Exécution des travaux de réhabilitation",null,null,"Le plan de gestion a été mis en œuvre en 2010-2011 :\n\n1- Les travaux d’excavation et de traitement hors site de la pollution présente au droit de l’ancienne zone à déchets (zones A et B) ont été exécutés début 2010 et ont été suivis de prélèvements et d’analyses en bords et fond de fouille, ainsi que d’une analyse des risques résiduels afin de vérifier la bonne dépollution de cette zone. La zone excavée a été remblayée avec des terres non polluées issues du tri des terres excavées et de matériaux calcaires inertes provenant de l’extérieur. \n\n2- Pour la zone non recouverte impactée en métaux située en rive gauche de la Crusnes, l’exploitant a réalisé une EQRS démontrant l’absence de risques sanitaires pour un travailleur présent à raison d’1 h/jour sur cette zone, compte tenu de l’usage industriel retenu. Néanmoins, après échange avec l’inspection des installations classées, la solution retenue est la suppression du contact direct avec la pollution présente sur cette zone par la mise en place d’une couche de terres inertes sur une épaisseur de 30 cm, sur l’ensemble de la zone non recouverte. Ces travaux ont été faits en 2011.\n\n3- Le traitement des eaux souterraines a été réalisé d’octobre 2010 à octobre 2011. 13 campagnes d’injection de peroxyde d’hydrogène (H2O2). Les taux d’abattement du chlorure de vinyle obtenus sur l’ensemble des piézomètres varient entre 60 et 100 %.  A l’issue du traitement, l’exploitant a fait établir un bilan quadriennal du suivi de la qualité des eaux souterraines et des eaux superficielles qui montre que les teneurs en chlorure de vinyle restent supérieures aux normes de potabilité (0,5 µg/l) issues de l’arrêté ministériel du 11 janvier 2007 relatif aux limites et références de qualité des eaux brutes et des eaux destinées à la consommation humaine, avec un impact toutefois limité, la concentration maximale mesurée en chlorure de vinyle sur l’ensemble des piézomètres depuis la fin du traitement étant de 1,2 µg/l.","Eaux superficielles - Sédiments","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols","Oxydation chimique"]
["SSP000276001","Exécution des travaux de réhabilitation",null,null,"L'inspection a constaté en mai 2008 que toutes les cuves ont été vidangées et les produits évacués.","Sol - Sous-sol","N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000276301","Surveillance environnementale",null,null,"Une surveillance des eaux souterraines a été mise en place en 2009.\nLes teneurs en COHV mesurées dans les eaux souterraines sont les suivantes : 29 µg/l en mars 2012 passant à 2.8 µg/l en septembre 2013, notamment en chlorure de vinyle (pour une valeur de référence de 0.5 µg/l). Il est confirmé qu'il n'existe pas de source de pollution en COHV alimentant la nappe.\nLa surveillance des eaux souterraines se poursuit.","Eaux souterraines","N/A","2","Chlorure de vinyle","COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP000278901","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000279401","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000279701","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000279701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000280101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000280401","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000280801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Interprétation de l''état des milieux (IEM)","N/A","Arsenic","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000280801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000281301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A","Baryum | Chrome | Cuivre | Cyanures libres","Autres éléments minéraux | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000281801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000281901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Solidification/stabilisation"]
["SSP000284701","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Piège hydraulique ou Confinement hydraulique | Ventilation de la zone non saturée (venting)","Filtration"]
["SSP000284701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A","Arsenic | Cadmium | Cuivre | Mercure | Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | COHV, solvants chlorés, fréons | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000289801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Ammonium | Arsenic | Chlorures","Autres éléments minéraux | Metaux et métalloïdes | Paramètres azotés | Phytosanitaires","N/A","N/A","N/A","N/A","N/A"]
["SSP000289901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000290201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Plomb","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000291001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Chrome | Trichloroéthylène","COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000293001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," Nouveau diagnostic en 2005","Sol - Sous-sol","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000293301","Exécution des travaux de réhabilitation",null,null,"Travaux de dépollution","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)","Confinement par couverture et étanchéification"]
["SSP000293701","Exécution des travaux de réhabilitation",null,null,"Réhabilitation","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000293901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Ammonium | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Paramètres azotés","N/A","N/A","N/A","N/A","N/A"]
["SSP000294401","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000294501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Chrome | Cuivre | Nickel","COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000294701","Surveillance environnementale","2003-10-15",null,"Résultat de la surveillance à la date du 2005-07-01 : LA SITUATION S'AMELIORE\nCommentaire : Par rapport de l'inspection des installations classées du 25/07/2017, il a été demandé à la société SAFRAN TRANSMISSION SYSTEMS (ex HISPANO SUIZA) de réaliser une campagne de suivi des eaux souterraines dans un délai de 4 mois conformément à l'arrêté préfectoral complémentaire du 15 octobre 2003.\n","Eaux souterraines","N/A","1",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000294801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000295201","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Piège hydraulique ou Confinement hydraulique | Ventilation de la zone non saturée (venting)"]
["SSP000297201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000298401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000298601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Chrome | Cuivre | Plomb | Trichloroéthylène","COHV, solvants chlorés, fréons | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000298701","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000299201","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000299401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Zinc","Benzène et dérivés | COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000299901","Surveillance environnementale","2002-06-01",null,"Résultat de la surveillance à la date du 2010-12-01 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000300201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000301101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000301501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Ammonium | Cadmium | Cuivre | Fer | Sulfates","Autres éléments minéraux | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes | Paramètres azotés","N/A","N/A","N/A","N/A","N/A"]
["SSP000301601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Zinc","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000302401","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000303301","Surveillance environnementale","2007-07-01",null,"Résultat de la surveillance à la date du 2012-03-01 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000303401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Ammonium | Cyanures libres","Autres éléments minéraux | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Paramètres azotés","N/A","N/A","N/A","N/A","N/A"]
["SSP000303901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000303901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000304801","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000305001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Arsenic | Chlorures | Chrome | Mercure | Nickel | Plomb | Sulfates","Autres éléments minéraux | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000305401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Zinc","Benzène et dérivés | COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000305601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000305901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Ammonium | Sulfates","Autres éléments minéraux | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Paramètres azotés","N/A","N/A","N/A","N/A","N/A"]
["SSP000306101","Surveillance environnementale","1997-02-01",null,"Résultat de la surveillance à la date du 2001-12-20 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000306401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Plomb | Zinc","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000307001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Arsenic | Nickel | Plomb","HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000307101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000307401","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000307701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000308301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000308401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Cadmium | Chrome | Cuivre | Mercure | Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Zinc","Benzène et dérivés | COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000308701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Fer | Molybdène","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000309101","Surveillance environnementale",null,null,"","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000309601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Ammonium","Paramètres azotés","N/A","N/A","N/A","N/A","N/A"]
["SSP000309801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage","N/A","N/A","N/A"]
["SSP000310101","Surveillance environnementale","1999-03-01",null,"Résultat de la surveillance à la date du 2009-11-01 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","1",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000310401","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000310801","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000311201","Surveillance environnementale","2000-03-01",null,"Résultat de la surveillance à la date du 2012-10-01 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","3",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000311501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage","N/A","N/A","N/A"]
["SSP000311801","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2010-10-08 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000311901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Chrome | Cuivre | Nickel | Zinc","HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000312401","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000312501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Chlorures | Cyanures libres | Sulfates","Autres éléments minéraux | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés)","N/A","N/A","N/A","N/A","N/A"]
["SSP000312801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Ammonium | Baryum | Chlorures | Sulfates","Autres éléments minéraux | Metaux et métalloïdes | Paramètres azotés","N/A","N/A","N/A","N/A","N/A"]
["SSP000313601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Arsenic | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000314701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000314901","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000315101","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000315201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Cadmium | Chlorures | Sulfates","Autres éléments minéraux | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000315901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cadmium | Chrome | Cuivre | Mercure | Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Zinc","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000316001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000316701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Analyse des enjeux sanitaires (EQRS, ARR)","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000316801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000317901","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000318001","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Ventilation de la zone non saturée (venting)","Filtration"]
["SSP000319001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000319701","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2013-10-22 : LA SITUATION RESTE STABLE\nCommentaire : présence de flottant sur 5 des 6 ouvrages\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000320301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000320501","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000321001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000322601","Surveillance environnementale","2011-11-22",null,"Résultat de la surveillance à la date du 2015-07-06 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000322601","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000322801","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2011-10-13 : LA SITUATION SE DEGRADE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000325001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000325801","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération","Confinement par couverture et étanchéification"]
["SSP000326601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Cuivre | Plomb | Zinc","HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000326701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000327001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Ventilation de la zone non saturée (venting)"]
["SSP000327501","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Piège hydraulique ou Confinement hydraulique"]
["SSP000327701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000327901","Surveillance environnementale","2010-10-01",null,"Résultat de la surveillance à la date du 2012-04-13 : LA SITUATION RESTE STABLE\nCommentaire : Pollution plus importante en amont\nInformations complémentaires : Demande d'allègement après une période de surveillance de trois ans formulée par l'exploitant en date du 21 août 2012. Acceptée, sauf en ce qui concerne la surveillance des COHV présents au droit du site.\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000328701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Cadmium | Cuivre | Mercure | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Trichloroéthylène | Zinc","Benzène et dérivés | COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000329401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Interprétation de l''état des milieux (IEM)","N/A","Arsenic | Cadmium | Chrome | Cuivre | Plomb | Zinc","HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000329701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000329801","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000330401","Surveillance environnementale","2004-09-01",null,"Résultat de la surveillance à la date du 2008-10-01 : LA SITUATION S'AMELIORE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000332401","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000333601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," 16 janvier 2008 : diagnostic complémentaire relatif à un projet d'aménagement de 39 logements ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cuivre | Cyanures libres | Nickel | Zinc","Autres éléments minéraux | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000333901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cadmium | Plomb | Trichloroéthylène | Zinc","COHV, solvants chlorés, fréons | Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000334201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Interprétation de l''état des milieux (IEM)","N/A",null,"COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP000334301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000335101","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000335201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Arsenic | Plomb | Trichloroéthylène | Zinc","COHV, solvants chlorés, fréons | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000336101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000336301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000337101","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Solidification/stabilisation"]
["SSP000337701","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique",null,"Filtration"]
["SSP000338501","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000338601","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000340601","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique"]
["SSP000342101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Chrome | Plomb | Trichloroéthylène","COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000343701","Surveillance environnementale","2015-03-01",null,"Résultat de la surveillance à la date du 2016-06-01 : LA SITUATION RESTE STABLE\nInformations complémentaires : La dernière campagne d’analyses des eaux souterraines réalisée en juin 2016 indique toujours une absence d’impact sur le paramètre des hydrocarbures mais un impact au trichloréthylène (TCE) sur le piézomètre 4 (PZ4) avec une teneur de 370 µg/l et le piézomètre 2 (PZ2) avec une teneur de 220 µg/l.\r\n\r\nLa valeur relevée en trichloroéthylène sur PZ4 en avril 2015 était de 2500 µg/l rendant impropre l’eau à la consommation humaine. \r\nLes analyses réalisées dans les puits situés sur la parcelle privée n° 2, et n° 419 contiguës au site, indique une absence d’impact au TCE.\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000343701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000344301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000344801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de gestion","N/A","Arsenic | Nickel | Plomb | Sulfates","Autres éléments minéraux | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000345501","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000345701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cyanures libres","Autres éléments minéraux | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000346501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000346701","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2013-10-18 : LA SITUATION S'AMELIORE\nInformations complémentaires : Teneur détectée d'hydrocarbures totaux bien en dessous de la valeur guide au droit de l'ancienne cuvette et l'absence dans les autres zones.\r\nAbsence / quasi-absence de BTEX (concentrations inférieures ou proches des seuils de détection du laboratoire) sur les quatre piézomètres suivis.\r\nAbsence / quasi-absence d'Hydrocarbures Aromatiques Polycycliques (HAP) sur l'ensemble des ouvrages. \n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000347201","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000347601","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique"]
["SSP000348101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000348301","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique"]
["SSP000349001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000349301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000350101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000350101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000350401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000350501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000350901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A","Arsenic | Chrome | Nickel | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | COHV, solvants chlorés, fréons | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000351201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage","N/A","N/A","N/A"]
["SSP000352101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cadmium | Chrome | Cuivre | Mercure | Nickel | Plomb | Zinc","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000352401","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...) | Pompage de rabattement ou de récupération","N/A","N/A","N/A"]
["SSP000352901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000353701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000353901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000354201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000355101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cyanures libres | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Autres éléments minéraux | Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés)","N/A","N/A","N/A","N/A","N/A"]
["SSP000355401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cyanures libres","Autres éléments minéraux | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000356001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cuivre | Zinc","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000356301","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000357001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000357201","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000357301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Pompage de rabattement ou de récupération","N/A","N/A","N/A"]
["SSP000357901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés | Phytosanitaires","N/A","N/A","N/A","N/A","N/A"]
["SSP000358401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000359001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Cyanures libres","Autres éléments minéraux","N/A","N/A","N/A","N/A","N/A"]
["SSP000359401","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000359501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000360001","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000360001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000360101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000360501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic","Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000361301","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000361701","Surveillance environnementale","2001-08-03",null,"Résultat de la surveillance à la date du 2004-11-10 : LA SITUATION S'AMELIORE\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000361901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage","N/A","N/A","N/A"]
["SSP000362801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000363201","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000363301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000363701","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000364901","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000365201","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000366901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000367201","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"   ","Eaux souterraines","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000367301","Surveillance environnementale","2003-07-01",null,"Résultat de la surveillance à la date du 2010-07-26 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000367501","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"  ","Eaux souterraines","Plan de gestion","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000367501","Exécution des travaux de réhabilitation",null,null,"  ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000367801","Surveillance environnementale","1995-10-01",null,"Résultat de la surveillance à la date du 2014-04-01 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000368101","Surveillance environnementale","1995-10-01",null,"Résultat de la surveillance à la date du 2012-10-18 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000368301","Exécution des travaux de réhabilitation",null,null,"  ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)","Confinement par couverture et étanchéification"]
["SSP000368501","Surveillance environnementale","1995-10-01",null,"Résultat de la surveillance à la date du 2012-10-01 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000368801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000369001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000369301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000369401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP000369801","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2006-08-11 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000370301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000370401","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage | Interdiction d'accès (clôture...) | Reconditionnement de produits dangereux, Reconditionnement de déchets","N/A","N/A","N/A"]
["SSP000370801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000371601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Fer | Nickel | Sulfates","Autres éléments minéraux | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000371701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000372001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique","Confinement par couverture et étanchéification"]
["SSP000372101","Surveillance environnementale","2000-07-06",null,"Résultat de la surveillance à la date du 2011-04-26 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000372201","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération","Confinement par couverture et étanchéification"]
["SSP000372401","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000372701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000373601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000375201","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"Dans le cadre de la liquidation judiciaire, un diagnostic de pollution de sols du site a été établi par un bureau d’études. Ses résultats et conclusions sont rassemblés dans un  rapport daté du 11 février 2014.\nLes analyses de sols opérées révèlent un impact significatif en hydrocarbures totaux (type gasoil ou fuel domestique) au droit du parking sud du site mais limité verticalement.\nCes nouveaux sondages ne montrent pas d’extension des  pollutions initialement identifiées dans le cadre  des investigations réalisées à la demande de l’ancienne société TRAILOR en 2004. Elles s’avèrent limitées.\nUn nouvel impact en hydrocarbures totaux et en hydrocarbures aromatiques polycycliques est observé au droit de la zone de brûlage sur un seul sondage entre 0 et 1 mètre de profondeur.\nLes risques potentiels pour les usagers et les employés sont constitués par contact direct avec les sols, l’ingestion de sol et de poussières impactées. Mais tous les sols sont recouverts, soit par une dalle béton à l’intérieur des bâtiments, soit par des enrobés goudronnés. Ce risque n’a donc pas été retenu.\nHors site, le risque pour les usagers des eaux souterraines n’est pas retenu.","Eaux souterraines","Diagnostic et Analyse","N/A","Indice hydrocarbures totaux - produits pétroliers","HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000375301","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000376501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Cadmium | Chrome | Cuivre | Mercure | Plomb | Zinc","COHV, solvants chlorés, fréons | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000376801","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000377001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Aluminium | Plomb","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000377401","Exécution des travaux de réhabilitation",null,null,"Les déchets présents sur le site (bonbonnes de gaz, benne de camion...) ont été éliminés par l'exploitant.\nLes deux emplacements ayant accueilli des dépôts de véhicules hors d'usage ont été clôturés.\nL'évacuation des carcasses des véhicules hors d'usage et le retrait des fluides inflammables a permis la suppression du risque d'incendie.","Sol - Sous-sol","N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000378001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Ventilation de la zone non saturée (venting)"]
["SSP000378601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000378901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000379301","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"Dans le cadre de la cessation définitive d'activité, un mémoire de notification de cessation d’activité a été établi le 6 août 2014. \nLe bureau d’études a procédé à des investigations de terrain en avril 2014. Elles ont consisté en la réalisation de 4 sondages dans les sols avec 3 prélèvements de gaz souterrains à l’intérieur du bâtiment, 1 sondage à proximité du local du transformateur et 1 sondage équipé d’un piézomètre dans l’ancienne zone de stockage extérieure des déchets.\n\nCes investigations de terrain ont mis en évidence des pollutions significatives des sols en hydrocarbures (jusque 2100 mg/kg de matière sèche), composés aromatiques (BTEX) et métaux ainsi que des eaux souterraines en composés organohalogénés volatils (COHV).","Sol - Sous-sol","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | COHV, solvants chlorés, fréons | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000380301","Exécution des travaux de réhabilitation",null,null,"En octobre 2001, la zone polluée a été excavée et les terres ont été dirigées vers un CET de classe 2. Ce qui a représenté une quantité de 272 tonnes.\nLe 13 février 2002, un inspecteur des installations classées de la DRIRE a effectué une visite de récolement de fin de travaux de dépollution.","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000380401","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"Le diagnostic complémentaire remis en janvier 2011 met en évidence :\n- la présence de 8 sources de pollution (hydrocarbures, métaux, HAP et composés organiques). \n- pas d'impact significatif sur les eaux souterraines (excepté sur l'eau distribuée au local du gardien - mise en évidence d'une concentration en plomb supérieure à la limite de qualité des eaux potables)\n-  la présence de solvants chlorés, naphtalène et hydrocarbures dans les gaz du sol.\n\n6 mesures de gaz du sol ont été effectuées au droit des sources les plus marquées ainsi qu’au droit de l’éventuel futur local de gardien. La présence de solvants chlorés, naphtalène et/ou hydrocarbures est mise en évidence dans les gaz du sol pour 5 des 6 piezairs ayant servi aux prélèvements.","Air","Diagnostic et Analyse","N/A","Naphtalène","COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000380401","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"Sur la base des constats de pollution mis en évidence (gaz du sol, eaux souterraines et pollution des sols) et du plan de gestion, le bureau d’études a procédé à une analyse des risques résiduels pour un usage industriel, laquelle conclut à un risque acceptable.","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000380701","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"Des prélèvements et analyses de sols ont été réalisés pour chacune des zones suspectées, après comparaisons des valeurs mesurées aux valeurs nationales de références (VDSS) et aux valeurs caractérisant le fond géochimique local, les zones suivantes ont été identifiées comme sources de pollutions liées aux activités industrielles :\n- le secteur des anciens hauts-fourneaux, de l'ancienne fonderie et l'ancienne forge et des laminoirs montrent des pollutions par du chrome et du plomb,\n- des pollutions par du cuivre et du chrome ont été détectées sous le stockage des sels et scories d'aluminium,\nAucune pollution par hydrocarbures n'a été détectée.\n\nDes prélèvements d'eaux souterraines ont été réalisés en amont et en aval du site, aucune trace de pollution liée aux métaux précédemment identifiés n'a été détectée par contre on observe une augmentation significative des teneurs en sodium et en potassium des eaux souterraines.\nCette augmentation s'explique certainement par la présence d'un stockage de sels et de scories d'affinage d'aluminium.","Sol - Sous-sol","Diagnostic et Analyse","N/A","Chrome | Plomb","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000380801","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"Dans le cadre de l'arrêt des activités, une Evaluation Simplifiée des Risques (ESR) a été effectuée.\n\nDans le cadre de cette étude, 25 sondages de sol ont été effectués. Les analyses montrent la présence de métaux lourds (Arsenic, Baryum, Chrome, Cuivre, Plomb et Vandium) dans les remblais constituant le sol du site.\nLes concentrations en polluants détectés sont inférieures aux VCI non sensibles, valeurs de constats d'impact définies dans le cadre d'un usage non sensible d'un site. Des Hydrocarbures (HAP et pthalates) et de PCB ont également été détectées dans les sols. L’état géochimique des sols est compatible avec un usage industriel du site. \n\nAfin de déterminer l'impact des sols sur les eaux souterraines, quatre piézomètres ont été implantés au droit du site. Les analyses réalisées sur les eaux souterraines montrent une contamination des eaux souterraines par des HAP '(6µg/l en 2004) et en hydrocarbure totaux (160 µg/l en 2004) sur un point du site. L'ESR classe le site en classe 2, à surveiller, pour son impact vis-à-vis des eaux souterraines. \nLes substances à surveiller sont les métaux lourds, les hydrocarbures totaux, les HAP et les PCB.\n\nCompte tenu des éléments ci-dessus, ce site a fait l'objet, le 15 mai 2006, d'un procès-verbal de récolement par l'inspection des installations classées relatif à la remise en état du site pour un usage industriel. ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000381301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de conception des travaux (PCT)","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000381601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de conception des travaux (PCT)","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000381701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Baryum | Cuivre | Plomb | Zinc","HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000382001","Surveillance environnementale",null,null,"Surveillance des sédiments","Eaux superficielles - Sédiments","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000382301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000382301","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000382501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000382701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000382901","Exécution des travaux de réhabilitation",null,null,"Avril 2001 : excavation et évacuation de 228 tonnes supplémentaires de terres polluées.","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000383101","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique"]
["SSP000383301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000383601","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Oxydation chimique | Ventilation de la zone non saturée (venting)"]
["SSP000383801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000383901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000384401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Ammonium","Hydrocarbures et indices liés | Paramètres azotés","N/A","N/A","N/A","N/A","N/A"]
["SSP000384601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Cuivre | Plomb","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000384801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000385101","Surveillance environnementale","2011-08-04",null,"Résultat de la surveillance à la date du 2011-11-04 : LA SITUATION S'AMELIORE\nInformations complémentaires : La campagne de novembre 2011 met en évidence :\r\n-la présence d'eaux souterraines comprise en 6,3 et 8,3 m de profondeur sur le site, et d'un puits captant les eaux souterraines des terrains calcaires sous-jacents,\r\n-un sens d'écoulement des eaux souterraines dirigé vers le nord-est avec un gradient hydraulique de l'ordre de 0,7%. Ce sens d'écoulement est cohérent à celui déterminé depuis juin 2006,\r\n-l'absence d'indice organoleptique de contamination au droit de l'ensemble des ouvrages prélevés lors de cette campagne,\r\n-au regard de l'ensemble des résultats, la persistance d'un impact en formaldéhyde et COHV en amont hydraulique du site à proximité du bâtiment accueillant l'ancien \"secteur finition\" et où une source sol de pollution en COHV a été extraite en mai 2010. Un impact résiduel est confirmé en novembre 2011 au droit des ouvrages PZ7 et PZ11, qui présentent des teneurs significatives en COHV. \r\n- une amélioration globale de la qualité des eaux au droit du site (diminution des teneurs en COHV en amont et aval du site) depuis le début du suivi. \n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000385401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Aluminium","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000385701","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000385801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000385901","Exécution des travaux de réhabilitation",null,null,"Mise sur rétention de la cuve.","Sol - Sous-sol","N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000386501","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)","Confinement par couverture et étanchéification"]
["SSP000386701","Exécution des travaux de réhabilitation","2009-01-01","2017-11-02","Les derniers travaux de dépollution ont été menés par la société Séché Eco Services, sous la supervision du bureau conseil Aquila Conseil ayant réalisé le plan de gestion. Ces travaux ont eu lieu entre le 19 octobre et le 2 novembre 2017.\nIls ont consisté comme prévu en l’excavation des terres polluées au niveau des zones identifiées.\n\nSelon les résultats d’analyses effectuées sur les échantillons prélevés, les terres excavées ont été soit :\n    • valorisées en tant que matières premières en cimenterie, avec ou sans criblage préalable (746 tonnes),\n    • enfouies (pour les matériaux grossiers) dans une installation de stockage de déchets non dangereux (85 tonnes),\n    • enfouies dans une installation de stockage de déchets dangereux (en raison de teneurs en antimoine trop élevées – 74 tonnes).\nAinsi, 905 tonnes de terres ont été évacuées du site.","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000388001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...) | Reconditionnement de produits dangereux, Reconditionnement de déchets","N/A","N/A","N/A"]
["SSP000388701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de gestion","N/A","Aluminium | Chrome | Cuivre | Plomb","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000388901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000389301","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000389701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Plomb","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000390001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols","Confinement par couverture et étanchéification"]
["SSP000390801","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000391001","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000392201","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique","Piège hydraulique ou Confinement hydraulique"]
["SSP000393601","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2016-07-07 : LA SITUATION RESTE STABLE\nInformations complémentaires : Poursuite de la surveillance des eaux souterraines à fréquence semestrielle.\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000394301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000395801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Chrome | Trichloroéthylène","COHV, solvants chlorés, fréons | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000395801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Cadmium | Chrome | Cuivre | Mercure | Nickel | Plomb | Zinc","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000396101","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000397001","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000397301","Exécution des travaux de réhabilitation",null,null,"Excavation des sols","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000397701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000398001","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000398701","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000399001","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000399701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Arsenic | Sulfates","Autres éléments minéraux | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000399801","Exécution des travaux de réhabilitation",null,null," Incinérattion","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000400301","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)","Confinement par couverture et étanchéification"]
["SSP000400801","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000401101","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000401401","Surveillance environnementale","2003-09-10",null,"Résultat de la surveillance à la date du 2007-10-01 : LA SITUATION S'AMELIORE\nCommentaire : Les hydrocarbures totaux ne sont pas dans les critères de potabilité de l'eau définis dans l'Annexe I du Décret n°2001-1220 du 20 décembre 2001 relatif aux eaux destinées à la consommation humaine. Pour le pentachlorophénols qui sont des <<pesticides>>, les valeurs mesurées respectent le critère de potabilité fixé par le Décret précité.\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000401701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Ammonium | Chlorures | Fer","Autres éléments minéraux | Metaux et métalloïdes | Paramètres azotés","N/A","N/A","N/A","N/A","N/A"]
["SSP000401801","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2013-11-06 : LA SITUATION SE DEGRADE\nCommentaire : Non satisfaisant aval.\nInformations complémentaires : Une pollution des eaux en aval hydraulique du site a été détectée lors de la dernière campagne.\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000402301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000402401","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000403001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A","Arsenic | Chrome | Cuivre | Plomb","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000403101","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique","Piège hydraulique ou Confinement hydraulique | Ventilation de la zone non saturée (venting)"]
["SSP000403601","Surveillance environnementale","2001-05-15",null,"Résultat de la surveillance à la date du 2009-04-01 : LA SITUATION RESTE STABLE\nInformations complémentaires : surveillance abandonnée suite à disparition de l'exploitant\nDate de fin envisagée de la surveillance : 2004-10-01","Eaux souterraines","N/A","6",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000404201","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","1",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000404901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Chrome | Cuivre | Plomb | Sulfates","Autres éléments minéraux | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000405101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000406001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000406001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Ventilation de la zone non saturée (venting)"]
["SSP000406401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000407201","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000407601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Plomb","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000407901","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2016-09-02 : LA SITUATION RESTE STABLE\nCommentaire : Une conductivité et des teneurs en azote NTK, sulfates et manganèse plus élevées en aval au droit des deux ouvrages PZ1 et PZ2 avec toutefois une atténuation au droit de PZ2.\r\nDes teneurs en DCO, COT, azote ( sous ses différentes formes) chlorures, chrome, nickel, cuivre, zinc, arsenic et fer légèrement supérieures en aval uniquement au droit de PZ1.\r\nCes constats sont relativement identiques  à ceux formulés au terme de la campagne précédente en mai 2016: la tendance est donc stationnaire.\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000408701","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000409401","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...) | Reconditionnement de produits dangereux, Reconditionnement de déchets","N/A","N/A","N/A"]
["SSP000410001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000410101","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000410801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de conception des travaux (PCT)","N/A","Arsenic | Chrome | Mercure","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000411301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de gestion","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000412401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Cyanures libres | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Autres éléments minéraux | Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés)","N/A","N/A","N/A","N/A","N/A"]
["SSP000412501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Phytosanitaires","N/A","N/A","N/A","N/A","N/A"]
["SSP000412701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000413001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000413601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000413901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000414701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A","Arsenic | Baryum | Cadmium | Cuivre | Plomb | Zinc","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000414901","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2017-02-07 : LA SITUATION RESTE STABLE\nCommentaire : stabilisation de la qualité des eaux souterraines en tébuconazole, propiconazole et cyperméthrine en PZ2 à Pz4\r\nchlorophénols, amélioration de la qualité des eaux souterraines (pentachloro proches LQ)\r\npesticides organochlorés, stabilisation de la qualité des eaux souterraines, diminution en dieldrine au droit de Pz4 et apparition béta-endosulfane\n","Eaux souterraines","N/A","1",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000415301","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique","Ventilation de la zone non saturée (venting)"]
["SSP000415401","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Biodégradation dynamisée (ou atténuation naturelle dynamisée)"]
["SSP000415801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Aluminium | Cadmium | Chlorures | Chrome | Nickel | Plomb","Autres éléments minéraux | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000415801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000416601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000416701","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000417901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Nickel | Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000418701","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000419301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000419401","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000419901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | COHV, solvants chlorés, fréons | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000419901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)","Ventilation de la zone non saturée (venting)"]
["SSP000420701","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000420901","Surveillance environnementale","2006-06-12",null,"Résultat de la surveillance à la date du 2006-10-12 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000421702","Surveillance environnementale","2003-12-01",null,"Résultat de la surveillance à la date du 2010-05-12 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000422001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000422301","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000422601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Aluminium","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000422901","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2005-02-23 : LA SITUATION RESTE STABLE\nInformations complémentaires : Surveillance à relancer\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000423801","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Ventilation de la zone non saturée (venting)"]
["SSP000424101","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000424301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000424501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000424801","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000427001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Zinc","HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000427501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cadmium | Chrome | Cuivre | Mercure | Nickel | Plomb | Zinc","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000427601","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000428301","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000428401","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000429002","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cyanures libres","Autres éléments minéraux | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000429301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Interprétation de l''état des milieux (IEM)","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000429701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Interprétation de l''état des milieux (IEM)","N/A","Chrome | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000430601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000431601","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du : 2016-09-20\nRésultat de la surveillance eaux souterraines : 3\nNaphtalène sur PZ3\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000431601","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000432001","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"  ","Eaux souterraines","Diagnostic et Analyse","N/A","Ammonium | Fer | Sulfates","Autres éléments minéraux | Hydrocarbures et indices liés | Metaux et métalloïdes | Paramètres azotés","N/A","N/A","N/A","N/A","N/A"]
["SSP000432201","Surveillance environnementale","2004-03-08",null,"Résultat de la surveillance à la date du 2008-04-15 : LA SITUATION RESTE STABLE\nCommentaire : Non satisfaisant SO4, NO3, NH4, NKJ\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000433901","Surveillance environnementale","2001-11-01",null,"Résultat de la surveillance à la date du 2011-09-22 : LA SITUATION S'AMELIORE\n","Eaux souterraines","N/A","1",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000435501","Surveillance environnementale","1993-01-01",null,"Résultat de la surveillance à la date du 2012-12-24 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000436201","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Ventilation de la zone non saturée (venting)"]
["SSP000439101","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000439101","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Ventilation de la zone non saturée (venting)"]
["SSP000441601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000442001","Surveillance environnementale","2003-05-01","2014-05-06","Résultat de la surveillance à la date du 2012-12-05 : LA SITUATION S'AMELIORE\nInformations complémentaires : teneurs en TCE et PCE légèrement supérieures à la valeur seuil du SDAGE et aux normes de potabilité, mais sans incidence sanitaire au regard de l'absence d'usage des eaux souterraines, qui ne constituent pas une nappe continue exploitable mais des écoulement superficiels temporaires.\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000442201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de gestion","N/A",null,"COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP000442301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000443101","Surveillance environnementale",null,null,"Conformément à la circulaire du 19 septembre 2002, Gaz de France met en place en 2006 un contrôle semestriel des eaux souterraines au droit du site, portant sur les HAP, cyanures, BTEX et phénols. ","Eaux souterraines","N/A","2","Cyanures libres | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Autres éléments minéraux | Autres phénols | Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés)","N/A","N/A","N/A","N/A","N/A"]
["SSP000443801","Surveillance environnementale","1998-01-01","2029-07-01","Résultat de la surveillance à la date du 2014-03-26 : LA SITUATION RESTE STABLE\nCommentaire : La surveillance a été renforcée par arrêté préfectoral du 24/09/2015 (ajout de paramètres)\nDate de fin envisagée de la surveillance : 2019-07-01","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000445101","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Piège hydraulique ou Confinement hydraulique | Ventilation de la zone non saturée (venting)"]
["SSP000445101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Pompage de rabattement ou de récupération","N/A","N/A","N/A"]
["SSP000445701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cuivre | Mercure | Plomb | Zinc","HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000446401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Mercure","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000447101","Surveillance environnementale",null,null,"","Eaux souterraines","N/A","1",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000447501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000448201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000448701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000448901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000449501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cadmium | Chrome","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000449901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A","Cadmium | Cuivre | Plomb | Trichloroéthylène | Zinc","COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000452601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Chrome | Plomb","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000452701","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2003-12-15 : LA SITUATION RESTE STABLE\nCommentaire : pas d'impact sur les eaux souterraines\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000452901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000454201","Surveillance environnementale","2001-03-01",null,"Résultat de la surveillance à la date du 2012-10-30 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000456301","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000457001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Chrome","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000457101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000457201","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","1",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000457701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000457801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000459101","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols","Confinement par couverture et étanchéification"]
["SSP000459601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000459901","Surveillance environnementale",null,null,"","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000460201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," Différentes études ont été menées sur ce site:\n\n- Une première étude a été menée par le CETE Normandie en 1989.\nLes investigations menées lors de cette étude ont permis de mettre en évidence la présence au droit des anciennes gravières de terres noires souillées par des hydrocarbures et sables gris noirs pollués ainsi que de limons silteux huileux à des profondeurs comprises entre 1,7 et 5, 3 m.\nLes résultats d'analyse montre des pollutions aux hydrocarbures allant jusqu'à 173 000 mg/kg et de teneurs en plomb (473mg/kg) et chrome (105 mg/kg)\n\n- A la demande de la DRIRE, la mairie du Grand Quevilly a fait réaliser une ESR en 2000 sur ce site. \n\nLes résultats de l'étape A ont conduit à un classement 2 (site devant faire l'objet d'un suivi) mais avec des incertitudes nécessitant des compléments d'étude qui ont été demandées à la mairie. \n\n- un diagnostic approfondi a été réalisé en 2004 pour le compte de la mairie de Grand-Quevilly.\nCette étude plus complète que les précédentes a été réalisée au vu de 25 sondages carottés et 39 fouilles.\nElle permis d'identifier trois zones de 12000 m2 , 7000 m2 et 6000 m2 polluées par des hydrocarbures et d'une zone de 13000 m2 d'enfouissement de déchets divers (détritus plastifiés, textiles, bidons, ferrailles, pneus, céramiques, verres et adhésifs ...) ainsi que de mâchefers.\nOutre les hydrocarbures dont les concentrations analysées lors de cette campagne sont comparables aux données précédemment identifiées, les éléments traces métalliques ont été analysés et ont permis d'identifier des impacts en arsenic, plomb, cuivre, chrome total, mercure et nickel.\nL'étude identifie également des pollutions de l'air du sol par des hydrocarbures aliphatiques et du chlorure de vinyle.  La méthode d'analyse semi-quantitative ne permet pas de valider l'assertion de l'étude quant à l'innocuité de ces pollutions en termes sanitaires. Par ailleurs nous notons la présence de mercure pouvant être également diffusé dans l'air du sol.\nUne évaluation sanitaire a été réalisée toujours en 2004 selon la méthodologie en usage au moment de l'étude (EDR). Différents scénarios y sont envisagés : zone résidentielle avec espace vert, scénario maison de retraite, scénario roserai, parc Naturel \"Nes Ziona\", jardin public.\nCette évaluation met en exergue la présence trop élevée d'arsenic de plomb et de mercure pour des scénarios de type résidentiel avec espace verts et maison de retraite.\nEn conclusion à cette étude, le rédacteur suggère la mise en place de contraintes d'aménagement:\n- suppression du risque lié au contact direct avec les polluants (traces métalliques) par la mise en place d'une couche de terre végétale d'au moins 30 cm au droit des futures surfaces découvertes ou par la mise en place d'un enrobé ou de bâtiments.\n- gestion des matériaux souillés lors des terrassements (évacuation et enfouissement en centre agréé)\n- limitation de l’aménagement au droit des zones reconnues comme souillées. \n- mise en place de servitudes réglementaires.\n\nCompte tenu des changements réglementaires intervenus en 2007, la Ville de Grand Quevilly a fait réaliser pour les zones devant faire l'objet d'un réaménagement résidentiel :\n- d'un examen critique des études précédentes,\n- d'un diagnostic complémentaire en septembre 2007,\n- d'une analyses des risques résiduels compte tenu des mesures de gestion proposées précédemment et des scénarios envisagés dans les précédentes études,\n- de calculs de concentrations maximales admissibles,\n- d'un bilan coût avantage.\nLes résultats d'analyse ont été comparés aux valeurs d'acceptation des centres de stockage de déchets.\n\nIl ressort des analyses que les échantillons analysés ne sont pas conformes à l'arrêté du 15 mars 2006 qui définit les terres pouvant être admises en décharges pour déchets inertes.\nCompte-tenu des mesures de gestion prévues, les risques ne sont pas acceptables pour la voie inhalation de gaz dans les habitations, pour une teneur résiduelle en benzène de 0,15 mg/kg dans les sols. Le rédacteur précise que les teneurs résiduelles sur le site devront être inférieures à cette valeur, ce qui implique de traiter la zone z3.\n\nLes remarques non exhaustives sur cette étude sont présentées ci-après :\n- La démarche n'est pas conforme aux dispositions des dispositions présentées par les textes de 2007;\n- Les prélèvements (dans des tranchées notamment) ne garantissent pas la validité des mesures de l'air du sol;\n- Les études se sont concentrées principalement sur l'emplacement des anciennes gravières. le nombre de tranchées et sondages est faible compte tenu de la surface de la zone;\n- Les règles de cumul des effets des différents polluants ne sont pas respectés;\n- L'impact sur la nappe a été insuffisamment étudié.\n\nLes analyses de fond de fouille et de bord de fouille, après travaux n'ont pas été réalisées ou communiquées, nous ne connaissons pas l'impact résiduel pour ce site. Aucun rapport de fin de travaux n'a été produit ou communiqué.\nDans ces conditions nous ne pouvons pas valider la démarche.\n\nLes études n'étant pas conformes à la norme et n'ayant pas entrainé la prise de servitudes d'utilité publiques comme proposé, il convient d'inscrire se site en secteur d'information sur les sols. Cette disposition, prise à titre conservatoire, permettra de garantir le maintien des informations sur ce site dans le plan local d'urbanisme et le maintien des mesures de gestion prises sur le site.","Sol - Sous-sol","Plan de gestion","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000460701","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000460801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000461301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000461701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés","N/A","N/A","N/A","N/A","N/A"]
["SSP000462701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Trichloroéthylène","Benzène et dérivés | COHV, solvants chlorés, fréons | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000463201","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000463301","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000464301","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000465001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000465501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A","Arsenic | Cadmium | Chrome | Cuivre | Nickel | Plomb | Zinc","Hydrocarbures et indices liés | Metaux et métalloïdes | Phytosanitaires","N/A","N/A","N/A","N/A","N/A"]
["SSP000465701","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000466201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000466701","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2009-01-21 : LA SITUATION SE DEGRADE\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000469001","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000469601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000470101","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000472701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000474001","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000474101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Chrome | Cyanures libres","Autres éléments minéraux | COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000474201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000478101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000482401","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000483401","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Pompage de rabattement ou de récupération","N/A","N/A","N/A"]
["SSP000483801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"COHV, solvants chlorés, fréons | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000484101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000484201","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols","Ventilation de la zone non saturée (venting)"]
["SSP000485001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...) | Reconditionnement de produits dangereux, Reconditionnement de déchets","N/A","N/A","N/A"]
["SSP000485101","Surveillance environnementale",null,null,"Commentaire : Absence d’impacts sur le milieu eaux superficielle.\r\nRéduction des teneur en polluant dans les eaux souterraines.\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000485501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000485901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000486901","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000488101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000488401","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000488701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Cyanures libres | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Autres éléments minéraux | Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000490001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique","Ventilation de la zone non saturée (venting)"]
["SSP000490101","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000492901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000493701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP000493901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000494801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"COHV, solvants chlorés, fréons | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000494901","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000495001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000502501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000505101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage","N/A","N/A","N/A"]
["SSP000505701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000507001","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique","Ventilation de la zone non saturée (venting)"]
["SSP000507701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Analyse des enjeux sanitaires (EQRS, ARR)","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000508801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," /","Eaux souterraines","Diagnostic et Analyse","N/A",null,"HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000509001","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2019-09-04 : LA SITUATION RESTE STABLE\nCommentaire : Lors de la campagne du 04/09/2019, le piézomètre Pz2bis, la somme des concentrations des 6 HAP(3.56µg/l) est supérieure à la valeur de réf ( 1µg/L).Concernant les ouvrages Pz3ter et Pz4 en position aval, les HAP sont quantifiés avec des concentrations globalement supérieures aux limites de quantification mais aucun dépassement de la valeur de réf pour la somme des 6 HAP n'est observé.Sur Pz1bis en position amont et Pz5 en position aval, les concentratiosn en HAP sont globalement inférieures ou proches des limites de quantification et aucun dépassement de la valeur n'est observé\nInformations complémentaires : L'examen des campagne de mesure de 2001 à sept 2019 révèle que :\r\n- s'agissant des HAP 3 piézomètres, l'un central, l'autre en amont latéral et l'autre en aval, sont les plus impactés par les HAP (teneurs de 1 à 250 µg/l) qui dépassent couramment les valeurs de référence (1 µg/l) concernant la somme des 6 HAP,\r\n- s'agissant des HCT le dernier dépassement de la valeur de référence date d'octobre 2010 en amont latéral (PZ3ter) ; depuis les teneurs ont progressivement baissé dans cet ouvrage et sont, depuis mars 2014, inférieures au seuil de quantification sur l'ensemble du réseau piézométrique.\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000509201","Exécution des travaux de réhabilitation",null,null,"/","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000509601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," /","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Cadmium | Chrome | Cuivre | Mercure | Nickel | Plomb | Zinc","HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000509901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," /","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000510401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000511101","Surveillance environnementale","2002-10-01",null,"Résultat de la surveillance à la date du 2019-04-26 : LA SITUATION S'AMELIORE\nCommentaire : Confirmation de la répartition de la pollution de la nappe sur site et de l'extension hors site. Diminution des concentrations en latéral.\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000511501","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"Diagnostic","Eaux souterraines","Diagnostic et Analyse","N/A","Arsenic | Cuivre | Mercure | Plomb","COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000514501","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000515801","Surveillance environnementale","2002-06-06",null,"Résultat de la surveillance à la date du 2013-11-18 : LA SITUATION RESTE STABLE\nInformations complémentaires : Un dépassement a été révélé sur un piézomètre (PZI) la somme du tétrachloroéthylène et du trichloroéthylène.\r\n\r\nLa présence de solvants chlorés est toujours observée en amont.\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000516401","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000517501","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000517801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Cadmium | Chrome | Cuivre | Nickel","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000518601","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000519001","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000520201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Cyanures libres | Plomb","Autres éléments minéraux | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000520301","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique","Confinement par couverture et étanchéification"]
["SSP000521301","Exécution des travaux de réhabilitation",null,null,"  /","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000521901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Mercure | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000532201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," Le plan de gestion environnemental fait suite aux investigations du milieu souterrain menées entre 2010 et 2016.","Sol - Sous-sol","Plan de gestion","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000532201","Exécution des travaux de réhabilitation",null,null," Les différentes études menées ont mis en évidence :\n\t Pour les sols :\n\t\t- un impact en hydrocarbures C5-C40 au droit des cuves TK08 et TK12 localisées au Nord-\t\tOuest du site et en bordure Ouest du sarcophage principal, avec une teneur maximale de 2700 mg/kg mesurée entre 1 et 5 m ;\n\t\t- un impact en hydrocarbures C5-C40 entre 0 et 3 m et entre 5,9 et 6 m au droit du sarcophage principal (parc à cuves semi-enterrées), de l’aire de chargement, de la station de pompage et du séparateur d’hydrocarbures, localisés au centre du site d’étude avec des teneurs maximales mesurées respectivement à 4 920 mg/kg et 9 670 mg/kg ;\n\t\t- un impact en hydrocarbures C5-C40 entre 1 et 2 m puis vers 6m au droit des canalisations enterrées et du sarcophage secondaire, situés à l’Est et au Nord-Est du site respectivement. La teneur maximale mesurée est de 7 225 mg/kg MS.\n\tPour les eaux souterraines : \n\t\t- un impact dissous en hydrocarbures C5-C40 associé à la présence de flottant a été mis en évidence au droit du site. ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...) | Pompage de rabattement ou de récupération","N/A","N/A","N/A"]
["SSP000535801","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique","Ventilation de la zone non saturée (venting)"]
["SSP000536001","Etude SSP et ingénierie des travaux de réhabilitation","2011-10-18","2012-08-20","Par courrier du 12 septembre 2011, le mandataire chargé de la liquidation a transmis le bilan environnemental ainsi que le rapport de mise en sécurité du site.",null,"Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000539501","Exécution des travaux de réhabilitation","2006-06-01",null," Après étude du plan d'action proposé par l'exploitant en juin 2006, l'inspection des installations classés lui a demandé des éléments complémentaires sur les objectifs de dépollution retenus et les travaux enagés. Il lui a également été demandé de proposer les éventuelles restrictions d'usage à mettre en oeuvre sur le site ainsi qu'un programme de surveillance de la qualité des eaux souterraines.","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution"]
["SSP000540701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000541301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000541601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Chlorures | Chrome | Fer | Zinc","Autres éléments minéraux | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000543101","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000543101","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000545101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000546101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," AP du 3 mars 2003\ndiagnostic du 24 octobre 2011 ","Eaux souterraines","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | COHV, solvants chlorés, fréons | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000547201","Exécution des travaux de réhabilitation",null,null,"terres polluées excavées","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Lavage à l'eau"]
["SSP000549201","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000549901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cadmium | Chrome | Cuivre | Mercure | Nickel | Plomb | Zinc","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000549901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000551601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Arsenic | Chrome | Sulfates","Autres éléments minéraux | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000551601","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000552101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cyanures libres | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Autres éléments minéraux | Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés)","N/A","N/A","N/A","N/A","N/A"]
["SSP000552401","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000553201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000555501","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Piège hydraulique ou Confinement hydraulique | Ventilation de la zone non saturée (venting)"]
["SSP000557601","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000558701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Nickel | Plomb","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000559701","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","1",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000559801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," /","Sol - Sous-sol","Plan de gestion","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000560101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000561201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Ammonium | Cyanures libres | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Autres éléments minéraux | Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Paramètres azotés","N/A","N/A","N/A","N/A","N/A"]
["SSP000562101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000563601","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000565201","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique","Biodégradation dynamisée (ou atténuation naturelle dynamisée) | Confinement par couverture et étanchéification"]
["SSP000565501","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols","Confinement par couverture et étanchéification"]
["SSP000566601","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2015-06-30 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000566601","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000566801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000567101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...) | Pompage de rabattement ou de récupération","N/A","N/A","N/A"]
["SSP000567501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000568001","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000568301","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000568601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000569501","Exécution des travaux de réhabilitation",null,null,"L'analyse des eaux de la nappe a mis en évidence l'absence dans les eaux souterraines de sous-produits issus de l'activité gazière.Cependant, la qualité des eaux souterraines fait l'objet d'analyses semestrielles  conformément aux exigences de l'arrêté précité.","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000569601","Surveillance environnementale",null,null,"","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000570601","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification | Ventilation de la zone non saturée (venting)"]
["SSP000570801","Surveillance environnementale","2004-04-26","2009-09-01","Résultat de la surveillance à la date du 2004-04-26 : LA SITUATION S'AMELIORE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000571401","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000573201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000578301","Exécution des travaux de réhabilitation",null,null," Collecte et traitement des lixiviats et du biogaz.","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000579901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000586801","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000586801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000587701","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000587801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000588701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000590301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000596301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000596802","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000596805","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000597101","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2011-03-01 : LA SITUATION S'AMELIORE\nCommentaire : surveillance par arrêté préfec du 7 avril 2010\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000597501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000597801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000598401","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000598801","Etude SSP et ingénierie des travaux de réhabilitation","1998-06-15",null,"Conformément aux engagements du protocole, ce site a fait l'objet d'un diagnostic initial dont les principaux objectifs sont, outre les recherches historiques et documentaires, la recherche des ouvrages enterrés, l'évaluation de l'impact du site sur les ressources locales en eaux (eaux souterraines et superficielles) et la caractérisation du sol superficiel pour évaluer les risques de contact direct et ceux liés à d'éventuelles émanations gazeuses.",null,"Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000605101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage","N/A","N/A","N/A"]
["SSP000610701","Surveillance environnementale","1999-07-12","2013-09-20","Dans les résultats des dernières campagnes (2014/2016) et sur l'ensemble des trois ouvrages contrôlés, certaines teneurs avaient diminués en 2014 et 2015 (HCT/BTEX/COHV) mais on retrouve certaines de ces teneurs (parfois en hausse), principalement les concentrations en Toluène, xylène, benzène trouvés au PZ3, qui étaient inférieures aux valeur de l'OMS depuis 2013, et qui sont en hausse.\nLes teneurs en Naphtalène au PZ3 qui étaient en baisse constante restent stables. Les teneurs en Phénol sont en diminution depuis la campagne de 2013/2014. Les concentrations en COHV pour les ouvrages PZ1; PZ2 et PZ3 sont inférieures à la limite de quantification. En conclusion, la surveillance doit être maintenue.\n",null,"N/A","1",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000614401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Arsenic | Nickel | Plomb | Trichloroéthylène | Zinc","COHV, solvants chlorés, fréons | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000616601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," .","Sol - Sous-sol","Diagnostic et Analyse","N/A","Mercure | Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Trichloroéthylène","Benzène et dérivés | COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000616801","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000618001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Ammonium | Cuivre | Mercure | Sélénium | Zinc","Hydrocarbures et indices liés | Metaux et métalloïdes | Paramètres azotés","N/A","N/A","N/A","N/A","N/A"]
["SSP000625101","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du : 2008-10-10\nRésultat de la surveillance eaux souterraines : 1\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000626301","Exécution des travaux de réhabilitation","2003-03-02","2003-02-03"," - décapage de toute la surface du site (sur une épaisseur de 20 cm) pour éliminer tous les déchets métalliques et autres laissés sur place,\n- élimination de ces terres dans deux centres agréés (1860 t de terre de classe 2 ont été évacuées au CET de FOUJU MOISENAY 77 et 431 t de terre de classe 1 ont été évacués au CET de GUITRANCOURT 78).\n- remise en état et en service du réseau de piézomètres existant (6 appareils),\n- les eaux stagnantes ont été analysées, pompées et vidées,\n- pendant une durée de 3 ans et chaque trimestre, dans chacun des 6 piézomètres, sera prélévé un échantillon représentatif d'eau par un laboratoire agréé. Les résultats de ces mesures seront adressés à l'inspection des installations classées.","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000632101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A",null,"Hydrocarbures et indices liés | Phytosanitaires","N/A","N/A","N/A","N/A","N/A"]
["SSP000634801","Etude SSP et ingénierie des travaux de réhabilitation","2003-12-11",null,"L'arrêté préfectoral n°03 DAI 2IC 356 du 11 décembre 2003 impose à l'exploitant de réaliser un diagnostic approfondi (dans un délai de 9 mois) et une étude détaillée des risques (dans un délai d'un an). Cet arrêté impose également:\n- la clôture du site,\n- les conditions de gardiennage,\n- les précautions à prendre lors des opérations d'investigations et en cas de travaux et d'excavations de terre au droit du site.\n\nCes documents ont été remis fin 2004 puis complétés en 2005 et 2006, notamment par une proposition de travaux de réhabilitation en vue de permettre une réutilisation du site pour un usage résidentiel.\n","Eaux souterraines","Diagnostic et Analyse","N/A","Aluminium | Trichloroéthylène","COHV, solvants chlorés, fréons | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000635001","Etude SSP et ingénierie des travaux de réhabilitation","2003-05-06",null,"Suite à la fermeture du site, M le Préfet de Seine-et-Marne a imposé, par arrêté préfectoral du 6 mai 2003, au liquidateur de la société MUELLER EUROPE, la réalisation d'un diagnostic initial et d'une étude simplifiée des risques (ESR). Ceux-ci ont été déposés le 24 décembre 2003.\nL’ESR conclut au classement du site en classe 1 : site nécessitant des investigations approfondies (diagnostic approfondi et évaluation détaillée des risques).",null,"Analyse des enjeux sanitaires (EQRS, ARR)","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000638301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000638401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000641001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cuivre | Mercure | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000641201","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols","Ventilation de la zone non saturée (venting)"]
["SSP000641901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000642401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de gestion","N/A","Trichloroéthylène","COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP000642801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000643301","Surveillance environnementale","2007-06-14",null,"Le réseau de surveillance est composé de 8 piézomètres, dans lesquels sont prélevés deux fois par an, des échantillons à des fins d’analyses.\nLes paramètres analysés sont les suivants :\n* dans les échantillons prélevés dans les ouvrages PTII, PZA, PZ3, PZ4, PZ5 et PZ2\n- les matières en suspension (MES),\n- la demande biochimique en oxygène (DBO),\n- la demande chimique en oxygène (DCO),\n- les agents de surface anioniques et non anioniques ;\n* dans les échantillons prélevés dans les ouvrages NPZ2 et NPZ9 : les hydrocarbures totaux.\n",null,"N/A","1",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000643701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000644201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...) | Pompage de rabattement ou de récupération","N/A","N/A","N/A"]
["SSP000644401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000644601","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000645201","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000646901","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000647101","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000650801","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000651401","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000652901","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"Sont situés sur la zone de l'ancienne décharge :\n- Un ensemble de 4 logements au nord-est du site ;\n- Une zone de stationnement au centre ;\n- Une aire de jeu avec espaces verts au sud-ouest ;\n- Un local associatif au sud-ouest \n- Un ruisseau en bordure du site, au sud. ",null,"Etude macro","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000652901","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"En 2020, des sondages du sol ainsi que des prélèvements en eaux souterraines et superficielles ont été réalisés. \nLes investigations du sol ont permis de mettre en évidence des impacts en cuivre, zinc, arsenic, plomb, mercure, cadmium, PCB, HAP, naphtalène et hydrocarbures.\nLes résultats d'analyses des eaux superficielles et souterraines n'ont détecté que des teneurs négligeables. ",null,"Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000657901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000658201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de conception des travaux (PCT)","N/A","Cadmium | Cuivre | Nickel | Plomb | Zinc","HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000658701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000659001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000660501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000660701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," /","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000689501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cyanures libres | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Autres éléments minéraux | Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000690001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000694301","Exécution des travaux de réhabilitation",null,null," /",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000695401","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2011-04-27 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","1",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000695901","Surveillance environnementale",null,null,"Informations complémentaires : Campagnes 2007/2008 : dépassement en 2007 des valeurs limites de qualité des eaux destinées à la consommation humaine pour les paramètres chrome, benzopyrène et tétrachloroéthylène.\r\nCampagne 2009 : concentrations relevées inférieures aux valeurs limites susvisées pour l'ensemble des paramètres, chrome non détecté, teneurs en baisse pour les paramètres HAP et métaux.\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000696501","Surveillance environnementale",null,null,"Résultat de la surveillance eaux souterraines : 1\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000696901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000697101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000697301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000697901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000698401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés | Phytosanitaires","N/A","N/A","N/A","N/A","N/A"]
["SSP000698801","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000699701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000700201","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000700401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de gestion","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000700801","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000701101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," /","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Chrome | Cuivre | Nickel | Plomb","HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000701901","Surveillance environnementale","2004-06-29",null,"Résultat de la surveillance à la date du 2013-11-25 : LA SITUATION RESTE STABLE\nCommentaire : Résultats conformes à l'arrêté.\nInformations complémentaires : Le plomb mesuré reste en deçà des seuils d'alerte, les éléments Cuivre et Zinc apparaissent prédominants et dans des quantités relativement stables.\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000702501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Arsenic | Chlorures | Zinc","Autres éléments minéraux | Metaux et métalloïdes | Phytosanitaires","N/A","N/A","N/A","N/A","N/A"]
["SSP000703001","Surveillance environnementale","2003-12-01","2014-07-29","Résultat de la surveillance à la date du 2014-07-29 : LA SITUATION RESTE STABLE\nCommentaire : Sur la dernière campagne de juillet 2014 pour l'ensemble des substances recherchées sur les piézomètres du site, les teneurs sont faibles voire inférieures au seuils de quantification analytique du laboratoire, à l’exception de :\r\n- en amont hydraulique (Pz2), en Benzo(a)pyrène (0.22 µg/l), en HAP (0.46 µg/l) et en plomb (69  µg/l),\r\n- en latéral hydraulique (Pz1bis), en benzo(a)pyrène (0.02 µg/l).\r\n\r\nRemarque : Compte-tenu du positionnement des piézomètres Pz1 et Pz2 en limite amont hydraulique du site, de la proximité des travaux et du caractère singulier du dépassement observé en HAP (après 15 campagnes sans mise en évidence de teneurs notables en HAP), il est vraisemblable que cet impact ponctuel puisse être lié aux opérations conduites sur le site voisin.\nInformations complémentaires : L'exploitant a transmis les derniers résultats de l'auto-surveillance des eaux souterraines sur la période allant d'avril 2009 à juillet 2014. Ces résultats sont globalement stables sur l'ensemble de la période étudié à raison d'une fréquence d'analyse semestrielle sur les paramètres suivants : pH ; HC ( C5-C10) ; HC (C10-C40) ; hydrocarbures totaux ; arsenic ; plomb ; cadmium ; chrome ; cuivre ; nickel ; mercure ; zinc ; chlorobenzène ; chlorure de vinyle ; dichlorométhane ; 1,2 - dochlorométhane ; cis-1,2-dichloroéthylène ; trans-1,2-dichloroéthylène ; trichloroéthylène ; tétrachloroéthylène ; benzène ; toluène ; éthylbenzène ; xylènes ; styrène ; fluoranthène ; benzo(b)fluoranthène ; benzo(k)fluoranthène ; benzo(a)pyrène indéno(1,2,3-c,d)pyrène ; benzo(g,h,i)pérylène ; HAP(4) et HAP(6).\nDate de fin envisagée de la surveillance : 2014-07-29","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000703501","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000706401","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2007-04-02 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000711301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Arsenic | Cadmium | Chrome | Cuivre | Mercure | Nickel | Plomb | Sélénium | Zinc","COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000712001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000713201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cuivre | Mercure | Plomb | Zinc","HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000713301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000713601","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000713901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000715501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000715801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000716901","Etude SSP et ingénierie des travaux de réhabilitation","2019-01-01","2019-01-01"," Gestion","Eaux souterraines","Plan de gestion","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000728801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Arsenic | Nickel | Plomb | Zinc","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000731901","Exécution des travaux de réhabilitation",null,null," En mars 2018 l'ADEME a achevé :\n    • les travaux d'excavation et remplacement localisé de terres polluées ;\n    • les investigations sur les eaux souterraines. Elles montrent des pollutions dues aux cyanures ponctuelles et localisées sur quelques parcelles de l'ancienne emprise de l'usine à gaz qui ne traduisent pas un transfert des contaminants sous forme d'une extension de panache de pollution en aval hydrogéologique. Cette pollution conduit l’ADEME à proposer une restriction d’usage des eaux souterraines pour les parcelles concernées (919, 920, 921, 922, 923, 924, 925 et 926). Elle porte sur la non utilisation des eaux souterraines pour des usages sensibles à savoir alimentaire (boisson, préparation des aliments…), d’hygiène corporelle et les usages connexes (arrosage du jardin potager, remplissage des piscines…).\n\nPar ailleurs, en ce qui concerne la parcelle 1221, au vu de l’absence d’une déclaration formelle de cessation d’activité, l’arrêté préfectoral du 22 août 2016 a été pris pour imposer à ENGIE la remise en état du site. Cet arrêté liste les actions devant être engagées pour rendre compatible l’état du site avec un usage industriel. Le 26 juin 2017, ENGIE a adressé à la préfecture d'Eure-et-Loir le rapport de fin de travaux visant à la réhabilitation et la mise en sécurité de cette parcelle pour un usage industriel.",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000734501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000740601","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"étude de sols et de la nappe","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000742001","Exécution des travaux de réhabilitation",null,null," Dépollution","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Oxydation chimique"]
["SSP000742101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000742501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP000742601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000743001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Mercure","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000743701","Surveillance environnementale","2003-09-24",null,"Résultat de la surveillance à la date du 2007-10-09 : LA SITUATION SE DEGRADE\nCommentaire : Non satisfaisant HCTX PZ4\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000744101","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2007-01-16 : LA SITUATION RESTE STABLE\nCommentaire : satisfaisant\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000744501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Aluminium | Cadmium | Chrome | Nickel | Plomb","COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000744801","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000745901","Exécution des travaux de réhabilitation",null,null,"Confinement","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000746801","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000747001","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Ventilation de la zone non saturée (venting)"]
["SSP000747401","Surveillance environnementale","2001-03-01",null,"Résultat de la surveillance à la date du 2018-04-03 : LA SITUATION RESTE STABLE\nCommentaire : Les résultats ont permis:\r\n- de confirmer le maintien d'un impact en Ni au droit des ouvrages PZ1 et PZ2 (avec des teneurs respectives de 125 et 58.2 ug/L pour une valeur seuil de 20 ug/L);\r\n- de confirmer la réapparition de teneurs anomaliques en Cd au droit de l'ouvrage PZ1 (13.5 ug/L avec une valeur seuil fixée à 5 ug/L) mis en évidence en octobre 2017.\nInformations complémentaires : Depuis 2014 présence de Cd en PZ1, origine, dalle fissurée.\r\nEn 2015, la situation se dégrade par rapport à 2005. Sens d'écoulement de la nappe variable, persistance des Cd, Ni et Zn sur PZ1 (supérieurs à la limite de qualité eau potable) et  Ni sur PZ2 (supérieur à la limite de qualité eau potable).\r\nLes résultats des campagnes de 2016 et de mars 2017 ont permis:\r\n- d'identifier le maintien d'un impact en Ni (PZ1 et PZ2);\r\n- de noter la disparition d'un impact en Cd au droit du PZ1\r\nLes campagnes d'octobre 2017 et d'avril 2018 ont confirmé le maintien de l'impact en Ni au droit des PZ1 et PZ2. Cependant, un impact en Cd a de nouveau été mis en évidence au droit du PZ1, ce qui n'avait plus été le cas depuis les campagnes de 2015.\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000747601","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000748801","Surveillance environnementale","1993-09-19",null,"Résultat de la surveillance à la date du 2015-10-29 : LA SITUATION RESTE STABLE\nCommentaire : Pas de pollution significative sur les piézomètres. Forte baisse des teneurs en métaux sur PZ2.\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000749101","Surveillance environnementale","2001-11-28",null,"Résultat de la surveillance à la date du 2014-07-30 : LA SITUATION RESTE STABLE\nCommentaire : Globalement, les teneurs observées s/les piézomètres situés à l'aval hydraulique (PZ8, PZ9) sont stables par rapport à la campagne précédente d'octobre 2013, excepté pour le naphtalène qui présente une hausse s/le piézomètre PZ8.\nInformations complémentaires : Dernière campagne de juillet : les analyses indiquent toujours la présence de plusieurs HAP s/les piézomètres PZ8 et PZ9. En outre, impacts relevés dans PZ8 pour les composés suivants : naphtalène, acénaphtylène, acénaphtène, fluorène, phénanthrène, anthracène, pyrène et fluoranthène ; impacts relevés également dans PZ9 correspondant aux composés suivants : naphtalène, acénaphtylène, acénapthène, fluorène, phénantrène et anthracène. Globalement, les teneurs observées s/les piézomètres situés à l'aval hydraulique (PZ8, PZ9) sont stables par rapport à la campagne précédente d'octobre 2013, excepté pour le naphtalène qui présente une hausse s/le piézomètre PZ8 (teneurs proches de celles de 2012). Par rapport au sens d'écoulement des eaux souterraines, aucune transfert ne s'effectue entre ces 2 ouvrages.\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000749801","Surveillance environnementale","2002-02-21",null,"Résultat de la surveillance à la date du 2014-12-01 : LA SITUATION RESTE STABLE\nCommentaire : Augmentation du Bore dans le Pz5 (199 ug/l) (74 ug/l) et présence de chlorophénols s/Pz5 (3,4 ug/l).\nInformations complémentaires : La campagne du 10 mars 2009 dans 3 puits (dont 2 aval) ne montre pas d'impact par les produits utilisés, ancien (PCP) et actuels (cuivre - acide borique).\r\n\r\nLa Campagne du 26/10/2009 \"basses eaux\" sur phénol, chloro-phénols (dont PCP), cuivre, bore, montre que :\r\n. seuls le bore (570 µg/l) et le cuivre (14 µg/l) sont détectés en Pz8 (inférieure à la valeur de référence \"eau potable \" : 1000 µg/l),\r\n. la présence de bore à l'aval des installations montre un impact des activités de l'établissement LABAT MERLE,\r\n. l'origine en serait le tas de déchet ancien, dit \"tas de retroussement. Cette affirmation nous paraît douteuse car ce tas est censé avoir été réhabilité, et car l'acide borique est une substance toujours utilisée par l'établissement LABAT MERLE pour le traitement des bois,\r\n. une attention doit cependant être apportée pour ne pas affecter la qualité de la nappe au droit des puits localisés en aval hydraulique et identifiés en 2003.\r\n\r\nLa campagne de mars 2010 montre que le phénol et les chlorophénols ne sont détectés ni à l'amont ni à l'aval hydraulique du site.\r\nLe cuivre n'est pas détecté au droit des ouvrages de suivi (concentrations inférieures à la limite de quantification du laboratoire)\r\nle bore est détecté au droit des ouvrages de suivi à des teneurs inférieurs aux valeurs guides ou réglementaires définies pour un usage eau potable. Par ailleurs, les teneurs mesurées pour les hautes eaux 2010 en amont et en aval du site demeurent du même ordre de grandeur.\r\n\r\nLa campagne de surveillance et d'analyses des eaux souterraines du 18 avril 2013, menée en période de hautes eaux, conduit aux constats suivants :\r\n. l'absence de dégradation de la qualité des eaux souterraines par le cuivre et le bore au droit du site ;\r\n. un impact du site sur la qualité des eaux souterraines par les chlorophénols. Ainsi, parmi les phénols et chlorophénols recherchés, seuls le pentachlorophénol, le 2,4 & 2,5 Dichlorophénol et le 2,3,4,6-tetrachlorophénol ont été mesurés à des teneurs dépassant les limites de quantification du laboratoire en Pz5.\r\nLe pentachlorophénol est mesuré à une teneur légèrement supérieure à la valeur de référence définie pour les eaux destinées à la consommation humaine par l'OMS. Le pentachlorophénol n'étant plus utilisé sur le site, cet impact ne peut être lié à un évènement récent lors de l'activité de LABAT MERLE.\r\nLes teneurs mesurées en amont en Bore, à l'état de traces, demeurent du même ordre de grandeur que lors des précédentes campagnes.\r\n\r\nLa campagne d'analyses menée le 20/03/2014, en période de hautes eaux, conduit aux constats suivants :\r\n- absence de dégradation de la qualité des eaux souterraines par le cuivre et le bore au droit du site ;\r\n- impact du site s/la qualité des aux souterraines par les chlorophénols ; le pentachlorophénol et le 2,3,4,6-tetrachlorophénol ont été mesurés à des teneurs significatives en Pz5.\r\nConclusions du rapport BURGEAP : le pentachlorophénol est mesuré à une teneur 8 fois supérieure à la valeur de référence définie pour les eaux destinées à la consommation humaine. Le pentachlorophénol n'étant plus utilisé s/le site depuis plusieurs années, cet impact ne peut être lié à un évènement récent lors de l'activité de LABAT MERLE. A noter que la teneur en pentachlorophénol est en nette augmentation (près de 5 fois supérieure) depuis la campagne précédente, et que cette variation pourrait s'expliquer par le niveau des eaux souterraines particulièrement haut en ce début d'année 2014.\r\n\r\nCampagne d'analyses du 24/10/2014 (période de basses eaux) :\r\n. présence, s/Pz5 (aval), de cuivre à l'état de traces (0,75 ug/l) et de bore à des concentrations plus importantes (199 ug/l) ;\r\n. impact du site s/la qualité des eaux souterraines par des chlorophénols : seuls le pentachlorophénol (3,4 ug/l) et le 2,3,4,6-Tetrachlorophénol (4,3 ug/l) ont été détectés au droit du Pz5 (point aval) ; les concentrations mesurées sont relativement faibles.\r\nConclusion de BURGEAP : Aucun impact significatif par les composés recherchés n'est donc identifié.\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000749801","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000750201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000750401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000750801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000751001","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","1",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000751701","Surveillance environnementale","2000-05-15",null,"Résultat de la surveillance à la date du 2011-07-22 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000751801","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2012-10-29 : LA SITUATION S'AMELIORE\nCommentaire : Hormis une valeur anormalement haute en PCB en 2012\n","Eaux souterraines","N/A","1",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000752201","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000752401","Surveillance environnementale","2008-03-03",null,"Résultat de la surveillance à la date du 2013-07-03 : LA SITUATION SE DEGRADE\nCommentaire : pour les eaux souterraines : non satisfaisant en DCO (PZ1), en aluminium (PZ1 et PZ2), en arsenic (PZ1), en manganèse (PZ1) et plomb (PZ1). pour les eaux superficielles : satisfaisant\nInformations complémentaires : La campagne de mars 2012 donne les résultats suivants :\r\n- pH : 8.37 au droit de P1 et 8.32 au droit de P2;\r\n- Conductivité : 514 microS/cm au droit de P1 et 474 microS/cm au droit de P2;\r\n- DCO : <30 mg/l en O2 au droit de P1 et P2;\r\n- indice HCT : <0.03 mg/l au droit de P1 et P2;\r\n- indice phénol : <0.01 mg/l au droit de P1 et P2;\r\n- aluminium : 0.10 mg/l au droit de P1 et 0.09 mg/l au droit de P2;\r\n- arsenic : <0.005 mg/l au droit de P1 et P2;\r\n- cadmium : <0.005 mg/l au droit de P1 et P2;\r\n- chrome : <0.005 mg/l au droit de P1 et P2;\r\n- manganèse : <0.005 mg/l au droit de P1 et P2;\r\n- molybdène : <0.005 mg/l au droit de P1 et P2;\r\n- nickel : <0.005 mg/l au droit de P1 et P2;\r\n- plomb : <0.005 mg/l au droit de P1 et P2.\r\n\r\nLa campagne de juin 2013 donne les résultats suivants (P1 étant inaccessible, seul P2 a été analysé):\r\n- DCO : <30 mg/l en O2 au droit de P2;\r\n- indice HCT : 0.05 mg/l au droit de P2;\r\n- indice phénol : <0.01 mg/l au droit de P2;\r\n- aluminium : <0.005 mg/l au droit de P2;\r\n- arsenic : <0.005 mg/l au droit de P2;\r\n- cadmium : <0.005 mg/l au droit de P2;\r\n- chrome : <0.005 mg/l au droit de P2;\r\n- manganèse : 0.031 mg/l au droit de P2;\r\n- molybdène : <0.005 mg/l au droit de P2;\r\n- nickel : <0.005 mg/l au droit de P2;\r\n- plomb : <0.03 mg/l au droit de P2.\r\n\r\nPour cette campagne de juin 2013, des teneurs normales ont été retrouvées au droit de PZ1 pour la DCO, l'aluminium, l'arsenic, le plomb et le manganèse. PZ2 présente une teneur au dessus du seuil défini pour les eaux potables par l'arrêté du 11 janvier 2007 pour l'aluminium. De même, PZ3 montre des teneurs supérieures aux seuils définis par l'arrêté décrit précédemment pour la DCO et le manganèse.\r\nL'ensemble des autres paramètres est soit inférieur aux seuils de comparaison pris pour référence, soit inférieur aux seuils de quantification analytique du laboratoire.\r\n\r\nPour les eaux superficielles, seul le point en aval a pu être prélevé du fait de l'inaccessibilité du point situé en amont. Les eaux superficielles prélevées au point aval du ruisseau Coustalou lors des campagnes 2011, 2012 et 2013 ne mettent en évidence aucune anomalie particulière. En effet, aucun paramètre ne dépasse les seuils définis pour les eaux potables potabilisables par l'arrêté du 11 janvier 2007. Cependant, des hydrocarbures et du manganèse sont détectés.\r\n\r\nAu regard de ces résultats, nous préconisons de poursuivre le suivi semestriel de la qualité des eaux souterraines au droit des 3 piézomètres et des eaux superficielles en amont et en aval de la décharge sur la base de 2 campagnes de prélèvements par an afin de:\r\n- surveiller l'évolution des teneurs anormalement élevées pour la DCO, l'aluminium, l'arsenic, le manganèse et le plomb au droit de PZ1, l'aluminium pour PZ2 ainsi que la DCO et le manganèse pour PZ3;\r\n- confirmer l'absence d'impact sur les eaux du Coustalou.\r\n\r\nLa présente campagne de prélèvement étant la dernière prévue, il est recommandé, conformément à l'arrêté préfectoral n°2008-63-4 du 3 mars 2008, de réaliser des bilan quadriennal.\r\n\r\nIl est reconduit également la recommandation préconisée dans les derniers rapports à savoir, que conformément à l'arrêté préfectoral du 3 mars 2008, le même programme analytique doit être réalisé sur les deux émergences identifiées lors de l'étude préalable à proximité immédiate et à l'aval hydraulique (au pied du mur de soutènement de l'ancienne voie ferrée) de la décharge.\r\n\r\nLa campagne du 03/06/2013 :\r\n- sens d'écoulement de la nappe confirme Nord-ESt,\r\n- pas d'indice organoleptique de contamination, pas de surnageant, pas d'odeur,\r\n- par référence aux eaux potables :\r\n- Pz1 impacté par DCO, Al, As Mn et Pb,\r\n- Pz2 impacté par Al,\r\nPas d'impact dans le Coustalou (traces HCTX et Mn),\r\nPz3 impacté en DCO et Mn\n","Eaux souterraines","N/A","1",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000752701","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000753301","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2011-07-03 : LA SITUATION SE DEGRADE\nInformations complémentaires : La surveillance des eaux souterraines prescrite par l'arrêté préfectoral du 05/10/1999 est maintenue et réalisée, les résultats sont régulièrement transmis. \r\n\r\nDepuis 2010, les résultats font apparaître un dépassement de la valeur de référence réglementaire eaux brutes  pour les hydrocarbures  avec des teneurs en augmentation sur PZ17 (situé en aval hydraulique) ainsi que la présence de flottant dont l'épaisseur augmente. \r\n\r\nUne évaluation des risques sanitaires, des investigations complémentaires dans le but d'identifier les causes et de cerner l'étendue de la pollution ont été demandées à l'exploitant. \r\n\r\nL'exploitant a décidé d'étendre son réseau de surveillance à l'extérieur du site en aval par la mise en place de trois piézomètres le long des voies ferrées\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000753701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Ventilation de la zone non saturée (venting)"]
["SSP000753901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Pompage de rabattement ou de récupération","N/A","N/A","N/A"]
["SSP000754101","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique","Confinement par couverture et étanchéification"]
["SSP000754301","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000754901","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000755201","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000755601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Trichloroéthylène","COHV, solvants chlorés, fréons | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF) | Phytosanitaires","N/A","N/A","N/A","N/A","N/A"]
["SSP000755801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Chrome | Cuivre | Nickel | Plomb | Zinc","COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000756001","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Piège hydraulique ou Confinement hydraulique"]
["SSP000756101","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000756501","Exécution des travaux de réhabilitation",null,null," A l'été 2021, les travaux de démantèlement de la station sont complétés par une dépollution des sols par excavation.","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols","Ventilation de la zone non saturée (venting)"]
["SSP000756701","Exécution des travaux de réhabilitation",null,null," Pompage en 1993","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution"]
["SSP000757701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Analyse des enjeux sanitaires (EQRS, ARR)","N/A",null,"HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés)","N/A","N/A","N/A","N/A","N/A"]
["SSP000757701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique","Biodégradation dynamisée (ou atténuation naturelle dynamisée) | Confinement par couverture et étanchéification"]
["SSP000758201","Exécution des travaux de réhabilitation",null,null,"   ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Solidification/stabilisation"]
["SSP000758301","Surveillance environnementale","2003-11-20",null,"Résultat de la surveillance à la date du 2013-10-04 : LA SITUATION RESTE STABLE\nCommentaire : Échantillons cités dans le rapport d'essais BRGM du 28 novembre 2013 intégré au rapport final 2013 de mars 2014\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000758601","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique","Piège hydraulique ou Confinement hydraulique | Ventilation de la zone non saturée (venting)"]
["SSP000758901","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2013-01-02 : LA SITUATION RESTE STABLE\nInformations complémentaires : La campagne de surveillance de la qualité des eaux d'août 2013 met en évidence des teneurs en métaux, HAP, PCB, COHV et BTEX faibles voire nulles pour l'ensemble des piézomètres, excepté pour le piézomètre PZ4 où une forte teneur en hydrocarbures est constatée. \n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000759201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Pompage de rabattement ou de récupération","N/A","N/A","N/A"]
["SSP000759301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000759901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Trichloroéthylène","Benzène et dérivés | COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP000759901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Trichloroéthylène","COHV, solvants chlorés, fréons | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000760901","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Piège hydraulique ou Confinement hydraulique | Ventilation de la zone non saturée (venting)"]
["SSP000761101","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Piège hydraulique ou Confinement hydraulique"]
["SSP000761401","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000761601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés)","N/A","N/A","N/A","N/A","N/A"]
["SSP000762401","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000762701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000763001","Exécution des travaux de réhabilitation",null,null," .",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000763701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Mercure | Trichloroéthylène","COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000764301","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000764501","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000765201","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Ventilation de la zone non saturée (venting)"]
["SSP000765401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ...","Eaux souterraines","Diagnostic et Analyse","N/A","Chlorures","Autres éléments minéraux","N/A","N/A","N/A","N/A","N/A"]
["SSP000765601","Exécution des travaux de réhabilitation",null,null," ...","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Piège hydraulique ou Confinement hydraulique"]
["SSP000765701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ...","Eaux souterraines","Diagnostic et Analyse","N/A","Ammonium | Arsenic | Cadmium | Chlorures | Chrome | Cuivre | Mercure | Nickel | Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Sulfates | Zinc","Autres éléments minéraux | Benzène et dérivés | COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes | Paramètres azotés | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF) | Phytosanitaires | Radioactifs, isotopes et traceurs","N/A","N/A","N/A","N/A","N/A"]
["SSP000765801","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000765901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000766601","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000766801","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Ventilation de la zone non saturée (venting)"]
["SSP000766901","Exécution des travaux de réhabilitation",null,null," ...","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique","Confinement par couverture et étanchéification | Piège hydraulique ou Confinement hydraulique"]
["SSP000767501","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Piège hydraulique ou Confinement hydraulique"]
["SSP000767701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000768601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Zinc","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000769101","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2007-09-14 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000769201","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000769501","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique"]
["SSP000769601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000769701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000769801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000770101","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000770301","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000770701","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2006-09-19 : LA SITUATION SE DEGRADE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000771001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"COHV, solvants chlorés, fréons | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000771201","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000771201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000771401","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000771901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de gestion","N/A","Trichloroéthylène","COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP000772401","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000772801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000773301","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2012-12-31 : LA SITUATION RESTE STABLE\nCommentaire : La raffinerie dispose d’un suivi trimestriel de la qualité des eaux souterraines mis en place depuis 2006, qui se base sur 25 piézomètres. e suivi indique principalement une pollution aux hydrocarbures et au benzène. Les concentrations pour ces deux polluants sont sur plusieurs piézomètres supérieures aux valeurs de référence prises généralement en compte et issues de l’arrêté du 11 janvier 2007 relatif aux limites et références de qualité des eaux brutes et des eaux destinées à la consommation humaine.\r\n\r\nIl apparaît que le seuil défini par l’arrêté du 11 janvier 2007 pour les hydrocarbures (1000 µg/l) est largement dépassé : \r\nsur une série de piézomètres situés au Nord du site : des teneurs allant jusqu’à 110 mg/l ont été décelées (piézomètre A13.5) ;\r\nsur une série de piézomètres situés au centre du site : des teneurs allant jusqu’à 56 mg/l ont été décelées (piézomètre A13.7) ;\r\nsur le puits de pompage P3 : partie sud du site une teneur de 160 mg/l a été détectée en 2007. Il est à noter que pour ce point, les concentrations observées depuis 2012 sont très proches de 1000 µg/l.\r\n\r\nPlusieurs secteurs de la raffinerie sont fortement impactés par la présence de benzène de la nappe d’eau souterraine :\r\nsecteur le plus à l’ouest du canal (nord ouest du site) : des valeurs de 27 mg/l ont été décelées alors que l’arrêté du 11 janvier 2007 prévoit 1µg/l que valeur limite pour les eaux destinées à la consommation humaine ;\r\nsecteur ouest du site (piézomètres A 37.1, A.33) : c’est le secteur où l’on observe les plus fortes concentrations en benzène : 600 mg/l en octobre 2006 ;\r\nd’autres secteurs : milieu et sud du site sont impactés mais dans une moindre mesure : jusqu’à 1 mg/l environ constaté.\r\n\r\nDes dépassements de seuils ont également été observés pour les paramètres suivants :\r\n- aromatiques volatils\r\n- organo-halogénés volatils\r\n- HAP\r\n- Métaux\r\n- Indice phénols\r\n\r\nConcernant le suivi piézométrique de la zone C, seuls 3 piézomètres (C1.1, C1.4 et C1.5 bis) font l’objet d’une analyse et le piézomètre C1.1 est fortement impacté par des hydrocarbures flottants empêchant la réalisation d’analyses (depuis septembre 2011).\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000773401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Baryum | Cadmium | Chrome | Cobalt | Cuivre | Molybdène | Plomb | Trichloroéthylène | Zinc","COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000773701","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2012-10-31 : LA SITUATION RESTE STABLE\nInformations complémentaires : Lors de la campagne du 10/09/2003, il a été décelé:\r\n- 16 mg/L de Fer au droit de PZ2 ;\r\n- 9 mg/L de manganèse au droit de PZ2 ;\r\n- 70 µg/L d'arsenic au droit de PZ7.\r\n\r\nUne surveillance des eaux souterraines est en place depuis le mois de mars 2007. La fréquence des campagnes est semestrielle sur 5 ouvrages. La dernière campagne renseignée date du moi d'octobre 2012.\r\n\r\nLes analyses ont mis en évidence une contamination permanente des eaux du site en: \r\n- Arsenic (avec un maximum observé à 340 µg/l en avril 2010 pour 120 µg/l en octobre 2012) ;\r\n- Manganèse (max de 37 mg/l en avril 2009, 7,9 mg/l en octobre 2012).\r\n\r\nD'autres paramètres présentent occasionnellement de fortes concentration comme le Plomb (92 µg/l en septembre 2007 et 22 µg/l en avril 2011).\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000773901","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2000-07-11 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000774101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de gestion","N/A","Cuivre | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | COHV, solvants chlorés, fréons | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000774301","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification | Piège hydraulique ou Confinement hydraulique"]
["SSP000774601","Surveillance environnementale",null,null,"Résultat de la surveillance eaux souterraines : 1\n","Eaux souterraines","N/A","1",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000774701","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000775901","Surveillance environnementale","2003-02-04",null,"Résultat de la surveillance à la date du 2000-08-18 : LA SITUATION RESTE STABLE\nCommentaire : non satisfaisant pour usage sensible\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000776201","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000776501","Surveillance environnementale","1992-01-15",null,"Résultat de la surveillance à la date du 2014-01-01 : LA SITUATION RESTE STABLE\nCommentaire : Présence d'hydrocarbures\nInformations complémentaires : Les analyses de Décembre 2001 montrent une augmentation des teneurs en Plomb, hydrocarbures totaux et HAP dans les trois piézomètres mais toutefois sans être alarmante. La campagne du 26/06/2005 montre une situation satisfaisante et stable par rapport aux dernières campagnes. L'intégration dans le temps des résultats de ce suivi doit permettre en outre de contrôler l'évolution du panache ainsi que la pertinence des travaux de dépollution qui seront entrepris à l'issue de l'étude technico-économique susvisée.\r\n\r\nEn Juin et Décembre 2008, une augmentation des concentrations en HCTX, Benzène (50µg/l), Toluène et Xylène (11 mg/l) a été observée.\r\n\r\nLa campagne de décembre 2013 montre une teneurs en hydrocarbures de 18,3 mg/l en Bz22 en augmentation par rapport à juin 2013.\r\nLa situation est normale en Bz 19, Pz2, Pz3, Pz14 (amélioration, disparition du benzène), Pz22, PzA, puits n°3 et n°4.\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000776501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Reconditionnement de produits dangereux, Reconditionnement de déchets","N/A","N/A","N/A"]
["SSP000776801","Surveillance environnementale","1995-11-01",null,"Résultat de la surveillance à la date du 2014-10-01 : LA SITUATION S'AMELIORE\nCommentaire : Surveillance \"article 65\" de l'AM du 02/02/1998 modifié\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000777001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Solidification/stabilisation","Confinement par couverture et étanchéification"]
["SSP000778001","Exécution des travaux de réhabilitation","1986-01-30","1991-01-01"," Un arrêté préfectoral en date du 30 janvier 1986 a prescrit à l'exploitant l'évacuation des déchets à l'origine de la pollution et la réalisation d'une étude hydrogéologique, déposée en 1986 qui concluait à une situation d'équilibre.\n53 000 tonnes de déchets ont été évacuées en décharge de classe 1 entre 1985 et 1991.\nL'exploitant a ensuite proposé de réaliser la reprise de certaines scories et leur confinement sur site. Ces déchets représentaient un volume de 35 000 m3.\nPar arrêté préfectoral en date du 8 octobre 1991, il a été prescrit à l'exploitant la réalisation d'une alvéole étanche, répondant aux spécifications techniques pour les stockages de déchets industriels spéciaux, destinée à recevoir les déchets de fonderie contenant de la sylvinite à plus de 10 % (chlorures de potassium et de sodium).",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Reconditionnement de produits dangereux, Reconditionnement de déchets","N/A","N/A","N/A"]
["SSP000779101","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)","Confinement par couverture et étanchéification"]
["SSP000779401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Arsenic | Baryum | Mercure | Trichloroéthylène","COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000779601","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000780201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000780601","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Ventilation de la zone non saturée (venting)"]
["SSP000780601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000781101","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","6",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000781301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Chlorures | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Autres éléments minéraux | Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000781601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de conception des travaux (PCT)","N/A",null,"Phytosanitaires","N/A","N/A","N/A","N/A","N/A"]
["SSP000781901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000782001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Pompage de rabattement ou de récupération","N/A","N/A","N/A"]
["SSP000782301","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000782601","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2008-09-29 : LA SITUATION RESTE STABLE\nInformations complémentaires : Stable pour le zinc et cyanure mais augmentation de la concentration en chrome.\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000782601","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000783601","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000783801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP000784001","Surveillance environnementale","1998-01-01",null,"Résultat de la surveillance à la date du : 2006-07-01\nRésultat de la surveillance eaux souterraines : 1\n","Eaux souterraines","N/A","5",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000784701","Surveillance environnementale","1994-09-07",null,"Résultat de la surveillance à la date du 2008-03-01 : LA SITUATION RESTE STABLE\nCommentaire : Présence notable de l'élément Fer\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000785001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000785401","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique"]
["SSP000785701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000785901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Chrome","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000786201","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000786401","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000786701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000787001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Baryum | Chlorures | Trichloroéthylène","Autres éléments minéraux | COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000787201","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000787901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000788001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000788201","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000788601","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000788701","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)","Confinement par couverture et étanchéification"]
["SSP000789001","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000789501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000789901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000790301","Surveillance environnementale","2004-06-30",null,"Résultat de la surveillance à la date du 2014-09-15 : LA SITUATION RESTE STABLE\nCommentaire : traces Zinc\nInformations complémentaires : Les campagnes des trois premiers trimestres 2008 montrent une situation satisfaisante et stable, avec toutefois un \"pic\" en Zinc sur le piézomètre P4 à l'aval hydraulique. Cependant, la valeur mesurée reste inférieure à la valeur de référence pour l'eau de consommation .\r\n\r\nLes campagnes des deux premiers trimestres 2009, confirme cette tendance avec des valeurs satisfaisantes et stables. Le \"pic\" de zinc s'observe toujours sur le piézomètre P4 avec des valeurs atteignant 169 µg/L.\r\nLes teneurs en mercure se situent en dessous du seuil de détection analytique, sauf au point P4 où des traces sont observées avec un maximum de 0,7 µg/l en juin 2007, qui n’a pas été observé depuis (la valeur limite pour l’eau de consommation est de 1 µg/l).\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000790501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Cuivre | Mercure | Nickel | Plomb | Zinc","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000790501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000791001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Aluminium | Arsenic | Cuivre | Plomb","COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000791101","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000791501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000791901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," /","Sol - Sous-sol","Diagnostic et Analyse","N/A","Chrome | Cuivre | Nickel | Plomb | Zinc","COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000792301","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Lavage à l'eau","Biodégradation dynamisée (ou atténuation naturelle dynamisée)"]
["SSP000792801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de conception des travaux (PCT)","N/A","Ammonium | Cadmium | Mercure | Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Zinc","Benzène et dérivés | COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes | Paramètres azotés | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000793101","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Piège hydraulique ou Confinement hydraulique"]
["SSP000793101","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du : 2012-09-23\nRésultat de la surveillance eaux souterraines : 1\nen attente de résultats par la société Oissel remediation\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000793701","Surveillance environnementale",null,null,"","Eaux souterraines","N/A","1",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000794301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000794601","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000794801","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000795201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Chrome","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000795401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Chrome | Cuivre | Cyanures libres | Trichloroéthylène","Autres éléments minéraux | COHV, solvants chlorés, fréons | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000796001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP000796101","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000797101","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000797201","Surveillance environnementale","1989-01-01",null,"Résultat de la surveillance eaux souterraines : 2\nEncore des fortes teneurs\n","Eaux souterraines","N/A","1",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000797401","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000797501","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000798101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Trichloroéthylène","Benzène et dérivés | COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000798501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000798701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000798901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"COHV, solvants chlorés, fréons | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000799101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...) | Pompage de rabattement ou de récupération","N/A","N/A","N/A"]
["SSP000799201","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000799801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," .","Sol - Sous-sol","Plan de conception des travaux (PCT)","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000799901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000800201","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000800601","Surveillance environnementale","2003-10-08",null,"Résultat de la surveillance à la date du 2009-11-01 : LA SITUATION RESTE STABLE\nCommentaire : Anomalies en hydrocarbures sur SP9 et SP12\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000801001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000801001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Reconditionnement de produits dangereux, Reconditionnement de déchets","N/A","N/A","N/A"]
["SSP000801301","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000801501","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000802001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000802201","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000802701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification | Ventilation de la zone non saturée (venting)"]
["SSP000803001","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2013-05-06 : LA SITUATION S'AMELIORE\nCommentaire : Les analyses d'eaux souterraines montrent une absence de quantification de polluants en 2013, cependant, des hauteurs de flottant importantes ont été relevées en 2011.\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000803601","Exécution des travaux de réhabilitation",null,null," Méthode biologique ou chimique","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000803701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Chrome | Fer","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000803901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000804101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Arsenic | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000804501","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000804701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000805001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000805301","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique"]
["SSP000806001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000806001","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000806901","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000807301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Arsenic | Cadmium | Chrome | Cuivre | Mercure | Nickel | Plomb | Zinc","Hydrocarbures et indices liés | Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000807801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000807901","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2016-12-12 : LA SITUATION RESTE STABLE\nInformations complémentaires : amélioration importante de mai 2015 à février 2016 puis stabilisation\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000808401","Surveillance environnementale",null,null,"Informations complémentaires : \r\nle suivi des eaux souterraines initié en 1998 met en évidence une atténuation des concentrations des polluants recherchés au niveau de l'ensemble des ouvrages. Les teneurs sont majoritairement en deçà des seuils de quantification. La présence limitée de chlorobenzène a été ponctuellement détectée (2002 et 2007). Un impact en PCB a été constaté jusqu'en 2010.\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000808501","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique"]
["SSP000808801","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000808801","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000810001","Exécution des travaux de réhabilitation",null,null," Incinération","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000810401","Surveillance environnementale","2001-02-02",null,"Résultat de la surveillance à la date du 2016-04-21 : LA SITUATION RESTE STABLE\nCommentaire : Traces\nInformations complémentaires : La campagne du 30/09/2014 montre que le Pz6 (proche du site SREE, aquifère des remblais) reste contaminé par le chlorobenzène (11 mg/l) et le benzène ; par contre, les PCB n’y ont pas été détectés lors de cette campagne. Ces derniers  ont été mesurés à une teneur maximal de 0,4 µg/l dans la nappe superficielle au droit du site, au niveau du Pz15.\r\n\r\nSynthèse de la campagne de mars 2015 :\r\n1 - Etat des eaux souterraines\r\nLes analyses réalisées en mars 2015 ont montré la présence, dans les eaux souterraines :\r\nSur le site et à proximité immédiate :\r\n- De PCB dans la nappe superficielle, avec des concentrations allant jusqu'à 1.8 μg/l de PCB totaux (Pz9) ; cette pollution reste bien présente depuis 2013 ;\r\n- Les autres polluants recherchés (COHV et BTEX) n'ont pas été détectés, sauf des traces de tétrachloroéthylène (en limite de quantification) dans le Pz9.\r\nDans les points situés à plus de 50 m du site :\r\n- Des traces de PCB sont détectées dans tous les piézomètres profonds (moins de 0.1 μg/l), peut-être en lien avec les travaux réalisés dans l’environnement ces derniers mois ;\r\n- Pas de PCB dans le Pz11 (Rue Delbos, nappe superficielle à plus de 50 m du site).\r\nCes analyses confirment la contamination des eaux souterraines par les PCB issus du site SREE, et montrent que la baisse observée en 2013, par rapport aux études antérieures, est globalement confirmée.\r\nOn observe toutefois une assez grande variabilité des résultats depuis janvier 2013 ; la partie profonde des \"argiles vasardes\" montre occasionnellement de faibles contaminations.\r\n\r\n2 - Impact qualitatif du site SREE sur les milieux environnants\r\n- Qualité des eaux souterraines hors site\r\nGlobalement, les analyses de mars 2015 confirment que l'état qualitatif des eaux souterraines hors du site est peu dégradé en dehors du Pz6 (situé à 2 m à l'est du site SREE) ; d'autre part la faible perméabilité des couches profondes et le faible gradient de la nappe ne sont pas favorables à une dissémination importante des polluants loin du site.\r\nL'axe drainant situé sous la rue Delbos ne paraît pas être un vecteur important de pollution : seules des traces occasionnelles de PCB sont observées dans le Pz10, situé à 75 m en aval du site dans l'axe de la rue Delbos (moins de 0.01 μg/l).\r\n- Modalités de circulation des eaux souterraines sous le site\r\nLes observations piézométriques et de la minéralisation globale permettent de confirmer les modalités de circulation des eaux souterraines sous le site, observées depuis janvier 2013 :\r\n  . La nappe superficielle des remblais et limons supérieurs du site circule vers le nord-est, en direction de la rue Delbos ; sa minéralisation fluctue en lien avec l'infiltration des eaux pluviales et de la recharge hivernale.\r\n  . La \"nappe profonde\" des \"argiles vasardes\", présente sous la couche d'argile, est aussi drainée par la rue Delbos. Son potentiel piézométrique montre qu'elle est captive (en pression sous la couche d'argile) sous le site : dans le Pz8, le niveau enregistré est généralement inférieur à celui de la nappe des remblais, sauf quand les niveaux supérieurs de celle-ci s’assèchent en période estivale.\r\nElle est habituellement plus basse que la nappe des remblais sous la rue Delbos et dans la zone d'influence du drainage (Pz 5, Pz8, Pz10), ce qui peut favoriser des échanges de la nappe des remblais vers la nappe profonde. Ce décalage devient très faible ou s’inverse en période sèche.\r\nLes niveaux relevés en 2013-2015 dans les piézomètres captant la \"nappe profonde\" sous la rue Delbos ne permettent pas de préciser la direction d'écoulement de cette nappe sous la rue.\r\n\r\nCampagne du 28/10/2015 sur les 3 piézomètres (PZ5, PZ15 et PZ7) de la surveillance post travaux de dépollution :\r\n- traces de Toluène entre 0,31 et 0,41 µg/l,\r\n- traces de chlorobenzènes en PZ5 très légèrement supérieures aux limites de quantification du laboratoire,\r\n- concentrations PCB en PZ5 et PZ7 inférieures aux limites de quantification du laboratoire,\r\n- traces PCB EN PZ15, très proches des seuils de quantification du laboratoire.\r\n\r\nCampagne du 21/04/2016 :\r\n• Composés Aromatiques Volatils - BTEX\r\nLes eaux prélevées au droit du piézomètre Pz5 présentent un impact par le toluène, avec 4,9 μg/l. Les\r\nanalyses montrent des teneurs pour les autres composés inférieures aux limites de quantification du\r\nlaboratoire sur cet ouvrage.\r\nLes deux autres ouvrages ne présentent pas un tel impact. Les teneurs pour les différents composés\r\ntestés sont inférieures aux limites de quantification du laboratoire.\r\n• Chlorobenzènes\r\nLes eaux prélevées au droit du piézomètre Pz15 présentent des traces de 1,2,4-trichlorobenzène, la\r\nteneur étant très légèrement supérieure à la limite de quantification du laboratoire (teneur de 0,03 μg/l\r\npour une limite de quantification de 0,01 μg/l).\r\nLes concentrations pour chacun des chlorobenzènes testés sur les deux autres ouvrages suivis sont\r\nstrictement inférieures aux limites de quantification du laboratoire.\r\n• Polychlorobiphényls - PCB\r\nLes concentrations pour chacun des PCB testés au droit de l'ouvrage Pz7 interceptant les zones\r\nsaturées des argiles (aval du site) sont toutes inférieures aux limites de quantification du laboratoire.\r\nLes eaux des zones saturées des remblais / argiles prélevées au droit de Pz15 mettent en évidence la\r\nprésence de PCB, avec une teneur globale de 1,3 μg/l pour la somme des 7 PCB testés. Les PCB\r\nprépondérants correspondent aux PCB 101, 138, 153 et 180 ;\r\nAu droit de Pz5, des traces de PCB ont été mises en évidence, avec cependant des teneurs très\r\nproches des limites de quantifications du laboratoire.\nDate de fin envisagée de la surveillance : 2017-06-30","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000810901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000810901","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000811501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000811801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de gestion","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | COHV, solvants chlorés, fréons | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000812401","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2010-11-23 : LA SITUATION RESTE STABLE\nCommentaire : pas de pollution en aval du site\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000812501","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000813201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000813401","Surveillance environnementale","2001-08-03",null,"Résultat de la surveillance à la date du 2009-09-21 : LA SITUATION RESTE STABLE\nCommentaire : Non satisfaisant AMS pz12\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000813901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Chrome","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000814001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...) | Reconditionnement de produits dangereux, Reconditionnement de déchets","N/A","N/A","N/A"]
["SSP000814501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de gestion","N/A","Aluminium | Chrome","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000814901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Trichloroéthylène","COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP000815101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Interprétation de l''état des milieux (IEM)","N/A","Arsenic | Cuivre | Plomb","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000815401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000815501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Nickel","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000815601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A","Cuivre | Cyanures libres | Nickel | Plomb | Zinc","Autres éléments minéraux | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000816001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cadmium | Nickel | Plomb | Sulfates","Autres éléments minéraux | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000816401","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000817001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Chrome | Plomb","HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000817301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Pompage de rabattement ou de récupération","N/A","N/A","N/A"]
["SSP000817701","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000817901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"COHV, solvants chlorés, fréons | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000818301","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2014-02-24 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000818901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000819601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"COHV, solvants chlorés, fréons | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000819801","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2007-04-01 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000820001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Nickel","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000820101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...) | Pompage de rabattement ou de récupération","N/A","N/A","N/A"]
["SSP000820601","Exécution des travaux de réhabilitation",null,null,"Dépollution","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols","Ventilation de la zone non saturée (venting)"]
["SSP000820901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Chrome","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000821401","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Ventilation de la zone non saturée (venting)"]
["SSP000821501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000821801","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique","Piège hydraulique ou Confinement hydraulique"]
["SSP000821801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Pompage de rabattement ou de récupération","N/A","N/A","N/A"]
["SSP000822301","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","1",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000822401","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000822901","Surveillance environnementale",null,null,"","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000823001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Chrome","HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000823301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Pompage de rabattement ou de récupération","N/A","N/A","N/A"]
["SSP000823501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000824101","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2009-05-20 : LA SITUATION RESTE STABLE\nCommentaire : présence de solvants halogénés\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000824301","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2011-05-18 : LA SITUATION RESTE STABLE\nCommentaire : surveillance de la concentration en uranium\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000824601","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000824801","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Piège hydraulique ou Confinement hydraulique"]
["SSP000825101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cuivre | Plomb | Zinc","COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000825201","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000825601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000825701","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000825801","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000826201","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique","Ventilation de la zone non saturée (venting)"]
["SSP000826301","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols","Biodégradation dynamisée (ou atténuation naturelle dynamisée)"]
["SSP000826801","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000827101","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","1",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000827201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Chlorures","Autres éléments minéraux","N/A","N/A","N/A","N/A","N/A"]
["SSP000827401","Surveillance environnementale","2006-01-01",null,"Résultat de la surveillance à la date du 2016-03-30 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000827901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000828101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Chrome | Cuivre | Nickel | Zinc","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000828301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage | Interdiction d'accès (clôture...) | Reconditionnement de produits dangereux, Reconditionnement de déchets","N/A","N/A","N/A"]
["SSP000828601","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000829401","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2001-03-31 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000829601","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000829901","Surveillance environnementale","2002-06-26",null,"Résultat de la surveillance à la date du 2008-10-09 : LA SITUATION S'AMELIORE\nCommentaire : Evolution favorable et pérenne de la qualité des e\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000830201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Aluminium | Sulfates | Trichloroéthylène","Autres éléments minéraux | COHV, solvants chlorés, fréons | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000830601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cobalt | Molybdène | Nickel | Plomb","Hydrocarbures et indices liés | Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000830801","Exécution des travaux de réhabilitation",null,null,"  Précisions données dans la description de l'instruction",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000831001","Surveillance environnementale","2002-06-01",null,"Résultat de la surveillance à la date du 2010-03-31 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000831101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Interprétation de l''état des milieux (IEM)","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000831601","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2010-10-01 : LA SITUATION RESTE STABLE\nCommentaire : traitement de certaines zones prévues\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000832001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000832101","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique","Biodégradation dynamisée (ou atténuation naturelle dynamisée)"]
["SSP000832601","Surveillance environnementale","1998-03-30",null,"Résultat de la surveillance à la date du 2006-12-06 : LA SITUATION RESTE STABLE\nCommentaire : pas d'impact du site constaté\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000832701","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000833001","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2010-09-24 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000833201","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Piège hydraulique ou Confinement hydraulique"]
["SSP000833801","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2012-12-05 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000834001","Surveillance environnementale","2000-10-27",null,"","Eaux souterraines","N/A","1",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000834401","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000834701","Surveillance environnementale",null,null,"Il a été demandé à L'EPML de suivre le degré de pollution en hydrocarbures totaux dans la nappe, à l'aval hydraulique de la citerne.\nCe suivi a eu lieu pendant un an (de décembre 1998 à novembre 1999). La teneur en hydrocarbures totaux a toujours été inférieure à 0.1 mg/l.","Eaux souterraines","N/A","2","Indice hydrocarbures totaux - produits pétroliers","Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000835201","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"Étude diagnostic de septembre 1994 et étude complémentaire.\n\nÉtude de réhabilitation de Janvier 1997.\n\nAu cours de ces études, des prélèvements et analyses de sols ont été effectués, ainsi que des analyses sur les eaux souterraines au droit du site.\nTrois secteurs pollués par des hydrocarbures ont été identifiés, il s'agit de l'ancienne aire de lavage, des secteurs des postes de chargements des camions et de déchargements des wagons le long des voies ferrées.","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000835401","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000835801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Baryum | Chrome | Cuivre | Nickel | Plomb","COHV, solvants chlorés, fréons | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000836101","Exécution des travaux de réhabilitation",null,null,"A noter que l'ensemble des déchets a été éliminé et que les transformateurs qui étaient employés sur le site ne contenaient pas d'huiles au Polychlorobiphényles (PCB). ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000836801","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000836901","Surveillance environnementale","2004-02-20",null,"Résultat de la surveillance à la date du 2008-02-13 : LA SITUATION S'AMELIORE\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000837301","Surveillance environnementale",null,null,"Compte tenu de la profondeur de la nappe, du caractère compact des terrains, de l'isolement des zones de contamination résiduelle, l'impact des contaminations résiduelles sur les eaux souterraines peut être exclu. Ainsi, seule la surveillance de l'étanchéité des cuves et tuyauteries associées est prévue.","Eaux souterraines","N/A","1",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000837701","Surveillance environnementale","2003-04-09",null,"Résultat de la surveillance à la date du 2013-10-18 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000838701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000839201","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000839501","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"Une évaluation simplifiée des risques (ESR) est remise à l'inspection le 11 février 2002. Cette ESR classe le site en 2, à surveiller, pour son impact sur les eaux souterraines (usage AEP), sur les eaux superficielles (usage non AEP) et pour les sols (usage non sensible).","Eaux souterraines","Analyse des enjeux sanitaires (EQRS, ARR)","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000840501","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2008-03-27 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000840601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...) | Reconditionnement de produits dangereux, Reconditionnement de déchets","N/A","N/A","N/A"]
["SSP000841401","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"Une étude détaillée des risques a donc été réalisée, faisant suite à l'ESR, afin de déterminer les risques générés pour la santé humaine par contact avec les poussières issues de ces tas. Cette étude d'impact démontre qu'il n'y a pas de risque pour l'Homme dans les conditions actuelles d'exploitation du site, c'est à dire accès limité uniquement aux personnels travaillant dans l'usine.","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000841501","Surveillance environnementale",null,null,"La surveillance des eaux souterraines et des eaux de l'Ingressin est prescrite par arrêté préfectoral du 23 octobre 2002.","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000842001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Ammonium | Chlorures | Cyanures libres | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Sulfates | Trichloroéthylène","Autres éléments minéraux | Benzène et dérivés | COHV, solvants chlorés, fréons | Paramètres azotés","N/A","N/A","N/A","N/A","N/A"]
["SSP000842201","Surveillance environnementale",null,null,"Un plan de surveillance des eaux souterraines a été établi, la surveillance est réalisée à partir d'un réseau de six piézomètres qui permettra de mesurer l'impact éventuel des sources identifiées sur les eaux de la nappe s'écoulant au droit du site. Cette surveillance est prescrite par arrêté préfectoral du 23 octobre 2003.","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000843101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Interprétation de l''état des milieux (IEM)","N/A","Arsenic | Chrome | Cobalt | Cuivre | Nickel | Plomb | Trichloroéthylène | Zinc","COHV, solvants chlorés, fréons | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000843401","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000843901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Baryum | Cadmium | Chrome | Mercure | Nickel | Plomb","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000844001","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"Le préfet a également imposé à la société BRENNTAG, par arrêté préfectoral du 03 juillet 2014, la réalisation d'une interprétation de l’état des milieux (IEM).\nCette dernière a transmis l'étude d'interprétation de l'état des milieux en février 2015.","Eaux souterraines","Interprétation de l''état des milieux (IEM)","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000844501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000844801","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2007-11-15 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000845101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de gestion","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000845301","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols","Confinement par couverture et étanchéification"]
["SSP000845501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Pompage de rabattement ou de récupération","N/A","N/A","N/A"]
["SSP000846101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Aluminium | Cadmium | Chrome | Cuivre | Nickel | Plomb | Zinc","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000846301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000846701","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Ventilation de la zone non saturée (venting)"]
["SSP000846901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique"]
["SSP000847401","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000847501","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000847601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000848301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000848901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Cuivre | Mercure","HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000849301","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2007-01-19 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","1",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000850001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000850201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Arsenic","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000850701","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2016-10-01 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000850801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cadmium | Chrome | Cuivre | Mercure | Plomb | Zinc","HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000851001","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2016-12-15 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000851401","Surveillance environnementale","2003-10-23",null,"Résultat de la surveillance eaux souterraines : 1\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000851801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000852001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000852501","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)","Ventilation de la zone non saturée (venting)"]
["SSP000852801","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000852801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Chrome | Cobalt | Mercure | Molybdène | Nickel | Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000853201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000853601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000853901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000854101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000854501","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2012-05-11 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000854501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000854901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000855001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000855401","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2006-02-01 : LA SITUATION S'AMELIORE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000856001","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2018-03-01 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000856601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage","N/A","N/A","N/A"]
["SSP000857101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage | Interdiction d'accès (clôture...) | Pompage de rabattement ou de récupération","N/A","N/A","N/A"]
["SSP000857701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)","Biodégradation dynamisée (ou atténuation naturelle dynamisée)"]
["SSP000857701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique","Biodégradation dynamisée (ou atténuation naturelle dynamisée)"]
["SSP000858301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000858401","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000858801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000859001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Arsenic | Cobalt | Nickel","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000859401","Surveillance environnementale","2002-02-01",null,"Résultat de la surveillance à la date du 2011-09-23 : LA SITUATION RESTE STABLE\nCommentaire : absence de pollution dans la nappe\nDate de fin envisagée de la surveillance : 2014-10-08","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000859501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Arsenic | Cadmium | Cuivre | Plomb | Zinc","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000859701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000859901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Chrome","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000860401","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)","Confinement par couverture et étanchéification"]
["SSP000860501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000860601","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000860801","Surveillance environnementale","2005-01-01",null,"Résultat de la surveillance à la date du 2010-10-11 : LA SITUATION RESTE STABLE\nCommentaire : PZ7 à sec en oct. 2010. Pas de confirmation des pollutions détectées en avril 2010. \r\n\r\n\nInformations complémentaires : 04/05/ 2006 : tensio actifs  détectés\r\n\r\nAoût 2006 : dépassements (piézomètres 1, 4 et 6) des valeurs de constat d'impact à usages sensibles en hydrocarbures totaux.\r\nDépassement de valeur de constat d'impact sur l'arsenic (piézomètre 6).\r\nPas d'analyse sur les tensio-actifs car le piézomètre 7 était à sec.\r\n\r\nAvril 2007 : tensio actifs  détectés. Mise en place d'investigations pour détecter des fuites sur la bâche du bassin de confinement.\r\n\r\nMai 2008 : agent de surface détecté sur PZ7(supérieur à la limite réglementaire).\r\n\r\nSeptembre 2008 : pas de pollution constatée.\r\n\r\nAvril 2009 : agent de surface détecté sur PZ7(supérieur à la limite réglementaire).\r\n\r\nAvril 2010 : agent de surface et indice phénol détecté sur PZ7(supérieur à la limite  à réglementaire). \r\n\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000861101","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000861301","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000861601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de gestion","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000861701","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000861901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"COHV, solvants chlorés, fréons | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000862201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cuivre | Plomb","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000862501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000862601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cadmium | Chrome","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000862901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000863101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Cuivre | Nickel | Plomb | Zinc","HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000863401","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Piège hydraulique ou Confinement hydraulique"]
["SSP000863601","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000864101","Surveillance environnementale","2002-04-05",null,"Résultat de la surveillance à la date du 2012-05-16 : LA SITUATION RESTE STABLE\nInformations complémentaires : Les résultats des dernières mesures dans les eaux souterraines ont montré la stabilité des résultats sur les différents paramètres :\r\n- des concentrations inférieures à la limite de quantification ou inférieures aux valeurs réglementaires les métaux, les BTEX et les composés organohalogénés volatils.\r\n- des concentrations inférieures à la limite de quantification pour les hydrocarbures à l'exception d'une mesure sur 1 piézomètre en mai 2012 où la concentration était légèrement supérieure (1,4 mg/l) à la limite de qualité des eaux brutes pour la production d'eau destinée à la consommation humaine (1 mg/l) ; cette concentration pourrait être liée à la présence et la manipulation de produits hydrocarburés dans la zone du piézomètre concerné ; les prochaines mesures permettront de confirmer ou d'infirmer la présence d'hydrocarbures.\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000864101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000864501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...) | Reconditionnement de produits dangereux, Reconditionnement de déchets","N/A","N/A","N/A"]
["SSP000864701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique"]
["SSP000865201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000865501","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000865801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de gestion","N/A","Ammonium | Arsenic | Plomb | Sulfates","Autres éléments minéraux | Metaux et métalloïdes | Paramètres azotés","N/A","N/A","N/A","N/A","N/A"]
["SSP000865801","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique"]
["SSP000866301","Surveillance environnementale","2000-11-28",null,"Résultat de la surveillance à la date du 2014-12-04 : LA SITUATION RESTE STABLE\nCommentaire : Depuis 2013, présence d'un pH acide, nitrates, ammonium, sulfates et fluorures au nord du site, sur au centre et proche aval. Sur ce dernier, un impact en métaux est également toujours observé depuis 2011.\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000866301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage","N/A","N/A","N/A"]
["SSP000867001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000867101","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000867601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000867901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000868101","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000868501","Surveillance environnementale","1997-05-29",null,"Résultat de la surveillance à la date du 2010-03-25 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000869001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Nickel | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000869101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000869601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000869801","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Piège hydraulique ou Confinement hydraulique"]
["SSP000870001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Chrome | Cuivre | Plomb","COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000870201","Surveillance environnementale","2005-01-01",null,"Résultat de la surveillance à la date du 2017-06-15 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000870501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000870701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique"]
["SSP000871001","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 1999-06-24 : LA SITUATION S'AMELIORE\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000871201","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","1",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000871401","Exécution des travaux de réhabilitation",null,null," site en activité",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000871701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Chrome","COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000872001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000872101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Reconditionnement de produits dangereux, Reconditionnement de déchets","N/A","N/A","N/A"]
["SSP000872701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000873101","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000873501","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000873701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de gestion","N/A","Ammonium | Chlorures | Nickel | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Autres éléments minéraux | Benzène et dérivés | COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | Metaux et métalloïdes | Paramètres azotés","N/A","N/A","N/A","N/A","N/A"]
["SSP000874201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," Plan de gestion de la pollution","Eaux souterraines","Plan de gestion","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000874201","Exécution des travaux de réhabilitation",null,null," Mise en sécurité",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000875001","Exécution des travaux de réhabilitation",null,null,"Travaux de dépollution : confinement par couverture et étanchéification","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000875201","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols","Ventilation de la zone non saturée (venting)"]
["SSP000875601","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000876001","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2004-02-12 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000876301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Chlorures","Autres éléments minéraux | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000876601","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2008-09-23 : LA SITUATION RESTE STABLE\nCommentaire : présence de trichloroéthylène de façon aléatoire\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000877001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000877401","Surveillance environnementale","2001-04-04","2002-02-28","Résultat de la surveillance à la date du 2002-02-28 : LA SITUATION RESTE STABLE\nInformations complémentaires : Un Arrêté Préfectoral en date du 5 janvier 2001 prescrit la mise en œuvre d'un programme de surveillance de la qualité des eaux souterraines pour une durée minimale de 2 ans.\r\n\r\nLes résultats de cette surveillance montrent des teneurs en hydrocarbures dans les eaux inférieures aux limites de détection (50 µg/l) à l'exception d'une teneur de 80 µg/l mise en évidence en décembre 2001 sur l'un des trois piézomètres. Les analyses de février 2002 ne montraient plus d'anomalies.\n","Eaux souterraines","N/A","1",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000877601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000878001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000878301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Chrome | Cuivre | Mercure","COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000878401","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000878801","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000879001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A","Mercure","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000879301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000879301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000879701","Surveillance environnementale","2003-03-05",null,"Résultat de la surveillance à la date du : 2012-12-12\nRésultat de la surveillance eaux souterraines : 1\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000880001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000880301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Trichloroéthylène","Benzène et dérivés | COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés)","N/A","N/A","N/A","N/A","N/A"]
["SSP000880401","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000880701","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000880901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000881501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Aluminium | Baryum | Fer","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000881501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Baryum | Cadmium | Chrome | Plomb | Zinc","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000881701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000882101","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du : 2018-11-01\nRésultat de la surveillance eaux souterraines : 2\nUne surveillance semestrielle de la qualité des eaux superficielles et souterraines est en place depuis le 20/06/2005.\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000882401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cuivre | Plomb | Zinc","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000882601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000883001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A","Arsenic | Cadmium | Chrome | Cuivre | Mercure | Nickel | Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Zinc","Benzène et dérivés | COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000883301","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000883501","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification | Piège hydraulique ou Confinement hydraulique"]
["SSP000883501","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000883801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de gestion","N/A","Arsenic | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000884001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Cadmium | Chlorures | Cuivre | Mercure | Plomb | Sulfates | Zinc","Autres éléments minéraux | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000884101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000885201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," Diagnostic de l'état du sous-sol","Eaux souterraines","Diagnostic et Analyse","N/A",null,"COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP000886201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000886501","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2015-11-01 : LA SITUATION RESTE STABLE\nCommentaire : Teneurs en biphényle encore importantes\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000886801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage","N/A","N/A","N/A"]
["SSP000886901","Surveillance environnementale","2000-01-01",null,"Résultat de la surveillance à la date du 2014-06-01 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000887201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Ammonium | Cadmium | Cyanures libres | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Autres éléments minéraux | Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes | Paramètres azotés","N/A","N/A","N/A","N/A","N/A"]
["SSP000887301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cuivre | Cyanures libres | Plomb","Autres éléments minéraux | Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000887501","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000887801","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"     ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Ammonium | Cyanures libres | Sulfates","Autres éléments minéraux | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Paramètres azotés","N/A","N/A","N/A","N/A","N/A"]
["SSP000888101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000888301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Chlorures | Plomb | Sulfates","Autres éléments minéraux | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000888501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000889101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Fer | Sulfates","Autres éléments minéraux | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000889101","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000889401","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000889701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Ammonium | Plomb | Sulfates","Autres éléments minéraux | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes | Paramètres azotés","N/A","N/A","N/A","N/A","N/A"]
["SSP000889901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000890301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000890601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cadmium | Sulfates","Autres éléments minéraux | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000891001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000891201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000891501","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2011-11-10 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000891801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000892301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"COHV, solvants chlorés, fréons | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000892601","Surveillance environnementale","1997-11-01",null,"Résultat de la surveillance à la date du 2016-10-21 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000893001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Aluminium | Ammonium | Arsenic | Baryum | Chlorures | Chrome | Fer | Plomb","Autres éléments minéraux | Metaux et métalloïdes | Paramètres azotés","N/A","N/A","N/A","N/A","N/A"]
["SSP000893101","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Ventilation de la zone non saturée (venting)"]
["SSP000893401","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000893601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000893901","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000894501","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000894801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000895101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000895401","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique"]
["SSP000895901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000896401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000896501","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000896601","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,null,"Filtration"]
["SSP000896801","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Ventilation de la zone non saturée (venting)"]
["SSP000897101","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000898101","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000898101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000898601","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du : 2011-10-17\nRésultat de la surveillance eaux souterraines : 1\nAbsence de pollution significative depuis 2004.\n","Eaux souterraines","N/A","1",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000898901","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000899201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000899301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000899901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000900001","Exécution des travaux de réhabilitation",null,null,"faits","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique","Ventilation de la zone non saturée (venting)"]
["SSP000900401","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000900501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Pompage de rabattement ou de récupération","N/A","N/A","N/A"]
["SSP000901101","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2009-11-13 : LA SITUATION RESTE STABLE\nCommentaire : forte variation hautes et basses eaux\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000901201","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000901701","Surveillance environnementale","2002-10-16",null,"Résultat de la surveillance à la date du 2012-12-28 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000901801","Surveillance environnementale","1998-11-05","2013-11-04","Résultat de la surveillance à la date du 2013-11-04 : LA SITUATION S'AMELIORE\nDate de fin envisagée de la surveillance : 2013-11-04","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000902501","Exécution des travaux de réhabilitation",null,null," Travaux de dépollution par oxydation chimique","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Oxydation chimique"]
["SSP000902501","Exécution des travaux de réhabilitation",null,null," Mise en sécurité du site effectuée",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000903401","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2003-12-01 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","1",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000903801","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2008-02-07 : LA SITUATION S'AMELIORE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000904201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Arsenic | Chlorures | Fer","Autres éléments minéraux | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000904401","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2008-04-03 : LA SITUATION RESTE STABLE\nCommentaire : présence de 1,2-dichlopropane supérieur au seuil\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000904401","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000904701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols","Biodégradation dynamisée (ou atténuation naturelle dynamisée) | Ventilation de la zone non saturée (venting)"]
["SSP000905001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique","Confinement par couverture et étanchéification"]
["SSP000905101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A","Arsenic | Cadmium | Cuivre | Mercure | Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Trichloroéthylène | Zinc","Benzène et dérivés | COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000905301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000906601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000907101","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000907301","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000907501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage","N/A","N/A","N/A"]
["SSP000907901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Trichloroéthylène | Zinc","COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000908401","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000908701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000909001","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du : 2011-03-04\nRésultat de la surveillance eaux souterraines : 1\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000909401","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2011-06-09 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000909701","Exécution des travaux de réhabilitation",null,null," .",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000910101","Etude SSP et ingénierie des travaux de réhabilitation","1999-02-23",null,"Par arrêté préfectoral en date du 23 février 1999, la société WIPELEC devait réaliser un diagnostic initial et une évaluation simplifiée des risques pour son établissement.",null,"Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000910601","Etude SSP et ingénierie des travaux de réhabilitation","1999-02-04","2006-11-24","Suite à différentes procédures de sanctions administratives et pénales, la société GALVACHAUD a transmis un diagnostic initial et une évaluation simplifiée des risques. Ces études conduisent en un classement du site en site banalisable. Toutefois cette étude a révélé un marquage au zinc sous la cuve de fluxion contenant du chlorure de zinc.\n\nL'inspection des installations classées a demandé des investigations complémentaires relatives à la caractérisation de la zone en cause et à l'impact de cette zone sur les eaux souterraines.\n\nLes compléments d'information demandés concluent à un classement du site en classe 2, nécessitant surveillance.\n",null,"Analyse des enjeux sanitaires (EQRS, ARR)","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000910701","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération","Confinement par couverture et étanchéification"]
["SSP000911301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," .","Sol - Sous-sol","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés","N/A","N/A","N/A","N/A","N/A"]
["SSP000911301","Exécution des travaux de réhabilitation",null,null," .","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000911801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A","Arsenic | Plomb","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000912001","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du : 2009-07-29\nRésultat de la surveillance eaux souterraines : 1\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000912201","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Lavage à l'eau","Confinement par couverture et étanchéification"]
["SSP000912401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Arsenic","HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000913301","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000913901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000918001","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000918101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000918701","Surveillance environnementale","2003-09-10",null,"Résultat de la surveillance à la date du 2013-03-01 : LA SITUATION RESTE STABLE\nCommentaire : présence d'hydrocarbures et de propiconazole décelée dans le forage du site\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000919101","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique"]
["SSP000919701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000920201","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000922001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Ammonium | Cyanures libres | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Autres éléments minéraux | Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Paramètres azotés","N/A","N/A","N/A","N/A","N/A"]
["SSP000922001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000922801","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000923201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000924101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Nickel | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Zinc","Benzène et dérivés | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000924301","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2009-04-14 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000924401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Chrome | Cuivre | Nickel | Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Trichloroéthylène | Zinc","Benzène et dérivés | COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000924501","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000924701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000925401","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du : 2014-04-25\nRésultat de la surveillance eaux souterraines : 1\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000925701","Surveillance environnementale",null,null,"","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000926101","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000926601","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000926901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000927001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000927301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000927901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000928601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cadmium | Cuivre | Plomb | Zinc","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000928901","Exécution des travaux de réhabilitation","2000-12-13","2002-08-01","Travaux de dépollution du site",null,"N/A","N/A","N/A","N/A","Travaux de dépollution"]
["SSP000929301","Surveillance environnementale","2003-06-01",null,"Résultat de la surveillance à la date du 2003-08-01 : LA SITUATION RESTE STABLE\nCommentaire : Lors de la campagne d'août 2003, un piézomètre a été étudié (AP-PZ3) et la présence en HCT a été détectée à 0,3 mg/L, celle du naphtalène à 0,15 µg/L, celle de l'arsenic à 20 µg/L, celle du baryum à 1500 µg/L et celle du manganèse à 2300 µg/L.\n","Eaux souterraines","N/A","3",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000929801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," .","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Cuivre | Plomb | Zinc","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000930201","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2013-09-12 : LA SITUATION RESTE STABLE\nCommentaire : Situation dégradée depuis la fuite du 17 mars 2011. Une surveillance renforcée et des essais de perméabilité ont été réalisés en conséquence.\r\nDepuis 2011, l'impact est confirmé et la situation reste globalement stable.\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000930801","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2015-10-31 : LA SITUATION RESTE STABLE\nCommentaire : et résultats sur la Seine stables\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000931001","Surveillance environnementale","2007-10-17","2011-12-07","Résultat de la surveillance à la date du 2011-12-07 : LA SITUATION RESTE STABLE\nInformations complémentaires : A l'issue de 14 campagne de surveillance de la nappe, la société Total a fait établir par l'organisme Serpol une synthèse technique d'évaluation des risques (rapport Serpol n°5418-25/15). Ce document recommande l'arrêt de la surveillance compte tenu de l'absence d'impact dans les eaux souterraines. \r\n\r\nL'inspection des installations classées, dans son rapport du 5 décembre 2012 a proposé à monsieur le préfet de la Savoie de faire savoir à l'exploitant que l'obligation de surveiller la nappe est suspendue et de délivrer le récépissé de cessation d'activité à celui-ci. Toutefois, il a été rappelé à l'exploitant qu'en application des dispositions de l'article R.512-66-2 du code de l'environnement, des prescriptions pourrait, le cas échéant lui être imposées pour la protection des intérêts mentionnés à l'article L.511-1 dudit code.\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000931201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage","N/A","N/A","N/A"]
["SSP000931701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de conception des travaux (PCT)","N/A",null,"COHV, solvants chlorés, fréons | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000932101","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2007-10-25 : LA SITUATION RESTE STABLE\nCommentaire : Situation satisfaisante: concentration en PCE < 3\n","Eaux souterraines","N/A","1",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000932101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000932601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," Plan de gestion","Sol - Sous-sol","Plan de gestion","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000932901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000933201","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000933301","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000934201","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)","Ventilation de la zone non saturée (venting)"]
["SSP000934401","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000935001","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2013-01-25 : LA SITUATION RESTE STABLE\nCommentaire : pour chaque dépôt.\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000935201","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","1",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000935701","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000935801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000936301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Arsenic | Baryum","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000936601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de gestion","N/A","Ammonium | Sulfates","Autres éléments minéraux | Paramètres azotés","N/A","N/A","N/A","N/A","N/A"]
["SSP000937201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000937501","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)","Confinement par couverture et étanchéification"]
["SSP000937701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Pompage de rabattement ou de récupération","N/A","N/A","N/A"]
["SSP000938201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Pompage de rabattement ou de récupération","N/A","N/A","N/A"]
["SSP000939401","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2014-03-11 : LA SITUATION RESTE STABLE\nInformations complémentaires : Seul le Mw14 reste impacté par le TCE+PCE à environ 30µg/l tous les autres piézomètres se situe en dessous des valeurs guide de potapilité pour ce paramètre.\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000939601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000939701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Ventilation de la zone non saturée (venting)"]
["SSP000940501","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique","Confinement par couverture et étanchéification"]
["SSP000940701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000941101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"COHV, solvants chlorés, fréons | Radioactifs, isotopes et traceurs","N/A","N/A","N/A","N/A","N/A"]
["SSP000941601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP000941801","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Ventilation de la zone non saturée (venting)"]
["SSP000942601","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000942701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000943001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000943601","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000943901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000944401","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000945001","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000945301","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Piège hydraulique ou Confinement hydraulique"]
["SSP000945701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000945801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000946501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000946601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000947201","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2012-06-19 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","1",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000947801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de gestion","N/A","Chlorures","Autres éléments minéraux","N/A","N/A","N/A","N/A","N/A"]
["SSP000948401","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000949001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP000949201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000949601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000950101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000950201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000951001","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","3",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000951201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000951801","Surveillance environnementale",null,null,"","Eaux souterraines","N/A","1",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000952201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000952701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Pompage de rabattement ou de récupération","N/A","N/A","N/A"]
["SSP000953001","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2014-10-22 : LA SITUATION RESTE STABLE\nCommentaire : Paramètres HCT, nickel et fluorures à suivre.\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000953401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Sulfates | Trichloroéthylène","Autres éléments minéraux | COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP000954001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000954601","Surveillance environnementale",null,null," La surveillance des eaux souterraines est effective depuis le 28/08/2002. Les analyses réalisées sur les eaux souterraines prélevées au droit du site, ne montrent pas d'impact  sur la qualité des eaux souterraines qui sont conformes aux critères de potabilité concernant leurs teneurs en HAP et métaux.","Eaux souterraines","N/A","2",null,"HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000955301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000955501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Trichloroéthylène","COHV, solvants chlorés, fréons | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000955701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Lavage à l'eau"]
["SSP000956201","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Oxydation chimique"]
["SSP000956801","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2010-03-19 : LA SITUATION SE DEGRADE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000956801","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique","Ventilation de la zone non saturée (venting)"]
["SSP000957501","Surveillance environnementale","2006-07-24",null,"Résultat de la surveillance à la date du 2010-03-15 : LA SITUATION RESTE STABLE\nCommentaire : pas de polluants dépassant les valeurs de référenc\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000958301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A","Arsenic | Chrome | Plomb","COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000958501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...) | Pompage de rabattement ou de récupération","N/A","N/A","N/A"]
["SSP000959101","Surveillance environnementale","2003-03-20",null,"Résultat de la surveillance à la date du 2013-12-31 : LA SITUATION SE DEGRADE\nCommentaire : Non satisfaisant\nInformations complémentaires : Présence de propiconazol à de très fortes concentrations sur Pz1, Pz5, le forage et en particulier sur Pz4.\r\nLa présence de lodocarbamate sur le forage en avril 2010 et en octobre 2011 laisse penser que les produits actuellement utilisés peuvent se retrouver dans la nappe.\r\nAvec l'absence de lodocarbamate jusqu'en 2009, la présence de propiconazole pendant cette période sur PZ1, PZ2, PZ3, PZ4 et PZ5 laisse penser que les produits incriminés sont des substances abandonnées par l'exploitant.\r\n\r\nUne seule présence d'IPBC sur le forage le 8 avril 2010 et à une concentration supérieure à la limite de potabilité (0,1 µg/l).\r\n\r\nPrésence de pentachlorophénol (PCP) à des concentrations parfois supérieures à la limite de potabilité (0,1 µg/l), en particulier sur Pz4 et Pz5. \r\nCette pollution est certainement ancienne, car le PCP n'est plus utilisé depuis plusieurs années. Elle provient  probablement du sol où la substance s'est accumulée pendant son utilisation et qui est relarguée par la suite.\r\n\r\nDétection d'hydrocarbures le 21 octobre 2009 dont l'origine est inconnue et dont la nature est du kérosène ou du gazole, d'après une spéciation complémentaire demandée par l'inspection des installations classées. Ils ne sont plus détectés par la suite.\r\n\r\nRapport de synthèse du suivi des eaux souterraines-Décembre 2013 : traces de propiconazole retrouvées dans tous les ouvrages sauf PZ2 et PZ3 situés à l'Est du site. Des traces de pentachlorphénol ont aussi été détectées au droit du PZ1 situé en amont du site par rapport à l'écoulement de la nappe. En avril et décembre 2013, pour l'ensemble des ouvrages impactés, les teneurs observées ont nettement diminué en comparaison avec celles observées en novembre 2012. Lors des 3 dernières campagnes, le piézomètres PZ4 est l'ouvrage qui présente les teneurs les plus importantes.\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000959401","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000959901","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du : 2012-12-03\nRésultat de la surveillance eaux souterraines : 1\nAucune tendance à l'évolution des concentrations ne semble se dessiner\n","Eaux souterraines","N/A","1",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000960201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cuivre | Plomb","COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000960201","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique"]
["SSP000961001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000961301","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000961601","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000961801","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2012-04-03 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000962501","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000963201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000963301","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2007-12-04 : LA SITUATION RESTE STABLE\nCommentaire : Pas d'anomalie hormis un point en arsenic.\nInformations complémentaires : Bilan pluriannuel de la surveillance à effectuer.\n","Eaux souterraines","N/A","3",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000963801","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000963901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés)","N/A","N/A","N/A","N/A","N/A"]
["SSP000964501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000964901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000965201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Trichloroéthylène","COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP000965501","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000965901","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000966401","Surveillance environnementale","2005-01-27",null,"Résultat de la surveillance à la date du 2009-05-25 : LA SITUATION S'AMELIORE\nCommentaire : La surveillance de la qualité des eaux souterraines a fait l'objet d'un allégement acté par l'arrêté préfectoral du 21/02/2008. Il a alors été prescrit des campagnes de suivi des teneurs en COHV trimestrielle et des campagnes semestrielle pour le suivi des concentrations en HCT. \r\n\r\nEn 2007, lorsqu'ils dépassaient le seuil de détection, les hydrocarbures totaux étaient toujours inférieurs à 250 µg/l. En 2008, ils étaient toujours inférieurs au seuil de détection (40 µg/l). Dans ce contexte, l'Inspection des Installations Classées a proposé d'arrêter l'analyse des hydrocarbures totaux dans un courrier au préfet daté du 25/05/2009.\r\n\r\nLes solvants chlorés recherchés sont quant à eux, toujours détectés, en amont comme en aval, sauf le chlorure de vinyle. \r\n\r\nLes concentrations obtenues sont relativement constantes : de l'ordre de 0,5 à 2 µg/l pour le trichloréthylène, de 2 à 20 µg/l pour le tetrachloréthylène, et de 0,1 à 0,5 µg/l pour le dichloréthylène en aval (presque toujours inférieur au seuil de détection en amont).\r\n\r\nÉtant donnée la stabilité de la concentration de ces polluants au fil du temps, l'Inspection des Installations Classées a proposé de poursuivre leur analyse à fréquence semestrielle seulement, avec une analyse en hautes eaux et une analyse en basses eaux.\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000966601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Arsenic | Nickel | Plomb","COHV, solvants chlorés, fréons | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000966601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000967001","Surveillance environnementale","1994-11-25",null,"Résultat de la surveillance à la date du 2004-02-04 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000967501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Sulfates","Autres éléments minéraux | COHV, solvants chlorés, fréons | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000967601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000967901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique","Ventilation de la zone non saturée (venting)"]
["SSP000968301","Surveillance environnementale",null,null,"Informations complémentaires : La surveillance des eaux souterraines est poursuivie.\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000968501","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000968801","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"Une ESR a été réalisée pour chacune des sources de pollutions. Toutes les sources ont été classées 3 à l'exception du sol au voisinage des anciennes forges classé, à surveiller, pour sa teneur en plomb. Actuellement cette zone est recouverte de béton, ce qui limite fortement les risques de transfert de substances polluantes.","Eaux souterraines","Analyse des enjeux sanitaires (EQRS, ARR)","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000969001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de conception des travaux (PCT)","N/A","Arsenic | Chrome | Cuivre | Mercure | Plomb","COHV, solvants chlorés, fréons | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000969401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Mercure | Plomb","Hydrocarbures et indices liés | Metaux et métalloïdes | Phytosanitaires","N/A","N/A","N/A","N/A","N/A"]
["SSP000969701","Surveillance environnementale","2004-01-01",null,"Résultat de la surveillance à la date du 2010-10-01 : LA SITUATION S'AMELIORE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000970101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Sulfates","Autres éléments minéraux","N/A","N/A","N/A","N/A","N/A"]
["SSP000970301","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000970701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000971001","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000971301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000972101","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000972201","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000972501","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Piège hydraulique ou Confinement hydraulique"]
["SSP000972701","Exécution des travaux de réhabilitation","2014-07-04",null,"Traitement de la nappe","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique","Piège hydraulique ou Confinement hydraulique"]
["SSP000973301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000973401","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000973901","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2006-01-16 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000973901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000974401","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000974501","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2006-05-12 : LA SITUATION RESTE STABLE\nCommentaire : les impacts en hydrocarbures et BTEX dans les eaux souterraines sont toujours d'actualité en 2006 (date de la dernière campagne connue).\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000974701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000975201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000975901","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Piège hydraulique ou Confinement hydraulique","Filtration"]
["SSP000976001","Surveillance environnementale","2001-07-01",null,"Résultat de la surveillance à la date du 2016-12-20 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000976101","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique"]
["SSP000976501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000976701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Cadmium | Chrome | Cuivre | Nickel | Plomb | Zinc","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000976801","Exécution des travaux de réhabilitation",null,null," Mise en sécurité",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000977301","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000977501","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2015-10-02 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000977601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000978001","Surveillance environnementale","2002-03-27",null,"Résultat de la surveillance à la date du 2007-01-01 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000978201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Reconditionnement de produits dangereux, Reconditionnement de déchets","N/A","N/A","N/A"]
["SSP000978501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000978901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique"]
["SSP000979001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000979701","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2012-11-09 : LA SITUATION RESTE STABLE\nCommentaire : Pour le secteur 1 (Partie à l'OUEST du chemin de bartenheim(4 puits de surveillance): L'examen de la qualité des eaux souterraines au droit du Puits de contrôle 413-7X-255 (aval immédiat de l'ancienne décharge communale) traduit d'une légère dégradation en Conductivité, Chlorures, Sulfates, Ammonium et HAP.\r\nL'examen de la qualité des eaux souterraines à l'aval hydraulique du secteur 1 , sur les 2 puits 413-7X-183 et 413-7X-184 (bordure aval du site) traduit d'une légère dégradation en :\r\n-- Conductivité, Chlorures, Sulfates mais à des concentrations inférieures aux normes de qualité en vigueur,\r\n-- Ammonium à une concentration légèrement supérieure à la norme de qualité en vigueur.\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000980501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000980801","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000981501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Plomb","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000981701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000981801","Surveillance environnementale","2008-01-15",null,"Résultat de la surveillance à la date du 2012-10-03 : LA SITUATION RESTE STABLE\nCommentaire : Dans le cadre de la surveillance quadriennale, les paramètres recherchés dans les eaux souterraines sont : hydrocarbures C5-C40, BTEX et naphtalène.\r\nLes résultats maximum : 9300 mg/L de HC C5-C40 au droit de P1 au droit des anciennes cuves, 2400 µg/L d'ethylbenzène au droit de P4 en limite de site en aval hydraulique, 380 µg/L de benzène au droit de P1.\nInformations complémentaires : Trois « aquifères » sont mis en évidence : un aquifère faiblement productif au niveau de l’ancienne station service (3,5 m de profondeur), un aquifère libre au sud de l’ancienne station service (5 m de profondeur), un aquifère captif au sud-est de l’ancienne station service (2,3 m de profondeur).\r\n\r\nLe sens d’écoulement général des eaux souterraines se fait en direction du nord à nord-ouest. La présence de lentilles argileuses rend complexe la circulation des eaux souterraines. A 10 m de profondeur, sous un autre niveau argileux, sont présentes des nappes apparemment captives. \r\n\r\nD'après les campagnes piézométriques, la nappe a été rencontrée entre 2 et 5 mètres de profondeur et s'écoule vers le nord à nord-ouest. Mais en raison de la destruction de certains ouvrages sur le site, notamment ceux situés en aval hydraulique de l'ancienne station-service, il n'est pas évident d'affirmer le sens d'écoulement. En avril 2011, le sens d'écoulement, stables depuis les relevés précédents, était orienté en direction du nord-ouest.\r\n\r\n5 ouvrages ont fait l'objet de prélèvements : 3 ouvrages localisés sur site et en limite de site (P1, P4 et PZ6), ainsi que 2 ouvrages hors site (PZ10 et PZ11). Les ouvrages sont localisés comme suit : P1 au droit des anciennes cuves, P2 , P3, P4, P5 et PZ6 en limite de site en aval hydraulique, PZ10 et PZ11 hors site, en aval hydraulique.\r\n\r\nLes résultats des analyses montrent que les concentrations en BTEX et hydrocarbures dissous relevées au droit de l'ancienne station se maintiennent à des teneurs inférieures aux valeurs limites de l'EDR. Le dépassement limité et ponctuel (480 µg/L en benzène) qui avait été constaté sur l'ouvrage PZ3 en avril 2011 n'a pas pu être contrôlé car l'ouvrage (comme PZ2, PZ3, PZ4, PZ7, PZ8, PZ9, PZ'1, PZ'2, PZ'3, S5 et S7) a été détruit au cours des travaux de modernisation du site.\r\n\r\nGlobalement, en ce qui concerne les piézomètres encore accessibles, les concentrations mesurées sont stables par rapport à la campagne de référence du 15 janvier 2008. A noter toutefois, une légère tendance à la hausse observée sur la campagne du 3 octobre 2012, au niveau des ouvrages au droit ou en limite de l'emplacement de l'ancienne station-service, mais une tendance à la baisse au niveau de ceux hors site en aval. \n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000981901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000982301","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP000983101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Plomb | Trichloroéthylène","COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000983101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000983801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000984301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Chrome","HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000984901","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000985001","Surveillance environnementale","2005-03-03","2008-04-30","Résultat de la surveillance à la date du 2008-04-30 : LA SITUATION RESTE STABLE\nCommentaire : Les concentrations en COHV restent stables sur l'ensemble des campagnes de suivi réalisées sur le site. Lors de la dernière campagne du mois de mars 2008, la concentrations en TCE+PCE atteignait 36.4 µg/l tandis que la concentration en Tétrachlorométhane s'élevait à 160 µg/L. \r\nCette pollution des eaux n'étant pas imputable à la société NEYRTEC ALSTOM, le bureau d'étude NORISKO Envmt a recommandé l’arrêt du suivi de la qualité des eaux souterraines.\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000985901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000986001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP000986301","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000986401","Surveillance environnementale","2004-01-20",null,"Résultat de la surveillance à la date du : 2015-07-31\nRésultat de la surveillance eaux souterraines : 1\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000986801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"COHV, solvants chlorés, fréons | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000987001","Exécution des travaux de réhabilitation","2013-06-18",null," Entre 2013 et 2017, plusieurs inspections ont été effectuées sur le site. Elles ont notamment conduit à engager une procédure de consignation de sommes à l’encontre du propriétaire terrains, en sa qualité de détenteur des déchets, par arrêté préfectoral du 13 décembre 2017 ; les tas de sables étant encore présents sur le site et sans protection efficace (bâches arrachées et détériorées par endroits).",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000987501","Surveillance environnementale",null,null,"","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000987701","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2015-06-22 : LA SITUATION RESTE STABLE\nCommentaire : Les teneurs en hydrocarbures, DCO, Etain, Toluène, MDI et TDI sont sous le seuil de quantification.\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000988401","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP000988501","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Piège hydraulique ou Confinement hydraulique | Ventilation de la zone non saturée (venting)"]
["SSP000989101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Arsenic | Nickel | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Sulfates","Autres éléments minéraux | Benzène et dérivés | COHV, solvants chlorés, fréons | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000989201","Surveillance environnementale","2003-06-01",null,"Résultat de la surveillance à la date du 2009-10-06 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000989301","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Ventilation de la zone non saturée (venting)"]
["SSP000989701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000990201","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique"]
["SSP000990901","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Piège hydraulique ou Confinement hydraulique"]
["SSP000991001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP000991101","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP000991401","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP000991701","Surveillance environnementale","2005-07-20",null,"Résultat de la surveillance à la date du 2010-08-09 : LA SITUATION S'AMELIORE\nCommentaire : Les résultats de la campagne du 09/08/2010 n'ont pas révélé d'anomalie dans les concentrations de cyanures dans les eaux souterraines.\nInformations complémentaires : Au vu des résultats de la dernière campagne de prélèvement des eaux souterraines, l'inspection des installations classées propose au Préfet de rendre caduc l'arrêté préfectoral du 27/05/2010.\n","Eaux souterraines","N/A","3",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000991901","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP000992201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000992401","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage | Interdiction d'accès (clôture...) | Pompage de rabattement ou de récupération","N/A","N/A","N/A"]
["SSP000992701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Ventilation de la zone non saturée (venting)"]
["SSP000992901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)","Confinement par couverture et étanchéification"]
["SSP000992901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000993201","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000993501","Surveillance environnementale","2001-03-08",null,"Résultat de la surveillance à la date du 2012-10-23 : LA SITUATION SE DEGRADE\n","Eaux souterraines","N/A","1",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000993701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000994301","Surveillance environnementale","2003-04-02",null,"Résultat de la surveillance à la date du 2015-10-29 : LA SITUATION SE DEGRADE\nCommentaire : Propiconazole supérieur à la norme sur PZ3 (piézo aval).\nInformations complémentaires : Présence de propiconazole depuis avril 2010 à des teneurs supérieures à la limite de potabilité (0,1 µg/l) sur les piézomètres à l'aval du site. Toutefois, aux dernières analyses effectuées en mars 2013, il n'y a plus de traces de propiconazole sur le PZ3(aval), mais la teneur en propiconazole est toujours supérieure à la valeur limite dans le PZ1(aval).\r\n\r\nDétection ponctuelle d'hydrocarbures sur l'ensemble des piézomètres : jusqu'en octobre 2011 sur PZ2 (amont)et jusqu'en avril 2010 sur PZ1 (aval). Depuis lors, les teneurs en hydrocarbures sont inférieures au seuil de détection.\r\n\r\nAbsence de détection de TCMTB et de carbendazime. Arrêt de leur analyse en novembre 2009.\r\n\r\nRapport des analyses piézométriques de mars 2013 :\r\n- plus de traces de propiconazole sur le Pz2(amont) et le Pz3 (aval),\r\n- sur le Pz1 (aval) : teneur propiconazole (17 ug/l) > valeur limite (2 ug/l).\r\n\r\nRapport analyses piézométriques de novembre 2013 :\r\n- sur le Pz1 (aval), la teneur en propiconazole (3 ug/l) est toujours > à la valeur limite (2 ug/l) ; \r\n\r\nCourriel de l'IIC à l'exploitant le 20/08/2014 demandant des explications sur cette non conformité.\r\n\r\nNouvelles analyses des eaux souterraines réalisées en avril 2014 et transmises par l'exploitant le 06/08/2014 : la teneur en propiconazole en Pz1 (6,4 ug/l) reste au dessus de la valeur seuil. L'exploitant indique qu'une vidange du bac de traitement sera réalisée pendant les congés d'août afin d'analyser le bon état de celui-ci. Une vérification approfondie de la cuvette de rétention sera aussi réalisée.\r\nAnalyses réalisées en octobre 2014 : Propiconazole supérieur à la norme sur les piézos aval : PZ1 (6,4 ug/l) et PZ3 (6 ug/l). Explications de l'exploitant : une cause possible de cette augmentation en propiconazole peut être liée au débordement du bac de trempage. Afin d'éviter cet incident, il prévoit les aménagements suivants :mise en place d'un capteur de niveau haut dans le bac de trempage afin d'arrêter le remplissage d'eau et d'un capteur de niveau très haut qui actionne une alarme sonore et arrête la centrale hydraulique de descente de la palette + mise en place d'un capteur de niveau dans la cuvette de rétention qui actionne une alarme sonore.\r\n\r\nAnalyses d'avril 2015 : propiconazole en baisse (0,14ug/l) sur le PZ3, mais en augmentation de 6,4ug/l à 11ug/l sur le PZ1. L'IPBC, pour lequel une analyse avait été demandée, ne sera analysé que lors de la prochaine campagne du second trimestre 2015.\r\n\r\nPrélèvements du 29/10/2015 : Teneur élevée en Propiconazole sur le PZ3 (8,3 ug/l) ; Présence persistante de propiconazole sur le PZ1 avec baisse teneur sur le dernier prélèvement (avr-2015: 11ug/l ; sept-2015: 1,4ug/l).\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000994501","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP000994601","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"En juin 2002 et en octobre 2004, des campagnes d'analyses, portant sur la teneur en plomb, des eaux et des sédiments du ruisseau du Château et de l'Aroffe ont été effectuées. Ces mesures ont montré que le eaux sont conformes aux critères de potabilité. En revanche, une contamination des sédiments par du plomb a été détectée en aval immédiat de la verrerie ; cette pollution est localisée sur quelques mètres au niveau du point de rejet de l'usine dans le ruisseau du château. Les analyses effectuées en aval n'ont pas révélé de contamination. ","Eaux superficielles - Sédiments","Diagnostic et Analyse","N/A","Plomb","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000994801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"Phytosanitaires","N/A","N/A","N/A","N/A","N/A"]
["SSP000995001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000995701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Molybdène","COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000995801","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Ventilation de la zone non saturée (venting)"]
["SSP000996101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic","HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000997201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cadmium | Cuivre","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP000997801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP000998401","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP000999401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Trichloroéthylène","COHV, solvants chlorés, fréons | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP000999601","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2005-01-01 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001000501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001000701","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique","Piège hydraulique ou Confinement hydraulique | Ventilation de la zone non saturée (venting)"]
["SSP001000901","Surveillance environnementale","2003-03-20",null,"Résultat de la surveillance à la date du 2015-10-02 : LA SITUATION RESTE STABLE\nCommentaire : Absence de dégradation de la qualité des eaux souterraines ; diminution sensible de la concentration en propiconazole au droit du PZ2.\nInformations complémentaires : La majeure partie des substances analysées, dont les substances actives des produits de traitement, ne sont pas détectées.\r\n\r\nLa présence récurrente de zinc et de plomb dans les eaux souterraines reste inexpliquée, car ils ne sont pas présents dans les produits utilisés par le passé et au moment de la rédaction du rapport par la Scierie LABADIE, d'après le rapport de surveillance du 18 octobre 2012.\r\n\r\nA noter la présence de cuivre sur le PZ1 le 15 décembre 2009 et de chrome sur le PZ3 le 06 décembre 2011 qui n'a pas été expliqué.\r\n\r\nLa campagne de prélèvements et d'analyses des eaux souterraines de février 2014 révèle la présence de Propiconazole :\r\n- sur le Pz3 (aval) lors du prélèvement effectué en octobre 2013 (0,28 ug/l). En février 2014, la présence de cette substance n'est pas identifiée ;\r\n- sur le Pz2 (aval) lors du prélèvement effectué en février 2014 (0,87 ug/l).\r\n\r\n22/08/2014 : Courrier IIC à l'exploitant, lui demandant  :\r\n. de justifier l'apparition du Propiconazole dans les eaux souterraines (substance non identifiée jusqu'alors), \r\n. de rechercher également les matières suivantes : Tébuconazole et Cyperméthrine, lors des prochaines campagnes d'analyses.\r\n\r\n28/12/2014 : Prélèvements effectués en octobre et décembre 2014 : hausse importante des valeurs en Propiconazole sur le PZ2 aval (13ug/l) en octobre et de la contre-analyse réalisée en décembre qui identifie 0,88ug/l (valeur qui se rapproche des mesures effectuées en février 2014).\r\n\r\n30/04/2015 : L'ensemble des éléments recherchés vérifie l'absence de dégradation de la qualité des eaux souterraines. La présence non significative de Propiconazole sur le PZ2 (1,8 ug/l) devra toutefois faire l'objet d'une attention particulière.\r\n\r\n02/10/2015 : pas de dégradation de la qualité des eaux souterraines ; diminution sensible de la concentration en Propiconazole sur le PZ2 (0,25 ug/l).\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001001901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP001002501","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2007-05-10 : LA SITUATION RESTE STABLE\nCommentaire : Satisfaisant\r\nAucun élément polluant détecté\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001002801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Nickel | Zinc","HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001003101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés","N/A","N/A","N/A","N/A","N/A"]
["SSP001003201","Surveillance environnementale","2005-02-23",null,"Résultat de la surveillance à la date du 2016-05-23 : LA SITUATION RESTE STABLE\nCommentaire : Propiconazole stable - Diminution du Bore\nInformations complémentaires : La campagne du 4 mai 2009 (hautes eaux) montre toujours la présence de propiconazole sur les 3 piézomètres mais à des valeurs encore plus faibles : de 0,3 à 1,2 microgramme/l. La recherche de carbendazime est arrêtée, le propiconazole étant un meilleur élément traceur. \r\n\r\nLe SINESTO B étant le nouveau produit de traitement utilisé depuis le 01/01/2008, ce composé organique a été recherché sous l'appellation substance Sinesto. Il a été mesuré à une teneur comprise entre 1,05 et 2,06 microgramme/l sur les 3 piézomètres. Le bore est détecté sur PZ1 (70 microgramme/l) et PZ3 (28 microgramme/l).\r\n\r\nAu cours de la campagne du 14 décembre 2009, le propiconazole (qui n'est plus utilisé depuis 2 ans) continu à être détecté à des valeurs fluctuantes : de 0,62 microgramme/l sur le PZ1 amont à 3,01 sur PZ2 et 2,99 microgramme/l sur le PZ3. Le chlorure de triméthylcocoammonium (substance active du nouveau produit SINESTO) n'est pas détecté. Le bore présent sous forme de tétraborate de sodium dans le sinesto est détecté sur PZ1 (51 microgramme/l) et PZ3 (32 microgramme/l).\r\n\r\nAu cours de la campagne du 18 avril 2011, le propiconazole n'a pas été mesuré. Le bore a été détecté sur les trois piézomètres (Pz1 = 38.1 µg/l; PZ2 = 29.9 µg/l; PZ3= 63.7 µg/l). Aucune trace de triméthylcocoammonium n'a été détectée.\r\n\r\nLa campagne du 14 septembre 2011 révèle des traces de propiconazole sur les trois piézomètres (Pz1 = 0.176 µg/l; PZ2 = 0.39 µg/l; PZ3= 0.326 µg/l). Le bore a été détecté sur les trois piézomètres (Pz1 = 53.8 µg/l; PZ2 = 43.3 µg/l; PZ3= 129 µg/l. Aucune trace de triméthylcocoammonium n'a été détectée, de même pour la campagne de mars 2012.\r\n\r\nLes campagne de l'année 2012 révèle des traces de propiconazole sur les trois piézomètres (Pz1 = 0.062 µg/l; PZ2 = 0.023 µg/l; PZ3= 0.41µg/l). Le bore a été détecté sur les trois piézomètres (Pz1 = 58 µg/l; PZ2 = 36 µg/l; PZ3= 110 µg/l. On note une baisse des paramètres. Aucune trace de triméthylcocoammonium n'a été détectée.\r\n\r\nLa campagne du premier semestre 2013 met toujours en avant des traces de propiconazole mais à des valeurs inférieures aux valeurs seuils.\r\n\r\nRésultats de la campagne du 26/03/2014 : baisse des teneurs en propiconazole dans les 3 piézomètres et baisse de la teneur en Indice hydrocarbures dans le Pz3 ; Bore en augmentation dans le Pz1 (73 ug/l) par rapport aux valeurs de 2012 et 2013 (la teneur maxi relevée au 1er semestre 2013 : 62 ug/l).\r\nCampagne du 09/09/2014 : Bore en augmentation dans le Pz1 (78 ug/l), teneur en propiconazole en augmentation dans les 3 piézomètres ; Baisse Indice Hydrocarbures (< 0,05 mg/l) dans les 3 piézomètres.\r\n\r\nCampagne du 30/09/2015 : diminution de la teneur en Bore dans les 3 piézomètres, mais augmentation du propiconazole, plus importante dans le Pz2 (0,168 ug/l).\r\n\r\nCampagne du 31/03/2016 : diminution du propiconazole dans le Pz2 (0,082 ug/l) mais augmentation dans le Pz1 (0,365 ug/l) ; diminution de la teneur en Bore  dans les 3 piézomètres.\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001004401","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP001004601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"Phytosanitaires","N/A","N/A","N/A","N/A","N/A"]
["SSP001005101","Surveillance environnementale","2003-09-30",null,"Résultat de la surveillance à la date du 2015-11-17 : LA SITUATION SE DEGRADE\nCommentaire : les résultats montrent un dépassement de la valeur limite de qualité en propiconazole sur les piézomètres PZ1 et PZ2\nInformations complémentaires : Recommandations :\r\n- La surveillance devra être maintenue pour le propiconazole lors des prochaines campagnes (semestrielles)\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001005601","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2013-03-26 : LA SITUATION RESTE STABLE\nCommentaire : Satisfaisant\nInformations complémentaires : Aucune anomalie n'a été mise en évidence au cours de la dernière campagne. L'ensemble des ouvrages ne présente pas de traces d'hydrocarbures ni de pesticides. Les concentrations des molécules recherchées sont inférieures aux Limites de Quantification des Méthodes analytiques du laboratoire.\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001007101","Surveillance environnementale",null,"2005-09-28","Résultat de la surveillance à la date du : 2005-09-28\nRésultat de la surveillance eaux souterraines : 1\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001008801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001009001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001009401","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001009901","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique","Confinement par couverture et étanchéification | Piège hydraulique ou Confinement hydraulique"]
["SSP001010401","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique","Piège hydraulique ou Confinement hydraulique","Filtration"]
["SSP001011101","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2012-12-31 : LA SITUATION RESTE STABLE\nCommentaire : Teneurs assez fortes en manganèse, sulfates, chlore et sodium.\nInformations complémentaires : Teneurs assez fortes en manganèse, qui sont au dessus de la limite de potabilité (50 µg/l) : constamment pour F1, F2, F3, Pz1 et régulièrement pour Pz2.\r\n\r\nTeneurs assez fortes en sulfates pour les piézomètres Pz4 et Pz5, souvent supérieures à la limite de potabilité (250 mg/l), excepté en novembre 2012.\r\n\r\nTeneurs assez fortes en chlore et sodium constamment sur Pz5 et de temps en temps sur Pz1 et Pz4.\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001011801","Surveillance environnementale",null,null,"","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001012101","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP001012901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001013501","Surveillance environnementale","2004-10-15",null,"Résultat de la surveillance à la date du 2012-11-26 : LA SITUATION RESTE STABLE\nInformations complémentaires : La campagne du 26/09/2012 montre la présence de métaux dans la nappe de surface et l'eau du fossé. En Novembre 2012, des PCB sont mesurés à l'état de traces (somme des 7 PCB 0,091 µg/l), proches de la limite de détection, en un point aval du fossé.\r\n\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001013901","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2010-08-31 : LA SITUATION S'AMELIORE\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001014201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | COHV, solvants chlorés, fréons | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001014501","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2006-07-05 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","1",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001014801","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP001015101","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP001015301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001016001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Cadmium | Chrome | Cuivre | Mercure | Nickel | Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Zinc","Benzène et dérivés | COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001016101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Trichloroéthylène","COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP001016701","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP001017101","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001017301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Cadmium | Cobalt | Cuivre | Nickel | Plomb | Zinc","COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001017401","Surveillance environnementale","2007-03-26",null,"Résultat de la surveillance à la date du 2010-03-15 : LA SITUATION S'AMELIORE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001017801","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,null,"Filtration"]
["SSP001018001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage","N/A","N/A","N/A"]
["SSP001019501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Chrome | Cuivre | Molybdène | Nickel","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001020401","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2017-11-09 : LA SITUATION SE DEGRADE\nCommentaire : Le suivi des eaux souterraines met en évidence la présence d'un impact en hydrocarbures au droit de l'ouvrage PZ8 depuis novembre 2016. Depuis juin 2017, des teneurs importantes sont également mesurées au droit de l'ouvrage PZ1 alors que les teneurs étaient inférieures au seuil de détection en juin et novembre 2016. Depuis juin 2016, les concentrations en hydrocarbures au droit des ouvrages PZ2 et PZ4 sont inférieures au seuil de détection ou faibles.\nInformations complémentaires : Les résultats d'analyses d'eaux souterraines de la campagne de novembre 2017 mettent en évidence un impact en hydrocarbures au droit des ouvrages PZ1 et PZ8 avec :\r\n- une teneur importante de 2400 µg/L au droit de PZ1,\r\n- la présence de gouttelettes de surnageant au droit de PZ8. les autres ouvrages présentent des concentrations négligeables ou inférieures au seuil de détection (la zone au droit de l'ouvrage PZ8 fait l'objet d'un dispositif de dépollution avec un système d'écrémage de la phase flottante).\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001020501","Surveillance environnementale",null,null,"Informations complémentaires : La situation reste stable mis à part la teneur en benzène qui demeure très supérieure aux valeurs de la VCI pour un usage non sensible. C'est un paramètre qu'il est important de suivre de près et d'en comprendre l'origine exacte. La mise en place de piézomètres supplémentaires près des zones où les teneurs en benzène sont importantes est actuellement en discussion. La mise en place de ce réseau de surveillance  supplémentaire permettra de pouvoir cibler de façon plus précise la source du polluant et ainsi de mieux la gérer. \r\n\r\nLe schéma conceptuel prévu en 2011 permettra d'avoir une vision globale de la problématique de pollution des sols liée en particulier au benzène au niveau de la plateforme pétrochimique (ESSO et EMCP).\r\nL'unité PP est arrêté depuis 2010.\r\nPar ailleurs, les  éléments du paragraphe C «description qualitative » seront intégrés dans le schéma conceptuel de la plateforme(surtout par rapport au benzène).\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001021501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A","Arsenic | Plomb","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001021701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de conception des travaux (PCT)","N/A","Cyanures libres","Autres éléments minéraux | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001022201","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001022701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Ventilation de la zone non saturée (venting)"]
["SSP001023201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Trichloroéthylène","COHV, solvants chlorés, fréons | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF) | Phytosanitaires","N/A","N/A","N/A","N/A","N/A"]
["SSP001023401","Surveillance environnementale",null,null,"Commentaire : HC non détecté- benzène et xylènes  détectés\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001024101","Surveillance environnementale","2006-06-18",null,"Résultat de la surveillance à la date du 2006-09-28 : LA SITUATION RESTE STABLE\nInformations complémentaires : Les résultats d'analyses de la campagne de septembre 2006 montrent :\r\n- 310 µg/L d'HCT au droit de PP1 ;\r\n- 34 µg/L de benzène au droit de PP1 ;\r\n- 150 µg/L de MTBE au droit de PP2.\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001024101","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique"]
["SSP001024901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP001025201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP001025801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001026101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001026601","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP001027401","Exécution des travaux de réhabilitation",null,null," Terrain clôturé par un bardage de chantier",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001027601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A",null,"HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001028701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP001029401","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001029901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001030101","Exécution des travaux de réhabilitation",null,null," rapport de fin de travaux référencé CU8426/JL174-3R de juillet 2008","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP001030701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP001030801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A","Arsenic | Cadmium | Chrome | Cuivre | Mercure | Nickel | Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Trichloroéthylène | Zinc","Benzène et dérivés | COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001031101","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Ventilation de la zone non saturée (venting)"]
["SSP001031201","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2011-05-16 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001032001","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP001032701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001033601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001033801","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP001034701","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP001034901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001035901","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP001036101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Plomb","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001037201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Arsenic | Cobalt | Nickel | Plomb","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001037801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Chrome | Cuivre | Mercure | Plomb | Zinc","COHV, solvants chlorés, fréons | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001037901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," Diagnostic et analyse","Sol - Sous-sol","Diagnostic et Analyse","N/A","Zinc","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001038201","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP001038801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP001038901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP001039001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP001039501","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"   ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP001039701","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001041401","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP001041601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001041801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de conception des travaux (PCT)","N/A","Trichloroéthylène","COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP001042401","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2014-11-15 : LA SITUATION S'AMELIORE\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001042701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"COHV, solvants chlorés, fréons | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001043201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de gestion","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | COHV, solvants chlorés, fréons | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001043401","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP001043501","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Ventilation de la zone non saturée (venting)"]
["SSP001044201","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP001044401","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique"]
["SSP001044901","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP001046101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Chrome | Trichloroéthylène","COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001046101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Chrome | Trichloroéthylène","COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001046701","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Piège hydraulique ou Confinement hydraulique | Ventilation de la zone non saturée (venting)"]
["SSP001046701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001047201","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)","Confinement par couverture et étanchéification"]
["SSP001047401","Surveillance environnementale","2009-05-01","2013-12-01","Résultat de la surveillance à la date du 2014-09-10 : LA SITUATION RESTE STABLE\nCommentaire : Les HCT n'ont pas été détectés sur les PZ1, PZ2 et Pz5.\r\nPar ailleurs, il a été constaté que l'épaisseur des flottants a augmenté sur PZ4. Il est préconisé d'effectuer un écrémage par semaine par préleveur jetable jusqu'à disparition du flottant, puis de réduire la fréquence à un écrémage par mois comme initialement indiqué dans l'arrêté du 22/03/2010.\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001048101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Cuivre | Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001048101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP001049101","Surveillance environnementale","2003-11-20",null,"Résultat de la surveillance à la date du 2007-07-15 : LA SITUATION SE DEGRADE\nCommentaire : non satisfaisant DCO\n","Eaux souterraines","N/A","1",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001049401","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2016-09-22 : LA SITUATION RESTE STABLE\nCommentaire : présence récurrente de \r\ntrichloroéthyléne,tétrachloroéthylène et chlorure de vinyl en aval du site\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001049701","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"Les études réalisées depuis 2007 ont mis en évidence les pollutions suivantes :\n- pollution par les solvants chlorés des sols de l'ancien atelier de nettoyage à sec ;\n- pollution par les solvants chlorés des sols de l'atelier de nettoyage à sec de linge plat ;\n- pollution localisée en hydrocarbures (HC) et hydrocarbures aromatiques polycyliques (HAP) des sols de la zone de stockage des cuves d'huiles et d'hydrocarbures.\nA noter que le terrain a fait l'objet en partie de remblais dont les pollutions ne peuvent être attribuées aux activités précédemment exercées sur le site (pollution hydrocarbures et arsenic).\n\nConcernant les eaux souterraines, des traces d’hydrocarbures ont été mises en évidence (teneurs inférieures aux valeurs de gestion couramment utilisées) et des composés organiques halogénés volatils (COHV) présentent des teneurs supérieures aux valeurs de gestion couramment utilisées.","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001049801","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP001050301","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001051001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de gestion","N/A","Arsenic","COHV, solvants chlorés, fréons | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001051401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001051601","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Barbotage in situ (sparging) | Ventilation de la zone non saturée (venting)"]
["SSP001051801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001052001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001052401","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique"]
["SSP001052501","Surveillance environnementale","2009-01-07",null,"Résultat de la surveillance à la date du 2009-09-30 : LA SITUATION RESTE STABLE\nCommentaire : absence d'impact notable sur la nappe\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001052901","Surveillance environnementale","2003-04-02",null,"Résultat de la surveillance à la date du 2013-10-27 : LA SITUATION S'AMELIORE\nCommentaire : Absence d'impact PCP et HCTX\nInformations complémentaires : La campagne 02/2005 ne montre pas de transfert de polluant dans la nappe.\r\n\r\nles résultats de la campagne du 27 octobre 2007 sont satisfaisants ( PZ1 : pH 5; conductivité 256; PZ2 : pH 4,9; conductivité 255 ; forage aval : pH 6,7; conductivité 192). Absence d'impact par HCT et PCP pour les 3 piézomètres.\r\n\r\nLa campagne 27 mars 2008 montre l'absence d'impact au niveau du Pz1, mais des traces de pentachlorophénols sont détectées dans le forage (0,9 µg/l).En l'absence de relevé des niveaux piezométriques, il est difficile de connaître le sens d'écoulement de la nappe, le Pz1 serait en aval et le forage en aval latéral.\r\n\r\nLa campagne 29/10/2009 montre l'absence d'impact par les PCP(<0,5 µg/l) et les hydrocarbures totaux (< 0,05 mg/l).\r\n\r\nLa campagne du 15/04/2010 montre l'absence d'impact sur les eaux souterraines au droit du site. Le sens d'écoulement de la nappe est de PZ2 vers PZ1. \r\n\r\nLa campagne du 27/10/2010 confirme la situation satisfaisante sur les 3 Piézos (hydrocarbures <0,05mg/l et PCP <0,1µg/l)\r\n\r\nLes campagnes du 3 mai 2011 et mars 2012 confirment la situation satisfaisante, aucun impact n'est observé au droit des piézomètres.\r\n\r\nMême constat pour le premier et le deuxième semestre 2013: aucune pollution n'a été détectée.\nDate de fin envisagée de la surveillance : 2011-06-30","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001053401","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP001053801","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP001054001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP001054601","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP001054801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Interprétation de l''état des milieux (IEM)","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001055601","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique"]
["SSP001055801","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP001056401","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Ventilation de la zone non saturée (venting)"]
["SSP001056801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cuivre | Plomb | Trichloroéthylène | Zinc","COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001056901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001057101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001057501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001058001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP001058501","Surveillance environnementale","2008-01-16",null,"Résultat de la surveillance à la date du 2014-05-16 : LA SITUATION RESTE STABLE\nCommentaire : - surveillance sur le site en aval (site STOCKMEIER) depuis fin 2004.\r\n- surveillance sur le site BODYCOTE depuis début 2008\nInformations complémentaires : Le puits de contrôle Amont Pz0545 ne traduit pas de pollution en solvants chlorés.\r\n\r\nLe puits Aval Pz 0547 (angle Nord-Est du site) met en évidence la présence de:\r\n- PCE: faibles concentrations (0,7 µg/l en Mai 2010, 2,58µg/l en Mai 2013 et 0,9 µg/l en Novembre 2013),\r\n- TCE: faibles concentrations (0,5 à 1,6 µg/l).\r\n\r\nLe puits Aval médian Pz0546 met en évidence la présence de :\r\n- PCE: des concentrations très fluctuantes et parfois proches ou supérieures à la norme de potabilité ( 13 µg/l en Janvier 2008; 44,8 µg/l en Mai 2010; 31 µg/l en Novembre 2013),\r\n- TCE: des concentrations très fluctuantes et parfois proches ou supérieures à la norme de potabilité ( 25 µg/l en Octobrer 2008; 20,40 µg/l en Novembre 2009).\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001058601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001058901","Exécution des travaux de réhabilitation",null,null," .","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP001059301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Arsenic | Cadmium | Cuivre | Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Zinc","Benzène et dérivés | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001059601","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP001060101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Arsenic | Plomb | Sulfates | Zinc","Autres éléments minéraux | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001060601","Surveillance environnementale","2007-09-01",null,"Résultat de la surveillance à la date du 2008-09-12 : LA SITUATION RESTE STABLE\nCommentaire : Absence hydrocarbure et cadmium\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001060701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001062301","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP001062401","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP001062901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001063201","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Ventilation de la zone non saturée (venting)"]
["SSP001064101","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2010-03-17 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001064501","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Lavage à l'eau"]
["SSP001065001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP001065601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," analyses sur les eaux souterraines de septembre 2020 et mars 2021","Eaux souterraines","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001066301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," -","Eaux souterraines","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | COHV, solvants chlorés, fréons | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001066601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001066901","Surveillance environnementale","1999-03-23",null,"Résultat de la surveillance à la date du 2015-01-14 : LA SITUATION S'AMELIORE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001067301","Surveillance environnementale","2009-03-10",null,"","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001067701","Surveillance environnementale",null,null,"","Eaux souterraines","N/A","1",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001068501","Exécution des travaux de réhabilitation",null,null," -","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Piège hydraulique ou Confinement hydraulique"]
["SSP001069101","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique","Confinement par couverture et étanchéification"]
["SSP001069301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de conception des travaux (PCT)","N/A",null,"COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP001070001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001070101","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP001070601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Cuivre | Mercure | Nickel | Zinc","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001070701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Pompage de rabattement ou de récupération","N/A","N/A","N/A"]
["SSP001071201","Surveillance environnementale","2011-11-24",null,"Résultat de la surveillance à la date du 2014-04-16 : LA SITUATION S'AMELIORE\nCommentaire : Présence de dichloroéthylène et trichloroéthane.\nInformations complémentaires : Analyses du 16 avril 2014\r\nLes niveaux sont en hausse (en comparaison de la campagne précédente de septembre 2013) et sont supérieurs à ceux de la campagne de « hautes-eaux » précédentes (avril 2013).\r\nLes teneurs en Hydrocarbures Totaux et CAV (dont BTEX) se maintiennent inférieures aux seuils de quantification du laboratoire pour l’ensemble des ouvrages.\r\nEn comparaison de la campagne de hautes-eaux précédente, une hausse relative à modérée des teneurs en cis-1,2-dichloroéthylène et 1,1,1-trichloroéthane (Pz6 uniquement) en relation avec les fortes précipitations du premier semestre 2014 ayant probablement entrainées une remobilisation locale d’une contamination résiduelle dans des terres habituellement hors d’eau. Les autres composés organiques volatiles montrent une tendance à la baisse.\r\nNotons que les teneurs mesurées montrent une tendance globale à la baisse de ces paramètres au cours du temps, et qu’aucun dépassement des seuils de potabilité (arrêté du 11/07/2007) n’est observé.\r\n\r\nAnalyses du 26 septembre 2013\r\nSur les piézomètres pour lesquels le trichloréthylène et/ou le tétrachloréthylène étaient analysés dans les campagnes antérieures, une tendance globale à la baisse des teneurs est observable.\r\nAucune trace de composés Aromatiques Volatils (CAV)n’a été identifiée sur l’ensemble des ouvrages.\r\nAbsence de détection des hydrocarbures.\r\n\r\nAnalyses d'avril 2012\r\nPrésence de trichloréthylène à des concentrations globalement en légère baisse (à confirmer pendant la suite de la surveillance) et inférieures à 20 µg/l (la valeur guide de l'OMS) sur les piézomètres Pz6, Pz16 (non détecté en avril 2012), Pz17 et Pz18.\r\n\r\nAbsence de détection de tétrachloréthylène en avril 2012, suite à une augmentation des concentrations sur Pz6, Pz16 et Pz18 en octobre 2011 par rapport à mai 2011.\r\n\r\nAbsence de détection de Composés Aromatiques Volatils (CAV).\r\n\r\nRésultats sur la base des prélèvements et analyses réalisées au droit des piézomètres depuis 2007 :\r\nAbsence de détection des hydrocarbures, excepté en août 2007 et en octobre 2009 sur Pz2 et Pz17 à des concentrations inférieures aux limites de qualité des eaux brutes.\r\n\r\nLes résultats des 8 campagnes (4 ans entre 2011 et 2014) de surveillance de la qualité\r\ndes eaux souterraines au droit du site de l’ancienne usine THYSSENKRUPP SOFEDIT\r\nd’Arudy (64), montrent :\r\n• Le maintien d’une direction principale d’écoulement des eaux souterraines vers\r\nl’est, et des variations des niveaux d’eau saisonnières ;\r\n• des teneurs en Hydrocarbures Totaux et CAV (dont BTEX) au droit des 5\r\npiézomètres qui se maintiennent inférieures aux seuils de quantification du\r\nlaboratoire pour l’ensemble des ouvrages ;\r\n• Une tendance globale à la baisse des teneurs en COHV (PCE et TCE\r\nprincipalement) avec l’absence de dépassement des seuils de potabilité (arrêté\r\ndu 11/07/2007) depuis avril 2011 pour ces 2 composés.\r\nAu cours du suivi quadriennal, la surveillance de la qualité de la nappe a permis de\r\nmettre en avant l’absence d’impact nécessitant la mise en place de mesures de gestion\r\ncomplémentaires particulières.\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001071501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP001072301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Cadmium","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001072401","Surveillance environnementale",null,null,"Dans le cadre de l'arrêté préfectoral du 11 juin 2010, l'exploitant a réalisé une surveillance semestrielle des eaux souterraines entre 2010 et 2012. Cette surveillance a mis en évidence des dépassements des valeurs de référence utilisées (valeurs issue de l'arrêté ministériel du 11 janvier 2007 relatif aux limites et référence de qualité pour les eaux potables) pour le paramètre fluorures en aval du site. Les COHV sont globalement en nette diminution, avec une exception lors de la campagne de mars 2012 durant laquelle ils ont été détectés à des teneurs de l'ordre de 20 µg/l.","Eaux souterraines","N/A","2",null,"COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP001072901","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP001073001","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP001073401","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001073901","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2008-12-10 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001075101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de gestion","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001075801","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification | Piège hydraulique ou Confinement hydraulique"]
["SSP001076701","Surveillance environnementale",null,null,"Commentaire : Concentrations en deçà des valeurs de référence.\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001077101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001077401","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001077601","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Piège hydraulique ou Confinement hydraulique"]
["SSP001077801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001078301","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"Suite à l'incident, un diagnostic a été réalisé en avril 2008. Une pollution aux hydrocarbures, composés volatils et BTEX a ainsi été mise en évidence dans les sols et eaux souterraines. \nCes pollutions ont conduit le Préfet à imposer, par arrêté préfectoral du 04 décembre 2008 puis par arrêté du 21 décembre 2010 :\n- la détermination de l'extension de la pollution des sols et des eaux souterraines\n- l'examen de la compatibilité entre les milieux et les enjeux\n- la définition, si nécessaire, de mesures de gestion du site pollué\n- la surveillance de la qualité des eaux souterraines\n\nLe rapport de suivi de la qualité de l'air ambiant et des eaux souterraines de décembre 2010 répond aux demandes formulées dans l'arrêté préfectoral. Il en ressort les constations suivantes :\n- l'extension latérale de la pollution dans les eaux souterraines est circonscrite au site\n- Les éléments figurant dans les rapports dans campagnes de suivi montrent une absence de risque pour la santé humaine.Pour autant la pollution mesuré dans les eaux souterraines ne permet pas de laisser la situation en l'état, une action de dépollution doit être engagée, même si aucune urgence n'est relevée.\n- L'exploitant indique avoir débuté les mesures de gestion","Eaux souterraines","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | COHV, solvants chlorés, fréons | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001078801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001079201","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP001079501","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001079801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Plomb | Zinc","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001080101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001080201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001080701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP001081001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001081401","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2014-12-31 : LA SITUATION S'AMELIORE\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001081901","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2015-06-15 : LA SITUATION RESTE STABLE\nDate de fin envisagée de la surveillance : 2015-12-01","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001082501","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP001082901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Ammonium | Arsenic | Baryum","Metaux et métalloïdes | Paramètres azotés","N/A","N/A","N/A","N/A","N/A"]
["SSP001083101","Surveillance environnementale","2012-10-31",null,"Résultat de la surveillance à la date du 2015-05-12 : LA SITUATION RESTE STABLE\nInformations complémentaires : Absence d'impact notable mesuré sur les eaux souterraines (présence de sulfates et chlorures largement en deçà des limites de potabilité). En mai 2015, la présence de cuivre (14 µg/L) a été détectée dans le piézomètre n°2 à proximité du dépôt de mâchefers \"Sous la Côte\".\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001083101","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP001083501","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP001083801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Interprétation de l''état des milieux (IEM)","N/A","Cuivre | Fer","COHV, solvants chlorés, fréons | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001084401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de gestion","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | COHV, solvants chlorés, fréons | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001084701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001084801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001085301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Ammonium | Chlorures | Mercure | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Sulfates","Autres éléments minéraux | Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Metaux et métalloïdes | Paramètres azotés","N/A","N/A","N/A","N/A","N/A"]
["SSP001085701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...) | Pompage de rabattement ou de récupération","N/A","N/A","N/A"]
["SSP001085801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cadmium | Zinc","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001086001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001086801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de gestion","N/A","Trichloroéthylène","COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP001087201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"COHV, solvants chlorés, fréons | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP001088601","Exécution des travaux de réhabilitation",null,null,"Travaux de dépollution","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP001088901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols","Confinement par couverture et étanchéification"]
["SSP001089001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage | Interdiction d'accès (clôture...) | Reconditionnement de produits dangereux, Reconditionnement de déchets","N/A","N/A","N/A"]
["SSP001089601","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Oxydation chimique"]
["SSP001089801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Trichloroéthylène","Benzène et dérivés | COHV, solvants chlorés, fréons | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP001089801","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001090201","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP001090501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001091201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001092101","Etude SSP et ingénierie des travaux de réhabilitation","2010-03-01",null,"En mars 2010, la société VOESTALPINE ROTEC France SA a transmis une étude de diagnostic approfondi et une évaluation quantifiée des risques sanitaires (EQRS), réalisées par l’APAVE le 1er mars 2010 et qui fait apparaître :\n- la présence de trichloréthylène en quantité plus importante qu’au droit de la zone de déchets (autour du sondage SD3). Au droit du bâtiment, les teneurs les plus élevées sont présentes en surface (inférieur à 1 mètre). Tous les prélèvements effectués à 3 mètres de profondeur sont inférieurs aux seuils de détection et un seul prélèvement à 6 m fait apparaître une teneur non négligeable en trichloréthylène. Cette disparité des teneurs en trichloréthylène, que ce soit en profondeur ou en localisation, liée au fait que le trichloréthylène n’a pas été utilisé sur le site selon les salariés de l’entreprise, font émettre l’hypothèse d’une pollution d’origine extérieure au site et rapportée sur place sous forme de remblais lors de la construction du site en 1980.\n- les résultats de la seconde campagne confirment la présence de pollution par des HCT uniquement en surface (moins de 1 mètre de profondeur). En revanche, on observe des teneurs importantes en HCT au niveau de SD43 et uniquement à 3 mètres de profondeur. Cette pollution au niveau de SD43 n’a pas d’extension horizontale et fait donc penser à une pollution d’origine externe (remblais pollués).\nL'EQRS conclut que le risque sanitaire est acceptable pour un usage non sensible (travailleur 10h en intérieur du batiment et 2h au droit de la zone déchets).Tout changement d'usage nécessiterait des investigations complémentaires.",null,"Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001092601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP001093001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001093501","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP001093701","Surveillance environnementale",null,null,"","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001094001","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"     ","Eaux souterraines","Diagnostic et Analyse","N/A","Arsenic | Cyanures libres","Autres éléments minéraux | COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP001094001","Exécution des travaux de réhabilitation",null,null,"    ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP001094301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001094701","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP001095301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Trichloroéthylène","Benzène et dérivés | COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP001095701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Trichloroéthylène","Benzène et dérivés | COHV, solvants chlorés, fréons | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001096201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001096301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Trichloroéthylène","COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP001096501","Etude SSP et ingénierie des travaux de réhabilitation","2014-08-11","2016-07-08","La solution de gestion par excavation et traitement hors site des terres impactées a été mise en œuvre.\nUn traitement de la nappe perchée a été effectué.","Sol - Sous-sol","Plan de gestion","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001096701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001097401","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP001097601","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique","Biodégradation dynamisée (ou atténuation naturelle dynamisée)"]
["SSP001097801","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2011-11-01 : LA SITUATION RESTE STABLE\nCommentaire : Les taux de HAP et d'hydrocarbures sont détectés à des concentrations inférieures au seuil de potabilité.\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001098101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Arsenic | Chrome | Nickel | Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Zinc","Benzène et dérivés | COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001098401","Surveillance environnementale","2009-01-22",null,"Résultat de la surveillance à la date du 2011-07-20 : LA SITUATION RESTE STABLE\nCommentaire : Par rapport à la valeur flash de 2007 ([HCT]= 99 000 µg/L sur Pz1) les concentrations retrouvées en 2010 et 2011 sont bien moins importantes et une certaine stabilité apparaît.\nInformations complémentaires : Les ouvrages Pz1 et Pz2 ayant été détruit lors des travaux de réaménagement du site, ils ont été remplacés par 2 nouveaux ouvrages implantés en aval théorique :\r\n- Pz2B : à proximité de l'emplacement de l'ancien ouvrage Pz3\r\n- Pz3B : dans la partie Est du site\r\n\r\n- HCT : . Pz 1 : 406 µg/L en 2010 et 1150 µg/L en 2011\r\n        . Pz 2 : 291 µg/L en 2010 \r\n        . Pz 3 : <50 µg/L en 2010\r\n        . Pz2B : 218 µg/L en 2011\r\n        . Pz3B : 405 µg/L en 2011\r\n\r\n- B(a)P : . Pz 1 : <0.01 µg/L en 2010 et 0.021 µg/L en 2011\r\n          . Pz 3 : <0.01 µg/L en 2010 \r\n          . Pz3B : 0.1 µg/L en 2011 \n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001098401","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP001099001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP001099301","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2009-12-01 : LA SITUATION RESTE STABLE\nInformations complémentaires : L'ensemble des résultats indiquent l'absence de pollution majeure de la nappe et notamment l'absence de composés organohalogénés volatils et de cyanures.\r\n\r\nDes traces de certains composés ont été toutefois notées dans le piézomètre PZ4 situé en aval hydraulique, en bordure nord-ouest du site : des composés aromatiques à des teneurs de l'ordre de 10 µg/l,\r\ndes composés aromatiques polycycliques (de l'ordre du seuil de détection, soit 3  µg/l pour la somme des 6 HAP), de l'aluminium et du fer à des concentrations respectives de 790 µg/l et 0,46  µg/l en décembre 2009, en cohérence avec les résultats des campagnes précédentes.\r\n\r\nAucun impact en aval du site n'a été identifié. Que ce soit dans le puits Meunier distant d'environ 200 m vers le nord ou au niveau du captage d'eau potable « Station des Alouettes », localisée à 3,75 km en aval hydraulique du site.\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001099501","Exécution des travaux de réhabilitation",null,null,".","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP001099701","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP001099901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Interprétation de l''état des milieux (IEM)","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001100201","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP001100201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP001100701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001101201","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001101301","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Ventilation de la zone non saturée (venting)"]
["SSP001101601","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP001101901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001102701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001103301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de gestion","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001103501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001103701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Cuivre","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001104501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001104701","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP001105201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Pompage de rabattement ou de récupération","N/A","N/A","N/A"]
["SSP001105601","Surveillance environnementale","2007-01-01",null,"Résultat de la surveillance à la date du 2013-03-20 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","1",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001107001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP001107701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001107901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP001108301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001109001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001109201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001109501","Etude SSP et ingénierie des travaux de réhabilitation","2008-01-11",null,"Une étude complémentaire du 06 mars 2008 a permis de disposer d'un recensement des points d'eau situés à proximité du site et utilisés pour un usage sensible.",null,"Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001109701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de gestion","N/A","Arsenic | Nickel","HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP001110101","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP001110501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Trichloroéthylène","COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP001110701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP001110801","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP001111001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001111401","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001111801","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001112101","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP001112201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001112401","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique"]
["SSP001112601","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001112701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de gestion","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001113001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001113101","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique"]
["SSP001113701","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2012-10-01 : LA SITUATION S'AMELIORE\nCommentaire : teneurs en baisse, faibles voire indétectables\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001114101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001114301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," .","Eaux souterraines","Analyse des enjeux sanitaires (EQRS, ARR)","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001114401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," .","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001114601","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP001114901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de gestion","N/A","Trichloroéthylène","COHV, solvants chlorés, fréons | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001115701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001115901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001116201","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP001116301","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP001116801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Mercure","COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001117001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001117701","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP001118001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001118701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Arsenic","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001119101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de gestion","N/A","Mercure","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001119601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Interprétation de l''état des milieux (IEM)","N/A","Arsenic","COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001119601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Interprétation de l''état des milieux (IEM)","N/A",null,"COHV, solvants chlorés, fréons | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001120001","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique","Confinement par couverture et étanchéification | Piège hydraulique ou Confinement hydraulique"]
["SSP001120001","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique","Confinement par couverture et étanchéification"]
["SSP001120301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001120601","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP001121401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Baryum | Plomb","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001121401","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP001121801","Surveillance environnementale","2012-10-01",null,"Résultat de la surveillance à la date du 2014-12-15 : LA SITUATION S'AMELIORE\nCommentaire : Impact persiste en BTEX et HCT avec la présence de maximums relevés au centre de la zone polluée (Pz6). Mais la tendance globale est tout de même à une baisse des teneurs observées.\nDate de fin envisagée de la surveillance : 2018-06-01","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001122001","Surveillance environnementale","2005-09-01",null,"Résultat de la surveillance à la date du 2005-09-01 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001122401","Surveillance environnementale","2007-10-01",null,"Résultat de la surveillance à la date du 2012-02-01 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001122901","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP001123201","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001123501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001123701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001124201","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001124801","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP001125001","Surveillance environnementale","2011-03-01",null,"Résultat de la surveillance à la date du 2012-05-21 : LA SITUATION RESTE STABLE\nInformations complémentaires : As en concentration légèrement supérieure aux valeurs de l'arrêté du 11/01/2007\r\nHCT en concentration supérieure aux valeurs de l'arrêté du 11/01/2007\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001125101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001126201","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001126301","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP001126501","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP001126701","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP001127001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001127401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001127501","Surveillance environnementale","1995-01-01",null,"Résultat de la surveillance à la date du : 2016-05-12\nRésultat de la surveillance eaux souterraines : 2\naugmentation importante sur la zone de traitement attirant et confinant la pollution dimunition sur les autres piézomètres\n","Eaux souterraines","N/A","1",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001127601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de gestion","N/A",null,"COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP001128201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de gestion","N/A",null,"COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés)","N/A","N/A","N/A","N/A","N/A"]
["SSP001128301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001129201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A",null,"PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP001129501","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP001129701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"COHV, solvants chlorés, fréons | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001130401","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)","Confinement par couverture et étanchéification"]
["SSP001130601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de gestion","N/A","Arsenic | Cadmium | Chrome | Nickel | Plomb | Zinc","COHV, solvants chlorés, fréons | Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP001131501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001132101","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique"]
["SSP001133101","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP001133301","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2016-08-31 : LA SITUATION RESTE STABLE\nCommentaire : La nappe souterraine  était fortement impactée en solvants chlorés (panache) au droit du site. Les premiers résultats des travaux commencent à s'observer lors de la surveillance des eaux souterraines.\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001134601","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"Dans le cadre de sa cessation d'activité, l'exploitant a transmis un mémoire en décembre 2014, complété en février 2015. \n\nCe mémoire comprenait notamment un diagnostic de l'état de pollution établi en mai 2014 par un bureau d'études. Ce diagnostic met en exergue :\n\n- la présence d'une teneur significative en hydrocarbures C10-C40 (22 000 mg/kg de matières sèche (MS)) à l'emplacement d'un ancien stockage de gasoil qui aurait fui lors du démantèlement des installations\n\n- la présence de deux teneurs notables en hydrocarbures C10-C40 (entre 500 et 700 mg/kg MS) à l'emplacement d'anciens stockages de plastifiants et à l'emplacement d'un autre ancien stockage de gasoil\n\nDes investigations complémentaires menées en janvier 2015 par le même bureau d'études ont :\n- confirmé la présence d'une pollution à l'emplacement d'un ancien stockage de gasoil : l'extension de la pollution est estimée à 110 m² sur une profondeur allant jusqu'à 2.5 mètres.\n- mis en évidence la présence d'hydrocarbures C10-C40 au droit des piézomètres Pz1 et Pz3 et d'HAP au droit des trois piézomètres. Le sens d'écoulement des eaux souterraines n'est cependant pas cohérent.","Sol - Sous-sol","Diagnostic et Analyse","N/A","C10-C40-Coupes hydrocarbures","HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001134701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001135201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP001135301","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP001135901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001136201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Cadmium | Cuivre | Mercure | Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Zinc","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001136801","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001137001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Baryum | Chrome | Cuivre | Mercure | Plomb | Trichloroéthylène","COHV, solvants chlorés, fréons | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001137501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cuivre | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Zinc","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001138201","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP001138501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"COHV, solvants chlorés, fréons | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001138601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001138901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de conception des travaux (PCT)","N/A",null,"COHV, solvants chlorés, fréons | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001139501","Surveillance environnementale","2007-03-14",null,"Résultat de la surveillance à la date du 2012-02-16 : LA SITUATION S'AMELIORE\nCommentaire : Lors de la campagne du 16/02/2012, aucun des composés recherchés n'a été quantifié (concentrations inférieures au seuil de quantification).\nInformations complémentaires : Au droit du site, deux niveaux aquifères sont identifiés à hauteur : des formations alluvionnaires superficielles récentes et subactuelles de type galets et gros graviers, soit vers 6-8 m de profondeur, en équilibre avec La Leysse ; des formations alluvionnaire quaternaires de type sables, soit vers 12,5 m de profondeur. Cette nappe est considérée comme semi-captive dans le secteur ; elle est peu vulnérable vis-à-vis d'une contamination en provenance du site. Le piézomètre PZ1 est à proximité immédiate de la fosse 2. Le PZ2 est en bordure de La Leysse, en amont hydraulique de la fosse 2. Ces 2 ouvrages captent la nappe des alluvions récentes et subactuelles. Entre 2007 et 2011 (bilan quadriennal), le suivi de la nappe met en évidence une absence de contamination des eaux souterraines prélevées sur PZ1 et PZ2.\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001139801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A","Cuivre","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001140001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Ventilation de la zone non saturée (venting)"]
["SSP001140201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001140501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001141101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Plomb","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001141301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001141501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP001142301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP001142501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP001142801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001143001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cadmium | Cuivre | Mercure | Nickel | Plomb | Zinc","HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP001143201","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols","Ventilation de la zone non saturée (venting)"]
["SSP001143901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A",null,"HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001144001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A","Trichloroéthylène","COHV, solvants chlorés, fréons | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001144001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001144501","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001144801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001145301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001145701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP001145901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP001146801","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP001147201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cadmium | Chrome | Cuivre | Nickel | Plomb | Zinc","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001147301","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique","Confinement par couverture et étanchéification"]
["SSP001147801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," .","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Cadmium | Cuivre | Mercure | Plomb | Zinc","HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF) | Phytosanitaires","N/A","N/A","N/A","N/A","N/A"]
["SSP001148501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP001149101","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)","Confinement par couverture et étanchéification"]
["SSP001150001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP001150401","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Piège hydraulique ou Confinement hydraulique"]
["SSP001151001","Surveillance environnementale","2011-10-01",null,"Résultat de la surveillance à la date du 2018-06-27 : LA SITUATION RESTE STABLE\nCommentaire : Aucun HCT n'est quantifié dans les eaux souterraines.\nInformations complémentaires : L'eau est rencontrée à une profondeur de 16 m. L'écoulement de la nappe se fait en direction du nord/nord-ouest. Le réseau piézométrique présente un gradient hydraulique de 0,63 % au droit du site.\r\n\r\nJanvier 2016 : La dix-neuvième campagne de suivi de qualité de nappe menée par TERÉO droit du dépôt Charvet La Mure Bianco de Romans sur Isère (26) a mis en évidence l'absence d'hydrocarbures dissous à l'échelle du réseau de surveillance.\r\nCompte tenu de l’absence d'hydrocarbures dissous dans les eaux souterraines, la périodicité des campagnes\r\nde prélèvements pourrait être réduite à deux campagnes par an. La société TEREO propose donc la\r\nréalisation d'un bilan quadriennal afin de solliciter un allègement des prescriptions préfectorales.\r\n\r\nBilan quadriennal du 26/3/2016 : Les campagnes d'investigations menées entre mai 2011 et janvier 2016 ont permis de mettre en évidence des teneurs en hydrocarbures C10-C40 conformes aux valeurs seuils réglementaires au sein des milieux objets de la surveillance pour le site CHARVET LA MURE BIANCO à Romans sur Isère (26)\r\nLes eaux souterraines circulant sous l'emprise du dépôt pétrolier sont exemptes de contamination\r\nhydrocarbonée depuis la mise en place de la surveillance en mai 2011. Le maintien de la surveillance des\r\neaux souterraines n'est actuellement justifié que par l'exploitation industrielle du site et l'existence de captages AEP situés à 1,5 km à l'aval hydraulique du site.\r\nLa ressource ne présente pas de variations piézométriques saisonnières.\r\nLa société TEREO propose le passage d'une surveillance trimestrielle à une périodicité semestrielle au droit de l'exploitation CHARVET LA MURE BIANCO de Romans sur Isère (26). Cette proposition devra être validée par la DREAL avant mise en application.\r\n\r\nJuillet 2016 : La vingtième campagne de suivi de qualité de nappe menée par TERÉO au droit du dépôt Charvet La Mure Bianco de Romans sur Isère (26) a mis en évidence l'absence d'hydrocarbures dissous à l'échelle du\r\nréseau de surveillance.\r\nCompte tenu de l’absence d'hydrocarbures dissous dans les eaux souterraines, la périodicité des campagnes\r\nde prélèvements pourrait être réduite à deux campagnes par an. La société TEREO a établi, en mars 2016,\r\nun bilan quadriennal afin de solliciter un allègement des prescriptions préfectorales. Dans l’attente de la\r\nvalidation de ces propositions, une surveillance trimestrielle est maintenue au droit du dépôt\r\nd’hydrocarbures CLMB de Romans sur Isère (26).\r\nUn bilan quadriennal a été effectué le 26/9/2016 avec demande d'allègement de la fréquence de réalisation des mesures.\r\nL’examen de ce bilan montre que depuis 2011, les eaux souterraines sont exemptes des composés recherchés (teneur maximum en hydrocarbures C10-C40 = 0,02 mg/l).\r\nAucune anomalie chimique n’est donc relevée entre l’amont et l’aval hydraulique du site et ce sur une période supérieure à 5 ans.\r\nCompte tenu de l’absence de saisonnalité des variations piézométriques et de l’absence d’hydrocarbures dissous dans les eaux souterraines, le cabinet TEREO estime que la périodicité des campagnes de prélèvements pourrait être réduite à deux campagnes par an.\r\n\r\nAPC n° 2016312-0016 du 04.11.2016 abrogeant & remplaçant les dispositions de l'AP n° 2013085-0014 du 23.03.2013 passant la fréquence des analyses de trimestrielle à semestrielle (HCT).\r\n\r\nMars 2017 : La vingtième quatrième campagne de suivi de qualité de nappe menée par TERÉO au droit du dépôt Charvet La Mure Bianco de Romans sur Isère (26) a mis en évidence l'absence d'hydrocarbures dissous à l'échelle du réseau de surveillance. La prochaine campagne de prélèvement est programmée en juillet 2017.\r\n\r\nJuillet 2017 : La campagne de suivi de qualité de nappe menée par TERÉO au droit du dépôt Charvet La Mure Bianco de Romans sur Isère (26) a mis en évidence l'absence d'hydrocarbures dissous à l'échelle du réseau de surveillance.\r\nUne saisonnalité des variations des conditions d'oxydo réduction a été mise en évidence : les eaux souterraines sont faiblement oxydantes voire réductrice au cours du mois d'octobre. Les autres paramètres physico-chimiques, ainsi que la piézométrie locale, ne présentent quant à eux aucune saisonnalité.La prochaine campagne de prélèvements est programmée en avril 2018\r\n\r\nAvril 2018 : La campagne de suivi de qualité de nappe menée par TERÉO au droit du dépôt Charvet La Mure Bianco de Romans sur Isère (26) a mis en évidence l'absence d'hydrocarbures dissous à l'échelle du réseau de surveillance. Les eaux souterraines sont faiblement oxydantes voire réductrice au cours du mois d'octobre. Les autres paramètres physico-chimiques, ainsi que la piézométrie locale, ne présentent quant à eux aucune saisonnalité. La prochaine campagne de prélèvements est programmée en octobre 2018.\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001151501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001151801","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP001152101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Aluminium | Fer | Plomb","HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001152301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001153401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Analyse des enjeux sanitaires (EQRS, ARR)","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001153601","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP001153901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cuivre | Mercure | Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Zinc","Benzène et dérivés | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001154101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001154601","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP001154701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP001155501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de gestion","N/A","Arsenic | Trichloroéthylène","COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001155501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A","Arsenic | Cyanures libres | Plomb | Trichloroéthylène","Autres éléments minéraux | COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001156101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A","Arsenic | Cadmium | Cuivre | Mercure | Plomb | Zinc","COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP001156501","Surveillance environnementale","2014-04-25",null,"Résultat de la surveillance à la date du 2017-04-03 : LA SITUATION RESTE STABLE\nCommentaire : Poursuite prévue pendant 4 ans par arrêté préfectoral du 17/08/2017\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001157101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP001159001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique"]
["SSP001159801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001159901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP001161701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique"]
["SSP001161901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001162701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP001163301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP001164201","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001164801","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP001164901","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP001165001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001165301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...) | Reconditionnement de produits dangereux, Reconditionnement de déchets","N/A","N/A","N/A"]
["SSP001165801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Nickel | Plomb","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001166201","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)","Confinement par couverture et étanchéification"]
["SSP001166301","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001166501","Surveillance environnementale","2015-04-01",null,"Commentaire : une surveillance a débuté qu'en 2015 donc peu de résultats\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001166901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001166901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001168101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP001168401","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001168901","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","1",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001169101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001169401","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001170501","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001171101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Arsenic | Baryum | Cadmium | Cyanures libres | Mercure | Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Trichloroéthylène","Autres éléments minéraux | Benzène et dérivés | COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001171301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001171601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001172301","Surveillance environnementale","2009-08-31",null,"Résultat de la surveillance à la date du 2013-04-24 : LA SITUATION RESTE STABLE\nInformations complémentaires : L'arrêté préfectoral du 18 janvier 2010 impose à KEOLIS la surveillance trimestrielle des eaux souterraines et du puits \"piscine\" sur les HCT ainsi que sur toutes substances identifiées en quantité significative dans les sols.\r\n\r\nLa surveillance des eaux souterraines via 5 piézomètres et du puits \"piscine\" (hors site) d'août 2009 à avril 2013 (13 campagnes) a mis en évidence les contaminations suivantes :\r\n- HCT sur P2 : 65 mg/L en août 2009, 34,9 mg/L en avril 2010 puis la phase dissoute n'a plus été analysée au droit de P2 compte tenu de la présence de flottants évalué à quelques centimètres d'épaisseur ;\r\n- HCT sur P4 : 0,43 mg/L en août 2009, 0,7 mg/L en avril 2010 puis inférieur à 0,1 mg/L ;\r\n- Benzène sur P2 : 9,2 µg/L en avril 2010 puis plus analysé ;\r\n- Ethylbenzène sur P2 : 46 µg/L en avril 2010 puis plus analysé ;\r\n- Xylène sur P2 : 217 µg/L en avril 2010 puis plus analysé ;\r\n- Benzo(a)pyrène sur P2 : 17 ng/L en avril 2010 puis plus analysé ;\r\n- Benzo(a)pyrène sur P3 : 11 ng/L en janvier 2011 et 19 ng/L en janvier 2012 ;\r\n- Benzo(a)pyrène sur P4 : 18 ng/L en avril 2011.\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001172401","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique"]
["SSP001172701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001173401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Plomb","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001174001","Surveillance environnementale",null,null,"","Eaux souterraines","N/A","1",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001174401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Cadmium | Chrome | Cuivre | Mercure | Nickel | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Zinc","Benzène et dérivés | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001175201","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP001175301","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2013-01-01 : LA SITUATION RESTE STABLE\nInformations complémentaires : Un projet d'arrêté de surveillance des eaux souterraines est en cours d'élaboration.\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001176001","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001176101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Chrome | Cuivre | Sulfates","Autres éléments minéraux | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001176501","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP001178301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Cadmium | Chrome | Cuivre | Mercure | Nickel | Plomb | Zinc","HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001179101","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","1",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001179601","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Piège hydraulique ou Confinement hydraulique"]
["SSP001180201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP001180301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001180901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de gestion","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001180901","Surveillance environnementale","2012-06-07",null,"Résultat de la surveillance à la date du 2013-08-10 : LA SITUATION S'AMELIORE\nCommentaire : La campagne de suivi piézométrique et analytique du 10 juillet 2013 a mis en évidence la présence d'une phase flottante d'hydrocarbures surnageants d'une épaisseur de 1 cm au droit de Pz6, en diminution par rapport à février 2013. Par rapport à la campagne de février 2012, on observe:\r\n- une teneur en HCT en très forte diminution malgré une concentration en HCT encore 16 fois supérieure à la valeur de référence au droit du Pz6\r\n- l'absence confirmée de contamination en HCT au droit de Pz1, Pz5 et Pz8\r\n- l'absence de concentration en HCT au droit de Pz4\r\n\r\nCompte tenu des résultats d'analyses obtenus lors de cette campagne de suivi, Il est préconisé de poursuivre le suivi de la nappe afin notamment de surveiller au droit de Pz6:\r\n- la présence de phase surnagente \r\n- l'évolution des teneur en HCT en diminution significative en juillet 2013\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001181401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de gestion","N/A","Arsenic | Cadmium | Chrome | Cuivre | Mercure | Nickel | Plomb | Zinc","COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001181501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001182001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001182301","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP001183101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"Phytosanitaires","N/A","N/A","N/A","N/A","N/A"]
["SSP001183101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cuivre | Mercure | Zinc","Metaux et métalloïdes | Phytosanitaires","N/A","N/A","N/A","N/A","N/A"]
["SSP001184201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP001184201","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001184801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A","Cadmium | Cuivre | Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Zinc","Benzène et dérivés | COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001185101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Sulfates","Autres éléments minéraux | Benzène et dérivés | COHV, solvants chlorés, fréons | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001185501","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP001186001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001186301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001186601","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique"]
["SSP001187201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Plomb","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001187601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001187901","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP001188601","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Ventilation de la zone non saturée (venting)"]
["SSP001189101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001189601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001190101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001191401","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001192401","Etude SSP et ingénierie des travaux de réhabilitation","2012-04-11","2012-07-06","Aussi, il a été demandé à Wabco, par arrêté préfectoral complémentaire du 11 avril 2012 de :\n- réaliser des prélèvements de gaz de sols et d’eaux souterraines dans les propriétés jouxtant le site industriel ;\n- réaliser une étude visant à s’assurer que l’état des milieux à l’extérieur du site soit compatible avec les usages constatés autour du site ;\n- transmettre les mesures de gestion à mettre en œuvre ;\n- mettre en place une surveillance des eaux souterraines sur site et hors site.",null,"Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001192601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001193001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cuivre | Zinc","Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP001193301","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001194501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP001194801","Surveillance environnementale",null,null,"","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001195401","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP001195901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001196701","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001196801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de conception des travaux (PCT)","N/A","Aluminium | Chlorures | Fer | Plomb | Sulfates | Zinc","Autres éléments minéraux | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001197901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Baryum | Sélénium | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001197901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001198301","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP001198601","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001199201","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001199501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Cadmium | Chrome | Cuivre | Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Trichloroéthylène | Zinc","Benzène et dérivés | COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP001200701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Cadmium | Chlorures | Chrome | Cuivre | Mercure | Nickel | Plomb | Zinc","Autres éléments minéraux | COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001200701","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP001204501","Surveillance environnementale","2011-01-13",null,"Résultat de la surveillance à la date du 2014-05-20 : LA SITUATION RESTE STABLE\nCommentaire : Aucun HAP ou HCT n'est détecté dans les eaux souterraines au droit des 3 piézomètres implantés sur le site.\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001204701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001205801","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP001207001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001207601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP001208001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP001208701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001209801","Surveillance environnementale",null,null,".","Eaux superficielles - Sédiments","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001211201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Chrome | Cuivre","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001211401","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2012-11-09 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001212201","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP001212701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP001213401","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001214501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001214701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP001214801","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001215101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001215301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001215501","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols","Confinement par couverture et étanchéification"]
["SSP001215701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Cadmium | Chrome | Cuivre | Mercure | Nickel | Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Zinc","Benzène et dérivés | COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP001216101","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001217101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Trichloroéthylène","COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP001217601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A","Arsenic","COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001218001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP001218501","Exécution des travaux de réhabilitation",null,null," Des travaux de confinement hydraulique ont été mis en place et visaient à stopper le transfert de la pollution vers le séparateur d'hydrocabures situé en aval. Ce confinement, réalisé par l'intermédiaire de techniques de pompage/écrémage en juin 2009 et octobre 2011, a permis la récupération d'environ 14m3 de phase libre de produit.",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Pompage de rabattement ou de récupération","N/A","N/A","N/A"]
["SSP001219101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001220001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de conception des travaux (PCT)","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001220801","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001221301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cadmium","Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP001221701","Exécution des travaux de réhabilitation",null,null," Octobre 2013/Janvier 2014: Excavation des remblais impactés par les hydrocarbures \n  - Juin 2014/Février 2016: Traitement in situ du perchloroéthylène (PCE) en phase pure accumulé sur la base de l'aquifère superficiel, à environ 8 mètres de profondeur, au droit de Pz2 et Pz4 (Pz: piézomètre)  ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001222201","Exécution des travaux de réhabilitation",null,null," Mise en sécurité effectuée",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP001222501","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001223601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de gestion","N/A",null,"COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP001223601","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Ventilation de la zone non saturée (venting)"]
["SSP001223801","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP001224101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001224701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001225501","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001226301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés","N/A","N/A","N/A","N/A","N/A"]
["SSP001226601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Zinc","HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001227401","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001227801","Etude SSP et ingénierie des travaux de réhabilitation","2014-02-24",null,"Interprétation de l'état des milieux des eaux souterraines et du sous sol","Eaux souterraines","Interprétation de l''état des milieux (IEM)","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001227901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage","N/A","N/A","N/A"]
["SSP001229801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001230601","Surveillance environnementale","1996-12-01",null,"Résultat de la surveillance à la date du 2018-12-14 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001230701","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"En avril 2016, la station-service n'a pas encore été démantelée.\n\nAussi, il est prévu :\n- la mise en sécurité des cuves et tuyauterie,\n- le démantèlement des structures aériennes,\n- la réalisation d'une étude hydrogéologique,\n- la réalisation d'un plan de gestion des pollutions.","Sol - Sous-sol","Plan de gestion","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001232001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001232301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001234201","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001234401","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique","Confinement par couverture et étanchéification"]
["SSP001234701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001235101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Arsenic | Baryum | Chrome | Cuivre | Mercure | Nickel | Plomb | Zinc","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001235501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001236101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001236701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Trichloroéthylène","COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP001236901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Nickel | Trichloroéthylène","COHV, solvants chlorés, fréons | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001237101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001237701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"COHV, solvants chlorés, fréons | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP001237801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001238601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Cuivre | Nickel | Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Zinc","Benzène et dérivés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001239001","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP001240701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP001241901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cyanures libres","Autres éléments minéraux | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001243901","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP001244201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage | Interdiction d'accès (clôture...) | Pompage de rabattement ou de récupération | Reconditionnement de produits dangereux, Reconditionnement de déchets","N/A","N/A","N/A"]
["SSP001244801","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001245401","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP001246001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001246301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Trichloroéthylène","Benzène et dérivés | COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP001247501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001248401","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP001248701","Exécution des travaux de réhabilitation",null,null,"Confinement par couverture et étanchéification","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP001249301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001249501","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)","Confinement par couverture et étanchéification"]
["SSP001249901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001250601","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001251601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP001252401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001253501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP001254001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Plomb","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001255501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001256401","Surveillance environnementale","2012-07-01",null,"Résultat de la surveillance à la date du 2014-08-01 : LA SITUATION S'AMELIORE\nCommentaire : 4 piézomètres sur le site :\r\n- le piézomètre amont (Pz amont)\r\n- le piézomètre Pz4 (neuf) implanté en aval proche de la source de pollution\r\n- le piézomètre Pz5 implanté en aval éloigne de la source de pollution et en position aval hydrogéologique latéral sur le site\r\n- le piézomètre Pz6 implanté en aval éloigne de la source de pollution et en position aval hydrogéologique sur le site.\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001256601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001258201","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP001258501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de gestion","N/A",null,"COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP001258601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP001259101","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001259401","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001261301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," En novembre 2017 et mai 2018, un suivi des eaux souterraines est réalisé à partir de Pz1 (amont) et de deux nouveaux piézomètres (Pz4 et Pz5), Pz2 et Pz3 ayant été détruits lors des travaux de démantèlement. Les hydrocarbures totaux sont absents ou présents en concentration inférieure à la limite de quantification. De faibles anomalies sont observées en BTEX sur l’ensemble des piézomètres (maximum à 2,1 µg/L) en novembre 2017. En mai 2018, les BTEX sont absents ou présents en concentration inférieure à la limite de quantification.(< 1 µg/L) Celles-ci sont non significatives d’un risque sanitaire ou pour l’environnement. Sur proposition de l'exploitant, l'inspection des installations classées accepte l'arrêt de la surveillance par courriel du 3 juillet 2018.\n","Eaux souterraines","Plan de gestion","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001261501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de conception des travaux (PCT)","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001261501","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP001263001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...) | Reconditionnement de produits dangereux, Reconditionnement de déchets","N/A","N/A","N/A"]
["SSP001263201","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001264301","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001264501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A","Cadmium | Cuivre | Mercure | Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Trichloroéthylène | Zinc","Benzène et dérivés | COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001265401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Interprétation de l''état des milieux (IEM)","N/A","Arsenic | Cadmium | Chlorures | Chrome | Cuivre | Mercure | Nickel | Plomb | Trichloroéthylène | Zinc","Autres éléments minéraux | COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP001265701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001265801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001265901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Fer | Plomb","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001265901","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2015-10-13 : LA SITUATION RESTE STABLE\nCommentaire : Anomalies en métaux\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001265901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cuivre | Cyanures libres","Autres éléments minéraux | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001266301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Arsenic | Plomb | Zinc","HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001266301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cadmium | Mercure | Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Zinc","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001266301","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001266301","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP001266301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001266401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001266401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001266501","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Ventilation de la zone non saturée (venting)"]
["SSP001266501","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique","Ventilation de la zone non saturée (venting)"]
["SSP001266501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP001266601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Aluminium | Arsenic | Cadmium | Cuivre | Fer | Plomb | Zinc","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001266601","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001266601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Cadmium | Chrome | Cuivre | Mercure | Molybdène | Nickel | Plomb | Zinc","COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP001266601","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP001266601","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP001266601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001267101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001267101","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2015-08-04 : LA SITUATION SE DEGRADE\nCommentaire : Hausse important des BTEX entre avril 2014 et août 2015\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001267101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001267201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001267301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A","Cuivre | Zinc","COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001267301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001267401","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001267401","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP001267401","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...) | Pompage de rabattement ou de récupération","N/A","N/A","N/A"]
["SSP001267601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001267701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cuivre","HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP001267701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001267801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001267801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Trichloroéthylène","COHV, solvants chlorés, fréons | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001267801","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001267801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001268001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001268001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001268001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP001268101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001268101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP001268201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Ammonium | Sulfates","Autres éléments minéraux | Paramètres azotés","N/A","N/A","N/A","N/A","N/A"]
["SSP001268301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001268401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Sulfates","Autres éléments minéraux","N/A","N/A","N/A","N/A","N/A"]
["SSP001268501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A","Sulfates","Autres éléments minéraux","N/A","N/A","N/A","N/A","N/A"]
["SSP001268501","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001268701","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP001268701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001268901","Surveillance environnementale","2010-06-01",null,"Résultat de la surveillance à la date du 2017-04-30 : LA SITUATION RESTE STABLE\nCommentaire : pic en fréon 11 à 290 microg/l en 2014. quasiment stable depuis octobre 2015 à moins de 26 microg/l (avril 2017)\nDate de fin envisagée de la surveillance : 2018-12-31","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001268901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Trichloroéthylène","COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001268901","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP001268901","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP001268901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001269001","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001269001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001269001","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP001269001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001269101","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001269101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001269201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001269201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001269201","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001269201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP001269301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001269301","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Biodégradation dynamisée (ou atténuation naturelle dynamisée)"]
["SSP001269301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP001269401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001269401","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP001269501","Surveillance environnementale","2017-04-27",null,"Résultat de la surveillance à la date du 2018-07-27 : LA SITUATION SE DEGRADE\nCommentaire : sens d’écoulement de la nappe est en direction du Ouest-Est.\nInformations complémentaires : -La présence de traces de cis-1,2-dichloroéthylène (1,2 μg/l) et de chlorure de vinyle (1,3 μg/l) au\r\nniveau du puits, situé en aval hydraulique. Seul le cis-1,2-dichloroéthylène est retrouvé sous forme\r\nde traces en amont, au droit de Pz A (0,83 μg/l). Son origine n’est pas connue.\r\n-La concentration en chlorure de vinyle mesurée au niveau du puits est supérieure à la valeur limite\r\ndéfinie par l’annexe 1 de l’arrêté du 11 janvier 2007 ainsi qu’à la valeur mesurée en avril 2017, qui\r\nétait alors de 0,4 μg/l ;\r\n-L’absence de COHV dans les eaux souterraines au droit du piézomètre Pz B ;\r\n- L’absence d’hydrocarbures HCT C10-C40 sur tous les échantillons analysés.\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001269501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001269601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," Plan de gestion","Eaux souterraines","Plan de gestion","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001269601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," Plan de gestion","Sol - Sous-sol","Plan de gestion","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001269901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Interprétation de l''état des milieux (IEM)","N/A",null,"COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP001270001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Plomb","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001270001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Chrome | Plomb | Zinc","HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001270001","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP001270001","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP001270001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP001270101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP001270201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de gestion","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | COHV, solvants chlorés, fréons | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001270201","Surveillance environnementale","2004-01-01",null,"Résultat de la surveillance à la date du 2018-06-27 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001270201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001270301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," Description","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001270301","Exécution des travaux de réhabilitation",null,null,"Travaux","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001270401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Chrome | Plomb","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001270401","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2018-09-10 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001270401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Chrome | Plomb","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001270501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP001270601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Trichloroéthylène","COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP001270601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Chrome | Cuivre | Nickel | Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Zinc","Benzène et dérivés | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001270601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001270901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Chrome","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001270901","Surveillance environnementale","2006-06-30",null,"Résultat de la surveillance à la date du 2018-01-30 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001271001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cuivre | Plomb","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001271101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001271201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Trichloroéthylène","COHV, solvants chlorés, fréons | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001271301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001271401","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001271401","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001271601","Exécution des travaux de réhabilitation",null,null," Travaux d'excavation et incinération","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP001271601","Exécution des travaux de réhabilitation",null,null," Mise en sécurité du site effectuée",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001271701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cuivre | Zinc","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001271701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001271701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique"]
["SSP001271801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Aluminium | Cuivre | Zinc","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001271801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001271801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001271901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cadmium | Cuivre | Mercure | Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001271901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001271901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001272001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001272001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001272001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001272101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001272401","Exécution des travaux de réhabilitation",null,null,"2/ S’agissant des mesures de gestion entreprises :\n\nLes diagnostics des sols réalisés entre novembre 2017 et mars 2018 ont révélé des contaminations diffuses au droit des installations existantes et anciennes. \n\nEn particulier au droit :\n- des cuves n°1, n°6, n°3 (inertée au béton) et n°2 (inertée au béton) ;\n- de la cuve d’huiles usées ;\n- du poste de distribution PL ;\n- des pistes de distributions et des volucompteurs VL ;\n- du séparateur à hydrocarbures.\n\nConformément à la méthodologie nationale de gestion des sites et sols pollués du 19 avril 2017, les mesures de gestion qui ont été engagées ont consisté à extraire les matériaux impactés par des hydrocarbures et présents au droit des installations précitées. \n\nSelon les justificatifs présentés, environ 1680 tonnes de terres ont été évacués vers un biocentre (EMTA à Issou dans les Yvelines) jusqu’à atteinte de concentrations résiduelles en hydrocarbures et BTEX  inférieures aux critères ISDI (installations de stockage de déchets inertes).\n\nEn effet, la teneur résiduelle maximale observée en HC est de 280 mg/kg MS (cuve n°2) et de 0,11 mg/kg  MS en BTEX (cuves n°3 et 6). Celles-ci sont  bien inférieures aux critères ISDI  fixés  à 500mg/kg MS pour les HC et 6 mg/kg MS pour les BTEX. \n\nLe remblaiement des zones excavées a été réalisé avec des matériaux sains provenant de la carrière CEMEX de Berville sur Seine.\nAussi, l’évaluation qualitative des risques sanitaires résiduels pour un usage industriel des terrains indique un risque négligeable au regard des teneurs résiduelles en hydrocarbures et BTEX.  Dans ce contexte, aucune surveillance environnementale n’est recommandée.\n\nPour conclure, conformément aux dispositions de l’article R512-66-1 du code de l’environnement, le site apparaît être dans un état tel qu’il ne puisse porter atteinte aux intérêts mentionnés à l’article L511-1 du Code de l’environnement et qu’il permette un usage futur comparable à la dernière période d’activité, c’est à dire un usage de type industriel. \n","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001272401","Exécution des travaux de réhabilitation",null,null,"2/ S’agissant des mesures de gestion entreprises :\n\nLes diagnostics des sols réalisés entre novembre 2017 et mars 2018 ont révélé des contaminations diffuses au droit des installations existantes et anciennes. \n\nEn particulier au droit :\n- des cuves n°1, n°6, n°3 (inertée au béton) et n°2 (inertée au béton) ;\n- de la cuve d’huiles usées ;\n- du poste de distribution PL ;\n- des pistes de distributions et des volucompteurs VL ;\n- du séparateur à hydrocarbures.\n\nConformément à la méthodologie nationale de gestion des sites et sols pollués du 19 avril 2017, les mesures de gestion qui ont été engagées ont consisté à extraire les matériaux impactés par des hydrocarbures et présents au droit des installations précitées. \n\nSelon les justificatifs présentés, environ 1680 tonnes de terres ont été évacués vers un biocentre (EMTA à Issou dans les Yvelines) jusqu’à atteinte de concentrations résiduelles en hydrocarbures et BTEX  inférieures aux critères ISDI (installations de stockage de déchets inertes).\n\nEn effet, la teneur résiduelle maximale observée en HC est de 280 mg/kg MS (cuve n°2) et de 0,11 mg/kg  MS en BTEX (cuves n°3 et 6). Celles-ci sont  bien inférieures aux critères ISDI  fixés  à 500mg/kg MS pour les HC et 6 mg/kg MS pour les BTEX. \n\nLe remblaiement des zones excavées a été réalisé avec des matériaux sains provenant de la carrière CEMEX de Berville sur Seine.\nAussi, l’évaluation qualitative des risques sanitaires résiduels pour un usage industriel des terrains indique un risque négligeable au regard des teneurs résiduelles en hydrocarbures et BTEX.  Dans ce contexte, aucune surveillance environnementale n’est recommandée.\n\nPour conclure, conformément aux dispositions de l’article R512-66-1 du code de l’environnement, le site apparaît être dans un état tel qu’il ne puisse porter atteinte aux intérêts mentionnés à l’article L511-1 du Code de l’environnement et qu’il permette un usage futur comparable à la dernière période d’activité, c’est à dire un usage de type industriel. \n","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP001272401","Exécution des travaux de réhabilitation",null,null," 1/ S’agissant du démantèlement des installations : \n\nLa station-service était implantée sur un terrain de 1900 m² et comprenait :\n-  2 bâtiments sur 150 m² (une boutique et un atelier),\n- une zone de stationnement, de distribution et de circulation  sur une emprise de 1000 m²,\n- une surface enherbée de 750 m².\n\nL’ensemble des installations a été démantelé à savoir : \n- l’aire de distribution de carburants composée de 2 ilôts VL et un volucompteur PL ;\n- la boutique et l’atelier ;\n- 2 cuves de stockage de carburants (la cuve n°1 de 30 m3 double enveloppe bi-compartimentée, la cuve n°6 de 30 m³ double enveloppe tri-compartimentée) ;\n- 3 cuves anciennes inertées au béton (cuves n°2 & n°3 et cuve dénommée « CHU ») ;\n- 1 cuve d’huiles usées nommée cuve « HU » ;\n- la zone de dépotage ;\n- les évents ;\n- un auvent ;\n- un séparateur à hydrocarbures et un décanteur.\n\nPour ce faire, vous avez fait intervenir les entreprises Castres Equipement, Bariau Leclerc et Transports Morieux sous la coordination de l’entreprise SUEZ.\n\nLes justificatifs (attestations des sous-traitants, BSD) afférents au dégazage et au démantèlement  des réservoirs d’hydrocarbures et tuyauteries ont été produits. \n\n\n",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001272501","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","3",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001272501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cadmium | Trichloroéthylène | Zinc","COHV, solvants chlorés, fréons | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001272601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"Phytosanitaires","N/A","N/A","N/A","N/A","N/A"]
["SSP001272601","Surveillance environnementale","2003-03-04",null,"Résultat de la surveillance à la date du 2019-10-01 : LA SITUATION S'AMELIORE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001272601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Phytosanitaires","N/A","N/A","N/A","N/A","N/A"]
["SSP001272801","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols","Biodégradation dynamisée (ou atténuation naturelle dynamisée)"]
["SSP001273001","Surveillance environnementale","2017-03-27",null,"Résultat de la surveillance à la date du 2018-07-04 : LA SITUATION RESTE STABLE\nCommentaire : les ouvrages PG3 et Pz5, présentent encore des teneurs significatives et supérieures aux valeurs de références.\n","Eaux souterraines","N/A","6",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001273001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001273201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001273201","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001273201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001273301","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP001273301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP001273701","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001273701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A",null,"HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001273701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP001273701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001273701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP001273801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001273901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP001274001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001274001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP001274001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP001274001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001274201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A",null,"COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP001274201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP001274401","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP001274801","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Biodégradation dynamisée (ou atténuation naturelle dynamisée) | Ventilation de la zone non saturée (venting)"]
["SSP001274801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP001274901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001275001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001275001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP001275201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001275201","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001275201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001275301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Trichloroéthylène","COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP001275301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Trichloroéthylène","COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | Phytosanitaires","N/A","N/A","N/A","N/A","N/A"]
["SSP001275401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001275401","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001275601","Etude SSP et ingénierie des travaux de réhabilitation","2016-01-01","2016-12-01","- En juin 2016, un diagnostic de l'état des sols a été réalisé à l'aide de sondages et de prélèvements. \n","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Cuivre | Mercure | Plomb | Zinc","HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001275601","Etude SSP et ingénierie des travaux de réhabilitation","2020-01-01","2020-12-31","- en 2020, un diagnostic des eaux souterraines a été réalisé ",null,"Diagnostic et Analyse","N/A","Cadmium | Nickel | Somme de COHV","COHV, solvants chlorés, fréons | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001275601","Etude SSP et ingénierie des travaux de réhabilitation","2020-01-01",null," études",null,"Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001275701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001275801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Arsenic | Cadmium | Cuivre | Mercure | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001275801","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001275801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP001275901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001276001","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2018-03-29 : LA SITUATION RESTE STABLE\nCommentaire : Pas d'incidence constatée\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001276101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Cadmium | Cuivre | Mercure","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001276201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Arsenic","COHV, solvants chlorés, fréons | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001276201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Cadmium | Chrome | Cuivre | Nickel | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Zinc","Benzène et dérivés | COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP001276201","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001276201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001276301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A",null,"HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001276301","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP001276301","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001276301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001276401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," Investigations complémentaires dans les eaux souterraines pour confirmer le sens d'écoulement","Eaux souterraines","Diagnostic et Analyse","N/A","Nickel","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001276401","Surveillance environnementale",null,null,"Surveillance annuelle des eaux souterraines","Eaux souterraines","N/A","1","Nickel | Somme de COHV","COHV, solvants chlorés, fréons | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001276601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001276601","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001276601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP001276701","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"\n\n",null,"Plan de gestion","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001276901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001276901","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP001276901","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP001276901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001276901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001277001","Surveillance environnementale","2018-03-01",null,"Résultat de la surveillance à la date du 2018-09-03 : LA SITUATION RESTE STABLE\nInformations complémentaires : les teneurs en perchlorates présentent des variations parfois importantes d'une campagne à l'autre, probablement en lien avec l'hydrologie et les conditions de prélèvement (hypothèse d'une stratification de la nappe).\n","Eaux souterraines","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001277001","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001277001","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001277301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001277401","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","4",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001277401","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Ventilation de la zone non saturée (venting)"]
["SSP001277501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Trichloroéthylène","Benzène et dérivés | COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP001277501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Trichloroéthylène","Benzène et dérivés | COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP001277501","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique","Ventilation de la zone non saturée (venting)"]
["SSP001277501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001277601","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"Etude de risques sanitaires","Eaux souterraines","Analyse des enjeux sanitaires (EQRS, ARR)","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001277601","Exécution des travaux de réhabilitation",null,null,"Travaux par oxydation chimique","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Oxydation chimique"]
["SSP001277601","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"Etude de risque sanitaire","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001277601","Exécution des travaux de réhabilitation",null,null," Travaux d'excavation des sols","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001277601","Exécution des travaux de réhabilitation",null,null,"Mise en sécurité du site effectuée",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001277701","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Piège hydraulique ou Confinement hydraulique"]
["SSP001277701","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2019-06-12 : LA SITUATION RESTE STABLE\nCommentaire : Pas d'impact\nDate de fin envisagée de la surveillance : 2020-06-12","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001277701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001277701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage | Interdiction d'accès (clôture...) | Pompage de rabattement ou de récupération","N/A","N/A","N/A"]
["SSP001277901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Phytosanitaires","N/A","N/A","N/A","N/A","N/A"]
["SSP001278101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001278301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001278301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP001278701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001278701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP001278901","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2018-10-17 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001278901","Surveillance environnementale",null,null,"","Eaux superficielles - Sédiments","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001278901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cuivre | Plomb | Zinc","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001278901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols","Confinement par couverture et étanchéification"]
["SSP001279001","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2018-07-31 : LA SITUATION RESTE STABLE\n","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001279001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Baryum | Molybdène","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001279601","Exécution des travaux de réhabilitation",null,null,"Elimination en installation de stockage des déchets dangereux (ISDD)","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP001280001","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Confinement par couverture et étanchéification"]
["SSP001280101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," Diagnostic et Analyse","Eaux souterraines","Diagnostic et Analyse","N/A","Trichloroéthylène","COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP001280101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," Diagnostic et Analyse","Sol - Sous-sol","Diagnostic et Analyse","N/A","Trichloroéthylène","COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP001280301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," Diagnostic et analyse","Sol - Sous-sol","Diagnostic et Analyse","N/A","Plomb","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001280501","Exécution des travaux de réhabilitation","2020-11-20","2021-03-23","-un repérage amiante\n-la condamnation des portes du bâtiment\n-l'enlèvement et le traitement de tous les déchets dangereux\n-le nettoyage des sols et des cuves\n-l'inertage et l'enlèvement de la cuve à gaz",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001280701","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001280801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Ammonium | Arsenic | Cuivre | Mercure | Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes | Paramètres azotés","N/A","N/A","N/A","N/A","N/A"]
["SSP001280801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Cadmium | Chrome | Cuivre | Mercure | Nickel | Plomb | Zinc","HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001280901","Exécution des travaux de réhabilitation",null,null," Elimination en installation de stockage des déchets non dangereux (ISDND)","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP001280901","Exécution des travaux de réhabilitation",null,null," Evacuation de produits ou de déchets",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP001281001","Exécution des travaux de réhabilitation",null,null,".","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001281201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001281501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001281601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP001281701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001281801","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP001282501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," Diagnostic","Eaux souterraines","Diagnostic et Analyse","N/A",null,"COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP001282501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," Diagnostic","Sol - Sous-sol","Diagnostic et Analyse","N/A","Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Zinc","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP001282501","Exécution des travaux de réhabilitation",null,null," Mise en sécurité du site effectuée",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001283101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," Suite à ce diagnostic, ANTEA Group suggère à l'exploitant une purge sélective de la zone contaminée jusqu'à atteindre les seuils de l'inerte pour les hydrocarbures C10-C40 (500mg/kg MS). La rétention devra être démantelée et les terres issues de l'excavation pourront être envoyées en centre de traitement ou de stockage adapté.","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001283401","Exécution des travaux de réhabilitation",null,null,"- Un retrait et un traitement hors site des terres impactées sur 1,5 m de profondeur, \n- la création d'une nouvelle rétention étanche.","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001283401","Exécution des travaux de réhabilitation",null,null,"- Un retrait et un traitement hors site des terres impactées sur 1,5 m de profondeur, \n- la création d'une nouvelle rétention étanche.","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP001283401","Exécution des travaux de réhabilitation",null,null,"- Un retrait et un traitement hors site des terres impactées sur 1,5 m de profondeur, \n- la création d'une nouvelle rétention étanche.","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode thermique"]
["SSP001284101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," .","Eaux souterraines","Diagnostic et Analyse","N/A","Ammonium | Arsenic | Baryum | Chlorures | Plomb | Sulfates | Zinc","Autres éléments minéraux | Metaux et métalloïdes | Paramètres azotés","N/A","N/A","N/A","N/A","N/A"]
["SSP001284101","Surveillance environnementale",null,null,".","Eaux superficielles - Sédiments","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001284101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," .","Sol - Sous-sol","Diagnostic et Analyse","N/A","Ammonium | Arsenic | Baryum | Cadmium | Chlorures | Chrome | Cuivre | Nickel | Plomb | Sulfates | Zinc","Autres éléments minéraux | Metaux et métalloïdes | Paramètres azotés","N/A","N/A","N/A","N/A","N/A"]
["SSP001284801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001284801","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001284801","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001285301","Exécution des travaux de réhabilitation",null,null," ","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution",null,null,"Oxydation chimique"]
["SSP001285301","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP001285301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001285601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de gestion","N/A","Zinc","HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001285601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A","Arsenic | Cadmium | Chrome | Cuivre | Mercure | Nickel | Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Zinc","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001286001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," Diagnostic et Analyse","Sol - Sous-sol","Diagnostic et Analyse","N/A","Plomb","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001286101","Surveillance environnementale",null,null,"Résultat de la surveillance à la date du 2019-11-06 : LA SITUATION RESTE STABLE\nDate de fin envisagée de la surveillance : 2023-12-31","Eaux souterraines","N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP001286101","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001286101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP001286201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Analyse des enjeux sanitaires (EQRS, ARR)","N/A",null,"COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP001286201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Arsenic | Cuivre | Plomb | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001286201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001286301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de gestion","N/A",null,"Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001286301","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A","Cuivre | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001286501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," Diagnostic","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cobalt","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001286801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de conception des travaux (PCT)","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001286801","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de conception des travaux (PCT)","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001286901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001286901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001287001","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,"HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001287101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001287201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001287401","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Cadmium | Chlorures | Molybdène | Zinc","Autres éléments minéraux | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001287401","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001287501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001287501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001287501","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001287501","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001287601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Diagnostic et Analyse","N/A","Trichloroéthylène","COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP001287601","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Arsenic | Cadmium | Plomb | Trichloroéthylène","COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001287701","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001287701","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Gardiennage | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001288001","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001288001","Exécution des travaux de réhabilitation",null,null," La notification de cessation d'activité du 24/09/2018 était accompagnée des justificatifs suivants :\n- transfert des batteries, des déchets non dangereux, des bouteilles de gaz (oxygène et propane), d'une cuve aérienne de carburants de 3000 litres et le poste de distribution associé sur le site de Villeneuve-le-Roi\n- pompage et nettoyage du séparateur à hydrocarbures\n- évacuation de métaux vers une société agrée\n\nLe site est clôturé et une portail fermé à clé en interdit l'accès.\n\nLes risques d'incendie et d'explosion sont nuls car tous les équipements et matériaux ont été enlevés du site.\n\nUn diagnostic des sols a été transmis en octobre 2018.",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001288101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," diagnostic","Sol - Sous-sol","Diagnostic et Analyse","N/A","Plomb","HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes | Phytosanitaires","N/A","N/A","N/A","N/A","N/A"]
["SSP001288101","Exécution des travaux de réhabilitation",null,null," elimination","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP001288101","Exécution des travaux de réhabilitation",null,null," interdiction d'accès",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001288301","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP001288501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Plan de gestion","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés","N/A","N/A","N/A","N/A","N/A"]
["SSP001288501","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Plan de gestion","N/A","Somme de benzene, toluene, ethylbenzene, xylenes (BTEX)","Benzène et dérivés | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP001288601","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP001288601","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Incinération"]
["SSP001288601","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001288901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Eaux souterraines","Interprétation de l''état des milieux (IEM)","N/A","Trichloroéthylène","COHV, solvants chlorés, fréons","N/A","N/A","N/A","N/A","N/A"]
["SSP001288901","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Interprétation de l''état des milieux (IEM)","N/A","Baryum | Chrome | Mercure | Plomb | Trichloroéthylène","COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés | Metaux et métalloïdes | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP001288901","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001288901","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP001289101","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Plomb | Zinc","Hydrocarbures et indices liés | Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001289101","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets dangereux (ISDD)"]
["SSP001289101","Exécution des travaux de réhabilitation",null,null," ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Elimination en installation de stockage des déchets non dangereux (ISDND)"]
["SSP001289101","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP001289101","Exécution des travaux de réhabilitation",null,null,"","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Méthode biologique ou chimique"]
["SSP001289101","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets","N/A","N/A","N/A"]
["SSP001289201","Etude SSP et ingénierie des travaux de réhabilitation",null,null," ","Sol - Sous-sol","Diagnostic et Analyse","N/A","Cuivre","Metaux et métalloïdes","N/A","N/A","N/A","N/A","N/A"]
["SSP001289201","Exécution des travaux de réhabilitation",null,null," ",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Evacuation de produits ou de déchets | Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP040002301","Etude SSP et ingénierie des travaux de réhabilitation","2013-10-31",null,"Diagnostic des sols réalisé par GRS Valtech\nRéalisation de 9 sondages sur l'ensemble du site\nLe rapport conclut à une absence d'impact des activités exercées par VEOLIA Propreté sur les sols du site\n","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040003701","Etude SSP et ingénierie des travaux de réhabilitation","2000-06-01",null,"HPC ENVIROTEC \n\nAu droit du bâtiment SU3\n\nÉvaluation de la qualité environnementale d’une partie de l’établissement en vue d’un futur projet de réaménagement :\n- 13 sondages sur des installations à risques, 6 autres disposés aléatoirement sur le site\n- prélèvements de gaz du sol sur 8 échantillons\n- prélèvements d’eaux souterraines sur 5 sondages\n\nSols : hydrocarbures présents au droit des sondages S10 et traces au niveau du S12. Teneurs en HAP supérieures aux valeurs de référence retenues au niveau du S9 et S7. Présence ponctuelle de métaux lourds dans les remblais contenant des mâchefers (Pb, Cu, As, Hg).\n\nEaux souterraines : présentent, au droit de l’ancienne station-service, des concentrations localisées de composés mono aromatiques (BTEX) et hydrocarbures totaux.\n\nGaz du sol : Risques de dégagement de phase organique volatile en hydrocarbures aliphatiques au droit de 7 sondages.","Air","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040003701","Etude SSP et ingénierie des travaux de réhabilitation","2000-08-01",null,"Au droit du bâtiment SU3\n\nRéalisation d’une nouvelle campagne pour caractériser :\n- l’extension spatiale des zones souillées par des hydrocabures\n- l’impact potentiel lié à la présence de cuivre\n\n15 nouveaux sondages implantés à proximité des sondages reconnus sensibles lors de la campagne de juin 2000, à savoir : S7, S14, S15, S2 et S8\n\nSols : Existence de 2 zones souillées par des hydrocarbures au niveau de la cuve d’hydrocabure souterraine et de la station de distribution d’essence\n\nGaz du sol : Pas de présence significatives d’hydrocarbures volatils sur site en dehors de la zone de l’ancienne station de distribution d’essence\n\nEaux souterraines : Extension limitée d’eaux souillées au droit de 3 zones distinctes, la zone stockage de fuel, partie nord du bâtiment F et l’ancienne station de distribution d’essence.","Air","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040003701","Etude SSP et ingénierie des travaux de réhabilitation","2000-08-01",null,"Au droit du bâtiment SU3\n\nRéalisation d’une nouvelle campagne pour caractériser :\n- l’extension spatiale des zones souillées par des hydrocabures\n- l’impact potentiel lié à la présence de cuivre\n\n15 nouveaux sondages implantés à proximité des sondages reconnus sensibles lors de la campagne de juin 2000, à savoir : S7, S14, S15, S2 et S8\n\nSols : Existence de 2 zones souillées par des hydrocarbures au niveau de la cuve d’hydrocabure souterraine et de la station de distribution d’essence\n\nGaz du sol : Pas de présence significatives d’hydrocarbures volatils sur site en dehors de la zone de l’ancienne station de distribution d’essence\n\nEaux souterraines : Extension limitée d’eaux souillées au droit de 3 zones distinctes, la zone stockage de fuel, partie nord du bâtiment F et l’ancienne station de distribution d’essence.","Eaux souterraines","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040003701","Etude SSP et ingénierie des travaux de réhabilitation","2000-06-01",null,"HPC ENVIROTEC \n\nAu droit du bâtiment SU3\n\nÉvaluation de la qualité environnementale d’une partie de l’établissement en vue d’un futur projet de réaménagement :\n- 13 sondages sur des installations à risques, 6 autres disposés aléatoirement sur le site\n- prélèvements de gaz du sol sur 8 échantillons\n- prélèvements d’eaux souterraines sur 5 sondages\n\nSols : hydrocarbures présents au droit des sondages S10 et traces au niveau du S12. Teneurs en HAP supérieures aux valeurs de référence retenues au niveau du S9 et S7. Présence ponctuelle de métaux lourds dans les remblais contenant des mâchefers (Pb, Cu, As, Hg).\n\nEaux souterraines : présentent, au droit de l’ancienne station-service, des concentrations localisées de composés mono aromatiques (BTEX) et hydrocarbures totaux.\n\nGaz du sol : Risques de dégagement de phase organique volatile en hydrocarbures aliphatiques au droit de 7 sondages.","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040003701","Etude SSP et ingénierie des travaux de réhabilitation","2000-08-01",null,"Au droit du bâtiment SU3\n\nRéalisation d’une nouvelle campagne pour caractériser :\n- l’extension spatiale des zones souillées par des hydrocabures\n- l’impact potentiel lié à la présence de cuivre\n\n15 nouveaux sondages implantés à proximité des sondages reconnus sensibles lors de la campagne de juin 2000, à savoir : S7, S14, S15, S2 et S8\n\nSols : Existence de 2 zones souillées par des hydrocarbures au niveau de la cuve d’hydrocabure souterraine et de la station de distribution d’essence\n\nGaz du sol : Pas de présence significatives d’hydrocarbures volatils sur site en dehors de la zone de l’ancienne station de distribution d’essence\n\nEaux souterraines : Extension limitée d’eaux souillées au droit de 3 zones distinctes, la zone stockage de fuel, partie nord du bâtiment F et l’ancienne station de distribution d’essence.","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040003701","Exécution des travaux de réhabilitation","2003-01-01",null,"Travaux de réhabilitation en 2003:\n\nAu droit du bâtiment SU3\n\n- Enlèvement des sols contaminés (environ 50 tonnes excavées)\n- Traitement des eaux souterraines peu profondes (pompage et écrémage), opération menée jusqu’à disparition du surnageant",null,"N/A","N/A","N/A","N/A","Travaux de dépollution"]
["SSP040004801","Etude SSP et ingénierie des travaux de réhabilitation","2002-01-01","2016-04-01","Les différents diagnostics réalisés en amont du plan de gestion mettait en avant 4 zones de pollution situées dans leur majeure partie au droit des zones excavées pour la réalisation des sous-sols :\n    • une zone impactée notablement en COHV avec une concentration maximale de 42,1 mg/kg. Il convient de noter que sur 207 analyses réalisées, des COHV sont détectés sur 114 d’entre eux ; \n    • une zone impactée en hydrocarbures totaux jusqu’au toit de la nappe avec des concentrations allant jusqu’à 23 900 mg/kg ;\n    • deux impacts ponctuels en PCB ;\n    • deux impacts localisés en HAP (en maille I12, impact non localisé dans le plan ci-dessous). \n\nPour les gaz du sol, sur l’ensemble des piézairs installés, les COHV ont été mesurés. Les concentrations mesurées dans les gaz du sol sont montées jusqu’à 3 607 mg/m³ (en E5). Des hydrocarbures volatils ont été également mesurés sur plusieurs piézairs (en S4 et E5) avec une concentration maximale de 224 mg/m³.","Air","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040004801","Etude SSP et ingénierie des travaux de réhabilitation","2020-01-22",null,"ADDENDUM A L'ANALYSE DES RISQUES\nRESIDUELS POST-TRAVAUX (réf 15-001314-DET-20.12-NOT-B01 Addendum)\n\nLe bureau d’études Arcadis a réalisé un addendum à son analyse des risques résiduels portant sur l’étude de l’impact du taux de ventilation dans le parking. Cette nouvelle analyse se justifie, car la ventilation du parking est prévue pour se déclencher suivant le taux de monoxyde de carbone mesuré en continu par des balises. Aussi, il est jugé probable l’exposition des employés ou du public fréquentant le parking, lors d’une période sans ventilation, ce que ne prenait pas en compte l’ARR présenté dans le rapport de fin de travaux du 16 décembre 2019.\nArcadis a modifié un unique paramètre sur sa modélisation qui est de fixer un taux de ventilation quasi nul de 0,01 v/h (le modèle ne prend pas en compte une ventilation nulle). Le scénario d’exposition est le suivant : bureau en RDC du bâtiment A sur 4 niveaux de sous-sol (8 h/j) et 0,5 h/j dans le parking non ventilé.\nConsidérant ces résultats et le souhait de BNP de garantir que la valeur de référence de qualité de l’air ambiant de 2,0 µg/m³ est respectée pour le public fréquentant les locaux, le bureau d’étude a calculé le taux de ventilation minimal qui devra être assuré en continu dans le parking afin que les teneurs en TCE dans l’air ambiant du parking soient en permanence inférieures à la valeur guide de 2 μg/m³.\nLe rétrocalcul a permis de conclure qu’un taux de ventilation minimal de 0,03 v/h est à respecter en continu dans le parking.\n\nLe bureau d’étude préconise 2 campagnes de prélèvements d’air ambiant au cours de la période de garantie de parfait achèvement. Il précise qu’elles seront réalisées sous mandat du maître d’ouvrage à savoir la SNC METAL 57. Ces campagnes porteraient sur les COHV, dans la mesure où ces composés contribuent significativement aux niveaux de risques. Par ailleurs, l’analyse des composés hydrocarburés pourrait être biaisée par le fonctionnement normal des bâtiments (gaz d’échappement dans le parking, etc.).","Air","Analyse des enjeux sanitaires (EQRS, ARR)","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040004801","Etude SSP et ingénierie des travaux de réhabilitation","2016-10-24",null,"Plan de gestion et Note complémentaire au PG du 31/05/2017 – ARCADIS\n\nLa définition des zones de pollutions concentrées a été réalisée uniquement sur le milieu sol, sur la base d’une bonne corrélation spatiale entre les impacts les plus importants sols, gaz du sol et eaux souterraines. Le traitement des sols aura un impact bénéfique sur la qualité des gaz du sol et également sur la nappe.\n\nAfin de définir un seuil au-delà duquel les concentrations pour un composé donné constituent une pollution concentrée, des analyses statistiques ont été faites pour 16 HAP, BTEX, HC C10-C40, COHV et PCB. Ces analyses portent sur la fréquence des concentrations mesurées et la répartition des fortes concentrations et permettent, pour chaque composé, de déterminer le bruit de fond des valeurs représentant les anomalies de pollution.\n\nLes seuils retenus sont les suivants :\n\nPour les HAP, 175 mg/kg\nPour les BETX, 5 mg/kg\nPour les PCB, 2 mg/kg\nPour les HC C10-C40, 4000 mg/kg\nPour les COHV, 7 mg/kg.\n\nIl apparaît que la majorité des zones de pollutions concentrées est présente dans la partie nord-ouest qui sera terrassée sur la base des plans projets, à l’exception :\n\n— d’une contamination en COHV localisée en partie sur le bâtiment qui sera conservé (BL2)\n— d’une contamination en 16 HAP au droit du bâtiment qui sera conservé (BL2).\n\n95 % du volume des mailles impactées présente sur l’emprise du projet seront gérées dans le cadre des travaux de réaménagement du site prévus par BNP PIE. Le volume des terres restant à traiter est estimé à 610 m3.\n\nTrois zones de pollutions concentrées, localisées hors de l’emprise des terrassements, resteront en place (une partie des mailles G8 et D12 (problématique COHV) et maille I12 (problématique HAP)). Ces zones feront l’objet de mesures de gestion complémentaires à la suite des travaux de terrassement.\n\nDans le cadre de la gestion des risques sanitaires, il restera 2 zones problématiques liées à la présence de TCE. Ces deux zones intègrent les mailles G8 et D12.\n\nLe volume estimatif des volumes à terrasser est basé sur les hypothèses suivantes :\n\n— fouille principale en R-4 : 68 080 m3\n— locaux techniques en R-1 : 6260 m3\n— décapage de l’ensemble de la superficie non concernée par l’emprise des sous-sols en vue de la réalisation d’un dallage neuf : 1410 m3.\n\nSoit au total 75 750 m3. À ces terrassements, il faut ajouter la gestion des cuttings des parois moulées, qui seront ancrées à 28 m de profondeur, soit 6840 m3 supplémentaires.\n\nPour les remblais et alluvions jusqu’à 8 m, les filières envisagées sont les suivantes :\n\n— Pour les terres qui ne présentent aucun dépassement des seuils ISDI (installation de stockage de déchets inertes) ou aucun indice susceptible de générer un refus, une ISDI.\n\n— Pour les terrains qui ne présentent que des dépassements des seuils ISDI pour la fraction soluble et les sulfates : une ancienne carrière de gypse.\n\n— Pour les terrains présentant un dépassement des seuils ISDI ou présentant des indices organoleptiques importants : un biocentre.\n\nPour les terrains présents entre 8 m et 13 m, le nombre de données analytiques disponibles est beaucoup plus réduit puisque seuls 3 sondages profonds ont été réalisés. Des investigations complémentaires vont être réalisées sur les terrains de 8 à 14 m de profondeur.\n\nÀ ce stade, les filières d’évacuation identifiées sont les mêmes que pour les tranches sus-jacentes.\n\nConcernant les parois moulées, à titre de simplification, ARCADIS a considéré l’envoi de 25 % des volumes correspondants en biocentre ou ISDND (installation de stockage de déchets non dangereux) et de 75 % des volumes restants en ISDI.\n\nConcernant le décapage pour la mise en place d’un nouveau dallage, à titre conservatoire, l’ensemble des terres concernées ont été considérées comme devant être traitées en biocentre.\n\nLa répartition finale est la suivante :\n\n— 26 847 m3 en ISDI (soit 35,5 % des terres)\n— 2578 m3 en comblement de carrières (soit 3,4 % des terres)\n— 46 305 m3 en biocentre (soit 61,1 % des terres).\n\nSur les 2 zones à traiter pour la problématique COHV, des poteaux porteurs seront présents, ces derniers assurant le soutien du bâtiment qui sera conservé et réaménagé.\n\nConcernant la problématique HAP, l’ensemble des infrastructures au droit de la maille I12 seront démolies.\n\nLes 2 techniques présélectionnées sont le traitement in-situ par venting et le traitement hors site après excavation/évacuation. Dans ce dernier cas, l’opération doit être complétée par des opérations de remblaiement.\n\nBNP ayant jugé la durée de 6 à 8 mois nécessaire pour le venting trop longue, le traitement par excavation et envoi en biocentre est privilégié.","Air","Plan de gestion","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040004801","Exécution des travaux de réhabilitation","2019-12-16",null,"Rapport de fin de travaux et ARR – ARCADIS (Réf. DET-20.10 -RPT-E02_Rapport de fin de travaux et ARR)\n\nLe rapport détaille la réalisation des travaux d'excavation sur les différentes zones avec un bilan des tonnages par filières d'élimination ainsi que les résultats des prélèvements de fonds et flans de fouille.\n\nIl présente également les résultats de l'ARR :\n\nBatiment A :\nLes valeurs modélisées au rez-de-chaussée et dans le parking sont inférieures aux valeurs repères du Haut Conseil pour la Santé Publique (HCSP).\nLe bureau d’études précise que par extrapolation, les niveaux de risques seront également acceptables pour les adultes et enfants amenés à fréquenter ce lieu. L’employé étant plus présent sur les lieux que le public de la zone commerciale.\nLe bureau d’études conclut donc à la compatibilité du terrain avec l’usage prévu tertiaire et commercial sur 4 niveaux de sous-sol.\n\nBâtiment B1 :\nLes valeurs modélisées dans le bâtiment B1 sont inférieures aux valeurs repères du Haut Conseil pour la Santé Publique (HCSP). Le bureau d’études conclut donc à la compatibilité du terrain avec l’usage prévu tertiaire.\n\nBâtiment B2 :\nLes valeurs modélisées dans le bâtiment sont inférieures aux valeurs repères du Haut Conseil pour la Santé Publique (HCSP). Le bureau d’études conclut donc à la compatibilité du terrain avec l’usage prévu tertiaire et commercial.\n\nÀ l’issue des travaux de BNP PARIBAS IMMOBILIER, le bureau d’études préconise de fixer des restrictions d’usage :\n    • Limiter à un usage tertiaire (employés et public non averti fréquentant les commerces) le rez‑de‑chaussée des bâtiments et les étages supérieurs ;\n    • Ne pas installer de poste de travail en sous-sol, sans étude préalable ;\n    • Conserver le bâtiment A sur 4 niveaux de sous-sol à usage de parking et de locaux techniques. Le taux de ventilation moyen sur une semaine du parking est de 1v/h et des locaux techniques de 0,5 v/h ;\n    • Construire les bâtiments B1 et B2 en partie sur sous-sol à usage de locaux techniques. Dans le bâtiment B1, le taux de ventilation moyen sur une semaine des locaux est au minimum de 0,5 v/h. Dans le bâtiment B2, le taux de ventilation moyen sur une semaine du hall est au minimum de 0,5 v/h et dans les bureaux et les sanitaires de 1v/h ;\n    • Recouvrir les espaces hors emprise des bâtiments et voiries par des matériaux sains (enrobé, terre d’apport propre, dalle béton) ;\n    • Ne pas installer de logements (de fonction ou autres), sans étude préalable ;\n    • Ne pas utiliser les eaux souterraines sur site pour autre chose que de la géothermie en circuit fermé (y compris pour l’arrosage des espaces verts, la climatisation, le remplissage de piscine ou de bassins d’agrément…), sans étude préalable ;\n    • Poser des canalisations AEP (Alimentation en Eau Potable) en PEHD au sein de remblai d’apport propre (de type sablon) ou dans des caniveaux techniques béton ou, à défaut, pose de canalisations métalliques ou en matériau anti-contaminant.\n      \n      Le bureau d’études précise également que les travaux doivent être faits dans des conditions permettant la protection du personnel et les déblais qui pourraient provenir de tels travaux devront être orientés vers des filières de traitement agréées.\nPar contre le bureau d’étude n’indique pas quelle forme pourrait prendre ces restrictions d’usage (SUP ou autre).","Air","N/A","N/A","N/A","N/A","Travaux de dépollution"]
["SSP040004801","Etude SSP et ingénierie des travaux de réhabilitation","2002-01-01","2016-04-01","Les différents diagnostics réalisés en amont du plan de gestion mettait en avant 4 zones de pollution situées dans leur majeure partie au droit des zones excavées pour la réalisation des sous-sols :\n    • une zone impactée notablement en COHV avec une concentration maximale de 42,1 mg/kg. Il convient de noter que sur 207 analyses réalisées, des COHV sont détectés sur 114 d’entre eux ; \n    • une zone impactée en hydrocarbures totaux jusqu’au toit de la nappe avec des concentrations allant jusqu’à 23 900 mg/kg ;\n    • deux impacts ponctuels en PCB ;\n    • deux impacts localisés en HAP (en maille I12, impact non localisé dans le plan ci-dessous). \n\nPour les gaz du sol, sur l’ensemble des piézairs installés, les COHV ont été mesurés. Les concentrations mesurées dans les gaz du sol sont montées jusqu’à 3 607 mg/m³ (en E5). Des hydrocarbures volatils ont été également mesurés sur plusieurs piézairs (en S4 et E5) avec une concentration maximale de 224 mg/m³.","Eaux souterraines","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040004801","Etude SSP et ingénierie des travaux de réhabilitation","2019-02-01",null,"Surveillance des eaux souterraines – ANTEA (Note technique n°19NT001)\n\nPour le suivi des eaux souterraines, des analyses à différents niveaux de la nappe sont réalisés (nappe des alluvions modernes, nappes des alluvions anciennes et nappe de la craie). Le dernier rapport de mesure reçu par l’inspection des installations classées concerne les mesures réalisées en février 2019.\n    • Au niveau de la zone impactée :\n      Les résultats de ce suivi montrent un impact notable de la nappe des alluvions modernes en COHV et en HCT (concentration de 38 770 µg/l en COHV notamment en Pz34 et concentration en HCT mesurée à 5 500 µg/l).\n      La nappe des alluvions anciennes est également impactée par des COHV (concentration mesurée à 2 230 µg/l en COHV en Pz136).\n      Pour la nappe de la craie, l’impact en COHV est minime à ce niveau. Le piézomètre Pz68 montre une somme des COHV de 6,8 μg/l.\n    • En aval de la zone impactée :\n      la concentration mesurée en COHV est très faible avec une concentration au maximum de 5,30 µg/l mesurée dans les alluvions anciennes (Pz146 bis)","Eaux souterraines","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040004801","Etude SSP et ingénierie des travaux de réhabilitation","2019-10-22",null,"Suivi fonctionnement de la barrière hydraulique – SITA REMEDIATION (Note de suivi n°05 – octobre 2019)","Eaux souterraines","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040004801","Etude SSP et ingénierie des travaux de réhabilitation","2016-10-24",null,"Plan de gestion et Note complémentaire au PG du 31/05/2017 – ARCADIS\n\nLa définition des zones de pollutions concentrées a été réalisée uniquement sur le milieu sol, sur la base d’une bonne corrélation spatiale entre les impacts les plus importants sols, gaz du sol et eaux souterraines. Le traitement des sols aura un impact bénéfique sur la qualité des gaz du sol et également sur la nappe.\n\nAfin de définir un seuil au-delà duquel les concentrations pour un composé donné constituent une pollution concentrée, des analyses statistiques ont été faites pour 16 HAP, BTEX, HC C10-C40, COHV et PCB. Ces analyses portent sur la fréquence des concentrations mesurées et la répartition des fortes concentrations et permettent, pour chaque composé, de déterminer le bruit de fond des valeurs représentant les anomalies de pollution.\n\nLes seuils retenus sont les suivants :\n\nPour les HAP, 175 mg/kg\nPour les BETX, 5 mg/kg\nPour les PCB, 2 mg/kg\nPour les HC C10-C40, 4000 mg/kg\nPour les COHV, 7 mg/kg.\n\nIl apparaît que la majorité des zones de pollutions concentrées est présente dans la partie nord-ouest qui sera terrassée sur la base des plans projets, à l’exception :\n\n— d’une contamination en COHV localisée en partie sur le bâtiment qui sera conservé (BL2)\n— d’une contamination en 16 HAP au droit du bâtiment qui sera conservé (BL2).\n\n95 % du volume des mailles impactées présente sur l’emprise du projet seront gérées dans le cadre des travaux de réaménagement du site prévus par BNP PIE. Le volume des terres restant à traiter est estimé à 610 m3.\n\nTrois zones de pollutions concentrées, localisées hors de l’emprise des terrassements, resteront en place (une partie des mailles G8 et D12 (problématique COHV) et maille I12 (problématique HAP)). Ces zones feront l’objet de mesures de gestion complémentaires à la suite des travaux de terrassement.\n\nDans le cadre de la gestion des risques sanitaires, il restera 2 zones problématiques liées à la présence de TCE. Ces deux zones intègrent les mailles G8 et D12.\n\nLe volume estimatif des volumes à terrasser est basé sur les hypothèses suivantes :\n\n— fouille principale en R-4 : 68 080 m3\n— locaux techniques en R-1 : 6260 m3\n— décapage de l’ensemble de la superficie non concernée par l’emprise des sous-sols en vue de la réalisation d’un dallage neuf : 1410 m3.\n\nSoit au total 75 750 m3. À ces terrassements, il faut ajouter la gestion des cuttings des parois moulées, qui seront ancrées à 28 m de profondeur, soit 6840 m3 supplémentaires.\n\nPour les remblais et alluvions jusqu’à 8 m, les filières envisagées sont les suivantes :\n\n— Pour les terres qui ne présentent aucun dépassement des seuils ISDI (installation de stockage de déchets inertes) ou aucun indice susceptible de générer un refus, une ISDI.\n\n— Pour les terrains qui ne présentent que des dépassements des seuils ISDI pour la fraction soluble et les sulfates : une ancienne carrière de gypse.\n\n— Pour les terrains présentant un dépassement des seuils ISDI ou présentant des indices organoleptiques importants : un biocentre.\n\nPour les terrains présents entre 8 m et 13 m, le nombre de données analytiques disponibles est beaucoup plus réduit puisque seuls 3 sondages profonds ont été réalisés. Des investigations complémentaires vont être réalisées sur les terrains de 8 à 14 m de profondeur.\n\nÀ ce stade, les filières d’évacuation identifiées sont les mêmes que pour les tranches sus-jacentes.\n\nConcernant les parois moulées, à titre de simplification, ARCADIS a considéré l’envoi de 25 % des volumes correspondants en biocentre ou ISDND (installation de stockage de déchets non dangereux) et de 75 % des volumes restants en ISDI.\n\nConcernant le décapage pour la mise en place d’un nouveau dallage, à titre conservatoire, l’ensemble des terres concernées ont été considérées comme devant être traitées en biocentre.\n\nLa répartition finale est la suivante :\n\n— 26 847 m3 en ISDI (soit 35,5 % des terres)\n— 2578 m3 en comblement de carrières (soit 3,4 % des terres)\n— 46 305 m3 en biocentre (soit 61,1 % des terres).\n\nSur les 2 zones à traiter pour la problématique COHV, des poteaux porteurs seront présents, ces derniers assurant le soutien du bâtiment qui sera conservé et réaménagé.\n\nConcernant la problématique HAP, l’ensemble des infrastructures au droit de la maille I12 seront démolies.\n\nLes 2 techniques présélectionnées sont le traitement in-situ par venting et le traitement hors site après excavation/évacuation. Dans ce dernier cas, l’opération doit être complétée par des opérations de remblaiement.\n\nBNP ayant jugé la durée de 6 à 8 mois nécessaire pour le venting trop longue, le traitement par excavation et envoi en biocentre est privilégié.","Eaux souterraines","Plan de gestion","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040004801","Etude SSP et ingénierie des travaux de réhabilitation","2017-04-28",null,"Plan de gestion – Rapport SERPOL n°8389 – VA\n\nRENAULT, en sa qualité d’ancien exploitant du bâtiment Squarecom, a mandaté SERPOL pour la réalisation d’essais de faisabilité pour l’identification et le dimensionnement préliminaire d’une solution de traitement des impacts résiduels situés à l’extérieur de l’emprise du futur bâtiment BNP PIE.\n\nLa surveillance des eaux souterraines hors emprise du bâtiment montre la présence d’impacts en solvants chlorés et en hydrocarbures. A ce jour, une barrière hydraulique permet de traiter les eaux souterraines impactées par des solvants chlorés et des hydrocarbures et de confiner l’impact au droit du bâtiment. Les eaux pompées sont traitées par stripping avant rejet au réseau d’assainissement, les vapeurs extraites étant traitées sur filtres à charbon actif. La barrière hydraulique est opérée par SUEZ Environnement.\n\nAprès construction du bâtiment, la source principale des impacts aura été supprimée et SERPOL considère que le maintien de la barrière hydraulique dans sa configuration actuelle n’est pas justifié. Cependant, de nouvelles mesures de gestion des impacts résiduels dans les sols et les eaux souterraines doivent être définis.\n\nLes contraintes liées à l’environnement du site devant être prises en compte dans le bilan coûts-avantages sont les suivantes :\n\n— la barrière hydraulique actuelle est localisée sur une emprise publique,\n— de nombreux réseaux existent au droit et à proximité de cette zone,\n— le local technique abritant les installations de traitement est situé au sous-sol du bâtiment BL1, qui sera démoli.\n— les immeubles environnants abritent principalement des logements : les travaux de dépollution devront limiter les nuisances aux riverains,\n— dans le cadre du projet d’aménagement, la mise en place d’une tente est envisagée pour éviter les émanations de vapeurs de solvants chlorés pendant le chantier de terrassement. La tente occupera le domaine public sur une largeur de 2 m au-delà de la limite actuelle du bâtiment,\n— les environs immédiats du site ont été récemment aménagés et sont constitués principalement d’espaces publics.\n\nEn raison de ces contraintes, les solutions de traitement hors site (excavation et élimination) ou sur site (excavation et traitement sur place) ne sont pas envisageables. Seules des techniques de traitement in situ peuvent être mises en œuvre.\n\nLes solutions de traitement par oxydation ou réduction chimique ou par stimulation de la biodégradation ont semblé les plus adaptées. Selon SERPOL, ces 2 techniques ne présentent pas d’interaction avec le projet BNPPIE et peuvent être réalisées en parallèle du projet de réaménagement, après la construction des parois moulées.Afin de garantir l’absence de migration des impacts vers les récepteurs sensibles du voisinage, il serait possible de coupler le traitement chimique ou biologique des eaux souterraines et l’action de confinement de la barrière hydraulique. En effet, le pompage des eaux souterraines permet une diffusion rapide des réactifs au sein de la zone à traiter. Après une période de 6 à 12 mois et l’observation de la baisse des concentrations, les installations de pompage pourraient être démantelées, le traitement se poursuivant par diffusion passive des réactifs.\n\nDes études complémentaires sont cependant nécessaires pour caractériser les conditions hydrogéologiques, influencées par la mise en place de la paroi moulée, ainsi que les conditions physico-chimiques des eaux souterraines pour identifier les réactifs les plus efficaces et leur dosage.\n\nIl n’apparaît pas pertinent de démarrer un traitement de la zone tant que la voie de migration des impacts n’est pas coupée par l’installation de la paroi moulée.En fin de terrassement au droit de l’emprise du projet BNPPIE, des contrôles de la qualité des sols seront réalisés, qui permettront de déterminer si un traitement complémentaire est nécessaire avant la pose du radier. Ce traitement pourra consister en un malaxage des sols du fond de fouille avec des réactifs permettant de dégrader les solvants chlorés (oxydation ou réduction chimique en fonction des caractéristiques physico-chimiques du milieu).","Eaux souterraines","Plan de gestion","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040004801","Exécution des travaux de réhabilitation","2019-12-16",null,"Rapport de fin de travaux et ARR – ARCADIS (Réf. DET-20.10 -RPT-E02_Rapport de fin de travaux et ARR)\n\nLe rapport détaille la réalisation des travaux d'excavation sur les différentes zones avec un bilan des tonnages par filières d'élimination ainsi que les résultats des prélèvements de fonds et flans de fouille.\n\nIl présente également les résultats de l'ARR :\n\nBatiment A :\nLes valeurs modélisées au rez-de-chaussée et dans le parking sont inférieures aux valeurs repères du Haut Conseil pour la Santé Publique (HCSP).\nLe bureau d’études précise que par extrapolation, les niveaux de risques seront également acceptables pour les adultes et enfants amenés à fréquenter ce lieu. L’employé étant plus présent sur les lieux que le public de la zone commerciale.\nLe bureau d’études conclut donc à la compatibilité du terrain avec l’usage prévu tertiaire et commercial sur 4 niveaux de sous-sol.\n\nBâtiment B1 :\nLes valeurs modélisées dans le bâtiment B1 sont inférieures aux valeurs repères du Haut Conseil pour la Santé Publique (HCSP). Le bureau d’études conclut donc à la compatibilité du terrain avec l’usage prévu tertiaire.\n\nBâtiment B2 :\nLes valeurs modélisées dans le bâtiment sont inférieures aux valeurs repères du Haut Conseil pour la Santé Publique (HCSP). Le bureau d’études conclut donc à la compatibilité du terrain avec l’usage prévu tertiaire et commercial.\n\nÀ l’issue des travaux de BNP PARIBAS IMMOBILIER, le bureau d’études préconise de fixer des restrictions d’usage :\n    • Limiter à un usage tertiaire (employés et public non averti fréquentant les commerces) le rez‑de‑chaussée des bâtiments et les étages supérieurs ;\n    • Ne pas installer de poste de travail en sous-sol, sans étude préalable ;\n    • Conserver le bâtiment A sur 4 niveaux de sous-sol à usage de parking et de locaux techniques. Le taux de ventilation moyen sur une semaine du parking est de 1v/h et des locaux techniques de 0,5 v/h ;\n    • Construire les bâtiments B1 et B2 en partie sur sous-sol à usage de locaux techniques. Dans le bâtiment B1, le taux de ventilation moyen sur une semaine des locaux est au minimum de 0,5 v/h. Dans le bâtiment B2, le taux de ventilation moyen sur une semaine du hall est au minimum de 0,5 v/h et dans les bureaux et les sanitaires de 1v/h ;\n    • Recouvrir les espaces hors emprise des bâtiments et voiries par des matériaux sains (enrobé, terre d’apport propre, dalle béton) ;\n    • Ne pas installer de logements (de fonction ou autres), sans étude préalable ;\n    • Ne pas utiliser les eaux souterraines sur site pour autre chose que de la géothermie en circuit fermé (y compris pour l’arrosage des espaces verts, la climatisation, le remplissage de piscine ou de bassins d’agrément…), sans étude préalable ;\n    • Poser des canalisations AEP (Alimentation en Eau Potable) en PEHD au sein de remblai d’apport propre (de type sablon) ou dans des caniveaux techniques béton ou, à défaut, pose de canalisations métalliques ou en matériau anti-contaminant.\n      \n      Le bureau d’études précise également que les travaux doivent être faits dans des conditions permettant la protection du personnel et les déblais qui pourraient provenir de tels travaux devront être orientés vers des filières de traitement agréées.\nPar contre le bureau d’étude n’indique pas quelle forme pourrait prendre ces restrictions d’usage (SUP ou autre).","Eaux souterraines","N/A","N/A","N/A","N/A","Travaux de dépollution"]
["SSP040004801","Exécution des travaux de réhabilitation","2019-10-22",null,"Suivi fonctionnement de la barrière hydraulique – SITA REMEDIATION (Note de suivi n°05 – octobre 2019)","Eaux souterraines","N/A","N/A","N/A","N/A","Mise en place de mesure de réhabilitation",null,"N/A","N/A","N/A"]
["SSP040004801","Etude SSP et ingénierie des travaux de réhabilitation","2002-01-01","2016-04-01","Les différents diagnostics réalisés en amont du plan de gestion mettait en avant 4 zones de pollution situées dans leur majeure partie au droit des zones excavées pour la réalisation des sous-sols :\n    • une zone impactée notablement en COHV avec une concentration maximale de 42,1 mg/kg. Il convient de noter que sur 207 analyses réalisées, des COHV sont détectés sur 114 d’entre eux ; \n    • une zone impactée en hydrocarbures totaux jusqu’au toit de la nappe avec des concentrations allant jusqu’à 23 900 mg/kg ;\n    • deux impacts ponctuels en PCB ;\n    • deux impacts localisés en HAP (en maille I12, impact non localisé dans le plan ci-dessous). \n\nPour les gaz du sol, sur l’ensemble des piézairs installés, les COHV ont été mesurés. Les concentrations mesurées dans les gaz du sol sont montées jusqu’à 3 607 mg/m³ (en E5). Des hydrocarbures volatils ont été également mesurés sur plusieurs piézairs (en S4 et E5) avec une concentration maximale de 224 mg/m³.","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040004801","Etude SSP et ingénierie des travaux de réhabilitation","2020-01-22",null,"ADDENDUM A L'ANALYSE DES RISQUES\nRESIDUELS POST-TRAVAUX (réf 15-001314-DET-20.12-NOT-B01 Addendum)\n\nLe bureau d’études Arcadis a réalisé un addendum à son analyse des risques résiduels portant sur l’étude de l’impact du taux de ventilation dans le parking. Cette nouvelle analyse se justifie, car la ventilation du parking est prévue pour se déclencher suivant le taux de monoxyde de carbone mesuré en continu par des balises. Aussi, il est jugé probable l’exposition des employés ou du public fréquentant le parking, lors d’une période sans ventilation, ce que ne prenait pas en compte l’ARR présenté dans le rapport de fin de travaux du 16 décembre 2019.\nArcadis a modifié un unique paramètre sur sa modélisation qui est de fixer un taux de ventilation quasi nul de 0,01 v/h (le modèle ne prend pas en compte une ventilation nulle). Le scénario d’exposition est le suivant : bureau en RDC du bâtiment A sur 4 niveaux de sous-sol (8 h/j) et 0,5 h/j dans le parking non ventilé.\nConsidérant ces résultats et le souhait de BNP de garantir que la valeur de référence de qualité de l’air ambiant de 2,0 µg/m³ est respectée pour le public fréquentant les locaux, le bureau d’étude a calculé le taux de ventilation minimal qui devra être assuré en continu dans le parking afin que les teneurs en TCE dans l’air ambiant du parking soient en permanence inférieures à la valeur guide de 2 μg/m³.\nLe rétrocalcul a permis de conclure qu’un taux de ventilation minimal de 0,03 v/h est à respecter en continu dans le parking.\n\nLe bureau d’étude préconise 2 campagnes de prélèvements d’air ambiant au cours de la période de garantie de parfait achèvement. Il précise qu’elles seront réalisées sous mandat du maître d’ouvrage à savoir la SNC METAL 57. Ces campagnes porteraient sur les COHV, dans la mesure où ces composés contribuent significativement aux niveaux de risques. Par ailleurs, l’analyse des composés hydrocarburés pourrait être biaisée par le fonctionnement normal des bâtiments (gaz d’échappement dans le parking, etc.).","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040004801","Etude SSP et ingénierie des travaux de réhabilitation","2016-10-24",null,"Plan de gestion et Note complémentaire au PG du 31/05/2017 – ARCADIS\n\nLa définition des zones de pollutions concentrées a été réalisée uniquement sur le milieu sol, sur la base d’une bonne corrélation spatiale entre les impacts les plus importants sols, gaz du sol et eaux souterraines. Le traitement des sols aura un impact bénéfique sur la qualité des gaz du sol et également sur la nappe.\n\nAfin de définir un seuil au-delà duquel les concentrations pour un composé donné constituent une pollution concentrée, des analyses statistiques ont été faites pour 16 HAP, BTEX, HC C10-C40, COHV et PCB. Ces analyses portent sur la fréquence des concentrations mesurées et la répartition des fortes concentrations et permettent, pour chaque composé, de déterminer le bruit de fond des valeurs représentant les anomalies de pollution.\n\nLes seuils retenus sont les suivants :\n\nPour les HAP, 175 mg/kg\nPour les BETX, 5 mg/kg\nPour les PCB, 2 mg/kg\nPour les HC C10-C40, 4000 mg/kg\nPour les COHV, 7 mg/kg.\n\nIl apparaît que la majorité des zones de pollutions concentrées est présente dans la partie nord-ouest qui sera terrassée sur la base des plans projets, à l’exception :\n\n— d’une contamination en COHV localisée en partie sur le bâtiment qui sera conservé (BL2)\n— d’une contamination en 16 HAP au droit du bâtiment qui sera conservé (BL2).\n\n95 % du volume des mailles impactées présente sur l’emprise du projet seront gérées dans le cadre des travaux de réaménagement du site prévus par BNP PIE. Le volume des terres restant à traiter est estimé à 610 m3.\n\nTrois zones de pollutions concentrées, localisées hors de l’emprise des terrassements, resteront en place (une partie des mailles G8 et D12 (problématique COHV) et maille I12 (problématique HAP)). Ces zones feront l’objet de mesures de gestion complémentaires à la suite des travaux de terrassement.\n\nDans le cadre de la gestion des risques sanitaires, il restera 2 zones problématiques liées à la présence de TCE. Ces deux zones intègrent les mailles G8 et D12.\n\nLe volume estimatif des volumes à terrasser est basé sur les hypothèses suivantes :\n\n— fouille principale en R-4 : 68 080 m3\n— locaux techniques en R-1 : 6260 m3\n— décapage de l’ensemble de la superficie non concernée par l’emprise des sous-sols en vue de la réalisation d’un dallage neuf : 1410 m3.\n\nSoit au total 75 750 m3. À ces terrassements, il faut ajouter la gestion des cuttings des parois moulées, qui seront ancrées à 28 m de profondeur, soit 6840 m3 supplémentaires.\n\nPour les remblais et alluvions jusqu’à 8 m, les filières envisagées sont les suivantes :\n\n— Pour les terres qui ne présentent aucun dépassement des seuils ISDI (installation de stockage de déchets inertes) ou aucun indice susceptible de générer un refus, une ISDI.\n\n— Pour les terrains qui ne présentent que des dépassements des seuils ISDI pour la fraction soluble et les sulfates : une ancienne carrière de gypse.\n\n— Pour les terrains présentant un dépassement des seuils ISDI ou présentant des indices organoleptiques importants : un biocentre.\n\nPour les terrains présents entre 8 m et 13 m, le nombre de données analytiques disponibles est beaucoup plus réduit puisque seuls 3 sondages profonds ont été réalisés. Des investigations complémentaires vont être réalisées sur les terrains de 8 à 14 m de profondeur.\n\nÀ ce stade, les filières d’évacuation identifiées sont les mêmes que pour les tranches sus-jacentes.\n\nConcernant les parois moulées, à titre de simplification, ARCADIS a considéré l’envoi de 25 % des volumes correspondants en biocentre ou ISDND (installation de stockage de déchets non dangereux) et de 75 % des volumes restants en ISDI.\n\nConcernant le décapage pour la mise en place d’un nouveau dallage, à titre conservatoire, l’ensemble des terres concernées ont été considérées comme devant être traitées en biocentre.\n\nLa répartition finale est la suivante :\n\n— 26 847 m3 en ISDI (soit 35,5 % des terres)\n— 2578 m3 en comblement de carrières (soit 3,4 % des terres)\n— 46 305 m3 en biocentre (soit 61,1 % des terres).\n\nSur les 2 zones à traiter pour la problématique COHV, des poteaux porteurs seront présents, ces derniers assurant le soutien du bâtiment qui sera conservé et réaménagé.\n\nConcernant la problématique HAP, l’ensemble des infrastructures au droit de la maille I12 seront démolies.\n\nLes 2 techniques présélectionnées sont le traitement in-situ par venting et le traitement hors site après excavation/évacuation. Dans ce dernier cas, l’opération doit être complétée par des opérations de remblaiement.\n\nBNP ayant jugé la durée de 6 à 8 mois nécessaire pour le venting trop longue, le traitement par excavation et envoi en biocentre est privilégié.","Sol - Sous-sol","Plan de gestion","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040004801","Etude SSP et ingénierie des travaux de réhabilitation","2017-04-28",null,"Plan de gestion – Rapport SERPOL n°8389 – VA\n\nRENAULT, en sa qualité d’ancien exploitant du bâtiment Squarecom, a mandaté SERPOL pour la réalisation d’essais de faisabilité pour l’identification et le dimensionnement préliminaire d’une solution de traitement des impacts résiduels situés à l’extérieur de l’emprise du futur bâtiment BNP PIE.\n\nLa surveillance des eaux souterraines hors emprise du bâtiment montre la présence d’impacts en solvants chlorés et en hydrocarbures. A ce jour, une barrière hydraulique permet de traiter les eaux souterraines impactées par des solvants chlorés et des hydrocarbures et de confiner l’impact au droit du bâtiment. Les eaux pompées sont traitées par stripping avant rejet au réseau d’assainissement, les vapeurs extraites étant traitées sur filtres à charbon actif. La barrière hydraulique est opérée par SUEZ Environnement.\n\nAprès construction du bâtiment, la source principale des impacts aura été supprimée et SERPOL considère que le maintien de la barrière hydraulique dans sa configuration actuelle n’est pas justifié. Cependant, de nouvelles mesures de gestion des impacts résiduels dans les sols et les eaux souterraines doivent être définis.\n\nLes contraintes liées à l’environnement du site devant être prises en compte dans le bilan coûts-avantages sont les suivantes :\n\n— la barrière hydraulique actuelle est localisée sur une emprise publique,\n— de nombreux réseaux existent au droit et à proximité de cette zone,\n— le local technique abritant les installations de traitement est situé au sous-sol du bâtiment BL1, qui sera démoli.\n— les immeubles environnants abritent principalement des logements : les travaux de dépollution devront limiter les nuisances aux riverains,\n— dans le cadre du projet d’aménagement, la mise en place d’une tente est envisagée pour éviter les émanations de vapeurs de solvants chlorés pendant le chantier de terrassement. La tente occupera le domaine public sur une largeur de 2 m au-delà de la limite actuelle du bâtiment,\n— les environs immédiats du site ont été récemment aménagés et sont constitués principalement d’espaces publics.\n\nEn raison de ces contraintes, les solutions de traitement hors site (excavation et élimination) ou sur site (excavation et traitement sur place) ne sont pas envisageables. Seules des techniques de traitement in situ peuvent être mises en œuvre.\n\nLes solutions de traitement par oxydation ou réduction chimique ou par stimulation de la biodégradation ont semblé les plus adaptées. Selon SERPOL, ces 2 techniques ne présentent pas d’interaction avec le projet BNPPIE et peuvent être réalisées en parallèle du projet de réaménagement, après la construction des parois moulées.Afin de garantir l’absence de migration des impacts vers les récepteurs sensibles du voisinage, il serait possible de coupler le traitement chimique ou biologique des eaux souterraines et l’action de confinement de la barrière hydraulique. En effet, le pompage des eaux souterraines permet une diffusion rapide des réactifs au sein de la zone à traiter. Après une période de 6 à 12 mois et l’observation de la baisse des concentrations, les installations de pompage pourraient être démantelées, le traitement se poursuivant par diffusion passive des réactifs.\n\nDes études complémentaires sont cependant nécessaires pour caractériser les conditions hydrogéologiques, influencées par la mise en place de la paroi moulée, ainsi que les conditions physico-chimiques des eaux souterraines pour identifier les réactifs les plus efficaces et leur dosage.\n\nIl n’apparaît pas pertinent de démarrer un traitement de la zone tant que la voie de migration des impacts n’est pas coupée par l’installation de la paroi moulée.En fin de terrassement au droit de l’emprise du projet BNPPIE, des contrôles de la qualité des sols seront réalisés, qui permettront de déterminer si un traitement complémentaire est nécessaire avant la pose du radier. Ce traitement pourra consister en un malaxage des sols du fond de fouille avec des réactifs permettant de dégrader les solvants chlorés (oxydation ou réduction chimique en fonction des caractéristiques physico-chimiques du milieu).","Sol - Sous-sol","Plan de gestion","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040004801","Exécution des travaux de réhabilitation","2019-12-16",null,"Rapport de fin de travaux et ARR – ARCADIS (Réf. DET-20.10 -RPT-E02_Rapport de fin de travaux et ARR)\n\nLe rapport détaille la réalisation des travaux d'excavation sur les différentes zones avec un bilan des tonnages par filières d'élimination ainsi que les résultats des prélèvements de fonds et flans de fouille.\n\nIl présente également les résultats de l'ARR :\n\nBatiment A :\nLes valeurs modélisées au rez-de-chaussée et dans le parking sont inférieures aux valeurs repères du Haut Conseil pour la Santé Publique (HCSP).\nLe bureau d’études précise que par extrapolation, les niveaux de risques seront également acceptables pour les adultes et enfants amenés à fréquenter ce lieu. L’employé étant plus présent sur les lieux que le public de la zone commerciale.\nLe bureau d’études conclut donc à la compatibilité du terrain avec l’usage prévu tertiaire et commercial sur 4 niveaux de sous-sol.\n\nBâtiment B1 :\nLes valeurs modélisées dans le bâtiment B1 sont inférieures aux valeurs repères du Haut Conseil pour la Santé Publique (HCSP). Le bureau d’études conclut donc à la compatibilité du terrain avec l’usage prévu tertiaire.\n\nBâtiment B2 :\nLes valeurs modélisées dans le bâtiment sont inférieures aux valeurs repères du Haut Conseil pour la Santé Publique (HCSP). Le bureau d’études conclut donc à la compatibilité du terrain avec l’usage prévu tertiaire et commercial.\n\nÀ l’issue des travaux de BNP PARIBAS IMMOBILIER, le bureau d’études préconise de fixer des restrictions d’usage :\n    • Limiter à un usage tertiaire (employés et public non averti fréquentant les commerces) le rez‑de‑chaussée des bâtiments et les étages supérieurs ;\n    • Ne pas installer de poste de travail en sous-sol, sans étude préalable ;\n    • Conserver le bâtiment A sur 4 niveaux de sous-sol à usage de parking et de locaux techniques. Le taux de ventilation moyen sur une semaine du parking est de 1v/h et des locaux techniques de 0,5 v/h ;\n    • Construire les bâtiments B1 et B2 en partie sur sous-sol à usage de locaux techniques. Dans le bâtiment B1, le taux de ventilation moyen sur une semaine des locaux est au minimum de 0,5 v/h. Dans le bâtiment B2, le taux de ventilation moyen sur une semaine du hall est au minimum de 0,5 v/h et dans les bureaux et les sanitaires de 1v/h ;\n    • Recouvrir les espaces hors emprise des bâtiments et voiries par des matériaux sains (enrobé, terre d’apport propre, dalle béton) ;\n    • Ne pas installer de logements (de fonction ou autres), sans étude préalable ;\n    • Ne pas utiliser les eaux souterraines sur site pour autre chose que de la géothermie en circuit fermé (y compris pour l’arrosage des espaces verts, la climatisation, le remplissage de piscine ou de bassins d’agrément…), sans étude préalable ;\n    • Poser des canalisations AEP (Alimentation en Eau Potable) en PEHD au sein de remblai d’apport propre (de type sablon) ou dans des caniveaux techniques béton ou, à défaut, pose de canalisations métalliques ou en matériau anti-contaminant.\n      \n      Le bureau d’études précise également que les travaux doivent être faits dans des conditions permettant la protection du personnel et les déblais qui pourraient provenir de tels travaux devront être orientés vers des filières de traitement agréées.\nPar contre le bureau d’étude n’indique pas quelle forme pourrait prendre ces restrictions d’usage (SUP ou autre).","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution"]
["SSP040004901","Etude SSP et ingénierie des travaux de réhabilitation","2014-06-02",null,"Diagnostic initial 02/06/2014\nLe diagnostic de l’état du sous-sol transmis par l’exploitant comprend :\n- une étude historique et documentaire des activités exercées sur le site,\n- une présentation des investigations réalisées sur le site.",null,"Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040004901","Etude SSP et ingénierie des travaux de réhabilitation","2018-03-04",null,"Rapport d’installation de 3 piézomètres.\n\nL’intervention a été réalisée les 3 et 4 mars 2018 et a consisté en la réalisation de 3 piézomètres à 10m de profondeur, Auncune venue d’eau n’a été détactée au cours des investigations et aucune trace d’éventuelle pollution n’a été relevée au droit des sondages.",null,"Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040004901","Exécution des travaux de réhabilitation","2017-09-04",null,"Démantèlement et remise en état de l’ancienne station service Combustible de Boulogne .\n\nDans le cadre de la remise en état du site, les 3 cuves et le séparateur d’hydrocarbures ont été nettoyés et dégazés les 19 et 20 juin 2017.\nLes cuves, une fois découpées, ont été transportées et éliminées dans un centre spécialisé.\nLes matériaux issus du démantèlement ont été triés sur place avant leur évacuation vers les centre spécialisés. Après l’évacuation des cuves et des bétons, il a été procédé à :\n- l’excavation des terres présentant des indices de souillure et le stockage dans un tas à part des terres inertes,\n- le tri des matériaux grossiers,\n- le chargement des terres contaminées pour évacuation en filière.\n\nDes prélèvements ont été effectués en fond et flancs de fouille afin de vérifier l’état des sols laissés en place à la suite des travaux d’excavation, Huit échantillons de réception ont été réalisés.\nLes résultats d’analyses indiquent :\n- l’absence de teneurs en HAP pour tous les échantillons analysés,\n- la présence de traces de BTEX au droit des échantillons ER5 et FF2 tout en restant inférieurs aux seuils définis,\n- la présence en HCT pour tous les échantillons analysés tout en restant inférieurs aux seuils définis à l’exception des échantillons ER4 (10 000 mg/kg) et ER5 (1 000 mg/kg).\n\nLes excavations au droit des échantillons ER4 et ER5 n’ont pas pu continuer en raison de la présence en limite de propriété du trottoir et des réseaux divers présents à ce niveau (limite technique).",null,"N/A","N/A","N/A","N/A","Travaux de dépollution"]
["SSP040005001","Etude SSP et ingénierie des travaux de réhabilitation","2017-08-31",null,"Plan de terrassement GINGER/BURGEAP 31/08/2017\n\nBOUYGUES CONSTRUCTION & RAZEL BEC a mandaté BURGEAP pour une mission d’assistance afin de gérer les terres impactées lors des travaux d’enlèvement des cuves.\n\nL’ensemble des observations et résultats effectués lors des précédents diagnostics a donc été synthétisé afin d’élaborer des plans de terrassements concernant la gestion des terres.\n\nAu total, environ 350 m3 de terres semblent impactées par des hydrocarbures et devront faire l’objet d’une évacuation hors site vers une filière adaptée (ISDND) lors des travaux d’enlèvement des cuves enterrées, et ne pourront être réutilisées sur site.",null,"Plan de conception des travaux (PCT)","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040005001","Etude SSP et ingénierie des travaux de réhabilitation","2018-04-09",null,"Rapport de prélèvement et analyse en fond et bord de fouille et ARR - BURGEAP\n\nBURGEAP conclut que l’état environnemental du site est compatible avec l’usage industriel prévu. A titre de rappel, le SIAAP conserve l’usage de son terrain pour l’implantation de l’usine de pré-traitement.",null,"Analyse des enjeux sanitaires (EQRS, ARR)","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040005301","Etude SSP et ingénierie des travaux de réhabilitation","2007-11-01",null,"Étude historique et documentaire réalisée par ANTEA (rapport référencé A.47754/A).\nL'étude a permis d'identifier 8 sources potentielles de pollution.","Eaux souterraines","Etude historique, documentaire et mémorielle","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040005301","Etude SSP et ingénierie des travaux de réhabilitation","2007-11-01",null,"Étude historique et documentaire réalisée par ANTEA (rapport référencé A.47754/A).\nL'étude a permis d'identifier 8 sources potentielles de pollution.","Sol - Sous-sol","Etude historique, documentaire et mémorielle","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040005301","Etude SSP et ingénierie des travaux de réhabilitation","2014-05-01",null,"Diagnostic environnemental – ARCADIS AFR-DIA905-09-0186-RPT-A02\n\nLes investigations de sols ont consisté en la réalisation de 5 sondages de sol entre 2 et 6m  de prof. En avril 2014. Le rapport indique que les sondages n’ont rencontré aucune eau souterraine.\n\nLes principaux résultats des analyses indiquent :\n- des traces d’hydrocarbures C10-C40 sur 3 sondages, avec un maximum de 97,9 mg/kg au point S4 entre 3 et 4 m de prof.\n- des teneurs inférieures à la limite de quantification pour les hydrocarbures  volatils (C5-C10) et les BTEX.\n\nLes teneurs en hydrocarbures C10-C40 observées sont très inférieures au seuil d’acceptation en ISDI (500 mg/kg).\nLe rapport conclut à l’absence de risque sanitaire suspecté, étant donné l’absence d’impact notable.","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040007701","Etude SSP et ingénierie des travaux de réhabilitation","2008-10-31",null,"Étude des eaux souterraines.",null,"Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040008501","Etude SSP et ingénierie des travaux de réhabilitation","2011-03-01",null,"Diagnostic ICF Environnement.\n\nConcernant les sols, 8 sondages de sol avaient été effectués en 2012 jusqu’à des profondeurs comprises entre 5,5 m et 6 m. Les investigations réalisées n’avaient pas mis en évidence d’impact notable en composés organiques au droit des sondages de sol réalisés (teneurs maximales de 85 mg/kg pour les HCT, 36 mg/kg pour la somme des HAP et teneurs traces localisées en BTEX, COHV et PCB). Des anomalies en métaux avaient été mises en évidence sur les remblais uniquement.\n\nLes eaux souterraines ne sont pas rencontrées au droit du site","Eaux souterraines","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040008501","Etude SSP et ingénierie des travaux de réhabilitation","2011-03-01",null,"Diagnostic ICF Environnement.\n\nConcernant les sols, 8 sondages de sol avaient été effectués en 2012 jusqu’à des profondeurs comprises entre 5,5 m et 6 m. Les investigations réalisées n’avaient pas mis en évidence d’impact notable en composés organiques au droit des sondages de sol réalisés (teneurs maximales de 85 mg/kg pour les HCT, 36 mg/kg pour la somme des HAP et teneurs traces localisées en BTEX, COHV et PCB). Des anomalies en métaux avaient été mises en évidence sur les remblais uniquement.\n\nLes eaux souterraines ne sont pas rencontrées au droit du site","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040008501","Etude SSP et ingénierie des travaux de réhabilitation","2017-05-05",null,"Diagnostic  AECOM, PAR-RAP-17-18644B\n\nLes investigations de 2017 réalisées par la société AECOM n’ont concerné que le prélèvement d’échantillons de sol en parois et fonds de fouille au droit des 2 anciennes cuves, suite à leur retrait. Il a été constaté les impacts suivants :\n- au niveau de la cuve n°1 : des teneurs élevées en hydrocarbures totaux (entre 3 400 mg/kg et 18 000 mg/kg) et la présence de HAP (21 mg/kg) et de BTEX (86 mg/kg) ;\n- au niveau de la cuve n°2 : des teneurs élevées en hydrocarbures totaux (entre 6 600 mg/kg et 9 900 mg/kg) et la présence de HAP (4,4 mg/kg) et de BTEX (2,3 mg/kg).\nLe bureau d’étude a alors précisé que les zones des cuves n°1 et n°2 sont situées au droit des futurs sous-sols et que leur excavation est ainsi prévue dans le cadre des travaux de réaménagement du site. Les excavations sont prévues jusqu’à une profondeur d’environ 11 mètres alors que le fond des cuves était situé à une profondeur de 4 mètres.",null,"Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040008501","Etude SSP et ingénierie des travaux de réhabilitation","2018-12-06",null,"Rapport de fin de travaux et ARR AECOM\n\nCe rapport de fin de travaux englobe les travaux de terrassement du projet porté par la SNC MARIGNAN\nRESIDENCES.\nPour les terres situées au droit de l’ancienne station-service, le bureau d’études détaille les excavations réalisées. Les terrassements ont commencé en avril 2018 et se sont terminés en septembre 2018, les terres ont été excavées sur une profondeur allant jusqu’à 11 à 12 m. Le bureau d’études précise que le projet global a conduit aux évacuations suivantes des terres :\n- 2 873 m³ de terres en Comblement de Carrière ;\n- 260 m³ de terres en ISDI+ ;\n- 2 410,42 tonnes de terres en Biocentre.\nSur la base des plans d’excavation par filière, les terres au droit de l’ancienne station-service ont été évacuées en biocentre. A l’issue de l’ensemble des excavations des mesures de fonds de fouille ont été réalisées.\nLe fond de fouille 26 présente un impact en HCT C10-C40 de 3 400 mg/kg (dont 1 300 mg/kg de HCT C12-C16 et 1400 mg/kg de HCT C16-C21). Sur le fond de fouilles 24 l’impact en HAP est de 52 mg/kg (dont 0,94 mg/kg de naphtalène). Les BTEX ne sont pas quantifiés.\n\nSur la base des résultats des concentrations mesurées en fond de fouilles, le bureau d’études réalise une\nanalyse des risques résiduels. Le bureau d’études conclut à la compatibilité du terrain avec l’aménagement prévu.",null,"Analyse des enjeux sanitaires (EQRS, ARR)","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040008801","Etude SSP et ingénierie des travaux de réhabilitation","2006-04-01",null,"Diagnostic initial\n\nll a permis la réalisation de sondages de sol ,de prélèvements de gaz de sols et un prélèvement d’eaux souterraine au niveau du sondage S8 où la présence d’eau a été identifiée à environ 1,90 m de profondeur.(cependant il ne s’agit pas d’une nappe souterraine mais vraisemblablement d’une accumulation d’eaux de pluie)\nCes prélèvements ont mis en évidence des teneurs en HCT et en xylène dans les sols ponctuellement ainsi que des HCT dans les gaz du sol.\nDans les eaux souterraines on a retrouvé des HCT, HAP et BTEX.","Eaux souterraines","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040008801","Etude SSP et ingénierie des travaux de réhabilitation","2006-04-01",null,"Diagnostic initial\n\nll a permis la réalisation de sondages de sol ,de prélèvements de gaz de sols et un prélèvement d’eaux souterraine au niveau du sondage S8 où la présence d’eau a été identifiée à environ 1,90 m de profondeur.(cependant il ne s’agit pas d’une nappe souterraine mais vraisemblablement d’une accumulation d’eaux de pluie)\nCes prélèvements ont mis en évidence des teneurs en HCT et en xylène dans les sols ponctuellement ainsi que des HCT dans les gaz du sol.\nDans les eaux souterraines on a retrouvé des HCT, HAP et BTEX.","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040008801","Etude SSP et ingénierie des travaux de réhabilitation","2006-06-01",null,"Le rapport conclut que le site ne nécessitait pas de travaux de dépollution dans l’immédiat, l’installation est toujours en fonctionnement.",null,"Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040010301","Etude SSP et ingénierie des travaux de réhabilitation","2015-12-28",null,"Diagnostic de pollution des sols établis par EGIS Structures et Environnement.\n\nQuatre sondages ont été réalisés le 14 décembre 2015. Pour l’ensemble des sondages, des refus à 50 cm de profondeur ont été constatés (couche de graves surmontée de sables très compacts).\n\nLes résultats mettent en évidence :\n– l’absence de BTEX et de COHV pour l’ensemble des sondages,\n– des traces d’HAP : la concentration maximale mesurée en HAP totaux est de 0,380 mg/kg MS,\n– la présence d’hydrocarbures : les concentrations mesurées sont comprises entre 420 et 620 mg/kg MS. Ils sont composés majoritairement de fractions lourdes (hydrocarbures non volatils),\n– la présence des différents métaux à des concentrations relativement faibles (en moyenne : 5mg/kg MS pour l’arsenic, 10 mg/kg MS pour le nickel, 15 mg/kg pour le plomb, 20 mg/kg pour le chrome).\n\nLe diagnostic conclu que ces impacts sont probablement inhérents à la qualité des remblais du site.\n\nPar ailleurs un schéma conceptuel pour un usage industriel a été établi. Les voies de transfert par contact direct et inhalation de composés volatils ne sont pas retenues.",null,"Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040010501","Etude SSP et ingénierie des travaux de réhabilitation","2016-04-18",null,"Diagnostic de pollution des sols – ICF Environnement (INV16027IB-V2)\n\nLes conclusions de ce diagnostic sont les suivantes :\n    • constatation d'une présence de métaux lourds à des teneurs supérieures à la note CIRE Ile-de-France du 3 juillet 2006 sur un des quatre sondages réalisés sur la parcelle sise 9-11 rue Sainte Marie. La présence de métaux lourds n'est pas un critère de refus pour les centres de stockage de déchets inertes ;\n    • nécessité d'un recouvrement a minima par 30 cm (après compactage) de terre saine au droit des espaces verts projetés afin de maîtriser les éventuels risques pour les futurs usagers des sites par contact direct ou ingestion des sols.",null,"Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040010601","Etude SSP et ingénierie des travaux de réhabilitation","2018-05-22",null,"Etude historique et de vulnérabilité – IDDEA (IDA180131)\n\nL’étude de vulnérabilité indique que : \n    • les nappes amenées à être rencontrées au droit du site sont la nappe des sables de Beauchamp qui est susceptible d’être retrouvée à 15 mètres de profondeur et la nappe des calcaires grossiers à environ 48 m de profondeur. La première nappe est considérée comme vulnérable, l’autre n’est pas retenue comme vulnérable ;\n    • pour les ouvrages de prélèvement de la nappe, l’ouvrage le plus proche est à plus de 800 m au nord du site selon la base de données BSS ;\n    • l’environnement proche du site n’est pas constitué de logement et aucun établissement sensible n’est recensé dans un rayon de 500 mètres autour du site.\n\nSur la base des données recueillies sur l’historique du site, en analysant les photos aériennes, le pétitionnaire a identifié les 8 zones potentiellement polluées. Les polluants recherchés sont les hydrocarbures, les BTEX, HAP, métaux et COHV.","Eaux souterraines","Etude historique, documentaire et mémorielle","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040010601","Etude SSP et ingénierie des travaux de réhabilitation","2019-01-16",null,"16/01/2019\nDiagnostic des milieux – IDDEA (IDA180253_MRB)\n\nSuite à l’étude historique et environnemental précitée, un diagnostic des milieux a été réalisé. Ce diagnostic comprend la réalisation de : \n- 11 sondages de sols carottés jusqu’à 30 mètres de profondeur\n- 16 sondages de 8 m de profondeur à la tarière\n- 5 sondages de 6 m de profondeur à la tarière\n- 5 piézomètres de 30 m de profondeur.\n\nLes analyses des sols réalisées mettent en avant : \n    • des impacts en métaux dans les sols et notamment sur les remblais. Sur les terres naturelles, des anomalies sont également retrouvées mais s’atténuent après une profondeur de 8 m. Les teneurs maximales mesurées sont de : \n        ◦ 2900 mg/kg en cuivre sur le sondage 19 (0-2 m), \n        ◦ 10,5 mg/kg en mercure sur le sondage 7 (0-2 m), \n        ◦ 550 mg/kg en nickel sur le sondage 8 (0-2 m), \n        ◦ 2600 mg/kg en plomb sur le sondage 8 (0-2 m) et \n        ◦ 6600 mg/kg en zinc sur le sondage 8 (0-2 m). \n    • des impacts en hydrocarbures avec une concentration maximale de 14 000 mg/kg sur le sondage 9 entre 0 et 2 mètres. Sur les 32 sondages réalisés, 9 présentent une concentration supérieure à 500 mg/kg. Les concentrations en HCT rencontrées tendent à diminuer avec la profondeur. \n    • Des impacts en HAP avec une concentration maximale de 700 mg/kg sur le sondage 26.\n    • Des impacts en PCB avec une concentration maximale de 64 mg/kg sur le sondage 8.\n    • Des impacts en COHV avec une concentration maximale de 2,4 mg/kg trouvée sur le sondage 8 (majoritairement du PCE et du TCE) ; \nLe bureau d’études conclut que les impacts sont corrélables avec l’historique du site, ces impacts étant localisés dans les zones de déchets observés dans les photos aériennes (Z1), sur la zone Z3 déjà impactée en PCB et HCT en 2010 et au niveau de l’ancienne huilerie, autour du sondage 26. \n\nPour les eaux souterraines, 5 piézomètres ont été installés. La nappe a été retrouvée à une profondeur d’environ 25 m. Le sens d’écoulement va vers le nord. \nLes analyses réalisées montrent un impact limité en COHV compris entre 10,8 et 44 µg/l. Toutefois, l’impact est plus important en amont hydraulique du site qu’en aval. Un impact limité a aussi été mesuré en HCT sur le piézomètre 23 au centre hydraulique du site (concentration de 355 µg/l).\n\nLe bureau d’études précise qu’à ce stade, le projet d’implantation prévisionnelle n’étant pas prévu, aucune ARR n’est réalisée.","Eaux souterraines","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040010601","Etude SSP et ingénierie des travaux de réhabilitation","2018-05-22",null,"Etude historique et de vulnérabilité – IDDEA (IDA180131)\n\nL’étude de vulnérabilité indique que : \n    • les nappes amenées à être rencontrées au droit du site sont la nappe des sables de Beauchamp qui est susceptible d’être retrouvée à 15 mètres de profondeur et la nappe des calcaires grossiers à environ 48 m de profondeur. La première nappe est considérée comme vulnérable, l’autre n’est pas retenue comme vulnérable ;\n    • pour les ouvrages de prélèvement de la nappe, l’ouvrage le plus proche est à plus de 800 m au nord du site selon la base de données BSS ;\n    • l’environnement proche du site n’est pas constitué de logement et aucun établissement sensible n’est recensé dans un rayon de 500 mètres autour du site.\n\nSur la base des données recueillies sur l’historique du site, en analysant les photos aériennes, le pétitionnaire a identifié les 8 zones potentiellement polluées. Les polluants recherchés sont les hydrocarbures, les BTEX, HAP, métaux et COHV.","Sol - Sous-sol","Etude historique, documentaire et mémorielle","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040010601","Etude SSP et ingénierie des travaux de réhabilitation","2019-01-16",null,"16/01/2019\nDiagnostic des milieux – IDDEA (IDA180253_MRB)\n\nSuite à l’étude historique et environnemental précitée, un diagnostic des milieux a été réalisé. Ce diagnostic comprend la réalisation de : \n- 11 sondages de sols carottés jusqu’à 30 mètres de profondeur\n- 16 sondages de 8 m de profondeur à la tarière\n- 5 sondages de 6 m de profondeur à la tarière\n- 5 piézomètres de 30 m de profondeur.\n\nLes analyses des sols réalisées mettent en avant : \n    • des impacts en métaux dans les sols et notamment sur les remblais. Sur les terres naturelles, des anomalies sont également retrouvées mais s’atténuent après une profondeur de 8 m. Les teneurs maximales mesurées sont de : \n        ◦ 2900 mg/kg en cuivre sur le sondage 19 (0-2 m), \n        ◦ 10,5 mg/kg en mercure sur le sondage 7 (0-2 m), \n        ◦ 550 mg/kg en nickel sur le sondage 8 (0-2 m), \n        ◦ 2600 mg/kg en plomb sur le sondage 8 (0-2 m) et \n        ◦ 6600 mg/kg en zinc sur le sondage 8 (0-2 m). \n    • des impacts en hydrocarbures avec une concentration maximale de 14 000 mg/kg sur le sondage 9 entre 0 et 2 mètres. Sur les 32 sondages réalisés, 9 présentent une concentration supérieure à 500 mg/kg. Les concentrations en HCT rencontrées tendent à diminuer avec la profondeur. \n    • Des impacts en HAP avec une concentration maximale de 700 mg/kg sur le sondage 26.\n    • Des impacts en PCB avec une concentration maximale de 64 mg/kg sur le sondage 8.\n    • Des impacts en COHV avec une concentration maximale de 2,4 mg/kg trouvée sur le sondage 8 (majoritairement du PCE et du TCE) ; \nLe bureau d’études conclut que les impacts sont corrélables avec l’historique du site, ces impacts étant localisés dans les zones de déchets observés dans les photos aériennes (Z1), sur la zone Z3 déjà impactée en PCB et HCT en 2010 et au niveau de l’ancienne huilerie, autour du sondage 26. \n\nPour les eaux souterraines, 5 piézomètres ont été installés. La nappe a été retrouvée à une profondeur d’environ 25 m. Le sens d’écoulement va vers le nord. \nLes analyses réalisées montrent un impact limité en COHV compris entre 10,8 et 44 µg/l. Toutefois, l’impact est plus important en amont hydraulique du site qu’en aval. Un impact limité a aussi été mesuré en HCT sur le piézomètre 23 au centre hydraulique du site (concentration de 355 µg/l).\n\nLe bureau d’études précise qu’à ce stade, le projet d’implantation prévisionnelle n’étant pas prévu, aucune ARR n’est réalisée.","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040010801","Exécution des travaux de réhabilitation",null,null,"Déconstruction de l'entrepôt avec désamiantage.",null,"N/A","N/A","N/A","N/A","Mesures constructives",null,"N/A","N/A","N/A"]
["SSP040011001","Surveillance environnementale",null,null,"Mise en place du contrôle de la légionnelle.",null,"N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040011101","Surveillance environnementale",null,null,"Suivi des prescriptions de prévention atmosphérique (COV).",null,"N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040011201","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"Forages, piézomètres, nettoyage et neutralisation des cuves.",null,"Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040011301","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"Étude du sol, des eaux souterraines et des gaz.","Air","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040011301","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"Étude du sol, des eaux souterraines et des gaz.","Eaux souterraines","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040011501","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"Deux diagnostic ont été réalisés grâce à 76 forages qui ont permis d’analyser les sols et les eaux souterraines ainsi que des piézairs.","Air","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040011501","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"Deux diagnostic ont été réalisés grâce à 76 forages qui ont permis d’analyser les sols et les eaux souterraines ainsi que des piézairs.","Eaux superficielles - Sédiments","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040011701","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"Des investigations ont été mené au travers de trois piézomètres, d’échantillonnage pour recueillir les gaz du sol.",null,"Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040011801","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"18 forages des sols ont été réalisés entre 3 et 5 mètres et 3 points de mesures des gaz du sol.","Eaux souterraines","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040011801","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"18 forages des sols ont été réalisés entre 3 et 5 mètres et 3 points de mesures des gaz du sol.","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040011901","Etude SSP et ingénierie des travaux de réhabilitation","2012-01-13",null,"Plan de gestion Veolia Proprete – GRS VALTECH\nZone du projet Veolia Proprete\n\nInvestigations complémentaires en novembre et décembre 2011 :\n- 9 sondages de sols afin de délimiter la zone reconnue souillée apar des COHV\n- pose d’un piézomètre de 10m de profondeur au droit de la zone précitée\n- pose de 2 piézairs au droit de cette zone\n\nCes investigations ont permis de : \n- confirmer la présence d’une légère pollution des sols par des COHV (PCE ou TCE). Cette contamination n’a pu être délimitée complètement par les sondages réalisés ;\n- mettre en évidence la présence d’une légère contamination par des HAP en partie Nord et Sud du site ainsi qu’au niveau de la bordure Nord-Ouest\n- confirmer la présence de teneurs en métaux et métalloïde anormalement élevée (As, Cu, Hg, Pb, Zn) généralisées à l’ensemble des remblais présents sur site et ponctuellement dans les terrains sous-jacebnts ;\n- montrer la présence d’un impact en COHV dans les eaux souterraines provenant potentiellement des sols ;\n- montrer l’absence de COHV dans les gaz du sol au droit de l’emprise du futur bâtiment.\nLes contaminations identifiées ne présentaient pas de risques pour les futurs usagers du site (recouvrement de sols par un revêtement de tyê enrobé ou béton, absence d’usage des eaux souterraines).","Air","Plan de gestion","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040011901","Etude SSP et ingénierie des travaux de réhabilitation","2001-11-20",null,"Diagnostic de sols et de la nappe – GERSTER référencé SP0/01/6431","Eaux souterraines","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040011901","Etude SSP et ingénierie des travaux de réhabilitation","2012-08-23",null,"Diagnostic complémentaire Veolia Propreté – GRS VALTECH n° 11110050 V2\n\nRéalisation de 3 sondages à 6 m  de prof. Et échantillonage des eaux souterraines au droit du piézomètres posé en 2011par GRS ainsi que 2 autres piézomètres existants localisés dans angles Sud Est et Nord Est (PZ Amont et PZ aval). Les résultats indiquent sur les eaux souterraines la présence de :\n- légères concentrations en HCT en aval latéral\n- de traces de HAP en amont et aval du site\n- de traces de xylènes totaux en aval/latéral\n- de teneurs en COHV en amont et partie centrale du site\n- de traces de métaux au sein des ouvrages localisés en partie centrale et Nord-Est du site.\nLe bureau d’étude indique que les concentrations observées dans les eaux ne permettaient pas d’affirmer que la qualité des sols au droit du site est à l’origine d’une dégradation de la qualité des eaux souterraines.\n\nCes résultats confirment que la qualité du sous-sol n’impliquait pas la mise en oeuvre de travaux de réhabilitation particuliers au regard du projet d’aménagement de Veolia.","Eaux souterraines","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040011901","Etude SSP et ingénierie des travaux de réhabilitation","2020-09-29",null,"Audit Environnemental des sols et de la nappe souterraine OPESLIA – GRS VALTECH n° 11200016 version B\n\nOPESLIA a souhaité réaliser un état des lieux de la qualité des sols et de la nappe souterraine au droit du site dans le cadre de la cessation d’activités.\nLes investigations ont eu lieu entre le 18 et le 26 août 2020, puis le 14 septembre 2020 :\n- réalisation de 20 sondages de sols\n- pose de 3 piézomètres dont un en amont et un en aval\n\nLes résultats ont mis en évidence, pour les sols :\n- des teneurs en plomb sur sol brut assez élevées sur l’ensemble du site (bruit de fond) ;\n- un spot de pollution en PCB entre 2 et 3m de prof. Au droit du sondage T4 et les sondages de délimitation T4-C et T4-D\n- un spot de pollution en HAP sur le sondage T8 entre 0 et 1m de prof. : pollution limitée au niveau de cette zone située sous dallage béton\n- les sondages T1, T2, T3, T5, T7, T10, T11, T12 et T13 présentent des teneurs comparables à celles obtenues lors de l’état initial\n- pour les autres sondages, les valeurs quantifiées sont cohérentes avec les valeurs retrouvées sur le site.\n\nPour les eaux souterraines, les investigations mettent en évidence la présence de TCE et PCE sur PZ et PZA à des teneurs légèrement supérieures à la limite pour les eaux potables. Ces teneurs se retrouvent dans les piézomètres aval du site et non en amont. Aucune valeur n’a été retrouvée dans les sols du site. La pollution au niveau des eaux souterraines peut être d’origine extérieure au site.\n\nLe bureau d’étude GRS VALTECH préconise : \n- la conservation des dallages et enrobés afin d’éviter tout risque sanitaire par contact direct avec les contaminations mises en évidence et afin de limiter la percolation des eaux de pluies dans les terrains ;\n- la conservation de la mémoire des contaminations mises en évidence ;\n- En cas de changement d’usage du site, un Plan de Gestion devra être réalisé avec une EQRS afin de définir les mesures de gestion nécessaires afin que l’état sanitaire du site soit en accord avec ce nouvel usage.","Eaux souterraines","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040011901","Etude SSP et ingénierie des travaux de réhabilitation","2012-01-13",null,"Plan de gestion Veolia Proprete – GRS VALTECH\nZone du projet Veolia Proprete\n\nInvestigations complémentaires en novembre et décembre 2011 :\n- 9 sondages de sols afin de délimiter la zone reconnue souillée apar des COHV\n- pose d’un piézomètre de 10m de profondeur au droit de la zone précitée\n- pose de 2 piézairs au droit de cette zone\n\nCes investigations ont permis de : \n- confirmer la présence d’une légère pollution des sols par des COHV (PCE ou TCE). Cette contamination n’a pu être délimitée complètement par les sondages réalisés ;\n- mettre en évidence la présence d’une légère contamination par des HAP en partie Nord et Sud du site ainsi qu’au niveau de la bordure Nord-Ouest\n- confirmer la présence de teneurs en métaux et métalloïde anormalement élevée (As, Cu, Hg, Pb, Zn) généralisées à l’ensemble des remblais présents sur site et ponctuellement dans les terrains sous-jacebnts ;\n- montrer la présence d’un impact en COHV dans les eaux souterraines provenant potentiellement des sols ;\n- montrer l’absence de COHV dans les gaz du sol au droit de l’emprise du futur bâtiment.\nLes contaminations identifiées ne présentaient pas de risques pour les futurs usagers du site (recouvrement de sols par un revêtement de tyê enrobé ou béton, absence d’usage des eaux souterraines).","Eaux souterraines","Plan de gestion","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040011901","Etude SSP et ingénierie des travaux de réhabilitation","2001-11-20",null,"Diagnostic de sols et de la nappe – GERSTER référencé SP0/01/6431","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040011901","Etude SSP et ingénierie des travaux de réhabilitation","2002-02-11",null,"Diagnostic complémentaire – GERSTER référencé 215.02.0002.E.A\nEstimation des volumes et coût de dépollution","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040011901","Etude SSP et ingénierie des travaux de réhabilitation","2007-08-01",null,"Diagnostic de pollution des sols dans le cadre de l’implantation de la société REP – rapport ATOS  Environnement AEPLA7106","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040011901","Etude SSP et ingénierie des travaux de réhabilitation","2010-11-01",null,"Diagnostic de pollution des sols Port de Gennevilliers – Etat initial Veolia – Rapport technique GUIGUES Environnement 10CT01926-RT01-Ports de Paris/Novembre 2010\n\nDiagnostic initial mandaté par le Port de Gennevilliers préalablement à l’implantation du projet Veolia (OPESLIA) afin d’établir l’état environnemental initial des sols.\nDix sondages d’une profondeur de 3 à 5 mètres ont été réalisés en octobre 2010.\nA l’issue de ce rapport, Veolia a fait procéder à la réalisation d’un plan de gestion puisque le rapport du bureau d’études concluait notamment à la présence d’une zone reconnue souillée par des composés organo-halogénés volatils en partie centrale du site.","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040011901","Etude SSP et ingénierie des travaux de réhabilitation","2012-08-23",null,"Diagnostic complémentaire Veolia Propreté – GRS VALTECH n° 11110050 V2\n\nRéalisation de 3 sondages à 6 m  de prof. Et échantillonage des eaux souterraines au droit du piézomètres posé en 2011par GRS ainsi que 2 autres piézomètres existants localisés dans angles Sud Est et Nord Est (PZ Amont et PZ aval). Les résultats indiquent sur les eaux souterraines la présence de :\n- légères concentrations en HCT en aval latéral\n- de traces de HAP en amont et aval du site\n- de traces de xylènes totaux en aval/latéral\n- de teneurs en COHV en amont et partie centrale du site\n- de traces de métaux au sein des ouvrages localisés en partie centrale et Nord-Est du site.\nLe bureau d’étude indique que les concentrations observées dans les eaux ne permettaient pas d’affirmer que la qualité des sols au droit du site est à l’origine d’une dégradation de la qualité des eaux souterraines.\n\nCes résultats confirment que la qualité du sous-sol n’impliquait pas la mise en oeuvre de travaux de réhabilitation particuliers au regard du projet d’aménagement de Veolia.","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040011901","Etude SSP et ingénierie des travaux de réhabilitation","2020-09-29",null,"Audit Environnemental des sols et de la nappe souterraine OPESLIA – GRS VALTECH n° 11200016 version B\n\nOPESLIA a souhaité réaliser un état des lieux de la qualité des sols et de la nappe souterraine au droit du site dans le cadre de la cessation d’activités.\nLes investigations ont eu lieu entre le 18 et le 26 août 2020, puis le 14 septembre 2020 :\n- réalisation de 20 sondages de sols\n- pose de 3 piézomètres dont un en amont et un en aval\n\nLes résultats ont mis en évidence, pour les sols :\n- des teneurs en plomb sur sol brut assez élevées sur l’ensemble du site (bruit de fond) ;\n- un spot de pollution en PCB entre 2 et 3m de prof. Au droit du sondage T4 et les sondages de délimitation T4-C et T4-D\n- un spot de pollution en HAP sur le sondage T8 entre 0 et 1m de prof. : pollution limitée au niveau de cette zone située sous dallage béton\n- les sondages T1, T2, T3, T5, T7, T10, T11, T12 et T13 présentent des teneurs comparables à celles obtenues lors de l’état initial\n- pour les autres sondages, les valeurs quantifiées sont cohérentes avec les valeurs retrouvées sur le site.\n\nPour les eaux souterraines, les investigations mettent en évidence la présence de TCE et PCE sur PZ et PZA à des teneurs légèrement supérieures à la limite pour les eaux potables. Ces teneurs se retrouvent dans les piézomètres aval du site et non en amont. Aucune valeur n’a été retrouvée dans les sols du site. La pollution au niveau des eaux souterraines peut être d’origine extérieure au site.\n\nLe bureau d’étude GRS VALTECH préconise : \n- la conservation des dallages et enrobés afin d’éviter tout risque sanitaire par contact direct avec les contaminations mises en évidence et afin de limiter la percolation des eaux de pluies dans les terrains ;\n- la conservation de la mémoire des contaminations mises en évidence ;\n- En cas de changement d’usage du site, un Plan de Gestion devra être réalisé avec une EQRS afin de définir les mesures de gestion nécessaires afin que l’état sanitaire du site soit en accord avec ce nouvel usage.","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040011901","Etude SSP et ingénierie des travaux de réhabilitation","2012-01-13",null,"Plan de gestion Veolia Proprete – GRS VALTECH\nZone du projet Veolia Proprete\n\nInvestigations complémentaires en novembre et décembre 2011 :\n- 9 sondages de sols afin de délimiter la zone reconnue souillée apar des COHV\n- pose d’un piézomètre de 10m de profondeur au droit de la zone précitée\n- pose de 2 piézairs au droit de cette zone\n\nCes investigations ont permis de : \n- confirmer la présence d’une légère pollution des sols par des COHV (PCE ou TCE). Cette contamination n’a pu être délimitée complètement par les sondages réalisés ;\n- mettre en évidence la présence d’une légère contamination par des HAP en partie Nord et Sud du site ainsi qu’au niveau de la bordure Nord-Ouest\n- confirmer la présence de teneurs en métaux et métalloïde anormalement élevée (As, Cu, Hg, Pb, Zn) généralisées à l’ensemble des remblais présents sur site et ponctuellement dans les terrains sous-jacebnts ;\n- montrer la présence d’un impact en COHV dans les eaux souterraines provenant potentiellement des sols ;\n- montrer l’absence de COHV dans les gaz du sol au droit de l’emprise du futur bâtiment.\nLes contaminations identifiées ne présentaient pas de risques pour les futurs usagers du site (recouvrement de sols par un revêtement de tyê enrobé ou béton, absence d’usage des eaux souterraines).","Sol - Sous-sol","Plan de gestion","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040011901","Exécution des travaux de réhabilitation","2013-02-20",null,"Validation d’une fouille – GRS VALTECH n°11110050 V2\n\nLa zone reconnue souillée a fait l’objet d’une purge de terres polluées par Veolia en septembre 2012. Les fouilles d’une profondeur de 2m environ étaient localisées au niveau de la zone des bureaux d’OPESLIA.","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution"]
["SSP040011901","Etude SSP et ingénierie des travaux de réhabilitation","2001-10-31",null,"Etude historique et documentaire – GERSTER référencé SP0/01/6249",null,"Etude historique, documentaire et mémorielle","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040012301","Etude SSP et ingénierie des travaux de réhabilitation","2007-02-16",null,"EDR - Socotec affaire qa 6401\n\nLes résultats obtenus pour cette EDR sur la base des hypothèses effectuées montrent que les niveaux de risques sanitaires sont acceptables pour l’ensemble de ces voies et de ces milieux d’exposition. (...) les prélèvements de fond de fouille non effectués à ce jour principalement au droit des futurs espaces verts permettront de confirmer le caractère conservatoire des hypothèses prises concernant la qualité de ces terres  sur ces zones.",null,"Analyse des enjeux sanitaires (EQRS, ARR)","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040012701","Etude SSP et ingénierie des travaux de réhabilitation","2020-01-27",null,"Plan de gestion – EODD (P04025.02 P)\n\nLe plan de gestion reprend les conclusions du diagnostic. Il émet les remarques suivantes concernant la délimitation de la zone des sols pollués : \n    • La zone de sols contaminés est délimitée au Nord et à l’Est par les infrastructures correspondant aux 2 niveaux de sous-sol du bâtiment ;\n    • Le panache de pollution dans les sols s’étend probablement en dehors des limites du site, sous l’emprise du trottoir au Sud, et potentiellement au niveau de l’avenue Benoît Frachon. De l’autre côté de l’avenue Benoît Frachon, à environ 12 m de la cuve, se trouve le tunnel de l’autoroute A86 dont la chaussée se trouve à environ -4 m par rapport au niveau du terrain naturel du garage et de la rue Frachon. Le bureau d’études conclut que le tunnel de l’A86 et ses infrastructures associées constituent une limite au panache de pollution des sols provenant de la zone de la cuve ;\n    • L’extension de la zone de sols contaminés à l’Ouest est selon le bureau d’études probablement limitée par la présence d’une rampe d’accès à un sous-sol à l’Ouest.\n\n\nPour les eaux souterraines, 3 piézomètres complémentaires ont été implantés autour de la cuve enterrée, en 2016, 2017 et 2019. Ces piézomètres captent la nappe alluviale dont le toit se trouve à environ 4 m de profondeur.\n\nSur les eaux souterraines, le bureau d’études indique que la présence des structures enterrées (sous-sol du garage, voiles du tunnel de l’A86) de part et d’autre de la zone de la cuve perturbe probablement localement les écoulements de la nappe et pourraient limiter l’extension latérale de la contamination des eaux souterraines.\n\nEn outre, en janvier 2018, des prélèvements d’air ambiant Paa1 et Paa2 ont été réalisés respectivement au 2ème et au 1er niveau de sous-sol du bâtiment. Un prélèvement local témoin (ELT) a été réalisé en extérieur. Un prélèvement des gaz du sol a été réalisé au sein d’un piézair à 3,5 m de profondeur, à proximité de la cuve enterrée et du piézomètre PZ1.\nSur la base des mesures d’air ambiant, le bureau d’études indique que les hydrocarbures et les BTEX, n’ayant pas été mesurés au droit des gaz du sol de la zone source, les concentrations mesurées dans les parkings semblent en lien avec le bruit de fond et l’impact de la circulation de véhicules à l’intérieur du parking.\n\nSur la base des données du diagnostic, le bureau d’études réalise une étude statistique permettant de définir les sources concentrées, avec la limite que le nombre de prélèvements de sol réalisé est assez faible. Le bureau d’études définit les sources concentrées de pollution dans les sols à 100 mg/kg pour les hydrocarbures C5-C10 et à 10 mg/kg en BTEX. \nPour les eaux souterraines, le bureau d’études indique que le panache de pollution constituant la source concentrée dans les eaux souterraines est estimé à une centaine de mètres carrés. Son extension est limitée par la rampe d’accès à l’ouest, les parkings au nord et l’autoroute au sud.\n\nLe bureau d’études retient 4 scénarios de gestion possibles compte tenu de la pollution présente : \n    1. Excavation sols pollués et oxydation nappe en fond de fouille ; \n    2. Oxydation in-situ des sols et de la nappe ;\n    3. Traitement couplé venting (sols)/sparging (nappe) ;\n    4. Confinement et surveillance de la nappe\n\nPour le scénario 1, le bureau d’études écarte ce scénario en raison des fortes contraintes dues aux avoisinants (incompatibilité avec le maintien de l’activité de garage, le coût élevé d’un blindage de fouille notamment). Pour les scénarios 2 et 3, le bureau d’études indique qu’il y a des incertitudes sur la faisabilité, que la zone est trop restreinte pour les installations de traitement et que le traitement ne sera que partiel en raison de l’absence de retrait des cuves. \nLe dernier scénario est alors retenu pour les raisons suivantes : \n    • la pollution est déjà confinée dans la configuration actuelle du site. La surveillance permet de garantir l'absence de migration et de dégradation du milieu. \n    • cette solution n’exclut pas la réalisation d’un traitement ultérieur. \n\nPour la surveillance, le bureau d’études propose de réaliser une surveillance des eaux souterraines et des piézairs sur une période de 4 ans. Pour compléter les modalités de surveillance, le bureau d’études propose l’installation d’un piézair complémentaire au nord-est du site.\n\nUne analyse des risques résiduels a été réalisée par le bureau d’études. Cette analyse résiduelle ne prend en compte que les résultats du piézair Pz1 pour ne prendre en compte que l’impact provenant du sol. Pour les hydrocarbures qui n’ont pas été quantifiés dans les gaz du sol, le bureau d’étude reprend alors la limite de quantification. Ces calculs démontrent la compatibilité du milieu avec l’usage industriel/tertiaire.","Air","Plan de gestion","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040012701","Etude SSP et ingénierie des travaux de réhabilitation","2016-11-24",null,"Diagnostic environnemental - IDDEA (IC160240)\n\nLe diagnostic a été réalisé par la société IDDEA Environnement. Sur la base de l’étude de l’historique du site, les investigations de terrain ont été ciblées au droit de la cuve enterrée de carburant. Elles ont consisté en 3 sondages de sol et un piézomètre. \nLa nappe alluviale a été rencontrée vers 3,90 m de profondeur. Elle est vulnérable aux pollutions de surface, bien qu’aucune utilisation ne soit connue à proximité. Au regard des résultats de l’analyse réalisée sur l’eau prélevée sur le piézomètre, aucun impact n’a été identifié au droit du site d’étude. Le sens d’écoulement de la nappe n’a pas été déterminé mais est supposé orienté vers le nord-ouest.\n\nDes impacts en HCT, BTEX et HAP ont été relevés, mais seules les valeurs en BTEX dépassent le seuil d’acceptation en ISDI. Les prélèvements au-delà de 3,90 m de profondeur ont été réalisés dans des sols saturés en eau.Un impact sur les sols lié aux anciennes installations classées est avéré. L’impact est notable pour les BTEX, avec des teneurs jusqu’à 358 mg/kg (seuil ISDI à 6 mg/kg), bien que l’imperméabilisation du site limite probablement les risques sanitaires et environnementaux.\n\nLe diagnostic se conclut par les recommandations suivantes :\n    • réaliser un suivi semestriel (campagne « hautes eaux » en mars et campagne « basses eaux » en septembre) de la nappe, sur une période de 4 ans ;\n    • réaliser une Interprétation de l’Etat des Milieux (IEM) afin de délimiter spatialement les impacts identifiés et de statuer sur une possible migration hors site des polluants identifiés sur le site ;\n    • réaliser une évaluation Quantitative des Risques Sanitaire (EQRS) afin de pouvoir statuer sur la compatibilité sanitaire entre l’état environnemental du site et son usage actuel ;\néventuellement, en fonction des conclusions de l’EQRS, réaliser un plan de gestion pouvant conduire à la dépollution du site.","Eaux souterraines","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040012701","Etude SSP et ingénierie des travaux de réhabilitation","2020-01-27",null,"Plan de gestion – EODD (P04025.02 P)\n\nLe plan de gestion reprend les conclusions du diagnostic. Il émet les remarques suivantes concernant la délimitation de la zone des sols pollués : \n    • La zone de sols contaminés est délimitée au Nord et à l’Est par les infrastructures correspondant aux 2 niveaux de sous-sol du bâtiment ;\n    • Le panache de pollution dans les sols s’étend probablement en dehors des limites du site, sous l’emprise du trottoir au Sud, et potentiellement au niveau de l’avenue Benoît Frachon. De l’autre côté de l’avenue Benoît Frachon, à environ 12 m de la cuve, se trouve le tunnel de l’autoroute A86 dont la chaussée se trouve à environ -4 m par rapport au niveau du terrain naturel du garage et de la rue Frachon. Le bureau d’études conclut que le tunnel de l’A86 et ses infrastructures associées constituent une limite au panache de pollution des sols provenant de la zone de la cuve ;\n    • L’extension de la zone de sols contaminés à l’Ouest est selon le bureau d’études probablement limitée par la présence d’une rampe d’accès à un sous-sol à l’Ouest.\n\n\nPour les eaux souterraines, 3 piézomètres complémentaires ont été implantés autour de la cuve enterrée, en 2016, 2017 et 2019. Ces piézomètres captent la nappe alluviale dont le toit se trouve à environ 4 m de profondeur.\n\nSur les eaux souterraines, le bureau d’études indique que la présence des structures enterrées (sous-sol du garage, voiles du tunnel de l’A86) de part et d’autre de la zone de la cuve perturbe probablement localement les écoulements de la nappe et pourraient limiter l’extension latérale de la contamination des eaux souterraines.\n\nEn outre, en janvier 2018, des prélèvements d’air ambiant Paa1 et Paa2 ont été réalisés respectivement au 2ème et au 1er niveau de sous-sol du bâtiment. Un prélèvement local témoin (ELT) a été réalisé en extérieur. Un prélèvement des gaz du sol a été réalisé au sein d’un piézair à 3,5 m de profondeur, à proximité de la cuve enterrée et du piézomètre PZ1.\nSur la base des mesures d’air ambiant, le bureau d’études indique que les hydrocarbures et les BTEX, n’ayant pas été mesurés au droit des gaz du sol de la zone source, les concentrations mesurées dans les parkings semblent en lien avec le bruit de fond et l’impact de la circulation de véhicules à l’intérieur du parking.\n\nSur la base des données du diagnostic, le bureau d’études réalise une étude statistique permettant de définir les sources concentrées, avec la limite que le nombre de prélèvements de sol réalisé est assez faible. Le bureau d’études définit les sources concentrées de pollution dans les sols à 100 mg/kg pour les hydrocarbures C5-C10 et à 10 mg/kg en BTEX. \nPour les eaux souterraines, le bureau d’études indique que le panache de pollution constituant la source concentrée dans les eaux souterraines est estimé à une centaine de mètres carrés. Son extension est limitée par la rampe d’accès à l’ouest, les parkings au nord et l’autoroute au sud.\n\nLe bureau d’études retient 4 scénarios de gestion possibles compte tenu de la pollution présente : \n    1. Excavation sols pollués et oxydation nappe en fond de fouille ; \n    2. Oxydation in-situ des sols et de la nappe ;\n    3. Traitement couplé venting (sols)/sparging (nappe) ;\n    4. Confinement et surveillance de la nappe\n\nPour le scénario 1, le bureau d’études écarte ce scénario en raison des fortes contraintes dues aux avoisinants (incompatibilité avec le maintien de l’activité de garage, le coût élevé d’un blindage de fouille notamment). Pour les scénarios 2 et 3, le bureau d’études indique qu’il y a des incertitudes sur la faisabilité, que la zone est trop restreinte pour les installations de traitement et que le traitement ne sera que partiel en raison de l’absence de retrait des cuves. \nLe dernier scénario est alors retenu pour les raisons suivantes : \n    • la pollution est déjà confinée dans la configuration actuelle du site. La surveillance permet de garantir l'absence de migration et de dégradation du milieu. \n    • cette solution n’exclut pas la réalisation d’un traitement ultérieur. \n\nPour la surveillance, le bureau d’études propose de réaliser une surveillance des eaux souterraines et des piézairs sur une période de 4 ans. Pour compléter les modalités de surveillance, le bureau d’études propose l’installation d’un piézair complémentaire au nord-est du site.\n\nUne analyse des risques résiduels a été réalisée par le bureau d’études. Cette analyse résiduelle ne prend en compte que les résultats du piézair Pz1 pour ne prendre en compte que l’impact provenant du sol. Pour les hydrocarbures qui n’ont pas été quantifiés dans les gaz du sol, le bureau d’étude reprend alors la limite de quantification. Ces calculs démontrent la compatibilité du milieu avec l’usage industriel/tertiaire.","Eaux souterraines","Plan de gestion","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040012701","Etude SSP et ingénierie des travaux de réhabilitation","2016-11-24",null,"Diagnostic environnemental - IDDEA (IC160240)\n\nLe diagnostic a été réalisé par la société IDDEA Environnement. Sur la base de l’étude de l’historique du site, les investigations de terrain ont été ciblées au droit de la cuve enterrée de carburant. Elles ont consisté en 3 sondages de sol et un piézomètre. \nLa nappe alluviale a été rencontrée vers 3,90 m de profondeur. Elle est vulnérable aux pollutions de surface, bien qu’aucune utilisation ne soit connue à proximité. Au regard des résultats de l’analyse réalisée sur l’eau prélevée sur le piézomètre, aucun impact n’a été identifié au droit du site d’étude. Le sens d’écoulement de la nappe n’a pas été déterminé mais est supposé orienté vers le nord-ouest.\n\nDes impacts en HCT, BTEX et HAP ont été relevés, mais seules les valeurs en BTEX dépassent le seuil d’acceptation en ISDI. Les prélèvements au-delà de 3,90 m de profondeur ont été réalisés dans des sols saturés en eau.Un impact sur les sols lié aux anciennes installations classées est avéré. L’impact est notable pour les BTEX, avec des teneurs jusqu’à 358 mg/kg (seuil ISDI à 6 mg/kg), bien que l’imperméabilisation du site limite probablement les risques sanitaires et environnementaux.\n\nLe diagnostic se conclut par les recommandations suivantes :\n    • réaliser un suivi semestriel (campagne « hautes eaux » en mars et campagne « basses eaux » en septembre) de la nappe, sur une période de 4 ans ;\n    • réaliser une Interprétation de l’Etat des Milieux (IEM) afin de délimiter spatialement les impacts identifiés et de statuer sur une possible migration hors site des polluants identifiés sur le site ;\n    • réaliser une évaluation Quantitative des Risques Sanitaire (EQRS) afin de pouvoir statuer sur la compatibilité sanitaire entre l’état environnemental du site et son usage actuel ;\néventuellement, en fonction des conclusions de l’EQRS, réaliser un plan de gestion pouvant conduire à la dépollution du site.","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040012701","Etude SSP et ingénierie des travaux de réhabilitation","2020-01-27",null,"Plan de gestion – EODD (P04025.02 P)\n\nLe plan de gestion reprend les conclusions du diagnostic. Il émet les remarques suivantes concernant la délimitation de la zone des sols pollués : \n    • La zone de sols contaminés est délimitée au Nord et à l’Est par les infrastructures correspondant aux 2 niveaux de sous-sol du bâtiment ;\n    • Le panache de pollution dans les sols s’étend probablement en dehors des limites du site, sous l’emprise du trottoir au Sud, et potentiellement au niveau de l’avenue Benoît Frachon. De l’autre côté de l’avenue Benoît Frachon, à environ 12 m de la cuve, se trouve le tunnel de l’autoroute A86 dont la chaussée se trouve à environ -4 m par rapport au niveau du terrain naturel du garage et de la rue Frachon. Le bureau d’études conclut que le tunnel de l’A86 et ses infrastructures associées constituent une limite au panache de pollution des sols provenant de la zone de la cuve ;\n    • L’extension de la zone de sols contaminés à l’Ouest est selon le bureau d’études probablement limitée par la présence d’une rampe d’accès à un sous-sol à l’Ouest.\n\n\nPour les eaux souterraines, 3 piézomètres complémentaires ont été implantés autour de la cuve enterrée, en 2016, 2017 et 2019. Ces piézomètres captent la nappe alluviale dont le toit se trouve à environ 4 m de profondeur.\n\nSur les eaux souterraines, le bureau d’études indique que la présence des structures enterrées (sous-sol du garage, voiles du tunnel de l’A86) de part et d’autre de la zone de la cuve perturbe probablement localement les écoulements de la nappe et pourraient limiter l’extension latérale de la contamination des eaux souterraines.\n\nEn outre, en janvier 2018, des prélèvements d’air ambiant Paa1 et Paa2 ont été réalisés respectivement au 2ème et au 1er niveau de sous-sol du bâtiment. Un prélèvement local témoin (ELT) a été réalisé en extérieur. Un prélèvement des gaz du sol a été réalisé au sein d’un piézair à 3,5 m de profondeur, à proximité de la cuve enterrée et du piézomètre PZ1.\nSur la base des mesures d’air ambiant, le bureau d’études indique que les hydrocarbures et les BTEX, n’ayant pas été mesurés au droit des gaz du sol de la zone source, les concentrations mesurées dans les parkings semblent en lien avec le bruit de fond et l’impact de la circulation de véhicules à l’intérieur du parking.\n\nSur la base des données du diagnostic, le bureau d’études réalise une étude statistique permettant de définir les sources concentrées, avec la limite que le nombre de prélèvements de sol réalisé est assez faible. Le bureau d’études définit les sources concentrées de pollution dans les sols à 100 mg/kg pour les hydrocarbures C5-C10 et à 10 mg/kg en BTEX. \nPour les eaux souterraines, le bureau d’études indique que le panache de pollution constituant la source concentrée dans les eaux souterraines est estimé à une centaine de mètres carrés. Son extension est limitée par la rampe d’accès à l’ouest, les parkings au nord et l’autoroute au sud.\n\nLe bureau d’études retient 4 scénarios de gestion possibles compte tenu de la pollution présente : \n    1. Excavation sols pollués et oxydation nappe en fond de fouille ; \n    2. Oxydation in-situ des sols et de la nappe ;\n    3. Traitement couplé venting (sols)/sparging (nappe) ;\n    4. Confinement et surveillance de la nappe\n\nPour le scénario 1, le bureau d’études écarte ce scénario en raison des fortes contraintes dues aux avoisinants (incompatibilité avec le maintien de l’activité de garage, le coût élevé d’un blindage de fouille notamment). Pour les scénarios 2 et 3, le bureau d’études indique qu’il y a des incertitudes sur la faisabilité, que la zone est trop restreinte pour les installations de traitement et que le traitement ne sera que partiel en raison de l’absence de retrait des cuves. \nLe dernier scénario est alors retenu pour les raisons suivantes : \n    • la pollution est déjà confinée dans la configuration actuelle du site. La surveillance permet de garantir l'absence de migration et de dégradation du milieu. \n    • cette solution n’exclut pas la réalisation d’un traitement ultérieur. \n\nPour la surveillance, le bureau d’études propose de réaliser une surveillance des eaux souterraines et des piézairs sur une période de 4 ans. Pour compléter les modalités de surveillance, le bureau d’études propose l’installation d’un piézair complémentaire au nord-est du site.\n\nUne analyse des risques résiduels a été réalisée par le bureau d’études. Cette analyse résiduelle ne prend en compte que les résultats du piézair Pz1 pour ne prendre en compte que l’impact provenant du sol. Pour les hydrocarbures qui n’ont pas été quantifiés dans les gaz du sol, le bureau d’étude reprend alors la limite de quantification. Ces calculs démontrent la compatibilité du milieu avec l’usage industriel/tertiaire.","Sol - Sous-sol","Plan de gestion","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040019601","Etude SSP et ingénierie des travaux de réhabilitation","2009-10-23",null,"Diagnostic NEODYME ENVISOL\n\nDans le cadre de la vente de la concession automobile FORD localisée à Créteil, la société PGA Motors a mandaté NEODYME ENVISOL pour la réalisation d’un diagnostic de pollution des sols sur ce site.\n      \nNEODYME ENVISOL a rédigé un rapport de diagnostic de pollution des sols en date du 23/10/09. Dans la conclusion de ce rapport, il est indiqué que le diagnostic de sols du site de Créteil a consisté en la réalisation de prélèvements et d’analyses d’échantillons de sols au niveau des zones à risques identifiées, lors d’un audit environnemental préalable. Celui-ci a mis en évidence que :\n       - Les sols recoupés étaient constitués au niveau du sous-sol de l’atelier par des calcaires blancs à cailloutis et en extérieur par des remblais sablograveleux noirs surmontant des argiles à silex marron et des calcaires blancs ;\n       - Le niveau statique des eaux souterraines au droit du site se trouve à environ 3 m de profondeur ;\n       - Plusieurs zones sensibles en terme de risque de pollution des sols ont été définies et investiguées (cuves d’huiles usagées, aire de lavage et séparateur d’hydrocarbures).\n       Les investigations réalisées n’ont pas mis en évidence la présence de source de pollution au niveau des sols au droit des zones investiguées. Dans le rapport de la société NEODYME ENVISOL, il est indiqué que ces conclusions ne sont valables que dans le cadre d’un usage industriel du site.","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040019701","Etude SSP et ingénierie des travaux de réhabilitation","2011-11-01",null,"GOLDER n°011503161034_V1 Contrôle environnemental du démantèlement de la station service","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040019701","Exécution des travaux de réhabilitation","2011-12-26",null,"DOE SECHE ECO SERVICE « travaux d’extraction d’infrastructures pétrolières »\n\nLes travaux de démantèlement ont été réalisés entre le 05/09/2011 et le 04/11/2011 : \n- Suppression du auvent ; \n- Vidange, nettoyage, dégazage et extraction des cuves ;\n- Terrassement de la zone des cuves et prélèvement partiel d’échantillons des flancs de fouille ;\n- Démolition des radiers et prélèvement d’échantillons en fond de fouille ;\n- Prélèvements d’échantillons au niveau des îlots de distribution, de la zone de dépotage et sur la zone des anciennes cuves ;\n- Evacuation de 30,50 tonnes de terres souillées (5100 mg/kg de HCT) vers le biocentre de SITA à Villeparisis (77) ;\n- Remblaiement des excavations.\n\nLe rapport conclut qu’après curage de la zone de dépotage, les analyses des fronts et fonds de fouilles montrent l’absence d’impact résiduel. Le site est compatible avec l’usage futur considéré : usage commercial.","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution"]
["SSP040020401","Etude SSP et ingénierie des travaux de réhabilitation","2009-11-18",null,"Diagnostic environnemental IDDEA   n°IC090215 version A\n\nLes prélèvements pour analyse ont concerné la parcelle s’étendant du 105 au 109 bis avenue du Président Kennedy sur la commune de Villeneuve-Saint-Georges.\nIl a été procédé à 7 sondages à la tarière (S1 à S7), de profondeur à partir du niveau du sol variant de 3 à 4,5 mètres, répartis, en fonction des informations fournies par le gérant, en tenant compte de l'activité et de la présence, antérieure ou non, d'équipements potentiellement polluants.\n\nLes analyses de sol, réalisées sur 9  échantillons en fonction des observations lithologiques & organoleptiques par le laboratoire AGROLAB (possédant les agréments MEEDDM & accréditations COFRAC nécessaires), ont concerné :\n    • Les hydrocarbures totaux (HCT) par GC-FID avec répartition des fractions carbonées, \n    • Les Métaux lourds ML (As, Cd, Cr, Cu, Hg, Ni, Pb, Zn), \n    • Les Hydrocarbures Aromatiques Polycycliques (HAP), \n    • Les Composés Organiques Volatils comprenant les Composés Organo-Halogénés Volatils (COHV) et les BTEX (Benzène, Toluène, Ethylbenzène, Xylènes).\n\nLa campagne de mesures effectuée sur la nappe a été réalisée au moyen de deux piézomètres positionnés les 23 et 26/09/09, respectivement en amont (pz1 à l’est du site, profondeur 7 m, niveau piézo 4,75 m) et en aval (pz2 au sud-ouest du site, profondeur 8,86 m, niveau piézo 3,85 m) hydraulique supposés du site sur les échantillons desquels ont été recherchés les paramètres suivants: HCT, Métaux Lourds, HAP , COHV et BTEX.\n\nLes analyses chimiques portant sur deux échantillons d’eau de nappe ont été effectuées par le laboratoire WESSLING (possédant les agréments MEEDDM & accréditations COFRAC nécessaires) et  les paramètres mesurés sont identiques à ceux recherchés dans les échantillons du sol.\n\nLes investigations de terrain et déterminations analytiques réalisées sur les sols et dans les eaux souterraines dans le cadre de cette étude ont mis en évidence :\n\n    • pour les échantillons de sol :\n        ◦ une odeur d’hydrocarbures et une couleur noire au droit du sondage S7 entre 0,9 et 1,7 m ainsi qu’au droit du sondage S2 entre 0,1 et 1 m ;\n        ◦ pour le sondage S3 notamment, des teneurs en métaux lourds ponctuellement supérieures (pour le cadmium, le cuivre, le mercure, le plomb et le zinc pour 3 échantillons sur les 9 analysés) ou entrant dans la gamme de valeurs couramment observées dans le cas de sols ordinaires ;\n        ◦ l’absence de pollution notable des sols par les HAP ;\n        ◦ l’absence de teneurs significatives en COHV et BTEX au droit des zones investiguées :\n        ◦ la présence de teneurs en HCT supérieures au critère de l’arrêté de mars 2006 au droit des sondages S2 entre 0,1 et 1 m, S3 entre 0,6 et 1,1 m et S7 entre 0,9 et 1,7 m.\n\n    • pour les échantillons prélevés dans les eaux souterraines : une absence d’impact notable pour tous les paramètres analysés :\n\n    • les teneurs mesurées en métaux lourds, hydrocarbures totaux, COHV et BTEX sont inférieures  à la limite de quantification du laboratoire et à celles de la qualité des eaux brutes pour la production d’eau potable conformément au décret du 11/01/2007 et aux valeurs de l’OMS quand elles sont disponibles ;\n    • les analyses relatives à la recherche des HAP indiquent des résultats inférieures aux valeurs seuils de qualité des eaux potables.\n\nSur la base des éléments décrits précédemment, le bureau d’études apporte les commentaires suivants :\n    • les impacts superficiels constatés en HCT (fractions lourdes essentiellement) au droit des sondages S2 (bâtiment faisant office de réfectoire et de vestiaire/ ancien atelier mécanique de garage) et S3 (parc de bennes en transit/ ancienne réserve en pièces détachées de garage) semblent être attribuables à des activités antérieures à celle qui était exercée par la société AFB FERNANDES ;\n    • l’anomalie relevée au niveau du sondage S7 (bac de rétention des hydrocarbures) serait quant à elle liée à l’activité exercée par la société AFB FERNANDES.","Eaux souterraines","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040020401","Etude SSP et ingénierie des travaux de réhabilitation","2009-11-18",null,"Diagnostic environnemental IDDEA   n°IC090215 version A\n\nLes prélèvements pour analyse ont concerné la parcelle s’étendant du 105 au 109 bis avenue du Président Kennedy sur la commune de Villeneuve-Saint-Georges.\nIl a été procédé à 7 sondages à la tarière (S1 à S7), de profondeur à partir du niveau du sol variant de 3 à 4,5 mètres, répartis, en fonction des informations fournies par le gérant, en tenant compte de l'activité et de la présence, antérieure ou non, d'équipements potentiellement polluants.\n\nLes analyses de sol, réalisées sur 9  échantillons en fonction des observations lithologiques & organoleptiques par le laboratoire AGROLAB (possédant les agréments MEEDDM & accréditations COFRAC nécessaires), ont concerné :\n    • Les hydrocarbures totaux (HCT) par GC-FID avec répartition des fractions carbonées, \n    • Les Métaux lourds ML (As, Cd, Cr, Cu, Hg, Ni, Pb, Zn), \n    • Les Hydrocarbures Aromatiques Polycycliques (HAP), \n    • Les Composés Organiques Volatils comprenant les Composés Organo-Halogénés Volatils (COHV) et les BTEX (Benzène, Toluène, Ethylbenzène, Xylènes).\n\nLa campagne de mesures effectuée sur la nappe a été réalisée au moyen de deux piézomètres positionnés les 23 et 26/09/09, respectivement en amont (pz1 à l’est du site, profondeur 7 m, niveau piézo 4,75 m) et en aval (pz2 au sud-ouest du site, profondeur 8,86 m, niveau piézo 3,85 m) hydraulique supposés du site sur les échantillons desquels ont été recherchés les paramètres suivants: HCT, Métaux Lourds, HAP , COHV et BTEX.\n\nLes analyses chimiques portant sur deux échantillons d’eau de nappe ont été effectuées par le laboratoire WESSLING (possédant les agréments MEEDDM & accréditations COFRAC nécessaires) et  les paramètres mesurés sont identiques à ceux recherchés dans les échantillons du sol.\n\nLes investigations de terrain et déterminations analytiques réalisées sur les sols et dans les eaux souterraines dans le cadre de cette étude ont mis en évidence :\n\n    • pour les échantillons de sol :\n        ◦ une odeur d’hydrocarbures et une couleur noire au droit du sondage S7 entre 0,9 et 1,7 m ainsi qu’au droit du sondage S2 entre 0,1 et 1 m ;\n        ◦ pour le sondage S3 notamment, des teneurs en métaux lourds ponctuellement supérieures (pour le cadmium, le cuivre, le mercure, le plomb et le zinc pour 3 échantillons sur les 9 analysés) ou entrant dans la gamme de valeurs couramment observées dans le cas de sols ordinaires ;\n        ◦ l’absence de pollution notable des sols par les HAP ;\n        ◦ l’absence de teneurs significatives en COHV et BTEX au droit des zones investiguées :\n        ◦ la présence de teneurs en HCT supérieures au critère de l’arrêté de mars 2006 au droit des sondages S2 entre 0,1 et 1 m, S3 entre 0,6 et 1,1 m et S7 entre 0,9 et 1,7 m.\n\n    • pour les échantillons prélevés dans les eaux souterraines : une absence d’impact notable pour tous les paramètres analysés :\n\n    • les teneurs mesurées en métaux lourds, hydrocarbures totaux, COHV et BTEX sont inférieures  à la limite de quantification du laboratoire et à celles de la qualité des eaux brutes pour la production d’eau potable conformément au décret du 11/01/2007 et aux valeurs de l’OMS quand elles sont disponibles ;\n    • les analyses relatives à la recherche des HAP indiquent des résultats inférieures aux valeurs seuils de qualité des eaux potables.\n\nSur la base des éléments décrits précédemment, le bureau d’études apporte les commentaires suivants :\n    • les impacts superficiels constatés en HCT (fractions lourdes essentiellement) au droit des sondages S2 (bâtiment faisant office de réfectoire et de vestiaire/ ancien atelier mécanique de garage) et S3 (parc de bennes en transit/ ancienne réserve en pièces détachées de garage) semblent être attribuables à des activités antérieures à celle qui était exercée par la société AFB FERNANDES ;\n    • l’anomalie relevée au niveau du sondage S7 (bac de rétention des hydrocarbures) serait quant à elle liée à l’activité exercée par la société AFB FERNANDES.","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040020501","Etude SSP et ingénierie des travaux de réhabilitation","2012-07-19",null,"Diagnostic environnemental ENVIRON\n\nLes sols du site sont constitués de remblais reposant sur des terrains naturels composés de limons argileux et argiles limoneuses. \nLa société ENVIRON a procédé à l’implantation de 18 sondages à 4 mètres de profondeur.\n      \n Trois piézomètres ont été réalisés jusqu’à 7,5 mètres et 9 mètres de profondeur. Trois échantillons de la nappe d’eau souterraine et un échantillon d’eau résiduaire ont été collectés le 11/04/2012 pour les HCT, COHV, BTEX, HAP et métaux lourds.\n\nAfin d’identifier les risques liés aux COHV dans l’air intérieur du bâtiment, 6 prélèvements d’air, nommés M1 à M5 et un blanc de transport ont été effectués le 29/10/2012, au droit des sondages ayant révélé la présence de traces de COHV.\n\nLes résultats des investigations menées par la société ENVIRON, mettent en évidence les points suivants :\n\na) dans les sols, zones extérieures du site :\n            ▪ des teneurs en métaux (cuivre, Plomb et Zinc) dans la gamme des valeurs observées dans le cas de fortes anomalies naturelles ;\n            ▪ des concentrations en BTEX, COHV et PCB inférieures aux seuils de détection ; \n            ▪ de faibles concentrations en HAP comprises entre 0,5 et 5,3 mg/kg ; \n            ▪ des teneurs traces comprises entre 20 et 65 mg/kg en hydrocarbures totaux (C10-C40) avec une concentration maximale (210 mg/kg) observée sur le sondage S3 entre    2,7 et 2,9 mètres de profondeur.\n\nb) Dans les sols, zones intérieures du site :\n    • des teneurs en cuivre supérieures à la gamme de valeurs observées dans le cas de fortes anomalies naturelles dans la zone de stockage et dans les locaux, façonnage, offset, reprographie et encre. Les concentrations présentes évoluent entre 120 et 4 900 mg/kg ;\n    • des teneurs en métaux (Cadmium, Plomb et Zinc) comprises dans la gamme de valeurs observées dans le cas de fortes anomalies naturelles dans la zone de stockage et dans les autres locaux ;\n    • des teneurs en BTEX, COHV, et PCB inférieures ou légèrement supérieures aux seuils de détection et des traces de HAP totaux, sur l’ensemble des sols ;\n    • des hydrocarbures globalement présents sur les sols superficiels du site, mais les concentrations restent inférieures au seuil d’acceptation en ISDI (installations de stockage de déchets inertes).\n\nc) Dans les eaux souterraines :\n    • des concentrations inférieures aux seuils de détection pour les métaux, une concentration de 6,1 et 6,4 µg/l en arsenic, des teneurs en BTEX de 6,9 µg/l, des traces de solvants chlorés au droit des PZ1 et PZ2 et aucun impact en HAP et HCT;\n    • un impact en perchloroéthylène, trichloroéthylène (2,9 et 1,12 µg/l ) et chlorure de vinyle de 0,66 µg/l supérieur au seuil (0,5 µg/l) défini par l’arrêté ministériel du 11/01/2007, a été constaté.\n\nd) Concernant les eaux résiduaires de la cuve:\nLes analyses effectuées sur les eaux résiduaires mettent en évidence :\n            ▪ des traces de BTEX ; \n            ▪ du naphtalène à hauteur de 0,79 µg/l ; \n            ▪ du trichloroéthylène (1,8 µg/l), du cis-1. 2- dichloroéthylène (0,35 µg/l), des hydrocarbures totaux à hauteur de 20 µg/l. et l’absence d’impact des métaux.\n\ne) Concernant la qualité de l’air intérieur\nLa présence de PCE (2,59 µg/m3) à l’état de traces au droit de M1, M2 et M5, teneurs restant en deçà des valeurs guides de la qualité de l’air intérieur définies par l’ANSES et l’OMS (250 µg/m3) pour le PCE en exposition long terme, a été constatée.\n\nLes résultats des analyses des sols, des eaux souterraines et de l’air intérieur n’ont révélé aucun impact significatif généralisé à l’ensemble du site et aucun impact en lien avec les activités menées par la Banque de France n’a été identifié.\n\nLe rapport d’analyse de la société ENVIRON indique que les anomalies de concentrations relevées ne sont pas susceptibles, de générer de risques sur site ou hors site.\n\nLe bâtiment sera transformé en ERP 5ème catégorie par la société Leroy Merlin France, nouveau locataire pour accueillir ses clients. \nAu vu des résultats pour l’ensemble des paramètres recherchés et vis-à-vis de l’usage futur du site, le rapport indique  qu’aucune action complémentaire ou de réhabilitation des sols ou des eaux souterraines n’est recommandée.",null,"Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040020801","Etude SSP et ingénierie des travaux de réhabilitation","2015-02-01",null,"Diagnostic environnemental - DEKRA INDUSTRIAL\n\nDes sources potentielles de pollution ont été recensées lors de l’étude historique et documentaire. Dans le cadre de la cessation d’activité, des investigations de terrain ont été menées en février 2015. Elles ont consisté en la réalisation de 10 sondages (S1 à S10) de 2 à 5 mètres de profondeur au droit des principales installations présentant un risque de contamination des sols (voir plan en annexe 1) et à la mise en place de 3 piézairs afin de lever tout doute quant à la présence de composés organiques volatils (COV).\n\nLes résultats d’analyses ont mis en évidence :\n    • de faibles teneurs en hydrocarbures aromatiques polycycliques (HAP) au droit de l’atelier de traitement de surface : 20 mg/kg de matières sèches (MS) et de l’atelier de tribofinition : 9,9 mg/kg MS.\n    • des impacts en éléments métalliques (traces) (valeurs observées dans le cas de fortes anomalies naturelles) dans les échantillons de plusieurs zones : \n          -station de traitement des effluents S5/0,1-0,7 m : présence de nickel (150 mg/kg MS) ;\n          -atelier de tribofinition S7/0,3-1,2 m : présence de cuivre (78 mg/kg MS) et de nickel (230 mg/kg MS) ;\n          -atelier de traitement de surface S8/0,05-0,5 m : présence de nickel (140 mg/kg MS) ;\n          -atelier de traitement de surface S9/0,4-1,4 m : présence de zinc (270 mg/kg MS) ;\n          -stockage de produits chimiques S10/0,05-0,7 m : présence de zinc (480 mg/kg MS) ;\n    • des traces de benzène, toluène, éthylbenzène et xylènes (BTEX) dans la zone de la station de traitement des effluents S5/0,1-0,7 m (0,30 mg/kg MS) et S5/0,7-1,5 m (0,43 mg/kg MS) ;\n    • des traces de composés organiques halogénés volatils (COHV) dans la zone de la station de traitement des effluents, de l’atelier de tribofinition et dans la zone de stockage des produits chimiques ;\n    • l’absence d’hydrocarbures totaux, de COHV, de BTEX et de naphtalène dans l’air du sol (voir tableau en annexe 4).\n\nLe rapport de DEKRA conclut :\n«[…/...] Cependant, au vu des résultats des analyses de sol (teneurs faibles à très faibles) et de gaz du sol (teneurs inférieures aux limites de quantification dans les gaz du sol), le site apparaît compatible en l’état avec l’usage projeté (usage de type industriel). […/...]\n\nEn cas de réaménagement du site, au vu des résultats d’analyses, une attention devra être apportée à la gestion des terres qui pourraient être excavées. […/...]\n\nAu regard de ces éléments, le site en son état actuel et pour l’usage futur considéré ne nécessite pas d’investigations complémentaires. […/...]»",null,"Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040021401","Etude SSP et ingénierie des travaux de réhabilitation","1997-04-11",null,"Diagnostic environnemental A.T.E\n\nLes travaux ont nécessité la réalisation de trois piézomètres PZ1, PZ2 et PZ3 jusqu’à 6,5-7m de profondeur permettant de préciser le sens d’écoulement de la nappe et  l’impact d’une pollution sur les eaux souterraines et de 14 sondages numérotés S4 à S17 jusqu’à 2,5 mètres de profondeur permettant de réaliser des prélèvements pour analyse.\n\nDes prélèvements, de gaz ont été réalisés sur tous les sondages pour étudier une éventuelle pollution par les hydrocarbures volatils.",null,"Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040023601","Etude SSP et ingénierie des travaux de réhabilitation","2004-04-15","2004-10-08","Le diagnostic de sol indique que 5 forages ont été d’abord réalisés le 15 avril 2004, puis 5 autres le 08/10/2004 :\n- Forage n°1 au droit de la cuve SP 98 –SUP (cuve n°2) \n- Forage n°2 pour le contrôle de la cuve de SP95 +Gazole (cuven°3)\n- Forage n°3 pour l’aire de dépotage\n- Forage n°4 pour les évents et le déshuileur\n- Forage n°5 pour la cuve n°3\n\nLes forages F101(6m), F102(10,2m) F104(6m), F105(7,5m) ont été réalisés pour délimiter la pollution verticalement et horizontalement.\nLes résultats des analyses ont mis en évidence un spot de pollution hydrocarbonée non délimité verticalement ni horizontalement au droit de la cuve n°3. Les résultats sont les suivants :\n- au droit de F2 (4,5-5 m) :\n    • BTEX = 1 400 mg/kg\n    • HCT = 1 200 mg/kg\n- au droit de F2 (5 – 5,3 m) :\n    • BTEX = 29 mg/kg\n    • HCT 110 mg/kg\n- au droit de F102 (ç,5 – 10 m) :\n    • BTEX = 290 mg/kg","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040024001","Etude SSP et ingénierie des travaux de réhabilitation","2004-02-10",null,"Réalisation de 6 sondages et 3 piézomètres\nDes indices de pollution (odeurs d’hydrocarbures, coloration grise, vapeurs d’hydrocarbures) existent dans les sols autour de 2 distributeurs de gazole sur la piste poids lourds.\nIl y a une possibilité d’existence d’une lentille d’hydrocabures surnageant sur la nappe en aval par rapport au sens d’écoulement de la nappe et à la source de pollution. ","Eaux souterraines","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040024001","Etude SSP et ingénierie des travaux de réhabilitation","2004-02-20",null,"Des analyses en hydrocarbures totaux et BTEX ont été réalisées sur les 3 piézomètres du site le 20/02/04 La concentration en hydrocarbures au droit de PZ1 a considérablement diminuée.","Eaux souterraines","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040024001","Etude SSP et ingénierie des travaux de réhabilitation","2004-09-01",null,"Des analyses en hydrocarbures totaux et BTEX ont été réalisées sur les 3 piézomètres du site le 01/09/04. On remarque que la teneur en hydrocarbures dans les piézomètres reste inférieure à la VCI non sensible. Une nouvelle campagne est programmée pour le mois de mars 2005, en période de “hautes eaux”.","Eaux souterraines","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040024001","Etude SSP et ingénierie des travaux de réhabilitation","2005-03-08",null,"Des analyses en hydrocarbures totaux et BTEX ont été réalisées sur les 3 piézomètres du site le 08/03/05.\n\nLe rapport conclut que la nappe prélevée se situe à une profondeur moyenne de 5,70 mètres de profondeur en septembre-octobre et entre 5,55 et 5,43 mètres de profondeur en février-mars soit un battement de nappe de 15-25 cm entre les deux périodes.\n\nLa teneur en hydrocarbures totaux au droit du piézomètre PZ1 (aval hydraulique) a fortement chuté depuis le 06 octobre 2003 (16,3 mg/l). Les résultats des deux derniers suivis de la nappe indiquent que la teneur en hydrocarbures  totaux dans la nappe est stable au droit des trois piézomètres. Ils sont inférieurs à la VCI usage non sensible et inférieurs au seuil de détection analytique (50 µg/l).\n\nLes BTEX n’ont pas été analysés au 08 mars 2005 car un incident de transport des échantillons sous flaconnage s’est produit. Toutefois, les teneurs relevées lors du suivi précédent indiquaient des teneurs nulles.","Eaux souterraines","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040024001","Etude SSP et ingénierie des travaux de réhabilitation","2004-02-10",null,"Réalisation de 6 sondages et 3 piézomètres\nDes indices de pollution (odeurs d’hydrocarbures, coloration grise, vapeurs d’hydrocarbures) existent dans les sols autour de 2 distributeurs de gazole sur la piste poids lourds.\nIl y a une possibilité d’existence d’une lentille d’hydrocabures surnageant sur la nappe en aval par rapport au sens d’écoulement de la nappe et à la source de pollution. ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040025201","Etude SSP et ingénierie des travaux de réhabilitation","2012-01-01",null,"Suivi de la qualité des eaux de la nappe pour 2012. \n\nUn nouveau piézomètre a été mis en place en amont hydraulique du site, en mars 2012. Les concentrations les plus importantes sont toujours mesurées dans les piézomètres situés en aval du site. La présence d’une source de pollution sur le site n’est plus exclue. \n\nEn juin 2012, des prélèvements ont été faits dans les deux piézairs présents sur le site. Du trichloréthylène (TCE) : (PZA2 = 158 µg/m3) et du tétrachloroéthylène (PCE) : (PZA2 = 405,5 µg/m3), ont été mis en évidence, sur les deux ouvrages mais avec des concentrations plus importantes sur le PZA2. Ces mêmes composés sont retrouvés dans l’air ambiant des bâtiments, mais à des teneurs très faibles : 0,29 µg/m3 pour le TCE, au maximum et 2,16 µg/m3 pour le PCE.","Air","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040025201","Etude SSP et ingénierie des travaux de réhabilitation","2015-07-01","2015-12-01","Surveillance des gaz du sol et de la nappe souterraine pour juillet et décembre 2015. \n\nLe réseau piézométrique comprend 6 ouvrages répartis sur l’ensemble du site. Les résultats de décembre 2015 confirment l’absence d’hydrocarbures et de BTEX et la présence de solvants chlorés. Pour le trichloréthylène, les teneurs les plus importantes sont mesurées sur le piézomètre PZ5 situé en amont du site (11 µg/l) et le tétrachloréthylène est mesuré sur tous les piézomètres avec les concentrations les plus importantes au droit des piézomètres amont PZ6 (48 µg/l) et PZ2 (47 µg/l) et aval PZ3 (47 µg/l). Les concentrations sont du même ordre de grandeur depuis décembre 2014.\n\nEn ce qui concerne les gaz du sol, les concentrations en trichloréthylène (TCE) et en tétrachloréthylène (PCE) étaient très élevées en juillet 2015, mais en dessous des limites de quantification en décembre 2015. Au droit du piézair Pza1, les concentrations étaient de 1080 µg/m³ pour le TCE et de 2300 µg/m³ pour le PCE en juillet 2015 et < 5,4 µg/m³ pour les deux composés en décembre 2015.\n\nLe bureau d’étude a conclu ses rapports en précisant que :\n    • pour les gaz du sol, l’amélioration de la qualité des gaz des sols sera à confirmer lors d’une prochaine campagne, à réaliser en période estivale ;\n    • pour l’eau de la nappe, les résultats semblent confirmer l’hypothèse d’une source active en PCE et TCE en amont du site. Cependant, compte-tenu des écarts de concentration entre l’amont et l’aval, une source sol présente au droit du site ne peut pas être exclue. Un diagnostic complémentaire permettrait de vérifier l’apport en solvants chlorés en provenance de l’extérieur du site et de statuer quant à la présence d’une source active sur site et en définir l’extension.","Air","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040025201","Etude SSP et ingénierie des travaux de réhabilitation","2016-05-13",null,"Diagnostic environnemental complémentaire - BURGEAP","Air","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040025201","Etude SSP et ingénierie des travaux de réhabilitation","2012-01-01",null,"Suivi de la qualité des eaux de la nappe pour 2012. \n\nUn nouveau piézomètre a été mis en place en amont hydraulique du site, en mars 2012. Les concentrations les plus importantes sont toujours mesurées dans les piézomètres situés en aval du site. La présence d’une source de pollution sur le site n’est plus exclue. \n\nEn juin 2012, des prélèvements ont été faits dans les deux piézairs présents sur le site. Du trichloréthylène (TCE) : (PZA2 = 158 µg/m3) et du tétrachloroéthylène (PCE) : (PZA2 = 405,5 µg/m3), ont été mis en évidence, sur les deux ouvrages mais avec des concentrations plus importantes sur le PZA2. Ces mêmes composés sont retrouvés dans l’air ambiant des bâtiments, mais à des teneurs très faibles : 0,29 µg/m3 pour le TCE, au maximum et 2,16 µg/m3 pour le PCE.","Eaux souterraines","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040025201","Etude SSP et ingénierie des travaux de réhabilitation","2015-07-01","2015-12-01","Surveillance des gaz du sol et de la nappe souterraine pour juillet et décembre 2015. \n\nLe réseau piézométrique comprend 6 ouvrages répartis sur l’ensemble du site. Les résultats de décembre 2015 confirment l’absence d’hydrocarbures et de BTEX et la présence de solvants chlorés. Pour le trichloréthylène, les teneurs les plus importantes sont mesurées sur le piézomètre PZ5 situé en amont du site (11 µg/l) et le tétrachloréthylène est mesuré sur tous les piézomètres avec les concentrations les plus importantes au droit des piézomètres amont PZ6 (48 µg/l) et PZ2 (47 µg/l) et aval PZ3 (47 µg/l). Les concentrations sont du même ordre de grandeur depuis décembre 2014.\n\nEn ce qui concerne les gaz du sol, les concentrations en trichloréthylène (TCE) et en tétrachloréthylène (PCE) étaient très élevées en juillet 2015, mais en dessous des limites de quantification en décembre 2015. Au droit du piézair Pza1, les concentrations étaient de 1080 µg/m³ pour le TCE et de 2300 µg/m³ pour le PCE en juillet 2015 et < 5,4 µg/m³ pour les deux composés en décembre 2015.\n\nLe bureau d’étude a conclu ses rapports en précisant que :\n    • pour les gaz du sol, l’amélioration de la qualité des gaz des sols sera à confirmer lors d’une prochaine campagne, à réaliser en période estivale ;\n    • pour l’eau de la nappe, les résultats semblent confirmer l’hypothèse d’une source active en PCE et TCE en amont du site. Cependant, compte-tenu des écarts de concentration entre l’amont et l’aval, une source sol présente au droit du site ne peut pas être exclue. Un diagnostic complémentaire permettrait de vérifier l’apport en solvants chlorés en provenance de l’extérieur du site et de statuer quant à la présence d’une source active sur site et en définir l’extension.","Eaux souterraines","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040025201","Etude SSP et ingénierie des travaux de réhabilitation","2016-05-13",null,"Diagnostic environnemental complémentaire - BURGEAP","Eaux souterraines","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040025201","Etude SSP et ingénierie des travaux de réhabilitation","2016-05-13",null,"Diagnostic environnemental complémentaire - BURGEAP","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040026001","Etude SSP et ingénierie des travaux de réhabilitation","2014-01-01",null,"Étude du sol, des eaux souterraines, air et gaz du sol.","Air","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040026001","Etude SSP et ingénierie des travaux de réhabilitation","2014-01-01",null,"Étude du sol, des eaux souterraines, air et gaz du sol.","Eaux souterraines","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040026001","Etude SSP et ingénierie des travaux de réhabilitation","2014-01-01",null,"Étude du sol, des eaux souterraines, air et gaz du sol.","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040028901","Exécution des travaux de réhabilitation",null,null,"Dégazage de la cuve","Eaux souterraines","N/A","N/A","N/A","N/A","Mise en place de mesure de réhabilitation",null,"N/A","N/A","N/A"]
["SSP040028901","Exécution des travaux de réhabilitation",null,null,"Dégazage de la cuve","Sol - Sous-sol","N/A","N/A","N/A","N/A","Mise en place de mesure de réhabilitation",null,"N/A","N/A","N/A"]
["SSP040029001","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"Analyses des eaux souterraines, traitement des sols de l'atelier.","Eaux souterraines","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040029001","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"Analyses des eaux souterraines, traitement des sols de l'atelier.","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040031001","Etude SSP et ingénierie des travaux de réhabilitation","2017-11-01",null,"Diagnostic environnemental – EGIS\n\nL’étude historique met en évidence le début de l’exploitation de dépôts de liquides inflammables sur site dès le 19 avril 1907 avant d’abriter, en complément, des activités de garage, d’ateliers mécaniques et de soudure soumis à autorisation à partir du 17 janvier 1924. Cette installation a subi plusieurs modifications (1966, 1969, 1970, 1982) avant d’être réaménagée par la société PEUGEOT SABRIE en 1985-1986 avec l’ajout du hall d’exposition et des bureaux et la suppression de l’aire de lavage.\n\nL’étude de vulnérabilité conclut au caractère :\n    • vulnérable de l’environnement, les premières couches géologiques rencontrées au droit de la zone d’étude étant particulièrement perméables et ne représentant pas de barrière naturelle entre une éventuelle pollution et les ressources aquifères ;\n    • peu sensible de l’environnement, les captages d’alimentation en eau potable (AEP) présents dans le périmètre d’étude étant soit non vulnérables (aquifère de l’Albien protégé) soit en amont hydraulique à plus de 4,8 km de la zone d’étude. Un captage industriel est, toutefois, situé à 200 m en aval hydraulique de la zone d’étude.\n\nLes activités potentiellement polluantes, passées et actuelles, identifiées sont :\n    • les zones de dépôts enterrés de liquides inflammables constituées, notamment, de :\n        ◦ une cuve enterrée de gasoil de 3 000 litres ;\n        ◦ une cuve enterrée de 30 000 litres bicompartimentée (10 000 litres d’essence et 20 000 litres de super), en fosse maçonnée, neutralisée ;\n        ◦ une cuve enterrée de 8 000 litres bicompartimentée (5 000 litres de super et 3 000 litres d’essence), en fosse maçonnée ;\n        ◦ une cuve enterrée de 10 000 litres bicompartimentée (4 000 litres de fioul domestique (FOD) et 6 000 litres de gasoil), en fosse maçonnée, neutralisée ;\n        ◦ une cuve enterrée de 3 000 litres d’huiles usagées en fosse maçonnée ;\n    • l’ancienne zone de dépotage et de distribution de carburant ;\n    • l’ancienne et la nouvelle aire de lavage ;\n    • le séparateur d’hydrocarbures associé à l’aire de lavage ;\n    • les ateliers mécaniques ;\n    • le stockage d’huiles sur rétention ;\n    • l’emplacement « fontaine de nettoyage » ;\n    • l’emplacement du compresseur ;\n    • la zone de stockage de déchets comprenant des fûts de filtres à huiles, de liquide de frein et d’aérosols, un cubitainer d’huiles usagées, ainsi qu’un bac accueillant des batteries usées.\n\nAu total, 37 sondages ont été réalisés.\nDes indices organoleptiques de contamination (odeurs de type hydrocarbures plus ou moins fortes ou odeur indéterminée) ont été identifiés dans les échantillons de prélèvement de sols prélevés à proximité de la fosse accueillant la cuve d’huiles usagées au droit des sondages S14a, S14bis, S14b, S16bis, S19, S20 et S24.\n\nAu total, 81 échantillons ont été analysés. Les résultats d’analyses réalisés ont permis à la société EGIS de mettre en évidence :\n\n    • Concernant les hydrocarbures C10-C40 :\n        ◦ un impact en hydrocarbures au niveau de l’ancienne zone de dépotage des carburants, circonscrit sur site, dont la superficie a été estimée à 9 m² sur une profondeur d’1 mètre, soit environ 9 m³ de terres impactées (concentration maximale analysée de 1 790 mg/kg de MS entre 0,2 et 1 m de profondeur au niveau du sondage S9) ;\n        ◦ un impact en hydrocarbures au niveau de l’ancien atelier de réparation/d’entretien mécanique/proximité de la fosse avec la cuve de 3 000 litres d’huiles usagées, qui semble circonscrit sur site, dont le volume de terres impactées a été estimé à 250 m³ (superficie de 5 à 35 m² pour une profondeur comprise entre 2 et 15 m).\n        ◦ un impact en hydrocarbures au niveau de l’atelier (coté Est), dans la zone d’entretien, près du second pont élévateur à proximité de l’ancienne fontaine de dégraissage, circonscrit sur site, dont la superficie est estimée à 15 m² sur une profondeur de 0,5 m, soit un volume de terres impactées d’environ 8 m³ (concentration maximale analysée de 725 mg/kg de MS entre 0,05 et 0,5 m de profondeur au niveau du sondage S17).\n\n    • Concernant les BTEX, un impact a été identifié au niveau de l’ancien atelier de réparation/d’entretien mécanique/proximité de la fosse avec la cuve de 3 000 litres d’huiles usagées, à une profondeur comprise entre 3 et 7,5 m, au niveau du sondage S24 (concentration maximale analysée de 28 mg/kg de MS entre 6 et 7,5 m de profondeur).\n    • Concernant les HAP, un impact a été identifié au niveau de la zone d’entretien près du pont-élévateur et de l’ancienne fontaine de dégraissage, au droit du sondage S17 (concentration maximale analysée de 270 mg/kg de MS entre 0,05 et 0,5 m de profondeur).\n    • Concernant les métaux, des dépassements de la valeur guide niveau 2 ASPITET ont été relevés pour :\n        ◦ le zinc au niveau du sondage S9 entre 0,2 et 1 m de profondeur (290 mg/kg de MS mesuré pour 250 mg/kg de MS);\n        ◦ le plomb au niveau des sondages S11 (profondeur de 0,05 à 1 m), S12 (profondeur de 0,05 à 1 m), S13 (profondeur de 0,1 à 1 m), S15 (profondeur de 0,05 à 1 m), S16 (profondeur de 0,05 à 1 m) et S17 (profondeur de 0,05 à 0,5 m). La concentration maximale a été mesurée au niveau du sondage S15 (740 mg/kg de MS pour 90 mg/kg de MS).\n          \nLa société EGIS émet l’hypothèse que ces dépassements du fond géochimique sont probablement liés à la qualité intrinsèque des remblais de surface.\n\n    • Investigations sur les eaux souterraines et résultats d’analyse :\nLes eaux souterraines ont été prélevées les 31 mai et 29 juin 2017.\nLes niveaux d’eaux observés lors de ces deux interventions étaient de 15,78 m le 31 mai 2017, puis de 15,66 m le 29 juin 2017.\nLes analyses effectuées ont permis de mettre en évidence des traces non significatives d’hydrocarbures HCT C10-C40, de HAP, de BTEX et de COHV, dont les concentrations mesurées étaient assez similaires entre les deux campagnes.\nUn léger impact en nickel a été observé (28 μg/l le 31 mai, puis 31 μg/l le 29 juin pour une valeur guide 20 μg/l) dont l’origine n’est pas connue (cet impact n’a pas été décelé dans les sols).\n\n    • Investigations sur les gaz du sol et résultats d’analyse :\nDes teneurs supérieures aux limites de quantification du laboratoire sont relevées pour les composés des BTEX et les hydrocarbures aromatiques C6-C10.\n\nLe schéma conceptuel proposé par la société EGIS amène à retenir un risque potentiel sur site, pour les futurs employés, par inhalation de composés volatils avec les sols impactés par les hydrocarbures. Ce risque est potentiel en milieu intérieur (sondages impactés – S14, S14bis, S17, PZ1, S18, S20, S24 et S 26 pour les HCT C10-C40 / S17 pour les HAP).","Air","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040031001","Etude SSP et ingénierie des travaux de réhabilitation","2017-11-01",null,"EQRS – EGIS \n\nL’ EQRS a été réalisée sur la base d’un usage industriel dans la configuration actuelle du site (bâtiment atelier au rez-de-chaussée) dans le cas d’une inhalation de polluants (BTEX et hydrocarbures aromatiques C6-C10 mesurés dans le gaz des sols) par les employés du garage dans l’air intérieur du bâtiment (atelier) constituant les cibles potentielles.\nSelon la société EGIS, les calculs de risques sanitaires ont mis en évidence que le risque sanitaire est considéré comme acceptable en modélisant le dégazage depuis les gaz des sols, en considérant la seule voie de transfert par inhalation, pour des employés du garage travaillant dans l’atelier.\n\nLa société EGIS recommande d’envisager de procéder à la purge des terres reconnues impactées dans la zone de la cuve d’huiles usagées posée en fosse non étanche jusqu’à limite technique (suivi par un bureau d’études spécialisé en environnement et envoi des terres en filière agréée). Un plan de gestion devra définir les meilleures modalités techniques à mettre en œuvre. \nCette recommandation figure également en conclusion de l’EQRS dans laquelle la société EGIS précise qu’ « afin de garantir la maîtrise des sources concentrées de pollution dans le contexte de l‘usage actuel du site et dans une optique d’amélioration de la qualité environnementale des milieux, une mesure de gestion de la source sol doit être mise en place ».","Air","Analyse des enjeux sanitaires (EQRS, ARR)","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040031001","Etude SSP et ingénierie des travaux de réhabilitation","2017-11-01",null,"Diagnostic environnemental – EGIS\n\nL’étude historique met en évidence le début de l’exploitation de dépôts de liquides inflammables sur site dès le 19 avril 1907 avant d’abriter, en complément, des activités de garage, d’ateliers mécaniques et de soudure soumis à autorisation à partir du 17 janvier 1924. Cette installation a subi plusieurs modifications (1966, 1969, 1970, 1982) avant d’être réaménagée par la société PEUGEOT SABRIE en 1985-1986 avec l’ajout du hall d’exposition et des bureaux et la suppression de l’aire de lavage.\n\nL’étude de vulnérabilité conclut au caractère :\n    • vulnérable de l’environnement, les premières couches géologiques rencontrées au droit de la zone d’étude étant particulièrement perméables et ne représentant pas de barrière naturelle entre une éventuelle pollution et les ressources aquifères ;\n    • peu sensible de l’environnement, les captages d’alimentation en eau potable (AEP) présents dans le périmètre d’étude étant soit non vulnérables (aquifère de l’Albien protégé) soit en amont hydraulique à plus de 4,8 km de la zone d’étude. Un captage industriel est, toutefois, situé à 200 m en aval hydraulique de la zone d’étude.\n\nLes activités potentiellement polluantes, passées et actuelles, identifiées sont :\n    • les zones de dépôts enterrés de liquides inflammables constituées, notamment, de :\n        ◦ une cuve enterrée de gasoil de 3 000 litres ;\n        ◦ une cuve enterrée de 30 000 litres bicompartimentée (10 000 litres d’essence et 20 000 litres de super), en fosse maçonnée, neutralisée ;\n        ◦ une cuve enterrée de 8 000 litres bicompartimentée (5 000 litres de super et 3 000 litres d’essence), en fosse maçonnée ;\n        ◦ une cuve enterrée de 10 000 litres bicompartimentée (4 000 litres de fioul domestique (FOD) et 6 000 litres de gasoil), en fosse maçonnée, neutralisée ;\n        ◦ une cuve enterrée de 3 000 litres d’huiles usagées en fosse maçonnée ;\n    • l’ancienne zone de dépotage et de distribution de carburant ;\n    • l’ancienne et la nouvelle aire de lavage ;\n    • le séparateur d’hydrocarbures associé à l’aire de lavage ;\n    • les ateliers mécaniques ;\n    • le stockage d’huiles sur rétention ;\n    • l’emplacement « fontaine de nettoyage » ;\n    • l’emplacement du compresseur ;\n    • la zone de stockage de déchets comprenant des fûts de filtres à huiles, de liquide de frein et d’aérosols, un cubitainer d’huiles usagées, ainsi qu’un bac accueillant des batteries usées.\n\nAu total, 37 sondages ont été réalisés.\nDes indices organoleptiques de contamination (odeurs de type hydrocarbures plus ou moins fortes ou odeur indéterminée) ont été identifiés dans les échantillons de prélèvement de sols prélevés à proximité de la fosse accueillant la cuve d’huiles usagées au droit des sondages S14a, S14bis, S14b, S16bis, S19, S20 et S24.\n\nAu total, 81 échantillons ont été analysés. Les résultats d’analyses réalisés ont permis à la société EGIS de mettre en évidence :\n\n    • Concernant les hydrocarbures C10-C40 :\n        ◦ un impact en hydrocarbures au niveau de l’ancienne zone de dépotage des carburants, circonscrit sur site, dont la superficie a été estimée à 9 m² sur une profondeur d’1 mètre, soit environ 9 m³ de terres impactées (concentration maximale analysée de 1 790 mg/kg de MS entre 0,2 et 1 m de profondeur au niveau du sondage S9) ;\n        ◦ un impact en hydrocarbures au niveau de l’ancien atelier de réparation/d’entretien mécanique/proximité de la fosse avec la cuve de 3 000 litres d’huiles usagées, qui semble circonscrit sur site, dont le volume de terres impactées a été estimé à 250 m³ (superficie de 5 à 35 m² pour une profondeur comprise entre 2 et 15 m).\n        ◦ un impact en hydrocarbures au niveau de l’atelier (coté Est), dans la zone d’entretien, près du second pont élévateur à proximité de l’ancienne fontaine de dégraissage, circonscrit sur site, dont la superficie est estimée à 15 m² sur une profondeur de 0,5 m, soit un volume de terres impactées d’environ 8 m³ (concentration maximale analysée de 725 mg/kg de MS entre 0,05 et 0,5 m de profondeur au niveau du sondage S17).\n\n    • Concernant les BTEX, un impact a été identifié au niveau de l’ancien atelier de réparation/d’entretien mécanique/proximité de la fosse avec la cuve de 3 000 litres d’huiles usagées, à une profondeur comprise entre 3 et 7,5 m, au niveau du sondage S24 (concentration maximale analysée de 28 mg/kg de MS entre 6 et 7,5 m de profondeur).\n    • Concernant les HAP, un impact a été identifié au niveau de la zone d’entretien près du pont-élévateur et de l’ancienne fontaine de dégraissage, au droit du sondage S17 (concentration maximale analysée de 270 mg/kg de MS entre 0,05 et 0,5 m de profondeur).\n    • Concernant les métaux, des dépassements de la valeur guide niveau 2 ASPITET ont été relevés pour :\n        ◦ le zinc au niveau du sondage S9 entre 0,2 et 1 m de profondeur (290 mg/kg de MS mesuré pour 250 mg/kg de MS);\n        ◦ le plomb au niveau des sondages S11 (profondeur de 0,05 à 1 m), S12 (profondeur de 0,05 à 1 m), S13 (profondeur de 0,1 à 1 m), S15 (profondeur de 0,05 à 1 m), S16 (profondeur de 0,05 à 1 m) et S17 (profondeur de 0,05 à 0,5 m). La concentration maximale a été mesurée au niveau du sondage S15 (740 mg/kg de MS pour 90 mg/kg de MS).\n          \nLa société EGIS émet l’hypothèse que ces dépassements du fond géochimique sont probablement liés à la qualité intrinsèque des remblais de surface.\n\n    • Investigations sur les eaux souterraines et résultats d’analyse :\nLes eaux souterraines ont été prélevées les 31 mai et 29 juin 2017.\nLes niveaux d’eaux observés lors de ces deux interventions étaient de 15,78 m le 31 mai 2017, puis de 15,66 m le 29 juin 2017.\nLes analyses effectuées ont permis de mettre en évidence des traces non significatives d’hydrocarbures HCT C10-C40, de HAP, de BTEX et de COHV, dont les concentrations mesurées étaient assez similaires entre les deux campagnes.\nUn léger impact en nickel a été observé (28 μg/l le 31 mai, puis 31 μg/l le 29 juin pour une valeur guide 20 μg/l) dont l’origine n’est pas connue (cet impact n’a pas été décelé dans les sols).\n\n    • Investigations sur les gaz du sol et résultats d’analyse :\nDes teneurs supérieures aux limites de quantification du laboratoire sont relevées pour les composés des BTEX et les hydrocarbures aromatiques C6-C10.\n\nLe schéma conceptuel proposé par la société EGIS amène à retenir un risque potentiel sur site, pour les futurs employés, par inhalation de composés volatils avec les sols impactés par les hydrocarbures. Ce risque est potentiel en milieu intérieur (sondages impactés – S14, S14bis, S17, PZ1, S18, S20, S24 et S 26 pour les HCT C10-C40 / S17 pour les HAP).","Eaux souterraines","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040031001","Etude SSP et ingénierie des travaux de réhabilitation","2017-11-01",null,"EQRS – EGIS \n\nL’ EQRS a été réalisée sur la base d’un usage industriel dans la configuration actuelle du site (bâtiment atelier au rez-de-chaussée) dans le cas d’une inhalation de polluants (BTEX et hydrocarbures aromatiques C6-C10 mesurés dans le gaz des sols) par les employés du garage dans l’air intérieur du bâtiment (atelier) constituant les cibles potentielles.\nSelon la société EGIS, les calculs de risques sanitaires ont mis en évidence que le risque sanitaire est considéré comme acceptable en modélisant le dégazage depuis les gaz des sols, en considérant la seule voie de transfert par inhalation, pour des employés du garage travaillant dans l’atelier.\n\nLa société EGIS recommande d’envisager de procéder à la purge des terres reconnues impactées dans la zone de la cuve d’huiles usagées posée en fosse non étanche jusqu’à limite technique (suivi par un bureau d’études spécialisé en environnement et envoi des terres en filière agréée). Un plan de gestion devra définir les meilleures modalités techniques à mettre en œuvre. \nCette recommandation figure également en conclusion de l’EQRS dans laquelle la société EGIS précise qu’ « afin de garantir la maîtrise des sources concentrées de pollution dans le contexte de l‘usage actuel du site et dans une optique d’amélioration de la qualité environnementale des milieux, une mesure de gestion de la source sol doit être mise en place ».","Eaux souterraines","Analyse des enjeux sanitaires (EQRS, ARR)","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040031001","Etude SSP et ingénierie des travaux de réhabilitation","2017-11-01",null,"Diagnostic environnemental – EGIS\n\nL’étude historique met en évidence le début de l’exploitation de dépôts de liquides inflammables sur site dès le 19 avril 1907 avant d’abriter, en complément, des activités de garage, d’ateliers mécaniques et de soudure soumis à autorisation à partir du 17 janvier 1924. Cette installation a subi plusieurs modifications (1966, 1969, 1970, 1982) avant d’être réaménagée par la société PEUGEOT SABRIE en 1985-1986 avec l’ajout du hall d’exposition et des bureaux et la suppression de l’aire de lavage.\n\nL’étude de vulnérabilité conclut au caractère :\n    • vulnérable de l’environnement, les premières couches géologiques rencontrées au droit de la zone d’étude étant particulièrement perméables et ne représentant pas de barrière naturelle entre une éventuelle pollution et les ressources aquifères ;\n    • peu sensible de l’environnement, les captages d’alimentation en eau potable (AEP) présents dans le périmètre d’étude étant soit non vulnérables (aquifère de l’Albien protégé) soit en amont hydraulique à plus de 4,8 km de la zone d’étude. Un captage industriel est, toutefois, situé à 200 m en aval hydraulique de la zone d’étude.\n\nLes activités potentiellement polluantes, passées et actuelles, identifiées sont :\n    • les zones de dépôts enterrés de liquides inflammables constituées, notamment, de :\n        ◦ une cuve enterrée de gasoil de 3 000 litres ;\n        ◦ une cuve enterrée de 30 000 litres bicompartimentée (10 000 litres d’essence et 20 000 litres de super), en fosse maçonnée, neutralisée ;\n        ◦ une cuve enterrée de 8 000 litres bicompartimentée (5 000 litres de super et 3 000 litres d’essence), en fosse maçonnée ;\n        ◦ une cuve enterrée de 10 000 litres bicompartimentée (4 000 litres de fioul domestique (FOD) et 6 000 litres de gasoil), en fosse maçonnée, neutralisée ;\n        ◦ une cuve enterrée de 3 000 litres d’huiles usagées en fosse maçonnée ;\n    • l’ancienne zone de dépotage et de distribution de carburant ;\n    • l’ancienne et la nouvelle aire de lavage ;\n    • le séparateur d’hydrocarbures associé à l’aire de lavage ;\n    • les ateliers mécaniques ;\n    • le stockage d’huiles sur rétention ;\n    • l’emplacement « fontaine de nettoyage » ;\n    • l’emplacement du compresseur ;\n    • la zone de stockage de déchets comprenant des fûts de filtres à huiles, de liquide de frein et d’aérosols, un cubitainer d’huiles usagées, ainsi qu’un bac accueillant des batteries usées.\n\nAu total, 37 sondages ont été réalisés.\nDes indices organoleptiques de contamination (odeurs de type hydrocarbures plus ou moins fortes ou odeur indéterminée) ont été identifiés dans les échantillons de prélèvement de sols prélevés à proximité de la fosse accueillant la cuve d’huiles usagées au droit des sondages S14a, S14bis, S14b, S16bis, S19, S20 et S24.\n\nAu total, 81 échantillons ont été analysés. Les résultats d’analyses réalisés ont permis à la société EGIS de mettre en évidence :\n\n    • Concernant les hydrocarbures C10-C40 :\n        ◦ un impact en hydrocarbures au niveau de l’ancienne zone de dépotage des carburants, circonscrit sur site, dont la superficie a été estimée à 9 m² sur une profondeur d’1 mètre, soit environ 9 m³ de terres impactées (concentration maximale analysée de 1 790 mg/kg de MS entre 0,2 et 1 m de profondeur au niveau du sondage S9) ;\n        ◦ un impact en hydrocarbures au niveau de l’ancien atelier de réparation/d’entretien mécanique/proximité de la fosse avec la cuve de 3 000 litres d’huiles usagées, qui semble circonscrit sur site, dont le volume de terres impactées a été estimé à 250 m³ (superficie de 5 à 35 m² pour une profondeur comprise entre 2 et 15 m).\n        ◦ un impact en hydrocarbures au niveau de l’atelier (coté Est), dans la zone d’entretien, près du second pont élévateur à proximité de l’ancienne fontaine de dégraissage, circonscrit sur site, dont la superficie est estimée à 15 m² sur une profondeur de 0,5 m, soit un volume de terres impactées d’environ 8 m³ (concentration maximale analysée de 725 mg/kg de MS entre 0,05 et 0,5 m de profondeur au niveau du sondage S17).\n\n    • Concernant les BTEX, un impact a été identifié au niveau de l’ancien atelier de réparation/d’entretien mécanique/proximité de la fosse avec la cuve de 3 000 litres d’huiles usagées, à une profondeur comprise entre 3 et 7,5 m, au niveau du sondage S24 (concentration maximale analysée de 28 mg/kg de MS entre 6 et 7,5 m de profondeur).\n    • Concernant les HAP, un impact a été identifié au niveau de la zone d’entretien près du pont-élévateur et de l’ancienne fontaine de dégraissage, au droit du sondage S17 (concentration maximale analysée de 270 mg/kg de MS entre 0,05 et 0,5 m de profondeur).\n    • Concernant les métaux, des dépassements de la valeur guide niveau 2 ASPITET ont été relevés pour :\n        ◦ le zinc au niveau du sondage S9 entre 0,2 et 1 m de profondeur (290 mg/kg de MS mesuré pour 250 mg/kg de MS);\n        ◦ le plomb au niveau des sondages S11 (profondeur de 0,05 à 1 m), S12 (profondeur de 0,05 à 1 m), S13 (profondeur de 0,1 à 1 m), S15 (profondeur de 0,05 à 1 m), S16 (profondeur de 0,05 à 1 m) et S17 (profondeur de 0,05 à 0,5 m). La concentration maximale a été mesurée au niveau du sondage S15 (740 mg/kg de MS pour 90 mg/kg de MS).\n          \nLa société EGIS émet l’hypothèse que ces dépassements du fond géochimique sont probablement liés à la qualité intrinsèque des remblais de surface.\n\n    • Investigations sur les eaux souterraines et résultats d’analyse :\nLes eaux souterraines ont été prélevées les 31 mai et 29 juin 2017.\nLes niveaux d’eaux observés lors de ces deux interventions étaient de 15,78 m le 31 mai 2017, puis de 15,66 m le 29 juin 2017.\nLes analyses effectuées ont permis de mettre en évidence des traces non significatives d’hydrocarbures HCT C10-C40, de HAP, de BTEX et de COHV, dont les concentrations mesurées étaient assez similaires entre les deux campagnes.\nUn léger impact en nickel a été observé (28 μg/l le 31 mai, puis 31 μg/l le 29 juin pour une valeur guide 20 μg/l) dont l’origine n’est pas connue (cet impact n’a pas été décelé dans les sols).\n\n    • Investigations sur les gaz du sol et résultats d’analyse :\nDes teneurs supérieures aux limites de quantification du laboratoire sont relevées pour les composés des BTEX et les hydrocarbures aromatiques C6-C10.\n\nLe schéma conceptuel proposé par la société EGIS amène à retenir un risque potentiel sur site, pour les futurs employés, par inhalation de composés volatils avec les sols impactés par les hydrocarbures. Ce risque est potentiel en milieu intérieur (sondages impactés – S14, S14bis, S17, PZ1, S18, S20, S24 et S 26 pour les HCT C10-C40 / S17 pour les HAP).","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040031001","Etude SSP et ingénierie des travaux de réhabilitation","2017-11-01",null,"EQRS – EGIS \n\nL’ EQRS a été réalisée sur la base d’un usage industriel dans la configuration actuelle du site (bâtiment atelier au rez-de-chaussée) dans le cas d’une inhalation de polluants (BTEX et hydrocarbures aromatiques C6-C10 mesurés dans le gaz des sols) par les employés du garage dans l’air intérieur du bâtiment (atelier) constituant les cibles potentielles.\nSelon la société EGIS, les calculs de risques sanitaires ont mis en évidence que le risque sanitaire est considéré comme acceptable en modélisant le dégazage depuis les gaz des sols, en considérant la seule voie de transfert par inhalation, pour des employés du garage travaillant dans l’atelier.\n\nLa société EGIS recommande d’envisager de procéder à la purge des terres reconnues impactées dans la zone de la cuve d’huiles usagées posée en fosse non étanche jusqu’à limite technique (suivi par un bureau d’études spécialisé en environnement et envoi des terres en filière agréée). Un plan de gestion devra définir les meilleures modalités techniques à mettre en œuvre. \nCette recommandation figure également en conclusion de l’EQRS dans laquelle la société EGIS précise qu’ « afin de garantir la maîtrise des sources concentrées de pollution dans le contexte de l‘usage actuel du site et dans une optique d’amélioration de la qualité environnementale des milieux, une mesure de gestion de la source sol doit être mise en place ».","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040031001","Etude SSP et ingénierie des travaux de réhabilitation","2018-04-01",null,"Plan de Gestion – EGIS\n\nUne caractérisation de l’état des milieux a été réalisée afin d’identifier les zones à intégrer dans le plan de gestion. Les zones retenues sont celles qui présentent des pollutions significatives et susceptibles d’avoir des conséquences aux regards des enjeux identifiés, de celles qui sont modérées et/ou confinées, avec un impact environnemental négligeable, et qui ne sont donc pas prises en compte dans la réflexion globale du plan de gestion.\nTrois zones de sols contaminés ont été identifiés, chacune possédant ses propres traceurs de pollution :\n    • la zone 1 (ancienne cuve d’huiles usagées en fosse non étanche) avec présence de HCT C10-C40 et BTEX ;\n    • la zone 2 (ancienne aire de dépotage de carburants) avec présence de HCT C10-C40 ;\n    • la zone 3 (ancienne fontaine de dégraissage) avec présence de HAP.\n      \nLa définition des sources concentrées a été effectuée à l’aide de méthodes d’interprétation statistique et de bilan massique fondé sur des méthodes déterministes.\nSelon la société EGIS, les résultats de ces deux méthodes convergent et font état :\n    • d’un seuil de coupure à 5 000 mg/kg MS pour les hydrocarbures HCT C10-C40. Le bilan massique de ce polluant permet d’identifier que la gamme de teneurs au-dessus de ce seuil de coupure correspond à 4 % du volume du sol et 86 % de la masse de polluant ;\n    • d’un seuil de coupure à 20 mg/kg MS pour les HAP. Le bilan massique de ce polluant permet d’identifier que la gamme de teneurs au-dessus de ce seuil de coupure correspond à 3 % du volume du sol et 31 % de la masse de polluant ;\n    • d’un seuil de coupure à 5 mg/kg MS pour les BTEX. Le bilan massique de ce polluant permet d’identifier que la gamme de teneurs au-dessus de ce seuil de coupure correspond à 17 % du volume du sol et 93 % de la masse de polluant.\n\nL’analyse des enjeux réalisée par la société EGIS a conclu à l’absence d’enjeux sanitaires et à l’existence d’un enjeu environnemental lié à la qualité des sols au droit du site. La société EGIS déclare qu’ « il convient de procéder à la mise en œuvre de mesures de gestion concernant les impacts identifiés pour le milieu sol au droit de la cuve enterrée d’huiles usagées placée en fosse non étanche et de l’ancienne fontaine de dégraissage, l’impact en hydrocarbures C10-C40 identifié au droit de l’ancienne zone de dépotage de carburants n’impliquant pas d’enjeu environnemental ni sanitaire ».\n\nLe plan de gestion définit les objectifs de dépollution et précise :\n    • les seuils de dépollution retenus :\n        ◦ teneurs en hydrocarbures C10-C40 supérieures à 5 000 mg/kg de MS, permettant de traiter 86 % de la masse de polluant ;\n        ◦ teneurs en hydrocarbures HAP supérieures à 20 mg/kg de MS, permettant de traiter 31 % de la masse de polluant ;\n        ◦ teneurs en hydrocarbures BTEX supérieures à 5 mg/kg de MS, permettant de traiter 93 % de la masse de polluant ;\n\nÀ l’issue de l’étude des solutions de gestion prenant en compte deux scénarios (conservation du bâtiment ou démolition du bâtiment) et du bilan coûts-avantages des deux solutions retenues pour chaque scénario, la société EGIS a retenu :\n    • dans le cas du maintien du bâtiment en place, le scénario de traitement des sols pollués qui obtient la meilleure note est celui de la désorption thermique, dont les critères de réduction de la masse de polluant et de nuisances moindres ressortent favorables, comparativement au scénario d’excavation et de traitement des terres hors site ;\n    • dans le cas de la démolition du bâtiment, les contraintes du bâti ne rentrant plus en compte, le scénario, de traitement par excavation séquentielles en pieux forés tubés obtient la meilleure note, principalement pour le coût et le délai de traitement moindre.\n      \nLes solutions retenues nécessitent des études de faisabilité pour permettre de préciser les coûts (étude géotechnique et repérage des réseaux et étude de dévoiement).",null,"Plan de gestion","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040031101","Etude SSP et ingénierie des travaux de réhabilitation","2019-10-01",null,"Diagnostic de pollution des sols complémentaires - TESORA \n\nCe diagnostic s’inscrit dans le cadre de la définition des contraintes environnementales du site vis-à-vis de l’aménagement envisagé, à savoir la construction de deux bâtiments de logements sur un niveau de sous-sol communiquant, ainsi que l’aménagement d’espaces verts collectifs. Le périmètre de cet aménagement inclut notamment les parcelles anciennement exploitées par la société GIBERT FRÈRES.\n\nCe diagnostic a été réalisé en complément du diagnostic effectué par la société AIC Environnement fin 2017 et comporte :\n    • des investigations sur les sols ;\n    • des investigations sur les gaz de sols ;\n    • une analyse des enjeux sanitaires ;\n    • des mesures simples de gestion.\n    • Investigations sur les sols :\n\nLes investigations complémentaires ont consisté en la réalisation de 20 sondages de sols, réalisés jusqu’à des profondeurs de 1,5 à 6 m, dont les 14 suivants, réalisés sur l’emprise des anciennes installations exploitées par la société GIBERT FRÈRES :\n    • 11 à proximité des zones de cuves enterrées de liquides inflammables (2 sondages ont subis plusieurs refus ce qui a limité la profondeur de ceux-ci respectivement à 2 m et à 1 m) ;\n    • 1 à proximité de l’aire de lavage de véhicule ;\n    • 1 à proximité de la fosse à charbon ;\n    • 1 à proximité du stockage de bois de chauffage.\n\nLes résultats des analyses de ces sondages, couplés avec ceux obtenus par la société AIC ENVIRONNEMENT, ont permis au bureau d’études TESORA de formuler les constats suivants au niveau de l’emprise de l’ancienne société GIBERT FRÈRES :\n\n    • au droit du futur sous-sol :\n        ◦ source en HAP au droit du sondage S5 (source AIC ENVIRONNEMENT), délimitée horizontalement par les sondages T11 et T12, et verticalement jusqu’à 2 m de profondeur ;\n        ◦ source en HAP et HCT au droit des sondages T7 et T8 ;\n        ◦ dépassement ponctuel de la valeur réglementaire en fraction soluble / sulfates pour 25 % des remblais (au niveau du sondage S3) ;\n        ◦ dépassement diffus des valeurs réglementaires en fluorures pour la lithologie argiles vertes (comprise entre 2 et 3 m de profondeur) ;\n\n    • au droit des futurs espaces verts :\n        ◦ source en HCT au droit du sondage S6 (AIC ENVIRONNEMENT) et des sondages T5 et T6, délimitée horizontalement par les sondages T2, T3 et T4, mais non délimitée verticalement (3 m de profondeur pris en compte au regard du changement de lithologie constaté à cette profondeur).\n          \nLes investigations de sols effectuées sur les parcelles autres que celles anciennement exploitées par la société GIBERT FRÈRES ont permis de mettre en évidence :\n    • au droit du futur sous-sol, l’absence d’anomalies en HCT, HAP, composés organo-halogénés volatils (COHV) et Benzène, Toluène, Éthylbenzène et Xylènes (BTEX) au niveau du futur fond de fouille, situé entre 3 et 4 m de profondeur ;\n    • au droit des futurs espaces verts, entre 0 et 1 m de profondeur :\n        ◦ des anomalies en arsenic, cadmium et cuivre supérieures au bruit de fond géochimique dans le cas des sols ordinaires au droit des sondages S5 et S6 ;\n        ◦ deux anomalies en nickel supérieures à la concentration régionale au droit des sondages S5 et S6 ;\n        ◦ une teneur significative en HAP (52 mg/kg) au droit de S5.\n\n    • Investigations sur les gaz de sol :\n\nTrois piézairs ont été implantés dans l’emprise de l’ancienne installation exploitée par la société GIBERT FRÈRES, au droit du futur sous-sol, de manière à contrôler le dégazage des sols. Deux piézairs (Pa1 et Pa2) ont été implantés dans la zone potentiellement la plus impactée, à savoir la zone des cuves enterrées, et le troisième pézair (Pa3) a été implanté en dehors de la zone de suspicion de pollution.\n\nSeul le Pa3 a pu faire l’objet d’un prélèvement de gaz de sol, les deux piézairs implantés dans la zone potentiellement la plus impactée présentant des niveaux d’eau respectifs de 2,36 m dans le Pa1 et de 2,11 m dans le Pa2.\n\nLes paramètres recherchés ont été les Total Petroleum Hydrocarbons (TPH), BTEX, naphtalène et mercure.\n\nLes résultats obtenus au niveau de Pa3 ont mis en évidence l’absence d’anomalie et le bureau d’études TESORA conclut qu’au vu de l’absence d’impact significatif mesuré dans les gaz de sols, aucun dégazage de composé volatil n’est susceptible d’engendrer un excès de risque pour les futurs usagers dans cette zone. Néanmoins, elle relève également qu’aucune mesure de gaz du sol n’ayant pu être effectuée dans la zone potentiellement polluée (zone des cuves), aucune indication concernant le potentiel dégazage des sols n’a pu être recueilli dans cette zone, zone dans laquelle la pollution est la plus probable.\n\n    • Schéma conceptuel :\n\nLe rapport comporte un schéma conceptuel dont les caractéristiques sont les suivantes :\n    • sources potentielles de pollution : la source concentrée en HCT et la teneur significative en arsenic ;\n    • milieux de transfert : les sols, les végétaux et l’air ambiant ;\n    • cibles : les enfants en bas-âge, les résidents enfants et adultes ;\n    • voies d’exposition : ingestion de sol et/ou de produits végétaux autoproduits, inhalation de poussières et/ou de substances toxiques volatiles (en raison de l’absence d’information sur le potentiel dégazage des sols au droit de la zone des cuves).\n\n    • Analyse des enjeux sanitaires :\n\nLe bureau d’études TESORA a considéré que l’estimation des risques liés à l’inhalation de poussières et à l’ingestion de végétaux se ferait en estimant les risques liés à l’ingestion de sol.\n\nL’analyse des risques par ingestion de terres au droit des espaces verts a été effectuée à partir des concentrations maximales mesurées au droit des sondages S6 et T5, sondages présentant les impacts les plus importants en arsenic, cadmium, cuivre, nickel et hydrocarbures.\n\nLe bureau d’études TESORA a justifié de la méthodologie utilisée, en accord avec la méthodologie nationale de gestion des sites et sols pollués d’avril 2017 (choix des valeurs toxicologiques de référence (VTR) retenues, paramètres d’exposition majorants) et a joint les feuilles de calcul correspondant aux sondages S5 et S6.\n\nLes résultats des calculs de risques indiquent, pour les futurs usagers du site qui auront accès aux espaces verts extérieurs, des niveaux de risques sanitaires inacceptables pour la voie d’exposition par ingestion de sol, pour les effets sans seuil. Une mesure de gestion devra être mise en place afin de rendre l’état du site compatible avec l’usage défini.\n\nLe bureau d’études TESORA préconise d’apporter 0,30 m de terre végétale saine au droit des futurs espaces verts ou 1 m de terre saine au droit des futurs espaces potagers afin de permettre de rétablir la compatibilité sanitaire du site.\n\nL’analyse des risques par inhalation de composés volatils dans l’air intérieur a été effectuée à partir des résultats des analyses effectuées sur le piézair Pa3, situé en dehors de la zone potentiellement impactée (la zone des cuves enterrées), et conclut en l’absence d’impact significatif mesuré dans les gaz de sols.\n\nLe bureau d’études TESORA conclut à l’absence de risque sanitaire inacceptable par inhalation de substances toxiques volatiles pour les futurs usagers.\nOr, cette conclusion doit être relativisée compte tenu de l’absence de résultats d’analyses des piézairs localisés sur la zone potentiellement la plus impactée, situé en partie au droit du futur sous-sol et en partie au droit des futurs espaces verts.\n\n    • Mesures de gestion de la pollution identifiée :\n      \nLa version du diagnostic complémentaire, daté du 1er octobre 2019, intègre des mesures de gestion au rapport initialement rédigé au 7 février 2019.\n\nLes mesures de gestion proposées consistent au retrait de toutes les sources de pollution organique et au recouvrement de la zone présentant la teneur en arsenic problématique.\n\n\nCe diagnostic complémentaire permet de :\n    • délimiter les zones impactées en HCT et en HAP, à l’exception de la délimitation verticale des impacts en HCT au niveau de la zone des cuves enterrées ;\n    • justifier de la mise en place de mesures de gestion visant à excaver les sources de pollution en HCT et HAP identifiées et à orienter les terres excavées dans des filières adaptées (Biocentre) ;\n    • justifier de la préconisation :\n        ◦ au niveau de la source concentrée en HCT dont la délimitation verticale n’a pas pu être vérifiée, de la réalisation en fond de fouille de 3 packs HCT et HAP afin de confirmer l’absence de migration de la source concentrée en profondeur dans les argiles vertes et garantir la bonne purge de la source concentrée ;\n        ◦ lors des terrassements des zones polluées, de la réalisation de prélèvements en bords et fonds de fouille afin de vérifier les concentrations résiduelles et s’assurer du retrait total des sources de pollution.\n\nToutefois, l’analyse du rapport établi par le bureau d’études TESORA appelle les remarques suivantes :\n    • aucune information n’est fournie quant au devenir des cuves enterrées inertées et du séparateur à hydrocarbures présents sur l’ancienne emprise de la société GIBERT FRÈRES ;\n    • aucune information n’est fournie quant au devenir de la dalle béton existante sur l’ancienne emprise de la société GIBERT FRÈRES ;\n    • la campagne d’analyse des gaz de sol menée n’a pas permis de caractériser (qualité et concentration) les gaz de sol émis au niveau de la zone des cuves enterrées ;\n    • une estimation des coûts des mesures de gestion proposées n’est pas précisée.","Air","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040031101","Etude SSP et ingénierie des travaux de réhabilitation","2017-01-01",null,"2017 – AIC Envionnement\n\nL’analyse par l’inspection des installations classées des documents fournis par l’exploitant fait apparaître l’existence de deux zones impactées aux hydrocarbures totaux (HCT) et aux hydrocarbures aromatiques polycycliques (HAP), la zone du séparateur d’hydrocarbures et la zone des cuves de stockage des liquides inflammables, qui semblent circonscrites au site et dont seule la voie de transfert par inhalation est retenue.\n\nToutefois, le diagnostic fourni par l’exploitant n’a pas permis à l’inspection des installations classées de vérifier que le site était compatible avec un usage futur du site comparable à celui de la dernière période d’exploitation, l’absence d’impact sanitaire par inhalation n’étant pas suffisamment justifié.","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040031101","Etude SSP et ingénierie des travaux de réhabilitation","2019-10-01",null,"Diagnostic de pollution des sols complémentaires - TESORA \n\nCe diagnostic s’inscrit dans le cadre de la définition des contraintes environnementales du site vis-à-vis de l’aménagement envisagé, à savoir la construction de deux bâtiments de logements sur un niveau de sous-sol communiquant, ainsi que l’aménagement d’espaces verts collectifs. Le périmètre de cet aménagement inclut notamment les parcelles anciennement exploitées par la société GIBERT FRÈRES.\n\nCe diagnostic a été réalisé en complément du diagnostic effectué par la société AIC Environnement fin 2017 et comporte :\n    • des investigations sur les sols ;\n    • des investigations sur les gaz de sols ;\n    • une analyse des enjeux sanitaires ;\n    • des mesures simples de gestion.\n    • Investigations sur les sols :\n\nLes investigations complémentaires ont consisté en la réalisation de 20 sondages de sols, réalisés jusqu’à des profondeurs de 1,5 à 6 m, dont les 14 suivants, réalisés sur l’emprise des anciennes installations exploitées par la société GIBERT FRÈRES :\n    • 11 à proximité des zones de cuves enterrées de liquides inflammables (2 sondages ont subis plusieurs refus ce qui a limité la profondeur de ceux-ci respectivement à 2 m et à 1 m) ;\n    • 1 à proximité de l’aire de lavage de véhicule ;\n    • 1 à proximité de la fosse à charbon ;\n    • 1 à proximité du stockage de bois de chauffage.\n\nLes résultats des analyses de ces sondages, couplés avec ceux obtenus par la société AIC ENVIRONNEMENT, ont permis au bureau d’études TESORA de formuler les constats suivants au niveau de l’emprise de l’ancienne société GIBERT FRÈRES :\n\n    • au droit du futur sous-sol :\n        ◦ source en HAP au droit du sondage S5 (source AIC ENVIRONNEMENT), délimitée horizontalement par les sondages T11 et T12, et verticalement jusqu’à 2 m de profondeur ;\n        ◦ source en HAP et HCT au droit des sondages T7 et T8 ;\n        ◦ dépassement ponctuel de la valeur réglementaire en fraction soluble / sulfates pour 25 % des remblais (au niveau du sondage S3) ;\n        ◦ dépassement diffus des valeurs réglementaires en fluorures pour la lithologie argiles vertes (comprise entre 2 et 3 m de profondeur) ;\n\n    • au droit des futurs espaces verts :\n        ◦ source en HCT au droit du sondage S6 (AIC ENVIRONNEMENT) et des sondages T5 et T6, délimitée horizontalement par les sondages T2, T3 et T4, mais non délimitée verticalement (3 m de profondeur pris en compte au regard du changement de lithologie constaté à cette profondeur).\n          \nLes investigations de sols effectuées sur les parcelles autres que celles anciennement exploitées par la société GIBERT FRÈRES ont permis de mettre en évidence :\n    • au droit du futur sous-sol, l’absence d’anomalies en HCT, HAP, composés organo-halogénés volatils (COHV) et Benzène, Toluène, Éthylbenzène et Xylènes (BTEX) au niveau du futur fond de fouille, situé entre 3 et 4 m de profondeur ;\n    • au droit des futurs espaces verts, entre 0 et 1 m de profondeur :\n        ◦ des anomalies en arsenic, cadmium et cuivre supérieures au bruit de fond géochimique dans le cas des sols ordinaires au droit des sondages S5 et S6 ;\n        ◦ deux anomalies en nickel supérieures à la concentration régionale au droit des sondages S5 et S6 ;\n        ◦ une teneur significative en HAP (52 mg/kg) au droit de S5.\n\n    • Investigations sur les gaz de sol :\n\nTrois piézairs ont été implantés dans l’emprise de l’ancienne installation exploitée par la société GIBERT FRÈRES, au droit du futur sous-sol, de manière à contrôler le dégazage des sols. Deux piézairs (Pa1 et Pa2) ont été implantés dans la zone potentiellement la plus impactée, à savoir la zone des cuves enterrées, et le troisième pézair (Pa3) a été implanté en dehors de la zone de suspicion de pollution.\n\nSeul le Pa3 a pu faire l’objet d’un prélèvement de gaz de sol, les deux piézairs implantés dans la zone potentiellement la plus impactée présentant des niveaux d’eau respectifs de 2,36 m dans le Pa1 et de 2,11 m dans le Pa2.\n\nLes paramètres recherchés ont été les Total Petroleum Hydrocarbons (TPH), BTEX, naphtalène et mercure.\n\nLes résultats obtenus au niveau de Pa3 ont mis en évidence l’absence d’anomalie et le bureau d’études TESORA conclut qu’au vu de l’absence d’impact significatif mesuré dans les gaz de sols, aucun dégazage de composé volatil n’est susceptible d’engendrer un excès de risque pour les futurs usagers dans cette zone. Néanmoins, elle relève également qu’aucune mesure de gaz du sol n’ayant pu être effectuée dans la zone potentiellement polluée (zone des cuves), aucune indication concernant le potentiel dégazage des sols n’a pu être recueilli dans cette zone, zone dans laquelle la pollution est la plus probable.\n\n    • Schéma conceptuel :\n\nLe rapport comporte un schéma conceptuel dont les caractéristiques sont les suivantes :\n    • sources potentielles de pollution : la source concentrée en HCT et la teneur significative en arsenic ;\n    • milieux de transfert : les sols, les végétaux et l’air ambiant ;\n    • cibles : les enfants en bas-âge, les résidents enfants et adultes ;\n    • voies d’exposition : ingestion de sol et/ou de produits végétaux autoproduits, inhalation de poussières et/ou de substances toxiques volatiles (en raison de l’absence d’information sur le potentiel dégazage des sols au droit de la zone des cuves).\n\n    • Analyse des enjeux sanitaires :\n\nLe bureau d’études TESORA a considéré que l’estimation des risques liés à l’inhalation de poussières et à l’ingestion de végétaux se ferait en estimant les risques liés à l’ingestion de sol.\n\nL’analyse des risques par ingestion de terres au droit des espaces verts a été effectuée à partir des concentrations maximales mesurées au droit des sondages S6 et T5, sondages présentant les impacts les plus importants en arsenic, cadmium, cuivre, nickel et hydrocarbures.\n\nLe bureau d’études TESORA a justifié de la méthodologie utilisée, en accord avec la méthodologie nationale de gestion des sites et sols pollués d’avril 2017 (choix des valeurs toxicologiques de référence (VTR) retenues, paramètres d’exposition majorants) et a joint les feuilles de calcul correspondant aux sondages S5 et S6.\n\nLes résultats des calculs de risques indiquent, pour les futurs usagers du site qui auront accès aux espaces verts extérieurs, des niveaux de risques sanitaires inacceptables pour la voie d’exposition par ingestion de sol, pour les effets sans seuil. Une mesure de gestion devra être mise en place afin de rendre l’état du site compatible avec l’usage défini.\n\nLe bureau d’études TESORA préconise d’apporter 0,30 m de terre végétale saine au droit des futurs espaces verts ou 1 m de terre saine au droit des futurs espaces potagers afin de permettre de rétablir la compatibilité sanitaire du site.\n\nL’analyse des risques par inhalation de composés volatils dans l’air intérieur a été effectuée à partir des résultats des analyses effectuées sur le piézair Pa3, situé en dehors de la zone potentiellement impactée (la zone des cuves enterrées), et conclut en l’absence d’impact significatif mesuré dans les gaz de sols.\n\nLe bureau d’études TESORA conclut à l’absence de risque sanitaire inacceptable par inhalation de substances toxiques volatiles pour les futurs usagers.\nOr, cette conclusion doit être relativisée compte tenu de l’absence de résultats d’analyses des piézairs localisés sur la zone potentiellement la plus impactée, situé en partie au droit du futur sous-sol et en partie au droit des futurs espaces verts.\n\n    • Mesures de gestion de la pollution identifiée :\n      \nLa version du diagnostic complémentaire, daté du 1er octobre 2019, intègre des mesures de gestion au rapport initialement rédigé au 7 février 2019.\n\nLes mesures de gestion proposées consistent au retrait de toutes les sources de pollution organique et au recouvrement de la zone présentant la teneur en arsenic problématique.\n\n\nCe diagnostic complémentaire permet de :\n    • délimiter les zones impactées en HCT et en HAP, à l’exception de la délimitation verticale des impacts en HCT au niveau de la zone des cuves enterrées ;\n    • justifier de la mise en place de mesures de gestion visant à excaver les sources de pollution en HCT et HAP identifiées et à orienter les terres excavées dans des filières adaptées (Biocentre) ;\n    • justifier de la préconisation :\n        ◦ au niveau de la source concentrée en HCT dont la délimitation verticale n’a pas pu être vérifiée, de la réalisation en fond de fouille de 3 packs HCT et HAP afin de confirmer l’absence de migration de la source concentrée en profondeur dans les argiles vertes et garantir la bonne purge de la source concentrée ;\n        ◦ lors des terrassements des zones polluées, de la réalisation de prélèvements en bords et fonds de fouille afin de vérifier les concentrations résiduelles et s’assurer du retrait total des sources de pollution.\n\nToutefois, l’analyse du rapport établi par le bureau d’études TESORA appelle les remarques suivantes :\n    • aucune information n’est fournie quant au devenir des cuves enterrées inertées et du séparateur à hydrocarbures présents sur l’ancienne emprise de la société GIBERT FRÈRES ;\n    • aucune information n’est fournie quant au devenir de la dalle béton existante sur l’ancienne emprise de la société GIBERT FRÈRES ;\n    • la campagne d’analyse des gaz de sol menée n’a pas permis de caractériser (qualité et concentration) les gaz de sol émis au niveau de la zone des cuves enterrées ;\n    • une estimation des coûts des mesures de gestion proposées n’est pas précisée.","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040031301","Etude SSP et ingénierie des travaux de réhabilitation","2020-07-22",null,"ARR – ICF Environnement\n\nL’ARR (Analyse des risques résiduels) datée du 22/07/2020, prend en compte les résultats des analyses réalisées entre septembre 2018 et mai 2020, dans les gaz du sol. Les scénarios retenus sont :\n    • l’inhalation de substances volatiles, dans l’air intérieur, par des employés travaillant dans des bureaux du site ;\n    • l’inhalation de substances volatiles, dans l’air extérieur, par des employés travaillant dans des bureaux du site ;\n    • l’inhalation de substances volatiles, dans l’air intérieur, par des employés travaillant dans l’un des halls du site ;\n    • l’inhalation de substances volatiles, dans l’air extérieur, par des employés travaillant dans l’un des halls du site .\n\nLes résultats des calculs de risque, indiquent des niveaux de risques sanitaires inférieurs aux seuils de référence.\n\nL’étude conclut au fait que le site est compatible avec l’usage envisagé : bâtiment à usage industriel et ERP.","Air","Analyse des enjeux sanitaires (EQRS, ARR)","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040031301","Etude SSP et ingénierie des travaux de réhabilitation","2020-07-22",null,"ARR – ICF Environnement\n\nL’ARR (Analyse des risques résiduels) datée du 22/07/2020, prend en compte les résultats des analyses réalisées entre septembre 2018 et mai 2020, dans les gaz du sol. Les scénarios retenus sont :\n    • l’inhalation de substances volatiles, dans l’air intérieur, par des employés travaillant dans des bureaux du site ;\n    • l’inhalation de substances volatiles, dans l’air extérieur, par des employés travaillant dans des bureaux du site ;\n    • l’inhalation de substances volatiles, dans l’air intérieur, par des employés travaillant dans l’un des halls du site ;\n    • l’inhalation de substances volatiles, dans l’air extérieur, par des employés travaillant dans l’un des halls du site .\n\nLes résultats des calculs de risque, indiquent des niveaux de risques sanitaires inférieurs aux seuils de référence.\n\nL’étude conclut au fait que le site est compatible avec l’usage envisagé : bâtiment à usage industriel et ERP.","Sol - Sous-sol","Analyse des enjeux sanitaires (EQRS, ARR)","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040031301","Exécution des travaux de réhabilitation","2020-07-01",null,"Rapport de fin de travaux – ICF Environnement\n\nHertel a mandaté ICF Environnement pour le suivi du chantier de dépollution de l’ancien site SPR localisé au 33 quai Marcel Boyer à Ivry-sur-Seine sur les parcelles cadastrales 69p, 70 et 284 de la section OA.\n\nConformément au PCT, les objectifs de dépollution pour les pollutions concentrées en solvants étaient :\n• 0,6 mg/m3 en Trichloroéthylène (TCE) pour la zone 1 « Atelier-fosses d’entretien » soit 400 m3 de\nterres impactées ;\n• 1,5 mg/m3 en Trichloroéthylène (TCE) pour la zone 2 « Stockage peinture hors-sol » soit 1 000 m3\nde terres impactées.\n\n\nPour répondre à ces objectifs, les travaux ci-dessous ont été réalisés :\n• Le dégazage et inertage de la cuve n°11,\n• Le dégazage, inertage et démantèlement de la cuve n°4 puis remblaiement,\n• Le dégazage, inertage et démantèlement des décanteurs n°6, séparateur n°5, ainsi que des fosses\nde lavage puis remblaiement,\n• L’entretien des séparateurs n° 13 et 14\n• Excavation et élimination des terres polluées des zones concentrées 1 et 2, des dalles de bétons\n• Remblaiement des excavations avec matériaux inertes.\n\nLes travaux de terrassement des terres ont été réalisés du 26 mai 2020 au 20 juillet 2020. Le personnel\nd’ICF Environnement est intervenu tout au long des travaux afin d’assurer la conformité des travaux avec le PCT, trier les terres selon le plan de terrassement, assurer l’orientation et la traçabilité des matériaux évacués, et effectuer la réception des travaux.\n\nLes quantités suivantes de matériaux ont été gérées :\n• 1994,36 T de terre polluées ont été évacuées vers la plateforme de tri et regroupement Mymat\n• 1750 T de terres d’apport inertes ont été remblayées\n• 180 T de bétons ont été évacuées vers la plateforme de tri et regroupement Mymat.\n\nDes prélèvements de réception sols et gaz du sols ont été réalisés afin de vérifier la qualité des terres\nrestant en place sur le site.\n\nLes analyses ont permis de constater l’atteinte des objectifs, avec la purge des pollutions concentrées\net la compatibilité sanitaire des terres en place.\n\nA l’issue des travaux présentés dans ce rapport travaux, l’évacuation des matériaux a été tracée et le\nsite est compatible avec le projet prévu.","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP040032801","Etude SSP et ingénierie des travaux de réhabilitation","2008-04-01",null,"Diagnostic environnemental - URS\n\nLe diagnostic environnemental communiqué comprend :\n    • une étude historique et documentaire du site ;\n    • une phase d’investigations, courant mars 2008, consistant en la réalisation de :\n        ◦ 4 sondages de sol, localisés à proximité des sources de pollution, réalisés à 4 m de profondeur (prélèvement de 4 échantillons pour analyse) ;\n        ◦ 4 sondages pour les prélèvements de gaz de sol à 1 m (prélèvement de 3 échantillons pour analyse) ;\n        ◦ un piézomètre réalisé à 10,5 m de profondeur ;\n    • les substances recherchées sont :\n        ◦ BTEX1, MTBE2, Naphtalène dans les gaz de sol ;\n        ◦ HCT3, BTEX et MTBE dans les fonds de sol.\n\nLe diagnostic environnemental conclut à :\n    1. une géologie assez homogène composée d’une couche de remblais reposant sur un horizon sablo-argileux puis sur une formation argileuse ;\n    2. qu’aucun captage d’eau destinée à la consommation humaine n’est présent dans une zone susceptible d’être influencée par la nappe repérée au droit du site ;\n    3. l’absence de contamination dans les échantillons de sol. Cependant, les analyses de gaz de sol ont montré des teneurs significatives en BTEX entre les deux cuves (S2 = concentration de 8,5 mg/m³ et 18,5 mg/m³ de toluène).","Air","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040032801","Etude SSP et ingénierie des travaux de réhabilitation","2008-04-01",null,"Diagnostic environnemental - URS\n\nLe diagnostic environnemental communiqué comprend :\n    • une étude historique et documentaire du site ;\n    • une phase d’investigations, courant mars 2008, consistant en la réalisation de :\n        ◦ 4 sondages de sol, localisés à proximité des sources de pollution, réalisés à 4 m de profondeur (prélèvement de 4 échantillons pour analyse) ;\n        ◦ 4 sondages pour les prélèvements de gaz de sol à 1 m (prélèvement de 3 échantillons pour analyse) ;\n        ◦ un piézomètre réalisé à 10,5 m de profondeur ;\n    • les substances recherchées sont :\n        ◦ BTEX1, MTBE2, Naphtalène dans les gaz de sol ;\n        ◦ HCT3, BTEX et MTBE dans les fonds de sol.\n\nLe diagnostic environnemental conclut à :\n    1. une géologie assez homogène composée d’une couche de remblais reposant sur un horizon sablo-argileux puis sur une formation argileuse ;\n    2. qu’aucun captage d’eau destinée à la consommation humaine n’est présent dans une zone susceptible d’être influencée par la nappe repérée au droit du site ;\n    3. l’absence de contamination dans les échantillons de sol. Cependant, les analyses de gaz de sol ont montré des teneurs significatives en BTEX entre les deux cuves (S2 = concentration de 8,5 mg/m³ et 18,5 mg/m³ de toluène).","Eaux souterraines","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040032801","Etude SSP et ingénierie des travaux de réhabilitation","2009-06-01","2010-05-01","Suivi nappe souterraine Juin 2009 et Mai 2010 – ATI Services\n\nIl ressort de ce suivi que :\n    • sur la partie Nord, il existe un niveau souterrain séparé de la surface par une dalle béton ;\n    • sur la moitié Sud, en contrebas de la partie Nord, la station service repose sur le « terrain naturel » ;\n    • le sondage de reconnaissance implanté entre les deux cuves de la station service a permis de vérifier la présence d’un niveau argileux protégeant les niveaux sous-jacents d’une éventuelle pollution. D’autre part, un impact en hydrocarbures totaux a été mesuré entre 5,2 m et 6,9 m de profondeur dans des terrains correspondants aux sablons des cuves. Cet impact n’est plus mesuré en début d’horizon argileux ;\n    • concernant les eaux de l’unique piézomètre PZ1, aucun indice organoleptique n’a été relevé.","Eaux souterraines","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040032801","Etude SSP et ingénierie des travaux de réhabilitation","2008-04-01",null,"Diagnostic environnemental - URS\n\nLe diagnostic environnemental communiqué comprend :\n    • une étude historique et documentaire du site ;\n    • une phase d’investigations, courant mars 2008, consistant en la réalisation de :\n        ◦ 4 sondages de sol, localisés à proximité des sources de pollution, réalisés à 4 m de profondeur (prélèvement de 4 échantillons pour analyse) ;\n        ◦ 4 sondages pour les prélèvements de gaz de sol à 1 m (prélèvement de 3 échantillons pour analyse) ;\n        ◦ un piézomètre réalisé à 10,5 m de profondeur ;\n    • les substances recherchées sont :\n        ◦ BTEX1, MTBE2, Naphtalène dans les gaz de sol ;\n        ◦ HCT3, BTEX et MTBE dans les fonds de sol.\n\nLe diagnostic environnemental conclut à :\n    1. une géologie assez homogène composée d’une couche de remblais reposant sur un horizon sablo-argileux puis sur une formation argileuse ;\n    2. qu’aucun captage d’eau destinée à la consommation humaine n’est présent dans une zone susceptible d’être influencée par la nappe repérée au droit du site ;\n    3. l’absence de contamination dans les échantillons de sol. Cependant, les analyses de gaz de sol ont montré des teneurs significatives en BTEX entre les deux cuves (S2 = concentration de 8,5 mg/m³ et 18,5 mg/m³ de toluène).","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040032801","Etude SSP et ingénierie des travaux de réhabilitation","2018-09-10",null,"Diagnostic complémentaire réalisé par ATI Service \n\nLa mise à jour de l’étude de sensibilité a mis en évidence :\n    • la présence de sources potentielles de pollution sur la station-service :\n        ◦ cuves, séparateur hydrocarbure, aire de dépotage, puits perdu ;\n    • la première nappe rencontrée au droit du site : nappe des alluvions de la Seine. Compte tenu de l’imperméabilité de l’horizon sus-jacent (argiles), la vulnérabilité de la nappe n’est pas retenue ;\n    • trois captages à usage potentiellement sensible et trois autres à usage non sensible sont recensés en latéral hydraulique du site dans un rayon de 2 km autour du site. Ces captages ne sont pas considérés vulnérables à une pollution venant du site (nappe souterraine non vulnérable au droit du site).\n      \nDe plus, lors de cette étude complémentaire 6 sondages (à une profondeur de 7 m) ont été réalisés au droit des sources potentielles de pollution et à proximité des anciennes investigations afin de délimiter l’extension des impacts déjà mis en évidence. 13 échantillons ont été envoyés au laboratoire pour être analysés.\n          \nLes résultats du diagnostic réalisé par ATI Services sur la station-service ont mis en évidence :\n    • la présence d’un dénivelé d’un 1 m environ au droit de la zone investiguée ;\n    • des remblais hétérogènes de nature sableux, sableux limoneux légèrement graveleux jusqu’à 3 m de profondeur, remblais argileux sableux jusqu’à 4,5 m-6,00 m puis argiles marron et vertes jusqu’à 7 m-7,50 m ;\n    • des indices organoleptiques (odeurs HCT et sols noirâtres) de pollution entre 3,00 m et 6,00 m de profondeur ;\n    • présence d’une zone concentrée en composés organiques volatils (mesures PID) dans les gaz des sols profonds (4,50 m-7,00 m) avec des teneurs allant de 130 à 580 ppm. Les teneurs s’atténuent en surface.\n    • des sols non inertes au sens de l’arrêté du 12 décembre 2014 au droit des sondages S5 (4,50 m-6,00 m), S6 (4,50 m-6,00 m), S6 (6,00 m-7,00 m), S7 (3,50 m-4,50 m) et S7 (4,50 m-6,00 m) ;\n    • des teneurs en C5-C10 (fraction volatile) allant de 17,7 mg/kg à 216 mg/kg au droit des sondages S5 (4,50 m-6,00 m), S6 (4,50 m-6,00 m), S6 (6,00 m-7,00 m), S7 (3,50 m-4,50 m) et S7 (4,50 m-6,00 m) ;\n    • l’absence de quantification en hydrocarbures C5-C10, hydrocarbures C10-C40 et BTEX au niveau de S2 et S3 ;\n    • des traces en composés volatils HCT C5-C10 et xylène au droit de S4 à 4,50 m-6,00 m de profondeur.\n\nUne zone concentrée en HCT, BTEX et composés organiques volatils est décelée au droit des sondages S1 (sondage ATI Services en mai 2010), S6, S7. Les polluants semblent prendre source en profondeur (entre 3,50 m-4,50 m et 6 m-7 m) dans l’horizon limoneux sableux ou sableux argileux puis être étalés latéralement sur le toit des argiles suivant des chemins préférentiels (en fonction de la perméabilité des sols).\n\nCompte tenu de la présence d’impact dans les sols, ATI Services préconise :\n    • de réaliser des prélèvements de gaz des sols et un prélèvement d’air ambiant dans le local de stockage contigu à la station-service ;\n    • de réaliser un contrôle de l’état des bords et fond de fouille en cas d’excavation des installations pétrolières ;\n    • d’évacuer les terres impactées, avérées lors de ce diagnostic, entre 3,50 m et 7,00 m vers une filière agréée (biocentre ou ISDND) ;\n    • une analyse quantitative des risques sanitaires, si besoin (selon les teneurs résiduelles du site), pour vérifier la compatibilité du site avec l’usage fixé.","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040032801","Exécution des travaux de réhabilitation","2019-05-13",null,"Rapport de fin de travaux –  Soléo Services\n\nD’après le rapport de fin de travaux, les travaux réalisés ont été les suivants :\n    • démantèlement de la station service ;\n    • retrait de la dalle de béton en surface ;\n    • extraction du séparateur à hydrocarbure et de la zone de dépotage ;\n    • retrait des 2 cuves et des canalisations associées ;\n    • élimination des bétons issus du dallage et des installations ;\n    • pompage du mélange eau + hydrocarbure contenu dans l’ancien séparateur découvert ;\n    • prélèvement de matériaux en bord de fouille ;\n    • transport et élimination des terres, des bétons et des cuves vers des filières agréées ;\n    • remblai de la fouille ;\n    • réfection partielle des revêtements de surface.\n\nLes travaux ont généré :\n    • 238,55 tonnes de terres polluées éliminées en biocentre chez SUEZ à Villeparisis (77) ;\n    • 23,28 tonnes de graves polluées et d’enrobés en ISDD éliminés chez EMTA à Guitrancourt (78) ;\n    • 3,9 tonnes d’eaux et de boues hydrocarburées éliminées chez SONOLUB (27).\n\nDe plus, lors de l’inspection, le représentant de l’exploitant a précisé à l’inspection des installations classées que :\n    • les travaux sur site se sont déroulés entre novembre 2018 et février 2019 suite à la cessation totale d’activité survenue le 10 novembre 2018 ;\n    • les cuves ont été dégazées par la société Tokheim et retirées. Elles ont été éliminées par la société Derichebourg Environnement. Les justificatifs d’intervention ont été transmis ;\n    • des HCT C10-C40, à des teneurs allant jusqu’à 3 900 mg/kg, ont été identifiés en un point situé en limite de site, au niveau des cuves, à 5 m de profondeur. 9 autres sondages réalisés sur le site, suite aux travaux, n’ont  pas permis de révéler d’impact significatif en hydrocarbures. Cependant, il y a une pollution au niveau des cuves mais l’exploitant a été bloqué par une incapacité technique ;\n    • 261,83 tonnes de terres ont été excavées et évacuées vers les biocentres de Villeparisis et Écharcon ainsi que vers la filière ISDD de EMTA à Guyancourt, pour traitement.\n\nLes terres, se situant au-dessus des radiers, sur lesquelles reposaient les cuves, ont été évacuées. Cependant, ces radiers étaient situés en limites techniques (canalisations de gaz, câbles, fondation du centre commercial …) et n’ont pas pu être retirés.","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution"]
["SSP040034201","Etude SSP et ingénierie des travaux de réhabilitation","2007-03-13",null,"Diagnostic - Société LISEC ref LN001207 DI du 13/03/07.\n\nCe rapport audit la zone des cuves de la distribution et de la piste. Concernant la zone de la cuve de 5 m3, celle-ci a été contrôlée lors des investigations ANTEA pour le compte du Haut Val de Marne Développement.\n\nCes différentes investigations montrent l’absence d’impact environnemental lié à l’activité de l’ancienne station service ELF.",null,"Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040035601","Etude SSP et ingénierie des travaux de réhabilitation","2019-01-01",null,"    • Sur la base des nouveaux résultats obtenus, la délimitation de la source de pollution concentrée retenue correspond à une surface d’environ 3500 m² (dont la délimitation en direction du nord-ouest, sous la rotonde, présente des incertitudes) de sol. \n      Sur la base des indices organoleptiques de terrain, deux zones peuvent être distinguées au sein de la source de pollution concentrée :\n        ◦ une zone autour du distributeur de secours, au nord, représentant une surface d’environ 100 m² ; la concentration maximale est de 10900 mg/kg entre 2 et 3 m de profondeur ;\n        ◦ une zone au droit de l’ancienne station-service, représentant une surface d’environ 3400 m². La présence de phase flottante a été observée au droit de deux ouvrages dans cette zone : PzE (jusqu’à 90 cm) et PzD (jusqu’à 8 cm). Les concentrations maximales ont été mesurées au droit du sondage NS6 (à proximité de PzE) entre 3 et 4 m de profondeur avec 20000 mg/kg, au droit du sondage GA-1 entre 1 et 2 m de profondeur avec 12000 mg/kg et autour de l’ancienne zone de dépotage entre 0,5 et 4 m de profondeur (13000 à 17000 mg/kg). »\n\n    • Mise à jour du plan de gestion :\n        ◦ Plan de gestion initial : « Les diagnostics environnementaux menés jusqu’en 2015 indiquaient un impact des sols et de la zone de battement (jusqu’à 3-4m) – le volume de terres présentant des concentrations supérieures à 2500 mg/kg en hydrocarbures totaux était estimée à environ 4120 m³.\n          L’analyse DU bilan coût-avantage avait conduit la SNCF à retenir un traitement de la zone source par méthode in-situ sur la base d’objectifs de réhabilitation d’une concentration de 3500 mg/kg en HCT et une diminution de 80% sur les fractions volatiles C12-C16.\n           En vue de mettre en œuvre le traitement in-situ une étude de faisabilité a été réalisée en 2017 par Golder – lors de cette étude, le volume de terres impactées présentant des concentrations supérieures à 2500 mg/kg a été estimé à entre 10000 et 13000 m3 soit environ 3 fois plus que lors des évaluations initiales (ces différentes estimations peuvent provenir par exemple du nombres de sondages utilisés pour la construction des isoconcentration, des profondeurs des sondages et donc des échantillons).\n          Cette modification importante des volumes impactés a amené la SNCF à remettre à plat les données du site pour réaliser une mise à jour du plan de gestion, objet de ce rapport ».\n\n        ◦ Mise à jour du plan de gestion :\n            ▪ seuil de coupure défini à 5000 mg/kg pour HCT C10-C40, 85,6 % de la masse de ce polluant dans les sols sera traitée pour 27 % du volume de sol impacté localisé dans les anciennes zones de distribution et les voies 21, 22 et 42 ;\n            ▪ volumes de terres impactées par des concentrations en HCT > 2500 mg/kg de MS estimés par ARTELIA entre 7000 et 9000 m³ ;\n            ▪ estimation de la masse en HCT C10-C40 en kg majoritairement comprise entre 2 et 4 m de profondeur dans les sols (61619 kg entre 2 et 3 m + 45927 kg entre 3 et 4 m) + masse importante (73600 kg) estimée dans la phase flottante (totale masse estimée à 203 345 kg) ;\n            ▪ « Étant donnée les informations obtenues à ce jour et la définition des pollutions concentrées dans le cadre de cette étude, les zones sources à traiter impliqueront donc la mise en place d’une solution de traitement qui permettra la réduction des concentrations en hydrocarbures dans les ‘milieux’ suivants :\n                • Phase flottante (environ 76000 kg d’hydrocarbures C10-C40 – produit pur qu’il convient de traiter en premier) afin d’envisager la mise en place de traitement efficace des zones non-saturées et saturées (listées ci-dessous) ;\n                • Zone non-saturée (sols) => entre 0 et environ 2,5m sur environ 3500 m2 ;\n                • Zone saturée (sols et indirectement la phase dissoute):\n                    ◦ Zone de battement de la nappe entre 2,5 et 3,5m ;\n                    ◦ Partie supérieure de la zone saturée entre environ 3,5 et 5 à 6m de profondeur (sur la base des informations obtenues sur les piézomètres PzF, PzG et PzH et la présence de fortes concentrations mesurées entre 3 et 4m) ».\n            ▪ Techniques envisageables : \n                • excavation : totale ou partielle ;\n                • traitement in-situ (biologique ou chimique) ;\n                • pompage/écrémage/traitement.\n            ▪ « Étant donné les contraintes du site, la solution impliquera la mise en place de différentes techniques listées ci-dessus. Le choix de la solution la plus adaptée dépendra de la mise en place de pilote sur site et des résultats obtenus. La réalisation d'essais pilote sur le site, dans le cadre d’un Plan de Conception des Travaux, permettra ainsi de définir la ou les techniques de traitement les plus adaptés à mettre en place sur le site et de consolider les coûts associés au traitement de la zone impactée. »\n            ▪ Évaluation des avantages et inconvénients des scénarios de réhabilitation envisageables :\n                • scénario 1 : traitement in-situ seul par phase : sur la base d’une efficacité estimée de l’ordre de 60 à 85 %, ce scénario permettrait de traiter environ 120 000 et 170 000 kg d’HCT totaux (soit environ 65 et 90 % de la masse d’HCT à traiter). Coût (hors coût de MOe, hors coût de redevance de rejet au réseau des eaux traitées et hors coût de mise en place d’un blindage ou de caisson pour la construction de la tranchée drainante) estimé entre 730000 et 1125000 € HT ;\n                  \n                • Scénario 2 (2 et 2 bis) : excavation sous caisson sur une surface limitée + traitement in-situ : \n                    ◦ scenario 2 : excavation sur surface limitée à 675 m² jusqu’ à 4 – 5 m de profondeur (volume de terres à excaver compris entre 2700 et 3375 m³ soit environ 49000 kg soit environ 35 % de la masse à traiter dans les sols) + traitement de la zone restante par mise en place d’un traitement in-situ (efficacité estimée de l’ordre de 60 à 85 %) = traitement d’environ 140000 et 180000 kg d’HCT totaux soit entre environ 68 et 88 % de la masse totale d’HCT. Coût (hors coût de MOe, hors coût de pompage et traitement des eaux en fond de fouille) estimé entre 1046200 et 1436500 € HT ;\n                    ◦ scenario 2bis : excavation sur surface limitée à 675 m² jusqu’ à 2,5 à 3 m de profondeur (volume de terres à excaver compris entre 1500 et 2100 m³ soit environ 42000 kg soit environ 30 % de la masse à traiter dans les sols) + traitement de la zone restante par mise en place d’un traitement in-situ (efficacité estimée de l’ordre de 60 à 85 %) = traitement d’environ 135000 et 173000 kg d’HCT totaux soit entre environ 66 et 85 % de la masse totale d’HCT. Coût (hors coût de MOe, hors coût de pompage et traitement des eaux en fond de fouille) estimé entre 659000 et 1037600 € HT ;\n                      \n                • Scénario 3 : Excavation avec blindage partiel incluant la dépose/repose de la voie 42 + traitement in-situ : excavation sur surface pouvant atteindre 1200 m² sur profondeur pouvant atteindre environ 5 m (volume de terres à excaver estimé à entre 3525 et 4100 m³ soit environ 52000 kg soit environ 40 % masse à traiter dans les sols) + traitement de la zone restante par mise en place d’un traitement in-situ (efficacité estimée de l’ordre de 60 à 85 %) = traitement d’environ 155000 et 190000 kg d’HCT totaux soit entre environ 76 et 93 % de la masse totale d’HCT. Coût (hors coût de MOe, hors coût de pompage et traitement des eaux en fond de fouille) estimé entre 1054900 et 1429600 € HT.\n\n                • Le bilan des scénarii aboutit aux notes globales suivantes : S1 : 58,5, S2 : 54, S2bis : 64,5 et S3 : 50 ; S1 et S2bis seraient les pus adaptés.\n                  Cependant, des études complémentaires sont nécessaires afin de lever les incertitudes, affiner chacun des scenarii et sélectionner la solution de traitement la plus pertinente pour la zone d’étude. Une MAJ de ces 3 scenarii devra être effectuée en fonction des résultats obtenus lors de ces études complémentaires.","Eaux souterraines","Plan de gestion","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040035601","Etude SSP et ingénierie des travaux de réhabilitation","2018-03-29",null,"Etude de faisabilité – GOLDER ASSOCIATES\n\nConcernant les travaux de réhabilitation, un diagnostic de traitement de faisabilité in situ a été établi par la société GOLDER ASSOCIATES le 29 mars 2018. Ce rapport indique :\n    • la réalisation d’investigations complémentaires en mars 2017 : 7 sondages de sols (GA1 à GA7) à la tarière à 4 m de profondeur sauf pour GA6 (5 m), 2 sondages au carottier (BH1 et BH2) à 4 m de profondeur, 2 piézomètres (PZD et PZE) à 7 m de profondeur et 4 piézairs à 3 m de profondeur ;\n      \n    • une bonne délimitation horizontale de la zone de pollution notamment au Sud et au NE, cependant délimitation de la pollution reste à approfondir à proximité et sous la rotonde (2 sondages, GA1 et GA2, réalisés au NO du site à proximité de la rotonde présentent encore de teneurs de l’ordre de 12 000 mg/kg MS en HCT C10-C40. Volume de terres polluées (concentration en HCT > 2500 mg/kg MS) estimé entre 10 000 et 13 000 m³ hors volume sous rotonde ;\n      \n    • présence de flottant au niveau des piézomètres PZD et PZE (0,7 m de flottant au niveau de PZE et 0,08 m au niveau de PZD). Caractérisation du flottant effectué au niveau de PZE : majorité de C7-C32 correspondant à un mélange de diesel ou fioul domestique de plus de 20 ans.","Eaux souterraines","Essais de faisabilité et de traitabilité","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040035601","Etude SSP et ingénierie des travaux de réhabilitation","2019-01-01",null,"    • Sur la base des nouveaux résultats obtenus, la délimitation de la source de pollution concentrée retenue correspond à une surface d’environ 3500 m² (dont la délimitation en direction du nord-ouest, sous la rotonde, présente des incertitudes) de sol. \n      Sur la base des indices organoleptiques de terrain, deux zones peuvent être distinguées au sein de la source de pollution concentrée :\n        ◦ une zone autour du distributeur de secours, au nord, représentant une surface d’environ 100 m² ; la concentration maximale est de 10900 mg/kg entre 2 et 3 m de profondeur ;\n        ◦ une zone au droit de l’ancienne station-service, représentant une surface d’environ 3400 m². La présence de phase flottante a été observée au droit de deux ouvrages dans cette zone : PzE (jusqu’à 90 cm) et PzD (jusqu’à 8 cm). Les concentrations maximales ont été mesurées au droit du sondage NS6 (à proximité de PzE) entre 3 et 4 m de profondeur avec 20000 mg/kg, au droit du sondage GA-1 entre 1 et 2 m de profondeur avec 12000 mg/kg et autour de l’ancienne zone de dépotage entre 0,5 et 4 m de profondeur (13000 à 17000 mg/kg). »\n\n    • Mise à jour du plan de gestion :\n        ◦ Plan de gestion initial : « Les diagnostics environnementaux menés jusqu’en 2015 indiquaient un impact des sols et de la zone de battement (jusqu’à 3-4m) – le volume de terres présentant des concentrations supérieures à 2500 mg/kg en hydrocarbures totaux était estimée à environ 4120 m³.\n          L’analyse DU bilan coût-avantage avait conduit la SNCF à retenir un traitement de la zone source par méthode in-situ sur la base d’objectifs de réhabilitation d’une concentration de 3500 mg/kg en HCT et une diminution de 80% sur les fractions volatiles C12-C16.\n           En vue de mettre en œuvre le traitement in-situ une étude de faisabilité a été réalisée en 2017 par Golder – lors de cette étude, le volume de terres impactées présentant des concentrations supérieures à 2500 mg/kg a été estimé à entre 10000 et 13000 m3 soit environ 3 fois plus que lors des évaluations initiales (ces différentes estimations peuvent provenir par exemple du nombres de sondages utilisés pour la construction des isoconcentration, des profondeurs des sondages et donc des échantillons).\n          Cette modification importante des volumes impactés a amené la SNCF à remettre à plat les données du site pour réaliser une mise à jour du plan de gestion, objet de ce rapport ».\n\n        ◦ Mise à jour du plan de gestion :\n            ▪ seuil de coupure défini à 5000 mg/kg pour HCT C10-C40, 85,6 % de la masse de ce polluant dans les sols sera traitée pour 27 % du volume de sol impacté localisé dans les anciennes zones de distribution et les voies 21, 22 et 42 ;\n            ▪ volumes de terres impactées par des concentrations en HCT > 2500 mg/kg de MS estimés par ARTELIA entre 7000 et 9000 m³ ;\n            ▪ estimation de la masse en HCT C10-C40 en kg majoritairement comprise entre 2 et 4 m de profondeur dans les sols (61619 kg entre 2 et 3 m + 45927 kg entre 3 et 4 m) + masse importante (73600 kg) estimée dans la phase flottante (totale masse estimée à 203 345 kg) ;\n            ▪ « Étant donnée les informations obtenues à ce jour et la définition des pollutions concentrées dans le cadre de cette étude, les zones sources à traiter impliqueront donc la mise en place d’une solution de traitement qui permettra la réduction des concentrations en hydrocarbures dans les ‘milieux’ suivants :\n                • Phase flottante (environ 76000 kg d’hydrocarbures C10-C40 – produit pur qu’il convient de traiter en premier) afin d’envisager la mise en place de traitement efficace des zones non-saturées et saturées (listées ci-dessous) ;\n                • Zone non-saturée (sols) => entre 0 et environ 2,5m sur environ 3500 m2 ;\n                • Zone saturée (sols et indirectement la phase dissoute):\n                    ◦ Zone de battement de la nappe entre 2,5 et 3,5m ;\n                    ◦ Partie supérieure de la zone saturée entre environ 3,5 et 5 à 6m de profondeur (sur la base des informations obtenues sur les piézomètres PzF, PzG et PzH et la présence de fortes concentrations mesurées entre 3 et 4m) ».\n            ▪ Techniques envisageables : \n                • excavation : totale ou partielle ;\n                • traitement in-situ (biologique ou chimique) ;\n                • pompage/écrémage/traitement.\n            ▪ « Étant donné les contraintes du site, la solution impliquera la mise en place de différentes techniques listées ci-dessus. Le choix de la solution la plus adaptée dépendra de la mise en place de pilote sur site et des résultats obtenus. La réalisation d'essais pilote sur le site, dans le cadre d’un Plan de Conception des Travaux, permettra ainsi de définir la ou les techniques de traitement les plus adaptés à mettre en place sur le site et de consolider les coûts associés au traitement de la zone impactée. »\n            ▪ Évaluation des avantages et inconvénients des scénarios de réhabilitation envisageables :\n                • scénario 1 : traitement in-situ seul par phase : sur la base d’une efficacité estimée de l’ordre de 60 à 85 %, ce scénario permettrait de traiter environ 120 000 et 170 000 kg d’HCT totaux (soit environ 65 et 90 % de la masse d’HCT à traiter). Coût (hors coût de MOe, hors coût de redevance de rejet au réseau des eaux traitées et hors coût de mise en place d’un blindage ou de caisson pour la construction de la tranchée drainante) estimé entre 730000 et 1125000 € HT ;\n                  \n                • Scénario 2 (2 et 2 bis) : excavation sous caisson sur une surface limitée + traitement in-situ : \n                    ◦ scenario 2 : excavation sur surface limitée à 675 m² jusqu’ à 4 – 5 m de profondeur (volume de terres à excaver compris entre 2700 et 3375 m³ soit environ 49000 kg soit environ 35 % de la masse à traiter dans les sols) + traitement de la zone restante par mise en place d’un traitement in-situ (efficacité estimée de l’ordre de 60 à 85 %) = traitement d’environ 140000 et 180000 kg d’HCT totaux soit entre environ 68 et 88 % de la masse totale d’HCT. Coût (hors coût de MOe, hors coût de pompage et traitement des eaux en fond de fouille) estimé entre 1046200 et 1436500 € HT ;\n                    ◦ scenario 2bis : excavation sur surface limitée à 675 m² jusqu’ à 2,5 à 3 m de profondeur (volume de terres à excaver compris entre 1500 et 2100 m³ soit environ 42000 kg soit environ 30 % de la masse à traiter dans les sols) + traitement de la zone restante par mise en place d’un traitement in-situ (efficacité estimée de l’ordre de 60 à 85 %) = traitement d’environ 135000 et 173000 kg d’HCT totaux soit entre environ 66 et 85 % de la masse totale d’HCT. Coût (hors coût de MOe, hors coût de pompage et traitement des eaux en fond de fouille) estimé entre 659000 et 1037600 € HT ;\n                      \n                • Scénario 3 : Excavation avec blindage partiel incluant la dépose/repose de la voie 42 + traitement in-situ : excavation sur surface pouvant atteindre 1200 m² sur profondeur pouvant atteindre environ 5 m (volume de terres à excaver estimé à entre 3525 et 4100 m³ soit environ 52000 kg soit environ 40 % masse à traiter dans les sols) + traitement de la zone restante par mise en place d’un traitement in-situ (efficacité estimée de l’ordre de 60 à 85 %) = traitement d’environ 155000 et 190000 kg d’HCT totaux soit entre environ 76 et 93 % de la masse totale d’HCT. Coût (hors coût de MOe, hors coût de pompage et traitement des eaux en fond de fouille) estimé entre 1054900 et 1429600 € HT.\n\n                • Le bilan des scénarii aboutit aux notes globales suivantes : S1 : 58,5, S2 : 54, S2bis : 64,5 et S3 : 50 ; S1 et S2bis seraient les pus adaptés.\n                  Cependant, des études complémentaires sont nécessaires afin de lever les incertitudes, affiner chacun des scenarii et sélectionner la solution de traitement la plus pertinente pour la zone d’étude. Une MAJ de ces 3 scenarii devra être effectuée en fonction des résultats obtenus lors de ces études complémentaires.","Sol - Sous-sol","Plan de gestion","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040035601","Etude SSP et ingénierie des travaux de réhabilitation","2018-03-29",null,"Etude de faisabilité – GOLDER ASSOCIATES\n\nConcernant les travaux de réhabilitation, un diagnostic de traitement de faisabilité in situ a été établi par la société GOLDER ASSOCIATES le 29 mars 2018. Ce rapport indique :\n    • la réalisation d’investigations complémentaires en mars 2017 : 7 sondages de sols (GA1 à GA7) à la tarière à 4 m de profondeur sauf pour GA6 (5 m), 2 sondages au carottier (BH1 et BH2) à 4 m de profondeur, 2 piézomètres (PZD et PZE) à 7 m de profondeur et 4 piézairs à 3 m de profondeur ;\n      \n    • une bonne délimitation horizontale de la zone de pollution notamment au Sud et au NE, cependant délimitation de la pollution reste à approfondir à proximité et sous la rotonde (2 sondages, GA1 et GA2, réalisés au NO du site à proximité de la rotonde présentent encore de teneurs de l’ordre de 12 000 mg/kg MS en HCT C10-C40. Volume de terres polluées (concentration en HCT > 2500 mg/kg MS) estimé entre 10 000 et 13 000 m³ hors volume sous rotonde ;\n      \n    • présence de flottant au niveau des piézomètres PZD et PZE (0,7 m de flottant au niveau de PZE et 0,08 m au niveau de PZD). Caractérisation du flottant effectué au niveau de PZE : majorité de C7-C32 correspondant à un mélange de diesel ou fioul domestique de plus de 20 ans.","Sol - Sous-sol","Essais de faisabilité et de traitabilité","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040044301","Etude SSP et ingénierie des travaux de réhabilitation","2019-04-16",null,"Diagnostic de l’état des milieux - BURGEAP\n\nDe nombreuses installations/stockages potentiellement polluants ont été identifiés à l’issue de l’étude historique et documentaire et de la visite du site. Ces dernières ont fait l’objet d’investigations, qui ont montré :\n- sur le milieu sol :\n    • présence de métaux et métalloïdes, notamment chrome, nickel et plomb, en concentrations 5 à 65 fois supérieures à celles du bruit de fond d’Ile-de-France au droit des sondages S1, S3, S5 et Pza3, de la surface à 1 à 3 m de profondeur ;\n    • Présence d’un impact ponctuel en hydrocarbures lourds (C16-C40), en concentration de 4 610 mg/kg, au droit du sondage S9 (compresseur en sous-sol). Cet impact n’a pas été délimité en profondeur ;\n\n- sur le milieu eaux souterraines : impact en PCE au droit du site ;\n\n- sur le milieu gaz des sols :\n    • SD1 (compresseur en sous-sol) : impact en HCT, BTEX, TCE ;\n    • Pza3 (piézomètre PZ1) : impact en TCE.\n\nLes teneurs ainsi calculées à partir de la teneur maximale mesurée sur les échantillons d’air sous dalle (SD1) et des gaz du sol (Pza3) :\n• \tDans le sous-sol, sont inférieures aux valeurs de comparaison quand elles existent, à l’exception de la teneur en benzène. Notons toutefois que la teneur calculée est de l’ordre, voire légèrement supérieure aux valeurs guides mais inférieure aux valeurs de bruit de fond pour les bureaux et les garages ;\n• \tdu rez-de-chaussée sont toutes inférieures aux valeurs de comparaison quand elles existent.\n\nLe rapport indique les recommandations suivantes : \n- Au vu de la présence généralisée de PCE dans les eaux souterraines présentes au droit du site nous recommandons de poursuivre le suivi de la qualité chimique des eaux souterraines au droit des trois piézomètres mis en place lors de ces investigations ;\n- En cas de changement d’usage une étude type Plan de Gestion (PG) avec Analyse des Risques Résiduels (ARR) devra être engagée afin de confirmer la compatibilité sanitaire du site avec l’usage prévu.","Air","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040044301","Etude SSP et ingénierie des travaux de réhabilitation","2019-04-16",null,"Diagnostic de l’état des milieux - BURGEAP\n\nDe nombreuses installations/stockages potentiellement polluants ont été identifiés à l’issue de l’étude historique et documentaire et de la visite du site. Ces dernières ont fait l’objet d’investigations, qui ont montré :\n- sur le milieu sol :\n    • présence de métaux et métalloïdes, notamment chrome, nickel et plomb, en concentrations 5 à 65 fois supérieures à celles du bruit de fond d’Ile-de-France au droit des sondages S1, S3, S5 et Pza3, de la surface à 1 à 3 m de profondeur ;\n    • Présence d’un impact ponctuel en hydrocarbures lourds (C16-C40), en concentration de 4 610 mg/kg, au droit du sondage S9 (compresseur en sous-sol). Cet impact n’a pas été délimité en profondeur ;\n\n- sur le milieu eaux souterraines : impact en PCE au droit du site ;\n\n- sur le milieu gaz des sols :\n    • SD1 (compresseur en sous-sol) : impact en HCT, BTEX, TCE ;\n    • Pza3 (piézomètre PZ1) : impact en TCE.\n\nLes teneurs ainsi calculées à partir de la teneur maximale mesurée sur les échantillons d’air sous dalle (SD1) et des gaz du sol (Pza3) :\n• \tDans le sous-sol, sont inférieures aux valeurs de comparaison quand elles existent, à l’exception de la teneur en benzène. Notons toutefois que la teneur calculée est de l’ordre, voire légèrement supérieure aux valeurs guides mais inférieure aux valeurs de bruit de fond pour les bureaux et les garages ;\n• \tdu rez-de-chaussée sont toutes inférieures aux valeurs de comparaison quand elles existent.\n\nLe rapport indique les recommandations suivantes : \n- Au vu de la présence généralisée de PCE dans les eaux souterraines présentes au droit du site nous recommandons de poursuivre le suivi de la qualité chimique des eaux souterraines au droit des trois piézomètres mis en place lors de ces investigations ;\n- En cas de changement d’usage une étude type Plan de Gestion (PG) avec Analyse des Risques Résiduels (ARR) devra être engagée afin de confirmer la compatibilité sanitaire du site avec l’usage prévu.","Eaux souterraines","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040044301","Etude SSP et ingénierie des travaux de réhabilitation","2019-04-16",null,"Diagnostic de l’état des milieux - BURGEAP\n\nDe nombreuses installations/stockages potentiellement polluants ont été identifiés à l’issue de l’étude historique et documentaire et de la visite du site. Ces dernières ont fait l’objet d’investigations, qui ont montré :\n- sur le milieu sol :\n    • présence de métaux et métalloïdes, notamment chrome, nickel et plomb, en concentrations 5 à 65 fois supérieures à celles du bruit de fond d’Ile-de-France au droit des sondages S1, S3, S5 et Pza3, de la surface à 1 à 3 m de profondeur ;\n    • Présence d’un impact ponctuel en hydrocarbures lourds (C16-C40), en concentration de 4 610 mg/kg, au droit du sondage S9 (compresseur en sous-sol). Cet impact n’a pas été délimité en profondeur ;\n\n- sur le milieu eaux souterraines : impact en PCE au droit du site ;\n\n- sur le milieu gaz des sols :\n    • SD1 (compresseur en sous-sol) : impact en HCT, BTEX, TCE ;\n    • Pza3 (piézomètre PZ1) : impact en TCE.\n\nLes teneurs ainsi calculées à partir de la teneur maximale mesurée sur les échantillons d’air sous dalle (SD1) et des gaz du sol (Pza3) :\n• \tDans le sous-sol, sont inférieures aux valeurs de comparaison quand elles existent, à l’exception de la teneur en benzène. Notons toutefois que la teneur calculée est de l’ordre, voire légèrement supérieure aux valeurs guides mais inférieure aux valeurs de bruit de fond pour les bureaux et les garages ;\n• \tdu rez-de-chaussée sont toutes inférieures aux valeurs de comparaison quand elles existent.\n\nLe rapport indique les recommandations suivantes : \n- Au vu de la présence généralisée de PCE dans les eaux souterraines présentes au droit du site nous recommandons de poursuivre le suivi de la qualité chimique des eaux souterraines au droit des trois piézomètres mis en place lors de ces investigations ;\n- En cas de changement d’usage une étude type Plan de Gestion (PG) avec Analyse des Risques Résiduels (ARR) devra être engagée afin de confirmer la compatibilité sanitaire du site avec l’usage prévu.","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040048801","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"Étude du sous-sol y compris des gaz.",null,"Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040049001","Exécution des travaux de réhabilitation",null,null,"dégazage des cuves",null,"N/A","N/A","N/A","N/A","Travaux de dépollution"]
["SSP040050001","Exécution des travaux de réhabilitation",null,null,"Dégazage et inertage des cuves","Sol - Sous-sol","N/A","N/A","N/A","N/A","Mise en place de mesure de réhabilitation",null,"N/A","N/A","N/A"]
["SSP040050001","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"Cinq sondages réalisés au droit des cuves",null,"Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040050101","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"Sondage de terrain","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040050101","Exécution des travaux de réhabilitation",null,null,"Neutralisation des risques incendie et d'explosions.",null,"N/A","N/A","N/A","N/A","Mesure de sécurité du site","Interdiction d'accès (clôture...)","N/A","N/A","N/A"]
["SSP040050401","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"Analyses du sol et sous-sol.",null,"Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040058501","Etude SSP et ingénierie des travaux de réhabilitation","2006-12-01",null,"Diagnostic initial de pollution des sols – BURGEAP \n\nLes résultats des analyses ont montré principalement :\n    • sur les métaux : les analyses montrent des concentrations en métaux cohérentes avec les valeurs de fonds géochimiques et même inférieures aux VDSS ;\n    • sur les hydrocarbures totaux : des anomalies localisées en 1 point du site, sur plusieurs profondeurs et telles que :\n        ◦ au droit de la cuve enterrée de récupération des huiles usagées, entre 3 m et  5m : des concentrations comprises entre 6 130 et 7 930 mg/kg de matière sèche. Les valeurs mesurées sont supérieures à la VCI usage sensible (5 000 mg/kg de MS) mais inférieures à la VCI usage non sensible (25 000 mg/kg de MS).\n    • sur les HAP: les concentrations mesurées sont inférieures aux VDSS (teneurs à l’état de traces).\n    • sur les COHV : un point semble impacté par du trichloroéthylène, les valeurs mesurées à moins de 1 m, au droit du stockage des fûts neufs d’huile, à l’intérieur du bâtiment, sont comprises entre 0,11 et 0,16 mg/kg de MS.\n    • Sur les BTEX : pas d’anomalies constatées.\n\nPour conclure et au vu des résultats des analyses des sols réalisées, l’exploitant indique que les sols, globalement, ne présentent pas de pollution, à l’exception des sondages au droit de la cuve enterrée de récupération d’huiles usagées et à proximité de la zone de stockage de fûts d’huiles neufs à l’intérieur du bâtiment.","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040066501","Etude SSP et ingénierie des travaux de réhabilitation","2016-07-07","2016-12-05","5 décembre 2016\nDiagnostic RSK Environnement 704039-R1\n\nLes investigations ont été effectuées le 7 juillet 2016 à l’aide de 5 sondages réalisés entre 1,5 et 5 m de profondeur au droit et à proximité immédiate des anciennes installations de la station-service (cuve, dépotage, volucompteur).\n\n11 échantillons de terres ont été analysés. Le programme analytique a porté sur les hydrocarbures totaux, les hydrocarbures aromatiques polycycliques (HAP) et les BTEX.\n\nAucune arrivée d’eau n’a été constatée lors des sondages.\n\nUne odeur d’hydrocarbures a été constatée au niveau du sondage S1 (entre 1,5 et 2 m) et en S2 (entre 1,4 et 5 m).\n\nLes résultats des analyses ont montré :\n    • Un impact en hydrocarbures totaux en S2-2 (19 000 mg/kg entrre 1,4 et 2 m), S2-3 (1 100 mg/kg entre 2,5 et 3 m), S2-4 (1 100 mg/kg entre 4,5 et 5m). Les concentrations diminuent avec la profondeur ;\n    • Aucun impact en BTEX ;\n    • Un imapct en HAP en S1-2 (150 mg/kg entre 1,5 et 2 m). Ce dépassement est délimité verticalement grâce aux échantillons S1-1 et S1-3.\n\nSelon le bureau d’étude, les impacts en hydrocarbures totaux et en HAP sont liés à la qualité des remblais utilisés pour le comblement de la cavité créée lors du démantèlement de la rétention de la cuve de gasoil.\n\nIl recommande de purger les matériaux impactés, de contrôler la qualité des terres présentes en bords et fond de fouille et de réaliser une ARR si nécessaire.\n\nAucune investigation n’a été réalisée au droit et à proximité de l’ancienne installation de distribution de liquides inflammables composée d’une cuve enterrée de 40 m3 et d’un volucompteur.","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040066801","Etude SSP et ingénierie des travaux de réhabilitation","2007-09-19",null,"Diagnostic de pollution -  L’Atelier d’Ecologie Urbaine\n\nRéalisation de 4 sondages aux alentours de la cuve enterrée et jusqu’à 4 m de profondeur.\n\nLe rapport conclut à une pollution résiduelle au niveau d’un sondage (P1) jusqu’à 0,6 m de profondeur :\n    • HCT : 734 mg/kg ;\n    • HAP : 45 mg/kg dont 41 mg/kg de naphtalène ;\n    • Xylènes : 298 mg/kg.\nLes autres sondages ne sont pas impactés.","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040066801","Etude SSP et ingénierie des travaux de réhabilitation","2018-08-27",null,"Note technique – Cabinet AIC\n\nDes prélèvements sur les bords et fond de fouille ont été réalisés par AIC en juillet 2018. Les résultats des analyses montrent des traces en naphtalène (maximum de 0,42 mg/kg), en xylènes totaux (maximum de 0,06 mg/kg), en HAP (maximum de 1,78 mg/kg) et en hydrocarbures C10-C40 (maximum de 91,8 mg/kg).\nLe cabinet conclut à l’absence de risque sanitaire au vu du projet de parking envisagé.","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040066801","Exécution des travaux de réhabilitation","2018-06-06","2018-07-06","Travaux d’excavation de sols impactés réalisés par D2A Recyval entre le 6 juin et le 6 juillet 2018.\n\n34,38 tonnes de terres excavées et évacuées en biocentre chez BIOGENIE.","Sol - Sous-sol","N/A","N/A","N/A","N/A","Travaux de dépollution",null,"Excavation des sols"]
["SSP040066901","Etude SSP et ingénierie des travaux de réhabilitation","2018-12-21",null,"Diagnostic de l’état du sous-sol – HPC Envirotec\n\nLes investigations ont été effectuées sur le site du 22 au 24 octobre 2018, du 4 au 7 novembre 2018 et le 9 novembre 2018 (échantillonnage des eaux souterraines). Elles ont consisté en la réalisation de 26 sondages de sols de 5 m  de profondeur dont 4 ont été équipés de piézairs temporaires à une profondeur de 2 m. Par ailleurs, 3 piézomètres ont été installés à des profondeurs de 12 à 18 m.\n\nLes résultats de ces premières investigations ont permis d’identifier des secteurs pollués notamment autour des anciennes cuves de stockage de carburants 7, 8 et 9 à proximité de l’aire de lavage. Les résultats d’analyses qui ont conduit à l’identification de zones reconnues impactées sont résumées ci-dessous.","Air","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040066901","Etude SSP et ingénierie des travaux de réhabilitation","2020-07-24",null,"Rapport daté du 24 juillet 2020 réalisé par HPC Envirotec à propos des investigations complémentaires, du plan de gestion et l’analyse ds risques sanitaires résiduels.","Air","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040066901","Etude SSP et ingénierie des travaux de réhabilitation","2018-12-21",null,"Diagnostic de l’état du sous-sol – HPC Envirotec\n\nLes investigations ont été effectuées sur le site du 22 au 24 octobre 2018, du 4 au 7 novembre 2018 et le 9 novembre 2018 (échantillonnage des eaux souterraines). Elles ont consisté en la réalisation de 26 sondages de sols de 5 m  de profondeur dont 4 ont été équipés de piézairs temporaires à une profondeur de 2 m. Par ailleurs, 3 piézomètres ont été installés à des profondeurs de 12 à 18 m.\n\nLes résultats de ces premières investigations ont permis d’identifier des secteurs pollués notamment autour des anciennes cuves de stockage de carburants 7, 8 et 9 à proximité de l’aire de lavage. Les résultats d’analyses qui ont conduit à l’identification de zones reconnues impactées sont résumées ci-dessous.","Eaux souterraines","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040066901","Etude SSP et ingénierie des travaux de réhabilitation","2020-07-24",null,"Rapport daté du 24 juillet 2020 réalisé par HPC Envirotec à propos des investigations complémentaires, du plan de gestion et l’analyse ds risques sanitaires résiduels.","Eaux souterraines","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040066901","Etude SSP et ingénierie des travaux de réhabilitation","2018-12-21",null,"Diagnostic de l’état du sous-sol – HPC Envirotec\n\nLes investigations ont été effectuées sur le site du 22 au 24 octobre 2018, du 4 au 7 novembre 2018 et le 9 novembre 2018 (échantillonnage des eaux souterraines). Elles ont consisté en la réalisation de 26 sondages de sols de 5 m  de profondeur dont 4 ont été équipés de piézairs temporaires à une profondeur de 2 m. Par ailleurs, 3 piézomètres ont été installés à des profondeurs de 12 à 18 m.\n\nLes résultats de ces premières investigations ont permis d’identifier des secteurs pollués notamment autour des anciennes cuves de stockage de carburants 7, 8 et 9 à proximité de l’aire de lavage. Les résultats d’analyses qui ont conduit à l’identification de zones reconnues impactées sont résumées ci-dessous.","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040066901","Etude SSP et ingénierie des travaux de réhabilitation","2019-01-22","2019-02-13","Suivi environnemental des travaux de démantèlement – HPC Envirotec\n\nSuite aux travaux des échantillons des matériaux laissés et/ou remis en place ont été prélevés et analysés afin de vérifier la qualité résiduelle des sols. Le rapport de suivi environnemental souligne quelques teneurs :\n    • en fond de fouille de la zone Ex 2 à 7 m de profondeur des teneurs maximales en hydrocarbures volatils C5-C10 de 247 mg/kg, en C10-C40 de 1 050 mg/kg et en BTEX de 61 mg/kg ont été mesurées;\n    • En fond de fouille de la zone Ex7 à 3 m  de profondeur des teneurs maximales en hydrocarbures C10-C40 de 11 600 mg/kg ;\n    • En fond de fouille de la zone Ex 10 à 2,7 m de profondeur des teneurs maximales en hydrocarbures C10-C40 de 902 mg/kg ;\n    • Dans les matériaux du Tas 7 remis en fouille qui présentent des teneurs en hydrocarbures C10-C40 de  1 320 mg/kg.\nLe rapport conclut à la présence de concentrations résiduelles significatives tout en indiquant que les valeurs restent faibles pour les zones Ex1, 2, 4, 5, et 9 et dans le smatériaux triés/remis en fouille.","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040066901","Etude SSP et ingénierie des travaux de réhabilitation","2020-07-24",null,"Rapport daté du 24 juillet 2020 réalisé par HPC Envirotec à propos des investigations complémentaires, du plan de gestion et l’analyse ds risques sanitaires résiduels.","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040067201","Etude SSP et ingénierie des travaux de réhabilitation","2020-03-30",null,"Rapport de « Diagnostic environnemental complémentaire n°2 » réalisé par la société ARCADIS et daté du 30 mars 2020 (réf : 18.000149-DIA-02-RPT-C01 ).\n\nCe rapport synthétise la campagne d’investigations complémentaires réalisée durant le mois d’août 2019. Elles comportent 3 sondages équipés en piézairs et une seconde campagne de mesures de la qualité des eaux souterraines et les gaz du sol.\n\nAprès un rappel des résultats des investigations antérieures, le bureau d’études indique que les nouveaux sondages ont été équipés en piézairs (PzrA, PzrB et PzrC) pour des profondeurs allant de 7 à 8 m. \n\nLe bureau d’études recommande de poursuivre le suivi de la qualité des eaux souterraines et d’obtenir les coupes techniques des piézomètres dans le cadre de la poursuite du suivi de la qualité des eaux souterraines ou de réaliser une inspection caméra sur ces ouvrages. Il indique que l’état du piézomètre Pz friche devra être évalué pour un remplacement éventuel.\n\nSur la base des résultats d’analyse, le bureau d’études indique que les piézairs (PzrA à PzrC) mis en place lors de ce diagnostic complémentaire ont permis de délimiter la pollution dans les gaz du sol mise en évidence au droit de Pzr2 vers l’ouest et vers le nord. Aucune délimitation n’a été réalisée vers le sud (station-service) et vers l’est (hors site, espace public). Une précision est cependant apportée pour indiquer qu’une incertitude reste sur la délimitation exacte de l’étendue de la pollution vers l’ouest.\n\nLes conclusions du rapport indiquent que les teneurs semblent avoir diminué entre les deux campagnes de mesures à l’exception de certains points ou paramètres. Elles précisent que la réalisation d’un plan de gestion sera nécessaire pour définir les mesures de gestion les plus adaptées à la maîtrise des pollutions et de leurs impacts.\n\n","Air","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040067201","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"Rapport « Diagnostic environnemental et étude technico-économique de gestion des déblais » réalisé par la société ARCADIS et daté du 30 mars 2020 (réf : 18.000149-DIA-01-RPT-C01)\n\nCe rapport, réalisé par la société ARCADIS, a connu plusieurs versions dont la première date de janvier 2019 et la version finale du 30 mars 2020. Les investigations environnementales initiales ont été réalisées en octobre 2018 avec un total 21 sondages de sols répartis sur le site sauf au droit de la station-service (encore en exploitation). 13 piézairs et des prélèvements sur les eaux souterraines ont été effectués en mars et avril 2019.\n\nLes résultats des analyses sur les échantillons prélevés mettent en évidence :\nDans les sols:\n\t– détection d’hydrocarbures C5-C10 avec des concertations comprises entre 1,2 mg/kg et 250 mg/kg et d’hydrocarbures C10-C40 avec une concentration maximale de 5 210 mg/kg au niveau de S6 en surface (180 mg/kg entre 1 m et 2 m de profondeur) ;\n\t– détection de BTEX avec une valeur maximale en S8 (6-7,5m) avec 110 mg/kg (12 mg/kg entre 7,5-9,5m) ;\n\t– détection de HAP sur 28 des 66 échantillons analysés avec des valeurs comprises majoritairement entre 0,07 mg/kg et 18 mg/kg pour les sondages sans dépassement. Trois valeurs dépassent 50 mg/kg avec comme concentration maximale 2 100 mg/kg sur S6 (0,05-1m) dont 30 mg/kg de Naphtalène ;\n\t– détection de COHV avec un maximum de 0,96 mg/kg observé en trichloroéthylène (TCE) et/ou le tétrachloroéthylène (PCE) sur S4 (1-2m).\n\nDans les eaux souterraines une concentration importante en TCE (380 µg/l en SP3 et 48 µg/l en Pzfriche) et PCE (21 µg/l en SP3).\n\nDans les gaz du sol:\n\t– des hydrocarbures C5-C16 détectés sur l’ensemble des piézairs avec notamment l’ouvrage Pzr12 (64 mg/m³) et l’ouvrage Pzr2 (proche de S8) qui présente un impact très important avec des valeurs comprises entre environ 36 g/m³ et 77 g/m³ (somme des tubes avec zones de mesure et contrôle) en fonction du temps de prélèvement réalisé ;\n\t– des BTEX détectés sur l’ensemble des piézairs avec une teneur maximale pour l’ouvrage Pzr2 qui présente un impact très important avec des valeurs comprises entre 6 g/m³ et 11 g/m³ en fonction du temps de prélèvement réalisé ;\n\t– des COHV détectés avec des valeurs comprises entre 22 µg/m³ et 2 378 µg/m³. Du trichloroéthylène (max. 213 µg/m³ en Pzr1) et du tétrachloroéthylène (max. 138 µg/m³ en Pzr2) sont également mesurés.\nLe rapport conclut qu’il y a probablement une minoration des concentrations mesurées en Pzr2 compte tenu de la saturation des deux tubes de prélèvement.\n\nSur la base de ces résultats, le bureau d’études a réalisé un schéma conceptuel prenant en compte les pollutions mesurées dans les rapports précédents (2014 à 2020). Les cibles considérées sont les futurs employés et usagers du projet ainsi que les utilisateurs du parc de stationnement qui seraient impactés par inhalation des gaz. Les voies de transfert retenues sont la percolation verticale des eaux de pluies, le transfert latéral via les écoulements de nappe et de subsurface et le dégazage des sols et eaux souterraines.\n\nEn fonction des données du projet SNC Paris 17 and Co, la société ARCADIS a réalisé une étude technico-économique de gestion des déblais. Cette estimation prend comme hypothèses des terrassements de 5,5 m en partie nord (parcelle DS5), 6,5 m au droit de l’actuel parc de stationnement et 16 m sur le reste du site.\n\nDans ses recommandations, le bureau d’études préconise de garder en mémoire l’emplacement des sols dans lesquels des substances ont été détectées et qui resteront après l’aménagement du site. Par ailleurs, il précise que les déblais ne devront pas être réutilisés sur ou hors site sans une justification adaptée.\n\nLa conclusion du rapport recommande de délimiter les impacts autour de l’ouvrage Pz2 qui n’a pas vocation à être excavé et de faire une seconde campagne de prélèvements dans les eaux souterraines et les gaz du sol dont une partie mettra en œuvre des canisters pour éviter les phénomènes de saturation. La réalisation d’une évaluation quantitative des risques sanitaires est aussi préconisée.","Air","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040067201","Etude SSP et ingénierie des travaux de réhabilitation","2014-12-02",null,"Rapport du diagnostic environnemental réalisé par la société ARCADIS à la demande de l’entreprise ESSO et daté du 2 décembre 2014 (réf : AFR-DIA-905-09-0583-RPT-VF)\n\nUn diagnostic environnemental de la station-service a été réalisé en 2014 par le bureau d’études ARCADIS à la demande de la société ESSO afin de dresser un état des lieux des éventuels impacts des installations pétrolières sur les milieux. Le programme d’investigation final a comporté la réalisation de 5 sondages de sol et d’un piézair. Des concentrations en hydrocarbures et BTEX ont été mesurées ([C5-C10]max = 243 mg/kg ; [C10-C40]max = 843 mg/kg ; [BTEX]max = 181 mg/kg) notamment au droit du sondage S2 situé proche de l’ancienne cuve 2, zone où une fuite a été détectée en 1998 (cf. le plan d’investigation ci-après). La conclusion du rapport ne recommandait pas d’investigations complémentaires.","Eaux souterraines","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040067201","Etude SSP et ingénierie des travaux de réhabilitation","2020-03-30",null,"Rapport de « Diagnostic environnemental complémentaire n°2 » réalisé par la société ARCADIS et daté du 30 mars 2020 (réf : 18.000149-DIA-02-RPT-C01 ).\n\nCe rapport synthétise la campagne d’investigations complémentaires réalisée durant le mois d’août 2019. Elles comportent 3 sondages équipés en piézairs et une seconde campagne de mesures de la qualité des eaux souterraines et les gaz du sol.\n\nAprès un rappel des résultats des investigations antérieures, le bureau d’études indique que les nouveaux sondages ont été équipés en piézairs (PzrA, PzrB et PzrC) pour des profondeurs allant de 7 à 8 m. \n\nLe bureau d’études recommande de poursuivre le suivi de la qualité des eaux souterraines et d’obtenir les coupes techniques des piézomètres dans le cadre de la poursuite du suivi de la qualité des eaux souterraines ou de réaliser une inspection caméra sur ces ouvrages. Il indique que l’état du piézomètre Pz friche devra être évalué pour un remplacement éventuel.\n\nSur la base des résultats d’analyse, le bureau d’études indique que les piézairs (PzrA à PzrC) mis en place lors de ce diagnostic complémentaire ont permis de délimiter la pollution dans les gaz du sol mise en évidence au droit de Pzr2 vers l’ouest et vers le nord. Aucune délimitation n’a été réalisée vers le sud (station-service) et vers l’est (hors site, espace public). Une précision est cependant apportée pour indiquer qu’une incertitude reste sur la délimitation exacte de l’étendue de la pollution vers l’ouest.\n\nLes conclusions du rapport indiquent que les teneurs semblent avoir diminué entre les deux campagnes de mesures à l’exception de certains points ou paramètres. Elles précisent que la réalisation d’un plan de gestion sera nécessaire pour définir les mesures de gestion les plus adaptées à la maîtrise des pollutions et de leurs impacts.\n\n","Eaux souterraines","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040067201","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"Rapport « Diagnostic environnemental et étude technico-économique de gestion des déblais » réalisé par la société ARCADIS et daté du 30 mars 2020 (réf : 18.000149-DIA-01-RPT-C01)\n\nCe rapport, réalisé par la société ARCADIS, a connu plusieurs versions dont la première date de janvier 2019 et la version finale du 30 mars 2020. Les investigations environnementales initiales ont été réalisées en octobre 2018 avec un total 21 sondages de sols répartis sur le site sauf au droit de la station-service (encore en exploitation). 13 piézairs et des prélèvements sur les eaux souterraines ont été effectués en mars et avril 2019.\n\nLes résultats des analyses sur les échantillons prélevés mettent en évidence :\nDans les sols:\n\t– détection d’hydrocarbures C5-C10 avec des concertations comprises entre 1,2 mg/kg et 250 mg/kg et d’hydrocarbures C10-C40 avec une concentration maximale de 5 210 mg/kg au niveau de S6 en surface (180 mg/kg entre 1 m et 2 m de profondeur) ;\n\t– détection de BTEX avec une valeur maximale en S8 (6-7,5m) avec 110 mg/kg (12 mg/kg entre 7,5-9,5m) ;\n\t– détection de HAP sur 28 des 66 échantillons analysés avec des valeurs comprises majoritairement entre 0,07 mg/kg et 18 mg/kg pour les sondages sans dépassement. Trois valeurs dépassent 50 mg/kg avec comme concentration maximale 2 100 mg/kg sur S6 (0,05-1m) dont 30 mg/kg de Naphtalène ;\n\t– détection de COHV avec un maximum de 0,96 mg/kg observé en trichloroéthylène (TCE) et/ou le tétrachloroéthylène (PCE) sur S4 (1-2m).\n\nDans les eaux souterraines une concentration importante en TCE (380 µg/l en SP3 et 48 µg/l en Pzfriche) et PCE (21 µg/l en SP3).\n\nDans les gaz du sol:\n\t– des hydrocarbures C5-C16 détectés sur l’ensemble des piézairs avec notamment l’ouvrage Pzr12 (64 mg/m³) et l’ouvrage Pzr2 (proche de S8) qui présente un impact très important avec des valeurs comprises entre environ 36 g/m³ et 77 g/m³ (somme des tubes avec zones de mesure et contrôle) en fonction du temps de prélèvement réalisé ;\n\t– des BTEX détectés sur l’ensemble des piézairs avec une teneur maximale pour l’ouvrage Pzr2 qui présente un impact très important avec des valeurs comprises entre 6 g/m³ et 11 g/m³ en fonction du temps de prélèvement réalisé ;\n\t– des COHV détectés avec des valeurs comprises entre 22 µg/m³ et 2 378 µg/m³. Du trichloroéthylène (max. 213 µg/m³ en Pzr1) et du tétrachloroéthylène (max. 138 µg/m³ en Pzr2) sont également mesurés.\nLe rapport conclut qu’il y a probablement une minoration des concentrations mesurées en Pzr2 compte tenu de la saturation des deux tubes de prélèvement.\n\nSur la base de ces résultats, le bureau d’études a réalisé un schéma conceptuel prenant en compte les pollutions mesurées dans les rapports précédents (2014 à 2020). Les cibles considérées sont les futurs employés et usagers du projet ainsi que les utilisateurs du parc de stationnement qui seraient impactés par inhalation des gaz. Les voies de transfert retenues sont la percolation verticale des eaux de pluies, le transfert latéral via les écoulements de nappe et de subsurface et le dégazage des sols et eaux souterraines.\n\nEn fonction des données du projet SNC Paris 17 and Co, la société ARCADIS a réalisé une étude technico-économique de gestion des déblais. Cette estimation prend comme hypothèses des terrassements de 5,5 m en partie nord (parcelle DS5), 6,5 m au droit de l’actuel parc de stationnement et 16 m sur le reste du site.\n\nDans ses recommandations, le bureau d’études préconise de garder en mémoire l’emplacement des sols dans lesquels des substances ont été détectées et qui resteront après l’aménagement du site. Par ailleurs, il précise que les déblais ne devront pas être réutilisés sur ou hors site sans une justification adaptée.\n\nLa conclusion du rapport recommande de délimiter les impacts autour de l’ouvrage Pz2 qui n’a pas vocation à être excavé et de faire une seconde campagne de prélèvements dans les eaux souterraines et les gaz du sol dont une partie mettra en œuvre des canisters pour éviter les phénomènes de saturation. La réalisation d’une évaluation quantitative des risques sanitaires est aussi préconisée.","Eaux souterraines","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040067201","Etude SSP et ingénierie des travaux de réhabilitation","2019-01-22",null,"Rapport « Étude historique et documentaire et vulnérabilité des milieux » réalisé par la société ARCADIS à la demande de la BNP Paribas Immobilier et daté du 22 janvier 2019 (réf : FR0147-DIA-01-RPT-A01)\n\nCe rapport, réalisé par la société ARCADIS, avait comme objectif l’identification des sources de pollutions potentielles et les vulnérabilités des milieux sur l’ensemble de la parcelle DS3 contenant le parc de stationnement et la station-service.\n\nSur le contexte environnemental, le rapport indique que la nappe est théoriquement située à 16 m de profondeur avec un sens d’écoulement vers le nord-ouest. Selon l’étude réalisée par ARCADIS en 2014 à l’aide d’un piézomètre, il semble qu’un écoulement de subsurface est présent au droit du site.\nD’autre part, l’étude recense trois sites en aval hydraulique pouvant avoir eu un impact sur le site. Il s’agit de la station-service Total située 32 avenue de la Porte de Saint Ouen, de l’Hôpital Bichat et de l’espace logistique GEODIS.\n\nSuite à une étude historique de la parcelle, le rapport identifie 9 sources potentielles de pollution dont une avec un risque fort de contamination (zone de la cuve 2 impliquée dans la fuite de 1998).\nLe rapport ayant été réalisé indépendamment des investigations de terrains effectuées par la société en octobre 2018, aucun programme d’investigations complémentaires n’est proposé.","Sol - Sous-sol","Etude historique, documentaire et mémorielle","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040067201","Etude SSP et ingénierie des travaux de réhabilitation","2006-06-01",null,"Rapport de la société SERPOL pour le compte de l’entreprise ESSO portant sur le « suivi des travaux de modernisation » daté de juin 2006 (réf : Rapport SERPOL n°5232) ;\n\nDans le cadre de l’automatisation de la station-service en 2006, la société SERPOL est intervenue suite à l’observation d’irisations et de suintements jaunes sur les murs du parc de stationnement souterrain pour vérifier la qualité des terrains au droit des installations pétrolières investiguées. Dans les éléments de contexte, le gérant de la station-service indique qu’une quantité de « 6 m³ de SP95 se sont déversés dans le terrain environ 10 ans plus tôt ». \n\nCet événement semble correspondre avec l’incident relevé en 1998 mais les quantités évoquées sont plus importantes. Le gérant a précisé que des pompages avaient été réalisés. Durant ces travaux trois zones de fouilles ont été investiguées (autour des cuves et du dépotage) et 72 tonnes de terres polluées ont été évacuées en centre agréé. Des concentrations en hydrocarbure C10-C40 allant jusqu’à 4 100 mg/kg ont été mesurées.\n\nCes éléments n’avaient pas été portés à la connaissance de l’inspection des installations classées et de la préfecture de police.","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040067201","Etude SSP et ingénierie des travaux de réhabilitation","2014-12-02",null,"Rapport du diagnostic environnemental réalisé par la société ARCADIS à la demande de l’entreprise ESSO et daté du 2 décembre 2014 (réf : AFR-DIA-905-09-0583-RPT-VF)\n\nUn diagnostic environnemental de la station-service a été réalisé en 2014 par le bureau d’études ARCADIS à la demande de la société ESSO afin de dresser un état des lieux des éventuels impacts des installations pétrolières sur les milieux. Le programme d’investigation final a comporté la réalisation de 5 sondages de sol et d’un piézair. Des concentrations en hydrocarbures et BTEX ont été mesurées ([C5-C10]max = 243 mg/kg ; [C10-C40]max = 843 mg/kg ; [BTEX]max = 181 mg/kg) notamment au droit du sondage S2 situé proche de l’ancienne cuve 2, zone où une fuite a été détectée en 1998 (cf. le plan d’investigation ci-après). La conclusion du rapport ne recommandait pas d’investigations complémentaires.","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040067201","Etude SSP et ingénierie des travaux de réhabilitation","2020-03-30",null,"Rapport de « Diagnostic environnemental complémentaire n°2 » réalisé par la société ARCADIS et daté du 30 mars 2020 (réf : 18.000149-DIA-02-RPT-C01 ).\n\nCe rapport synthétise la campagne d’investigations complémentaires réalisée durant le mois d’août 2019. Elles comportent 3 sondages équipés en piézairs et une seconde campagne de mesures de la qualité des eaux souterraines et les gaz du sol.\n\nAprès un rappel des résultats des investigations antérieures, le bureau d’études indique que les nouveaux sondages ont été équipés en piézairs (PzrA, PzrB et PzrC) pour des profondeurs allant de 7 à 8 m. \n\nLe bureau d’études recommande de poursuivre le suivi de la qualité des eaux souterraines et d’obtenir les coupes techniques des piézomètres dans le cadre de la poursuite du suivi de la qualité des eaux souterraines ou de réaliser une inspection caméra sur ces ouvrages. Il indique que l’état du piézomètre Pz friche devra être évalué pour un remplacement éventuel.\n\nSur la base des résultats d’analyse, le bureau d’études indique que les piézairs (PzrA à PzrC) mis en place lors de ce diagnostic complémentaire ont permis de délimiter la pollution dans les gaz du sol mise en évidence au droit de Pzr2 vers l’ouest et vers le nord. Aucune délimitation n’a été réalisée vers le sud (station-service) et vers l’est (hors site, espace public). Une précision est cependant apportée pour indiquer qu’une incertitude reste sur la délimitation exacte de l’étendue de la pollution vers l’ouest.\n\nLes conclusions du rapport indiquent que les teneurs semblent avoir diminué entre les deux campagnes de mesures à l’exception de certains points ou paramètres. Elles précisent que la réalisation d’un plan de gestion sera nécessaire pour définir les mesures de gestion les plus adaptées à la maîtrise des pollutions et de leurs impacts.\n\n","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040067201","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"Rapport « Diagnostic environnemental et étude technico-économique de gestion des déblais » réalisé par la société ARCADIS et daté du 30 mars 2020 (réf : 18.000149-DIA-01-RPT-C01)\n\nCe rapport, réalisé par la société ARCADIS, a connu plusieurs versions dont la première date de janvier 2019 et la version finale du 30 mars 2020. Les investigations environnementales initiales ont été réalisées en octobre 2018 avec un total 21 sondages de sols répartis sur le site sauf au droit de la station-service (encore en exploitation). 13 piézairs et des prélèvements sur les eaux souterraines ont été effectués en mars et avril 2019.\n\nLes résultats des analyses sur les échantillons prélevés mettent en évidence :\nDans les sols:\n\t– détection d’hydrocarbures C5-C10 avec des concertations comprises entre 1,2 mg/kg et 250 mg/kg et d’hydrocarbures C10-C40 avec une concentration maximale de 5 210 mg/kg au niveau de S6 en surface (180 mg/kg entre 1 m et 2 m de profondeur) ;\n\t– détection de BTEX avec une valeur maximale en S8 (6-7,5m) avec 110 mg/kg (12 mg/kg entre 7,5-9,5m) ;\n\t– détection de HAP sur 28 des 66 échantillons analysés avec des valeurs comprises majoritairement entre 0,07 mg/kg et 18 mg/kg pour les sondages sans dépassement. Trois valeurs dépassent 50 mg/kg avec comme concentration maximale 2 100 mg/kg sur S6 (0,05-1m) dont 30 mg/kg de Naphtalène ;\n\t– détection de COHV avec un maximum de 0,96 mg/kg observé en trichloroéthylène (TCE) et/ou le tétrachloroéthylène (PCE) sur S4 (1-2m).\n\nDans les eaux souterraines une concentration importante en TCE (380 µg/l en SP3 et 48 µg/l en Pzfriche) et PCE (21 µg/l en SP3).\n\nDans les gaz du sol:\n\t– des hydrocarbures C5-C16 détectés sur l’ensemble des piézairs avec notamment l’ouvrage Pzr12 (64 mg/m³) et l’ouvrage Pzr2 (proche de S8) qui présente un impact très important avec des valeurs comprises entre environ 36 g/m³ et 77 g/m³ (somme des tubes avec zones de mesure et contrôle) en fonction du temps de prélèvement réalisé ;\n\t– des BTEX détectés sur l’ensemble des piézairs avec une teneur maximale pour l’ouvrage Pzr2 qui présente un impact très important avec des valeurs comprises entre 6 g/m³ et 11 g/m³ en fonction du temps de prélèvement réalisé ;\n\t– des COHV détectés avec des valeurs comprises entre 22 µg/m³ et 2 378 µg/m³. Du trichloroéthylène (max. 213 µg/m³ en Pzr1) et du tétrachloroéthylène (max. 138 µg/m³ en Pzr2) sont également mesurés.\nLe rapport conclut qu’il y a probablement une minoration des concentrations mesurées en Pzr2 compte tenu de la saturation des deux tubes de prélèvement.\n\nSur la base de ces résultats, le bureau d’études a réalisé un schéma conceptuel prenant en compte les pollutions mesurées dans les rapports précédents (2014 à 2020). Les cibles considérées sont les futurs employés et usagers du projet ainsi que les utilisateurs du parc de stationnement qui seraient impactés par inhalation des gaz. Les voies de transfert retenues sont la percolation verticale des eaux de pluies, le transfert latéral via les écoulements de nappe et de subsurface et le dégazage des sols et eaux souterraines.\n\nEn fonction des données du projet SNC Paris 17 and Co, la société ARCADIS a réalisé une étude technico-économique de gestion des déblais. Cette estimation prend comme hypothèses des terrassements de 5,5 m en partie nord (parcelle DS5), 6,5 m au droit de l’actuel parc de stationnement et 16 m sur le reste du site.\n\nDans ses recommandations, le bureau d’études préconise de garder en mémoire l’emplacement des sols dans lesquels des substances ont été détectées et qui resteront après l’aménagement du site. Par ailleurs, il précise que les déblais ne devront pas être réutilisés sur ou hors site sans une justification adaptée.\n\nLa conclusion du rapport recommande de délimiter les impacts autour de l’ouvrage Pz2 qui n’a pas vocation à être excavé et de faire une seconde campagne de prélèvements dans les eaux souterraines et les gaz du sol dont une partie mettra en œuvre des canisters pour éviter les phénomènes de saturation. La réalisation d’une évaluation quantitative des risques sanitaires est aussi préconisée.","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040067201","Etude SSP et ingénierie des travaux de réhabilitation","2020-05-24",null,"Rapport de « Diagnostic environnemental complémentaire sur les sols » réalisé par la société ARCADIS à la demande de la BNP Paribas Immobilier et daté du 24 mai 2020 (réf : 18.000149-DIA-05-RPT-B01)",null,"Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040067201","Etude SSP et ingénierie des travaux de réhabilitation","2020-03-30",null,"Rapport d’« évaluation quantitative des risques sanitaires » réalisé par la société ARCADIS et daté du 30 mars 2020 (AFR-EQRS-03-RPT-C01)",null,"Analyse des enjeux sanitaires (EQRS, ARR)","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040067201","Etude SSP et ingénierie des travaux de réhabilitation","2020-05-24",null,"Rapport de « Plan de gestion » réalisé par la société ARCADIS à la demande de la BNP Paribas Immobilier et daté du 24 mai 2020 (réf : AFR-PG-04-RPT-C01)",null,"Plan de gestion","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040067801","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"Mémoire sur l'impact d'une potentiel pollution.","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040068001","Exécution des travaux de réhabilitation",null,null,"Remplissage de sablon de la cuve d’essence",null,"N/A","N/A","N/A","N/A","Mise en place de mesure de réhabilitation",null,"N/A","N/A","N/A"]
["SSP040068501","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"Une campagne d’investigation fût faites par la réalisation de 15 sondages avec l’analyse de 25 échantillons de sols ainsi que le suivi des eaux souterraines avec l’installation de 3 piézomètres.\n",null,"Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040069601","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"Le mémoire concernant l'impact sur l'environnement.","Eaux souterraines","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP040084301","Etude SSP et ingénierie des travaux de réhabilitation","2016-04-01",null,"Afin d’identifier les pollutions sur le site, plusieurs investigations de terrain ont été menées entre 2014 et 2015 : \n    • Un diagnostic daté d’avril 2014 rapport référencé W1147P09 ;\n    • Un diagnostic daté de juillet 2014 rapport référencé W1147P09 ;\n    • Un diagnostic complémentaire daté de janvier 2015 rapport référencé W1147P10 ;\n    • Un diagnostic complémentaire daté de juillet 2015 rapport référencé W1147P14.\n\nParallèlement à ces études, 13 piézomètres ont été installés et six campagnes de suivi de la qualité de la nappe ont été réalisées afin de caractériser le panache de pollution sur le site.\n\nUn plan de gestion a été finalisé en avril 2016 référencé W1147P14 afin de proposer des solutions de gestion concernant les impacts majeurs retenus sur : \n    • les sols : zone de stockage de batteries usagées principalement polluée par des hydrocarbures entre 0 et 5 m de profondeur sur 30 m² de surface (150 m3 environ) ;\n    • les eaux souterraines : impact en hydrocarbures au droit des piézomètres Pz4 et Pz6 (autour de la zone de stockage des batteries).\n\nLa méthodologie nationale de gestion des sites et sols pollués ayant été actualisée en avril 2017, l’ancien exploitant CITROEN a souhaité revoir son plan de gestion et a transmis par courrier du 12 octobre 2020 reçu en DREAL le 28 octobre 2020 une actualisation du plan de gestion.\n",null,"Plan de gestion","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP069619301","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"La consultation des missions aériennes de la photothèque a permis de déterminer un début d'activité de service sur le site  compris entre 1969 et 1974. \nPour les occupations visibles, la cessation d’activité pour le garage automobile-carrosserie est postérieure à 2013.\n\nPar ailleurs, le site n’est pas soumis à la réglementation des Installations Classées pour la Protection de l’Environnement (ICPE).\n",null,"Etude historique, documentaire et mémorielle","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP069619301","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"Les analyses et mesures PID du sol ont permet d'évaluer la qualité du sol en mesurant les composés cités ci-dessous :\n- ETM et assimilés ;\n- HCT / Hydrocarbures totaux C10-C40 ;\n- HAP ;\n- BTEX / Hydrocarbures Composés Aromatiques ;\n- PCB / Polychlorobiphényls ;\n- COHV / Composés Organiques Halogénés Volatils ;\n- Composés Organiques Volatils (COV, air des sols).\n\nLes investigations du sol ont permis de mettre en évidence des sources de contaminations :\n- En Éléments Traces Métalliques & assimilés / métaux lourds ;\n- En Hydrocarbures totaux / HCT ;\n- En Hydrocarbures Aromatiques Polycycliques / HAP, à l’état de traces ;\n- En Hydrocarbures Composés Aromatiques / BTEX ;\n- En Polychlorobiphényls / PCB ;\n- En Composés Organiques Volatils / COV.\n",null,"Diagnostic et Analyse","N/A",null,"COHV, solvants chlorés, fréons | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP41830801","Surveillance environnementale",null,null,"Surveillance des sols au droit des points référencés par socotec le 31 juillet 2020 ou équivalent. \n\nFréquence tous les 5 ans ","Sol - Sous-sol","N/A","1","Indice hydrocarbures totaux - produits pétroliers | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Somme HAP (15 molécules)","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP41830801","Surveillance environnementale",null,null,"sur les paramètres suivants: \n- hydrocarbures totaux \n- BTEX totaux \n- somme des HAP \n\nFréquence: 2 campagnes par an ",null,"N/A","2",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP44363501","Surveillance environnementale",null,null," Fréquence: 2 campagne par an ","Eaux souterraines","N/A","2","Indice hydrocarbures totaux - produits pétroliers | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Somme HAP (15 molécules)","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP44363501","Surveillance environnementale",null,null,"Surveillance effectuée sur les points référencés dans le rapport de Socotec du 31 juillet 2020. \n\nFréquence: campagne tous les 5 ans ","Sol - Sous-sol","N/A","1","Indice hydrocarbures totaux - produits pétroliers | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Somme HAP (15 molécules)","Benzène et dérivés | HAP (Hydrocarbures aromatiques, polycycliques, pyrolytiques et dérivés) | Hydrocarbures et indices liés","N/A","N/A","N/A","N/A","N/A"]
["SSP50548401","Surveillance environnementale","2021-07-01",null,"Une inspection s’est déroulée sur le 22 janvier 2021 dans le cadre de la demande de restitution des parcelles A2 et A3 au grand port maritime du Havre (GPMH). Suite à cette visite, l'inspection a demandé de transmettre de nouvelles analyses des eaux souterraines afin de démontrer l’efficacité des opérations de dépollution réalisées.\nEn effet, les résultats d’analyses des eaux souterraines mettaient en évidence la présence de concentrations en éléments traces métalliques et en sulfates supérieures aux valeurs seuils, définies par l’arrêté ministériel du 17 décembre 2008 établissant les critères d’évaluation et les modalités de détermination de l’état des eaux souterraines, au niveau des piézomètres Pz10, Pz11 et Pz12.\n\nL'exploitant propose :\n    • d'installer dans le courant du deuxième semestre 2021 un nouveau piézomètre au plus près des anciens piézomètres Pz10, Pz11 et Pz12 ;\n    • de mesurer les teneurs en métaux sur l’ensemble des piézomètres.\n\nAvis avis favorable aux propositions précitées. L'exploitant doit réaliser a minima cinq campagnes de mesures des eaux souterraines. À l’issue de ces cinq campagnes d’analyses, l'exploitant transmettra un bilan de suivi de la qualité des eaux souterraines.\n\nEn cas de persistance des dépassements des valeurs limites, l'exploitant devra  remettre un dossier de servitudes d’utilités publiques relatives à l’usage des eaux souterraines.\n\nLes parcelles A2 et A3 peuvent être restituées au GPMH sous réserve du respect des demandes précitées.",null,"N/A","5",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP52626901","Exécution des travaux de réhabilitation",null,null,"Compte tenu de la présence de pollutions résiduelles au droit du site et des hypothèses prises en compte dans l’analyse des risques sanitaires, les restrictions d’usages suivantes devront être respectées :\n    • Maintien d’un usage industriel ;\n    • Maintien d’une couverture des sols (enrobé, dalle béton, terre végétale ou tout recouvrement de protection équivalente) ;\n    • Réalisation de nouvelles canalisations d’eau potable en matériaux non perméables aux polluants et mises en place dans des matériaux sains ;\n    • Interdiction d’utilisation des eaux souterraines au droit du site sauf réalisation, aux frais et sous la responsabilité de la personne à l’origine d’un nouvel usage, d’études et de mesures garantissant l’absence de tout risque inacceptable pour la santé et l’environnement en fonction de l’usage prévu, conformément à la réglementation et à la méthodologie applicables ;\n    • Interdiction de jardins potagers (à l’exception des cultures hors sol), d’arbres fruitiers et d’élevages animaliers à des fins de consommation ou de tout autre aménagement pouvant être à l’origine d’une production de denrées alimentaires humaines ou animales ;\n    • Tous travaux entrepris affectant le sol ou le sous-sol du site (notamment travaux d’affouillement ou d’excavation de terres) font l’objet, aux frais et sous la responsabilité de la personne à l’origine de ces travaux, de mesures adaptées de gestion, d’hygiène, de sécurité, de précaution et le cas échéant d’élimination, conformément à la réglementation applicable. Ces travaux ne doivent pas avoir pour effet de remobiliser, solubiliser, ou faire migrer les polluants notamment vers les eaux de surface et les eaux souterraines ou dans l’air. Toute réutilisation de terres polluées sur site est tracée, les polluants caractérisés (nature, tonnage, teneurs,...), et localisés sur un plan conservé par le propriétaire.\n\nEn cas de changement d’usage, l’article L. 556-1 du code de l’environnement s’applique. Cet article stipule qu’en cas de modification de l'usage du site, le maître d'ouvrage à l'origine du changement d'usage est tenu d'assurer la compatibilité du terrain avec son nouvel usage. Pour cela, il doit définir les mesures de gestion de la pollution, selon les modalités précisées aux articles R. 556-1, R. 556-3 et R. 556-5 du code de l'environnement, les mettre en œuvre, et joindre à la demande de permis de construire ou d'aménager l'attestation (ATTES) délivrée par un bureau d'études certifié dans le domaine des sites et sols pollués justifiant cette mise en œuvre. ","Eaux souterraines","N/A","N/A","N/A","N/A","Restriction d'usage proposée",null,"N/A","N/A","N/A"]
["SSP52626901","Etude SSP et ingénierie des travaux de réhabilitation","2014-01-27","2019-09-27","La société CLEAN 38 a fait réaliser plusieurs diagnostics environnementaux au droit de son site en 2013, 2014, 2018 et 2019 :\n    • Diagnostic de pollution des sols – 27/01/2014 – GALTIER EXPERTISE ENVIRONNEMENT\n    • Diagnostic de pollution complémentaire des sols et des eaux souterraines – 07/09/2015 – GALTIER EXPERTISE ENVIRONNEMENT\n    • Diagnostic complémentaire de la qualité des milieux et plan de gestion – 27/09/2019 – ENVISOL \n\nCes diagnostics ont mis en évidence :\n\n> dans les sols :\n- la présence d’hydrocarbures dans les sols de manière diffuse sur le site avec des sources plus concentrées :\n    • au droit de la zone des dix cuves enterrées de gasoil au sud-est du site avec des concentrations jusqu’à 2800 mg/kg entre 1,5 et 3,2 m de profondeur ;\n    • au droit de la station-service avec des concentrations jusqu’à 1700 mg/kg entre 1 et 2,5 m de profondeur ;\n    • au droit de l’ancienne cuve enterrée d’essence au nord-ouest du bâtiment avec des concentrations jusqu’à 1000 mg/kg entre 1 et 2 m de profondeur ;\n      \n- un impact diffus en métaux lourds dans les remblais du site avec des impacts localisés plus significatifs correspondant aux valeurs des fortes anomalies naturelles selon la base de données de l’INRA/ASPITET :\n        ◦ impacts en plomb (jusqu’à 720 mg/kg) au droit de l’ancienne aire de lavage au nord du bâtiment ;\n        ◦ impacts en cadmium (1,4 mg/kg) à proximité de la nouvelle aire de lavage ;\n        ◦ impacts en cuivre (jusqu’à 240 mg/kg) au droit de l’atelier de vidange, de l’ancienne cuve d’essence et de l’ancienne aire de lavage ;\n\n- des traces de tétrachloroethylène (PCE) et de trichloréthylène (TCE) au droit de l’ancienne zone de distribution de carburants (à l’ouest), de l’atelier de vidange, de l’ancienne aire de lavage et de l’ancienne cuve d’essence (jusqu’à 0,31 mg/kg de PCE et 0,13 mg/kg de TCE) ;\n\n- des traces diffuses de HAP (<20 mg/kg) ;\n\n\n> dans les eaux souterraines :\n    • la présence de chlorure de vinyle au droit des piézomètres Pz2 (50 µg/l) et Pz3 (1,4 à 4,4 µg/l) situés en aval hydraulique du site et des traces de COVH sur les deux autres piézomètres mais en concentration plus faible ;\n    • la présence d’hydrocarbures au droit du Pz4 situé à proximité des anciennes cuves d’eaux hydrocarburées ;\n    • des traces de métaux sur les piézomètres (As, Cr, Cu et Zn).\n\n\n> dans les gaz du sol :\n    • un impact généralisé en hydrocarbures volatils avec les concentrations les plus élevées au droit de la zone des dix cuves enterrées de gasoil, de l’ancienne cuve d’essence, de la station-service et des aires de lavage ;\n    • un impact généralisé en solvants chlorés (principalement TCE et PCE) avec les concentrations les plus élevées au droit des fosses de vidange (9037 µg/m³), de l’ancienne cuve d’essence et de sa zone de distribution (4604 µg/m³) et des aires de lavage (2482 à 3567 µg/m³) ;\n    • un impact généralisé en BTEX sur le site, principalement en xylènes et éthylbenzène, avec des concentrations en xylènes de 932 à 4574 µg/m³ et en éthylbenzène de 226 à 1157 µg/m³. ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP52626901","Etude SSP et ingénierie des travaux de réhabilitation","2019-09-27",null,"plan de gestion – 27/09/2019 – ENVISOL \n\nL’exploitant a retenu dans son plan de gestion un seuil de coupure de 900 mg/kg pour les hydrocarbures dans les sols. Ce seuil de coupure permet de traiter 50 % de la masse totale d’hydrocarbures contenus dans 20 % du volume total de terre. Ce seuil de coupure est retenu comme objectif de dépollution pour les hydrocarbures.\nLe plan de gestion ne retient pas de seuil de coupure pour les COHV car il considère que les COHV adsorbés sont présents au droit des zones à dépolluer en hydrocarbures et/ou à proximité d’infrastructures à démanteler. Les terres impactées aux COHV seront donc éliminées avec les terres impactées aux hydrocarbures.\n\nLe plan de gestion ne propose pas non plus de seuil de coupure pour les BTEX contenus dans les gaz du sol dont la pollution est diffuse sur tout le site.\n\nÀ partir du seuil de coupure en hydrocarbures, 3 zones de sources concentrées en hydrocarbures ont été identifiées :\n    • Zone des anciennes cuves enterrées de gasoil au sud-est du site ;\n    • Zone de la station-service ;\n    • Zone de l’ancienne cuve enterrée d’essence.\n\nBien qu’aucun seuil de coupure n’ait été déterminé pour les COVH, 5 spots impactés en COHV adsorbés dans les sols ont été identifiés.\n\nLes mesures de gestion prévues par l’exploitant consistent à traiter les 3 zones de sources concentrées en hydrocarbures, ainsi que les 5 spots en COHV adsorbés.\n\nL’exploitant a étudié les différentes solutions techniques possibles pour traiter ces zones de sources concentrées et a finalement retenu la solution d’excavation des terres polluées avec un traitement hors site.","Sol - Sous-sol","Plan de gestion","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP52626901","Exécution des travaux de réhabilitation",null,null,"Compte tenu de la présence de pollutions résiduelles au droit du site et des hypothèses prises en compte dans l’analyse des risques sanitaires, les restrictions d’usages suivantes devront être respectées :\n    • Maintien d’un usage industriel ;\n    • Maintien d’une couverture des sols (enrobé, dalle béton, terre végétale ou tout recouvrement de protection équivalente) ;\n    • Réalisation de nouvelles canalisations d’eau potable en matériaux non perméables aux polluants et mises en place dans des matériaux sains ;\n    • Interdiction d’utilisation des eaux souterraines au droit du site sauf réalisation, aux frais et sous la responsabilité de la personne à l’origine d’un nouvel usage, d’études et de mesures garantissant l’absence de tout risque inacceptable pour la santé et l’environnement en fonction de l’usage prévu, conformément à la réglementation et à la méthodologie applicables ;\n    • Interdiction de jardins potagers (à l’exception des cultures hors sol), d’arbres fruitiers et d’élevages animaliers à des fins de consommation ou de tout autre aménagement pouvant être à l’origine d’une production de denrées alimentaires humaines ou animales ;\n    • Tous travaux entrepris affectant le sol ou le sous-sol du site (notamment travaux d’affouillement ou d’excavation de terres) font l’objet, aux frais et sous la responsabilité de la personne à l’origine de ces travaux, de mesures adaptées de gestion, d’hygiène, de sécurité, de précaution et le cas échéant d’élimination, conformément à la réglementation applicable. Ces travaux ne doivent pas avoir pour effet de remobiliser, solubiliser, ou faire migrer les polluants notamment vers les eaux de surface et les eaux souterraines ou dans l’air. Toute réutilisation de terres polluées sur site est tracée, les polluants caractérisés (nature, tonnage, teneurs,...), et localisés sur un plan conservé par le propriétaire.\n\nEn cas de changement d’usage, l’article L. 556-1 du code de l’environnement s’applique. Cet article stipule qu’en cas de modification de l'usage du site, le maître d'ouvrage à l'origine du changement d'usage est tenu d'assurer la compatibilité du terrain avec son nouvel usage. Pour cela, il doit définir les mesures de gestion de la pollution, selon les modalités précisées aux articles R. 556-1, R. 556-3 et R. 556-5 du code de l'environnement, les mettre en œuvre, et joindre à la demande de permis de construire ou d'aménager l'attestation (ATTES) délivrée par un bureau d'études certifié dans le domaine des sites et sols pollués justifiant cette mise en œuvre. ","Sol - Sous-sol","N/A","N/A","N/A","N/A","Restriction d'usage proposée",null,"N/A","N/A","N/A"]
["SSP52626901","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"L’exploitant a réalisé une analyse des risques sanitaires à partir des résultats d’analyses des gaz du sol. Pour cette étude, seule la voie d’exposition par inhalation de gaz est prise en compte. L’analyse conclut à un risque acceptable pour un usage industriel sans travaux de dépollution sous réserve de restrictions d’usage permettant de couper les voies de transfert par ingestion et par inhalation de vapeurs polluées telles que le recouvrement des sols, l’absence d’usage des eaux souterraines, l’utilisation de matériaux non perméables aux polluants pour les réseaux d’eau potable.\n\nBien que l’analyse des risques mette en évidence que l’état du site avant travaux est compatible avec un usage industriel, l’exploitant a fait réaliser un plan de gestion afin de traiter les sources concentrées de pollution conformément à la méthodologie nationale relative aux sites et sols pollués. ",null,"Analyse des enjeux sanitaires (EQRS, ARR)","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP52626901","Exécution des travaux de réhabilitation","2019-12-09","2020-02-21","Les travaux de dépollution ont été réalisés du 09 décembre 2019 au 21 février 2020. Huit zones ont été excavées :\n\n    • Ft1 et Ft2 : Zones des 10 cuves enterrées de gasoil (impacts hydrocarbures et BTEX)\n    • Ft3 : Zone de l’ancienne cuve enterrée d’essence (impacts hydrocarbures, BTEX)\n    • Ft4 : Zone des cuves d’eaux hydrocarburées et de la cuve d’huiles usagées (impacts hydrocarbures et COHV)\n    • Ft5 : Zone de l’aire de lavage (impacts COHV, hydrocarbures, BTEX)\n    • Ft6 : Zone de la station-service (impacts hydrocarbures)\n    • Ft7 : Zone de l’ancienne aire de lavage (impacts COHV, BTEX, hydrocarbures)\n    • Ft8 : Zone de l’ancienne aire de distribution de carburant (impacts COHV et BTEX)\n\nAu total, 1021 m³ de terres ont été excavés. Les terres excavées ont fait l’objet de contrôles par lot de 100 m³ afin de déterminer si ces terres devaient être évacuées hors site ou si elles pouvaient être réutilisées sur site. Ainsi, parmi les terres excavées, 819,9 t ont été éliminées hors site en centre de traitement autorisés. Les terres excavées qui ne présentaient pas d’indices organoleptiques de pollutions, qui ne présentaient pas de pollution à la mesure au PID et qui présentaient une concentration en hydrocarbures inférieure au seuil de coupure (900 mg/kg) ont été utilisées en remblais sur le site.\n\nPar ailleurs, les zones excavées ont été remblayées avec des matériaux de type 80/120 pour la partie sous le niveau de la nappe et avec des matériaux tout-venant pour le remblaiement jusqu’au niveau final. Ces matériaux proviennent de la carrière Budillon-Rabatel d’Izeaux.\n\nÀ l’issue des excavations, des analyses des bords et fonds de fouilles ont été réalisées afin de vérifier l’atteinte de l’objectif de dépollution. L’ensemble des échantillons prélevés avait une concentration en hydrocarbures inférieure à l’objectif de dépollution fixé dans le plan de gestion à 900 mg/kg. Les résultats montrent des concentrations résiduelles en hydrocarbures inférieures à 500 mg/kg, à l’exception de la zone Ft6 (station-service) qui présente sur deux analyses de bords de fouille des concentrations de 620 et 750 mg/kg.\n\nCes investigations post-travaux ont mis en évidence :\n    • dans les eaux souterraines : une baisse de la concentration en chlorure de vinyle au droit du Pz3 (0,3 µg/l). Toutefois, lors de ces investigations complémentaires, il n’y a pas eu d’analyses sur les piézomètres situés en aval hydraulique de l’atelier de vidange et des aires de lavages, les ouvrages Pz2 et Pz4 ayant été détruits lors des travaux d’excavation.\n    • dans les gaz du sol : une baisse significative des concentrations en BTEX, COHV et hydrocarbures volatils. Les concentrations résiduelles maximales constatées sont :\n        ◦ pour les BTEX : 46 µg/m³ à proximité de la station-service ;\n        ◦ pour les COHV : 1893 µg/m³ (principalement du PCE) au droit des fosses de vidange où aucune excavation n’a été réalisée compte tenu du maintien du bâtiment. Cette concentration reste significative.\n        ◦ pour les hydrocarbures : 19 µg/m³ pour les HC aliphatiques au niveau de la cour de stockage des citernes routières et 122 µg/m³ pour les HC aromatiques à proximité de l’ancienne cuve d’essence.\n\nL’exploitant a fait réaliser une analyse des risques résiduels à partir des concentrations résiduelles mesurées lors des investigations post-travaux et en considérant un usage futur de type industriel.\n\nL’analyse de risques se base sur les hypothèses suivantes :\n    • les sols sont recouverts par le bâti, une dalle béton ou de l’enrobé ;\n    • il n’y aura pas d’utilisation des eaux souterraines au droit du site ;\n    • les futures conduites d’eau potable seront en PEHD ou PVC et mises en place dans des matériaux sains ;\n    • il n’y aura pas de cultures, ni d’élevage sur le site.\n\nAinsi, les voies d’exposition par ingestion de sol, inhalation de poussières, inhalation de vapeurs d’eau, ingestion d’eau, ingestion d’aliments d’origine végétale ou animale et absorption cutanée ne sont pas considérées dans l’analyse des risques résiduels prédictive.\n\nLa seule voie d’exposition prise en compte est l’inhalation de polluants sous forme gazeuse.\n\nL’analyse de risque conclut à un risque acceptable pour un usage industriel. ",null,"N/A","N/A","N/A","N/A","Travaux de dépollution"]
["SSP52715701","Etude SSP et ingénierie des travaux de réhabilitation","2019-10-04","2019-10-04","Une première étude, réalisée le 4 octobre 2019 par la société INGEOS, a mis en évidence :\n\n-dans les sols, la présence d’hydrocarbures (concentration maximale : 9900 mg/kg), de HAP (hydrocarbures aromatiques polycycliques) (concentrations maximales 9.7 mg/kg), de BTEX (benzène, toluène, éthylbenzène et xylènes) (concentration totale maximale : 9.2 mg/kg et absence de benzène) et de métaux ( concentrations maximales en chrome : 64 mg/kg, cuivre : 45 mg/kg, plomb : 49 mg/kg, zinc : 100 mg/kg,\n- dans les eaux souterraines de très faibles teneurs en zinc (concentration maximale : 11 µg/l), en hydrocarbures de fraction C12-C16 (concentration maximale : 11 µg/l), en hydrocarbures de fraction C16-C20 (concentration maximale : 7 µg/l), en hydrocarbures aromatiques polycycliques (concentration maximale totale : 0,12 µg/l) et en perchloréthylène (concentration maximale : 0,2 µg/l).\n- dans les eaux superficielles, constituées par un ruisseau busé traversant le site, de très faibles teneurs en chrome (concentration maximale : 7,5 µg/l), en cuivre (concentration maximale : 15 µg/l), en zinc (concentration maximale : 10 µg/l), et en perchloréthylène (concentration maximale : 0,2 µg/l).","Eaux souterraines","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP52715701","Etude SSP et ingénierie des travaux de réhabilitation","2020-07-09","2021-01-28","La société SOLER Environnement a réalisé un diagnostic de sol pour le compte de la mairie de Cranves-Sales sur les parcelles 1367, 388, 1573 destinées à accueillir le bâtiment abritant des activités sportives. Cette étude a mis en évidence : \n\nlors d'une première campagne d'analyses complémentaires réalisée en mai 2020\n\n- dans les sols, la présence d’hydrocarbures (concentration maximale : 540 mg/kg) et de métaux ( concentrations maximales en cadmium : 7.8 mg/kg, cuivre : 470 mg/kg, plomb : 3100 mg/kg, zinc : 370 mg/kg),\n- l'absence d'anomalie dans les eaux souterraines.\n\nLors d'une seconde étude réalisée en octobre 2020\n\n- dans les sols, la présence d’hydrocarbures (concentration maximale : 2400 mg/kg) et de métaux ( concentrations maximales en chrome : 68 mg/kg, cuivre : 39 mg/kg, plomb : 430 mg/kg, zinc : 160 mg/kg).\n\n\n\n\n","Eaux souterraines","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP52715701","Etude SSP et ingénierie des travaux de réhabilitation","2019-10-04","2019-10-04","Une première étude, réalisée le 4 octobre 2019 par la société INGEOS, a mis en évidence :\n\n-dans les sols, la présence d’hydrocarbures (concentration maximale : 9900 mg/kg), de HAP (hydrocarbures aromatiques polycycliques) (concentrations maximales 9.7 mg/kg), de BTEX (benzène, toluène, éthylbenzène et xylènes) (concentration totale maximale : 9.2 mg/kg et absence de benzène) et de métaux ( concentrations maximales en chrome : 64 mg/kg, cuivre : 45 mg/kg, plomb : 49 mg/kg, zinc : 100 mg/kg,\n- dans les eaux souterraines de très faibles teneurs en zinc (concentration maximale : 11 µg/l), en hydrocarbures de fraction C12-C16 (concentration maximale : 11 µg/l), en hydrocarbures de fraction C16-C20 (concentration maximale : 7 µg/l), en hydrocarbures aromatiques polycycliques (concentration maximale totale : 0,12 µg/l) et en perchloréthylène (concentration maximale : 0,2 µg/l).\n- dans les eaux superficielles, constituées par un ruisseau busé traversant le site, de très faibles teneurs en chrome (concentration maximale : 7,5 µg/l), en cuivre (concentration maximale : 15 µg/l), en zinc (concentration maximale : 10 µg/l), et en perchloréthylène (concentration maximale : 0,2 µg/l).","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP52715701","Etude SSP et ingénierie des travaux de réhabilitation","2020-07-09","2021-01-28","La société SOLER Environnement a réalisé un diagnostic de sol pour le compte de la mairie de Cranves-Sales sur les parcelles 1367, 388, 1573 destinées à accueillir le bâtiment abritant des activités sportives. Cette étude a mis en évidence : \n\nlors d'une première campagne d'analyses complémentaires réalisée en mai 2020\n\n- dans les sols, la présence d’hydrocarbures (concentration maximale : 540 mg/kg) et de métaux ( concentrations maximales en cadmium : 7.8 mg/kg, cuivre : 470 mg/kg, plomb : 3100 mg/kg, zinc : 370 mg/kg),\n- l'absence d'anomalie dans les eaux souterraines.\n\nLors d'une seconde étude réalisée en octobre 2020\n\n- dans les sols, la présence d’hydrocarbures (concentration maximale : 2400 mg/kg) et de métaux ( concentrations maximales en chrome : 68 mg/kg, cuivre : 39 mg/kg, plomb : 430 mg/kg, zinc : 160 mg/kg).\n\n\n\n\n","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP52715701","Etude SSP et ingénierie des travaux de réhabilitation","2021-01-21","2021-01-21","La société SOLER Environnement a réalisé un diagnostic de sol pour le compte de la société COGEDIM sur les parcelles 1361, 1362, 2038, 2096, 2097, destinées à accueillir le programme  immobilier de logements. Cette étude a mis en évidence : \n\n- dans les sols, la présence d’hydrocarbures (concentration maximale : 2800 mg/kg), de HAP (concentrations maximales 1.2 mg/kg en benzo(a)pyrène), et de métaux (concentrations maximales en cadmium : 8.6 mg/kg, chrome : 61 mg/kg, cuivre : 170 mg/kg, plomb : 1100 mg/kg, zinc : 560 mg/kg,\n- l'absence d'anomalie dans les eaux souterraines de façon cohérente avec le faible pouvoir de lixiviation mesurés sur les échantillons de sol.\n",null,"Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP52715701","Etude SSP et ingénierie des travaux de réhabilitation","2020-09-29","2021-07-27","L'APAVE a réalisé les études suivantes dans le cadre de la procédure de cessation d'activité conduite par M. BRAND : \n\n- le 29 septembre 2020 \"prélèvements, mesures, observations et/ou analyses sur les sols et interprétation des résultats, constituant un état des lieux des zones qui avaient fait l'objet des premiers travaux de dépollution,\n- le 26 juillet 2021 \"Analyses des enjeux sanitaires\" qui prend en compte les résultats de l'ensemble des diagnostics de sol réalisés jusqu'alors, par les différents bureaux d'études,\n- le 27 juillet 2021, \"Plan de gestion\" qui propose des modalités de traitement du site afin de permettre sa réoccupation par les projets retenus.\n\nL'évaluation des risques sanitaires conclut que fait l'inventaire des expositions des personnes susceptibles de fréquenter l'ancien site dans le cadre de sa réoccupation par des logements et un bâtiments destiné à des activités sportives est acceptable sauf pour les exposition à l'exception des deux scénarios suivants : \n- ingestion de poussières de sol,\n- ingestion de végétaux produits sur le site.\n\nLe plan de gestion propose des dispositions de traitement des pollutions permettant :\n- d'éliminer les points chauds et les pollutions concentrées et, dans ce cadre, il détermine par une approche statistique ce qu'il convient de considérer comme tels.\n- de rendre acceptable du point de vue sanitaire la réoccupation du site. \n\nLe plan de gestion propose en conclusion de retenir les seuils de dépollutions suivants dans l'objectif de suppression des points chauds et des pollutions concentrées : \n- hydrocarbures : 500 mg/kg, \n- hydrocarbures aromatiques polycycliques : 5 mg/kg,\n- cadmium : 5 mg/kg,\n- cuivre : 80 mg/kg,\n- zinc : 280 mg/kg,\n- plomb : 500 mg/kg.\nLes excavations correspondant à ces seuils de pollution résiduelle sont évaluées entre 1030 et 1530 m3 soit entre 1860 et 2780 tonnes. Ces terres seront ensuite traitées dans des filières correspondant à leur caractéristiques chimiques.\n\nPar ailleurs, pour permettre de garantir l'acceptabilité de la réoccupation du site et au vu des conclusion de l'étude sanitaire,  le plan de gestion propose : \n- la couverture de l'intégralité de la surface du site afin supprimer les possibilité d'ingestion de terres impactées par l'activité passée, \n- l'interdiction de jardin potager,\n- la mise en place de canalisations d'adduction d'eau potable étanches aux composés volatils dans des remblais propres pour éviter toute pénétration de polluants.\n\nDes échanges entre les différentes parties sont en cours concernant ce plan de gestion. ",null,"Analyse des enjeux sanitaires (EQRS, ARR)","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP53656202","Surveillance environnementale","2019-06-21",null,"Modalités de surveillance des eaux souterraines précisées dans \"description\"","Eaux souterraines","N/A","2","C5-C40-Coupes hydrocarbures | Chlorobenzene | Conductivité électrique de l'eau non ramenée à une température conventionnelle | Potentiel en Hydrogène (pH) | Somme de COHV | Somme des 7 PCBi | Somme équivalent toxique dioxine, furane, PCB-DL","Chlorobenzène et mono-aromatiques halogénés | COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF) | Physique","N/A","N/A","N/A","N/A","N/A"]
["SSP53656202","Surveillance environnementale",null,null,"Modalités de surveillance des gaz du sol précisées dans \"description\"",null,"N/A","4","C10-C16-Coupes hydrocarbures | C5-C10-Coupes hydrocarbures | Chlorobenzene | Somme de benzene, toluene, ethylbenzene, xylenes (BTEX) | Somme de COHV | Somme des 7 PCBi","Benzène et dérivés | Chlorobenzène et mono-aromatiques halogénés | COHV, solvants chlorés, fréons | Hydrocarbures et indices liés | PCB (arochlors), PCT, Dioxines, Furanes (PCDD, PCDF)","N/A","N/A","N/A","N/A","N/A"]
["SSP55300901","Etude SSP et ingénierie des travaux de réhabilitation","2017-03-03",null,"L’étude de sols réalisée par le bureau d’études ARTELIA en octobre 2016, a constitué en l’exécution de :\n•\t60 sondages au droit des installations potentiellement polluantes de l’hôpital, de la station d’épuration des eaux usées de l’hôpital et de la décharge,\n•\t5 prélèvements de dalles de béton dans les bâtiments où des activités à risque potentiel de pollution  ont été pratiquées et dans un bâtiment pour lequel aucune activité polluante n’est connue,\n•\t7 prélèvements d’eaux souterraines (4 piézomètres et 3 en sous-sol),\n•\t2 prélèvements de sédiments des bassins de l’ancienne station d’épuration des eaux usées afin de les caractériser chimiquement en vue d’une évacuation.\n\nDes sondages ont été également réalisés dans le local du service technique, la fosse de la chaufferie et un point central de l’hôpital.\n\n4 piézomètres (PZ1, PZ2, PZ3, PZ4) de 5 mètres de profondeur ont été implantés le 17 octobre 2016 en périphérie du site de l’hôpital.\n\nLes analyses menées dans le cadre des investigations ont porté sur la recherche et le dosage des substances polluantes suivantes : hydrocarbures totaux (C5-C40), BTEX, HAP, COHV, 8 éléments traces métalliques et PCB.\n\nLe diagnostic environnemental du site réalisé par le bureau d’études ARTELIA de septembre 2016 à janvier 2017 montre l’existence de plusieurs sources de pollution ou zones polluées :\n•\tune seule zone source en polluants organiques (hydrocarbures). Cette zone est définie comme source au regard du bruit de fond géochimique local mais selon le retour d’expérience du bureau d’études ARTELIA, elle serait non significative,\n•\tune zone source en métaux et métalloïdes (mercure), également impactée par des dioxines et furanes. L’emprise de la zone reste à définir (Voir § 3.5 Propositions d’investigations complémentaire ci-dessus),\n•\tdes impacts ponctuels en métaux,\n•\tdes impacts diffus en métaux et en HAP, définis au regard du bruit de fond géochimique local. Ces impacts ne sont représentatifs ni de risques sanitaires ni de gestion particulière des terres concernées en cas d’excavation et d’évacuation,\n•\tdes sols au droit du site ne répondant pas aux critères de qualité d’un déchet inerte au regard des leurs teneurs en fluorures et sulfates,\n•\tdes impacts ponctuels sur la dalle en béton de l’hôpital qu’il conviendra de gérer en filière de traitement spécifique,\n•\tdes sédiments contenus dans la station d’épuration des eaux usées de l’hôpital pollués et à gérer en filière de traitement autorisée à cet effet lors de son démantèlement.\n\n",null,"Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP55300901","Exécution des travaux de réhabilitation","2019-05-09","2019-07-17","Les rapports de fin de travaux indiquent que les travaux de dépollution se sont déroulés du 20 mai au 17 juillet 2019 pour la zone « Hôpital » (version : V0A du 28/08/2019)\n  \nA l’issue des terrassements, un contrôle analytique des bords et fonds de fouille a validé le respect des seuils de réhabilitations.\n\nChaque lot de terre a été caractérisé avant évacuation pour définir son orientation en filière de traitement. L’exploitant a justifié l’envoi des terres polluées vers des filières autorisées à les recevoir, les bordereaux étant annexés au rapport de fin de travaux.",null,"N/A","N/A","N/A","N/A","Travaux de dépollution"]
["SSP55300901","Exécution des travaux de réhabilitation","2020-03-03","2021-02-09","Au sein du bassin 1, toutes les boues et les eaux, au sein du décanteur primaire, du décanteur final et du filtre percolateur, ont été complètement retirées au mois de mars 2020.\n\nAu niveau du bassin 2, (bassin à zéolithe) la pollution était imputable au mât d’aspersion de l’eau qui permettait une filtration efficace par la roche à zéolithe.\n\nLors de l’étude sur ce bassin, il a été conclu la présence de 15 m³ de matériaux drainants ainsi que le béton à proximité du mât d’aspersion.\n\nLes travaux du 3 mars 2020 au 9 février 2021 ont permis de retirer l’ensemble des matériaux impactés (curage manuel et conditionnement en fût de 60 l des matériaux impactés).",null,"N/A","N/A","N/A","N/A","Travaux de dépollution"]
["SSP57105301","Etude SSP et ingénierie des travaux de réhabilitation","2012-12-14","2012-12-14","Un diagnostic de la qualité des milieux sols et eaux souterraines a été effectué par GINGER ENVIRONNEMENT & INFRASTRUCTURES - Service Sites et Sols pollués (GEI-SSP) en 2012. Le rapport correspondant, en date du 14/12/12 a mis en évidence les conclusions suivantes : \n\n    • Aucune problématique liée à la présence de métaux lourds \n    • Pas d’impact sur les eaux souterraines (aucune trace de polluants relevée)\n    • Poche de pollution aux hydrocarbures (limitée en profondeur à la couche superficielle et en étendue à une superficie de l’ordre de 100 m²) : une concentration en HCT de l’ordre de 2 300 mg/kg MS avait été relevé\n\nGEI-SSP recommandait d’excaver la poche de pollution. ",null,"Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP57105301","Etude SSP et ingénierie des travaux de réhabilitation","2018-09-17","2018-09-17","SOCOTEC a procédé à une analyse des risques résiduels pour la santé humaine, avec comme usage futur de la parcelle d’étude, un aménagement en jardin public. \n\nL’hypothèse prise en considération est celle d’un aménagement en jardin public avec un apport de terre végétale sur au moins 30 m d’épaisseur et les allées de remblais d’apports sains ainsi que la mise en place d’une interface entre les sols restant en place et les matériaux saints rapportés. \n\nLes composés hydrocarbures totaux C10-C12, benzène et naphtalène ont été étudiés. Les cibles qui ont été considérées comme susceptibles d’être exposées sont les passants et riverains (adultes et enfants). \n\nL’analyse des risques résiduels a mis en évidence des niveaux de risques sanitaires, liés aux effets à seuils et sans seuil calculés, acceptables pour les cibles considérées (quotient de danger cumulé inférieur à 1 et excès de risques individuels inférieur à 10-5). \n\nLes contaminations relevées dans les sols ont été jugées compatibles avec l’aménagement et l’usage du site défini (aménagement d’un jardin public). \n",null,"Analyse des enjeux sanitaires (EQRS, ARR)","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP57105301","Exécution des travaux de réhabilitation","2017-05-10","2017-05-11","SUEZ Remediation est intervenu du 10 au 11 mai 2017 sur la parcelle 2017 pour une dépollution des sols, dans la zone identifiée par GEI-SSP. 56 tonnes de terres ont été évacuées en ISDND. Des contrôles post-travaux et une remise en état par remblaiement de la fouille et recouvrement de terres végétales ont été réalisées. \n\nLes conclusions, issues des contrôles de récolement, sont les suivantes :\n\n    • Les teneurs en hydrocarbures des échantillons prélevés présentaient des teneurs en hydrocarbures toutes inférieures aux seuls d’acceptation des matériaux dans les ISDI\n    • 4 échantillons  présentaient des trace d’HC supérieures au bruit de fond des appareils de mesure pour les deux coupes les plus lourdes (C21 à C35 et C35 à C40)\n    • 1 échantillon présentait des traces d’HC pour toutes les coupes pétrolières (C10 à C40) avec les concentrations les plus élevées pour les coupes les plus lourdes. \n",null,"N/A","N/A","N/A","N/A","Travaux de dépollution"]
["SSP57138401","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"Des déchets résiduels (pneus, bois, pièces diverses...) sont toujours présents dans les deux sites et n'ont pas été évacués par la liquidation car elle ne disposait pas des moyens financiers requis. ","Sol - Sous-sol","Etude macro","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP57138401","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"3  prélèvements de sols superficiels (15 à 20cm de profondeur) ont été réalisé sur la parcelle 620 à l'aide d'une foreuse hydraulique aux endroits suivants :\n- Entrée du local de dépollution ;\n- Bâtiment du local de dépollution ;\n- Arrière du local de dépollution.\nCes forages ayant pour but de déterminer des polluants potentiels.\n\nCes sondages ont permis de mettre en évidence des impacts en hydrocarbures et HAP à l'extérieur du bâtiment affecté à la dépollution des VTHU. \n\nSeul le site de dépollution à fait l'objet de quelques prélèvements du sol compte tenu des moyens financiers. Des investigations complémentaires seront donc à déclencher préalablement à la réutilisation ou à la vente des deux sites. ","Sol - Sous-sol","Diagnostic et Analyse","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]
["SSP57138401","Etude SSP et ingénierie des travaux de réhabilitation",null,null,"Les études historique, documentaire et mémorielle ont permis d'identifier le site, son historique et ses usages. \n\nDifférents risques de pollution ont ainsi pu être déterminé :\n- Risque d'écoulements de carburants et autres liquides de VTHU ;\n- Risque d'écoulements par des fissures dans la dalle de béton assurant l'imperméabilisation de la zone de dépollution des VTHU ;\n- D'un incendie par les eaux d'extinction. ",null,"Etude historique, documentaire et mémorielle","N/A",null,null,"N/A","N/A","N/A","N/A","N/A"]